"No","ClassNo","ClassName_en","FXY","ElementName_en","Note_en","BUFR_Unit","BUFR_Scale","BUFR_ReferenceValue","BUFR_DataWidth_Bits","CREX_Unit","CREX_Scale","CREX_DataWidth_Char","Status"
1.00,"00","BUFR/CREX table entries","000001","Table A: entry",,"CCITT IA5","0","0","24","Character","0","3","Operational"
2.00,"00","BUFR/CREX table entries","000002","Table A: data category description, line 1",,"CCITT IA5","0","0","256","Character","0","32","Operational"
3.00,"00","BUFR/CREX table entries","000003","Table A: data category description, line 2",,"CCITT IA5","0","0","256","Character","0","32","Operational"
4.00,"00","BUFR/CREX table entries","000004","BUFR/CREX Master table","(see Note 1)","CCITT IA5","0","0","16","Character","0","2","Operational"
5.00,"00","BUFR/CREX table entries","000005","BUFR/CREX edition number",,"CCITT IA5","0","0","24","Character","0","3","Operational"
6.00,"00","BUFR/CREX table entries","000006","BUFR Master table version number","(see Note 2)","CCITT IA5","0","0","16","Character","0","2","Operational"
7.00,"00","BUFR/CREX table entries","000007","CREX Master table version number","(see Note 3)","CCITT IA5","0","0","16","Character","0","2","Operational"
8.00,"00","BUFR/CREX table entries","000008","BUFR Local table version number","(see Note 4)","CCITT IA5","0","0","16","Character","0","2","Operational"
9.00,"00","BUFR/CREX table entries","000010","F descriptor to be added or defined",,"CCITT IA5","0","0","8","Character","0","1","Operational"
10.00,"00","BUFR/CREX table entries","000011","X descriptor to be added or defined",,"CCITT IA5","0","0","16","Character","0","2","Operational"
11.00,"00","BUFR/CREX table entries","000012","Y descriptor to be added or defined",,"CCITT IA5","0","0","24","Character","0","3","Operational"
12.00,"00","BUFR/CREX table entries","000013","Element name, line 1",,"CCITT IA5","0","0","256","Character","0","32","Operational"
13.00,"00","BUFR/CREX table entries","000014","Element name, line 2",,"CCITT IA5","0","0","256","Character","0","32","Operational"
14.00,"00","BUFR/CREX table entries","000015","Units name",,"CCITT IA5","0","0","192","Character","0","24","Operational"
15.00,"00","BUFR/CREX table entries","000016","Units scale sign",,"CCITT IA5","0","0","8","Character","0","1","Operational"
16.00,"00","BUFR/CREX table entries","000017","Units scale",,"CCITT IA5","0","0","24","Character","0","3","Operational"
17.00,"00","BUFR/CREX table entries","000018","Units reference sign",,"CCITT IA5","0","0","8","Character","0","1","Operational"
18.00,"00","BUFR/CREX table entries","000019","Units reference value",,"CCITT IA5","0","0","80","Character","0","10","Operational"
19.00,"00","BUFR/CREX table entries","000020","Element data width",,"CCITT IA5","0","0","24","Character","0","3","Operational"
20.00,"00","BUFR/CREX table entries","000024","Code figure",,"CCITT IA5","0","0","64","Character","0","8","Operational"
21.00,"00","BUFR/CREX table entries","000025","Code figure meaning",,"CCITT IA5","0","0","496","Character","0","62","Operational"
22.00,"00","BUFR/CREX table entries","000026","Bit number",,"CCITT IA5","0","0","48","Character","0","6","Operational"
23.00,"00","BUFR/CREX table entries","000027","Bit number meaning",,"CCITT IA5","0","0","496","Character","0","62","Operational"
24.00,"00","BUFR/CREX table entries","000030","Descriptor defining sequence",,"CCITT IA5","0","0","48","Character","0","6","Operational"
25.00,"01","BUFR/CREX Identification","001001","WMO block number",,"Numeric","0","0","7","Numeric","0","2","Operational"
26.00,"01","BUFR/CREX Identification","001002","WMO station number",,"Numeric","0","0","10","Numeric","0","3","Operational"
27.00,"01","BUFR/CREX Identification","001003","WMO Region number/geographical area",,"Code table","0","0","3","Code table","0","1","Operational"
28.00,"01","BUFR/CREX Identification","001004","WMO Region sub-area","(see Note 9)","Numeric","0","0","3","Numeric","0","1","Operational"
29.00,"01","BUFR/CREX Identification","001005","Buoy/platform identifier",,"Numeric","0","0","17","Numeric","0","5","Operational"
30.00,"01","BUFR/CREX Identification","001006","Aircraft flight number",,"CCITT IA5","0","0","64","Character","0","8","Operational"
31.00,"01","BUFR/CREX Identification","001007","Satellite identifier",,"Code table","0","0","10","Code table","0","4","Operational"
32.00,"01","BUFR/CREX Identification","001008","Aircraft registration number or other identification",,"CCITT IA5","0","0","64","Character","0","8","Operational"
33.00,"01","BUFR/CREX Identification","001009","Type of commercial aircraft",,"CCITT IA5","0","0","64","Character","0","8","Operational"
34.00,"01","BUFR/CREX Identification","001010","Stationary buoy platform identifier; e.g. C-MAN buoys",,"CCITT IA5","0","0","64","Character","0","8","Operational"
35.00,"01","BUFR/CREX Identification","001011","Ship or mobile land station identifier",,"CCITT IA5","0","0","72","Character","0","9","Operational"
36.00,"01","BUFR/CREX Identification","001012","Direction of motion of moving observing platform","*","degree true","0","0","9","degree true","0","3","Operational"
37.00,"01","BUFR/CREX Identification","001013","Speed of motion of moving observing platform","*","m/s","0","0","10","m/s","0","3","Operational"
38.00,"01","BUFR/CREX Identification","001014","Platform drift speed (high precision)",,"m/s","2","0","10","m/s","2","4","Operational"
39.00,"01","BUFR/CREX Identification","001015","Station or site name",,"CCITT IA5","0","0","160","Character","0","20","Operational"
40.00,"01","BUFR/CREX Identification","001018","Short station or site name",,"CCITT IA5","0","0","40","Character","0","5","Operational"
41.00,"01","BUFR/CREX Identification","001019","Long station or site name",,"CCITT IA5","0","0","256","Character","0","32","Operational"
42.00,"01","BUFR/CREX Identification","001020","WMO Region sub-area",,"Numeric","0","0","4","Numeric","0","2","Operational"
43.00,"01","BUFR/CREX Identification","001021","Synoptic feature identifier",,"Numeric","0","0","14","Numeric","0","4","Operational"
44.00,"01","BUFR/CREX Identification","001022","Name of feature","(see Note 11)","CCITT IA5","0","0","224","Character","0","28","Operational"
45.00,"01","BUFR/CREX Identification","001023","Observation sequence number",,"Numeric","0","0","9","Numeric","0","3","Operational"
46.00,"01","BUFR/CREX Identification","001024","Wind speed source",,"Code table","0","0","5","Code table","0","2","Operational"
47.00,"01","BUFR/CREX Identification","001025","Storm identifier","(see Note 1)","CCITT IA5","0","0","24","Character","0","3","Operational"
48.00,"01","BUFR/CREX Identification","001026","WMO storm name","**","CCITT IA5","0","0","64","Character","0","8","Operational"
49.00,"01","BUFR/CREX Identification","001027","WMO long storm name","**","CCITT IA5","0","0","80","Character","0","10","Operational"
50.00,"01","BUFR/CREX Identification","001028","Aerosol optical depth (AOD) source",,"Code table","0","0","5","Code table","0","2","Operational"
51.00,"01","BUFR/CREX Identification","001029","SSI source",,"Code table","0","0","5","Code table","0","2","Operational"
52.00,"01","BUFR/CREX Identification","001030","Numerical model identifier","(see Note 13)","CCITT IA5","0","0","128","Character","0","16","Operational"
53.00,"01","BUFR/CREX Identification","001031","Identification of originating/generating centre","(see Note 10)","Code table","0","0","16","Code table","0","5","Operational"
54.00,"01","BUFR/CREX Identification","001032","Generating application","(Notes 3, 4 and 5)","Code table defined by originating/generating centre","0","0","8","Code table","0","3","Operational"
55.00,"01","BUFR/CREX Identification","001033","Identification of originating/generating centre",,"Common Code table C-1","0","0","8","Common Code table C-1","0","3","Operational"
56.00,"01","BUFR/CREX Identification","001034","Identification of originating/generating sub-centre",,"Common Code table C-12","0","0","8","Common Code table C-12","0","3","Operational"
57.00,"01","BUFR/CREX Identification","001035","Originating centre",,"Common Code table C-11","0","0","16","Common Code Table C-11","0","5","Operational"
58.00,"01","BUFR/CREX Identification","001036","Agency in charge of operating the observing platform",,"Code table","0","0","20","Code table","0","7","Operational"
59.00,"01","BUFR/CREX Identification","001037","SIGMET sequence identifier",,"CCITT IA5","0","0","24","Character","0","3","Operational"
60.00,"01","BUFR/CREX Identification","001038","Source of sea ice fraction",,"Code table","0","0","5","Code table","0","2","Operational"
61.00,"01","BUFR/CREX Identification","001039","Graphical Area Forecast (GFA) sequence identifier",,"CCITT IA5","0","0","40","Character","0","5","Operational"
62.00,"01","BUFR/CREX Identification","001040","Processing centre ID code",,"CCITT IA5","0","0","48","Character","0","6","Operational"
63.00,"01","BUFR/CREX Identification","001041","Absolute platform velocity - first component","(see Note 6)","m/s","5","-1073741824","31","m/s","5","10","Operational"
64.00,"01","BUFR/CREX Identification","001042","Absolute platform velocity - second component","(see Note 6)","m/s","5","-1073741824","31","m/s","5","10","Operational"
65.00,"01","BUFR/CREX Identification","001043","Absolute platform velocity - third component","(see Note 6)","m/s","5","-1073741824","31","m/s","5","10","Operational"
66.00,"01","BUFR/CREX Identification","001050","Platform transmitter ID number",,"Numeric","0","0","17","Numeric","0","6","Operational"
67.00,"01","BUFR/CREX Identification","001051","Platform transmitter ID number",,"CCITT IA5","0","0","96","Character","0","12","Operational"
68.00,"01","BUFR/CREX Identification","001052","Platform transmitter ID",,"Code table","0","0","3","Code table","0","1","Operational"
69.00,"01","BUFR/CREX Identification","001053","Tsunameter report sequence number triggered by a tsunami event",,"Numeric","0","0","7","Numeric","0","2","Operational"
70.00,"01","BUFR/CREX Identification","001060","Aircraft reporting point (Beacon identifier)",,"CCITT IA5","0","0","64","Character","0","8","Operational"
71.00,"01","BUFR/CREX Identification","001062","Short ICAO location indicator",,"CCITT IA5","0","0","32","Character","0","4","Operational"
72.00,"01","BUFR/CREX Identification","001063","ICAO location indicator",,"CCITT IA5","0","0","64","Character","0","8","Operational"
73.00,"01","BUFR/CREX Identification","001064","Runway designator",,"CCITT IA5","0","0","32","Character","0","4","Operational"
74.00,"01","BUFR/CREX Identification","001065","ICAO region identifier",,"CCITT IA5","0","0","256","Character","0","32","Operational"
75.00,"01","BUFR/CREX Identification","001075","Tide station identification",,"CCITT IA5","0","0","40","Character","0","5","Operational"
76.00,"01","BUFR/CREX Identification","001079","Unique identifier for the profile",,"CCITT IA5","0","0","64","Character","0","8","Operational"
77.00,"01","BUFR/CREX Identification","001080","Ship line number according to SOOP",,"CCITT IA5","0","0","32","Character","0","4","Operational"
78.00,"01","BUFR/CREX Identification","001081","Radiosonde serial number",,"CCITT IA5","0","0","160","Character","0","20","Operational"
79.00,"01","BUFR/CREX Identification","001082","Radiosonde ascension number","(see Note 12)","Numeric","0","0","14","Numeric","0","4","Operational"
80.00,"01","BUFR/CREX Identification","001083","Radiosonde release number","(see Note 12)","Numeric","0","0","3","Numeric","0","1","Operational"
81.00,"01","BUFR/CREX Identification","001085","Observing platform manufacturer's model",,"CCITT IA5","0","0","160","Character","0","20","Operational"
82.00,"01","BUFR/CREX Identification","001086","Observing platform manufacturer's serial number",,"CCITT IA5","0","0","256","Character","0","32","Operational"
83.00,"01","BUFR/CREX Identification","001087","WMO marine observing platform extended identifier",,"Numeric","0","0","23","Numeric","0","7","Operational"
84.00,"01","BUFR/CREX Identification","001090","Technique for making up initial perturbations",,"Code table","0","0","8","Code table","0","3","Operational"
85.00,"01","BUFR/CREX Identification","001091","Ensemble member number",,"Numeric","0","0","10","Numeric","0","4","Operational"
86.00,"01","BUFR/CREX Identification","001092","Type of ensemble forecast",,"Code table","0","0","8","Code table","0","3","Operational"
87.00,"01","BUFR/CREX Identification","001093","Balloon lot number",,"CCITT IA5","0","0","96","Character","0","12","Operational"
88.00,"01","BUFR/CREX Identification","001094","WBAN number",,"Numeric","0","0","17","Numeric","0","5","Operational"
89.00,"01","BUFR/CREX Identification","001095","Observer identification",,"CCITT IA5","0","0","32","Character","0","4","Operational"
90.00,"01","BUFR/CREX Identification","001096","Station acquisition",,"CCITT IA5","0","0","160","Character","0","20","Operational"
93.00,"01","BUFR/CREX Identification","001099","Unique product definition",,"CCITT IA5","0","0","248","Character","0","31","Operational"
94.00,"01","BUFR/CREX Identification","001101","State identifier",,"Code table","0","0","10","Code table","0","3","Operational"
95.00,"01","BUFR/CREX Identification","001102","National station number",,"Numeric","0","0","30","Numeric","0","9","Operational"
96.00,"01","BUFR/CREX Identification","001103","IMO Number. Unique Lloyd's register",,"Numeric","0","0","24","Numeric","0","7","Operational"
97.00,"01","BUFR/CREX Identification","001110","Aircraft tail number",,"CCITT IA5","0","0","48","Character","0","6","Operational"
98.00,"01","BUFR/CREX Identification","001111","Origination airport",,"CCITT IA5","0","0","24","Character","0","3","Operational"
99.00,"01","BUFR/CREX Identification","001112","Destination airport",,"CCITT IA5","0","0","24","Character","0","3","Operational"
100.00,"01","BUFR/CREX Identification","001113","Template version number defined by originating centre",,"Numeric","1","0","9","Numeric","1","3","Operational"
102.00,"01","BUFR/CREX Identification","001115","Identifier of the cruise or mission under which the data were collected",,"CCITT IA5","0","0","160","Character","0","20","Operational"
103.00,"01","BUFR/CREX Identification","001124","Grid point identifier",,"Numeric","0","0","24","Numeric","0","8","Operational"
104.00,"01","BUFR/CREX Identification","001144","Snapshot identifier",,"Numeric","0","0","31","Numeric","0","10","Operational"
105.00,"02","BUFR/CREX Instrumentation","002001","Type of station",,"Code table","0","0","2","Code table","0","1","Operational"
106.00,"02","BUFR/CREX Instrumentation","002002","Type of instrumentation for wind measurement",,"Flag table","0","0","4","Flag table","0","2","Operational"
107.00,"02","BUFR/CREX Instrumentation","002003","Type of measuring equipment used",,"Code table","0","0","4","Code table","0","2","Operational"
108.00,"02","BUFR/CREX Instrumentation","002004","Type of instrumentation for evaporation measurement or type of crop for which evapotranspiration is reported",,"Code table","0","0","4","Code table","0","2","Operational"
109.00,"02","BUFR/CREX Instrumentation","002005","Precision of temperature observation",,"K","2","0","7","K","2","3","Operational"
111.00,"02","BUFR/CREX Instrumentation","002007","Type of sensor for water level measuring instrument",,"Code table","0","0","6","Code table","0","2","Operational"
113.00,"02","BUFR/CREX Instrumentation","002011","Radiosonde type",,"Code table","0","0","8","Code table","0","3","Operational"
114.00,"02","BUFR/CREX Instrumentation","002012","Radiosonde computational method",,"Code table","0","0","4","Code table","0","2","Operational"
115.00,"02","BUFR/CREX Instrumentation","002013","Solar and infrared radiation correction",,"Code table","0","0","4","Code table","0","2","Operational"
116.00,"02","BUFR/CREX Instrumentation","002014","Tracking technique/status of system used",,"Code table","0","0","7","Code table","0","3","Operational"
117.00,"02","BUFR/CREX Instrumentation","002015","Radiosonde completeness",,"Code table","0","0","4","Code table","0","2","Operational"
118.00,"02","BUFR/CREX Instrumentation","002016","Radiosonde configuration",,"Flag table","0","0","5","Flag table","0","2","Operational"
119.00,"02","BUFR/CREX Instrumentation","002017","Correction algorithms for humidity measurements",,"Code table","0","0","5","Code table","0","2","Operational"
120.00,"02","BUFR/CREX Instrumentation","002019","Satellite instruments",,"Code table","0","0","11","Code table","0","4","Operational"
121.00,"02","BUFR/CREX Instrumentation","002020","Satellite classification",,"Code table","0","0","9","Code table","0","3","Operational"
122.00,"02","BUFR/CREX Instrumentation","002021","Satellite instrument data used in processing","*","Flag table","0","0","9","Flag table","0","3","Operational"
123.00,"02","BUFR/CREX Instrumentation","002022","Satellite data-processing technique used",,"Flag table","0","0","8","Flag table","0","3","Operational"
124.00,"02","BUFR/CREX Instrumentation","002023","Satellite-derived wind computation method",,"Code table","0","0","4","Code table","0","2","Operational"
125.00,"02","BUFR/CREX Instrumentation","002024","Integrated mean humidity computational method",,"Code table","0","0","4","Code table","0","2","Operational"
126.00,"02","BUFR/CREX Instrumentation","002025","Satellite channel(s) used in computation",,"Flag table","0","0","25","Flag table","0","9","Operational"
127.00,"02","BUFR/CREX Instrumentation","002026","Cross-track resolution",,"m","2","0","12","m","2","4","Operational"
128.00,"02","BUFR/CREX Instrumentation","002027","Along-track resolution",,"m","2","0","12","m","2","4","Operational"
129.00,"02","BUFR/CREX Instrumentation","002028","Segment size at nadir in x-direction",,"m","0","0","18","m","0","6","Operational"
130.00,"02","BUFR/CREX Instrumentation","002029","Segment size at nadir in y-direction",,"m","0","0","18","m","0","6","Operational"
131.00,"02","BUFR/CREX Instrumentation","002030","Method of current measurement",,"Code table","0","0","3","Code table","0","1","Operational"
132.00,"02","BUFR/CREX Instrumentation","002031","Duration and time of current measurement",,"Code table","0","0","5","Code table","0","2","Operational"
133.00,"02","BUFR/CREX Instrumentation","002032","Indicator for digitization",,"Code table","0","0","2","Code table","0","1","Operational"
134.00,"02","BUFR/CREX Instrumentation","002033","Method of salinity/depth measurement",,"Code table","0","0","3","Code table","0","1","Operational"
135.00,"02","BUFR/CREX Instrumentation","002034","Drogue type",,"Code table","0","0","5","Code table","0","2","Operational"
136.00,"02","BUFR/CREX Instrumentation","002035","Cable length",,"m","0","0","9","m","0","3","Operational"
137.00,"02","BUFR/CREX Instrumentation","002036","Buoy type",,"Code table","0","0","2","Code table","0","1","Operational"
138.00,"02","BUFR/CREX Instrumentation","002037","Method of tidal observation",,"Code table","0","0","3","Code table","0","1","Operational"
139.00,"02","BUFR/CREX Instrumentation","002038","Method of water temperature and/or salinity measurement",,"Code table","0","0","4","Code table","0","2","Operational"
140.00,"02","BUFR/CREX Instrumentation","002039","Method of wet-bulb temperature measurement",,"Code table","0","0","3","Code table","0","1","Operational"
141.00,"02","BUFR/CREX Instrumentation","002040","Method of removing velocity and motion of platform from current",,"Code table","0","0","4","Code table","0","2","Operational"
142.00,"02","BUFR/CREX Instrumentation","002041","Method for estimating reports related to synoptic features",,"Code table","0","0","6","Code table","0","2","Operational"
143.00,"02","BUFR/CREX Instrumentation","002042","Indicator for sea-surface current speed",,"Code table","0","0","2","Code table","0","1","Operational"
144.00,"02","BUFR/CREX Instrumentation","002044","Indicator for method of calculating spectral wave data",,"Code table","0","0","4","Code table","0","2","Operational"
145.00,"02","BUFR/CREX Instrumentation","002045","Indicator for type of platform",,"Code table","0","0","4","Code table","0","2","Operational"
146.00,"02","BUFR/CREX Instrumentation","002046","Wave measurement instrumentation",,"Code table","0","0","4","Code table","0","2","Operational"
147.00,"02","BUFR/CREX Instrumentation","002047","Deep-ocean tsunameter type",,"Code table","0","0","7","Code table","0","2","Operational"
148.00,"02","BUFR/CREX Instrumentation","002048","Satellite sensor indicator",,"Code table","0","0","4","Code table","0","2","Operational"
149.00,"02","BUFR/CREX Instrumentation","002049","Geostationary satellite data-processing technique used",,"Flag table","0","0","8","Flag table","0","3","Operational"
150.00,"02","BUFR/CREX Instrumentation","002050","Geostationary sounder satellite channels used",,"Flag table","0","0","20","Flag table","0","7","Operational"
151.00,"02","BUFR/CREX Instrumentation","002051","Indicator to specify observing method for extreme temperatures",,"Code table","0","0","4","Code table","0","2","Operational"
152.00,"02","BUFR/CREX Instrumentation","002052","Geostationary imager satellite channels used",,"Flag table","0","0","6","Flag table","0","2","Operational"
153.00,"02","BUFR/CREX Instrumentation","002053","GOES-I/M brightness temperature characteristics",,"Code table","0","0","4","Code table","0","2","Operational"
154.00,"02","BUFR/CREX Instrumentation","002054","GOES-I/M soundings parameter characteristics",,"Code table","0","0","4","Code table","0","2","Operational"
155.00,"02","BUFR/CREX Instrumentation","002055","Geostationary soundings statistical parameters",,"Code table","0","0","4","Code table","0","2","Operational"
156.00,"02","BUFR/CREX Instrumentation","002056","Geostationary soundings accuracy statistics",,"Code table","0","0","4","Code table","0","2","Operational"
157.00,"02","BUFR/CREX Instrumentation","002057","Origin of first-guess information for GOES-I/M soundings",,"Code table","0","0","4","Code table","0","2","Operational"
158.00,"02","BUFR/CREX Instrumentation","002058","Valid times of first-guess information for GOES-I/M soundings",,"Code table","0","0","4","Code table","0","2","Operational"
159.00,"02","BUFR/CREX Instrumentation","002059","Origin of analysis information for GOES-I/M soundings",,"Code table","0","0","4","Code table","0","2","Operational"
160.00,"02","BUFR/CREX Instrumentation","002060","Origin of surface information for GOES-I/M soundings",,"Code table","0","0","4","Code table","0","2","Operational"
161.00,"02","BUFR/CREX Instrumentation","002061","Aircraft navigational system",,"Code table","0","0","3","Code table","0","1","Operational"
162.00,"02","BUFR/CREX Instrumentation","002062","Type of aircraft data relay system",,"Code table","0","0","4","Code table","0","2","Operational"
163.00,"02","BUFR/CREX Instrumentation","002063","Aircraft roll angle",,"deg","2","-18000","16","deg","2","5","Operational"
164.00,"02","BUFR/CREX Instrumentation","002064","Aircraft roll angle quality",,"Code table","0","0","2","Code table","0","1","Operational"
165.00,"02","BUFR/CREX Instrumentation","002065","ACARS ground-receiving station",,"CCITT IA5","0","0","40","Character","0","5","Operational"
166.00,"02","BUFR/CREX Instrumentation","002066","Radiosonde ground receiving system",,"Code table","0","0","6","Code table","0","2","Operational"
167.00,"02","BUFR/CREX Instrumentation","002067","Radiosonde operating frequency",,"Hz","-5","0","15","Hz","-5","5","Operational"
168.00,"02","BUFR/CREX Instrumentation","002070","Original specification of latitude/longitude",,"Code table","0","0","4","Code table","0","2","Operational"
169.00,"02","BUFR/CREX Instrumentation","002071","Spectrographic wavelength",,"m","13","0","30","m","13","10","Operational"
170.00,"02","BUFR/CREX Instrumentation","002072","Spectrographic width",,"m","13","0","30","m","13","10","Operational"
171.00,"02","BUFR/CREX Instrumentation","002080","Balloon manufacturer",,"Code table","0","0","6","Code table","0","2","Operational"
172.00,"02","BUFR/CREX Instrumentation","002081","Type of balloon",,"Code table","0","0","5","Code table","0","2","Operational"
173.00,"02","BUFR/CREX Instrumentation","002082","Weight of balloon",,"kg","3","0","12","kg","3","4","Operational"
174.00,"02","BUFR/CREX Instrumentation","002083","Type of balloon shelter",,"Code table","0","0","4","Code table","0","2","Operational"
175.00,"02","BUFR/CREX Instrumentation","002084","Type of gas used in balloon",,"Code table","0","0","4","Code table","0","2","Operational"
176.00,"02","BUFR/CREX Instrumentation","002085","Amount of gas used in balloon",,"kg","3","0","13","kg","3","4","Operational"
177.00,"02","BUFR/CREX Instrumentation","002086","Balloon flight train length",,"m","1","0","10","m","1","4","Operational"
178.00,"02","BUFR/CREX Instrumentation","002091","Entry sensor 4/20 mA",,"A","4","0","10","A","4","3","Operational"
179.00,"02","BUFR/CREX Instrumentation","002095","Type of pressure sensor",,"Code table","0","0","5","Code table","0","2","Operational"
180.00,"02","BUFR/CREX Instrumentation","002096","Type of temperature sensor",,"Code table","0","0","5","Code table","0","2","Operational"
181.00,"02","BUFR/CREX Instrumentation","002097","Type of humidity sensor",,"Code table","0","0","5","Code table","0","2","Operational"
183.00,"02","BUFR/CREX Instrumentation","002099","Polarization",,"Code table","0","0","3","Code table","0","1","Operational"
184.00,"02","BUFR/CREX Instrumentation","002100","Radar constant","**","dB","1","0","12","dB","1","4","Operational"
185.00,"02","BUFR/CREX Instrumentation","002101","Type of antenna",,"Code table","0","0","4","Code table","0","2","Operational"
186.00,"02","BUFR/CREX Instrumentation","002102","Antenna height above tower base",,"m","0","0","8","m","0","3","Operational"
187.00,"02","BUFR/CREX Instrumentation","002103","Radome",,"Flag table","0","0","2","Flag table","0","1","Operational"
188.00,"02","BUFR/CREX Instrumentation","002104","Antenna polarization",,"Code table","0","0","4","Code table","0","2","Operational"
189.00,"02","BUFR/CREX Instrumentation","002105","Maximum antenna gain",,"dB","0","0","6","dB","0","2","Operational"
190.00,"02","BUFR/CREX Instrumentation","002106","3-dB beamwidth",,"deg","1","0","6","deg","1","2","Operational"
191.00,"02","BUFR/CREX Instrumentation","002107","Sidelobe suppression",,"dB","0","0","6","dB","0","2","Operational"
192.00,"02","BUFR/CREX Instrumentation","002108","Crosspol discrimination (on axis)",,"dB","0","0","6","dB","0","2","Operational"
193.00,"02","BUFR/CREX Instrumentation","002109","Antenna speed (azimuth)",,"deg/s","2","0","12","deg/s","2","4","Operational"
194.00,"02","BUFR/CREX Instrumentation","002110","Antenna speed (elevation)",,"deg/s","2","0","12","deg/s","2","4","Operational"
195.00,"02","BUFR/CREX Instrumentation","002111","Radar incidence angle",,"deg","1","0","10","deg","1","4","Operational"
196.00,"02","BUFR/CREX Instrumentation","002112","Radar look angle",,"deg","1","0","12","deg","1","4","Operational"
197.00,"02","BUFR/CREX Instrumentation","002113","Number of azimuth looks",,"Numeric","0","0","4","Numeric","0","2","Operational"
198.00,"02","BUFR/CREX Instrumentation","002114","Antenna effective surface area",,"m2","0","0","15","m2","0","5","Operational"
199.00,"02","BUFR/CREX Instrumentation","002115","Type of surface observing equipment",,"Code table","0","0","5","Code table","0","2","Operational"
200.00,"02","BUFR/CREX Instrumentation","002116","Percentage of 320 MHz band processed",,"%","0","0","7","%","0","3","Operational"
201.00,"02","BUFR/CREX Instrumentation","002117","Percentage of 80 MHz band processed",,"%","0","0","7","%","0","3","Operational"
202.00,"02","BUFR/CREX Instrumentation","002118","Percentage of 20 MHz band processed",,"%","0","0","7","%","0","3","Operational"
203.00,"02","BUFR/CREX Instrumentation","002119","RA-2 instrument operations",,"Code table","0","0","3","Code table","0","1","Operational"
204.00,"02","BUFR/CREX Instrumentation","002120","Ocean wave frequency",,"Hz","3","0","10","Hz","3","4","Operational"
205.00,"02","BUFR/CREX Instrumentation","002121","Mean frequency",,"Hz","-8","0","7","Hz","-8","3","Operational"
206.00,"02","BUFR/CREX Instrumentation","002122","Frequency agility range",,"Hz","-6","-128","8","Hz","-6","3","Operational"
207.00,"02","BUFR/CREX Instrumentation","002123","Peak power",,"W","-4","0","7","W","-4","3","Operational"
208.00,"02","BUFR/CREX Instrumentation","002124","Average power",,"W","-1","0","7","W","-1","3","Operational"
209.00,"02","BUFR/CREX Instrumentation","002125","Pulse repetition frequency",,"Hz","-1","0","8","Hz","-1","3","Operational"
210.00,"02","BUFR/CREX Instrumentation","002126","Pulse width",,"s","7","0","6","s","7","2","Operational"
211.00,"02","BUFR/CREX Instrumentation","002127","Receiver intermediate frequency",,"Hz","-6","0","7","Hz","-6","3","Operational"
212.00,"02","BUFR/CREX Instrumentation","002128","Intermediate frequency bandwidth",,"Hz","-5","0","6","Hz","-5","2","Operational"
213.00,"02","BUFR/CREX Instrumentation","002129","Minimum detectable signal",,"dB","0","-150","5","dB","0","3","Operational"
214.00,"02","BUFR/CREX Instrumentation","002130","Dynamic range",,"dB","0","0","7","dB","0","3","Operational"
215.00,"02","BUFR/CREX Instrumentation","002131","Sensitivity time control (STC)",,"Flag table","0","0","2","Flag table","0","1","Operational"
216.00,"02","BUFR/CREX Instrumentation","002132","Azimuth pointing accuracy",,"deg","2","0","6","deg","2","2","Operational"
217.00,"02","BUFR/CREX Instrumentation","002133","Elevation pointing accuracy",,"deg","2","0","6","deg","2","2","Operational"
218.00,"02","BUFR/CREX Instrumentation","002134","Antenna beam azimuth",,"deg","2","0","16","deg","2","5","Operational"
219.00,"02","BUFR/CREX Instrumentation","002135","Antenna elevation",,"deg","2","-9000","15","deg","2","5","Operational"
220.00,"02","BUFR/CREX Instrumentation","002136","Range processed by range attenuation correction",,"m","-3","0","16","m","-3","5","Operational"
221.00,"02","BUFR/CREX Instrumentation","002137","Radar dual PRF ratio",,"Code table","0","0","4","Code table","0","2","Operational"
222.00,"02","BUFR/CREX Instrumentation","002138","Antenna rotation direction",,"Code table","0","0","2","Code table","0","1","Operational"
223.00,"02","BUFR/CREX Instrumentation","002139","SIRAL instrument configuration",,"Code table","0","0","2","Code table","0","1","Operational"
224.00,"02","BUFR/CREX Instrumentation","002140","Satellite radar beam azimuth angle","(see Note 4)","deg","0","0","9","deg","0","3","Operational"
225.00,"02","BUFR/CREX Instrumentation","002141","Measurement type",,"CCITT IA5","0","0","24","Character","0","3","Operational"
226.00,"02","BUFR/CREX Instrumentation","002142","Ozone instrument serial number/identification","(see Note 5)","CCITT IA5","0","0","32","Character","0","4","Operational"
227.00,"02","BUFR/CREX Instrumentation","002143","Ozone instrument type",,"Code table","0","0","7","Code table","0","3","Operational"
228.00,"02","BUFR/CREX Instrumentation","002144","Light source type for Brewer spectrophotometer",,"Code table","0","0","4","Code table","0","2","Operational"
229.00,"02","BUFR/CREX Instrumentation","002145","Wavelength setting for Dobson instruments",,"Code table","0","0","4","Code table","0","2","Operational"
230.00,"02","BUFR/CREX Instrumentation","002146","Source conditions for Dobson instruments",,"Code table","0","0","4","Code table","0","2","Operational"
231.00,"02","BUFR/CREX Instrumentation","002147","Method of transmission to collection centre",,"Code table","0","0","6","Code table","0","2","Operational"
232.00,"02","BUFR/CREX Instrumentation","002148","Data collection and/or location system",,"Code table","0","0","5","Code table","0","2","Operational"
233.00,"02","BUFR/CREX Instrumentation","002149","Type of data buoy",,"Code table","0","0","6","Code table","0","2","Operational"
234.00,"02","BUFR/CREX Instrumentation","002150","TOVS/ATOVS/AVHRR instrumentation channel number",,"Code table","0","0","6","Code table","0","2","Operational"
235.00,"02","BUFR/CREX Instrumentation","002151","Radiometer identifier",,"Code table","0","0","11","Code table","0","4","Operational"
236.00,"02","BUFR/CREX Instrumentation","002152","Satellite instrument used in data processing","(see Note 6)","Flag table","0","0","31","Flag table","0","10","Operational"
237.00,"02","BUFR/CREX Instrumentation","002153","Satellite channel centre frequency",,"Hz","-8","0","26","Hz","-8","8","Operational"
238.00,"02","BUFR/CREX Instrumentation","002154","Satellite channel band width",,"Hz","-8","0","26","Hz","-8","8","Operational"
239.00,"02","BUFR/CREX Instrumentation","002155","Satellite channel wavelength",,"m","9","0","16","m","9","5","Operational"
240.00,"02","BUFR/CREX Instrumentation","002156","Percentage of valid KU ocean retracker measurements",,"%","0","0","7","%","0","3","Operational"
241.00,"02","BUFR/CREX Instrumentation","002157","Percentage of valid S ocean retracker measurements",,"%","0","0","7","%","0","3","Operational"
242.00,"02","BUFR/CREX Instrumentation","002158","RA-2 instrument",,"Flag table","0","0","9","Flag table","0","3","Operational"
243.00,"02","BUFR/CREX Instrumentation","002159","MWR instrument",,"Flag table","0","0","8","Flag table","0","3","Operational"
244.00,"02","BUFR/CREX Instrumentation","002160","Wave length of the radar",,"Code table","0","0","4","Code table","0","2","Operational"
245.00,"02","BUFR/CREX Instrumentation","002163","Height assignment method",,"Code table","0","0","4","Code table","0","2","Operational"
246.00,"02","BUFR/CREX Instrumentation","002164","Tracer correlation method",,"Code table","0","0","3","Code table","0","1","Operational"
247.00,"02","BUFR/CREX Instrumentation","002165","Radiance type flags",,"Flag table","0","0","15","Flag table","0","5","Operational"
248.00,"02","BUFR/CREX Instrumentation","002166","Radiance type",,"Code table","0","0","4","Code table","0","2","Operational"
249.00,"02","BUFR/CREX Instrumentation","002167","Radiance computational method",,"Code table","0","0","4","Code table","0","2","Operational"
250.00,"02","BUFR/CREX Instrumentation","002168","Hydrostatic pressure of lower end of cable (thermistor string)",,"Pa","-3","0","16","kPa","0","5","Operational"
251.00,"02","BUFR/CREX Instrumentation","002169","Anemometer type",,"Code table","0","0","4","Code table","0","2","Operational"
252.00,"02","BUFR/CREX Instrumentation","002170","Aircraft humidity sensors",,"Code table","0","0","6","Code table","0","2","Operational"
253.00,"02","BUFR/CREX Instrumentation","002171","Instrument serial number for water temperature profile measurement",,"CCITT IA5","0","0","64","Character","0","8","Operational"
254.00,"02","BUFR/CREX Instrumentation","002172","Product type for retrieved atmospheric gases",,"Code table","0","0","8","Code table","0","3","Operational"
255.00,"02","BUFR/CREX Instrumentation","002173","Square of the off-nadir angle","(see Note 7)","deg2","4","0","10","deg2","4","4","Operational"
256.00,"02","BUFR/CREX Instrumentation","002174","Mean across track pixel number",,"Numeric","0","0","9","Numeric","0","3","Operational"
257.00,"02","BUFR/CREX Instrumentation","002175","Method of precipitation measurement",,"Code table","0","0","4","Code table","0","2","Operational"
258.00,"02","BUFR/CREX Instrumentation","002176","Method of state of ground measurement",,"Code table","0","0","4","Code table","0","2","Operational"
259.00,"02","BUFR/CREX Instrumentation","002177","Method of snow depth measurement",,"Code table","0","0","4","Code table","0","2","Operational"
260.00,"02","BUFR/CREX Instrumentation","002178","Method of liquid content measurement of precipitation",,"Code table","0","0","4","Code table","0","2","Operational"
261.00,"02","BUFR/CREX Instrumentation","002179","Type of sky condition algorithm",,"Code table","0","0","4","Code table","0","2","Operational"
262.00,"02","BUFR/CREX Instrumentation","002180","Main present weather detecting system",,"Code table","0","0","4","Code table","0","2","Operational"
263.00,"02","BUFR/CREX Instrumentation","002181","Supplementary present weather sensor",,"Flag table","0","0","21","Flag table","0","7","Operational"
264.00,"02","BUFR/CREX Instrumentation","002182","Visibility measurement system",,"Code table","0","0","4","Code table","0","2","Operational"
265.00,"02","BUFR/CREX Instrumentation","002183","Cloud detection system",,"Code table","0","0","4","Code table","0","2","Operational"
266.00,"02","BUFR/CREX Instrumentation","002184","Type of lightning detection sensor",,"Code table","0","0","4","Code table","0","2","Operational"
267.00,"02","BUFR/CREX Instrumentation","002185","Method of evaporation measurement",,"Code table","0","0","4","Code table","0","2","Operational"
268.00,"02","BUFR/CREX Instrumentation","002186","Capability to detect precipitation phenomena",,"Flag table","0","0","30","Flag table","0","10","Operational"
269.00,"02","BUFR/CREX Instrumentation","002187","Capability to detect other weather phenomena",,"Flag table","0","0","18","Flag table","0","6","Operational"
270.00,"02","BUFR/CREX Instrumentation","002188","Capability to detect obscuration",,"Flag table","0","0","21","Flag table","0","7","Operational"
271.00,"02","BUFR/CREX Instrumentation","002189","Capability to discriminate lightning strikes",,"Flag table","0","0","12","Flag table","0","4","Operational"
272.00,"02","BUFR/CREX Instrumentation","002190","Lagrangian drifter submergence (% time submerged)",,"%","0","0","7","%","0","3","Operational"
273.00,"02","BUFR/CREX Instrumentation","002191","Geopotential height calculation",,"Code table","0","0","4","Code table","0","2","Operational"
283.00,"03","BUFR/CREX Instrumentation","003010","Method of sea/water current measurement",,"Code table","0","0","4","Code table","0","2","Operational"
284.00,"03","BUFR/CREX Instrumentation","003011","Method of depth calculation",,"Code table","0","0","2","Code table","0","1","Operational"
285.00,"03","BUFR/CREX Instrumentation","003012","Instrument type/sensor for dissolved oxygen measurement",,"Code table","0","0","4","Code table","0","2","Operational"
289.00,"04","BUFR/CREX Location (time)","004001","Year",,"a","0","0","12","a","0","4","Operational"
290.00,"04","BUFR/CREX Location (time)","004002","Month",,"mon","0","0","4","mon","0","2","Operational"
291.00,"04","BUFR/CREX Location (time)","004003","Day",,"d","0","0","6","d","0","2","Operational"
292.00,"04","BUFR/CREX Location (time)","004004","Hour",,"h","0","0","5","h","0","2","Operational"
293.00,"04","BUFR/CREX Location (time)","004005","Minute",,"min","0","0","6","min","0","2","Operational"
294.00,"04","BUFR/CREX Location (time)","004006","Second",,"s","0","0","6","s","0","2","Operational"
295.00,"04","BUFR/CREX Location (time)","004007","Seconds within a minute (microsecond accuracy)",,"s","6","0","26","s","6","8","Operational"
297.00,"04","BUFR/CREX Location (time)","004011","Time increment",,"a","0","-1024","11","a","0","4","Operational"
298.00,"04","BUFR/CREX Location (time)","004012","Time increment",,"mon","0","-1024","11","mon","0","4","Operational"
299.00,"04","BUFR/CREX Location (time)","004013","Time increment",,"d","0","-1024","11","d","0","4","Operational"
300.00,"04","BUFR/CREX Location (time)","004014","Time increment",,"h","0","-1024","11","h","0","4","Operational"
301.00,"04","BUFR/CREX Location (time)","004015","Time increment",,"min","0","-2048","12","min","0","4","Operational"
302.00,"04","BUFR/CREX Location (time)","004016","Time increment",,"s","0","-4096","13","s","0","4","Operational"
303.00,"04","BUFR/CREX Location (time)","004017","Reference time period for accumulated or extreme data",,"min","0","-1440","12","min","0","4","Operational"
304.00,"04","BUFR/CREX Location (time)","004021","Time period or displacement",,"a","0","-1024","11","a","0","4","Operational"
305.00,"04","BUFR/CREX Location (time)","004022","Time period or displacement",,"mon","0","-1024","11","mon","0","4","Operational"
306.00,"04","BUFR/CREX Location (time)","004023","Time period or displacement",,"d","0","-1024","11","d","0","4","Operational"
307.00,"04","BUFR/CREX Location (time)","004024","Time period or displacement",,"h","0","-2048","12","h","0","4","Operational"
308.00,"04","BUFR/CREX Location (time)","004025","Time period or displacement",,"min","0","-2048","12","min","0","4","Operational"
309.00,"04","BUFR/CREX Location (time)","004026","Time period or displacement",,"s","0","-4096","13","s","0","4","Operational"
310.00,"04","BUFR/CREX Location (time)","004031","Duration of time relating to following value",,"h","0","0","8","h","0","3","Operational"
311.00,"04","BUFR/CREX Location (time)","004032","Duration of time relating to following value",,"min","0","0","6","min","0","2","Operational"
312.00,"04","BUFR/CREX Location (time)","004041","Time difference, UTC - LMT","(see Note 6)","min","0","-1440","12","min","0","4","Operational"
313.00,"04","BUFR/CREX Location (time)","004043","Day of the year",,"d","0","0","9","d","0","3","Operational"
314.00,"04","BUFR/CREX Location (time)","004051","Principal time of daily reading of maximum temperature",,"h","0","0","5","h","0","2","Operational"
315.00,"04","BUFR/CREX Location (time)","004052","Principal time of daily reading of minimum temperature",,"h","0","0","5","h","0","2","Operational"
316.00,"04","BUFR/CREX Location (time)","004053","Number of days with precipitation equal to or more than 1 mm",,"Numeric","0","0"," 6","Numeric","0","2","Operational"
317.00,"04","BUFR/CREX Location (time)","004059","Times of observation used to compute the reported mean values",,"Flag table","0","0","6","Flag table","0","2","Operational"
318.00,"04","BUFR/CREX Location (time)","004065","Short time increment",,"min","0","-128","8","min","0","2","Operational"
319.00,"04","BUFR/CREX Location (time)","004066","Short time increment",,"s","0","-128","8","s","0","2","Operational"
320.00,"04","BUFR/CREX Location (time)","004073","Short time period or displacement",,"d","0","-128","8","d","0","2","Operational"
321.00,"04","BUFR/CREX Location (time)","004074","Short time period or displacement",,"h","0","-128","8","h","0","2","Operational"
322.00,"04","BUFR/CREX Location (time)","004075","Short time period or displacement",,"min","0","-128","8","min","0","2","Operational"
323.00,"04","BUFR/CREX Location (time)","004080","Averaging period for following value",,"Code table","0","0","4","Code table","0","2","Operational"
324.00,"04","BUFR/CREX Location (time)","004086","Long time period or displacement",,"s","0","-8192","15","s","0","5","Operational"
325.00,"05","BUFR/CREX Location (horizontal - 1)","005001","Latitude (high accuracy)",,"deg","5","-9000000","25","deg","5","7","Operational"
326.00,"05","BUFR/CREX Location (horizontal - 1)","005002","Latitude (coarse accuracy)",,"deg","2","-9000","15","deg","2","4","Operational"
327.00,"05","BUFR/CREX Location (horizontal - 1)","005011","Latitude increment (high accuracy)",,"deg","5","-9000000","25","deg","5","7","Operational"
328.00,"05","BUFR/CREX Location (horizontal - 1)","005012","Latitude increment (coarse accuracy)",,"deg","2","-9000","15","deg","2","4","Operational"
329.00,"05","BUFR/CREX Location (horizontal - 1)","005015","Latitude displacement (high accuracy)",,"deg","5","-9000000","25","deg","5","7","Operational"
330.00,"05","BUFR/CREX Location (horizontal - 1)","005016","Latitude displacement (coarse accuracy)",,"deg","2","-9000","15","deg","2","4","Operational"
331.00,"05","BUFR/CREX Location (horizontal - 1)","005021","Bearing or azimuth",,"degree true","2","0","16","degree true","2","5","Operational"
332.00,"05","BUFR/CREX Location (horizontal - 1)","005022","Solar azimuth",,"degree true","2","0","16","degree true","2","5","Operational"
333.00,"05","BUFR/CREX Location (horizontal - 1)","005023","Sun to satellite azimuth difference",,"deg","1","-1800","12","deg","1","4","Operational"
334.00,"05","BUFR/CREX Location (horizontal - 1)","005030","Direction (spectral)",,"deg","0","0","12","deg","0","4","Operational"
335.00,"05","BUFR/CREX Location (horizontal - 1)","005031","Row number",,"Numeric","0","0","12","Numeric","0","4","Operational"
336.00,"05","BUFR/CREX Location (horizontal - 1)","005033","Pixel size on horizontal - 1",,"m","-1","0","16","m","-1","5","Operational"
337.00,"05","BUFR/CREX Location (horizontal - 1)","005034","Along track row number",,"Numeric","0","0","11","Numeric","0","4","Operational"
338.00,"05","BUFR/CREX Location (horizontal - 1)","005035","Maximum size of x-dimension",,"Numeric","0","0","12","Numeric","0","4","Operational"
339.00,"05","BUFR/CREX Location (horizontal - 1)","005036","Ship transect number according to SOOP",,"Numeric","0","0","7","Numeric","0","2","Operational"
340.00,"05","BUFR/CREX Location (horizontal - 1)","005040","Orbit number",,"Numeric","0","0","24","Numeric","0","8","Operational"
341.00,"05","BUFR/CREX Location (horizontal - 1)","005041","Scan line number",,"Numeric","0","0","8","Numeric","0","3","Operational"
342.00,"05","BUFR/CREX Location (horizontal - 1)","005042","Channel number",,"Numeric","0","0","6","Numeric","0","2","Operational"
343.00,"05","BUFR/CREX Location (horizontal - 1)","005043","Field of view number",,"Numeric","0","0","8","Numeric","0","3","Operational"
344.00,"05","BUFR/CREX Location (horizontal - 1)","005044","Satellite cycle number",,"Numeric","0","0","11","Numeric","0","4","Operational"
345.00,"05","BUFR/CREX Location (horizontal - 1)","005045","Field of regard number",,"Numeric","0","0","8","Numeric","0","3","Operational"
346.00,"05","BUFR/CREX Location (horizontal - 1)","005052","Channel number increment",,"Numeric","0","0","5","Numeric","0","2","Operational"
347.00,"05","BUFR/CREX Location (horizontal - 1)","005053","Field of view number increment",,"Numeric","0","0","5","Numeric","0","2","Operational"
348.00,"05","BUFR/CREX Location (horizontal - 1)","005060","Y angular position from centre of gravity",,"deg","6","-8000000","24","deg","6","8","Operational"
349.00,"05","BUFR/CREX Location (horizontal - 1)","005061","Z angular position from centre of gravity",,"deg","6","-8000000","24","deg","6","8","Operational"
351.00,"06","BUFR/CREX Location (horizontal - 2)","006001","Longitude (high accuracy)",,"deg","5","-18000000","26","deg","5","8","Operational"
352.00,"06","BUFR/CREX Location (horizontal - 2)","006002","Longitude (coarse accuracy)",,"deg","2","-18000","16","deg","2","5","Operational"
353.00,"06","BUFR/CREX Location (horizontal - 2)","006011","Longitude increment (high accuracy)",,"deg","5","-18000000","26","deg","5","8","Operational"
354.00,"06","BUFR/CREX Location (horizontal - 2)","006012","Longitude increment (coarse accuracy)",,"deg","2","-18000","16","deg","2","5","Operational"
355.00,"06","BUFR/CREX Location (horizontal - 2)","006015","Longitude displacement (high accuracy)",,"deg","5","-18000000","26","deg","5","8","Operational"
356.00,"06","BUFR/CREX Location (horizontal - 2)","006016","Longitude displacement (coarse accuracy)",,"deg","2","-18000","16","deg","2","5","Operational"
357.00,"06","BUFR/CREX Location (horizontal - 2)","006021","Distance",,"m","-1","0","13","m","-1","4","Operational"
358.00,"06","BUFR/CREX Location (horizontal - 2)","006029","Wave number",,"/m","1","0","22","/m","1","7","Operational"
359.00,"06","BUFR/CREX Location (horizontal - 2)","006030","Wave number (spectral)",,"rad/m","5","0","13","rad/m","5","4","Operational"
360.00,"06","BUFR/CREX Location (horizontal - 2)","006031","Column number",,"Numeric","0","0","12","Numeric","0","4","Operational"
361.00,"06","BUFR/CREX Location (horizontal - 2)","006033","Pixel size on horizontal - 2",,"m","-1","0","16","m","-1","5","Operational"
362.00,"06","BUFR/CREX Location (horizontal - 2)","006034","Cross-track cell number",,"Numeric","0","0","7","Numeric","0","3","Operational"
363.00,"06","BUFR/CREX Location (horizontal - 2)","006035","Maximum size of y-dimension",,"Numeric","0","0","12","Numeric","0","4","Operational"
364.00,"06","BUFR/CREX Location (horizontal - 2)","006040","Radius of confidence",,"m","0","0","13","m","0","4","Operational"
365.00,"07","BUFR/CREX Location (vertical)","007001","Height of station","(see Note 1)","m","0","-400","15","m","0","5","Operational"
366.00,"07","BUFR/CREX Location (vertical)","007002","Height or altitude",,"m","-1","-40","16","m","-1","5","Operational"
367.00,"07","BUFR/CREX Location (vertical)","007003","Geopotential",,"m2 s-2","-1","-400","17","m2 s-2","-1","6","Operational"
368.00,"07","BUFR/CREX Location (vertical)","007004","Pressure",,"Pa","-1","0","14","Pa","-1","5","Operational"
369.00,"07","BUFR/CREX Location (vertical)","007005","Height increment",,"m","0","-400","12","m","0","4","Operational"
370.00,"07","BUFR/CREX Location (vertical)","007006","Height above station",,"m","0","0","15","m","0","5","Operational"
371.00,"07","BUFR/CREX Location (vertical)","007007","Height",,"m","0","-1000","17","m","0","6","Operational"
372.00,"07","BUFR/CREX Location (vertical)","007008","Geopotential",,"m2 s-2","0","-10000","20","m2 s-2","0","7","Operational"
373.00,"07","BUFR/CREX Location (vertical)","007009","Geopotential height",,"gpm","0","-1000","17","gpm","0","5","Operational"
374.00,"07","BUFR/CREX Location (vertical)","007010","Flight level",,"m","0","-1024","16","ft","-1","5","Operational"
376.00,"07","BUFR/CREX Location (vertical)","007012","Grid point altitude",,"m","2","-50000","20","m","2","7","Operational"
377.00,"07","BUFR/CREX Location (vertical)","007021","Elevation","(see Note 2)","deg","2","-9000","15","deg","2","5","Operational"
378.00,"07","BUFR/CREX Location (vertical)","007022","Solar elevation",,"deg","2","-9000","15","deg","2","5","Operational"
379.00,"07","BUFR/CREX Location (vertical)","007024","Satellite zenith angle",,"deg","2","-9000","15","deg","2","5","Operational"
380.00,"07","BUFR/CREX Location (vertical)","007025","Solar zenith angle",,"deg","2","-9000","15","deg","2","5","Operational"
381.00,"07","BUFR/CREX Location (vertical)","007026","Satellite zenith angle",,"deg","4","-900000","21","deg","4","7","Operational"
382.00,"07","BUFR/CREX Location (vertical)","007030","Height of station ground above mean sea level","(see Note 3)","m","1","-4000","17","m","1","5","Operational"
383.00,"07","BUFR/CREX Location (vertical)","007031","Height of barometer above mean sea level","(see Note 4)","m","1","-4000","17","m","1","5","Operational"
384.00,"07","BUFR/CREX Location (vertical)","007032","Height of sensor above local ground (or deck of marine platform)","(see Note 5)","m","2","0","16","m","2","5","Operational"
385.00,"07","BUFR/CREX Location (vertical)","007033","Height of sensor above water surface","(see Note 6)","m","1","0","12","m","1","4","Operational"
386.00,"07","BUFR/CREX Location (vertical)","007035","Maximum size of z-dimension",,"Numeric","0","0","12","Numeric","0","4","Operational"
387.00,"07","BUFR/CREX Location (vertical)","007036","Level index of z",,"Numeric","0","0","12","Numeric","0","4","Operational"
388.00,"07","BUFR/CREX Location (vertical)","007040","Impact parameter","(see Note 7)","m","1","62000000","22","m","1","8","Operational"
389.00,"07","BUFR/CREX Location (vertical)","007061","Depth below land surface",,"m","2","0","14","m","2","5","Operational"
390.00,"07","BUFR/CREX Location (vertical)","007062","Depth below sea/water surface",,"m","1","0","17","m","1","6","Operational"
391.00,"07","BUFR/CREX Location (vertical)","007063","Depth below sea/water surface (cm)",,"m","2","0","20","m","2","7","Operational"
392.00,"07","BUFR/CREX Location (vertical)","007064","Representative height of sensor above station","(see Note 8)","m","0","0","4","m","0","2","Operational"
393.00,"07","BUFR/CREX Location (vertical)","007065","Water pressure",,"Pa","-3","0","17","Pa","-3","6","Operational"
394.00,"07","BUFR/CREX Location (vertical)","007070","Drogue depth",,"m","0","0","10","m","0","4","Operational"
395.00,"08","BUFR/CREX Significance qualifiers","008001","Vertical sounding significance",,"Flag table","0","0","7","Flag table","0","3","Operational"
396.00,"08","BUFR/CREX Significance qualifiers","008002","Vertical significance (surface observations)",,"Code table","0","0","6","Code table","0","2","Operational"
397.00,"08","BUFR/CREX Significance qualifiers","008003","Vertical significance (satellite observations)",,"Code table","0","0","6","Code table","0","2","Operational"
398.00,"08","BUFR/CREX Significance qualifiers","008004","Phase of aircraft flight",,"Code table","0","0","3","Code table","0","1","Operational"
399.00,"08","BUFR/CREX Significance qualifiers","008005","Meteorological attribute significance",,"Code table","0","0","4","Code table","0","2","Operational"
400.00,"08","BUFR/CREX Significance qualifiers","008006","Ozone vertical sounding significance",,"Flag table","0","0","9","Flag table","0","3","Operational"
401.00,"08","BUFR/CREX Significance qualifiers","008007","Dimensional significance",,"Code table","0","0","4","Code table","0","2","Operational"
402.00,"08","BUFR/CREX Significance qualifiers","008008","Radiation vertical sounding significance",,"Flag table","0","0","9","Flag table","0","3","Operational"
403.00,"08","BUFR/CREX Significance qualifiers","008009","Detailed phase of flight",,"Code table","0","0","4","Code table","0","2","Operational"
404.00,"08","BUFR/CREX Significance qualifiers","008010","Surface qualifier (for temperature data)",,"Code table","0","0","5","Code table","0","2","Operational"
405.00,"08","BUFR/CREX Significance qualifiers","008011","Meteorological feature",,"Code table","0","0","6","Code table","0","2","Operational"
406.00,"08","BUFR/CREX Significance qualifiers","008012","Land/sea qualifier",,"Code table","0","0","2","Code table","0","1","Operational"
407.00,"08","BUFR/CREX Significance qualifiers","008013","Day/night qualifier",,"Code table","0","0","2","Code table","0","1","Operational"
408.00,"08","BUFR/CREX Significance qualifiers","008014","Qualifier for runway visual range",,"Code table","0","0","4","Code table","0","2","Operational"
409.00,"08","BUFR/CREX Significance qualifiers","008015","Significant qualifier for sensor",,"Code table","0","0","3","Code table","0","1","Operational"
410.00,"08","BUFR/CREX Significance qualifiers","008016","Change qualifier of a trend-type forecast or an aerodrome forecast",,"Code table","0","0","3","Code table","0","1","Operational"
411.00,"08","BUFR/CREX Significance qualifiers","008017","Qualifier of the time when the forecast change is expected",,"Code table","0","0","2","Code table","0","1","Operational"
412.00,"08","BUFR/CREX Significance qualifiers","008018","SEAWINDS land/ice surface type",,"Flag table","0","0","17","Flag table","0","6","Operational"
413.00,"08","BUFR/CREX Significance qualifiers","008019","Qualifier for following centre identifier",,"Code table","0","0","4","Code table","0","2","Operational"
414.00,"08","BUFR/CREX Significance qualifiers","008020","Total number of missing entities (with respect to accumulation or average)",,"Numeric","0","0","16","Numeric","0","5","Operational"
415.00,"08","BUFR/CREX Significance qualifiers","008021","Time significance",,"Code table","0","0","5","Code table","0","2","Operational"
416.00,"08","BUFR/CREX Significance qualifiers","008022","Total number (with respect to accumulation or average)",,"Numeric","0","0","16","Numeric","0","5","Operational"
417.00,"08","BUFR/CREX Significance qualifiers","008023","First-order statistics",,"Code table","0","0","6","Code table","0","2","Operational"
418.00,"08","BUFR/CREX Significance qualifiers","008024","Difference statistics",,"Code table","0","0","6","Code table","0","2","Operational"
419.00,"08","BUFR/CREX Significance qualifiers","008025","Time difference qualifier","(see Note 5)","Code table","0","0","4","Code table","0","2","Operational"
420.00,"08","BUFR/CREX Significance qualifiers","008026","Matrix significance",,"Code table","0","0","6","Code table","0","2","Operational"
422.00,"08","BUFR/CREX Significance qualifiers","008029","Surface type",,"Code table","0","0","8","Code table","0","3","Operational"
423.00,"08","BUFR/CREX Significance qualifiers","008030","Manual on Codes (Volume I.1, Section C) Code table from which data are derived",,"Numeric","0","0","13","Numeric","0","4","Operational"
424.00,"08","BUFR/CREX Significance qualifiers","008031","Data category - CREX table A",,"Numeric","0","0","8","Numeric","0","3","Operational"
425.00,"08","BUFR/CREX Significance qualifiers","008032","Status of operation",,"Code table","0","0","4","Code table","0","2","Operational"
426.00,"08","BUFR/CREX Significance qualifiers","008033","Method of derivation of percentage confidence","(see Note 6)","Code table","0","0","7","Code table","0","3","Operational"
428.00,"08","BUFR/CREX Significance qualifiers","008035","Type of monitoring exercise",,"Code table","0","0","3","Code table","0","1","Operational"
429.00,"08","BUFR/CREX Significance qualifiers","008036","Type of centre or station performing monitoring",,"Code table","0","0","3","Code table","0","1","Operational"
430.00,"08","BUFR/CREX Significance qualifiers","008039","Time significance (Aviation forecast)",,"Code table","0","0","6","Code table","0","2","Operational"
431.00,"08","BUFR/CREX Significance qualifiers","008040","Flight level significance",,"Code table","0","0","6","Code table","0","2","Operational"
432.00,"08","BUFR/CREX Significance qualifiers","008041","Data significance",,"Code table","0","0","5","Code table","0","2","Operational"
433.00,"08","BUFR/CREX Significance qualifiers","008042","Extended vertical sounding significance",,"Flag table","0","0","18","Flag table","0","6","Operational"
434.00,"08","BUFR/CREX Significance qualifiers","008043","Atmospheric chemical or physical constituent type",,"Code table","0","0","8","Code table","0","3","Operational"
435.00,"08","BUFR/CREX Significance qualifiers","008044","CAS registry number",,"CCITT IA5","0","0","88","Character","0","11","Operational"
437.00,"08","BUFR/CREX Significance qualifiers","008046","Atmospheric chemical or physical constituent type",,"Common Code table C-14","0","0","16","Common Code table C-14","0","5","Operational"
438.00,"08","BUFR/CREX Significance qualifiers","008049","Number of observations",,"Numeric","0","0","8","Numeric","0","3","Operational"
439.00,"08","BUFR/CREX Significance qualifiers","008050","Qualifier for number of missing values in calculation of statistic",,"Code table","0","0","4","Code table","0","2","Operational"
440.00,"08","BUFR/CREX Significance qualifiers","008051","Qualifier for number of missing values in calculation of statistic",,"Code table","0","0","3","Code table","0","1","Operational"
441.00,"08","BUFR/CREX Significance qualifiers","008052","Condition for which number of days of occurrence follows",,"Code table","0","0","5","Code table","0","2","Operational"
442.00,"08","BUFR/CREX Significance qualifiers","008053","Day of occurrence qualifier",,"Code table","0","0","2","Code table","0","1","Operational"
443.00,"08","BUFR/CREX Significance qualifiers","008054","Qualifier for wind speed or wind gusts",,"Code table","0","0","3","Code table","0","1","Operational"
444.00,"08","BUFR/CREX Significance qualifiers","008060","Sample scanning mode significance",,"Code table","0","0","4","Code table","0","2","Operational"
445.00,"08","BUFR/CREX Significance qualifiers","008065","Sun-glint indicator",,"Code table","0","0","2","Code table","0","1","Operational"
446.00,"08","BUFR/CREX Significance qualifiers","008066","Semi-transparency indicator",,"Code table","0","0","2","Code table","0","1","Operational"
447.00,"08","BUFR/CREX Significance qualifiers","008070","TOVS/ATOVS product qualifier",,"Code table","0","0","4","Code table","0","2","Operational"
448.00,"08","BUFR/CREX Significance qualifiers","008072","Pixel(s) type",,"Code table","0","0","3","Code table","0","1","Operational"
449.00,"08","BUFR/CREX Significance qualifiers","008074","Altimeter echo type",,"Code table","0","0","2","Code table","0","1","Operational"
450.00,"08","BUFR/CREX Significance qualifiers","008075","Ascending/descending orbit qualifier",,"Code table","0","0","2","Code table","0","1","Operational"
451.00,"08","BUFR/CREX Significance qualifiers","008076","Type of band",,"Code table","0","0","6","Code table","0","2","Operational"
452.00,"08","BUFR/CREX Significance qualifiers","008077","Radiometer sensed surface type",,"Code table","0","0","7","Code table","0","3","Operational"
453.00,"08","BUFR/CREX Significance qualifiers","008079","Product status",,"Code table","0","0","4","Code table","0","2","Operational"
454.00,"08","BUFR/CREX Significance qualifiers","008080","Qualifier for GTSPP quality flag",,"Code table","0","0","6","Code table","0","2","Operational"
455.00,"08","BUFR/CREX Significance qualifiers","008081","Type of equipment",,"Code table","0","0","6","Code table","0","2","Operational"
456.00,"08","BUFR/CREX Significance qualifiers","008082","Modification of sensor height to another value",,"Code table","0","0","3","Code table","0","1","Operational"
457.00,"08","BUFR/CREX Significance qualifiers","008083","Nominal value indicator",,"Flag table","0","0","15","Flag table","0","5","Operational"
458.00,"08","BUFR/CREX Significance qualifiers","008085","Beam identifier",,"Code table","0","0","3","Code table","0","1","Operational"
459.00,"08","BUFR/CREX Significance qualifiers","008086","Vertical significance for NWP",,"Flag table","0","0","12","Flag table","0","4","Operational"
460.00,"08","BUFR/CREX Significance qualifiers","008087","Corner position of observation",,"Code table","0","0","3","Code table","0","1","Operational"
461.00,"08","BUFR/CREX Significance qualifiers","008090","Decimal scale of following significands",,"Numeric","0","-127","8","Numeric","0","3","Operational"
462.00,"10","BUFR/CREX Non-coordinate location (vertical)","010001","Height of land surface",,"m","0","-400","15","m","0","5","Operational"
463.00,"10","BUFR/CREX Non-coordinate location (vertical)","010002","Height",,"m","-1","-40","16","m","-1","5","Operational"
464.00,"10","BUFR/CREX Non-coordinate location (vertical)","010003","Geopotential",,"m2 s-2","-1","-400","17","m2 s-2","-1","6","Operational"
465.00,"10","BUFR/CREX Non-coordinate location (vertical)","010004","Pressure",,"Pa","-1","0","14","Pa","-1","5","Operational"
466.00,"10","BUFR/CREX Non-coordinate location (vertical)","010007","Height",,"m","0","-1000","17","m","0","6","Operational"
467.00,"10","BUFR/CREX Non-coordinate location (vertical)","010008","Geopotential",,"m2 s-2","0","-10000","20","m2 s-2","0","7","Operational"
468.00,"10","BUFR/CREX Non-coordinate location (vertical)","010009","Geopotential height",,"gpm","0","-1000","17","gpm","0","5","Operational"
469.00,"10","BUFR/CREX Non-coordinate location (vertical)","010010","Minimum pressure reduced to mean sea level",,"Pa","-1","0","14","Pa","-1","5","Operational"
470.00,"10","BUFR/CREX Non-coordinate location (vertical)","010011","Maximum pressure reduced to mean sea level",,"Pa","-1","0","14","Pa","-1","5","Operational"
473.00,"10","BUFR/CREX Non-coordinate location (vertical)","010031","In direction of the North Pole, distance from the Earth's centre","(see Notes 2 and 3)","m","2","-1073741824","31","m","2","10","Operational"
474.00,"10","BUFR/CREX Non-coordinate location (vertical)","010032","Satellite distance to Earth's centre",,"m","1","0","27","m","2","9","Operational"
475.00,"10","BUFR/CREX Non-coordinate location (vertical)","010033","Altitude (platform to ellipsoid)",,"m","1","0","27","m","2","9","Operational"
476.00,"10","BUFR/CREX Non-coordinate location (vertical)","010034","Earth's radius",,"m","1","0","27","m","2","9","Operational"
477.00,"10","BUFR/CREX Non-coordinate location (vertical)","010035","Earth's local radius of curvature",,"m","1","62000000","22","m","1","8","Operational"
478.00,"10","BUFR/CREX Non-coordinate location (vertical)","010036","Geoid undulation","(see Note 4)","m","2","-15000","15","m","2","6","Operational"
479.00,"10","BUFR/CREX Non-coordinate location (vertical)","010040","Number of retrieved layers",,"Numeric","0","0","10","Numeric","0","4","Operational"
480.00,"10","BUFR/CREX Non-coordinate location (vertical)","010050","Standard deviation altitude",,"m","2","0","16","m","2","5","Operational"
481.00,"10","BUFR/CREX Non-coordinate location (vertical)","010051","Pressure reduced to mean sea level",,"Pa","-1","0","14","Pa","-1","5","Operational"
482.00,"10","BUFR/CREX Non-coordinate location (vertical)","010052","Altimeter setting (QNH)",,"Pa","-1","0","14","Pa","-1","5","Operational"
483.00,"10","BUFR/CREX Non-coordinate location (vertical)","010053","Global navigation satellite system altitude",,"m","0","-1000","17","m","0","5","Operational"
484.00,"10","BUFR/CREX Non-coordinate location (vertical)","010060","Pressure change",,"Pa","-1","-1024","11","Pa","-1","4","Operational"
485.00,"10","BUFR/CREX Non-coordinate location (vertical)","010061","3-hour pressure change",,"Pa","-1","-500","10","Pa","-1","4","Operational"
486.00,"10","BUFR/CREX Non-coordinate location (vertical)","010062","24-hour pressure change",,"Pa","-1","-1000","11","Pa","-1","4","Operational"
487.00,"10","BUFR/CREX Non-coordinate location (vertical)","010063","Characteristic of pressure tendency",,"Code table","0","0","4","Code table","0","2","Operational"
488.00,"10","BUFR/CREX Non-coordinate location (vertical)","010064","SIGMET cruising level",,"Code table","0","0","3","Code table","0","1","Operational"
489.00,"10","BUFR/CREX Non-coordinate location (vertical)","010070","Indicated aircraft altitude",,"m","0","-400","16","m","0","5","Operational"
491.00,"10","BUFR/CREX Non-coordinate location (vertical)","010079","Off-nadir angle of the satellite from platform data",,"deg","4","0","16","deg","4","5","Operational"
492.00,"10","BUFR/CREX Non-coordinate location (vertical)","010080","Viewing zenith angle",,"deg","2","-9000","15","deg","2","5","Operational"
493.00,"10","BUFR/CREX Non-coordinate location (vertical)","010081","Altitude of COG above reference ellipsoid",,"m","3","0","31","m","3","10","Operational"
494.00,"10","BUFR/CREX Non-coordinate location (vertical)","010082","Instantaneous altitude rate",,"m/s","3","-65536","17","m/s","3","6","Operational"
495.00,"10","BUFR/CREX Non-coordinate location (vertical)","010083","Squared off-nadir angle of the satellite from platform data",,"deg2","2","0","16","deg2","2","5","Operational"
496.00,"10","BUFR/CREX Non-coordinate location (vertical)","010084","Squared off-nadir angle of the satellite from waveform data",,"deg2","2","0","16","deg2","2","5","Operational"
497.00,"10","BUFR/CREX Non-coordinate location (vertical)","010085","Mean sea-surface height",,"m","3","-131072","18","m","3","6","Operational"
498.00,"10","BUFR/CREX Non-coordinate location (vertical)","010086","Geoid's height",,"m","3","-131072","18","m","3","6","Operational"
499.00,"10","BUFR/CREX Non-coordinate location (vertical)","010087","Ocean depth/land elevation",,"m","1","-131072","18","m","1","6","Operational"
500.00,"10","BUFR/CREX Non-coordinate location (vertical)","010088","Total geocentric ocean tide height (solution 1)",,"m","3","-32768","16","m","3","5","Operational"
501.00,"10","BUFR/CREX Non-coordinate location (vertical)","010089","Total geocentric ocean tide height (solution 2)",,"m","3","-32768","16","m","3","5","Operational"
502.00,"10","BUFR/CREX Non-coordinate location (vertical)","010090","Long period tide height",,"m","3","-32768","16","m","3","5","Operational"
503.00,"10","BUFR/CREX Non-coordinate location (vertical)","010091","Tidal loading height",,"m","3","-32768","16","m","3","5","Operational"
504.00,"10","BUFR/CREX Non-coordinate location (vertical)","010092","Solid Earth tide height",,"m","3","-32768","16","m","3","5","Operational"
505.00,"10","BUFR/CREX Non-coordinate location (vertical)","010093","Geocentric pole tide height",,"m","3","-32768","16","m","3","5","Operational"
506.00,"10","BUFR/CREX Non-coordinate location (vertical)","010095","Height of atmosphere used",,"m","0","0","16","m","0","5","Operational"
507.00,"10","BUFR/CREX Non-coordinate location (vertical)","010096","Mean dynamic topography",,"m","3","-131072","18","m","3","6","Operational"
508.00,"10","BUFR/CREX Non-coordinate location (vertical)","010097","Mean sea-surface height from altimeter only",,"m","3","-131072","18","m","3","6","Operational"
509.00,"10","BUFR/CREX Non-coordinate location (vertical)","010098","Loading tide height geocentric ocean tide solution 1",,"m","4","-2000","12","m","4","4","Operational"
510.00,"10","BUFR/CREX Non-coordinate location (vertical)","010099","Loading tide height geocentric ocean tide solution 2",,"m","4","-2000","12","m","4","4","Operational"
511.00,"10","BUFR/CREX Non-coordinate location (vertical)","010100","Non-equilibrium long period tide height",,"m","4","-2000","12","m","4","4","Operational"
512.00,"10","BUFR/CREX Non-coordinate location (vertical)","010101","Squared off-nadir angle of the satellite from waveform data",,"deg2","2","-32768","16","deg2","2","5","Operational"
513.00,"10","BUFR/CREX Non-coordinate location (vertical)","010102","Sea-surface height anomaly",,"m","3","-32768","16","m","3","5","Operational"
514.00,"11","BUFR/CREX Wind and turbulence","011001","Wind direction",,"degree true","0","0","9","degree true","0","3","Operational"
515.00,"11","BUFR/CREX Wind and turbulence","011002","Wind speed",,"m/s","1","0","12","m/s","1","4","Operational"
516.00,"11","BUFR/CREX Wind and turbulence","011003","u-component",,"m/s","1","-4096","13","m/s","1","4","Operational"
517.00,"11","BUFR/CREX Wind and turbulence","011004","v-component",,"m/s","1","-4096","13","m/s","1","4","Operational"
518.00,"11","BUFR/CREX Wind and turbulence","011005","w-component",,"Pa/s","1","-512","10","Pa/s","1","4","Operational"
519.00,"11","BUFR/CREX Wind and turbulence","011006","w-component",,"m/s","2","-4096","13","m/s","2","4","Operational"
522.00,"11","BUFR/CREX Wind and turbulence","011010","Wind direction associated with wind speed which follows",,"degree true","0","0","9","degree true","0","3","Operational"
523.00,"11","BUFR/CREX Wind and turbulence","011011","Wind direction at 10 m",,"degree true","0","0","9","degree true","0","3","Operational"
524.00,"11","BUFR/CREX Wind and turbulence","011012","Wind speed at 10 m",,"m/s","1","0","12","m/s","1","4","Operational"
525.00,"11","BUFR/CREX Wind and turbulence","011013","Wind direction at 5 m",,"degree true","0","0","9","degree true","0","3","Operational"
526.00,"11","BUFR/CREX Wind and turbulence","011014","Wind speed at 5 m",,"m/s","1","0","12","m/s","1","4","Operational"
527.00,"11","BUFR/CREX Wind and turbulence","011016","Extreme counterclockwise wind direction of a variable wind",,"degree true","0","0","9","degree true","0","3","Operational"
528.00,"11","BUFR/CREX Wind and turbulence","011017","Extreme clockwise wind direction of a variable wind",,"degree true","0","0","9","degree true","0","3","Operational"
529.00,"11","BUFR/CREX Wind and turbulence","011019","Steadiness of wind","(see Note 6)","%","0","0","7","%","0","3","Operational"
530.00,"11","BUFR/CREX Wind and turbulence","011021","Relative vorticity",,"/s","9","-65536","17","/s","9","6","Operational"
531.00,"11","BUFR/CREX Wind and turbulence","011022","Divergence",,"/s","9","-65536","17","/s","9","6","Operational"
532.00,"11","BUFR/CREX Wind and turbulence","011023","Velocity potential",,"m2/s","-2","-65536","17","m2/s","-2","6","Operational"
533.00,"11","BUFR/CREX Wind and turbulence","011030","Extended degree of turbulence",,"Code table","0","0","6","Code table","0","2","Operational"
534.00,"11","BUFR/CREX Wind and turbulence","011031","Degree of turbulence",,"Code table","0","0","4","Code table","0","2","Operational"
535.00,"11","BUFR/CREX Wind and turbulence","011032","Height of base of turbulence",,"m","-1","-40","16","m","-1","5","Operational"
536.00,"11","BUFR/CREX Wind and turbulence","011033","Height of top of turbulence",,"m","-1","-40","16","m","-1","5","Operational"
537.00,"11","BUFR/CREX Wind and turbulence","011034","Vertical gust velocity",,"m/s","1","-1024","11","m/s","1","4","Operational"
538.00,"11","BUFR/CREX Wind and turbulence","011035","Vertical gust acceleration",,"m s-2","2","-8192","14","m s-2","2","5","Operational"
539.00,"11","BUFR/CREX Wind and turbulence","011036","Maximum derived equivalent vertical gust speed",,"m/s","1","0","10","m/s","1","4","Operational"
540.00,"11","BUFR/CREX Wind and turbulence","011037","Turbulence index",,"Code table","0","0","6","Code table","0","2","Operational"
541.00,"11","BUFR/CREX Wind and turbulence","011038","Time of occurrence of peak eddy dissipation rate",,"Code table","0","0","5","Code table","0","2","Operational"
542.00,"11","BUFR/CREX Wind and turbulence","011039","Extended time of occurrence of peak eddy dissipation rate",,"Code table","0","0","6","Code table","0","2","Operational"
543.00,"11","BUFR/CREX Wind and turbulence","011040","Maximum wind speed (mean wind)",,"m/s","1","0","12","m/s","1","4","Operational"
544.00,"11","BUFR/CREX Wind and turbulence","011041","Maximum wind gust speed",,"m/s","1","0","12","m/s","1","4","Operational"
545.00,"11","BUFR/CREX Wind and turbulence","011042","Maximum wind speed (10-minute mean wind)",,"m/s","1","0","12","m/s","1","4","Operational"
546.00,"11","BUFR/CREX Wind and turbulence","011043","Maximum wind gust direction",,"degree true","0","0","9","degree true","0","3","Operational"
547.00,"11","BUFR/CREX Wind and turbulence","011044","Mean wind direction for surface - 1 500 m (5 000 feet)",,"degree true","0","0","9","degree true","0","3","Operational"
548.00,"11","BUFR/CREX Wind and turbulence","011045","Mean wind speed for surface - 1 500 m (5 000 feet)",,"m/s","1","0","12","m/s","1","4","Operational"
549.00,"11","BUFR/CREX Wind and turbulence","011046","Maximum instantaneous wind speed",,"m/s","1","0","12","m/s","1","4","Operational"
550.00,"11","BUFR/CREX Wind and turbulence","011047","Maximum instantaneous wind speed over 10 minutes",,"m/s","1","0","12","m/s","1","4","Operational"
551.00,"11","BUFR/CREX Wind and turbulence","011049","Standard deviation of wind direction",,"degree true","0","0","9","degree true","0","3","Operational"
552.00,"11","BUFR/CREX Wind and turbulence","011050","Standard deviation of horizontal wind speed",,"m/s","1","0","12","m/s","1","4","Operational"
553.00,"11","BUFR/CREX Wind and turbulence","011051","Standard deviation of vertical wind speed",,"m/s","1","0","8","m/s","1","3","Operational"
554.00,"11","BUFR/CREX Wind and turbulence","011052","Formal uncertainty in wind speed",,"m/s","2","0","13","m/s","2","5","Operational"
555.00,"11","BUFR/CREX Wind and turbulence","011053","Formal uncertainty in wind direction",,"degree true","2","0","15","degree true","2","5","Operational"
556.00,"11","BUFR/CREX Wind and turbulence","011054","Mean wind direction for 1 500 - 3 000 m",,"degree true","0","0","9","degree true","0","3","Operational"
557.00,"11","BUFR/CREX Wind and turbulence","011055","Mean wind speed for 1 500 - 3 000 m",,"m/s","1","0","12","m/s","1","4","Operational"
558.00,"11","BUFR/CREX Wind and turbulence","011061","Absolute wind shear in 1 km layer below",,"m/s","1","0","12","m/s","1","4","Operational"
559.00,"11","BUFR/CREX Wind and turbulence","011062","Absolute wind shear in 1 km layer above",,"m/s","1","0","12","m/s","1","4","Operational"
560.00,"11","BUFR/CREX Wind and turbulence","011070","Designator of the runway affected by wind shear (including ALL)",,"CCITT IA5","0","0","32","Character","0","4","Operational"
561.00,"11","BUFR/CREX Wind and turbulence","011071","Turbulent vertical momentum flux",,"m2 s-2","3","-128","14","m2 s-2","3","5","Operational"
562.00,"11","BUFR/CREX Wind and turbulence","011072","Turbulent vertical buoyancy flux",,"K m s-1","3","-128","11","K m s-1","3","4","Operational"
563.00,"11","BUFR/CREX Wind and turbulence","011073","Turbulent kinetic energy",,"m2 s-2","2","-1024","13","m2 s-2","2","4","Operational"
564.00,"11","BUFR/CREX Wind and turbulence","011074","Dissipation energy",,"m2 s-2","2","-1024","10","m2 s-2","2","4","Operational"
565.00,"11","BUFR/CREX Wind and turbulence","011075","Mean turbulence intensity (eddy dissipation rate)",,"m2/3 s-1","2","0","8","m2/3 s-1","2","3","Operational"
566.00,"11","BUFR/CREX Wind and turbulence","011076","Peak turbulence intensity (eddy dissipation rate)",,"m2/3 s-1","2","0","8","m2/3 s-1","2","3","Operational"
567.00,"11","BUFR/CREX Wind and turbulence","011077","Reporting interval or averaging time for eddy dissipation rate",,"s","0","0","12","s","0","4","Operational"
568.00,"11","BUFR/CREX Wind and turbulence","011081","Model wind direction at 10 m",,"degree true","2","0","16","degree true","2","5","Operational"
569.00,"11","BUFR/CREX Wind and turbulence","011082","Model wind speed at 10 m",,"m/s","2","0","14","m/s","2","4","Operational"
570.00,"11","BUFR/CREX Wind and turbulence","011083","Wind speed",,"km/h","0","0","9","km/h","0","3","Operational"
571.00,"11","BUFR/CREX Wind and turbulence","011084","Wind speed",,"kt","0","0","8","kt","0","3","Operational"
572.00,"11","BUFR/CREX Wind and turbulence","011085","Maximum wind gust speed",,"km/h","0","0","9","km/h","0","3","Operational"
573.00,"11","BUFR/CREX Wind and turbulence","011086","Maximum wind gust speed",,"kt","0","0","8","kt","0","3","Operational"
574.00,"11","BUFR/CREX Wind and turbulence","011095","u-component of the model wind vector",,"m/s","1","-4096","13","m/s","1","4","Operational"
575.00,"11","BUFR/CREX Wind and turbulence","011096","v-component of the model wind vector",,"m/s","1","-4096","13","m/s","1","4","Operational"
576.00,"11","BUFR/CREX Wind and turbulence","011097","Wind speed from altimeter",,"m/s","2","0","12","m/s","2","4","Operational"
577.00,"11","BUFR/CREX Wind and turbulence","011098","Wind speed from radiometer",,"m/s","2","0","12","m/s","2","4","Operational"
578.00,"11","BUFR/CREX Wind and turbulence","011100","Aircraft true airspeed",,"m/s","1","0","12","m/s","1","4","Operational"
579.00,"11","BUFR/CREX Wind and turbulence","011101","Aircraft ground speed u-component",,"m/s","1","-4096","13","m/s","1","4","Operational"
580.00,"11","BUFR/CREX Wind and turbulence","011102","Aircraft ground speed v-component",,"m/s","1","-4096","13","m/s","1","4","Operational"
581.00,"11","BUFR/CREX Wind and turbulence","011103","Aircraft ground speed w-component",,"m/s","1","-512","10","m/s","1","3","Operational"
582.00,"11","BUFR/CREX Wind and turbulence","011104","Aircraft true heading",,"degree true","0","0","9","degree true","0","3","Operational"
583.00,"11","BUFR/CREX Wind and turbulence","011105","EDR algorithm version",,"Numeric","0","0","6","Numeric","0","2","Operational"
584.00,"11","BUFR/CREX Wind and turbulence","011106","Running minimum confidence",,"Numeric","1","0","4","Numeric","1","2","Operational"
585.00,"11","BUFR/CREX Wind and turbulence","011107","Maximum number bad inputs",,"Numeric","0","0","5","Numeric","0","2","Operational"
586.00,"11","BUFR/CREX Wind and turbulence","011108","Peak location",,"Numeric","1","0","4","Numeric","1","2","Operational"
587.00,"11","BUFR/CREX Wind and turbulence","011109","Number of good EDR",,"Numeric","0","0","4","Numeric","0","2","Operational"
593.00,"12","BUFR/CREX Temperature","012001","Temperature/air temperature",,"K","1","0","12","C","1","3","Operational"
594.00,"12","BUFR/CREX Temperature","012002","Wet-bulb temperature",,"K","1","0","12","C","1","3","Operational"
595.00,"12","BUFR/CREX Temperature","012003","Dewpoint temperature",,"K","1","0","12","C","1","3","Operational"
596.00,"12","BUFR/CREX Temperature","012004","Air temperature at 2 m",,"K","1","0","12","C","1","3","Operational"
597.00,"12","BUFR/CREX Temperature","012005","Wet-bulb temperature at 2 m",,"K","1","0","12","C","1","3","Operational"
598.00,"12","BUFR/CREX Temperature","012006","Dewpoint temperature at 2 m",,"K","1","0","12","C","1","3","Operational"
599.00,"12","BUFR/CREX Temperature","012007","Virtual temperature",,"K","1","0","12","C","1","3","Operational"
601.00,"12","BUFR/CREX Temperature","012011","Maximum temperature, at height and over period specified",,"K","1","0","12","C","1","3","Operational"
602.00,"12","BUFR/CREX Temperature","012012","Minimum temperature, at height and over period specified",,"K","1","0","12","C","1","3","Operational"
603.00,"12","BUFR/CREX Temperature","012013","Ground minimum temperature, past 12 hours",,"K","1","0","12","C","1","3","Operational"
604.00,"12","BUFR/CREX Temperature","012014","Maximum temperature at 2 m, past 12 hours",,"K","1","0","12","C","1","3","Operational"
605.00,"12","BUFR/CREX Temperature","012015","Minimum temperature at 2 m, past 12 hours",,"K","1","0","12","C","1","3","Operational"
606.00,"12","BUFR/CREX Temperature","012016","Maximum temperature at 2 m, past 24 hours",,"K","1","0","12","C","1","3","Operational"
607.00,"12","BUFR/CREX Temperature","012017","Minimum temperature at 2 m, past 24 hours",,"K","1","0","12","C","1","3","Operational"
608.00,"12","BUFR/CREX Temperature","012021","Maximum temperature at 2 m",,"K","2","0","16","C","2","4","Operational"
609.00,"12","BUFR/CREX Temperature","012022","Minimum temperature at 2 m",,"K","2","0","16","C","2","4","Operational"
610.00,"12","BUFR/CREX Temperature","012023","Temperature",,"C","0","-99","8","C","0","2","Operational"
611.00,"12","BUFR/CREX Temperature","012024","Dewpoint temperature",,"C","0","-99","8","C","0","2","Operational"
612.00,"12","BUFR/CREX Temperature","012030","Soil temperature",,"K","1","0","12","C","1","3","Operational"
613.00,"12","BUFR/CREX Temperature","012049","Temperature change over specified period",,"K","0","-30","6","C","0","2","Operational"
614.00,"12","BUFR/CREX Temperature","012051","Standard deviation temperature",,"K","1","0","10","C","1","3","Operational"
615.00,"12","BUFR/CREX Temperature","012052","Highest daily mean temperature",,"K","1","0","12","C","1","3","Operational"
616.00,"12","BUFR/CREX Temperature","012053","Lowest daily mean temperature",,"K","1","0","12","C","1","3","Operational"
617.00,"12","BUFR/CREX Temperature","012060","AWS enclosure internal temperature",,"K","1","0","12","C","1","3","Operational"
618.00,"12","BUFR/CREX Temperature","012061","Skin temperature",,"K","1","0","12","C","1","3","Operational"
619.00,"12","BUFR/CREX Temperature","012062","Equivalent black body temperature",,"K","1","0","12","C","1","3","Operational"
620.00,"12","BUFR/CREX Temperature","012063","Brightness temperature",,"K","1","0","12","C","1","3","Operational"
621.00,"12","BUFR/CREX Temperature","012064","Instrument temperature",,"K","1","0","12","K","1","4","Operational"
622.00,"12","BUFR/CREX Temperature","012065","Standard deviation brightness temperature",,"K","1","0","12","K","1","4","Operational"
623.00,"12","BUFR/CREX Temperature","012066","Antenna temperature",,"K","2","0","16","C","2","5","Operational"
624.00,"12","BUFR/CREX Temperature","012070","Warm load temperature",,"K","2","0","16","K","2","5","Operational"
625.00,"12","BUFR/CREX Temperature","012071","Coldest cluster temperature",,"K","1","0","12","K","1","4","Operational"
626.00,"12","BUFR/CREX Temperature","012072","Radiance",,"W m-2 sr-1","6","0","31","W m-2 sr-1","6","9","Operational"
627.00,"12","BUFR/CREX Temperature","012075","Spectral radiance",,"W m-3 sr-1","-3","0","16","W m-3 sr-1","-3","5","Operational"
628.00,"12","BUFR/CREX Temperature","012076","Radiance","(see Note 2)","W m-2 sr-1","3","0","16","W m-2 sr-1","3","5","Operational"
629.00,"12","BUFR/CREX Temperature","012080","Brightness temperature real part",,"K","2","-10000","16","K","2","5","Operational"
630.00,"12","BUFR/CREX Temperature","012081","Brightness temperature imaginary part",,"K","2","-10000","16","K","2","5","Operational"
631.00,"12","BUFR/CREX Temperature","012082","Pixel radiometric accuracy",,"K","2","0","12","K","2","4","Operational"
632.00,"12","BUFR/CREX Temperature","012101","Temperature/air temperature",,"K","2","0","16","C","2","4","Operational"
633.00,"12","BUFR/CREX Temperature","012102","Wet-bulb temperature",,"K","2","0","16","C","2","4","Operational"
634.00,"12","BUFR/CREX Temperature","012103","Dewpoint temperature",,"K","2","0","16","C","2","4","Operational"
635.00,"12","BUFR/CREX Temperature","012104","Air temperature at 2 m",,"K","2","0","16","C","2","4","Operational"
636.00,"12","BUFR/CREX Temperature","012105","Web-bulb temperature at 2 m",,"K","2","0","16","C","2","4","Operational"
637.00,"12","BUFR/CREX Temperature","012106","Dewpoint temperature at 2 m",,"K","2","0","16","C","2","4","Operational"
638.00,"12","BUFR/CREX Temperature","012107","Virtual temperature",,"K","2","0","16","C","2","4","Operational"
639.00,"12","BUFR/CREX Temperature","012111","Maximum temperature, at height and over period specified",,"K","2","0","16","C","2","4","Operational"
640.00,"12","BUFR/CREX Temperature","012112","Minimum temperature, at height and over period specified",,"K","2","0","16","C","2","4","Operational"
641.00,"12","BUFR/CREX Temperature","012113","Ground minimum temperature, past 12 hours",,"K","2","0","16","C","2","4","Operational"
642.00,"12","BUFR/CREX Temperature","012114","Maximum temperature at 2 m, past 12 hours",,"K","2","0","16","C","2","4","Operational"
643.00,"12","BUFR/CREX Temperature","012115","Minimum temperature at 2 m, past 12 hours",,"K","2","0","16","C","2","4","Operational"
644.00,"12","BUFR/CREX Temperature","012116","Maximum temperature at 2 m, past 24 hours",,"K","2","0","16","C","2","4","Operational"
645.00,"12","BUFR/CREX Temperature","012117","Minimum temperature at 2 m, past 24 hours",,"K","2","0","16","C","2","4","Operational"
646.00,"12","BUFR/CREX Temperature","012118","Maximum temperature at height specified, past 24 hours",,"K","2","0","16","C","2","4","Operational"
647.00,"12","BUFR/CREX Temperature","012119","Minimum temperature at height specified, past 24 hours",,"K","2","0","16","C","2","4","Operational"
648.00,"12","BUFR/CREX Temperature","012120","Ground temperature",,"K","2","0","16","C","2","4","Operational"
649.00,"12","BUFR/CREX Temperature","012121","Ground minimum temperature",,"K","2","0","16","C","2","4","Operational"
650.00,"12","BUFR/CREX Temperature","012122","Ground minimum temperature of the preceding night",,"K","2","0","16","C","2","4","Operational"
651.00,"12","BUFR/CREX Temperature","012130","Soil temperature",,"K","2","0","16","C","2","4","Operational"
652.00,"12","BUFR/CREX Temperature","012131","Snow temperature",,"K","2","0","16","C","2","4","Operational"
653.00,"12","BUFR/CREX Temperature","012132","Ice surface temperature",,"K","2","0","16","C","2","4","Operational"
656.00,"12","BUFR/CREX Temperature","012151","Standard deviation of daily mean temperature",,"K","2","0","12","C","2","4","Operational"
657.00,"12","BUFR/CREX Temperature","012152","Highest daily mean temperature",,"K","2","0","16","C","2","4","Operational"
658.00,"12","BUFR/CREX Temperature","012153","Lowest daily mean temperature",,"K","2","0","16","C","2","4","Operational"
659.00,"12","BUFR/CREX Temperature","012158","Noise-equivalent delta temperature while viewing cold target",,"K","2","0","12","C","2","4","Operational"
660.00,"12","BUFR/CREX Temperature","012159","Noise-equivalent delta temperature while viewing warm target",,"K","2","0","12","C","2","4","Operational"
661.00,"12","BUFR/CREX Temperature","012161","Skin temperature",,"K","2","0","16","C","2","4","Operational"
662.00,"12","BUFR/CREX Temperature","012162","Equivalent black body temperature",,"K","2","0","16","C","2","4","Operational"
663.00,"12","BUFR/CREX Temperature","012163","Brightness temperature",,"K","2","0","16","C","2","4","Operational"
664.00,"12","BUFR/CREX Temperature","012164","Instrument temperature",,"K","2","0","16","K","2","5","Operational"
665.00,"12","BUFR/CREX Temperature","012165","Direct sun brightness temperature",,"K","0","0","23","K","0","7","Operational"
666.00,"12","BUFR/CREX Temperature","012166","Snapshot accuracy",,"K","1","-4000","13","K","1","4","Operational"
667.00,"12","BUFR/CREX Temperature","012167","Radiometric accuracy (pure polarization)",,"K","1","0","9","K","1","3","Operational"
668.00,"12","BUFR/CREX Temperature","012168","Radiometric accuracy (cross polarization)",,"K","1","0","9","K","1","3","Operational"
669.00,"12","BUFR/CREX Temperature","012171","Coldest cluster temperature",,"K","2","0","16","K","2","5","Operational"
670.00,"12","BUFR/CREX Temperature","012180","Averaged 12 micron BT for all clear pixels at nadir",,"K","2","0","16","K","2","5","Operational"
671.00,"12","BUFR/CREX Temperature","012181","Averaged 11 micron BT for all clear pixels at nadir",,"K","2","0","16","K","2","5","Operational"
672.00,"12","BUFR/CREX Temperature","012182","Averaged 3.7 micron BT for all clear pixels at nadir",,"K","2","0","16","K","2","5","Operational"
673.00,"12","BUFR/CREX Temperature","012183","Averaged 12 micron BT for all clear pixels, forward view",,"K","2","0","16","K","2","5","Operational"
674.00,"12","BUFR/CREX Temperature","012184","Averaged 11 micron BT for all clear pixels, forward view",,"K","2","0","16","K","2","5","Operational"
675.00,"12","BUFR/CREX Temperature","012185","Averaged 3.7 micron BT for all clear pixels, forward view",,"K","2","0","16","K","2","5","Operational"
676.00,"12","BUFR/CREX Temperature","012186","Mean nadir sea-surface temperature",,"K","2","0","16","K","2","5","Operational"
677.00,"12","BUFR/CREX Temperature","012187","Mean dual view sea-surface temperature",,"K","2","0","16","K","2","5","Operational"
678.00,"12","BUFR/CREX Temperature","012188","Interpolated 23.8 GHz brightness T from MWR",,"K","2","0","16","K","2","5","Operational"
679.00,"12","BUFR/CREX Temperature","012189","Interpolated 36.5 GHz brightness T from MWR",,"K","2","0","16","K","2","5","Operational"
680.00,"13","BUFR/CREX Hydrographic and hydrological elements","013001","Specific humidity",,"kg/kg","5","0","14","kg/kg","5","5","Operational"
681.00,"13","BUFR/CREX Hydrographic and hydrological elements","013002","Mixing ratio",,"kg/kg","5","0","14","kg/kg","5","5","Operational"
682.00,"13","BUFR/CREX Hydrographic and hydrological elements","013003","Relative humidity",,"%","0","0","7","%","0","3","Operational"
683.00,"13","BUFR/CREX Hydrographic and hydrological elements","013004","Vapour pressure",,"Pa","-1","0","10","Pa","-1","4","Operational"
684.00,"13","BUFR/CREX Hydrographic and hydrological elements","013005","Vapour density",,"kg m-3","3","0","7","kg m-3","3","3","Operational"
685.00,"13","BUFR/CREX Hydrographic and hydrological elements","013006","Mixing heights",,"m","-1","-40","16","m","-1","5","Operational"
686.00,"13","BUFR/CREX Hydrographic and hydrological elements","013007","Minimum relative humidity",,"%","0","0","7","%","0","3","Operational"
687.00,"13","BUFR/CREX Hydrographic and hydrological elements","013008","Maximum relative humidity",,"%","0","0","7","%","0","3","Operational"
688.00,"13","BUFR/CREX Hydrographic and hydrological elements","013009","Relative humidity","(see Note 6)","%","1","-1000","12","%","1","4","Operational"
689.00,"13","BUFR/CREX Hydrographic and hydrological elements","013011","Total precipitation/total water equivalent",,"kg m-2","1","-1","14","kg m-2","1","5","Operational"
690.00,"13","BUFR/CREX Hydrographic and hydrological elements","013012","Depth of fresh snow",,"m","2","-2","12","m","2","4","Operational"
691.00,"13","BUFR/CREX Hydrographic and hydrological elements","013013","Total snow depth",,"m","2","-2","16","m","2","5","Operational"
692.00,"13","BUFR/CREX Hydrographic and hydrological elements","013014","Rainfall/water equivalent of snow (averaged rate)",,"kg m-2 s-1","4","0","12","kg m-2 s-1","4","4","Operational"
693.00,"13","BUFR/CREX Hydrographic and hydrological elements","013015","Snowfall (averaged rate)",,"m/s","7","0","12","m/s","7","4","Operational"
694.00,"13","BUFR/CREX Hydrographic and hydrological elements","013016","Precipitable water",,"kg m-2","0","0","7","kg m-2","0","3","Operational"
695.00,"13","BUFR/CREX Hydrographic and hydrological elements","013019","Total precipitation past 1 hour",,"kg m-2","1","-1","14","kg m-2","1","4","Operational"
696.00,"13","BUFR/CREX Hydrographic and hydrological elements","013020","Total precipitation past 3 hours",,"kg m-2","1","-1","14","kg m-2","1","5","Operational"
697.00,"13","BUFR/CREX Hydrographic and hydrological elements","013021","Total precipitation past 6 hours",,"kg m-2","1","-1","14","kg m-2","1","5","Operational"
698.00,"13","BUFR/CREX Hydrographic and hydrological elements","013022","Total precipitation past 12 hours",,"kg m-2","1","-1","14","kg m-2","1","5","Operational"
699.00,"13","BUFR/CREX Hydrographic and hydrological elements","013023","Total precipitation past 24 hours",,"kg m-2","1","-1","14","kg m-2","1","5","Operational"
700.00,"13","BUFR/CREX Hydrographic and hydrological elements","013031","Evapotranspiration",,"kg m-2","0","0","7","kg m-2","0","3","Operational"
701.00,"13","BUFR/CREX Hydrographic and hydrological elements","013032","Evaporation/evapotranspiration","(see Note 5)","kg m-2","1","0","8","kg m-2","1","3","Operational"
702.00,"13","BUFR/CREX Hydrographic and hydrological elements","013033","Evaporation/evapotranspiration",,"kg m-2","1","0","10","kg m-2","1","4","Operational"
703.00,"13","BUFR/CREX Hydrographic and hydrological elements","013038","Superadiabatic indicator",,"Code table","0","0","2","Code table","0","1","Operational"
704.00,"13","BUFR/CREX Hydrographic and hydrological elements","013039","Terrain type (ice/snow)",,"Code table","0","0","3","Code table","0","1","Operational"
705.00,"13","BUFR/CREX Hydrographic and hydrological elements","013040","Surface flag",,"Code table","0","0","4","Code table","0","2","Operational"
706.00,"13","BUFR/CREX Hydrographic and hydrological elements","013041","Pasquill-Gifford stability category",,"Code table","0","0","4","Code table","0","2","Operational"
707.00,"13","BUFR/CREX Hydrographic and hydrological elements","013042","Parcel lifted index (to 500 hPa)","(see Notes 3 and 4)","K","0","-20","6","K","0","2","Operational"
708.00,"13","BUFR/CREX Hydrographic and hydrological elements","013043","Best lifted index (to 500 hPa)","(see Notes 3 and 4)","K","0","-20","6","K","0","2","Operational"
709.00,"13","BUFR/CREX Hydrographic and hydrological elements","013044","K index",,"K","0","-30","8","K","0","3","Operational"
710.00,"13","BUFR/CREX Hydrographic and hydrological elements","013045","KO index",,"K","0","-30","8","K","0","3","Operational"
711.00,"13","BUFR/CREX Hydrographic and hydrological elements","013046","Maximum buoyancy",,"K","0","-30","8","K","0","3","Operational"
712.00,"13","BUFR/CREX Hydrographic and hydrological elements","013047","Modified Showalter stability index","(see Note 7)","K","0","-60","6","C","0","2","Operational"
713.00,"13","BUFR/CREX Hydrographic and hydrological elements","013048","Water fraction",,"%","1","0","10","%","1","4","Operational"
714.00,"13","BUFR/CREX Hydrographic and hydrological elements","013051","Frequency group, precipitation",,"Code table","0","0","4","Code table","0","2","Operational"
715.00,"13","BUFR/CREX Hydrographic and hydrological elements","013052","Highest daily amount of precipitation",,"kg m-2","1","-1","14","kg m-2","1","5","Operational"
716.00,"13","BUFR/CREX Hydrographic and hydrological elements","013055","Intensity of precipitation",,"kg m-2 s-1","4","0","8","mm/h","1","4","Operational"
717.00,"13","BUFR/CREX Hydrographic and hydrological elements","013056","Character and intensity of precipitation",,"Code table","0","0","4","Code table","0","2","Operational"
718.00,"13","BUFR/CREX Hydrographic and hydrological elements","013057","Time of beginning or end of precipitation",,"Code table","0","0","4","Code table","0","2","Operational"
719.00,"13","BUFR/CREX Hydrographic and hydrological elements","013058","Size of precipitating element",,"m","4","0","7","mm","1","3","Operational"
720.00,"13","BUFR/CREX Hydrographic and hydrological elements","013059","Number of flashes (thunderstorm)",,"Numeric","0","0","7","Numeric","0","3","Operational"
721.00,"13","BUFR/CREX Hydrographic and hydrological elements","013060","Total accumulated precipitation",,"kg m-2","1","-1","17","kg m-2","1","5","Operational"
722.00,"13","BUFR/CREX Hydrographic and hydrological elements","013071","Upstream water level",,"m","2","0","14","m","2","4","Operational"
723.00,"13","BUFR/CREX Hydrographic and hydrological elements","013072","Downstream water level",,"m","2","0","14","m","2","4","Operational"
724.00,"13","BUFR/CREX Hydrographic and hydrological elements","013073","Maximum water level",,"m","2","0","14","m","2","4","Operational"
725.00,"13","BUFR/CREX Hydrographic and hydrological elements","013074","Ground water level",,"m","2","0","18","m","2","6","Operational"
726.00,"13","BUFR/CREX Hydrographic and hydrological elements","013080","Water pH",,"pH unit","1","0","10","pH unit","1","3","Operational"
727.00,"13","BUFR/CREX Hydrographic and hydrological elements","013081","Water conductivity",,"S/m","3","0","14","S/m","3","4","Operational"
728.00,"13","BUFR/CREX Hydrographic and hydrological elements","013082","Water temperature",,"K","1","0","12","K","1","4","Operational"
729.00,"13","BUFR/CREX Hydrographic and hydrological elements","013083","Dissolved oxygen",,"kg m-3","6","0","15","kg m-3","6","5","Operational"
730.00,"13","BUFR/CREX Hydrographic and hydrological elements","013084","Turbidity",,"lm","0","0","14","lm","0","4","Operational"
731.00,"13","BUFR/CREX Hydrographic and hydrological elements","013085","Oxidation Reduction Potential (ORP)",,"V","3","0","14","V","3","4","Operational"
732.00,"13","BUFR/CREX Hydrographic and hydrological elements","013090","Radiometer water vapour content",,"kg m-2","1","0","10","kg m-2","1","4","Operational"
733.00,"13","BUFR/CREX Hydrographic and hydrological elements","013091","Radiometer liquid content",,"kg m-2","2","0","8","kg m-2","2","3","Operational"
734.00,"13","BUFR/CREX Hydrographic and hydrological elements","013093","Cloud optical thickness",,"Numeric","0","0","8","Numeric","0","3","Operational"
735.00,"13","BUFR/CREX Hydrographic and hydrological elements","013095","Total column water vapour",,"kg m-2","4","0","19","kg m-2","4","6","Operational"
736.00,"13","BUFR/CREX Hydrographic and hydrological elements","013096","MWR water vapour content",,"kg m-2","2","0","14","kg m-2","2","5","Operational"
737.00,"13","BUFR/CREX Hydrographic and hydrological elements","013097","MWR liquid water content",,"kg m-2","2","0","14","kg m-2","2","5","Operational"
738.00,"13","BUFR/CREX Hydrographic and hydrological elements","013098","Integrated water vapour density",,"kg m-2","8","0","30","kg m-2","8","10","Operational"
739.00,"13","BUFR/CREX Hydrographic and hydrological elements","013099","Log10 of integrated cloud particle density",,"log(m-2)","1","0","7","log(m-2)","1","3","Operational"
740.00,"13","BUFR/CREX Hydrographic and hydrological elements","013100","Log10 of integrated cloud particle area",,"log(m2 m-2)","1","-70","7","log(m2 m-2)","1","2","Operational"
741.00,"13","BUFR/CREX Hydrographic and hydrological elements","013101","Log10 of integrated cloud particle volume",,"log(m3 m-2)","1","-140","7","log(m3 m-2)","1","3","Operational"
742.00,"13","BUFR/CREX Hydrographic and hydrological elements","013110","Mass mixing ratio",,"%","0","0","7","%","0","3","Operational"
743.00,"13","BUFR/CREX Hydrographic and hydrological elements","013111","Soil moisture",,"g/kg","0","0","10","g/kg","0","4","Operational"
744.00,"13","BUFR/CREX Hydrographic and hydrological elements","013112","Object wetness duration",,"s","0","0","17","s","0","5","Operational"
745.00,"13","BUFR/CREX Hydrographic and hydrological elements","013114","Rate of ice accretion",,"kg m-2 h-1","1","0","11","kg m-2 h-1","1","4","Operational"
746.00,"13","BUFR/CREX Hydrographic and hydrological elements","013115","Ice thickness","(see Note 9)","m","2","0","19","m","2","6","Operational"
747.00,"13","BUFR/CREX Hydrographic and hydrological elements","013117","Snow density (liquid water content)",,"kg m-3","0","0","10","kg m-3","0","3","Operational"
748.00,"13","BUFR/CREX Hydrographic and hydrological elements","013118","Depth of fresh snow (high accuracy)","(see Note 10)","m","3","-2","14","m","3","5","Operational"
751.00,"13","BUFR/CREX Hydrographic and hydrological elements","013155","Intensity of precipitation (high accuracy)","(see Note 8)","kg m-2 s-1","5","-1","16","mm/h","2","5","Operational"
752.00,"13","BUFR/CREX Hydrographic and hydrological elements","013160","Radiometer liquid content",,"kg m-2","2","-350","10","kg m-2","2","3","Operational"
753.00,"14","BUFR/CREX Radiation and radiance","014001","Long-wave radiation, integrated over 24 hours",,"J m-2","-3","-65536","17","J m-2","-3","5","Operational"
754.00,"14","BUFR/CREX Radiation and radiance","014002","Long-wave radiation, integrated over period specified",,"J m-2","-3","-65536","17","J m-2","-3","5","Operational"
755.00,"14","BUFR/CREX Radiation and radiance","014003","Short-wave radiation, integrated over 24 hours",,"J m-2","-3","-65536","17","J m-2","-3","5","Operational"
756.00,"14","BUFR/CREX Radiation and radiance","014004","Short-wave radiation, integrated over period specified",,"J m-2","-3","-65536","17","J m-2","-3","5","Operational"
757.00,"14","BUFR/CREX Radiation and radiance","014011","Net long-wave radiation, integrated over 24 hours",,"J m-2","-3","-65536","17","J m-2","-3","5","Operational"
758.00,"14","BUFR/CREX Radiation and radiance","014012","Net long-wave radiation, integrated over period specified",,"J m-2","-3","-65536","17","J m-2","-3","5","Operational"
759.00,"14","BUFR/CREX Radiation and radiance","014013","Net short-wave radiation, integrated over 24 hours",,"J m-2","-3","-65536","17","J m-2","-3","5","Operational"
760.00,"14","BUFR/CREX Radiation and radiance","014014","Net short-wave radiation, integrated over period specified",,"J m-2","-3","-65536","17","J m-2","-3","5","Operational"
761.00,"14","BUFR/CREX Radiation and radiance","014015","Net radiation, integrated over 24 hours",,"J m-2","-4","-16384","15","J m-2","-4","5","Operational"
762.00,"14","BUFR/CREX Radiation and radiance","014016","Net radiation, integrated over period specified",,"J m-2","-4","-16384","15","J m-2","-4","5","Operational"
763.00,"14","BUFR/CREX Radiation and radiance","014017","Instantaneous long-wave radiation",,"W m-2","0","-512","10","W m-2","0","4","Operational"
764.00,"14","BUFR/CREX Radiation and radiance","014018","Instantaneous short-wave radiation",,"W m-2","0","-2048","12","W m-2","0","4","Operational"
765.00,"14","BUFR/CREX Radiation and radiance","014019","Surface albedo",,"%","0","0","7","%","0","3","Operational"
766.00,"14","BUFR/CREX Radiation and radiance","014020","Global solar radiation, integrated over 24 hours",,"J m-2","-4","0","15","J m-2","-4","5","Operational"
767.00,"14","BUFR/CREX Radiation and radiance","014021","Global solar radiation, integrated over period specified",,"J m-2","-4","0","15","J m-2","-4","5","Operational"
768.00,"14","BUFR/CREX Radiation and radiance","014022","Diffuse solar radiation, integrated over 24 hours",,"J m-2","-4","0","15","J m-2","-4","5","Operational"
769.00,"14","BUFR/CREX Radiation and radiance","014023","Diffuse solar radiation, integrated over period specified",,"J m-2","-4","0","15","J m-2","-4","5","Operational"
770.00,"14","BUFR/CREX Radiation and radiance","014024","Direct solar radiation, integrated over 24 hours",,"J m-2","-4","0","15","J m-2","-4","5","Operational"
771.00,"14","BUFR/CREX Radiation and radiance","014025","Direct solar radiation, integrated over period specified",,"J m-2","-4","0","15","J m-2","-4","5","Operational"
772.00,"14","BUFR/CREX Radiation and radiance","014026","Albedo at the top of clouds",,"%","0","0","7","%","0","3","Operational"
773.00,"14","BUFR/CREX Radiation and radiance","014027","Albedo",,"%","0","0","7","%","0","3","Operational"
774.00,"14","BUFR/CREX Radiation and radiance","014028","Global solar radiation (high accuracy), integrated over period specified",,"J m-2","-2","0","20","J m-2","-2","6","Operational"
775.00,"14","BUFR/CREX Radiation and radiance","014029","Diffuse solar radiation (high accuracy), integrated over period specified",,"J m-2","-2","0","20","J m-2","-2","6","Operational"
776.00,"14","BUFR/CREX Radiation and radiance","014030","Direct solar radiation (high accuracy), integrated over period specified",,"J m-2","-2","0","20","J m-2","-2","6","Operational"
777.00,"14","BUFR/CREX Radiation and radiance","014031","Total sunshine",,"min","0","0","11","min","0","4","Operational"
778.00,"14","BUFR/CREX Radiation and radiance","014032","Total sunshine",,"h","0","0","10","h","0","4","Operational"
779.00,"14","BUFR/CREX Radiation and radiance","014033","Total sunshine",,"%","0","0","9","%","0","3","Operational"
780.00,"14","BUFR/CREX Radiation and radiance","014034","Sunshine over period specified",,"min","0","0","11","min","0","4","Operational"
781.00,"14","BUFR/CREX Radiation and radiance","014035","Solar radiation flux",,"W m-2","1","0","14","W m-2","1","5","Operational"
782.00,"14","BUFR/CREX Radiation and radiance","014042","Bidirectional reflectance",,"%","0","0","7","%","0","3","Operational"
783.00,"14","BUFR/CREX Radiation and radiance","014043","Channel radiance",,"W m-2 sr-1 um-1","4","0","23","W m-2 sr-1 um-1","4","7","Operational"
784.00,"14","BUFR/CREX Radiation and radiance","014044","Channel radiance",,"W m-2 sr-1 cm","7","-100000","22","W m-2 sr-1 cm","7","7","Operational"
785.00,"14","BUFR/CREX Radiation and radiance","014045","Channel radiance","(see Note 4)","W m-2 sr-1 cm","0","0","11","W m-2 sr-1 cm","0","4","Operational"
786.00,"14","BUFR/CREX Radiation and radiance","014046","Scaled IASI radiance","(see Note 6)","W m-2 sr-1 m","0","-5000","16","W m-2 sr-1 m","0","5","Operational"
787.00,"14","BUFR/CREX Radiation and radiance","014047","Scaled mean AVHRR radiance",,"W m-2 sr-1 m","0","0","31","W m-2 sr-1 m","0","10","Operational"
788.00,"14","BUFR/CREX Radiation and radiance","014048","Scaled standard deviation AVHRR radiance",,"W m-2 sr-1 m","0","0","31","W m-2 sr-1 m","0","10","Operational"
789.00,"14","BUFR/CREX Radiation and radiance","014050","Emissivity","(see Note 5)","%","1","0","10","%","1","4","Operational"
790.00,"14","BUFR/CREX Radiation and radiance","014051","Direct solar radiation integrated over last hour",,"J m-2","-3","0","14","J m-2","-3","4","Operational"
791.00,"14","BUFR/CREX Radiation and radiance","014052","Global upward solar radiation, integrated over period specified",,"J m-2","-2","-1048574","20","J m-2","-2","7","Operational"
792.00,"14","BUFR/CREX Radiation and radiance","014053","Net radiation (high accuracy), integrated over period specified",,"J m-2","-2","-1048574","21","J m-2","-2","7","Operational"
793.00,"14","BUFR/CREX Radiation and radiance","014054","Photosynthetically active radiation, integrated over period specified",,"J m-2","-3","0","16","J m-2","-3","5","Operational"
794.00,"14","BUFR/CREX Radiation and radiance","014055","Solar activity index",,"Numeric","0","-32768","16","Numeric","0","5","Operational"
795.00,"14","BUFR/CREX Radiation and radiance","014056","Background luminance",,"Cd m-2","0","0","18","Cd m-2","0","6","Operational"
796.00,"14","BUFR/CREX Radiation and radiance","014057","Soil heat flux",,"J m-2","-2","-1048574","21","J m-2","-2","7","Operational"
798.00,"14","BUFR/CREX Radiation and radiance","014072","Global UV irradiation","(see Note 8)","J m-2","0","-4000000","23","J m-2","0","7","Operational"
800.00,"15","BUFR/CREX Physical/chemical constituents","015001","Total ozone",,"DU","0","0","10","DU","0","4","Operational"
801.00,"15","BUFR/CREX Physical/chemical constituents","015002","Air mass (slant path at 22 km)",,"Numeric","2","0","10","Numeric","2","3","Operational"
802.00,"15","BUFR/CREX Physical/chemical constituents","015003","Measured ozone partial pressure (sounding)","(see Note 1)","Pa","4","0","9","nbar","0","3","Operational"
803.00,"15","BUFR/CREX Physical/chemical constituents","015004","Ozone sounding correction factor (CF)","(see Note 2)","Numeric","3","0","11","Numeric","3","4","Operational"
804.00,"15","BUFR/CREX Physical/chemical constituents","015005","Ozone p","(see Note 3)","DU","0","0","10","DU","0","3","Operational"
806.00,"15","BUFR/CREX Physical/chemical constituents","015008","Significand of volumetric mixing ratio",,"Numeric","0","0","10","Numeric","0","4","Operational"
809.00,"15","BUFR/CREX Physical/chemical constituents","015011","Log10 of integrated electron density",,"log (m-2)","3","14000","13","log (m-2)","3","4","Operational"
810.00,"15","BUFR/CREX Physical/chemical constituents","015012","Total electron count per square metre",,"m-2","-16","0","6","m-2","-16","2","Operational"
811.00,"15","BUFR/CREX Physical/chemical constituents","015015","Maximum image spectral component before normalization",,"Numeric","0","0","31","Numeric","0","10","Operational"
812.00,"15","BUFR/CREX Physical/chemical constituents","015020","Integrated ozone density",,"kg m-2","8","0","21","kg m-2","8","7","Operational"
813.00,"15","BUFR/CREX Physical/chemical constituents","015021","Integrated mass density",,"kg m-2","11","0","31","kg m-2","11","10","Operational"
816.00,"15","BUFR/CREX Physical/chemical constituents","015024","Optical depth",,"Numeric","4","0","24","Numeric","4","8","Operational"
817.00,"15","BUFR/CREX Physical/chemical constituents","015025","Type of pollutant",,"Code table","0","0","4","Code table","0","2","Operational"
818.00,"15","BUFR/CREX Physical/chemical constituents","015026","Concentration of pollutant (mol mol-1)",,"mol/mol","9","0","9","mol/mol","9","3","Operational"
819.00,"15","BUFR/CREX Physical/chemical constituents","015027","Concentration of pollutant (kg m-3)",,"kg m-3","9","0","10","kg m-3","9","4","Operational"
821.00,"15","BUFR/CREX Physical/chemical constituents","015029","Extinction coefficient",,"/m","9","0","30","/m","9","10","Operational"
822.00,"15","BUFR/CREX Physical/chemical constituents","015030","Aerosol contamination index","(see Note 6)","Numeric","2","-1000","12","Numeric","2","4","Operational"
823.00,"15","BUFR/CREX Physical/chemical constituents","015031","Atmospheric path delay in satellite signal",,"m","4","10000","15","m","4","5","Operational"
824.00,"15","BUFR/CREX Physical/chemical constituents","015032","Estimated error in atmospheric path delay",,"m","4","0","10","m","4","4","Operational"
825.00,"15","BUFR/CREX Physical/chemical constituents","015033","Difference in path delays for limb views at extremes of scan",,"m","5","-10000","15","m","5","5","Operational"
826.00,"15","BUFR/CREX Physical/chemical constituents","015034","Estimated error in path delay difference",,"m","5","0","14","m","5","5","Operational"
827.00,"15","BUFR/CREX Physical/chemical constituents","015035","Component of zenith path delay due to water vapour",,"m","4","0","14","m","4","5","Operational"
828.00,"15","BUFR/CREX Physical/chemical constituents","015036","Atmospheric refractivity","(see Note 5)","N units","3","0","19","N units","3","6","Operational"
829.00,"15","BUFR/CREX Physical/chemical constituents","015037","Bending angle",,"rad","8","-100000","23","rad","8","7","Operational"
831.00,"15","BUFR/CREX Physical/chemical constituents","015041","Sulphur dioxide index","(see Note 7)","Numeric","2","-1200","14","Numeric","2","4","Operational"
832.00,"15","BUFR/CREX Physical/chemical constituents","015042","Reflectance",,"%","2","0","14","%","2","5","Operational"
835.00,"15","BUFR/CREX Physical/chemical constituents","015045","Sulphur dioxide","(see Note 8)","DU","2","-2000","15","DU","2","5","Operational"
836.00,"15","BUFR/CREX Physical/chemical constituents","015046","Volcano contamination index","(see Note 9)","Numeric","2","-1000","11","Numeric","2","4","Operational"
837.00,"15","BUFR/CREX Physical/chemical constituents","015049","Aerosol Angstrom wavelength exponent",,"Numeric","3","-2000","14","Numeric","3","5","Operational"
838.00,"15","BUFR/CREX Physical/chemical constituents","015051","Meteorological optical range",,"m","0","0","18","m","0","6","Operational"
839.00,"15","BUFR/CREX Physical/chemical constituents","015052","Log10 of number density of aerosol particles with diameter greater than 5 nm",,"log (m-3)","1","60","6","log (m-3)","1","3","Operational"
840.00,"15","BUFR/CREX Physical/chemical constituents","015053","Log10 of number density of aerosol particles with diameter greater than 14 nm",,"log (m-3)","2","600","9","log (m-3)","2","4","Operational"
841.00,"15","BUFR/CREX Physical/chemical constituents","015054","Log10 of number density of aerosol particles with diameter between 0.25 and 2.5 µm",,"log (m-3)","2","550","9","log (m-3)","2","4","Operational"
842.00,"15","BUFR/CREX Physical/chemical constituents","015055","Non volatile aerosol ratio",,"Numeric","2","0","7","Numeric","2","3","Operational"
843.00,"15","BUFR/CREX Physical/chemical constituents","015062","Aerosol optical thickness",,"Numeric","3","-1000","14","Numeric","3","5","Operational"
844.00,"19","BUFR/CREX Synoptic features","019001","Type of synoptic feature",,"Code table","0","0","6","Code table","0","2","Operational"
845.00,"19","BUFR/CREX Synoptic features","019002","Effective radius of feature","(see Note 1)","m","-2","0","12","m","-2","4","Operational"
846.00,"19","BUFR/CREX Synoptic features","019003","Wind speed threshold","(see Note 2)","m/s","0","0","8","m/s","0","3","Operational"
847.00,"19","BUFR/CREX Synoptic features","019004","Effective radius with respect to wind speeds above threshold","(see Note 2)","m","-2","0","12","m","-2","4","Operational"
848.00,"19","BUFR/CREX Synoptic features","019005","Direction of motion of feature","(see Note 3)","degree true","0","0","9","degree true","0","3","Operational"
849.00,"19","BUFR/CREX Synoptic features","019006","Speed of motion of feature","(see Note 3)","m/s","2","0","14","m/s","2","5","Operational"
850.00,"19","BUFR/CREX Synoptic features","019007","Effective radius of feature",,"m","-3","0","12","m","-3","4","Operational"
851.00,"19","BUFR/CREX Synoptic features","019008","Vertical extent of circulation",,"Code table","0","0","3","Code table","0","1","Operational"
852.00,"19","BUFR/CREX Synoptic features","019009","Effective radius with respect to wind speeds above threshold (large storms)",,"m","-3","0","12","m","-3","4","Operational"
853.00,"19","BUFR/CREX Synoptic features","019010","Method for tracking the centre of synoptic feature",,"Code table","0","0","4","Code table","0","2","Operational"
854.00,"19","BUFR/CREX Synoptic features","019100","Time interval to calculate the movement of the tropical cyclone",,"Code table","0","0","4","Code table","0","2","Operational"
855.00,"19","BUFR/CREX Synoptic features","019101","Accuracy of the position of the centre of the tropical cyclone",,"Code table","0","0","4","Code table","0","2","Operational"
856.00,"19","BUFR/CREX Synoptic features","019102","Shape and definition of the eye of the tropical cyclone",,"Code table","0","0","3","Code table","0","1","Operational"
857.00,"19","BUFR/CREX Synoptic features","019103","Diameter of major axis of the eye of the tropical cyclone",,"Code table","0","0","4","Code table","0","2","Operational"
858.00,"19","BUFR/CREX Synoptic features","019104","Change in character of the eye during the 30 minutes",,"Code table","0","0","4","Code table","0","2","Operational"
859.00,"19","BUFR/CREX Synoptic features","019105","Distance between the end of spiral band and the centre",,"Code table","0","0","4","Code table","0","2","Operational"
860.00,"19","BUFR/CREX Synoptic features","019106","Identification number of tropical cyclone",,"Numeric","0","0","7","Numeric","0","3","Operational"
861.00,"19","BUFR/CREX Synoptic features","019107","Time interval over which the movement of the tropical cyclone has been calculated",,"Code table","0","0","4","Code table","0","2","Operational"
862.00,"19","BUFR/CREX Synoptic features","019108","Accuracy of geographical position of the tropical cyclone",,"Code table","0","0","3","Code table","0","1","Operational"
863.00,"19","BUFR/CREX Synoptic features","019109","Mean diameter of the overcast cloud of the tropical cyclone",,"Code table","0","0","4","Code table","0","2","Operational"
864.00,"19","BUFR/CREX Synoptic features","019110","Apparent 24-hour change in intensity of the tropical cyclone",,"Code table","0","0","4","Code table","0","2","Operational"
865.00,"19","BUFR/CREX Synoptic features","019111","Current Intensity (CI) number of the tropical cyclone",,"Numeric","1","0","7","Numeric","1","3","Operational"
866.00,"19","BUFR/CREX Synoptic features","019112","Data Tropical (DT) number of the tropical cyclone",,"Numeric","1","0","7","Numeric","1","3","Operational"
867.00,"19","BUFR/CREX Synoptic features","019113","Cloud pattern type of the DT-number",,"Code table","0","0","4","Code table","0","2","Operational"
868.00,"19","BUFR/CREX Synoptic features","019114","Model Expected Tropical (MET) number of the tropical cyclone",,"Numeric","1","0","7","Numeric","1","3","Operational"
869.00,"19","BUFR/CREX Synoptic features","019115","Trend of the past 24-hour change (+: Developed, -: Weakened)",,"Numeric","1","-30","6","Numeric","1","2","Operational"
870.00,"19","BUFR/CREX Synoptic features","019116","Pattern Tropical (PT) number of the tropical cyclone",,"Numeric","1","0","7","Numeric","1","3","Operational"
871.00,"19","BUFR/CREX Synoptic features","019117","Cloud picture type of the PT-number",,"Code table","0","0","3","Code table","0","1","Operational"
872.00,"19","BUFR/CREX Synoptic features","019118","Final Tropical (T) number of the tropical cyclone",,"Numeric","1","0","7","Numeric","1","3","Operational"
873.00,"19","BUFR/CREX Synoptic features","019119","Type of the final T-number",,"Code table","0","0","3","Code table","0","1","Operational"
874.00,"19","BUFR/CREX Synoptic features","019150","Typhoon International Common Number (Typhoon Committee)",,"CCITT IA5","0","0","32","Character","0","4","Operational"
875.00,"20","BUFR/CREX Observed phenomena","020001","Horizontal visibility",,"m","-1","0","13","m","-1","4","Operational"
876.00,"20","BUFR/CREX Observed phenomena","020002","Vertical visibility",,"m","-1","0","7","m","-1","3","Operational"
877.00,"20","BUFR/CREX Observed phenomena","020003","Present weather","(see Note 1)","Code table","0","0","9","Code table","0","3","Operational"
878.00,"20","BUFR/CREX Observed phenomena","020004","Past weather (1)","(see Note 2)","Code table","0","0","5","Code table","0","2","Operational"
879.00,"20","BUFR/CREX Observed phenomena","020005","Past weather (2)","(see Note 2)","Code table","0","0","5","Code table","0","2","Operational"
880.00,"20","BUFR/CREX Observed phenomena","020006","Flight rules",,"Code table","0","0","3","Code table","0","1","Operational"
881.00,"20","BUFR/CREX Observed phenomena","020008","Cloud distribution for aviation",,"Code table","0","0","5","Code table","0","2","Operational"
882.00,"20","BUFR/CREX Observed phenomena","020009","General weather indicator (TAF/METAR)",,"Code table","0","0","4","Code table","0","2","Operational"
883.00,"20","BUFR/CREX Observed phenomena","020010","Cloud cover (total)","(see Note 5)","%","0","0","7","%","0","3","Operational"
884.00,"20","BUFR/CREX Observed phenomena","020011","Cloud amount",,"Code table","0","0","4","Code table","0","2","Operational"
885.00,"20","BUFR/CREX Observed phenomena","020012","Cloud type",,"Code table","0","0","6","Code table","0","2","Operational"
886.00,"20","BUFR/CREX Observed phenomena","020013","Height of base of cloud",,"m","-1","-40","11","m","-1","4","Operational"
887.00,"20","BUFR/CREX Observed phenomena","020014","Height of top of cloud",,"m","-1","-40","11","m","-1","4","Operational"
888.00,"20","BUFR/CREX Observed phenomena","020015","Pressure at base of cloud",,"Pa","-1","0","14","Pa","-1","5","Operational"
889.00,"20","BUFR/CREX Observed phenomena","020016","Pressure at top of cloud",,"Pa","-1","0","14","Pa","-1","5","Operational"
890.00,"20","BUFR/CREX Observed phenomena","020017","Cloud top description",,"Code table","0","0","4","Code table","0","2","Operational"
891.00,"20","BUFR/CREX Observed phenomena","020018","Tendency of runway visual range",,"Code table","0","0","2","Code table","0","1","Operational"
892.00,"20","BUFR/CREX Observed phenomena","020019","Significant present or forecast weather","(see Note 15)","CCITT IA5","0","0","72","Character","0","9","Operational"
893.00,"20","BUFR/CREX Observed phenomena","020020","Significant recent weather phenomena","(see Note 15)","CCITT IA5","0","0","32","Character","0","4","Operational"
894.00,"20","BUFR/CREX Observed phenomena","020021","Type of precipitation",,"Flag table","0","0","30","Flag table","0","10","Operational"
895.00,"20","BUFR/CREX Observed phenomena","020022","Character of precipitation",,"Code table","0","0","4","Code table","0","2","Operational"
896.00,"20","BUFR/CREX Observed phenomena","020023","Other weather phenomena",,"Flag table","0","0","18","Flag table","0","6","Operational"
897.00,"20","BUFR/CREX Observed phenomena","020024","Intensity of phenomena",,"Code table","0","0","3","Code table","0","1","Operational"
898.00,"20","BUFR/CREX Observed phenomena","020025","Obscuration",,"Flag table","0","0","21","Flag table","0","7","Operational"
899.00,"20","BUFR/CREX Observed phenomena","020026","Character of obscuration",,"Code table","0","0","4","Code table","0","2","Operational"
900.00,"20","BUFR/CREX Observed phenomena","020027","Phenomena occurrence",,"Flag table","0","0","9","Flag table","0","3","Operational"
901.00,"20","BUFR/CREX Observed phenomena","020028","Expected change in intensity",,"Code table","0","0","3","Code table","0","1","Operational"
902.00,"20","BUFR/CREX Observed phenomena","020029","Rain flag",,"Code table","0","0","2","Code table","0","1","Operational"
903.00,"20","BUFR/CREX Observed phenomena","020031","Ice deposit (thickness)",,"m","2","0","7","m","2","3","Operational"
904.00,"20","BUFR/CREX Observed phenomena","020032","Rate of ice accretion (estimated)",,"Code table","0","0","3","Code table","0","1","Operational"
905.00,"20","BUFR/CREX Observed phenomena","020033","Cause of ice accretion",,"Flag table","0","0","4","Flag table","0","2","Operational"
906.00,"20","BUFR/CREX Observed phenomena","020034","Sea ice concentration",,"Code table","0","0","5","Code table","0","2","Operational"
907.00,"20","BUFR/CREX Observed phenomena","020035","Amount and type of ice",,"Code table","0","0","4","Code table","0","2","Operational"
908.00,"20","BUFR/CREX Observed phenomena","020036","Ice situation",,"Code table","0","0","5","Code table","0","2","Operational"
909.00,"20","BUFR/CREX Observed phenomena","020037","Ice development",,"Code table","0","0","5","Code table","0","2","Operational"
910.00,"20","BUFR/CREX Observed phenomena","020038","Bearing of ice edge","(see Note 3)","degree true","0","0","12","degree true","0","3","Operational"
911.00,"20","BUFR/CREX Observed phenomena","020039","Ice distance",,"m","-1","0","13","m","-1","4","Operational"
912.00,"20","BUFR/CREX Observed phenomena","020040","Evolution of drift snow",,"Code table","0","0","4","Code table","0","2","Operational"
913.00,"20","BUFR/CREX Observed phenomena","020041","Airframe icing",,"Code table","0","0","4","Code table","0","2","Operational"
914.00,"20","BUFR/CREX Observed phenomena","020042","Airframe icing present",,"Code table","0","0","2","Code table","0","1","Operational"
915.00,"20","BUFR/CREX Observed phenomena","020043","Peak liquid water content",,"kg m-3","4","0","7","kg m-3","4","2","Operational"
916.00,"20","BUFR/CREX Observed phenomena","020044","Average liquid water content",,"kg m-3","4","0","7","kg m-3","4","2","Operational"
917.00,"20","BUFR/CREX Observed phenomena","020045","Supercooled large droplet (SLD) conditions",,"Code table","0","0","2","Code table","0","1","Operational"
918.00,"20","BUFR/CREX Observed phenomena","020048","Evolution of feature",,"Code table","0","0","4","Code table","0","2","Operational"
919.00,"20","BUFR/CREX Observed phenomena","020050","Cloud index",,"Code table","0","0","8","Code table","0","3","Operational"
920.00,"20","BUFR/CREX Observed phenomena","020051","Amount of low clouds",,"%","0","0","7","%","0","3","Operational"
921.00,"20","BUFR/CREX Observed phenomena","020052","Amount of middle clouds",,"%","0","0","7","%","0","3","Operational"
922.00,"20","BUFR/CREX Observed phenomena","020053","Amount of high clouds",,"%","0","0","7","%","0","3","Operational"
923.00,"20","BUFR/CREX Observed phenomena","020054","True direction from which a phenomenon or clouds are moving or in which they are observed","(see Note 17)","degree true","0","0","9","degree true","0","3","Operational"
924.00,"20","BUFR/CREX Observed phenomena","020055","State of sky in the tropics",,"Code table","0","0","4","Code table","0","2","Operational"
925.00,"20","BUFR/CREX Observed phenomena","020056","Cloud phase",,"Code table","0","0","3","Code table","0","1","Operational"
926.00,"20","BUFR/CREX Observed phenomena","020058","Visibility seawards from a coastal station",,"m","-1","0","13","m","-1","4","Operational"
927.00,"20","BUFR/CREX Observed phenomena","020059","Minimum horizontal visibility",,"m","-1","0","9","m","-1","3","Operational"
928.00,"20","BUFR/CREX Observed phenomena","020060","Prevailing horizontal visibility","(see Note 7)","m","-1","0","10","m","-1","4","Operational"
929.00,"20","BUFR/CREX Observed phenomena","020061","Runway visual range (RVR)",,"m","0","0","12","m","0","4","Operational"
930.00,"20","BUFR/CREX Observed phenomena","020062","State of the ground (with or without snow)",,"Code table","0","0","5","Code table","0","2","Operational"
931.00,"20","BUFR/CREX Observed phenomena","020063","Special phenomena",,"Code table","0","0","10","Code table","0","4","Operational"
932.00,"20","BUFR/CREX Observed phenomena","020065","Snow cover","(see Note 4)","%","0","0","7","%","0","3","Operational"
933.00,"20","BUFR/CREX Observed phenomena","020066","Maximum diameter of hailstones",,"m","3","0","8","m","3","3","Operational"
934.00,"20","BUFR/CREX Observed phenomena","020067","Diameter of deposit",,"m","3","0","9","m","3","3","Operational"
935.00,"20","BUFR/CREX Observed phenomena","020070","Minimum number of atmospherics",,"Numeric","0","0","7","Numeric","0","3","Operational"
936.00,"20","BUFR/CREX Observed phenomena","020071","Accuracy of fix and rate of atmospherics",,"Code table","0","0","4","Code table","0","2","Operational"
939.00,"20","BUFR/CREX Observed phenomena","020081","Cloud amount in segment",,"%","0","0","7","%","0","3","Operational"
940.00,"20","BUFR/CREX Observed phenomena","020082","Amount segment cloud free",,"%","0","0","7","%","0","3","Operational"
941.00,"20","BUFR/CREX Observed phenomena","020083","Amount of segment covered by scene",,"%","0","0","7","%","0","3","Operational"
942.00,"20","BUFR/CREX Observed phenomena","020085","General condition of runway",,"Code table","0","0","4","Code table","0","1","Operational"
943.00,"20","BUFR/CREX Observed phenomena","020086","Runway deposits",,"Code table","0","0","4","Code table","0","1","Operational"
944.00,"20","BUFR/CREX Observed phenomena","020087","Runway contamination",,"Code table","0","0","4","Code table","0","1","Operational"
945.00,"20","BUFR/CREX Observed phenomena","020088","Depth of runway deposits",,"m","3","0","12","m","0","4","Operational"
946.00,"20","BUFR/CREX Observed phenomena","020089","Runway friction coefficient",,"Code table","0","0","7","Code table","0","2","Operational"
947.00,"20","BUFR/CREX Observed phenomena","020090","Special clouds",,"Code table","0","0","4","Code table","0","2","Operational"
948.00,"20","BUFR/CREX Observed phenomena","020091","Vertical visibility",,"ft","-2","0","10","ft","-2","3","Operational"
949.00,"20","BUFR/CREX Observed phenomena","020092","Height of base of cloud",,"ft","-2","0","10","ft","-2","3","Operational"
950.00,"20","BUFR/CREX Observed phenomena","020093","Height of inversion",,"m","-1","0","8","m","-1","3","Operational"
951.00,"20","BUFR/CREX Observed phenomena","020095","Ice probability",,"Numeric","3","0","10","Numeric","3","4","Operational"
952.00,"20","BUFR/CREX Observed phenomena","020096","Ice age (""A"" parameter)",,"dB","2","-4096","13","dB","2","4","Operational"
953.00,"20","BUFR/CREX Observed phenomena","020101","Locust (acridian) name",,"Code table","0","0","4","Code table","0","2","Operational"
954.00,"20","BUFR/CREX Observed phenomena","020102","Locust (maturity) colour",,"Code table","0","0","4","Code table","0","2","Operational"
955.00,"20","BUFR/CREX Observed phenomena","020103","Stage of development of locusts",,"Code table","0","0","4","Code table","0","2","Operational"
956.00,"20","BUFR/CREX Observed phenomena","020104","Organization state of swarm or band of locusts",,"Code table","0","0","4","Code table","0","2","Operational"
957.00,"20","BUFR/CREX Observed phenomena","020105","Size of swarm or band of locusts and duration of passage of swarm",,"Code table","0","0","4","Code table","0","2","Operational"
958.00,"20","BUFR/CREX Observed phenomena","020106","Locust population density",,"Code table","0","0","4","Code table","0","2","Operational"
959.00,"20","BUFR/CREX Observed phenomena","020107","Direction of movements of locust swarm",,"Code table","0","0","4","Code table","0","2","Operational"
960.00,"20","BUFR/CREX Observed phenomena","020108","Extent of vegetation",,"Code table","0","0","4","Code table","0","2","Operational"
961.00,"20","BUFR/CREX Observed phenomena","020111","x-axis error ellipse major component","(see Notes 8 and 9)","m","-1","0","17","m","-1","6","Operational"
962.00,"20","BUFR/CREX Observed phenomena","020112","y-axis error ellipse minor component","(see Notes 8 and 9)","m","-1","0","17","m","-1","6","Operational"
963.00,"20","BUFR/CREX Observed phenomena","020113","z-axis error ellipse component","(see Note 9)","m","-1","0","17","m","-1","6","Operational"
964.00,"20","BUFR/CREX Observed phenomena","020114","Angle of x-axis in error ellipse","(see Note 10)","deg","2","-18000","16","deg","2","5","Operational"
965.00,"20","BUFR/CREX Observed phenomena","020115","Angle of z-axis in error ellipse","(see Note 11)","deg","2","-18000","16","deg","2","5","Operational"
966.00,"20","BUFR/CREX Observed phenomena","020116","Emission height of cloud stroke",,"m","0","0","16","m","0","5","Operational"
967.00,"20","BUFR/CREX Observed phenomena","020117","Amplitude of lightning strike",,"A","-1","-32000","16","A","-1","5","Operational"
968.00,"20","BUFR/CREX Observed phenomena","020118","Lightning detection error",,"m","0","0","19","m","0","6","Operational"
969.00,"20","BUFR/CREX Observed phenomena","020119","Lightning discharge polarity",,"Code table","0","0","2","Code table","0","1","Operational"
970.00,"20","BUFR/CREX Observed phenomena","020121","Threshold value for polarity decision","(see Note 12)","V","3","0","16","V","3","5","Operational"
971.00,"20","BUFR/CREX Observed phenomena","020122","Threshold value for polarity decision","(see Note 13)","A","0","0","16","A","0","5","Operational"
972.00,"20","BUFR/CREX Observed phenomena","020123","Minimum threshold for detection","(see Note 14)","V/m","3","0","16","V/m","3","5","Operational"
973.00,"20","BUFR/CREX Observed phenomena","020124","Lightning stroke or flash",,"Code table","0","0","2","Code table","0","1","Operational"
974.00,"20","BUFR/CREX Observed phenomena","020126","Lightning rate of discharge",,"/h","0","0","23","/h","0","7","Operational"
975.00,"20","BUFR/CREX Observed phenomena","020127","Lightning - distance from station",,"m","-3","0","8","m","-3","3","Operational"
976.00,"20","BUFR/CREX Observed phenomena","020128","Lightning - direction from station",,"degree true","1","0","12","degree true","1","4","Operational"
977.00,"20","BUFR/CREX Observed phenomena","020130","Cloud hydrometeor concentration","(see Note 16)","Numeric","0","0","10","Numeric","0","3","Operational"
978.00,"20","BUFR/CREX Observed phenomena","020131","Effective radius of cloud hydrometeors",,"m","5","0","6","m","5","2","Operational"
979.00,"20","BUFR/CREX Observed phenomena","020132","Cloud liquid water content",,"kg m-3","5","0","11","kg m-3","5","4","Operational"
980.00,"20","BUFR/CREX Observed phenomena","020133","Hydrometeor radius",,"m","5","0","6","m","5","2","Operational"
981.00,"20","BUFR/CREX Observed phenomena","020135","Ice mass (on a rod)",,"kg/m","1","0","10","kg/m","1","3","Operational"
982.00,"20","BUFR/CREX Observed phenomena","020136","Supplementary cloud type",,"Code table","0","0","9","Code table","0","3","Operational"
983.00,"20","BUFR/CREX Observed phenomena","020137","Evolution of clouds",,"Code table","0","0","4","Code table","0","2","Operational"
984.00,"21","BUFR/CREX Radar data","021001","Horizontal reflectivity",,"dB","0","-64","7","dB","0","3","Operational"
985.00,"21","BUFR/CREX Radar data","021002","Vertical reflectivity",,"dB","0","-64","7","dB","0","3","Operational"
986.00,"21","BUFR/CREX Radar data","021003","Differential reflectivity",,"dB","1","-5","7","dB","1","3","Operational"
987.00,"21","BUFR/CREX Radar data","021005","Linear depolarization ratio",,"dB","0","-65","6","dB","0","2","Operational"
988.00,"21","BUFR/CREX Radar data","021006","Circular depolarization ratio",,"dB","0","-65","6","dB","0","2","Operational"
989.00,"21","BUFR/CREX Radar data","021011","Doppler mean velocity in x-direction",,"m/s","0","-128","8","m/s","0","3","Operational"
990.00,"21","BUFR/CREX Radar data","021012","Doppler mean velocity in y-direction",,"m/s","0","-128","8","m/s","0","3","Operational"
991.00,"21","BUFR/CREX Radar data","021013","Doppler mean velocity in z-direction",,"m/s","0","-128","8","m/s","0","3","Operational"
992.00,"21","BUFR/CREX Radar data","021014","Doppler mean velocity (radial)",,"m/s","1","-4096","13","m/s","1","4","Operational"
993.00,"21","BUFR/CREX Radar data","021017","Doppler velocity spectral width",,"m/s","1","0","8","m/s","1","3","Operational"
994.00,"21","BUFR/CREX Radar data","021018","Extended NYQUIST velocity",,"m/s","1","0","10","m/s","1","4","Operational"
995.00,"21","BUFR/CREX Radar data","021019","High NYQUIST velocity",,"m/s","1","0","10","m/s","1","3","Operational"
996.00,"21","BUFR/CREX Radar data","021021","Echo tops",,"m","-3","0","4","m","-3","2","Operational"
997.00,"21","BUFR/CREX Radar data","021022","Range bin offset",,"m","1","0","14","m","1","5","Operational"
998.00,"21","BUFR/CREX Radar data","021023","Range bin size",,"m","0","0","14","m","0","5","Operational"
999.00,"21","BUFR/CREX Radar data","021024","Azimuth offset",,"deg","1","0","12","deg","1","4","Operational"
1000.00,"21","BUFR/CREX Radar data","021025","Azimuthal resolution",,"deg","1","0","8","deg","1","3","Operational"
1002.00,"21","BUFR/CREX Radar data","021030","Signal to noise ratio",,"dB","0","-32","8","dB","0","3","Operational"
1003.00,"21","BUFR/CREX Radar data","021031","Vertically integrated liquid-water content",,"kg m-2","0","0","7","kg m-2","0","3","Operational"
1004.00,"21","BUFR/CREX Radar data","021036","Radar rainfall intensity",,"m/s","7","0","12","m/s","7","4","Operational"
1005.00,"21","BUFR/CREX Radar data","021041","Bright-band height",,"m","-2","0","8","m","-2","3","Operational"
1006.00,"21","BUFR/CREX Radar data","021051","Signal power above 1 mW",,"dB","0","-256","8","dB","0","3","Operational"
1007.00,"21","BUFR/CREX Radar data","021062","Backscatter",,"dB","2","-5000","13","dB","2","4","Operational"
1008.00,"21","BUFR/CREX Radar data","021063","Radiometric resolution (noise value)",,"%","1","0","10","%","1","4","Operational"
1009.00,"21","BUFR/CREX Radar data","021064","Clutter noise estimate",,"Numeric","0","0","8","Numeric","0","3","Operational"
1010.00,"21","BUFR/CREX Radar data","021065","Missing packet counter",,"Numeric","0","-127","8","Numeric","0","3","Operational"
1011.00,"21","BUFR/CREX Radar data","021066","Wave scatterometer product confidence data",,"Flag table","0","0","12","Flag table","0","4","Operational"
1012.00,"21","BUFR/CREX Radar data","021067","Wind product confidence data",,"Flag table","0","0","13","Flag table","0","5","Operational"
1013.00,"21","BUFR/CREX Radar data","021068","Radar altimeter product confidence data",,"Flag table","0","0","8","Flag table","0","3","Operational"
1014.00,"21","BUFR/CREX Radar data","021069","SST product confidence data",,"Flag table","0","0","10","Flag table","0","4","Operational"
1015.00,"21","BUFR/CREX Radar data","021070","SST product confidence data (SADIST-2)",,"Flag table","0","0","23","Flag table","0","6","Operational"
1016.00,"21","BUFR/CREX Radar data","021071","Peakiness",,"Numeric","0","0","16","Numeric","0","5","Operational"
1017.00,"21","BUFR/CREX Radar data","021072","Satellite altimeter calibration status",,"Flag table","0","0","4","Flag table","0","2","Operational"
1018.00,"21","BUFR/CREX Radar data","021073","Satellite altimeter instrument mode",,"Flag table","0","0","9","Flag table","0","3","Operational"
1019.00,"21","BUFR/CREX Radar data","021075","Image spectrum intensity",,"Numeric","0","0","8","Numeric","0","3","Operational"
1020.00,"21","BUFR/CREX Radar data","021076","Representation of intensities",,"Code table","0","0","3","Code table","0","1","Operational"
1021.00,"21","BUFR/CREX Radar data","021077","Altitude correction (ionosphere)",,"m","3","0","14","m","3","5","Operational"
1022.00,"21","BUFR/CREX Radar data","021078","Altitude correction (dry troposphere)",,"m","3","0","9","m","3","3","Operational"
1023.00,"21","BUFR/CREX Radar data","021079","Altitude correction (wet troposphere)",,"m","3","2000","10","m","3","4","Operational"
1024.00,"21","BUFR/CREX Radar data","021080","Altitude correction (calibration constant)",,"m","3","0","11","m","3","4","Operational"
1025.00,"21","BUFR/CREX Radar data","021081","Open loop correction (height-time loop)",,"m","3","0","10","m","3","4","Operational"
1026.00,"21","BUFR/CREX Radar data","021082","Open loop correction (auto gain control)",,"dB","3","-3000","14","dB","3","5","Operational"
1027.00,"21","BUFR/CREX Radar data","021083","Warm target calibration",,"Numeric","0","0","16","Numeric","0","5","Operational"
1028.00,"21","BUFR/CREX Radar data","021084","Cold target calibration",,"Numeric","0","0","16","Numeric","0","5","Operational"
1029.00,"21","BUFR/CREX Radar data","021085","ATSR sea-surface temperature across-track band number",,"Numeric","0","0","4","Numeric","0","2","Operational"
1030.00,"21","BUFR/CREX Radar data","021086","Number of pixels in nadir only, average",,"Numeric","0","0","9","Numeric","0","3","Operational"
1031.00,"21","BUFR/CREX Radar data","021087","Number of pixels in dual view, average",,"Numeric","0","0","9","Numeric","0","3","Operational"
1032.00,"21","BUFR/CREX Radar data","021088","Wet backscatter",,"dB","2","-5000","13","dB","2","4","Operational"
1033.00,"21","BUFR/CREX Radar data","021091","Radar signal Doppler spectrum 0th moment",,"dB","0","-100","8","dB","0","3","Operational"
1034.00,"21","BUFR/CREX Radar data","021092","RASS signal Doppler spectrum 0th moment, referring to RASS signal",,"dB","0","-100","8","dB","0","3","Operational"
1035.00,"21","BUFR/CREX Radar data","021093","Ku band peakiness",,"Numeric","3","0","16","Numeric","3","5","Operational"
1036.00,"21","BUFR/CREX Radar data","021094","S band peakiness",,"Numeric","3","0","16","Numeric","3","5","Operational"
1037.00,"21","BUFR/CREX Radar data","021101","Number of vector ambiguities",,"Numeric","0","0","3","Numeric","0","1","Operational"
1038.00,"21","BUFR/CREX Radar data","021102","Index of selected wind vector",,"Numeric","0","0","3","Numeric","0","1","Operational"
1039.00,"21","BUFR/CREX Radar data","021103","Total number of sigma-0 measurements",,"Numeric","0","0","5","Numeric","0","2","Operational"
1040.00,"21","BUFR/CREX Radar data","021104","Likelihood computed for solution",,"Numeric","3","-30000","15","Numeric","3","5","Operational"
1041.00,"21","BUFR/CREX Radar data","021105","Normalized radar cross-section",,"dB","2","-10000","14","dB","2","5","Operational"
1042.00,"21","BUFR/CREX Radar data","021106","Kp variance coefficient (alpha)",,"Numeric","3","0","14","Numeric","3","5","Operational"
1043.00,"21","BUFR/CREX Radar data","021107","Kp variance coefficient (beta)",,"Numeric","8","0","16","Numeric","8","5","Operational"
1044.00,"21","BUFR/CREX Radar data","021109","SEAWINDS wind vector cell quality",,"Flag table","0","0","17","Flag table","0","6","Operational"
1045.00,"21","BUFR/CREX Radar data","021110","Number of inner-beam sigma-0 (forward of satellite)",,"Numeric","0","0","6","Numeric","0","2","Operational"
1046.00,"21","BUFR/CREX Radar data","021111","Number of outer-beam sigma-0 (forward of satellite)",,"Numeric","0","0","6","Numeric","0","2","Operational"
1047.00,"21","BUFR/CREX Radar data","021112","Number of inner-beam sigma-0 (aft of satellite)",,"Numeric","0","0","6","Numeric","0","2","Operational"
1048.00,"21","BUFR/CREX Radar data","021113","Number of outer-beam sigma-0 (aft of satellite)",,"Numeric","0","0","6","Numeric","0","2","Operational"
1049.00,"21","BUFR/CREX Radar data","021114","Kp variance coefficient (gamma)",,"dB","3","-140000","18","dB","3","6","Operational"
1050.00,"21","BUFR/CREX Radar data","021115","SEAWINDS sigma-0 quality",,"Flag table","0","0","17","Flag table","0","6","Operational"
1051.00,"21","BUFR/CREX Radar data","021116","SEAWINDS sigma-0 mode",,"Flag table","0","0","17","Flag table","0","6","Operational"
1052.00,"21","BUFR/CREX Radar data","021117","Sigma-0 variance quality control",,"Numeric","2","0","16","Numeric","2","5","Operational"
1053.00,"21","BUFR/CREX Radar data","021118","Attenuation correction on sigma-0",,"dB","2","-10000","14","dB","2","5","Operational"
1054.00,"21","BUFR/CREX Radar data","021119","Wind scatterometer geophysical model function",,"Code table","0","0","6","Code table","0","2","Operational"
1055.00,"21","BUFR/CREX Radar data","021120","Probability of rain",,"Numeric","3","0","10","Numeric","3","4","Operational"
1056.00,"21","BUFR/CREX Radar data","021121","SEAWINDS NOF rain index","*","Numeric","0","0","8","Numeric","0","3","Operational"
1057.00,"21","BUFR/CREX Radar data","021122","Attenuation correction on sigma-0 (from tB)",,"dB","2","-10000","14","dB","2","5","Operational"
1058.00,"21","BUFR/CREX Radar data","021123","SEAWINDS normalized radar cross-section",,"dB","2","-30000","15","dB","2","5","Operational"
1059.00,"21","BUFR/CREX Radar data","021128","Number of valid points per second used to derive previous parameters",,"Numeric","0","0","8","Numeric","0","3","Operational"
1060.00,"21","BUFR/CREX Radar data","021130","Spectrum total energy",,"Numeric","6","0","28","Numeric","6","9","Operational"
1061.00,"21","BUFR/CREX Radar data","021131","Spectrum max energy",,"Numeric","6","0","28","Numeric","6","9","Operational"
1062.00,"21","BUFR/CREX Radar data","021132","Direction of spectrum max on higher resolution grid",,"deg","3","0","19","deg","3","6","Operational"
1063.00,"21","BUFR/CREX Radar data","021133","Wavelength of spectrum max on higher resolution grid",,"m","3","0","29","m","3","9","Operational"
1064.00,"21","BUFR/CREX Radar data","021134","Range resolution of cress covariance spectrum",,"rad/m","3","0","19","rad/m","3","6","Operational"
1065.00,"21","BUFR/CREX Radar data","021135","Real part of cross spectra polar grid number of bins",,"Numeric","3","-524288","20","Numeric","3","7","Operational"
1066.00,"21","BUFR/CREX Radar data","021136","Imaginary part of cross spectra polar grid number of bins",,"Numeric","3","-524288","20","Numeric","3","7","Operational"
1067.00,"21","BUFR/CREX Radar data","021137","Ku band corrected ocean backscatter coefficient",,"dB","2","-32768","16","dB","2","5","Operational"
1068.00,"21","BUFR/CREX Radar data","021138","Std Ku band corrected ocean backscatter coefficient",,"dB","2","-32768","16","dB","2","5","Operational"
1069.00,"21","BUFR/CREX Radar data","021139","Ku band net instrumental correction for AGC",,"dB","2","-2048","12","dB","2","4","Operational"
1070.00,"21","BUFR/CREX Radar data","021140","S band corrected ocean backscatter coefficient",,"dB","2","-32768","16","dB","2","5","Operational"
1071.00,"21","BUFR/CREX Radar data","021141","Std S band corrected ocean backscatter coefficient",,"dB","2","-32768","16","dB","2","5","Operational"
1072.00,"21","BUFR/CREX Radar data","021142","S band net instrumental correction for AGC",,"dB","2","-1024","11","dB","2","4","Operational"
1073.00,"21","BUFR/CREX Radar data","021143","Ku band rain attenuation",,"dB","2","-1073741824","31","dB","2","10","Operational"
1074.00,"21","BUFR/CREX Radar data","021144","Altimeter rain flag",,"Flag table","0","0","2","Flag table","0","1","Operational"
1075.00,"21","BUFR/CREX Radar data","021145","Ku band automatic gain control",,"dB","2","0","13","dB","2","4","Operational"
1076.00,"21","BUFR/CREX Radar data","021146","RMS Ku band automatic gain control",,"dB","2","0","8","dB","2","3","Operational"
1077.00,"21","BUFR/CREX Radar data","021147","Number of valid points for Ku band automatic gain control",,"Numeric","0","0","5","Numeric","0","2","Operational"
1078.00,"21","BUFR/CREX Radar data","021148","Trailing edge variation flag",,"Flag table","0","0","9","Flag table","0","3","Operational"
1079.00,"21","BUFR/CREX Radar data","021150","Beam collocation",,"Code table","0","0","2","Code table","0","1","Operational"
1080.00,"21","BUFR/CREX Radar data","021151","Estimated error in sigma-0 at 40 degrees incidence angle",,"dB","2","0","9","dB","2","3","Operational"
1081.00,"21","BUFR/CREX Radar data","021152","Slope at 40 degrees incidence angle",,"dB/deg","2","-80","7","dB/deg","2","2","Operational"
1082.00,"21","BUFR/CREX Radar data","021153","Estimated error in slope at 40 degrees incidence angle",,"dB/deg","2","-40","6","dB/deg","2","2","Operational"
1083.00,"21","BUFR/CREX Radar data","021154","Soil moisture sensitivity",,"dB","2","0","12","dB","2","4","Operational"
1084.00,"21","BUFR/CREX Radar data","021155","Wind vector cell quality",,"Flag table","0","0","24","Flag table","0","8","Operational"
1085.00,"21","BUFR/CREX Radar data","021156","Backscatter distance",,"Numeric","1","-4096","13","Numeric","1","4","Operational"
1086.00,"21","BUFR/CREX Radar data","021157","Loss per unit length of atmosphere used",,"dB/m","10","0","22","dB/m","10","7","Operational"
1087.00,"21","BUFR/CREX Radar data","021158","ASCAT Kp estimate quality",,"Code table","0","0","2","Code table","0","1","Operational"
1088.00,"21","BUFR/CREX Radar data","021159","ASCAT sigma-0 usability",,"Code table","0","0","2","Code table","0","1","Operational"
1089.00,"21","BUFR/CREX Radar data","021160","ASCAT use of synthetic data",,"Numeric","3","0","10","Numeric","3","4","Operational"
1090.00,"21","BUFR/CREX Radar data","021161","ASCAT synthetic data quantity",,"Numeric","3","0","10","Numeric","3","4","Operational"
1091.00,"21","BUFR/CREX Radar data","021162","ASCAT satellite orbit and attitude quality",,"Numeric","3","0","10","Numeric","3","4","Operational"
1092.00,"21","BUFR/CREX Radar data","021163","ASCAT solar array reflection contamination",,"Numeric","3","0","10","Numeric","3","4","Operational"
1093.00,"21","BUFR/CREX Radar data","021164","ASCAT telemetry presence and quality",,"Numeric","3","0","10","Numeric","3","4","Operational"
1094.00,"21","BUFR/CREX Radar data","021165","ASCAT extrapolated reference function presence",,"Numeric","3","0","10","Numeric","3","4","Operational"
1095.00,"21","BUFR/CREX Radar data","021166","Land fraction",,"Numeric","3","0","10","Numeric","3","4","Operational"
1096.00,"21","BUFR/CREX Radar data","021169","Ice presence indicator",,"Code table","0","0","2","Code table","0","1","Operational"
1097.00,"21","BUFR/CREX Radar data","021170","C band corrected ocean backscatter coefficient",,"dB","2","-32768","16","dB","2","5","Operational"
1098.00,"21","BUFR/CREX Radar data","021171","RMS C band corrected ocean backscatter coefficient",,"dB","2","-32768","16","dB","2","5","Operational"
1099.00,"21","BUFR/CREX Radar data","021172","C band net instrumental correction for AGC",,"dB","2","-2048","12","dB","2","4","Operational"
1100.00,"21","BUFR/CREX Radar data","021173","C band automatic gain control",,"dB","2","0","13","dB","2","4","Operational"
1101.00,"21","BUFR/CREX Radar data","021174","RMS C band automatic gain control",,"dB","2","0","9","dB","2","3","Operational"
1102.00,"21","BUFR/CREX Radar data","021175","Number of valid points for C band automatic gain control",,"Numeric","0","0","10","Numeric","0","4","Operational"
1103.00,"21","BUFR/CREX Radar data","021176","High frequency variability correction",,"m","3","0","16","m","3","5","Operational"
1104.00,"21","BUFR/CREX Radar data","021177","Corrected OCOG backscatter coefficient",,"dB","2","0","16","dB","2","5","Operational"
1105.00,"21","BUFR/CREX Radar data","021178","STD of 20 Hz OCOG backscatter coefficient",,"dB","2","0","16","dB","2","5","Operational"
1106.00,"21","BUFR/CREX Radar data","021179","Number of 20 Hz valid points for OCOG backscatter coefficient",,"Numeric","0","0","16","Numeric","0","5","Operational"
1107.00,"21","BUFR/CREX Radar data","021180","Number of 20 Hz valid points for ocean backscatter coefficient",,"Numeric","0","0","8","Numeric","0","3","Operational"
1108.00,"21","BUFR/CREX Radar data","021181","20 Hz ocean backscatter coefficient",,"dB","2","0","16","dB","2","5","Operational"
1109.00,"21","BUFR/CREX Radar data","021182","20 Hz Ku band peakiness",,"Numeric","3","0","16","Numeric","3","5","Operational"
1110.00,"21","BUFR/CREX Radar data","021183","Specific band corrected ocean backscatter coefficient",,"dB","2","-32768","16","dB","2","5","Operational"
1111.00,"21","BUFR/CREX Radar data","021184","STD specific band corrected ocean backscatter coefficient",,"dB","2","-32768","16","dB","2","5","Operational"
1112.00,"21","BUFR/CREX Radar data","021185","Specific band net instrumental correction for agc",,"dB","2","-2048","12","dB","2","4","Operational"
1113.00,"21","BUFR/CREX Radar data","021186","Specific band automatic gain control",,"dB","2","0","13","dB","2","4","Operational"
1114.00,"21","BUFR/CREX Radar data","021187","RMS specific band automatic gain control",,"dB","2","0","8","dB","2","3","Operational"
1115.00,"21","BUFR/CREX Radar data","021188","Number of valid points for specific band automatic gain control",,"Numeric","0","0","7","Numeric","0","3","Operational"
1116.00,"22","BUFR/CREX Oceanographic elements","022001","Direction of waves",,"degree true","0","0","9","degree true","0","3","Operational"
1117.00,"22","BUFR/CREX Oceanographic elements","022002","Direction of wind waves",,"degree true","0","0","9","degree true","0","3","Operational"
1118.00,"22","BUFR/CREX Oceanographic elements","022003","Direction of swell waves",,"degree true","0","0","9","degree true","0","3","Operational"
1119.00,"22","BUFR/CREX Oceanographic elements","022004","Direction of current","(see Note 7)","degree true","0","0","9","degree true","0","3","Operational"
1120.00,"22","BUFR/CREX Oceanographic elements","022005","Direction of sea-surface current",,"degree true","0","0","9","degree true","0","3","Operational"
1121.00,"22","BUFR/CREX Oceanographic elements","022011","Period of waves",,"s","0","0","6","s","0","2","Operational"
1122.00,"22","BUFR/CREX Oceanographic elements","022012","Period of wind waves",,"s","0","0","6","s","0","2","Operational"
1123.00,"22","BUFR/CREX Oceanographic elements","022013","Period of swell waves",,"s","0","0","6","s","0","2","Operational"
1124.00,"22","BUFR/CREX Oceanographic elements","022021","Height of waves",,"m","1","0","10","m","1","4","Operational"
1125.00,"22","BUFR/CREX Oceanographic elements","022022","Height of wind waves",,"m","1","0","10","m","1","4","Operational"
1126.00,"22","BUFR/CREX Oceanographic elements","022023","Height of swell waves",,"m","1","0","10","m","1","4","Operational"
1127.00,"22","BUFR/CREX Oceanographic elements","022025","Standard deviation wave height",,"m","2","0","10","m","2","4","Operational"
1128.00,"22","BUFR/CREX Oceanographic elements","022026","Standard deviation of significant wave height",,"m","2","0","10","m","2","4","Operational"
1129.00,"22","BUFR/CREX Oceanographic elements","022031","Speed of current",,"m/s","2","0","13","m/s","2","4","Operational"
1130.00,"22","BUFR/CREX Oceanographic elements","022032","Speed of sea-surface current",,"m/s","2","0","13","m/s","2","4","Operational"
1131.00,"22","BUFR/CREX Oceanographic elements","022035","Tidal elevation with respect to local chart datum",,"m","2","0","14","m","2","4","Operational"
1132.00,"22","BUFR/CREX Oceanographic elements","022036","Meteorological residual tidal elevation (surge or offset)",,"m","2","0","14","m","2","4","Operational"
1133.00,"22","BUFR/CREX Oceanographic elements","022037","Tidal elevation with respect to national land datum",,"m","3","-10000","15","m","3","5","Operational"
1134.00,"22","BUFR/CREX Oceanographic elements","022038","Tidal elevation with respect to local chart datum",,"m","3","-10000","15","m","3","5","Operational"
1135.00,"22","BUFR/CREX Oceanographic elements","022039","Meteorological residual tidal elevation (surge or offset)","(see Note 4)","m","3","-5000","13","m","3","4","Operational"
1136.00,"22","BUFR/CREX Oceanographic elements","022040","Meteorological residual tidal elevation (surge or offset)","(see Note 4)","m","3","-5000","14","m","3","5","Operational"
1137.00,"22","BUFR/CREX Oceanographic elements","022041","Sea-surface temperature (15-day running mean)",,"K","1","0","12","K","1","4","Operational"
1138.00,"22","BUFR/CREX Oceanographic elements","022042","Sea/water temperature",,"K","1","0","12","K","1","4","Operational"
1139.00,"22","BUFR/CREX Oceanographic elements","022043","Sea/water temperature",,"K","2","0","15","K","2","5","Operational"
1140.00,"22","BUFR/CREX Oceanographic elements","022044","Sound velocity",,"m/s","1","0","14","m/s","1","5","Operational"
1141.00,"22","BUFR/CREX Oceanographic elements","022045","Sea/water temperature",,"K","3","0","19","K","3","6","Operational"
1142.00,"22","BUFR/CREX Oceanographic elements","022046","Sea ice fraction",,"Numeric","2","0","7","Numeric","2","3","Operational"
1143.00,"22","BUFR/CREX Oceanographic elements","022049","Sea-surface temperature",,"K","2","0","15","K","2","5","Operational"
1144.00,"22","BUFR/CREX Oceanographic elements","022050","Standard deviation sea-surface temperature",,"K","2","0","8","K","2","3","Operational"
1145.00,"22","BUFR/CREX Oceanographic elements","022055","Float cycle number",,"Numeric","0","0","10","Numeric","0","3","Operational"
1146.00,"22","BUFR/CREX Oceanographic elements","022056","Direction of profile",,"Code table","0","0","2","Code table","0","1","Operational"
1147.00,"22","BUFR/CREX Oceanographic elements","022059","Sea-surface salinity",,"0/00","2","0","14","0/00","2","5","Operational"
1148.00,"22","BUFR/CREX Oceanographic elements","022060","Lagrangian drifter drogue status",,"Code table","0","0","3","Code table","0","1","Operational"
1149.00,"22","BUFR/CREX Oceanographic elements","022061","State of the sea",,"Code table","0","0","4","Code table","0","2","Operational"
1150.00,"22","BUFR/CREX Oceanographic elements","022062","Salinity",,"0/00","2","0","14","0/00","2","5","Operational"
1151.00,"22","BUFR/CREX Oceanographic elements","022063","Total water depth",,"m","0","0","14","m","0","5","Operational"
1152.00,"22","BUFR/CREX Oceanographic elements","022064","Salinity",,"0/00","3","0","17","0/00","3","6","Operational"
1153.00,"22","BUFR/CREX Oceanographic elements","022065","Water pressure",,"Pa","-3","0","17","Pa","-3","6","Operational"
1154.00,"22","BUFR/CREX Oceanographic elements","022066","Water conductivity",,"S/m","6","0","26","S/m","6","8","Operational"
1155.00,"22","BUFR/CREX Oceanographic elements","022067","Instrument type for water temperature/salinity profile measurement",,"Code table","0","0","10","Code table","0","4","Operational"
1156.00,"22","BUFR/CREX Oceanographic elements","022068","Water temperature profile recorder types",,"Code table","0","0","7","Code table","0","3","Operational"
1157.00,"22","BUFR/CREX Oceanographic elements","022069","Spectral wave density",,"m2/Hz","3","0","22","m2/Hz","3","7","Operational"
1158.00,"22","BUFR/CREX Oceanographic elements","022070","Significant wave height",,"m","2","0","13","m","2","4","Operational"
1159.00,"22","BUFR/CREX Oceanographic elements","022071","Spectral peak wave period",,"s","1","0","9","s","1","3","Operational"
1160.00,"22","BUFR/CREX Oceanographic elements","022072","Spectral peak wave length",,"m","0","0","13","m","0","4","Operational"
1161.00,"22","BUFR/CREX Oceanographic elements","022073","Maximum wave height",,"m","2","0","13","m","2","4","Operational"
1162.00,"22","BUFR/CREX Oceanographic elements","022074","Average wave period",,"s","1","0","9","s","1","3","Operational"
1163.00,"22","BUFR/CREX Oceanographic elements","022075","Average wave length",,"m","0","0","13","m","0","4","Operational"
1164.00,"22","BUFR/CREX Oceanographic elements","022076","Direction from which dominant waves are coming",,"degree true","0","0","9","degree true","0","3","Operational"
1165.00,"22","BUFR/CREX Oceanographic elements","022077","Directional spread of dominant wave",,"deg","0","0","9","deg","0","3","Operational"
1166.00,"22","BUFR/CREX Oceanographic elements","022078","Duration of wave record",,"s","0","0","12","s","0","4","Operational"
1167.00,"22","BUFR/CREX Oceanographic elements","022079","Length of wave record",,"m","0","0","16","m","0","5","Operational"
1168.00,"22","BUFR/CREX Oceanographic elements","022080","Waveband central frequency",,"Hz","3","0","10","Hz","3","4","Operational"
1169.00,"22","BUFR/CREX Oceanographic elements","022081","Waveband central wave number",,"/m","5","0","13","/m","5","4","Operational"
1170.00,"22","BUFR/CREX Oceanographic elements","022082","Maximum non-directional spectral wave density",,"m2 s","2","0","20","m2 s","2","7","Operational"
1171.00,"22","BUFR/CREX Oceanographic elements","022083","Maximum non-directional spectral wave number",,"m3","2","0","20","m3","2","7","Operational"
1172.00,"22","BUFR/CREX Oceanographic elements","022084","Band containing maximum non-directional spectral wave density",,"Numeric","0","0","7","Numeric","0","3","Operational"
1173.00,"22","BUFR/CREX Oceanographic elements","022085","Spectral wave density ratio",,"Numeric","0","0","7","Numeric","0","3","Operational"
1174.00,"22","BUFR/CREX Oceanographic elements","022086","Mean direction from which waves are coming",,"degree true","0","0","9","degree true","0","3","Operational"
1175.00,"22","BUFR/CREX Oceanographic elements","022087","Principal direction from which waves are coming",,"degree true","0","0","9","degree true","0","3","Operational"
1176.00,"22","BUFR/CREX Oceanographic elements","022088","First normalized polar coordinate from Fourier coefficients",,"Numeric","2","0","7","Numeric","2","3","Operational"
1177.00,"22","BUFR/CREX Oceanographic elements","022089","Second normalized polar coordinate from Fourier coefficients",,"Numeric","2","0","7","Numeric","2","3","Operational"
1178.00,"22","BUFR/CREX Oceanographic elements","022090","Non-directional spectral estimate by wave frequency",,"m2 s","2","0","20","m2 s","2","7","Operational"
1179.00,"22","BUFR/CREX Oceanographic elements","022091","Non-directional spectral estimate by wave number",,"m3","2","0","20","m3","2","7","Operational"
1180.00,"22","BUFR/CREX Oceanographic elements","022092","Directional spectral estimate by wave frequency",,"m2 rad-1 s","2","0","20","m2 rad-1 s","2","7","Operational"
1181.00,"22","BUFR/CREX Oceanographic elements","022093","Directional spectral estimate by wave number",,"m4","2","0","20","m4","2","7","Operational"
1182.00,"22","BUFR/CREX Oceanographic elements","022094","Total number of wave bands",,"Numeric","0","0","7","Numeric","0","3","Operational"
1183.00,"22","BUFR/CREX Oceanographic elements","022095","Directional spread of individual waves",,"deg","0","0","8","deg","0","3","Operational"
1184.00,"22","BUFR/CREX Oceanographic elements","022096","Spectral band width",,"/s","3","0","4","/s","3","2","Operational"
1185.00,"22","BUFR/CREX Oceanographic elements","022097","Mean wavelength > 731 m of image spectrum at low wave numbers",,"m","0","0","14","m","0","5","Operational"
1186.00,"22","BUFR/CREX Oceanographic elements","022098","Wavelength spread (wavelength > 731 m) at low wave numbers",,"m","0","0","14","m","0","5","Operational"
1187.00,"22","BUFR/CREX Oceanographic elements","022099","Mean direction at low wave numbers (wavelength > 731 m)",,"degree true","0","0","9","degree true","0","3","Operational"
1188.00,"22","BUFR/CREX Oceanographic elements","022100","Direction spread at low wave numbers (wavelength > 731 m)",,"deg","0","0","9","deg","0","3","Operational"
1189.00,"22","BUFR/CREX Oceanographic elements","022101","Total energy (wavelength > 731m) at low wave numbers",,"Numeric","0","0","31","Numeric","0","10","Operational"
1190.00,"22","BUFR/CREX Oceanographic elements","022120","Tide station automated water level check",,"Code table","0","0","5","Code table","0","2","Operational"
1191.00,"22","BUFR/CREX Oceanographic elements","022121","Tide station manual water level check",,"Code table","0","0","5","Code table","0","2","Operational"
1192.00,"22","BUFR/CREX Oceanographic elements","022122","Tide station automated meteorological data check",,"Code table","0","0","5","Code table","0","2","Operational"
1193.00,"22","BUFR/CREX Oceanographic elements","022123","Tide station manual meteorological data check",,"Code table","0","0","5","Code table","0","2","Operational"
1194.00,"22","BUFR/CREX Oceanographic elements","022130","Number of valid points for specific band",,"Numeric","0","0","10","Numeric","0","4","Operational"
1195.00,"22","BUFR/CREX Oceanographic elements","022131","RMS specific band significant wave height",,"m","3","0","16","m","3","5","Operational"
1196.00,"22","BUFR/CREX Oceanographic elements","022132","Number of valid points for specific band significant wave height",,"Numeric","0","0","10","Numeric","0","4","Operational"
1197.00,"22","BUFR/CREX Oceanographic elements","022133","Specific band net instrument correction for signficant wave height",,"m","3","-1000","11","m","3","4","Operational"
1198.00,"22","BUFR/CREX Oceanographic elements","022134","Number of valid points for specific band backscatter",,"Numeric","0","0","10","Numeric","0","4","Operational"
1199.00,"22","BUFR/CREX Oceanographic elements","022141","Sea-surface temperature (15-day running mean)",,"K","2","0","15","K","2","5","Operational"
1200.00,"22","BUFR/CREX Oceanographic elements","022142","Square of significant wave height",,"m2","3","-33554432  ","26","m2","3","8","Operational"
1201.00,"22","BUFR/CREX Oceanographic elements","022143","STD of 20 Hz SWH squared",,"m2","3","-8388608","24","m2","3","8","Operational"
1202.00,"22","BUFR/CREX Oceanographic elements","022144","Number of 20 Hz valid points for SWH-squared",,"Numeric","0","0","9","Numeric","0","3","Operational"
1203.00,"22","BUFR/CREX Oceanographic elements","022145","STD of 20 Hz ocean range",,"m","3","-33554432  ","31","m","3","10","Operational"
1204.00,"22","BUFR/CREX Oceanographic elements","022146","OCOG range",,"m","3","0","31","m","3","10","Operational"
1205.00,"22","BUFR/CREX Oceanographic elements","022147","STD of 20 Hz OCOG range",,"m","3","-8388608","31","m","3","10","Operational"
1206.00,"22","BUFR/CREX Oceanographic elements","022148","Number of 20 Hz valid points for ocean range",,"Numeric","0","0","9","Numeric","0","3","Operational"
1207.00,"22","BUFR/CREX Oceanographic elements","022149","20 Hz significant wave height squared",,"m2","3","-33554432  ","26","m2","3","8","Operational"
1208.00,"22","BUFR/CREX Oceanographic elements","022150","Number of 18 Hz valid points for Ku band",,"Numeric","0","0","10","Numeric","0","4","Operational"
1209.00,"22","BUFR/CREX Oceanographic elements","022151","Ku band ocean range",,"m","3","0","31","m","3","10","Operational"
1210.00,"22","BUFR/CREX Oceanographic elements","022152","STD of 18 Hz Ku band ocean range",,"m","3","0","16","m","3","5","Operational"
1211.00,"22","BUFR/CREX Oceanographic elements","022153","Number of 18 Hz valid points for S band",,"Numeric","0","0","10","Numeric","0","4","Operational"
1212.00,"22","BUFR/CREX Oceanographic elements","022154","S band ocean range",,"m","3","0","31","m","3","10","Operational"
1213.00,"22","BUFR/CREX Oceanographic elements","022155","STD of 18 Hz S band ocean range",,"m","3","0","16","m","3","5","Operational"
1214.00,"22","BUFR/CREX Oceanographic elements","022156","Ku band significant wave height",,"m","3","0","16","m","3","5","Operational"
1215.00,"22","BUFR/CREX Oceanographic elements","022157","STD of 18 Hz Ku band ocean range",,"m","3","0","16","m","3","5","Operational"
1216.00,"22","BUFR/CREX Oceanographic elements","022158","S band significant wave height",,"m","3","0","16","m","3","5","Operational"
1217.00,"22","BUFR/CREX Oceanographic elements","022159","STD of 18 Hz S band significant wave height",,"m","3","0","16","m","3","5","Operational"
1218.00,"22","BUFR/CREX Oceanographic elements","022160","Normalized inverse wave age",,"Numeric","6","0","21","Numeric","6","7","Operational"
1219.00,"22","BUFR/CREX Oceanographic elements","022161","Wave spectra",,"m4","4","0","27","m4","4","9","Operational"
1220.00,"22","BUFR/CREX Oceanographic elements","022162","RMS of 20 Hz Ku band ocean range",,"m","3","0","16","m","3","5","Operational"
1221.00,"22","BUFR/CREX Oceanographic elements","022163","Number of 20 Hz valid points for Ku band",,"Numeric","0","0","10","Numeric","0","4","Operational"
1222.00,"22","BUFR/CREX Oceanographic elements","022164","RMS 20 Hz Ku band significant wave height",,"m","3","0","16","m","3","5","Operational"
1223.00,"22","BUFR/CREX Oceanographic elements","022165","Number of 20 Hz valid points for Ku band significant wave height",,"Numeric","0","0","10","Numeric","0","4","Operational"
1224.00,"22","BUFR/CREX Oceanographic elements","022166","Ku band net instrumental correction for significant wave height",,"m","3","-1000","11","m","3","4","Operational"
1225.00,"22","BUFR/CREX Oceanographic elements","022167","Number of valid points for Ku band backscatter",,"Numeric","0","0","10","Numeric","0","4","Operational"
1226.00,"22","BUFR/CREX Oceanographic elements","022168","C band ocean range",,"m","3","0","31","m","3","10","Operational"
1227.00,"22","BUFR/CREX Oceanographic elements","022169","RMS of C band ocean range",,"m","3","0","16","m","3","5","Operational"
1228.00,"22","BUFR/CREX Oceanographic elements","022170","Number of 20 Hz valid points for C band",,"Numeric","0","0","10","Numeric","0","4","Operational"
1229.00,"22","BUFR/CREX Oceanographic elements","022171","C band significant wave height",,"m","3","0","16","m","3","5","Operational"
1230.00,"22","BUFR/CREX Oceanographic elements","022172","RMS 20 Hz C band significant wave height",,"m","3","0","16","m","3","5","Operational"
1231.00,"22","BUFR/CREX Oceanographic elements","022173","Number of 20 Hz valid points for C band significant wave height",,"Numeric","0","0","10","Numeric","0","4","Operational"
1232.00,"22","BUFR/CREX Oceanographic elements","022174","C band net instrumental correction for significant wave height",,"m","3","-1000","11","m","3","4","Operational"
1233.00,"22","BUFR/CREX Oceanographic elements","022175","Number of valid points for C band backscatter",,"Numeric","0","0","10","Numeric","0","4","Operational"
1234.00,"22","BUFR/CREX Oceanographic elements","022177","Height of XBT/XCTD launcher",,"m","0","0","6","m","0","3","Operational"
1235.00,"22","BUFR/CREX Oceanographic elements","022178","XBT/XCTD launcher type",,"Code table","0","0","8","Code table","0","3","Operational"
1239.00,"22","BUFR/CREX Oceanographic elements","022182","Water column height","(see Note 9)","m","3","0","23","m","3","7","Operational"
1240.00,"22","BUFR/CREX Oceanographic elements","022184","Water column height deviation from the reference value",,"m","3","-2000","12","m","3","4","Operational"
1241.00,"22","BUFR/CREX Oceanographic elements","022185","BPR transmission count",,"Numeric","0","0","10","Numeric","0","3","Operational"
1244.00,"22","BUFR/CREX Oceanographic elements","022188","Dissolved oxygen",,"umol/kg","3","0","19","umol/kg","3","6","Operational"
1245.00,"22","BUFR/CREX Oceanographic elements","022189","Specific band ocean range",,"m","3","0","31","m","3","10","Operational"
1246.00,"22","BUFR/CREX Oceanographic elements","022190","Specific band significant wave height",,"m","3","0","16","m","3","5","Operational"
1247.00,"22","BUFR/CREX Oceanographic elements","022191","RMS of specific band ocean range",,"m","4","0","16","m","4","5","Operational"
1248.00,"23","BUFR/CREX Dispersal and transport","023001","Accident early notification - article applicable",,"Code table","0","0","3","Code table","0","1","Operational"
1249.00,"23","BUFR/CREX Dispersal and transport","023002","Activity or facility involved in incident",,"Code table","0","0","5","Code table","0","2","Operational"
1250.00,"23","BUFR/CREX Dispersal and transport","023003","Type of release",,"Code table","0","0","3","Code table","0","1","Operational"
1251.00,"23","BUFR/CREX Dispersal and transport","023004","Countermeasures taken near border",,"Code table","0","0","3","Code table","0","1","Operational"
1252.00,"23","BUFR/CREX Dispersal and transport","023005","Cause of incident",,"Code table","0","0","2","Code table","0","1","Operational"
1253.00,"23","BUFR/CREX Dispersal and transport","023006","Incident situation",,"Code table","0","0","3","Code table","0","1","Operational"
1254.00,"23","BUFR/CREX Dispersal and transport","023007","Characteristics of release",,"Code table","0","0","3","Code table","0","1","Operational"
1255.00,"23","BUFR/CREX Dispersal and transport","023008","State of current release",,"Code table","0","0","2","Code table","0","1","Operational"
1256.00,"23","BUFR/CREX Dispersal and transport","023009","State of expected release",,"Code table","0","0","2","Code table","0","1","Operational"
1257.00,"23","BUFR/CREX Dispersal and transport","023016","Possibility of significant chemical toxic health effect",,"Code table","0","0","2","Code table","0","1","Operational"
1258.00,"23","BUFR/CREX Dispersal and transport","023017","Flow discharge of major recipient",,"m3/s","6","0","20","m3/s","6","7","Operational"
1259.00,"23","BUFR/CREX Dispersal and transport","023018","Release behaviour over time",,"Code table","0","0","3","Code table","0","1","Operational"
1260.00,"23","BUFR/CREX Dispersal and transport","023019","Actual release height",,"m","0","-15000","17","m","0","6","Operational"
1261.00,"23","BUFR/CREX Dispersal and transport","023021","Effective release height",,"m","0","-15000","17","m","0","6","Operational"
1262.00,"23","BUFR/CREX Dispersal and transport","023022","Distance of release point or site of incident",,"m","0","0","24","m","0","8","Operational"
1263.00,"23","BUFR/CREX Dispersal and transport","023023","Main transport speed in the atmosphere",,"m/s","1","0","12","m/s","1","4","Operational"
1264.00,"23","BUFR/CREX Dispersal and transport","023024","Main transport speed in water",,"m/s","2","0","13","m/s","2","4","Operational"
1265.00,"23","BUFR/CREX Dispersal and transport","023025","Main transport speed in ground water",,"m/s","2","0","13","m/s","2","4","Operational"
1266.00,"23","BUFR/CREX Dispersal and transport","023027","Main transport direction in the atmosphere",,"degree true","0","0","9","degree true","0","3","Operational"
1267.00,"23","BUFR/CREX Dispersal and transport","023028","Main transport direction in water",,"degree true","0","0","9","degree true","0","3","Operational"
1268.00,"23","BUFR/CREX Dispersal and transport","023029","Main transport direction in ground water",,"degree true","0","0","9","degree true","0","3","Operational"
1269.00,"23","BUFR/CREX Dispersal and transport","023031","Possibility that plume will encounter precipitation in State in which incident occurred",,"Code table","0","0","2","Code table","0","1","Operational"
1270.00,"23","BUFR/CREX Dispersal and transport","023032","Plume will encounter change in wind direction and/or speed flag",,"Code table","0","0","2","Code table","0","1","Operational"
1271.00,"23","BUFR/CREX Dispersal and transport","023040","Flow discharge - river",,"m3/s","1","0","22","m3/s","1","7","Operational"
1272.00,"23","BUFR/CREX Dispersal and transport","023041","Flow discharge - well",,"m3/s","3","0","16","m3/s","3","5","Operational"
1273.00,"24","BUFR/CREX Radiological elements","024001","Estimate of amount of radioactivity released up to specified time",,"Bq","-11","0","28","Bq","-11","9","Operational"
1274.00,"24","BUFR/CREX Radiological elements","024002","Estimated maximum potential release",,"Bq","-11","0","28","Bq","-11","9","Operational"
1275.00,"24","BUFR/CREX Radiological elements","024003","Composition of release",,"Code table","0","0","5","Code table","0","2","Operational"
1276.00,"24","BUFR/CREX Radiological elements","024004","Element name",,"CCITT IA5","0","0","16","Character","0","2","Operational"
1277.00,"24","BUFR/CREX Radiological elements","024005","Isotope mass",,"Numeric","0","0","9","Numeric","0","3","Operational"
1278.00,"24","BUFR/CREX Radiological elements","024011","Dose","*","mSv","2","0","32","mSv","2","10","Operational"
1279.00,"24","BUFR/CREX Radiological elements","024012","Trajectory dose (defined location and expected time of arrival)",,"mSv","2","0","32","mSv","2","10","Operational"
1280.00,"24","BUFR/CREX Radiological elements","024013","Gamma dose in air along the main transport path (defined location and time period)",,"mSv","2","0","32","mSv","2","10","Operational"
1281.00,"24","BUFR/CREX Radiological elements","024014","Gamma radiation dose rate","(see Note 2)","nSv/h","1","0","14","nSv/h","1","4","Operational"
1282.00,"24","BUFR/CREX Radiological elements","024021","Air concentration (of named isotope type including gross beta)",,"Bq m-3","2","0","32","Bq m-3","2","10","Operational"
1283.00,"24","BUFR/CREX Radiological elements","024022","Concentration in precipitation (of named isotope type)",,"Bq/l","2","0","32","Bq/l","2","10","Operational"
1284.00,"24","BUFR/CREX Radiological elements","024023","Pulse rate of beta radiation",,"/s","1","0","14","/s","1","4","Operational"
1285.00,"24","BUFR/CREX Radiological elements","024024","Pulse rate of gamma radiation",,"/s","1","0","14","/s","1","4","Operational"
1286.00,"25","BUFR/CREX Processing information","025001","Range-gate length",,"m","-1","0","6","m","-1","2","Operational"
1287.00,"25","BUFR/CREX Processing information","025002","Number of gates averaged",,"Numeric","0","0","4","Numeric","0","2","Operational"
1288.00,"25","BUFR/CREX Processing information","025003","Number of integrated pulses",,"Numeric","0","0","8","Numeric","0","3","Operational"
1289.00,"25","BUFR/CREX Processing information","025004","Echo processing",,"Code table","0","0","2","Code table","0","1","Operational"
1290.00,"25","BUFR/CREX Processing information","025005","Echo integration",,"Code table","0","0","2","Code table","0","1","Operational"
1291.00,"25","BUFR/CREX Processing information","025006","Z to R conversion",,"Code table","0","0","3","Code table","0","1","Operational"
1292.00,"25","BUFR/CREX Processing information","025007","Z to R conversion factor",,"Numeric","0","0","12","Numeric","0","4","Operational"
1293.00,"25","BUFR/CREX Processing information","025008","Z to R conversion exponent",,"Numeric","2","0","9","Numeric","2","3","Operational"
1294.00,"25","BUFR/CREX Processing information","025009","Calibration method","(see Note 3)","Flag table","0","0","4","Flag table","0","2","Operational"
1295.00,"25","BUFR/CREX Processing information","025010","Clutter treatment",,"Code table","0","0","4","Code table","0","2","Operational"
1296.00,"25","BUFR/CREX Processing information","025011","Ground occultation correction (screening)",,"Code table","0","0","2","Code table","0","1","Operational"
1297.00,"25","BUFR/CREX Processing information","025012","Range attenuation correction",,"Code table","0","0","2","Code table","0","1","Operational"
1298.00,"25","BUFR/CREX Processing information","025013","Bright-band correction",,"Flag table","0","0","2","Flag table","0","1","Operational"
1299.00,"25","BUFR/CREX Processing information","025014","Azimuth clutter cut-off","(see Note 1)","Numeric","0","0","12","Numeric","0","4","Operational"
1300.00,"25","BUFR/CREX Processing information","025015","Radome attenuation correction",,"Flag table","0","0","2","Flag table","0","1","Operational"
1301.00,"25","BUFR/CREX Processing information","025016","Clear-air attenuation correction",,"dB/m","5","0","6","dB/m","5","2","Operational"
1302.00,"25","BUFR/CREX Processing information","025017","Precipitation attenuation correction",,"Flag table","0","0","2","Flag table","0","1","Operational"
1303.00,"25","BUFR/CREX Processing information","025018","A to Z law for attenuation factor",,"Numeric","7","0","6","Numeric","7","2","Operational"
1304.00,"25","BUFR/CREX Processing information","025019","A to Z law for attenuation exponent",,"Numeric","2","0","7","Numeric","2","3","Operational"
1305.00,"25","BUFR/CREX Processing information","025020","Mean speed estimation",,"Code table","0","0","2","Code table","0","1","Operational"
1306.00,"25","BUFR/CREX Processing information","025021","Wind computation enhancement",,"Flag table","0","0","8","Flag table","0","3","Operational"
1307.00,"25","BUFR/CREX Processing information","025022","GHRSST rejection flag","*","Flag table","0","0","9","Flag table","0","3","Operational"
1308.00,"25","BUFR/CREX Processing information","025023","GHRSST confidence flag",,"Flag table","0","0","9","Flag table","0","3","Operational"
1309.00,"25","BUFR/CREX Processing information","025024","GHRSST data quality",,"Code table","0","0","4","Code table","0","2","Operational"
1310.00,"25","BUFR/CREX Processing information","025025","Battery voltage",,"V","1","0","9","V","1","3","Operational"
1311.00,"25","BUFR/CREX Processing information","025026","Battery voltage (large range)",,"V","1","0","12","V","1","4","Operational"
1312.00,"25","BUFR/CREX Processing information","025028","Operator or manufacturer defined parameter",,"Numeric","1","-16384","15","Numeric","1","5","Operational"
1313.00,"25","BUFR/CREX Processing information","025029","Calibration method","(see Note 3)","Flag table","0","0","6","Flag table","0","2","Operational"
1314.00,"25","BUFR/CREX Processing information","025030","Running mean sea-surface temperature usage",,"Code table","0","0","2","Code table","0","1","Operational"
1315.00,"25","BUFR/CREX Processing information","025031","NWP-generated vertical profile thinning method",,"Code table","0","0","3","Code table","0","1","Operational"
1316.00,"25","BUFR/CREX Processing information","025032","Wind profiler mode information","(see Note 2)","Code table","0","0","2","Code table","0","1","Operational"
1317.00,"25","BUFR/CREX Processing information","025033","Wind profiler submode information","(see Note 2)","Code table","0","0","2","Code table","0","1","Operational"
1318.00,"25","BUFR/CREX Processing information","025034","Wind profiler quality control test results","(see Note 2)","Flag table","0","0","4","Flag table","0","2","Operational"
1319.00,"25","BUFR/CREX Processing information","025035","Decision method for polarity","(see Note 5)","Code table","0","0","3","Code table","0","1","Operational"
1320.00,"25","BUFR/CREX Processing information","025036","Atmospherics location method",,"Code table","0","0","4","Code table","0","2","Operational"
1321.00,"25","BUFR/CREX Processing information","025037","SST bias",,"K","2","-127","8","K","2","3","Operational"
1322.00,"25","BUFR/CREX Processing information","025038","Difference between SST and analysis",,"K","1","-127","8","K","1","3","Operational"
1323.00,"25","BUFR/CREX Processing information","025040","CO2 wind product derivation",,"Code table","0","0","4","Code table","0","2","Operational"
1324.00,"25","BUFR/CREX Processing information","025041","Moving platform direction reporting method",,"Code table","0","0","2","Code table","0","1","Operational"
1325.00,"25","BUFR/CREX Processing information","025042","Moving platform speed reporting method",,"Code table","0","0","2","Code table","0","1","Operational"
1326.00,"25","BUFR/CREX Processing information","025043","Wave sampling interval (time)",,"s","4","0","15","s","4","5","Operational"
1327.00,"25","BUFR/CREX Processing information","025044","Wave sampling interval (space)",,"m","2","0","14","m","2","5","Operational"
1328.00,"25","BUFR/CREX Processing information","025045","HIRS channel combination",,"Flag table","0","0","21","Flag table","0","7","Operational"
1329.00,"25","BUFR/CREX Processing information","025046","MSU channel combination",,"Flag table","0","0","5","Flag table","0","2","Operational"
1330.00,"25","BUFR/CREX Processing information","025047","SSU channel combination",,"Flag table","0","0","4","Flag table","0","2","Operational"
1331.00,"25","BUFR/CREX Processing information","025048","AMSU-A channel combination",,"Flag table","0","0","16","Flag table","0","6","Operational"
1332.00,"25","BUFR/CREX Processing information","025049","AMSU-B channel combination",,"Flag table","0","0","6","Flag table","0","2","Operational"
1333.00,"25","BUFR/CREX Processing information","025050","Principal component score",,"Numeric","4","-131072","18","Numeric","4","6","Operational"
1334.00,"25","BUFR/CREX Processing information","025051","AVHRR channel combination",,"Flag table","0","0","7","Flag table","0","3","Operational"
1335.00,"25","BUFR/CREX Processing information","025052","Log10 of principal components normalized fit to data",,"Numeric","4","0","15","Numeric","4","5","Operational"
1336.00,"25","BUFR/CREX Processing information","025053","Observation quality",,"Flag table","0","0","12","Flag table","0","4","Operational"
1337.00,"25","BUFR/CREX Processing information","025054","SSMIS subframe ID number",,"Numeric","0","0","5","Numeric","0","2","Operational"
1338.00,"25","BUFR/CREX Processing information","025055","Multiplexer housekeeping",,"K","2","0","16","K","2","5","Operational"
1339.00,"25","BUFR/CREX Processing information","025060","Software identification","(see Note 2)","Numeric","0","0","14","Numeric","0","5","Operational"
1340.00,"25","BUFR/CREX Processing information","025061","Software identification and version number",,"CCITT IA5","0","0","96","Character","0","12","Operational"
1341.00,"25","BUFR/CREX Processing information","025062","Database identification",,"Numeric","0","0","14","Numeric","0","5","Operational"
1342.00,"25","BUFR/CREX Processing information","025063","Central processor or system identifier","(see Note 6)","Code table","0","0","8","Code table","0","3","Operational"
1343.00,"25","BUFR/CREX Processing information","025065","Orientation correction (azimuth)",,"deg","2","-1000","11","deg","2","4","Operational"
1344.00,"25","BUFR/CREX Processing information","025066","Orientation correction (elevation)",,"deg","2","-1000","11","deg","2","4","Operational"
1345.00,"25","BUFR/CREX Processing information","025067","Radiosonde release point pressure correction",,"Pa","0","-8000","14","Pa","0","4","Operational"
1346.00,"25","BUFR/CREX Processing information","025068","Number of archive recomputes",,"Numeric","0","0","7","Numeric","0","3","Operational"
1347.00,"25","BUFR/CREX Processing information","025069","Flight level pressure corrections",,"Flag table","0","0","8","Flag table","0","3","Operational"
1348.00,"25","BUFR/CREX Processing information","025070","Major frame count",,"Numeric","0","0","4","Numeric","0","2","Operational"
1349.00,"25","BUFR/CREX Processing information","025071","Frame count",,"Numeric","0","0","5","Numeric","0","2","Operational"
1350.00,"25","BUFR/CREX Processing information","025075","Satellite antenna corrections version number",,"Numeric","0","0","5","Numeric","0","2","Operational"
1351.00,"25","BUFR/CREX Processing information","025076","Log10 of (temperature-radiance central wave number) for ATOVS",,"log (m-1)","8","0","30","log (m-1)","8","10","Operational"
1352.00,"25","BUFR/CREX Processing information","025077","Bandwidth correction coefficient 1 for ATOVS",,"Numeric","5","-100000","18","Numeric","5","7","Operational"
1353.00,"25","BUFR/CREX Processing information","025078","Bandwidth correction coefficient 2 for ATOVS",,"Numeric","5","0","17","Numeric","5","6","Operational"
1354.00,"25","BUFR/CREX Processing information","025079","Albedo-radiance solar filtered irradiance for ATOVS",,"W m-2","4","0","24","W m-2","4","8","Operational"
1355.00,"25","BUFR/CREX Processing information","025080","Albedo-radiance equivalent filter width for ATOVS",,"m","10","0","14","m","10","5","Operational"
1356.00,"25","BUFR/CREX Processing information","025081","Incidence angle",,"deg","3","0","17","deg","3","6","Operational"
1357.00,"25","BUFR/CREX Processing information","025082","Azimuth angle",,"deg","3","0","19","deg","3","6","Operational"
1358.00,"25","BUFR/CREX Processing information","025083","Faraday rotational angle",,"deg","3","0","19","deg","3","6","Operational"
1359.00,"25","BUFR/CREX Processing information","025084","Geometric rotational angle",,"deg","5","0","26","deg","5","8","Operational"
1360.00,"25","BUFR/CREX Processing information","025085","Fraction of clear pixels in HIRS FOV",,"Numeric","0","0","7","Numeric","0","3","Operational"
1361.00,"25","BUFR/CREX Processing information","025086","Depth correction indicator",,"Code table","0","0","2","Code table","0","1","Operational"
1362.00,"25","BUFR/CREX Processing information","025090","Orbit state flag",,"Code table","0","0","4","Code table","0","2","Operational"
1363.00,"25","BUFR/CREX Processing information","025091","Structure constant of the refraction index (Cn2)",,"dB","3","-18192","13","dB","3","5","Operational"
1364.00,"25","BUFR/CREX Processing information","025092","Acoustic propagation velocity",,"m/s","2","28000","14","m/s","2","5","Operational"
1365.00,"25","BUFR/CREX Processing information","025093","RASS computation correction",,"Flag table","0","0","8","Flag table","0","3","Operational"
1366.00,"25","BUFR/CREX Processing information","025095","Altimeter state flag",,"Flag table","0","0","2","Flag table","0","1","Operational"
1367.00,"25","BUFR/CREX Processing information","025096","Radiometer state flag",,"Flag table","0","0","5","Flag table","0","2","Operational"
1368.00,"25","BUFR/CREX Processing information","025097","Three-dimensional error estimate of the navigator orbit",,"Code table","0","0","4","Code table","0","2","Operational"
1369.00,"25","BUFR/CREX Processing information","025098","Altimeter data quality flag",,"Flag table","0","0","9","Flag table","0","3","Operational"
1370.00,"25","BUFR/CREX Processing information","025099","Altimeter correction quality flag",,"Flag table","0","0","9","Flag table","0","3","Operational"
1371.00,"25","BUFR/CREX Processing information","025100","XBT/XCTD fall rate equation coefficient a",,"Numeric","5","0","20","Numeric","5","6","Operational"
1372.00,"25","BUFR/CREX Processing information","025101","XBT/XCTD fall rate equation coefficient b",,"Numeric","5","-500000","21","Numeric","5","6","Operational"
1373.00,"25","BUFR/CREX Processing information","025102","Number of missing lines excluding data gaps",,"Numeric","0","0","8","Numeric","0","3","Operational"
1374.00,"25","BUFR/CREX Processing information","025103","Number of directional bins",,"Numeric","0","0","8","Numeric","0","3","Operational"
1375.00,"25","BUFR/CREX Processing information","025104","Number of wavelength bins",,"Numeric","0","0","8","Numeric","0","3","Operational"
1376.00,"25","BUFR/CREX Processing information","025105","First directional bin",,"deg","3","0","19","deg","3","6","Operational"
1377.00,"25","BUFR/CREX Processing information","025106","Directional bin step",,"deg","3","0","19","deg","3","6","Operational"
1378.00,"25","BUFR/CREX Processing information","025107","First wavelength bin",,"m","3","0","29","m","3","9","Operational"
1379.00,"25","BUFR/CREX Processing information","025108","Last wavelength bin",,"m","3","0","29","m","3","9","Operational"
1380.00,"25","BUFR/CREX Processing information","025110","Image processing summary",,"Flag table","0","0","10","Flag table","0","4","Operational"
1381.00,"25","BUFR/CREX Processing information","025111","Number of input data gaps",,"Numeric","0","0","8","Numeric","0","3","Operational"
1382.00,"25","BUFR/CREX Processing information","025112","Band specific altimeter data quality flag",,"Flag table","0","0","9","Flag table","0","3","Operational"
1383.00,"25","BUFR/CREX Processing information","025113","Band specific altimeter correction quality flag",,"Flag table","0","0","9","Flag table","0","3","Operational"
1384.00,"25","BUFR/CREX Processing information","025120","RA2-L2-processing flag",,"Code table","0","0","2","Code table","0","1","Operational"
1385.00,"25","BUFR/CREX Processing information","025121","RA2-L2-processing quality",,"%","0","0","7","%","0","3","Operational"
1386.00,"25","BUFR/CREX Processing information","025122","Hardware configuration for RF",,"Code table","0","0","2","Code table","0","1","Operational"
1387.00,"25","BUFR/CREX Processing information","025123","Hardware configuration for HPA",,"Code table","0","0","2","Code table","0","1","Operational"
1388.00,"25","BUFR/CREX Processing information","025124","MWR-L2-processing flag",,"Code table","0","0","2","Code table","0","1","Operational"
1389.00,"25","BUFR/CREX Processing information","025125","MWR-L2-processing quality",,"%","0","0","7","%","0","3","Operational"
1390.00,"25","BUFR/CREX Processing information","025126","Model dry tropospheric correction",,"m","3","-32768","16","m","3","5","Operational"
1391.00,"25","BUFR/CREX Processing information","025127","Inverted barometer correction",,"m","3","-32768","16","m","3","5","Operational"
1392.00,"25","BUFR/CREX Processing information","025128","Model wet tropospheric correction",,"m","3","-32768","16","m","3","5","Operational"
1393.00,"25","BUFR/CREX Processing information","025129","MWR derived wet tropospheric correction",,"m","3","-32768","16","m","3","5","Operational"
1394.00,"25","BUFR/CREX Processing information","025130","RA2 ionospheric correction on Ku band",,"m","3","-32768","16","m","3","5","Operational"
1395.00,"25","BUFR/CREX Processing information","025131","Ionospheric correction from Doris on Ku band",,"m","3","-32768","16","m","3","5","Operational"
1396.00,"25","BUFR/CREX Processing information","025132","Ionospheric correction from model on Ku band",,"m","3","-32768","16","m","3","5","Operational"
1397.00,"25","BUFR/CREX Processing information","025133","Sea state bias correction on Ku band",,"m","3","-32768","16","m","3","5","Operational"
1398.00,"25","BUFR/CREX Processing information","025134","RA2 ionospheric correction on S band",,"m","3","-32768","16","m","3","5","Operational"
1399.00,"25","BUFR/CREX Processing information","025135","Ionospheric correction from Doris on S band",,"m","3","-32768","16","m","3","5","Operational"
1400.00,"25","BUFR/CREX Processing information","025136","Ionospheric correction from model on S band",,"m","3","-32768","16","m","3","5","Operational"
1401.00,"25","BUFR/CREX Processing information","025137","Sea state bias correction on S band",,"m","3","-32768","16","m","3","5","Operational"
1402.00,"25","BUFR/CREX Processing information","025138","Average signal-to-noise ratio",,"Numeric","0","-2048","12","Numeric","0","4","Operational"
1403.00,"25","BUFR/CREX Processing information","025140","Start channel",,"Numeric","0","0","14","Numeric","0","5","Operational"
1404.00,"25","BUFR/CREX Processing information","025141","End channel",,"Numeric","0","0","14","Numeric","0","5","Operational"
1405.00,"25","BUFR/CREX Processing information","025142","Channel scale factor",,"Numeric","0","0","6","Numeric","0","2","Operational"
1406.00,"25","BUFR/CREX Processing information","025143","Linear coefficient",,"Numeric","6","-5000000","24","Numeric","6","8","Operational"
1410.00,"25","BUFR/CREX Processing information","025150","Method of tropical cyclone intensity analysis using satellite data",,"Code table","0","0","4","Code table","0","2","Operational"
1414.00,"25","BUFR/CREX Processing information","025160","Ku band net instrumental correction",,"m","4","-120000","18","m","4","6","Operational"
1415.00,"25","BUFR/CREX Processing information","025161","C band net instrumental correction",,"m","4","-120000","18","m","4","6","Operational"
1416.00,"25","BUFR/CREX Processing information","025162","Sea state bias correction on C band",,"m","4","-6000","13","m","4","4","Operational"
1417.00,"25","BUFR/CREX Processing information","025163","Altimeter ionospheric correction on Ku band",,"m","3","-32768","16","m","3","5","Operational"
1418.00,"25","BUFR/CREX Processing information","025164","Radiometer wet tropospheric correction",,"m","4","-5000","13","m","4","4","Operational"
1419.00,"25","BUFR/CREX Processing information","025165","Ionospheric correction from model on specific band",,"m","4","-32768","16","m","4","5","Operational"
1420.00,"25","BUFR/CREX Processing information","025166","Sea state bias correction on specific band",,"m","4","-32768","16","m","4","5","Operational"
1421.00,"25","BUFR/CREX Processing information","025167","Specific band net instrumental correction",,"m","4","-120000","18","m","4","6","Operational"
1422.00,"25","BUFR/CREX Processing information","025170","Sampling interval (time)",,"s","0","0","10","s","0","4","Operational"
1423.00,"25","BUFR/CREX Processing information","025171","Sample averaging period",,"s","0","0","10","s","0","4","Operational"
1424.00,"25","BUFR/CREX Processing information","025172","Number of samples",,"Numeric","0","0","10","Numeric","0","4","Operational"
1425.00,"25","BUFR/CREX Processing information","025174","SMOS information flag",,"Flag table","0","0","14","Flag table","0","5","Operational"
1426.00,"25","BUFR/CREX Processing information","025175","Modified residual","(see Note 7)","Numeric","2","0","13","Numeric","2","4","Operational"
1427.00,"25","BUFR/CREX Processing information","025180","LRM per cent","*","%","2","0","16","%","2","5","Operational"
1428.00,"25","BUFR/CREX Processing information","025181","L2 processing flag",,"Code table","0","0","2","Code table","0","1","Operational"
1429.00,"25","BUFR/CREX Processing information","025182","L1 processing flag",,"Code table","0","0","2","Code table","0","1","Operational"
1430.00,"25","BUFR/CREX Processing information","025183","L1 processing quality",,"%","2","0","14","%","2","5","Operational"
1431.00,"25","BUFR/CREX Processing information","025184","L2 product status",,"Code table","0","0","2","Code table","0","1","Operational"
1434.00,"26","BUFR/CREX Non-coordinate location (time)","026001","Principal time of daily reading in UTC of maximum temperature",,"h","1","0","12","h","1","3","Operational"
1435.00,"26","BUFR/CREX Non-coordinate location (time)","026002","Principal time of daily reading in UTC of minimum temperature",,"h","1","0","12","h","1","3","Operational"
1436.00,"26","BUFR/CREX Non-coordinate location (time)","026003","Time difference",,"min","0","-1440","12","min","0","4","Operational"
1437.00,"26","BUFR/CREX Non-coordinate location (time)","026010","Hours included",,"Flag table","0","0","26","Flag table","0","9","Operational"
1438.00,"26","BUFR/CREX Non-coordinate location (time)","026020","Duration of precipitation",,"min","0","0","11","min","0","4","Operational"
1439.00,"26","BUFR/CREX Non-coordinate location (time)","026021","Year",,"a","0","0","12","a","0","4","Operational"
1440.00,"26","BUFR/CREX Non-coordinate location (time)","026022","Month",,"mon","0","0","4","mon","0","2","Operational"
1441.00,"26","BUFR/CREX Non-coordinate location (time)","026023","Day",,"d","0","0","6","d","0","2","Operational"
1442.00,"26","BUFR/CREX Non-coordinate location (time)","026030","Measurement integration time",,"s","2","0","8","s","2","3","Operational"
1443.00,"27","BUFR/CREX Non-coordinate location (horizontal - 1)","027001","Latitude (high accuracy)",,"deg","5","-9000000","25","deg","5","7","Operational"
1444.00,"27","BUFR/CREX Non-coordinate location (horizontal - 1)","027002","Latitude (coarse accuracy)",,"deg","2","-9000","15","deg","2","4","Operational"
1445.00,"27","BUFR/CREX Non-coordinate location (horizontal - 1)","027003","Alternate latitude (coarse accuracy)",,"deg","2","-9000","15","deg","2","4","Operational"
1446.00,"27","BUFR/CREX Non-coordinate location (horizontal - 1)","027004","Alternate latitude (high accuracy)",,"deg","5","-9000000","25","deg","5","7","Operational"
1447.00,"27","BUFR/CREX Non-coordinate location (horizontal - 1)","027010","Footprint axis 1",,"m","-1","0","14","m","-1","5","Operational"
1448.00,"27","BUFR/CREX Non-coordinate location (horizontal - 1)","027020","Satellite location counter",,"Numeric","0","0","16","Numeric","0","5","Operational"
1449.00,"27","BUFR/CREX Non-coordinate location (horizontal - 1)","027021","Satellite sublocation dimension",,"Numeric","0","0","16","Numeric","0","5","Operational"
1450.00,"27","BUFR/CREX Non-coordinate location (horizontal - 1)","027031","In direction of 0 degrees longitude, distance from the Earth's centre",,"m","2","-1073741824","31","m","2","10","Operational"
1451.00,"27","BUFR/CREX Non-coordinate location (horizontal - 1)","027080","Viewing azimuth angle",,"degree true","2","0","16","degree true","0","5","Operational"
1452.00,"28","BUFR/CREX Non-coordinate location (horizontal - 2)","028001","Longitude (high accuracy)",,"deg","5","-18000000","26","deg","5","8","Operational"
1453.00,"28","BUFR/CREX Non-coordinate location (horizontal - 2)","028002","Longitude (coarse accuracy)",,"deg","2","-18000","16","deg","2","5","Operational"
1454.00,"28","BUFR/CREX Non-coordinate location (horizontal - 2)","028003","Alternate longitude (coarse accuracy)",,"deg","2","-18000","16","deg","2","5","Operational"
1455.00,"28","BUFR/CREX Non-coordinate location (horizontal - 2)","028004","Alternate longitude (high accuracy)",,"deg","5","-18000000","26","deg","5","8","Operational"
1456.00,"28","BUFR/CREX Non-coordinate location (horizontal - 2)","028010","Footprint axis 2",,"m","-1","0","14","m","-1","5","Operational"
1457.00,"28","BUFR/CREX Non-coordinate location (horizontal - 2)","028031","In direction 90 degrees East, distance from the Earth's centre",,"m","2","-1073741824","31","m","2","10","Operational"
1458.00,"29","BUFR/CREX Map data","029001","Projection type",,"Code table","0","0","3","Code table","0","1","Operational"
1459.00,"29","BUFR/CREX Map data","029002","Coordinate grid type",,"Code table","0","0","3","Code table","0","1","Operational"
1460.00,"30","BUFR/CREX Image","030001","Pixel value (4 bits)",,"Numeric","0","0","4","Numeric","0","2","Operational"
1461.00,"30","BUFR/CREX Image","030002","Pixel value (8 bits)",,"Numeric","0","0","8","Numeric","0","3","Operational"
1462.00,"30","BUFR/CREX Image","030004","Pixel value (16 bits)",,"Numeric","0","0","16","Numeric","0","5","Operational"
1463.00,"30","BUFR/CREX Image","030010","Number of grid points",,"Numeric","0","0","13","Numeric","0","4","Operational"
1464.00,"30","BUFR/CREX Image","030021","Number of pixels per row",,"Numeric","0","0","12","Numeric","0","4","Operational"
1465.00,"30","BUFR/CREX Image","030022","Number of pixels per column",,"Numeric","0","0","12","Numeric","0","4","Operational"
1466.00,"30","BUFR/CREX Image","030031","Picture type",,"Code table","0","0","4","Code table","0","2","Operational"
1467.00,"30","BUFR/CREX Image","030032","Combination with other data",,"Flag table","0","0","16","Flag table","0","6","Operational"
1468.00,"30","BUFR/CREX Image","030033","Number of bins along the radial",,"Numeric","0","0","12","Numeric","0","4","Operational"
1469.00,"30","BUFR/CREX Image","030034","Number of azimuths",,"Numeric","0","0","12","Numeric","0","4","Operational"
1470.00,"31","BUFR/CREX Data description operator qualifiers","031000","Short delayed descriptor replication factor",,"Numeric","0","0","1",,,,"Operational"
1471.00,"31","BUFR/CREX Data description operator qualifiers","031001","Delayed descriptor replication factor",,"Numeric","0","0","8",,,,"Operational"
1472.00,"31","BUFR/CREX Data description operator qualifiers","031002","Extended delayed descriptor replication factor",,"Numeric","0","0","16",,,,"Operational"
1473.00,"31","BUFR/CREX Data description operator qualifiers","031011","Delayed descriptor and data repetition factor",,"Numeric","0","0","8",,,,"Operational"
1474.00,"31","BUFR/CREX Data description operator qualifiers","031012","Extended delayed descriptor and data repetition factor",,"Numeric","0","0","16",,,,"Operational"
1475.00,"31","BUFR/CREX Data description operator qualifiers","031021","Associated field significance",,"Code table","0","0","6",,,,"Operational"
1476.00,"31","BUFR/CREX Data description operator qualifiers","031031","Data present indicator",,"Flag table","0","0","1",,,,"Operational"
1477.00,"33","BUFR/CREX Quality information","033002","Quality information",,"Code table","0","0","2","Code table","0","1","Operational"
1478.00,"33","BUFR/CREX Quality information","033003","Quality information",,"Code table","0","0","3","Code table","0","1","Operational"
1479.00,"33","BUFR/CREX Quality information","033005","Quality information (AWS data)",,"Flag table","0","0","30","Flag table","0","10","Operational"
1480.00,"33","BUFR/CREX Quality information","033006","Internal measurement status information (AWS)",,"Code table","0","0","3","Code table","0","1","Operational"
1481.00,"33","BUFR/CREX Quality information","033007","Per cent confidence",,"%","0","0","7","%","0","3","Operational"
1483.00,"33","BUFR/CREX Quality information","033015","Data quality-check indicator",,"Code table","0","0","6","Code table","0","2","Operational"
1484.00,"33","BUFR/CREX Quality information","033020","Quality control indication of following value",,"Code table","0","0","3","Code table","0","1","Operational"
1485.00,"33","BUFR/CREX Quality information","033021","Quality of following value",,"Code table","0","0","2","Code table","0","1","Operational"
1486.00,"33","BUFR/CREX Quality information","033022","Quality of buoy satellite transmission",,"Code table","0","0","2","Code table","0","1","Operational"
1487.00,"33","BUFR/CREX Quality information","033023","Quality of buoy location",,"Code table","0","0","2","Code table","0","1","Operational"
1488.00,"33","BUFR/CREX Quality information","033024","Station elevation quality mark (for mobile stations)",,"Code table","0","0","4","Code table","0","2","Operational"
1489.00,"33","BUFR/CREX Quality information","033025","ACARS interpolated values indicator",,"Code table","0","0","3","Code table","0","1","Operational"
1490.00,"33","BUFR/CREX Quality information","033026","Moisture quality",,"Code table","0","0","6","Code table","0","2","Operational"
1491.00,"33","BUFR/CREX Quality information","033027","Location quality class (range of radius of 66 % confidence)",,"Code table","0","0","3","Code table","0","1","Operational"
1492.00,"33","BUFR/CREX Quality information","033028","Snapshot overall quality",,"Code table","0","0","3","Code table","0","1","Operational"
1494.00,"33","BUFR/CREX Quality information","033030","Scan line status flags for ATOVS",,"Flag table","0","0","24","Flag table","0","8","Operational"
1495.00,"33","BUFR/CREX Quality information","033031","Scan line quality flags for ATOVS",,"Flag table","0","0","24","Flag table","0","8","Operational"
1496.00,"33","BUFR/CREX Quality information","033032","Channel quality flags for ATOVS",,"Flag table","0","0","24","Flag table","0","8","Operational"
1497.00,"33","BUFR/CREX Quality information","033033","Field of view quality flags for ATOVS",,"Flag table","0","0","24","Flag table","0","8","Operational"
1498.00,"33","BUFR/CREX Quality information","033035","Manual/automatic quality control",,"Code table","0","0","4","Code table","0","2","Operational"
1499.00,"33","BUFR/CREX Quality information","033036","Nominal confidence threshold",,"%","0","0","7","%","0","3","Operational"
1500.00,"33","BUFR/CREX Quality information","033037","Wind correlation error",,"Flag table","0","0","20","Flag table","0","7","Operational"
1501.00,"33","BUFR/CREX Quality information","033038","Quality flags for ground-based GNSS data",,"Flag table","0","0","10","Flag table","0","4","Operational"
1502.00,"33","BUFR/CREX Quality information","033039","Quality flags for radio occultation data",,"Flag table","0","0","16","Flag table","0","6","Operational"
1503.00,"33","BUFR/CREX Quality information","033040","Confidence interval",,"%","0","0","7","%","0","3","Operational"
1504.00,"33","BUFR/CREX Quality information","033041","Attribute of following value",,"Code table","0","0","2","Code table","0","1","Operational"
1505.00,"33","BUFR/CREX Quality information","033042","Type of limit represented by following value",,"Code table","0","0","3","Code table","0","1","Operational"
1506.00,"33","BUFR/CREX Quality information","033043","AST confidence",,"Flag table","0","0","8","Flag table","0","3","Operational"
1507.00,"33","BUFR/CREX Quality information","033044","ASAR quality information",,"Flag table","0","0","15","Flag table","0","5","Operational"
1508.00,"33","BUFR/CREX Quality information","033045","Probability of following event","(see Notes 1 and 3)","%","0","0","7","%","0","3","Operational"
1509.00,"33","BUFR/CREX Quality information","033046","Conditional probability of following event with respect to specified conditioning event","(see Notes 1, 2 and 3)","%","0","0","7","%","0","3","Operational"
1510.00,"33","BUFR/CREX Quality information","033047","Measurement confidence data",,"Flag table","0","0","31","Flag table","0","11","Operational"
1511.00,"33","BUFR/CREX Quality information","033048","Confidence measure of SAR inversion",,"Code table","0","0","2","Code table","0","1","Operational"
1512.00,"33","BUFR/CREX Quality information","033049","Confidence measure of wind retrieval",,"Code table","0","0","2","Code table","0","1","Operational"
1513.00,"33","BUFR/CREX Quality information","033050","Global GTSPP quality flag",,"Code table","0","0","4","Code table","0","2","Operational"
1514.00,"33","BUFR/CREX Quality information","033052","S band ocean retracking quality",,"Flag table","0","0","21","Flag table","0","7","Operational"
1515.00,"33","BUFR/CREX Quality information","033053","Ku band ocean retracking quality",,"Flag table","0","0","21","Flag table","0","7","Operational"
1516.00,"33","BUFR/CREX Quality information","033060","GqisFlagQual - individual IASI-System quality flag",,"Code table","0","0","2","Code table","0","1","Operational"
1517.00,"33","BUFR/CREX Quality information","033061","GqisQualIndex - indicator for instrument noise performance (contributions from spectral and radiometric calibration)",,"%","0","0","7","%","0","3","Operational"
1518.00,"33","BUFR/CREX Quality information","033062","GqisQualIndexLoc - indicator for geometric quality index",,"%","0","0","7","%","0","3","Operational"
1519.00,"33","BUFR/CREX Quality information","033063","GqisQualIndexRad - indicator for instrument noise performance (contributions from radiometric calibration)",,"%","0","0","7","%","0","3","Operational"
1520.00,"33","BUFR/CREX Quality information","033064","GqisQualIndexSpect - indicator for instrument noise performance (contributions from spectral calibration)",,"%","0","0","7","%","0","3","Operational"
1521.00,"33","BUFR/CREX Quality information","033065","GqisSysTecSondQual - output of system TEC (Technical Expertise Centre) quality function",,"Numeric","0","0","24","Numeric","0","8","Operational"
1522.00,"33","BUFR/CREX Quality information","033070","Total ozone quality",,"Code table","0","0","4","Code table","0","2","Operational"
1523.00,"33","BUFR/CREX Quality information","033071","Profile ozone quality",,"Code table","0","0","4","Code table","0","2","Operational"
1524.00,"33","BUFR/CREX Quality information","033072","Ozone error",,"Code table","0","0","5","Code table","0","2","Operational"
1525.00,"33","BUFR/CREX Quality information","033075","Scan-level quality flags",,"Flag table","0","0","13","Flag table","0","5","Operational"
1526.00,"33","BUFR/CREX Quality information","033076","Calibration quality flags",,"Flag table","0","0","9","Flag table","0","3","Operational"
1527.00,"33","BUFR/CREX Quality information","033077","Field-of-view quality flags",,"Flag table","0","0","19","Flag table","0","7","Operational"
1528.00,"33","BUFR/CREX Quality information","033078","Geolocation quality",,"Code table","0","0","4","Code table","0","2","Operational"
1529.00,"33","BUFR/CREX Quality information","033079","Granule level quality flags",,"Flag table","0","0","16","Flag table","0","6","Operational"
1530.00,"33","BUFR/CREX Quality information","033080","Scan level quality flags",,"Flag table","0","0","20","Flag table","0","7","Operational"
1531.00,"33","BUFR/CREX Quality information","033081","Channel data quality flags",,"Flag table","0","0","12","Flag table","0","4","Operational"
1532.00,"33","BUFR/CREX Quality information","033082","Geolocation quality flags",,"Flag table","0","0","16","Flag table","0","6","Operational"
1533.00,"33","BUFR/CREX Quality information","033083","Radiance data quality flags",,"Flag table","0","0","16","Flag table","0","6","Operational"
1534.00,"33","BUFR/CREX Quality information","033084","Pixel level quality flags",,"Flag table","0","0","16","Flag table","0","6","Operational"
1535.00,"33","BUFR/CREX Quality information","033085","Aerosol optical thickness quality flags",,"Flag table","0","0","18","Flag table","0","6","Operational"
1536.00,"33","BUFR/CREX Quality information","033086","Quality of pixel level retrieval",,"Code table","0","0","3","Code table","0","1","Operational"
1537.00,"33","BUFR/CREX Quality information","033087","Extent of satellite within South Atlantic anomaly (based on climatological data)",,"Code table","0","0","4","Code table","0","1","Operational"
1538.00,"33","BUFR/CREX Quality information","033088","Ozone total column quality flag",,"Flag table","0","0","18","Flag table","0","6","Operational"
1539.00,"35","BUFR/CREX Data monitoring information","035000","FM and Regional Code number",,"Code table","0","0","10","Code table","0","3","Operational"
1540.00,"35","BUFR/CREX Data monitoring information","035001","Time frame for monitoring",,"Code table","0","0","3","Code table","0","1","Operational"
1541.00,"35","BUFR/CREX Data monitoring information","035011","Number of reports actually received",,"Numeric","0","0","14","Numeric","0","4","Operational"
1542.00,"35","BUFR/CREX Data monitoring information","035021","Bulletin being monitored (TTAAii)",,"CCITT IA5","0","0","48","Character","0","6","Operational"
1543.00,"35","BUFR/CREX Data monitoring information","035022","Bulletin being monitored (YYGGgg)",,"CCITT IA5","0","0","48","Character","0","6","Operational"
1544.00,"35","BUFR/CREX Data monitoring information","035023","Bulletin being monitored (CCCC)",,"CCITT IA5","0","0","32","Character","0","4","Operational"
1545.00,"35","BUFR/CREX Data monitoring information","035024","Bulletin being monitored (BBB)",,"CCITT IA5","0","0","24","Character","0","3","Operational"
1546.00,"35","BUFR/CREX Data monitoring information","035030","Discrepancies in the availability of expected data",,"Code table","0","0","4","Code table","0","1","Operational"
1547.00,"35","BUFR/CREX Data monitoring information","035031","Qualifier on monitoring results",,"Code table","0","0","7","Code table","0","2","Operational"
1548.00,"35","BUFR/CREX Data monitoring information","035032","Cause of missing data",,"Code table","0","0","4","Code table","0","1","Operational"
1549.00,"35","BUFR/CREX Data monitoring information","035033","Observation and collection deficiencies",,"Code table","0","0","7","Code table","0","2","Operational"
1550.00,"35","BUFR/CREX Data monitoring information","035034","Statistical trends for availability of data (during the survey period(s))",,"Code table","0","0","3","Code table","0","1","Operational"
1551.00,"35","BUFR/CREX Data monitoring information","035035","Reason for termination",,"Code table","0","0","5","Code table","0","2","Operational"
1552.00,"40","BUFR/CREX Satellite data","040001","Surface soil moisture (ms)",,"%","1","0","10","%","1","4","Operational"
1553.00,"40","BUFR/CREX Satellite data","040002","Estimated error in surface soil moisture",,"%","1","0","10","%","1","4","Operational"
1554.00,"40","BUFR/CREX Satellite data","040003","Mean surface soil moisture",,"Numeric","3","0","10","Numeric","3","4","Operational"
1555.00,"40","BUFR/CREX Satellite data","040004","Rain fall detection",,"Numeric","3","0","10","Numeric","3","4","Operational"
1556.00,"40","BUFR/CREX Satellite data","040005","Soil moisture correction flag",,"Flag table","0","0","8","Flag table","0","3","Operational"
1557.00,"40","BUFR/CREX Satellite data","040006","Soil moisture processing flag",,"Flag table","0","0","16","Flag table","0","6","Operational"
1558.00,"40","BUFR/CREX Satellite data","040007","Soil moisture quality",,"%","1","0","10","%","1","4","Operational"
1559.00,"40","BUFR/CREX Satellite data","040008","Frozen land surface fraction",,"%","1","0","10","%","1","4","Operational"
1560.00,"40","BUFR/CREX Satellite data","040009","Inundation and wetland fraction",,"%","1","0","10","%","1","4","Operational"
1561.00,"40","BUFR/CREX Satellite data","040010","Topographic complexity",,"%","1","0","10","%","1","4","Operational"
1562.00,"40","BUFR/CREX Satellite data","040011","Interpolation flag",,"Flag table","0","0","8","Flag table","0","3","Operational"
1563.00,"40","BUFR/CREX Satellite data","040012","Radiometer data quality flag",,"Flag table","0","0","8","Flag table","0","3","Operational"
1564.00,"40","BUFR/CREX Satellite data","040013","Radiometer brightness temperature interpretation flag",,"Code table","0","0","3","Code table","0","1","Operational"
1565.00,"40","BUFR/CREX Satellite data","040014","High-frequency fluctuations of the sea-surface topography correction",,"m","4","-3000","13","m","4","4","Operational"
1566.00,"40","BUFR/CREX Satellite data","040015","Normalized differential vegetation index (NDVI)",,"Numeric","2","-100","8","Numeric","2","3","Operational"
1567.00,"40","BUFR/CREX Satellite data","040016","Residual RMS in band",,"Numeric","3","0","14","Numeric","3","5","Operational"
1568.00,"40","BUFR/CREX Satellite data","040017","Non-normalized principal component score",,"Numeric","0","-1073741824","31","Numeric","0","10","Operational"
1569.00,"40","BUFR/CREX Satellite data","040018","GIacAvgImagIIS - average of imager measurements",,"W m-2 sr-1 m","6","0","24","W m-2 sr-1 m","6","8","Operational"
1570.00,"40","BUFR/CREX Satellite data","040019","GIacVarImagIIS - variance of imager measurements",,"W m-2 sr-1 m","6","0","24","W m-2 sr-1 m","6","8","Operational"
1571.00,"40","BUFR/CREX Satellite data","040020","GqisFlagQualDetailed - quality flag for the system",,"Flag table","0","0","17","Flag table","0","6","Operational"
1572.00,"40","BUFR/CREX Satellite data","040021","Fraction of weighted AVHRR pixel in IASI FOV covered with snow/ice",,"%","0","0","7","%","0","3","Operational"
1573.00,"40","BUFR/CREX Satellite data","040022","Number of missing, bad or failed AVHRR pixels",,"Numeric","0","0","7","Numeric","0","3","Operational"
1574.00,"40","BUFR/CREX Satellite data","040023","Auxiliary altimeter state flags",,"Flag table","0","0","5","Flag table","0","2","Operational"
1575.00,"40","BUFR/CREX Satellite data","040024","Meteorological map availability",,"Code table","0","0","3","Code table","0","1","Operational"
1576.00,"40","BUFR/CREX Satellite data","040025","Interpolation flag for mean diurnal tide",,"Code table","0","0","2","Code table","0","1","Operational"
1577.00,"40","BUFR/CREX Satellite data","040026","Score quantization factor",,"Numeric","2","0","16","Numeric","2","5","Operational"
