"No","ClassNo","ClassName_en","FXY","ElementName_en","Note_en","BUFR_Unit","BUFR_Scale","BUFR_ReferenceValue","BUFR_DataWidth_Bits","CREX_Unit","CREX_Scale","CREX_DataWidth_Char","Status"
1.00,"00","BUFR/CREX table entries","000001","Table A: entry",,"CCITT IA5","0","0","24","Character","0","3","Operational"
2.00,"00","BUFR/CREX table entries","000002","Table A: data category description, line 1",,"CCITT IA5","0","0","256","Character","0","32","Operational"
3.00,"00","BUFR/CREX table entries","000003","Table A: data category description, line 2",,"CCITT IA5","0","0","256","Character","0","32","Operational"
4.00,"00","BUFR/CREX table entries","000004","BUFR/CREX Master table","(see Note 1)","CCITT IA5","0","0","16","Character","0","2","Operational"
5.00,"00","BUFR/CREX table entries","000005","BUFR/CREX edition number",,"CCITT IA5","0","0","24","Character","0","3","Operational"
6.00,"00","BUFR/CREX table entries","000006","BUFR Master table Version number","(see Note 2)","CCITT IA5","0","0","16","Character","0","2","Operational"
7.00,"00","BUFR/CREX table entries","000007","CREX Master table version number","(see Note 3)","CCITT IA5","0","0","16","Character","0","2","Operational"
8.00,"00","BUFR/CREX table entries","000008","BUFR Local table version number","(see Note 4)","CCITT IA5","0","0","16","Character","0","2","Operational"
9.00,"00","BUFR/CREX table entries","000010","F descriptor to be added or defined",,"CCITT IA5","0","0","8","Character","0","1","Operational"
10.00,"00","BUFR/CREX table entries","000011","X descriptor to be added or defined",,"CCITT IA5","0","0","16","Character","0","2","Operational"
11.00,"00","BUFR/CREX table entries","000012","Y descriptor to be added or defined",,"CCITT IA5","0","0","24","Character","0","3","Operational"
12.00,"00","BUFR/CREX table entries","000013","Element name, line 1",,"CCITT IA5","0","0","256","Character","0","32","Operational"
13.00,"00","BUFR/CREX table entries","000014","Element name, line 2",,"CCITT IA5","0","0","256","Character","0","32","Operational"
14.00,"00","BUFR/CREX table entries","000015","Units name",,"CCITT IA5","0","0","192","Character","0","24","Operational"
15.00,"00","BUFR/CREX table entries","000016","Units scale sign",,"CCITT IA5","0","0","8","Character","0","1","Operational"
16.00,"00","BUFR/CREX table entries","000017","Units scale",,"CCITT IA5","0","0","24","Character","0","3","Operational"
17.00,"00","BUFR/CREX table entries","000018","Units reference sign",,"CCITT IA5","0","0","8","Character","0","1","Operational"
18.00,"00","BUFR/CREX table entries","000019","Units reference value",,"CCITT IA5","0","0","80","Character","0","10","Operational"
19.00,"00","BUFR/CREX table entries","000020","Element data width",,"CCITT IA5","0","0","24","Character","0","3","Operational"
20.00,"00","BUFR/CREX table entries","000024","Code figure",,"CCITT IA5","0","0","64","Character","0","8","Operational"
21.00,"00","BUFR/CREX table entries","000025","Code figure meaning",,"CCITT IA5","0","0","496","Character","0","62","Operational"
22.00,"00","BUFR/CREX table entries","000026","Bit number",,"CCITT IA5","0","0","48","Character","0","6","Operational"
23.00,"00","BUFR/CREX table entries","000027","Bit number meaning",,"CCITT IA5","0","0","496","Character","0","62","Operational"
24.00,"00","BUFR/CREX table entries","000030","Descriptor defining sequence",,"CCITT IA5","0","0","48","Character","0","6","Operational"
25.00,"01","Identification","001001","WMO block number",,"Numeric","0","0","7","Numeric","0","2","Operational"
26.00,"01","Identification","001002","WMO station number",,"Numeric","0","0","10","Numeric","0","3","Operational"
27.00,"01","Identification","001003","WMO Region number/geographical area",,"Code table","0","0","3","Code table","0","1","Operational"
28.00,"01","Identification","001004","WMO Region sub-area","(see Note 9)","Numeric","0","0","3","Numeric","0","1","Operational"
29.00,"01","Identification","001005","Buoy/platform identifier",,"Numeric","0","0","17","Numeric","0","5","Operational"
30.00,"01","Identification","001006","Aircraft flight number",,"CCITT IA5","0","0","64","Character","0","8","Operational"
31.00,"01","Identification","001007","Satellite identifier",,"Code table","0","0","10","Code table","0","4","Operational"
32.00,"01","Identification","001008","Aircraft registration number or other identification",,"CCITT IA5","0","0","64","Character","0","8","Operational"
33.00,"01","Identification","001009","Type of commercial aircraft",,"CCITT IA5","0","0","64","Character","0","8","Operational"
34.00,"01","Identification","001010","Stationary buoy platform identifier; e.g. C-MAN buoys",,"CCITT IA5","0","0","64","Character","0","8","Operational"
35.00,"01","Identification","001011","Ship or mobile land station identifier",,"CCITT IA5","0","0","72","Character","0","9","Operational"
36.00,"01","Identification","001012","Direction of motion of moving observing platform","*","degree true","0","0","9","degree true","0","3","Operational"
37.00,"01","Identification","001013","Speed of motion of moving observing platform","*","m/s","0","0","10","m/s","0","3","Operational"
38.00,"01","Identification","001014","Platform drift speed (high precision)",,"m/s","2","0","10","m/s","2","4","Operational"
39.00,"01","Identification","001015","Station or site name",,"CCITT IA5","0","0","160","Character","0","20","Operational"
40.00,"01","Identification","001018","Short station or site name",,"CCITT IA5","0","0","40","Character","0","5","Operational"
41.00,"01","Identification","001019","Long station or site name",,"CCITT IA5","0","0","256","Character","0","32","Operational"
42.00,"01","Identification","001020","WMO Region sub-area",,"Numeric","0","0","4","Numeric","0","2","Operational"
43.00,"01","Identification","001021","Synoptic feature identifier",,"Numeric","0","0","14","Numeric","0","4","Operational"
44.00,"01","Identification","001022","Name of feature","(see Note 11)","CCITT IA5","0","0","224","Character","0","28","Operational"
45.00,"01","Identification","001023","Observation sequence number",,"Numeric","0","0","9","Numeric","0","3","Operational"
46.00,"01","Identification","001024","Wind speed source",,"Code table","0","0","5","Code table","0","2","Operational"
47.00,"01","Identification","001025","Storm identifier","(see Note 1)","CCITT IA5","0","0","24","Character","0","3","Operational"
48.00,"01","Identification","001026","WMO storm name","**","CCITT IA5","0","0","64","Character","0","8","Operational"
49.00,"01","Identification","001027","WMO long storm name","**","CCITT IA5","0","0","80","Character","0","10","Operational"
50.00,"01","Identification","001028","Aerosol optical depth (AOD) source",,"Code table","0","0","5","Code table","0","2","Operational"
51.00,"01","Identification","001029","SSI source",,"Code table","0","0","5","Code table","0","2","Operational"
52.00,"01","Identification","001030","Numerical model identifier","(see Note 13)","CCITT IA5","0","0","128","Character","0","16","Operational"
53.00,"01","Identification","001031","Identification of originating/generating centre","(see Note 10)","Code table","0","0","16","Code table","0","5","Operational"
54.00,"01","Identification","001032","Generating application","(Notes 3, 4 and 5)","Code table defined by originating/generating centre","0","0","8","Code table","0","3","Operational"
55.00,"01","Identification","001033","Identification of originating/generating centre",,"Common Code table C-1","0","0","8","Common Code table C-1","0","3","Operational"
56.00,"01","Identification","001034","Identification of originating/generating sub-centre",,"Common Code table C-12","0","0","8","Common Code table C-12","0","3","Operational"
57.00,"01","Identification","001035","Originating centre",,"Common Code table C-11","0","0","16","Common Code Table C-11","0","5","Operational"
58.00,"01","Identification","001036","Agency in charge of operating the observing platform",,"Code table","0","0","20","Code table","0","7","Operational"
59.00,"01","Identification","001037","SIGMET sequence identifier",,"CCITT IA5","0","0","24","Character","0","3","Operational"
60.00,"01","Identification","001038","Source of sea ice fraction",,"Code table","0","0","5","Code table","0","2","Operational"
61.00,"01","Identification","001039","Graphical Area Forecast (GFA) sequence identifier",,"CCITT IA5","0","0","40","Character","0","5","Operational"
62.00,"01","Identification","001040","Processing centre ID code",,"CCITT IA5","0","0","48","Character","0","6","Operational"
63.00,"01","Identification","001041","Absolute platform velocity - first component","(see Note 6)","m/s","5","-1073741824","31","m/s","5","10","Operational"
64.00,"01","Identification","001042","Absolute platform velocity - second component","(see Note 6)","m/s","5","-1073741824","31","m/s","5","10","Operational"
65.00,"01","Identification","001043","Absolute platform velocity - third component","(see Note 6)","m/s","5","-1073741824","31","m/s","5","10","Operational"
66.00,"01","Identification","001050","Platform transmitter ID number",,"Numeric","0","0","17","Numeric","0","6","Operational"
67.00,"01","Identification","001051","Platform transmitter ID number",,"CCITT IA5","0","0","96","Character","0","12","Operational"
68.00,"01","Identification","001052","Platform transmitter ID",,"Code table","0","0","3","Code table","0","1","Operational"
69.00,"01","Identification","001053","Tsunameter report sequence number triggered by a tsunami event",,"Numeric","0","0","7","Numeric","0","2","Operational"
70.00,"01","Identification","001060","Aircraft reporting point (Beacon identifier)",,"CCITT IA5","0","0","64","Character","0","8","Operational"
71.00,"01","Identification","001062","Short ICAO location indicator",,"CCITT IA5","0","0","32","Character","0","4","Operational"
72.00,"01","Identification","001063","ICAO location indicator",,"CCITT IA5","0","0","64","Character","0","8","Operational"
73.00,"01","Identification","001064","Runway designator",,"CCITT IA5","0","0","32","Character","0","4","Operational"
74.00,"01","Identification","001065","ICAO region identifier",,"CCITT IA5","0","0","256","Character","0","32","Operational"
75.00,"01","Identification","001075","Tide station identification",,"CCITT IA5","0","0","40","Character","0","5","Operational"
76.00,"01","Identification","001079","Unique identifier for the profile",,"CCITT IA5","0","0","64","Character","0","8","Operational"
77.00,"01","Identification","001080","Ship line number according to SOOP",,"CCITT IA5","0","0","32","Character","0","4","Operational"
78.00,"01","Identification","001081","Radiosonde serial number",,"CCITT IA5","0","0","160","Character","0","20","Operational"
79.00,"01","Identification","001082","Radiosonde ascension number","(see Note 12)","Numeric","0","0","14","Numeric","0","4","Operational"
80.00,"01","Identification","001083","Radiosonde release number","(see Note 12)","Numeric","0","0","3","Numeric","0","1","Operational"
81.00,"01","Identification","001085","Observing platform manufacturer's model",,"CCITT IA5","0","0","160","Character","0","20","Operational"
82.00,"01","Identification","001086","Observing platform manufacturer's serial number",,"CCITT IA5","0","0","256","Character","0","32","Operational"
83.00,"01","Identification","001087","WMO marine observing platform extended identifier",,"Numeric","0","0","23","Numeric","0","7","Operational"
84.00,"01","Identification","001090","Technique for making up initial perturbations",,"Code table","0","0","8","Code table","0","3","Operational"
85.00,"01","Identification","001091","Ensemble member number",,"Numeric","0","0","10","Numeric","0","4","Operational"
86.00,"01","Identification","001092","Type of ensemble forecast",,"Code table","0","0","8","Code table","0","3","Operational"
87.00,"01","Identification","001093","Balloon lot number",,"CCITT IA5","0","0","96","Character","0","12","Operational"
88.00,"01","Identification","001094","WBAN number",,"Numeric","0","0","17","Numeric","0","5","Operational"
89.00,"01","Identification","001095","Observer identification",,"CCITT IA5","0","0","32","Character","0","4","Operational"
90.00,"01","Identification","001096","Station acquisition",,"CCITT IA5","0","0","160","Character","0","20","Operational"
93.00,"01","Identification","001099","Unique product definition",,"CCITT IA5","0","0","248","Character","0","31","Operational"
94.00,"01","Identification","001101","State identifier",,"Code table","0","0","10","Code table","0","3","Operational"
95.00,"01","Identification","001102","National station number",,"Numeric","0","0","30","Numeric","0","9","Operational"
96.00,"01","Identification","001103","IMO Number. Unique Lloyd's registry",,"Numeric","0","0","24","Numeric","0","7","Operational"
97.00,"01","Identification","001110","Aircraft tail number",,"CCITT IA5","0","0","48","Character","0","6","Operational"
98.00,"01","Identification","001111","Origination airport",,"CCITT IA5","0","0","24","Character","0","3","Operational"
99.00,"01","Identification","001112","Destination airport",,"CCITT IA5","0","0","24","Character","0","3","Operational"
101.00,"01","Identification","001124","Grid point identifier",,"Numeric","0","0","24","Numeric","0","8","Operational"
102.00,"01","Identification","001144","Snapshot identifier",,"Numeric","0","0","31","Numeric","0","10","Operational"
103.00,"02","Instrumentation","002001","Type of station",,"Code table","0","0","2","Code table","0","1","Operational"
104.00,"02","Instrumentation","002002","Type of instrumentation for wind measurement",,"Flag table","0","0","4","Flag table","0","2","Operational"
105.00,"02","Instrumentation","002003","Type of measuring equipment used",,"Code table","0","0","4","Code table","0","2","Operational"
106.00,"02","Instrumentation","002004","Type of instrumentation for evaporation measurement or type of crop for which evapotranspiration is reported",,"Code table","0","0","4","Code table","0","2","Operational"
107.00,"02","Instrumentation","002005","Precision of temperature observation",,"K","2","0","7","K","2","3","Operational"
109.00,"02","Instrumentation","002011","Radiosonde type",,"Code table","0","0","8","Code table","0","3","Operational"
110.00,"02","Instrumentation","002012","Radiosonde computational method",,"Code table","0","0","4","Code table","0","2","Operational"
111.00,"02","Instrumentation","002013","Solar and infrared radiation correction",,"Code table","0","0","4","Code table","0","2","Operational"
112.00,"02","Instrumentation","002014","Tracking technique/status of system used",,"Code table","0","0","7","Code table","0","3","Operational"
113.00,"02","Instrumentation","002015","Radiosonde completeness",,"Code table","0","0","4","Code table","0","2","Operational"
114.00,"02","Instrumentation","002016","Radiosonde configuration",,"Flag table","0","0","5","Flag table","0","2","Operational"
115.00,"02","Instrumentation","002017","Correction algorithms for humidity measurements",,"Code table","0","0","5","Code table","0","2","Operational"
116.00,"02","Instrumentation","002019","Satellite instruments",,"Code table","0","0","11","Code table","0","4","Operational"
117.00,"02","Instrumentation","002020","Satellite classification",,"Code table","0","0","9","Code table","0","3","Operational"
118.00,"02","Instrumentation","002021","Satellite instrument data used in processing","*","Flag table","0","0","9","Flag table","0","3","Operational"
119.00,"02","Instrumentation","002022","Satellite data-processing technique used",,"Flag table","0","0","8","Flag table","0","3","Operational"
120.00,"02","Instrumentation","002023","Satellite-derived wind computation method",,"Code table","0","0","4","Code table","0","2","Operational"
121.00,"02","Instrumentation","002024","Integrated mean humidity computational method",,"Code table","0","0","4","Code table","0","2","Operational"
122.00,"02","Instrumentation","002025","Satellite channel(s) used in computation",,"Flag table","0","0","25","Flag table","0","9","Operational"
123.00,"02","Instrumentation","002026","Cross-track resolution",,"m","2","0","12","m","2","4","Operational"
124.00,"02","Instrumentation","002027","Along-track resolution",,"m","2","0","12","m","2","4","Operational"
125.00,"02","Instrumentation","002028","Segment size at nadir in x-direction",,"m","0","0","18","m","0","6","Operational"
126.00,"02","Instrumentation","002029","Segment size at nadir in y-direction",,"m","0","0","18","m","0","6","Operational"
127.00,"02","Instrumentation","002030","Method of current measurement",,"Code table","0","0","3","Code table","0","1","Operational"
128.00,"02","Instrumentation","002031","Duration and time of current measurement",,"Code table","0","0","5","Code table","0","2","Operational"
129.00,"02","Instrumentation","002032","Indicator for digitization",,"Code table","0","0","2","Code table","0","1","Operational"
130.00,"02","Instrumentation","002033","Method of salinity/depth measurement",,"Code table","0","0","3","Code table","0","1","Operational"
131.00,"02","Instrumentation","002034","Drogue type",,"Code table","0","0","5","Code table","0","2","Operational"
132.00,"02","Instrumentation","002035","Cable length",,"m","0","0","9","m","0","3","Operational"
133.00,"02","Instrumentation","002036","Buoy type",,"Code table","0","0","2","Code table","0","1","Operational"
134.00,"02","Instrumentation","002037","Method of tidal observation",,"Code table","0","0","3","Code table","0","1","Operational"
135.00,"02","Instrumentation","002038","Method of water temperature and/or salinity measurement",,"Code table","0","0","4","Code table","0","2","Operational"
136.00,"02","Instrumentation","002039","Method of wet-bulb temperature measurement",,"Code table","0","0","3","Code table","0","1","Operational"
137.00,"02","Instrumentation","002040","Method of removing velocity and motion of platform from current",,"Code table","0","0","4","Code table","0","2","Operational"
138.00,"02","Instrumentation","002041","Method for estimating reports related to synoptic features",,"Code table","0","0","6","Code table","0","2","Operational"
139.00,"02","Instrumentation","002042","Indicator for sea surface current speed",,"Code table","0","0","2","Code table","0","1","Operational"
140.00,"02","Instrumentation","002044","Indicator for method of calculating spectral wave data",,"Code table","0","0","4","Code table","0","2","Operational"
141.00,"02","Instrumentation","002045","Indicator for type of platform",,"Code table","0","0","4","Code table","0","2","Operational"
142.00,"02","Instrumentation","002046","Wave measurement instrumentation",,"Code table","0","0","4","Code table","0","2","Operational"
143.00,"02","Instrumentation","002047","Deep-ocean tsunameter type",,"Code table","0","0","7","Code table","0","2","Operational"
144.00,"02","Instrumentation","002048","Satellite sensor indicator",,"Code table","0","0","4","Code table","0","2","Operational"
145.00,"02","Instrumentation","002049","Geostationary satellite data-processing technique used",,"Flag table","0","0","8","Flag table","0","3","Operational"
146.00,"02","Instrumentation","002050","Geostationary sounder satellite channels used",,"Flag table","0","0","20","Flag table","0","7","Operational"
147.00,"02","Instrumentation","002051","Indicator to specify observing method for extreme temperatures",,"Code table","0","0","4","Code table","0","2","Operational"
148.00,"02","Instrumentation","002052","Geostationary imager satellite channels used",,"Flag table","0","0","6","Flag table","0","2","Operational"
149.00,"02","Instrumentation","002053","GOES-I/M brightness temperature characteristics",,"Code table","0","0","4","Code table","0","2","Operational"
150.00,"02","Instrumentation","002054","GOES-I/M soundings parameter characteristics",,"Code table","0","0","4","Code table","0","2","Operational"
151.00,"02","Instrumentation","002055","Geostationary soundings statistical parameters",,"Code table","0","0","4","Code table","0","2","Operational"
152.00,"02","Instrumentation","002056","Geostationary soundings accuracy statistics",,"Code table","0","0","4","Code table","0","2","Operational"
153.00,"02","Instrumentation","002057","Origin of first-guess information for GOES-I/M soundings",,"Code table","0","0","4","Code table","0","2","Operational"
154.00,"02","Instrumentation","002058","Valid times of first guess information for GOES-I/M soundings",,"Code table","0","0","4","Code table","0","2","Operational"
155.00,"02","Instrumentation","002059","Origin of analysis information for GOES-I/M soundings",,"Code table","0","0","4","Code table","0","2","Operational"
156.00,"02","Instrumentation","002060","Origin of surface information for GOES-I/M soundings",,"Code table","0","0","4","Code table","0","2","Operational"
157.00,"02","Instrumentation","002061","Aircraft navigational system",,"Code table","0","0","3","Code table","0","1","Operational"
158.00,"02","Instrumentation","002062","Type of aircraft data relay system",,"Code table","0","0","4","Code table","0","2","Operational"
159.00,"02","Instrumentation","002063","Aircraft roll angle",,"deg","2","-18000","16","deg","2","5","Operational"
160.00,"02","Instrumentation","002064","Aircraft roll angle quality",,"Code table","0","0","2","Code table","0","1","Operational"
161.00,"02","Instrumentation","002065","ACARS ground-receiving station",,"CCITT IA5","0","0","40","Character","0","5","Operational"
162.00,"02","Instrumentation","002066","Radiosonde ground receiving system",,"Code table","0","0","6","Code table","0","2","Operational"
163.00,"02","Instrumentation","002067","Radiosonde operating frequency",,"Hz","-5","0","15","Hz","-5","5","Operational"
164.00,"02","Instrumentation","002070","Original specification of latitude/longitude",,"Code table","0","0","4","Code table","0","2","Operational"
165.00,"02","Instrumentation","002071","Spectrographic wavelength",,"m","13","0","30","m","13","10","Operational"
166.00,"02","Instrumentation","002072","Spectrographic width",,"m","13","0","30","m","13","10","Operational"
167.00,"02","Instrumentation","002080","Balloon manufacturer",,"Code table","0","0","6","Code table","0","2","Operational"
168.00,"02","Instrumentation","002081","Type of balloon",,"Code table","0","0","5","Code table","0","2","Operational"
169.00,"02","Instrumentation","002082","Weight of balloon",,"kg","3","0","12","kg","3","4","Operational"
170.00,"02","Instrumentation","002083","Type of balloon shelter",,"Code table","0","0","4","Code table","0","2","Operational"
171.00,"02","Instrumentation","002084","Type of gas used in balloon",,"Code table","0","0","4","Code table","0","2","Operational"
172.00,"02","Instrumentation","002085","Amount of gas used in balloon",,"kg","3","0","13","kg","3","4","Operational"
173.00,"02","Instrumentation","002086","Balloon flight train length",,"m","1","0","10","m","1","4","Operational"
174.00,"02","Instrumentation","002091","Entry sensor 4/20 mA",,"A","4","0","10","A","4","3","Operational"
175.00,"02","Instrumentation","002095","Type of pressure sensor",,"Code table","0","0","5","Code table","0","2","Operational"
176.00,"02","Instrumentation","002096","Type of temperature sensor",,"Code table","0","0","5","Code table","0","2","Operational"
177.00,"02","Instrumentation","002097","Type of humidity sensor",,"Code table","0","0","5","Code table","0","2","Operational"
179.00,"02","Instrumentation","002099","Polarization",,"Code table","0","0","3","Code table","0","1","Operational"
180.00,"02","Instrumentation","002100","Radar constant","**","dB","1","0","12","dB","1","4","Operational"
181.00,"02","Instrumentation","002101","Type of antenna",,"Code table","0","0","4","Code table","0","2","Operational"
182.00,"02","Instrumentation","002102","Antenna height above tower base",,"m","0","0","8","m","0","3","Operational"
183.00,"02","Instrumentation","002103","Radome",,"Flag table","0","0","2","Flag table","0","1","Operational"
184.00,"02","Instrumentation","002104","Antenna polarization",,"Code table","0","0","4","Code table","0","2","Operational"
185.00,"02","Instrumentation","002105","Maximum antenna gain",,"dB","0","0","6","dB","0","2","Operational"
186.00,"02","Instrumentation","002106","3-dB beamwidth",,"deg","1","0","6","deg","1","2","Operational"
187.00,"02","Instrumentation","002107","Sidelobe suppression",,"dB","0","0","6","dB","0","2","Operational"
188.00,"02","Instrumentation","002108","Crosspol discrimination (on axis)",,"dB","0","0","6","dB","0","2","Operational"
189.00,"02","Instrumentation","002109","Antenna speed (azimuth)",,"deg/s","2","0","12","deg/s","2","4","Operational"
190.00,"02","Instrumentation","002110","Antenna speed (elevation)",,"deg/s","2","0","12","deg/s","2","4","Operational"
191.00,"02","Instrumentation","002111","Radar incidence angle",,"deg","1","0","10","deg","1","4","Operational"
192.00,"02","Instrumentation","002112","Radar look angle",,"deg","1","0","12","deg","1","4","Operational"
193.00,"02","Instrumentation","002113","Number of azimuth looks",,"Numeric","0","0","4","Numeric","0","2","Operational"
194.00,"02","Instrumentation","002114","Antenna effective surface area",,"m2","0","0","15","m2","0","5","Operational"
195.00,"02","Instrumentation","002115","Type of surface observing equipment",,"Code table","0","0","5","Code table","0","2","Operational"
196.00,"02","Instrumentation","002116","Percentage of 320 MHz band processed",,"%","0","0","7","%","0","3","Operational"
197.00,"02","Instrumentation","002117","Percentage of 80 MHz band processed",,"%","0","0","7","%","0","3","Operational"
198.00,"02","Instrumentation","002118","Percentage of 20 MHz band processed",,"%","0","0","7","%","0","3","Operational"
199.00,"02","Instrumentation","002119","Instrument operations",,"Code table","0","0","3","Code table","0","1","Operational"
200.00,"02","Instrumentation","002120","Ocean wave frequency",,"Hz","3","0","10","Hz","3","4","Operational"
201.00,"02","Instrumentation","002121","Mean frequency",,"Hz","-8","0","7","Hz","-8","3","Operational"
202.00,"02","Instrumentation","002122","Frequency agility range",,"Hz","-6","-128","8","Hz","-6","3","Operational"
203.00,"02","Instrumentation","002123","Peak power",,"W","-4","0","7","W","-4","3","Operational"
204.00,"02","Instrumentation","002124","Average power",,"W","-1","0","7","W","-1","3","Operational"
205.00,"02","Instrumentation","002125","Pulse repetition frequency",,"Hz","-1","0","8","Hz","-1","3","Operational"
206.00,"02","Instrumentation","002126","Pulse width",,"s","7","0","6","s","7","2","Operational"
207.00,"02","Instrumentation","002127","Receiver intermediate frequency",,"Hz","-6","0","7","Hz","-6","3","Operational"
208.00,"02","Instrumentation","002128","Intermediate frequency bandwidth",,"Hz","-5","0","6","Hz","-5","2","Operational"
209.00,"02","Instrumentation","002129","Minimum detectable signal",,"dB","0","-150","5","dB","0","3","Operational"
210.00,"02","Instrumentation","002130","Dynamic range",,"dB","0","0","7","dB","0","3","Operational"
211.00,"02","Instrumentation","002131","Sensitivity time control (STC)",,"Flag table","0","0","2","Flag table","0","1","Operational"
212.00,"02","Instrumentation","002132","Azimuth pointing accuracy",,"deg","2","0","6","deg","2","2","Operational"
213.00,"02","Instrumentation","002133","Elevation pointing accuracy",,"deg","2","0","6","deg","2","2","Operational"
214.00,"02","Instrumentation","002134","Antenna beam azimuth",,"deg","2","0","16","deg","2","5","Operational"
215.00,"02","Instrumentation","002135","Antenna elevation",,"deg","2","-9000","15","deg","2","5","Operational"
216.00,"02","Instrumentation","002136","Range processed by range attenuation correction",,"m","-3","0","16","m","-3","5","Operational"
217.00,"02","Instrumentation","002137","Radar dual PRF ratio",,"Code table","0","0","4","Code table","0","2","Operational"
218.00,"02","Instrumentation","002138","Antenna rotation direction",,"Code table","0","0","2","Code table","0","1","Operational"
219.00,"02","Instrumentation","002139","SIRAL instrument configuration",,"Code table","0","0","2","Code table","0","1","Operational"
220.00,"02","Instrumentation","002140","Satellite radar beam azimuth angle",,"deg","0","0","9","deg","0","3","Operational"
221.00,"02","Instrumentation","002141","Measurement type","(see Note 4)","CCITT IA5","0","0","24","Character","0","3","Operational"
222.00,"02","Instrumentation","002142","Ozone instrument serial number/identification","(see Note 5)","CCITT IA5","0","0","32","Character","0","4","Operational"
223.00,"02","Instrumentation","002143","Ozone instrument type",,"Code table","0","0","7","Code table","0","3","Operational"
224.00,"02","Instrumentation","002144","Light source type for Brewer spectrophotometer",,"Code table","0","0","4","Code table","0","2","Operational"
225.00,"02","Instrumentation","002145","Wavelength setting for Dobson instruments",,"Code table","0","0","4","Code table","0","2","Operational"
226.00,"02","Instrumentation","002146","Source conditions for Dobson instruments",,"Code table","0","0","4","Code table","0","2","Operational"
228.00,"02","Instrumentation","002148","Data collection and/or location system",,"Code table","0","0","5","Code table","0","2","Operational"
229.00,"02","Instrumentation","002149","Type of data buoy",,"Code table","0","0","6","Code table","0","2","Operational"
230.00,"02","Instrumentation","002150","TOVS/ATOVS/AVHRR instrumentation channel number",,"Code table","0","0","6","Code table","0","2","Operational"
231.00,"02","Instrumentation","002151","Radiometer identifier",,"Code table","0","0","11","Code table","0","4","Operational"
232.00,"02","Instrumentation","002152","Satellite instrument used in data processing","(see Note 6)","Flag table","0","0","31","Flag table","0","10","Operational"
233.00,"02","Instrumentation","002153","Satellite channel centre frequency",,"Hz","-8","0","26","Hz","-8","8","Operational"
234.00,"02","Instrumentation","002154","Satellite channel band width",,"Hz","-8","0","26","Hz","-8","8","Operational"
235.00,"02","Instrumentation","002155","Satellite channel wavelength",,"m","9","0","16","m","9","5","Operational"
236.00,"02","Instrumentation","002156","Percentage of valid KU ocean retracker measurements",,"%","0","0","7","%","0","3","Operational"
237.00,"02","Instrumentation","002157","Percentage of valid S ocean retracker measurements",,"%","0","0","7","%","0","3","Operational"
238.00,"02","Instrumentation","002158","RA-2 instruments",,"Flag table","0","0","9","Flag table","0","3","Operational"
239.00,"02","Instrumentation","002159","MWR instruments",,"Flag table","0","0","8","Flag table","0","3","Operational"
240.00,"02","Instrumentation","002160","Wave length of the radar",,"Code table","0","0","4","Code table","0","2","Operational"
241.00,"02","Instrumentation","002163","Height assignment method",,"Code table","0","0","4","Code table","0","2","Operational"
242.00,"02","Instrumentation","002164","Tracer correlation method",,"Code table","0","0","3","Code table","0","1","Operational"
243.00,"02","Instrumentation","002165","Radiance type flags",,"Flag table","0","0","15","Flag table","0","5","Operational"
244.00,"02","Instrumentation","002166","Radiance type",,"Code table","0","0","4","Code table","0","2","Operational"
245.00,"02","Instrumentation","002167","Radiance computational method",,"Code table","0","0","4","Code table","0","2","Operational"
246.00,"02","Instrumentation","002168","Hydrostatic pressure of lower end of cable (thermistor string)",,"Pa","-3","0","16","kPa","0","5","Operational"
247.00,"02","Instrumentation","002169","Anemometer type",,"Code table","0","0","4","Code table","0","2","Operational"
248.00,"02","Instrumentation","002170","Aircraft humidity sensors",,"Code table","0","0","6","Code table","0","2","Operational"
249.00,"02","Instrumentation","002171","Instrument serial number for water temperature profile measurement",,"CCITT IA5","0","0","64","Character","0","8","Operational"
250.00,"02","Instrumentation","002172","Product type for retrieved atmospheric gases",,"Code table","0","0","8","Code table","0","3","Operational"
251.00,"02","Instrumentation","002173","Square of the off-nadir angle","(see Note 7)","deg2","4","0","10","deg2","4","4","Operational"
252.00,"02","Instrumentation","002174","Mean across track pixel number",,"Numeric","0","0","9","Numeric","0","3","Operational"
253.00,"02","Instrumentation","002175","Method of precipitation measurement",,"Code table","0","0","4","Code table","0","2","Operational"
254.00,"02","Instrumentation","002176","Method of state of ground measurement",,"Code table","0","0","4","Code table","0","2","Operational"
255.00,"02","Instrumentation","002177","Method of snow depth measurement",,"Code table","0","0","4","Code table","0","2","Operational"
256.00,"02","Instrumentation","002178","Method of liquid content measurement of precipitation",,"Code table","0","0","4","Code table","0","2","Operational"
257.00,"02","Instrumentation","002179","Type of sky condition algorithm",,"Code table","0","0","4","Code table","0","2","Operational"
258.00,"02","Instrumentation","002180","Main present weather detecting system",,"Code table","0","0","4","Code table","0","2","Operational"
259.00,"02","Instrumentation","002181","Supplementary present weather sensor",,"Flag table","0","0","21","Flag table","0","7","Operational"
260.00,"02","Instrumentation","002182","Visibility measurement system",,"Code table","0","0","4","Code table","0","2","Operational"
261.00,"02","Instrumentation","002183","Cloud detection system",,"Code table","0","0","4","Code table","0","2","Operational"
262.00,"02","Instrumentation","002184","Type of lightning detection sensor",,"Code table","0","0","4","Code table","0","2","Operational"
263.00,"02","Instrumentation","002185","Method of evaporation measurement",,"Code table","0","0","4","Code table","0","2","Operational"
264.00,"02","Instrumentation","002186","Capability to detect precipitation phenomena",,"Flag table","0","0","30","Flag table","0","10","Operational"
265.00,"02","Instrumentation","002187","Capability to detect other weather phenomena",,"Flag table","0","0","18","Flag table","0","6","Operational"
266.00,"02","Instrumentation","002188","Capability to detect obscuration",,"Flag table","0","0","21","Flag table","0","7","Operational"
267.00,"02","Instrumentation","002189","Capability to discriminate lightning strikes",,"Flag table","0","0","12","Flag table","0","4","Operational"
268.00,"02","Instrumentation","002190","Lagrangian drifter submergence (% time submerged)",,"%","0","0","7","%","0","3","Operational"
269.00,"02","Instrumentation","002191","Geopotential height calculation",,"Code table","0","0","4","Code table","0","2","Operational"
270.00,"04","Location (time)","004001","Year",,"a","0","0","12","a","0","4","Operational"
271.00,"04","Location (time)","004002","Month",,"mon","0","0","4","mon","0","2","Operational"
272.00,"04","Location (time)","004003","Day",,"d","0","0","6","d","0","2","Operational"
273.00,"04","Location (time)","004004","Hour",,"h","0","0","5","h","0","2","Operational"
274.00,"04","Location (time)","004005","Minute",,"min","0","0","6","min","0","2","Operational"
275.00,"04","Location (time)","004006","Second",,"s","0","0","6","s","0","2","Operational"
276.00,"04","Location (time)","004007","Seconds within a minute (microsecond accuracy)",,"s","6","0","26","s","6","8","Operational"
278.00,"04","Location (time)","004011","Time increment",,"a","0","-1024","11","a","0","4","Operational"
279.00,"04","Location (time)","004012","Time increment",,"mon","0","-1024","11","mon","0","4","Operational"
280.00,"04","Location (time)","004013","Time increment",,"d","0","-1024","11","d","0","4","Operational"
281.00,"04","Location (time)","004014","Time increment",,"h","0","-1024","11","h","0","4","Operational"
282.00,"04","Location (time)","004015","Time increment",,"min","0","-2048","12","min","0","4","Operational"
283.00,"04","Location (time)","004016","Time increment",,"s","0","-4096","13","s","0","4","Operational"
284.00,"04","Location (time)","004017","Reference time period for accumulated or extreme data",,"min","0","-1440","12","min","0","4","Operational"
285.00,"04","Location (time)","004021","Time period or displacement",,"a","0","-1024","11","a","0","4","Operational"
286.00,"04","Location (time)","004022","Time period or displacement",,"mon","0","-1024","11","mon","0","4","Operational"
287.00,"04","Location (time)","004023","Time period or displacement",,"d","0","-1024","11","d","0","4","Operational"
288.00,"04","Location (time)","004024","Time period or displacement",,"h","0","-2048","12","h","0","4","Operational"
289.00,"04","Location (time)","004025","Time period or displacement",,"min","0","-2048","12","min","0","4","Operational"
290.00,"04","Location (time)","004026","Time period or displacement",,"s","0","-4096","13","s","0","4","Operational"
291.00,"04","Location (time)","004031","Duration of time relating to following value",,"h","0","0","8","h","0","3","Operational"
292.00,"04","Location (time)","004032","Duration of time relating to following value",,"min","0","0","6","min","0","2","Operational"
293.00,"04","Location (time)","004041","Time difference, UTC - LMT","(see Note 6)","min","0","-1440","12","min","0","4","Operational"
294.00,"04","Location (time)","004043","Day of the year",,"d","0","0","9","d","0","3","Operational"
295.00,"04","Location (time)","004051","Principal time of daily reading of maximum temperature",,"h","0","0","5","h","0","2","Operational"
296.00,"04","Location (time)","004052","Principal time of daily reading of minimum temperature",,"h","0","0","5","h","0","2","Operational"
297.00,"04","Location (time)","004053","Number of days with precipitation equal to or more than 1 mm",,"Numeric","0","0"," 6","Numeric","0","2","Operational"
298.00,"04","Location (time)","004059","Times of observation used to compute the reported mean values",,"Flag table","0","0","6","Flag table","0","2","Operational"
299.00,"04","Location (time)","004065","Short time increment",,"min","0","-128","8","min","0","2","Operational"
300.00,"04","Location (time)","004066","Short time increment",,"s","0","-128","8","s","0","2","Operational"
301.00,"04","Location (time)","004073","Short time period or displacement",,"d","0","-128","8","d","0","2","Operational"
302.00,"04","Location (time)","004074","Short time period or displacement",,"h","0","-128","8","h","0","2","Operational"
303.00,"04","Location (time)","004075","Short time period or displacement",,"min","0","-128","8","min","0","2","Operational"
304.00,"04","Location (time)","004080","Averaging period for following value",,"Code table","0","0","4","Code table","0","2","Operational"
305.00,"04","Location (time)","004086","Long time period or displacement",,"s","0","-8192","15","s","0","5","Operational"
306.00,"05","Location (horizontal - 1)","005001","Latitude (high accuracy)",,"deg","5","-9000000","25","deg","5","7","Operational"
307.00,"05","Location (horizontal - 1)","005002","Latitude (coarse accuracy)",,"deg","2","-9000","15","deg","2","4","Operational"
308.00,"05","Location (horizontal - 1)","005011","Latitude increment (high accuracy)",,"deg","5","-9000000","25","deg","5","7","Operational"
309.00,"05","Location (horizontal - 1)","005012","Latitude increment (coarse accuracy)",,"deg","2","-9000","15","deg","2","4","Operational"
310.00,"05","Location (horizontal - 1)","005015","Latitude displacement (high accuracy)",,"deg","5","-9000000","25","deg","5","7","Operational"
311.00,"05","Location (horizontal - 1)","005016","Latitude displacement (coarse accuracy)",,"deg","2","-9000","15","deg","2","4","Operational"
312.00,"05","Location (horizontal - 1)","005021","Bearing or azimuth",,"degree true","2","0","16","degree true","2","5","Operational"
313.00,"05","Location (horizontal - 1)","005022","Solar azimuth",,"degree true","2","0","16","degree true","2","5","Operational"
314.00,"05","Location (horizontal - 1)","005023","Sun to satellite azimuth difference",,"deg","1","-1800","12","deg","1","4","Operational"
315.00,"05","Location (horizontal - 1)","005030","Direction (spectral)",,"deg","0","0","12","deg","0","4","Operational"
316.00,"05","Location (horizontal - 1)","005031","Row number",,"Numeric","0","0","12","Numeric","0","4","Operational"
317.00,"05","Location (horizontal - 1)","005033","Pixel size on horizontal - 1",,"m","-1","0","16","m","-1","5","Operational"
318.00,"05","Location (horizontal - 1)","005034","Along track row number",,"Numeric","0","0","11","Numeric","0","4","Operational"
319.00,"05","Location (horizontal - 1)","005035","Maximum size of x-dimension",,"Numeric","0","0","12","Numeric","0","4","Operational"
320.00,"05","Location (horizontal - 1)","005036","Ship transect number according to SOOP",,"Numeric","0","0","7","Numeric","0","2","Operational"
321.00,"05","Location (horizontal - 1)","005040","Orbit number",,"Numeric","0","0","24","Numeric","0","8","Operational"
322.00,"05","Location (horizontal - 1)","005041","Scan line number",,"Numeric","0","0","8","Numeric","0","3","Operational"
323.00,"05","Location (horizontal - 1)","005042","Channel number",,"Numeric","0","0","6","Numeric","0","2","Operational"
324.00,"05","Location (horizontal - 1)","005043","Field of view number",,"Numeric","0","0","8","Numeric","0","3","Operational"
325.00,"05","Location (horizontal - 1)","005044","Satellite cycle number",,"Numeric","0","0","11","Numeric","0","4","Operational"
326.00,"05","Location (horizontal - 1)","005045","Field of regard number",,"Numeric","0","0","8","Numeric","0","3","Operational"
327.00,"05","Location (horizontal - 1)","005052","Channel number increment",,"Numeric","0","0","5","Numeric","0","2","Operational"
328.00,"05","Location (horizontal - 1)","005053","Field of view number increment",,"Numeric","0","0","5","Numeric","0","2","Operational"
329.00,"05","Location (horizontal - 1)","005060","Y angular position from centre of gravity",,"deg","6","-8000000","24","deg","6","8","Operational"
330.00,"05","Location (horizontal - 1)","005061","Z angular position from centre of gravity",,"deg","6","-8000000","24","deg","6","8","Operational"
331.00,"06","Location (horizontal - 2)","006001","Longitude (high accuracy)",,"deg","5","-18000000","26","deg","5","8","Operational"
332.00,"06","Location (horizontal - 2)","006002","Longitude (coarse accuracy)",,"deg","2","-18000","16","deg","2","5","Operational"
333.00,"06","Location (horizontal - 2)","006011","Longitude increment (high accuracy)",,"deg","5","-18000000","26","deg","5","8","Operational"
334.00,"06","Location (horizontal - 2)","006012","Longitude increment (coarse accuracy)",,"deg","2","-18000","16","deg","2","5","Operational"
335.00,"06","Location (horizontal - 2)","006015","Longitude displacement (high accuracy)",,"deg","5","-18000000","26","deg","5","8","Operational"
336.00,"06","Location (horizontal - 2)","006016","Longitude displacement (coarse accuracy)",,"deg","2","-18000","16","deg","2","5","Operational"
337.00,"06","Location (horizontal - 2)","006021","Distance",,"m","-1","0","13","m","-1","4","Operational"
338.00,"06","Location (horizontal - 2)","006029","Wave number",,"m-1","1","0","22","m-1","1","7","Operational"
339.00,"06","Location (horizontal - 2)","006030","Wave number (spectral)",,"rad/m","5","0","13","rad/m","5","4","Operational"
340.00,"06","Location (horizontal - 2)","006031","Column number",,"Numeric","0","0","12","Numeric","0","4","Operational"
341.00,"06","Location (horizontal - 2)","006033","Pixel size on horizontal - 2",,"m","-1","0","16","m","-1","5","Operational"
342.00,"06","Location (horizontal - 2)","006034","Cross-track cell number",,"Numeric","0","0","7","Numeric","0","3","Operational"
343.00,"06","Location (horizontal - 2)","006035","Maximum size of y-dimension",,"Numeric","0","0","12","Numeric","0","4","Operational"
344.00,"06","Location (horizontal - 2)","006040","Radius of confidence",,"m","0","0","13","m","0","4","Operational"
345.00,"07","Location (vertical)","007001","Height of station","(see Note 1)","m","0","-400","15","m","0","5","Operational"
346.00,"07","Location (vertical)","007002","Height or altitude",,"m","-1","-40","16","m","-1","5","Operational"
347.00,"07","Location (vertical)","007003","Geopotential",,"m2 s-2","-1","-400","17","m2 s-2","-1","6","Operational"
348.00,"07","Location (vertical)","007004","Pressure",,"Pa","-1","0","14","Pa","-1","5","Operational"
349.00,"07","Location (vertical)","007005","Height increment",,"m","0","-400","12","m","0","4","Operational"
350.00,"07","Location (vertical)","007006","Height above station",,"m","0","0","15","m","0","5","Operational"
351.00,"07","Location (vertical)","007007","Height",,"m","0","-1000","17","m","0","6","Operational"
352.00,"07","Location (vertical)","007008","Geopotential",,"m2 s-2","0","-10000","20","m2 s-2","0","7","Operational"
353.00,"07","Location (vertical)","007009","Geopotential height",,"gpm","0","-1000","17","gpm","0","5","Operational"
354.00,"07","Location (vertical)","007010","Flight level",,"m","0","-1024","16","ft","-1","5","Operational"
356.00,"07","Location (vertical)","007012","Grid point altitude",,"m","2","-50000","20","m","2","7","Operational"
357.00,"07","Location (vertical)","007021","Elevation","(see Note 2)","deg","2","-9000","15","deg","2","5","Operational"
358.00,"07","Location (vertical)","007022","Solar elevation",,"deg","2","-9000","15","deg","2","5","Operational"
359.00,"07","Location (vertical)","007024","Satellite zenith angle",,"deg","2","-9000","15","deg","2","5","Operational"
360.00,"07","Location (vertical)","007025","Solar zenith angle",,"deg","2","-9000","15","deg","2","5","Operational"
361.00,"07","Location (vertical)","007026","Satellite zenith angle",,"deg","4","-900000","21","deg","4","7","Operational"
362.00,"07","Location (vertical)","007030","Height of station ground above mean sea level","(see Note 3)","m","1","-4000","17","m","1","5","Operational"
363.00,"07","Location (vertical)","007031","Height of barometer above mean sea level","(see Note 4)","m","1","-4000","17","m","1","5","Operational"
364.00,"07","Location (vertical)","007032","Height of sensor above local ground (or deck of marine platform)","(see Note 5)","m","2","0","16","m","2","5","Operational"
365.00,"07","Location (vertical)","007033","Height of sensor above water surface","(see Note 6)","m","1","0","12","m","1","4","Operational"
366.00,"07","Location (vertical)","007035","Maximum size of z-dimension",,"Numeric","0","0","12","Numeric","0","4","Operational"
367.00,"07","Location (vertical)","007036","Level index of z",,"Numeric","0","0","12","Numeric","0","4","Operational"
368.00,"07","Location (vertical)","007040","Impact parameter","(see Note 7)","m","1","62000000","22","m","1","8","Operational"
369.00,"07","Location (vertical)","007061","Depth below land surface",,"m","2","0","14","m","2","5","Operational"
370.00,"07","Location (vertical)","007062","Depth below sea/water surface",,"m","1","0","17","m","1","6","Operational"
371.00,"07","Location (vertical)","007063","Depth below sea/water surface (cm)",,"m","2","0","20","m","2","7","Operational"
372.00,"07","Location (vertical)","007064","Representative height of sensor above station","(see Note 8)","m","0","0","4","m","0","2","Operational"
373.00,"07","Location (vertical)","007065","Water pressure",,"Pa","-3","0","17","Pa","-3","6","Operational"
374.00,"07","Location (vertical)","007070","Drogue depth",,"m","0","0","10","m","0","4","Operational"
375.00,"08","Significance qualifiers","008001","Vertical sounding significance",,"Flag table","0","0","7","Flag table","0","3","Operational"
376.00,"08","Significance qualifiers","008002","Vertical significance (surface observations)",,"Code table","0","0","6","Code table","0","2","Operational"
377.00,"08","Significance qualifiers","008003","Vertical significance (satellite observations)",,"Code table","0","0","6","Code table","0","2","Operational"
378.00,"08","Significance qualifiers","008004","Phase of aircraft flight",,"Code table","0","0","3","Code table","0","1","Operational"
379.00,"08","Significance qualifiers","008005","Meteorological attribute significance",,"Code table","0","0","4","Code table","0","2","Operational"
380.00,"08","Significance qualifiers","008006","Ozone vertical sounding significance",,"Flag table","0","0","9","Flag table","0","3","Operational"
381.00,"08","Significance qualifiers","008007","Dimensional significance",,"Code table","0","0","4","Code table","0","2","Operational"
382.00,"08","Significance qualifiers","008008","Radiation vertical sounding significance",,"Flag table","0","0","9","Flag table","0","3","Operational"
383.00,"08","Significance qualifiers","008009","Detailed phase of flight",,"Code table","0","0","4","Code table","0","2","Operational"
384.00,"08","Significance qualifiers","008010","Surface qualifier (temperature data)",,"Code table","0","0","5","Code table","0","2","Operational"
385.00,"08","Significance qualifiers","008011","Meteorological feature",,"Code table","0","0","6","Code table","0","2","Operational"
386.00,"08","Significance qualifiers","008012","Land/sea qualifier",,"Code table","0","0","2","Code table","0","1","Operational"
387.00,"08","Significance qualifiers","008013","Day/night qualifier",,"Code table","0","0","2","Code table","0","1","Operational"
388.00,"08","Significance qualifiers","008014","Qualifier for runway visual range",,"Code table","0","0","4","Code table","0","2","Operational"
390.00,"08","Significance qualifiers","008016","Change qualifier of a trend-type forecast or an aerodrome forecast",,"Code table","0","0","3","Code table","0","1","Operational"
391.00,"08","Significance qualifiers","008017","Qualifier of the time when the forecast change is expected",,"Code table","0","0","2","Code table","0","1","Operational"
392.00,"08","Significance qualifiers","008018","SEAWINDS land/ice surface type",,"Flag table","0","0","17","Flag table","0","6","Operational"
393.00,"08","Significance qualifiers","008019","Qualifier for following centre identifier",,"Code table","0","0","4","Code table","0","2","Operational"
394.00,"08","Significance qualifiers","008020","Total number of missing entities (with respect to accumulation or average)",,"Numeric","0","0","16","Numeric","0","5","Operational"
395.00,"08","Significance qualifiers","008021","Time significance",,"Code table","0","0","5","Code table","0","2","Operational"
396.00,"08","Significance qualifiers","008022","Total number (with respect to accumulation or average)",,"Numeric","0","0","16","Numeric","0","5","Operational"
397.00,"08","Significance qualifiers","008023","First-order statistics",,"Code table","0","0","6","Code table","0","2","Operational"
398.00,"08","Significance qualifiers","008024","Difference statistics",,"Code table","0","0","6","Code table","0","2","Operational"
399.00,"08","Significance qualifiers","008025","Time difference qualifier","(see Note 5)","Code table","0","0","4","Code table","0","2","Operational"
400.00,"08","Significance qualifiers","008026","Matrix significance",,"Code table","0","0","6","Code table","0","2","Operational"
402.00,"08","Significance qualifiers","008029","Surface type",,"Code table","0","0","8","Code table","0","3","Operational"
403.00,"08","Significance qualifiers","008030","Manual on Codes (Volume I.1, Section C) Code table from which data are derived",,"Numeric","0","0","13","Numeric","0","4","Operational"
404.00,"08","Significance qualifiers","008031","Data category - CREX table A",,"Numeric","0","0","8","Numeric","0","3","Operational"
406.00,"08","Significance qualifiers","008033","Method of derivation of percentage confidence","(see Note 6)","Code table","0","0","7","Code table","0","3","Operational"
407.00,"08","Significance qualifiers","008035","Type of monitoring exercise",,"Code table","0","0","3","Code table","0","1","Operational"
408.00,"08","Significance qualifiers","008036","Type of centre or station performing monitoring",,"Code table","0","0","3","Code table","0","1","Operational"
409.00,"08","Significance qualifiers","008039","Time significance (Aviation forecast)",,"Code table","0","0","6","Code table","0","2","Operational"
410.00,"08","Significance qualifiers","008040","Flight level significance",,"Code table","0","0","6","Code table","0","2","Operational"
411.00,"08","Significance qualifiers","008041","Data significance",,"Code table","0","0","5","Code table","0","2","Operational"
412.00,"08","Significance qualifiers","008042","Extended vertical sounding significance",,"Flag table","0","0","18","Flag table","0","6","Operational"
413.00,"08","Significance qualifiers","008043","Atmospheric chemical or physical constituent type",,"Code table","0","0","8","Code table","0","3","Operational"
416.00,"08","Significance qualifiers","008046","Atmospheric chemical or physical constituent type",,"Common Code table C-14","0","0","16","Common Code table C-14","0","5","Operational"
417.00,"08","Significance qualifiers","008049","Number of observations",,"Numeric","0","0","8","Numeric","0","3","Operational"
418.00,"08","Significance qualifiers","008050","Qualifier for number of missing values in calculation of statistic",,"Code table","0","0","4","Code table","0","2","Operational"
419.00,"08","Significance qualifiers","008051","Qualifier for number of missing values in calculation of statistic",,"Code table","0","0","3","Code table","0","1","Operational"
420.00,"08","Significance qualifiers","008052","Condition for which number of days of occurrence follows",,"Code table","0","0","5","Code table","0","2","Operational"
421.00,"08","Significance qualifiers","008053","Day of occurrence qualifier",,"Code table","0","0","2","Code table","0","1","Operational"
422.00,"08","Significance qualifiers","008054","Qualifier for wind speed or wind gusts",,"Code table","0","0","3","Code table","0","1","Operational"
423.00,"08","Significance qualifiers","008060","Sample scanning mode significance",,"Code table","0","0","4","Code table","0","2","Operational"
424.00,"08","Significance qualifiers","008065","Sun-glint indicator",,"Code table","0","0","2","Code table","0","1","Operational"
425.00,"08","Significance qualifiers","008066","Semi-transparency indicator",,"Code table","0","0","2","Code table","0","1","Operational"
426.00,"08","Significance qualifiers","008070","TOVS/ATOVS product qualifier",,"Code table","0","0","4","Code table","0","2","Operational"
427.00,"08","Significance qualifiers","008072","Pixel(s) type",,"Code table","0","0","3","Code table","0","1","Operational"
428.00,"08","Significance qualifiers","008074","Altimeter echo type",,"Code table","0","0","2","Code table","0","1","Operational"
429.00,"08","Significance qualifiers","008075","Ascending/descending orbit qualifier",,"Code table","0","0","2","Code table","0","1","Operational"
430.00,"08","Significance qualifiers","008076","Type of band",,"Code table","0","0","6","Code table","0","2","Operational"
431.00,"08","Significance qualifiers","008077","Radiometer sensed surface type",,"Code table","0","0","7","Code table","0","3","Operational"
432.00,"08","Significance qualifiers","008079","Product status",,"Code table","0","0","4","Code table","0","2","Operational"
433.00,"08","Significance qualifiers","008080","Qualifier for GTSPP quality flag",,"Code table","0","0","6","Code table","0","2","Operational"
434.00,"08","Significance qualifiers","008081","Type of equipment",,"Code table","0","0","6","Code table","0","2","Operational"
435.00,"08","Significance qualifiers","008082","Modification of sensor height to another value",,"Code table","0","0","3","Code table","0","1","Operational"
436.00,"08","Significance qualifiers","008083","Nominal value indicator",,"Flag table","0","0","15","Flag table","0","5","Operational"
437.00,"08","Significance qualifiers","008085","Beam identifier",,"Code table","0","0","3","Code table","0","1","Operational"
438.00,"08","Significance qualifiers","008086","Vertical significance for NWP",,"Flag table","0","0","12","Flag table","0","4","Operational"
439.00,"08","Significance qualifiers","008090","Decimal scale of following significands",,"Numeric","0","-127","8","Numeric","0","3","Operational"
440.00,"10","Non-coordinate location (vertical)","010001","Height of land surface",,"m","0","-400","15","m","0","5","Operational"
441.00,"10","Non-coordinate location (vertical)","010002","Height",,"m","-1","-40","16","m","-1","5","Operational"
442.00,"10","Non-coordinate location (vertical)","010003","Geopotential",,"m2 s-2","-1","-400","17","m2 s-2","-1","6","Operational"
443.00,"10","Non-coordinate location (vertical)","010004","Pressure",,"Pa","-1","0","14","Pa","-1","5","Operational"
444.00,"10","Non-coordinate location (vertical)","010007","Height",,"m","0","-1000","17","m","0","6","Operational"
445.00,"10","Non-coordinate location (vertical)","010008","Geopotential",,"m2 s-2","0","-10000","20","m2 s-2","0","7","Operational"
446.00,"10","Non-coordinate location (vertical)","010009","Geopotential height",,"gpm","0","-1000","17","gpm","0","5","Operational"
447.00,"10","Non-coordinate location (vertical)","010010","Minimum pressure reduced to mean sea level",,"Pa","-1","0","14","Pa","-1","5","Operational"
448.00,"10","Non-coordinate location (vertical)","010011","Maximum pressure reduced to mean sea level",,"Pa","-1","0","14","Pa","-1","5","Operational"
449.00,"10","Non-coordinate location (vertical)","010031","In direction of the North Pole, distance from the Earth's centre","(see Notes 2 and 3)","m","2","-1073741824","31","m","2","10","Operational"
450.00,"10","Non-coordinate location (vertical)","010032","Satellite distance to Earth's centre",,"m","1","0","27","m","2","9","Operational"
451.00,"10","Non-coordinate location (vertical)","010033","Altitude (platform to ellipsoid)",,"m","1","0","27","m","2","9","Operational"
452.00,"10","Non-coordinate location (vertical)","010034","Earth's radius",,"m","1","0","27","m","2","9","Operational"
453.00,"10","Non-coordinate location (vertical)","010035","Earth's local radius of curvature",,"m","1","62000000","22","m","1","8","Operational"
454.00,"10","Non-coordinate location (vertical)","010036","Geoid undulation","(see Note 4)","m","2","-15000","15","m","2","6","Operational"
455.00,"10","Non-coordinate location (vertical)","010040","Number of retrieved layers",,"Numeric","0","0","10","Numeric","0","4","Operational"
456.00,"10","Non-coordinate location (vertical)","010050","Standard deviation altitude",,"m","2","0","16","m","2","5","Operational"
457.00,"10","Non-coordinate location (vertical)","010051","Pressure reduced to mean sea level",,"Pa","-1","0","14","Pa","-1","5","Operational"
458.00,"10","Non-coordinate location (vertical)","010052","Altimeter setting (QNH)",,"Pa","-1","0","14","Pa","-1","5","Operational"
459.00,"10","Non-coordinate location (vertical)","010053","Global navigation satellite system altitude",,"m","0","-1000","17","m","0","5","Operational"
460.00,"10","Non-coordinate location (vertical)","010060","Pressure change",,"Pa","-1","-1024","11","Pa","-1","4","Operational"
461.00,"10","Non-coordinate location (vertical)","010061","3-hour pressure change",,"Pa","-1","-500","10","Pa","-1","4","Operational"
462.00,"10","Non-coordinate location (vertical)","010062","24-hour pressure change",,"Pa","-1","-1000","11","Pa","-1","4","Operational"
463.00,"10","Non-coordinate location (vertical)","010063","Characteristic of pressure tendency",,"Code table","0","0","4","Code table","0","2","Operational"
464.00,"10","Non-coordinate location (vertical)","010064","SIGMET cruising level",,"Code table","0","0","3","Code table","0","1","Operational"
465.00,"10","Non-coordinate location (vertical)","010070","Indicated aircraft altitude",,"m","0","-400","16","m","0","5","Operational"
466.00,"10","Non-coordinate location (vertical)","010079","Off nadir angle of the satellite from platform data",,"deg","4","0","16","deg","4","5","Operational"
467.00,"10","Non-coordinate location (vertical)","010080","Viewing zenith angle",,"deg","2","-9000","15","deg","2","5","Operational"
468.00,"10","Non-coordinate location (vertical)","010081","Altitude of COG above reference ellipsoid",,"m","3","0","31","m","3","10","Operational"
469.00,"10","Non-coordinate location (vertical)","010082","Instantaneous altitude rate",,"m/s","3","-65536","17","m/s","3","6","Operational"
470.00,"10","Non-coordinate location (vertical)","010083","Squared off nadir angle of the satellite from platform data",,"deg2","2","0","16","deg2","2","5","Operational"
471.00,"10","Non-coordinate location (vertical)","010084","Squared off nadir angle of the satellite from waveform data",,"deg2","2","0","16","deg2","2","5","Operational"
472.00,"10","Non-coordinate location (vertical)","010085","Mean sea surface height",,"m","3","-131072","18","m","3","6","Operational"
473.00,"10","Non-coordinate location (vertical)","010086","Geoid's height",,"m","3","-131072","18","m","3","6","Operational"
474.00,"10","Non-coordinate location (vertical)","010087","Ocean depth/land elevation",,"m","1","-131072","18","m","1","6","Operational"
475.00,"10","Non-coordinate location (vertical)","010088","Total geocentric ocean tide height (solution 1)",,"m","3","-32768","16","m","3","5","Operational"
476.00,"10","Non-coordinate location (vertical)","010089","Total geocentric ocean tide height (solution 2)",,"m","3","-32768","16","m","3","5","Operational"
477.00,"10","Non-coordinate location (vertical)","010090","Long period tide height",,"m","3","-32768","16","m","3","5","Operational"
478.00,"10","Non-coordinate location (vertical)","010091","Tidal loading height",,"m","3","-32768","16","m","3","5","Operational"
479.00,"10","Non-coordinate location (vertical)","010092","Solid Earth tide height",,"m","3","-32768","16","m","3","5","Operational"
480.00,"10","Non-coordinate location (vertical)","010093","Geocentric pole tide height",,"m","3","-32768","16","m","3","5","Operational"
481.00,"10","Non-coordinate location (vertical)","010095","Height of atmosphere used",,"m","0","0","16","m","0","5","Operational"
482.00,"10","Non-coordinate location (vertical)","010096","Mean dynamic topography",,"m","3","-131072","18","m","3","6","Operational"
483.00,"10","Non-coordinate location (vertical)","010097","Mean sea surface height from altimeter only",,"m","3","-131072","18","m","3","6","Operational"
484.00,"10","Non-coordinate location (vertical)","010098","Loading tide height geocentric ocean tide solution 1",,"m","4","-2000","12","m","4","4","Operational"
485.00,"10","Non-coordinate location (vertical)","010099","Loading tide height geocentric ocean tide solution 2",,"m","4","-2000","12","m","4","4","Operational"
486.00,"10","Non-coordinate location (vertical)","010100","Non-equilibrium long period tide height",,"m","4","-2000","12","m","4","4","Operational"
487.00,"10","Non-coordinate location (vertical)","010101","Squared off nadir angle of the satellite from waveform data",,"deg2","2","-32768","16","deg2","2","5","Operational"
488.00,"10","Non-coordinate location (vertical)","010102","Sea surface height anomaly",,"m","3","-32768","16","m","3","5","Operational"
489.00,"11","Wind and turbulence","011001","Wind direction",,"degree true","0","0","9","degree true","0","3","Operational"
490.00,"11","Wind and turbulence","011002","Wind speed",,"m/s","1","0","12","m/s","1","4","Operational"
491.00,"11","Wind and turbulence","011003","u-component",,"m/s","1","-4096","13","m/s","1","4","Operational"
492.00,"11","Wind and turbulence","011004","v-component",,"m/s","1","-4096","13","m/s","1","4","Operational"
493.00,"11","Wind and turbulence","011005","w-component",,"Pa/s","1","-512","10","Pa/s","1","4","Operational"
494.00,"11","Wind and turbulence","011006","w-component",,"m/s","2","-4096","13","m/s","2","4","Operational"
495.00,"11","Wind and turbulence","011010","Wind direction associated with wind speed which follows",,"degree true","0","0","9","degree true","0","3","Operational"
496.00,"11","Wind and turbulence","011011","Wind direction at 10 m",,"degree true","0","0","9","degree true","0","3","Operational"
497.00,"11","Wind and turbulence","011012","Wind speed at 10 m",,"m/s","1","0","12","m/s","1","4","Operational"
498.00,"11","Wind and turbulence","011013","Wind direction at 5 m",,"degree true","0","0","9","degree true","0","3","Operational"
499.00,"11","Wind and turbulence","011014","Wind speed at 5 m",,"m/s","1","0","12","m/s","1","4","Operational"
500.00,"11","Wind and turbulence","011016","Extreme counterclockwise wind direction of a variable wind",,"degree true","0","0","9","degree true","0","3","Operational"
501.00,"11","Wind and turbulence","011017","Extreme clockwise wind direction of a variable wind",,"degree true","0","0","9","degree true","0","3","Operational"
502.00,"11","Wind and turbulence","011019","Steadiness of wind","(see Note 6)","%","0","0","7","%","0","3","Operational"
503.00,"11","Wind and turbulence","011021","Relative vorticity",,"/s","9","-65536","17","/s","9","6","Operational"
504.00,"11","Wind and turbulence","011022","Divergence",,"/s","9","-65536","17","/s","9","6","Operational"
505.00,"11","Wind and turbulence","011023","Velocity potential",,"m2/s","-2","-65536","17","m2/s","-2","6","Operational"
506.00,"11","Wind and turbulence","011030","Extended degree of turbulence",,"Code table","0","0","6","Code table","0","2","Operational"
507.00,"11","Wind and turbulence","011031","Degree of turbulence",,"Code table","0","0","4","Code table","0","2","Operational"
508.00,"11","Wind and turbulence","011032","Height of base of turbulence",,"m","-1","-40","16","m","-1","5","Operational"
509.00,"11","Wind and turbulence","011033","Height of top of turbulence",,"m","-1","-40","16","m","-1","5","Operational"
510.00,"11","Wind and turbulence","011034","Vertical gust velocity",,"m/s","1","-1024","11","m/s","1","4","Operational"
511.00,"11","Wind and turbulence","011035","Vertical gust acceleration",,"m s-2","2","-8192","14","m s-2","2","5","Operational"
512.00,"11","Wind and turbulence","011036","Maximum derived equivalent vertical gust speed",,"m/s","1","0","10","m/s","1","4","Operational"
513.00,"11","Wind and turbulence","011037","Turbulence index",,"Code table","0","0","6","Code table","0","2","Operational"
514.00,"11","Wind and turbulence","011038","Time of occurrence of peak eddy dissipation rate",,"Code table","0","0","5","Code table","0","2","Operational"
515.00,"11","Wind and turbulence","011039","Extended time of occurrence of peak eddy dissipation rate",,"Code table","0","0","6","Code table","0","2","Operational"
516.00,"11","Wind and turbulence","011040","Maximum wind speed (mean wind)",,"m/s","1","0","12","m/s","1","4","Operational"
517.00,"11","Wind and turbulence","011041","Maximum wind gust speed",,"m/s","1","0","12","m/s","1","4","Operational"
518.00,"11","Wind and turbulence","011042","Maximum wind speed (10-minute mean wind)",,"m/s","1","0","12","m/s","1","4","Operational"
519.00,"11","Wind and turbulence","011043","Maximum wind gust direction",,"degree true","0","0","9","degree true","0","3","Operational"
520.00,"11","Wind and turbulence","011044","Mean wind direction for surface - 1 500 m (5 000 feet)",,"degree true","0","0","9","degree true","0","3","Operational"
521.00,"11","Wind and turbulence","011045","Mean wind speed for surface - 1 500 m (5 000 feet)",,"m/s","1","0","12","m/s","1","4","Operational"
522.00,"11","Wind and turbulence","011046","Maximum instantaneous wind speed",,"m/s","1","0","12","m/s","1","4","Operational"
523.00,"11","Wind and turbulence","011047","Maximum instantaneous wind speed over 10 minutes",,"m/s","1","0","12","m/s","1","4","Operational"
524.00,"11","Wind and turbulence","011049","Standard deviation of wind direction",,"degree true","0","0","9","degree true","0","3","Operational"
525.00,"11","Wind and turbulence","011050","Standard deviation of horizontal wind speed",,"m/s","1","0","12","m/s","1","4","Operational"
526.00,"11","Wind and turbulence","011051","Standard deviation of vertical wind speed",,"m/s","1","0","8","m/s","1","3","Operational"
527.00,"11","Wind and turbulence","011052","Formal uncertainty in wind speed",,"m/s","2","0","13","m/s","2","5","Operational"
528.00,"11","Wind and turbulence","011053","Formal uncertainty in wind direction",,"degree true","2","0","15","degree true","2","5","Operational"
529.00,"11","Wind and turbulence","011054","Mean wind direction for 1 500 - 3 000 m",,"degree true","0","0","9","degree true","0","3","Operational"
530.00,"11","Wind and turbulence","011055","Mean wind speed for 1 500 - 3 000 m",,"m/s","1","0","12","m/s","1","4","Operational"
531.00,"11","Wind and turbulence","011061","Absolute wind shear in 1 km layer below",,"m/s","1","0","12","m/s","1","4","Operational"
532.00,"11","Wind and turbulence","011062","Absolute wind shear in 1 km layer above",,"m/s","1","0","12","m/s","1","4","Operational"
533.00,"11","Wind and turbulence","011070","Designator of the runway affected by wind shear (including ALL)",,"CCITT IA5","0","0","32","Character","0","4","Operational"
534.00,"11","Wind and turbulence","011071","Turbulent vertical momentum flux",,"m2 s-2","3","-128","14","m2 s-2","3","5","Operational"
535.00,"11","Wind and turbulence","011072","Turbulent vertical buoyancy flux",,"K m s-1","3","-128","11","K m s-1","3","4","Operational"
536.00,"11","Wind and turbulence","011073","Turbulent kinetic energy",,"m2 s-2","2","-1024","13","m2 s-2","2","4","Operational"
537.00,"11","Wind and turbulence","011074","Dissipation energy",,"m2 s-2","2","-1024","10","m2 s-2","2","4","Operational"
538.00,"11","Wind and turbulence","011075","Mean turbulence intensity (eddy dissipation rate)",,"m2/3 s-1","2","0","8","m2/3 s-1","2","3","Operational"
539.00,"11","Wind and turbulence","011076","Peak turbulence intensity (eddy dissipation rate)",,"m2/3 s-1","2","0","8","m2/3 s-1","2","3","Operational"
540.00,"11","Wind and turbulence","011077","Reporting interval or averaging time for eddy dissipation rate",,"s","0","0","12","s","0","4","Operational"
541.00,"11","Wind and turbulence","011081","Model wind direction at 10 m",,"degree true","2","0","16","degree true","2","5","Operational"
542.00,"11","Wind and turbulence","011082","Model wind speed at 10 m",,"m/s","2","0","14","m/s","2","4","Operational"
543.00,"11","Wind and turbulence","011083","Wind speed",,"km/h","0","0","9","km/h","0","3","Operational"
544.00,"11","Wind and turbulence","011084","Wind speed",,"kt","0","0","8","kt","0","3","Operational"
545.00,"11","Wind and turbulence","011085","Maximum wind gust speed",,"km/h","0","0","9","km/h","0","3","Operational"
546.00,"11","Wind and turbulence","011086","Maximum wind gust speed",,"kt","0","0","8","kt","0","3","Operational"
547.00,"11","Wind and turbulence","011095","u-component of the model wind vector",,"m/s","1","-4096","13","m/s","1","4","Operational"
548.00,"11","Wind and turbulence","011096","v-component of the model wind vector",,"m/s","1","-4096","13","m/s","1","4","Operational"
549.00,"11","Wind and turbulence","011097","Wind speed from altimeter",,"m/s","2","0","12","m/s","2","4","Operational"
550.00,"11","Wind and turbulence","011098","Wind speed from radiometer",,"m/s","2","0","12","m/s","2","4","Operational"
551.00,"11","Wind and turbulence","011100","Aircraft true airspeed",,"m/s","1","0","12","m/s","1","4","Operational"
552.00,"11","Wind and turbulence","011101","Aircraft ground speed u-component",,"m/s","1","-4096","13","m/s","1","4","Operational"
553.00,"11","Wind and turbulence","011102","Aircraft ground speed v-component",,"m/s","1","-4096","13","m/s","1","4","Operational"
554.00,"11","Wind and turbulence","011103","Aircraft ground speed w-component",,"m/s","1","-512","10","m/s","1","3","Operational"
555.00,"11","Wind and turbulence","011104","Aircraft true heading",,"degree true","0","0","9","degree true","0","3","Operational"
556.00,"11","Wind and turbulence","011105","EDR algorithm version",,"Numeric","0","0","6","Numeric","0","2","Operational"
557.00,"11","Wind and turbulence","011106","Running minimum confidence",,"Numeric","1","0","4","Numeric","1","2","Operational"
558.00,"11","Wind and turbulence","011107","Maximum number bad inputs",,"Numeric","0","0","5","Numeric","0","2","Operational"
559.00,"11","Wind and turbulence","011108","Peak location",,"Numeric","1","0","4","Numeric","1","2","Operational"
560.00,"11","Wind and turbulence","011109","Number of good EDR",,"Numeric","0","0","4","Numeric","0","2","Operational"
561.00,"12","Temperature","012001","Temperature/air temperature",,"K","1","0","12","C","1","3","Operational"
562.00,"12","Temperature","012002","Wet-bulb temperature",,"K","1","0","12","C","1","3","Operational"
563.00,"12","Temperature","012003","Dew-point temperature",,"K","1","0","12","C","1","3","Operational"
564.00,"12","Temperature","012004","Air temperature at 2 m",,"K","1","0","12","C","1","3","Operational"
565.00,"12","Temperature","012005","Wet-bulb temperature at 2 m",,"K","1","0","12","C","1","3","Operational"
566.00,"12","Temperature","012006","Dew-point temperature at 2 m",,"K","1","0","12","C","1","3","Operational"
567.00,"12","Temperature","012007","Virtual temperature",,"K","1","0","12","C","1","3","Operational"
568.00,"12","Temperature","012011","Maximum temperature, at height and over period specified",,"K","1","0","12","C","1","3","Operational"
569.00,"12","Temperature","012012","Minimum temperature, at height and over period specified",,"K","1","0","12","C","1","3","Operational"
570.00,"12","Temperature","012013","Ground minimum temperature, past 12 hours",,"K","1","0","12","C","1","3","Operational"
571.00,"12","Temperature","012014","Maximum temperature at 2 m, past 12 hours",,"K","1","0","12","C","1","3","Operational"
572.00,"12","Temperature","012015","Minimum temperature at 2 m, past 12 hours",,"K","1","0","12","C","1","3","Operational"
573.00,"12","Temperature","012016","Maximum temperature at 2 m, past 24 hours",,"K","1","0","12","C","1","3","Operational"
574.00,"12","Temperature","012017","Minimum temperature at 2 m, past 24 hours",,"K","1","0","12","C","1","3","Operational"
575.00,"12","Temperature","012021","Maximum temperature at 2 m",,"K","2","0","16","C","2","4","Operational"
576.00,"12","Temperature","012022","Minimum temperature at 2 m",,"K","2","0","16","C","2","4","Operational"
577.00,"12","Temperature","012023","Temperature",,"C","0","-99","8","C","0","2","Operational"
578.00,"12","Temperature","012024","Dew-point temperature",,"C","0","-99","8","C","0","2","Operational"
579.00,"12","Temperature","012030","Soil temperature",,"K","1","0","12","C","1","3","Operational"
580.00,"12","Temperature","012049","Temperature change over specified period",,"K","0","-30","6","C","0","2","Operational"
581.00,"12","Temperature","012051","Standard deviation temperature",,"K","1","0","10","C","1","3","Operational"
582.00,"12","Temperature","012052","Highest daily mean temperature",,"K","1","0","12","C","1","3","Operational"
583.00,"12","Temperature","012053","Lowest daily mean temperature",,"K","1","0","12","C","1","3","Operational"
585.00,"12","Temperature","012061","Skin temperature",,"K","1","0","12","C","1","3","Operational"
586.00,"12","Temperature","012062","Equivalent black body temperature",,"K","1","0","12","C","1","3","Operational"
587.00,"12","Temperature","012063","Brightness temperature",,"K","1","0","12","C","1","3","Operational"
588.00,"12","Temperature","012064","Instrument temperature",,"K","1","0","12","K","1","4","Operational"
589.00,"12","Temperature","012065","Standard deviation brightness temperature",,"K","1","0","12","K","1","4","Operational"
590.00,"12","Temperature","012066","Antenna temperature",,"K","2","0","16","C","2","5","Operational"
591.00,"12","Temperature","012070","Warm load temperature",,"K","2","0","16","K","2","5","Operational"
592.00,"12","Temperature","012071","Coldest cluster temperature",,"K","1","0","12","K","1","4","Operational"
593.00,"12","Temperature","012072","Radiance",,"W m-2 sr-1","6","0","31","W m-2 sr-1","6","9","Operational"
594.00,"12","Temperature","012075","Spectral radiance",,"W m-3 sr-1","-3","0","16","W m-3 sr-1","-3","5","Operational"
595.00,"12","Temperature","012076","Radiance","(see Note 2)","W m-2 sr-1","3","0","16","W m-2 sr-1","3","5","Operational"
596.00,"12","Temperature","012080","Brightness temperature real part",,"K","2","-10000","16","K","2","5","Operational"
597.00,"12","Temperature","012081","Brightness temperature imaginary part",,"K","2","-10000","16","K","2","5","Operational"
598.00,"12","Temperature","012082","Pixel radiometric accuracy",,"K","2","0","12","K","2","4","Operational"
599.00,"12","Temperature","012101","Temperature/air temperature",,"K","2","0","16","C","2","4","Operational"
600.00,"12","Temperature","012102","Wet-bulb temperature",,"K","2","0","16","C","2","4","Operational"
601.00,"12","Temperature","012103","Dew-point temperature",,"K","2","0","16","C","2","4","Operational"
602.00,"12","Temperature","012104","Air temperature at 2 m",,"K","2","0","16","C","2","4","Operational"
603.00,"12","Temperature","012105","Web-bulb temperature at 2 m",,"K","2","0","16","C","2","4","Operational"
604.00,"12","Temperature","012106","Dew-point temperature at 2 m",,"K","2","0","16","C","2","4","Operational"
605.00,"12","Temperature","012107","Virtual temperature",,"K","2","0","16","C","2","4","Operational"
606.00,"12","Temperature","012111","Maximum temperature, at height and over period specified",,"K","2","0","16","C","2","4","Operational"
607.00,"12","Temperature","012112","Minimum temperature, at height and over period specified",,"K","2","0","16","C","2","4","Operational"
608.00,"12","Temperature","012113","Ground minimum temperature, past 12 hours",,"K","2","0","16","C","2","4","Operational"
609.00,"12","Temperature","012114","Maximum temperature at 2 m, past 12 hours",,"K","2","0","16","C","2","4","Operational"
610.00,"12","Temperature","012115","Minimum temperature at 2 m, past 12 hours",,"K","2","0","16","C","2","4","Operational"
611.00,"12","Temperature","012116","Maximum temperature at 2 m, past 24 hours",,"K","2","0","16","C","2","4","Operational"
612.00,"12","Temperature","012117","Minimum temperature at 2 m, past 24 hours",,"K","2","0","16","C","2","4","Operational"
613.00,"12","Temperature","012118","Maximum temperature at height specified, past 24 hours",,"K","2","0","16","C","2","4","Operational"
614.00,"12","Temperature","012119","Minimum temperature at height specified, past 24 hours",,"K","2","0","16","C","2","4","Operational"
615.00,"12","Temperature","012120","Ground temperature",,"K","2","0","16","C","2","4","Operational"
616.00,"12","Temperature","012121","Ground minimum temperature",,"K","2","0","16","C","2","4","Operational"
617.00,"12","Temperature","012122","Ground minimum temperature of the preceding night",,"K","2","0","16","C","2","4","Operational"
618.00,"12","Temperature","012130","Soil temperature",,"K","2","0","16","C","2","4","Operational"
619.00,"12","Temperature","012131","Snow temperature",,"K","2","0","16","C","2","4","Operational"
620.00,"12","Temperature","012132","Ice surface temperature",,"K","2","0","16","C","2","4","Operational"
621.00,"12","Temperature","012151","Standard deviation of daily mean temperature",,"K","2","0","12","C","2","4","Operational"
622.00,"12","Temperature","012152","Highest daily mean temperature",,"K","2","0","16","C","2","4","Operational"
623.00,"12","Temperature","012153","Lowest daily mean temperature",,"K","2","0","16","C","2","4","Operational"
624.00,"12","Temperature","012158","Noise-equivalent delta temperature while viewing cold target",,"K","2","0","12","C","2","4","Operational"
625.00,"12","Temperature","012159","Noise-equivalent delta temperature while viewing warm target",,"K","2","0","12","C","2","4","Operational"
626.00,"12","Temperature","012161","Skin temperature",,"K","2","0","16","C","2","4","Operational"
627.00,"12","Temperature","012162","Equivalent black body temperature",,"K","2","0","16","C","2","4","Operational"
628.00,"12","Temperature","012163","Brightness temperature",,"K","2","0","16","C","2","4","Operational"
629.00,"12","Temperature","012164","Instrument temperature",,"K","2","0","16","K","2","5","Operational"
630.00,"12","Temperature","012165","Direct sun brightness temperature",,"K","0","0","23","K","0","7","Operational"
631.00,"12","Temperature","012166","Snapshot accuracy",,"K","1","-4000","13","K","1","4","Operational"
632.00,"12","Temperature","012167","Radiometric accuracy (pure polarization)",,"K","1","0","9","K","1","3","Operational"
633.00,"12","Temperature","012168","Radiometric accuracy (cross polarization)",,"K","1","0","9","K","1","3","Operational"
634.00,"12","Temperature","012171","Coldest cluster temperature",,"K","2","0","16","K","2","5","Operational"
635.00,"12","Temperature","012180","Averaged 12 micron BT for all clear pixels at nadir",,"K","2","0","16","K","2","5","Operational"
636.00,"12","Temperature","012181","Averaged 11 micron BT for all clear pixels at nadir",,"K","2","0","16","K","2","5","Operational"
637.00,"12","Temperature","012182","Averaged 3.7 micron BT for all clear pixels at nadir",,"K","2","0","16","K","2","5","Operational"
638.00,"12","Temperature","012183","Averaged 12 micron BT for all clear pixels, forward view",,"K","2","0","16","K","2","5","Operational"
639.00,"12","Temperature","012184","Averaged 11 micron BT for all clear pixels, forward view",,"K","2","0","16","K","2","5","Operational"
640.00,"12","Temperature","012185","Averaged 3.7 micron BT for all clear pixels, forward view",,"K","2","0","16","K","2","5","Operational"
641.00,"12","Temperature","012186","Mean nadir sea-surface temperature",,"K","2","0","16","K","2","5","Operational"
642.00,"12","Temperature","012187","Mean dual view sea-surface temperature",,"K","2","0","16","K","2","5","Operational"
643.00,"12","Temperature","012188","Interpolated 23.8 GHz brightness T from MWR",,"K","2","0","16","K","2","5","Operational"
644.00,"12","Temperature","012189","Interpolated 36.5 GHz brightness T from MWR",,"K","2","0","16","K","2","5","Operational"
645.00,"13","Hydrographic and hydrological elements","013001","Specific humidity",,"kg/kg","5","0","14","kg/kg","5","5","Operational"
646.00,"13","Hydrographic and hydrological elements","013002","Mixing ratio",,"kg/kg","5","0","14","kg/kg","5","5","Operational"
647.00,"13","Hydrographic and hydrological elements","013003","Relative humidity",,"%","0","0","7","%","0","3","Operational"
648.00,"13","Hydrographic and hydrological elements","013004","Vapour pressure",,"Pa","-1","0","10","Pa","-1","4","Operational"
649.00,"13","Hydrographic and hydrological elements","013005","Vapour density",,"kg m-3","3","0","7","kg m-3","3","3","Operational"
650.00,"13","Hydrographic and hydrological elements","013006","Mixing heights",,"m","-1","-40","16","m","-1","5","Operational"
651.00,"13","Hydrographic and hydrological elements","013007","Minimum relative humidity",,"%","0","0","7","%","0","3","Operational"
652.00,"13","Hydrographic and hydrological elements","013008","Maximum relative humidity",,"%","0","0","7","%","0","3","Operational"
653.00,"13","Hydrographic and hydrological elements","013009","Relative humidity","(see Note 6)","%","1","-1000","12","%","1","4","Operational"
654.00,"13","Hydrographic and hydrological elements","013011","Total precipitation/total water equivalent",,"kg m-2","1","-1","14","kg m-2","1","5","Operational"
655.00,"13","Hydrographic and hydrological elements","013012","Depth of fresh snow",,"m","2","-2","12","m","2","4","Operational"
656.00,"13","Hydrographic and hydrological elements","013013","Total snow depth",,"m","2","-2","16","m","2","5","Operational"
657.00,"13","Hydrographic and hydrological elements","013014","Rainfall/water equivalent of snow (averaged rate)",,"kg m-2 s-1","4","0","12","kg m-2 s-1","4","4","Operational"
658.00,"13","Hydrographic and hydrological elements","013015","Snowfall (averaged rate)",,"m/s","7","0","12","m/s","7","4","Operational"
659.00,"13","Hydrographic and hydrological elements","013016","Precipitable water",,"kg m-2","0","0","7","kg m-2","0","3","Operational"
660.00,"13","Hydrographic and hydrological elements","013019","Total precipitation past 1 hour",,"kg m-2","1","-1","14","kg m-2","1","4","Operational"
661.00,"13","Hydrographic and hydrological elements","013020","Total precipitation past 3 hours",,"kg m-2","1","-1","14","kg m-2","1","5","Operational"
662.00,"13","Hydrographic and hydrological elements","013021","Total precipitation past 6 hours",,"kg m-2","1","-1","14","kg m-2","1","5","Operational"
663.00,"13","Hydrographic and hydrological elements","013022","Total precipitation past 12 hours",,"kg m-2","1","-1","14","kg m-2","1","5","Operational"
664.00,"13","Hydrographic and hydrological elements","013023","Total precipitation past 24 hours",,"kg m-2","1","-1","14","kg m-2","1","5","Operational"
665.00,"13","Hydrographic and hydrological elements","013031","Evapotranspiration",,"kg m-2","0","0","7","kg m-2","0","3","Operational"
666.00,"13","Hydrographic and hydrological elements","013032","Evaporation/evapotranspiration","(see Note 5)","kg m-2","1","0","8","kg m-2","1","3","Operational"
667.00,"13","Hydrographic and hydrological elements","013033","Evaporation/evapotranspiration",,"kg m-2","1","0","10","kg m-2","1","4","Operational"
668.00,"13","Hydrographic and hydrological elements","013038","Superadiabatic indicator",,"Code table","0","0","2","Code table","0","1","Operational"
669.00,"13","Hydrographic and hydrological elements","013039","Terrain type (ice/snow)",,"Code table","0","0","3","Code table","0","1","Operational"
670.00,"13","Hydrographic and hydrological elements","013040","Surface flag",,"Code table","0","0","4","Code table","0","2","Operational"
671.00,"13","Hydrographic and hydrological elements","013041","Pasquill-Gifford stability category",,"Code table","0","0","4","Code table","0","2","Operational"
672.00,"13","Hydrographic and hydrological elements","013042","Parcel lifted index (to 500 hPa)","(see Notes 3 and 4)","K","0","-20","6","K","0","2","Operational"
673.00,"13","Hydrographic and hydrological elements","013043","Best lifted index (to 500 hPa)","(see Notes 3 and 4)","K","0","-20","6","K","0","2","Operational"
674.00,"13","Hydrographic and hydrological elements","013044","K index",,"K","0","-30","8","K","0","3","Operational"
675.00,"13","Hydrographic and hydrological elements","013045","KO index",,"K","0","-30","8","K","0","3","Operational"
676.00,"13","Hydrographic and hydrological elements","013046","Maximum buoyancy",,"K","0","-30","8","K","0","3","Operational"
677.00,"13","Hydrographic and hydrological elements","013047","Modified Showalter stability index","(see Note 7)","K","0","-60","6","C","0","2","Operational"
678.00,"13","Hydrographic and hydrological elements","013048","Water fraction",,"%","1","0","10","%","1","4","Operational"
679.00,"13","Hydrographic and hydrological elements","013051","Frequency group, precipitation",,"Code table","0","0","4","Code table","0","2","Operational"
680.00,"13","Hydrographic and hydrological elements","013052","Highest daily amount of precipitation",,"kg m-2","1","-1","14","kg m-2","1","5","Operational"
681.00,"13","Hydrographic and hydrological elements","013055","Intensity of precipitation",,"kg m-2 s-1","4","0","8","mm/h","1","4","Operational"
682.00,"13","Hydrographic and hydrological elements","013056","Character and intensity of precipitation",,"Code table","0","0","4","Code table","0","2","Operational"
683.00,"13","Hydrographic and hydrological elements","013057","Time of beginning or end of precipitation",,"Code table","0","0","4","Code table","0","2","Operational"
684.00,"13","Hydrographic and hydrological elements","013058","Size of precipitating element",,"m","4","0","7","mm","1","3","Operational"
685.00,"13","Hydrographic and hydrological elements","013059","Number of flashes (thunderstorm)",,"Numeric","0","0","7","Numeric","0","3","Operational"
686.00,"13","Hydrographic and hydrological elements","013060","Total accumulated precipitation",,"kg m-2","1","-1","17","kg m-2","1","5","Operational"
687.00,"13","Hydrographic and hydrological elements","013071","Upstream water level",,"m","2","0","14","m","2","4","Operational"
688.00,"13","Hydrographic and hydrological elements","013072","Downstream water level",,"m","2","0","14","m","2","4","Operational"
689.00,"13","Hydrographic and hydrological elements","013073","Maximum water level",,"m","2","0","14","m","2","4","Operational"
690.00,"13","Hydrographic and hydrological elements","013074","Ground water level",,"m","2","0","18","m","2","6","Operational"
691.00,"13","Hydrographic and hydrological elements","013080","Water pH",,"pH unit","1","0","10","pH unit","1","3","Operational"
692.00,"13","Hydrographic and hydrological elements","013081","Water conductivity",,"S/m","3","0","14","S/m","3","4","Operational"
693.00,"13","Hydrographic and hydrological elements","013082","Water temperature",,"K","1","0","12","K","1","4","Operational"
694.00,"13","Hydrographic and hydrological elements","013083","Dissolved oxygen",,"kg m-3","6","0","15","kg m-3","6","5","Operational"
695.00,"13","Hydrographic and hydrological elements","013084","Turbidity",,"lm","0","0","14","lm","0","4","Operational"
696.00,"13","Hydrographic and hydrological elements","013085","Oxydation Reduction Potential (ORP)",,"V","3","0","14","V","3","4","Operational"
697.00,"13","Hydrographic and hydrological elements","013090","Radiometer water vapour content",,"kg m-2","1","0","10","kg m-2","1","4","Operational"
698.00,"13","Hydrographic and hydrological elements","013091","Radiometer liquid content",,"kg m-2","2","0","8","kg m-2","2","3","Operational"
699.00,"13","Hydrographic and hydrological elements","013093","Cloud optical thickness",,"Numeric","0","0","8","Numeric","0","3","Operational"
700.00,"13","Hydrographic and hydrological elements","013095","Total column water vapour",,"kg m-2","4","0","19","kg m-2","4","6","Operational"
701.00,"13","Hydrographic and hydrological elements","013096","MWR water vapour content",,"kg m-2","2","0","14","kg m-2","2","5","Operational"
702.00,"13","Hydrographic and hydrological elements","013097","MWR liquid water content",,"kg m-2","2","0","14","kg m-2","2","5","Operational"
703.00,"13","Hydrographic and hydrological elements","013098","Integrated water vapour density",,"kg m-2","8","0","30","kg m-2","8","10","Operational"
704.00,"13","Hydrographic and hydrological elements","013099","Log_10 of integrated cloud particle density",,"log(m-2)","1","0","7","log(m-2)","1","3","Operational"
705.00,"13","Hydrographic and hydrological elements","013100","Log_10 of integrated cloud particle area ",,"log(m2 m-2)","1","-70","7","log(m2 m-2)","1","2","Operational"
706.00,"13","Hydrographic and hydrological elements","013101","Log_10 of integrated cloud particle volume ",,"log(m3 m-2)","1","-140","7","log(m3 m-2)","1","3","Operational"
707.00,"13","Hydrographic and hydrological elements","013110","Mass mixing ratio",,"%","0","0","7","%","0","3","Operational"
708.00,"13","Hydrographic and hydrological elements","013111","Soil moisture",,"g/kg","0","0","10","g/kg","0","4","Operational"
709.00,"13","Hydrographic and hydrological elements","013112","Object wetness duration",,"s","0","0","17","s","0","5","Operational"
710.00,"13","Hydrographic and hydrological elements","013114","Rate of ice accretion",,"kg m-2 h-1","1","0","11","kg m-2 h-1","1","4","Operational"
711.00,"13","Hydrographic and hydrological elements","013115","Ice thickness",,"m","2","0","19","m","2","6","Operational"
712.00,"13","Hydrographic and hydrological elements","013117","Snow density (liquid water content)",,"kg m-3","0","0","10","kg m-3","0","3","Operational"
713.00,"13","Hydrographic and hydrological elements","013118","Depth of fresh snow (high accuracy)",,"m","3","-2","14","m","3","5","Operational"
714.00,"13","Hydrographic and hydrological elements","013155","Intensity of precipitation (high accuracy)","(see Note 8)","kg m-2 s-1","5","-1","16","mm/h","2","5","Operational"
715.00,"14","Radiation and radiance","014001","Long-wave radiation, integrated over 24 hours",,"J m-2","-3","-65536","17","J m-2","-3","5","Operational"
716.00,"14","Radiation and radiance","014002","Long-wave radiation, integrated over period specified",,"J m-2","-3","-65536","17","J m-2","-3","5","Operational"
717.00,"14","Radiation and radiance","014003","Short-wave radiation, integrated over 24 hours",,"J m-2","-3","-65536","17","J m-2","-3","5","Operational"
718.00,"14","Radiation and radiance","014004","Short-wave radiation, integrated over period specified",,"J m-2","-3","-65536","17","J m-2","-3","5","Operational"
719.00,"14","Radiation and radiance","014011","Net long-wave radiation, integrated over 24 hours",,"J m-2","-3","-65536","17","J m-2","-3","5","Operational"
720.00,"14","Radiation and radiance","014012","Net long-wave radiation, integrated over period specified",,"J m-2","-3","-65536","17","J m-2","-3","5","Operational"
721.00,"14","Radiation and radiance","014013","Net short-wave radiation, integrated over 24 hours",,"J m-2","-3","-65536","17","J m-2","-3","5","Operational"
722.00,"14","Radiation and radiance","014014","Net short-wave radiation, integrated over period specified",,"J m-2","-3","-65536","17","J m-2","-3","5","Operational"
723.00,"14","Radiation and radiance","014015","Net radiation, integrated over 24 hours",,"J m-2","-4","-16384","15","J m-2","-4","5","Operational"
724.00,"14","Radiation and radiance","014016","Net radiation, integrated over period specified",,"J m-2","-4","-16384","15","J m-2","-4","5","Operational"
725.00,"14","Radiation and radiance","014017","Instantaneous long-wave radiation",,"W m-2","0","-512","10","W m-2","0","4","Operational"
726.00,"14","Radiation and radiance","014018","Instantaneous short-wave radiation",,"W m-2","0","-2048","12","W m-2","0","4","Operational"
727.00,"14","Radiation and radiance","014019","Surface albedo",,"%","0","0","7","%","0","3","Operational"
728.00,"14","Radiation and radiance","014020","Global solar radiation, integrated over 24 hours",,"J m-2","-4","0","15","J m-2","-4","5","Operational"
729.00,"14","Radiation and radiance","014021","Global solar radiation, integrated over period specified",,"J m-2","-4","0","15","J m-2","-4","5","Operational"
730.00,"14","Radiation and radiance","014022","Diffuse solar radiation, integrated over 24 hours",,"J m-2","-4","0","15","J m-2","-4","5","Operational"
731.00,"14","Radiation and radiance","014023","Diffuse solar radiation, integrated over period specified",,"J m-2","-4","0","15","J m-2","-4","5","Operational"
732.00,"14","Radiation and radiance","014024","Direct solar radiation, integrated over 24 hours",,"J m-2","-4","0","15","J m-2","-4","5","Operational"
733.00,"14","Radiation and radiance","014025","Direct solar radiation, integrated over period specified",,"J m-2","-4","0","15","J m-2","-4","5","Operational"
734.00,"14","Radiation and radiance","014026","Albedo at the top of clouds",,"%","0","0","7","%","0","3","Operational"
735.00,"14","Radiation and radiance","014027","Albedo",,"%","0","0","7","%","0","3","Operational"
736.00,"14","Radiation and radiance","014028","Global solar radiation (high accuracy), integrated over period specified",,"J m-2","-2","0","20","J m-2","-2","6","Operational"
737.00,"14","Radiation and radiance","014029","Diffuse solar radiation (high accuracy), integrated over period specified",,"J m-2","-2","0","20","J m-2","-2","6","Operational"
738.00,"14","Radiation and radiance","014030","Direct solar radiation (high accuracy), integrated over period specified",,"J m-2","-2","0","20","J m-2","-2","6","Operational"
739.00,"14","Radiation and radiance","014031","Total sunshine",,"min","0","0","11","min","0","4","Operational"
740.00,"14","Radiation and radiance","014032","Total sunshine",,"h","0","0","10","h","0","4","Operational"
741.00,"14","Radiation and radiance","014033","Total sunshine",,"%","0","0","9","%","0","3","Operational"
742.00,"14","Radiation and radiance","014034","Sunshine over period specified",,"min","0","0","11","min","0","4","Operational"
743.00,"14","Radiation and radiance","014035","Solar Radiation Flux",,"W m-2","1","0","14","W m-2","1","5","Operational"
744.00,"14","Radiation and radiance","014042","Bidirectional reflectance",,"%","0","0","7","%","0","3","Operational"
745.00,"14","Radiation and radiance","014043","Channel radiance",,"W m-2 sr-1 um-1","4","0","23","W m-2 sr-1 um-1","4","7","Operational"
746.00,"14","Radiation and radiance","014044","Channel radiance",,"W m-2 sr-1 cm","7","-100000","22","W m-2 sr-1 cm","7","7","Operational"
747.00,"14","Radiation and radiance","014045","Channel radiance","(see Note 4)","W m-2 sr-1 cm","0","0","11","W m-2 sr-1 cm","0","4","Operational"
748.00,"14","Radiation and radiance","014046","Scaled IASI radiance","(see Note 6)","W m-2 sr-1 m","0","-5000","16","W m-2 sr-1 m","0","5","Operational"
749.00,"14","Radiation and radiance","014047","Scaled mean AVHRR radiance",,"W m-2 sr-1 m","0","0","31","W m-2 sr-1 m","0","10","Operational"
750.00,"14","Radiation and radiance","014048","Scaled standard deviation AVHRR radiance",,"W m-2 sr-1 m","0","0","31","W m-2 sr-1 m","0","10","Operational"
751.00,"14","Radiation and radiance","014050","Emissivity","(see Note 5)","%","1","0","10","%","1","4","Operational"
752.00,"14","Radiation and radiance","014051","Direct solar radiation integrated over last hour",,"J m-2","-3","0","14","J m-2","-3","4","Operational"
753.00,"14","Radiation and radiance","014052","Global upward solar radiation, integrated over period specified",,"J m-2","-2","-1048574","20","J m-2","-2","7","Operational"
754.00,"14","Radiation and radiance","014053","Net radiation (high accuracy), integrated over period specified",,"J m-2","-2","-1048574","21","J m-2","-2","7","Operational"
755.00,"14","Radiation and radiance","014054","Photosynthetically active radiation, integrated over period specified",,"J m-2","-3","0","16","J m-2","-3","5","Operational"
756.00,"14","Radiation and radiance","014055","Solar activity index",,"Numeric","0","-32768","16","Numeric","0","5","Operational"
757.00,"14","Radiation and radiance","014056","Background luminance",,"Cd m-2","0","0","18","Cd m-2","0","6","Operational"
758.00,"14","Radiation and radiance","014057","Soil heat flux",,"J m-2","-2","-1048574","21","J m-2","-2","7","Operational"
760.00,"14","Radiation and radiance","014072","Global UV irradiation","(see Note 8)","J m-2","0","-4000000","23","J m-2","0","7","Operational"
762.00,"15","Physical/chemical constituents","015001","Total ozone",,"DU","0","0","10","DU","0","4","Operational"
763.00,"15","Physical/chemical constituents","015002","Air mass (slant path at 22 km)",,"Numeric","2","0","10","Numeric","2","3","Operational"
764.00,"15","Physical/chemical constituents","015003","Measured ozone partial pressure (sounding)","(see Note 1)","Pa","4","0","9","nbar","0","3","Operational"
765.00,"15","Physical/chemical constituents","015004","Ozone sounding correction factor (CF)","(see Note 2)","Numeric","3","0","11","Numeric","3","4","Operational"
766.00,"15","Physical/chemical constituents","015005","Ozone p","(see Note 3)","DU","0","0","10","DU","0","3","Operational"
768.00,"15","Physical/chemical constituents","015008","Significand of volumetric mixing ratio",,"Numeric","0","0","10","Numeric","0","4","Operational"
771.00,"15","Physical/chemical constituents","015011","Log 10 of integrated electron density",,"log (m-2)","3","14000","13","log (m-2)","3","4","Operational"
772.00,"15","Physical/chemical constituents","015012","Total electron count per square metre",,"m-2","-16","0","6","m-2","-16","2","Operational"
773.00,"15","Physical/chemical constituents","015015","Maximum image spectral component before normalization",,"Numeric","0","0","31","Numeric","0","10","Operational"
774.00,"15","Physical/chemical constituents","015020","Integrated ozone density",,"kg m-2","8","0","21","kg m-2","8","7","Operational"
775.00,"15","Physical/chemical constituents","015021","Integrated mass density",,"kg m-2","11","0","31","kg m-2","11","10","Operational"
778.00,"15","Physical/chemical constituents","015024","Optical depth",,"Numeric","4","0","24","Numeric","4","8","Operational"
779.00,"15","Physical/chemical constituents","015025","Type of pollutant",,"Code table","0","0","4","Code table","0","2","Operational"
780.00,"15","Physical/chemical constituents","015026","Concentration of pollutant (mol mol-1)",,"mol/mol","9","0","9","mol/mol","9","3","Operational"
781.00,"15","Physical/chemical constituents","015027","Concentration of pollutant (kg m-3)",,"kg m-3","9","0","10","kg m-3","9","4","Operational"
783.00,"15","Physical/chemical constituents","015029","Extinction coefficient",,"m-1","9","0","30","m-1","9","10","Operational"
784.00,"15","Physical/chemical constituents","015030","Aerosol contamination index","(see Note 6)","Numeric","2","-1000","12","Numeric","2","4","Operational"
785.00,"15","Physical/chemical constituents","015031","Atmospheric path delay in satellite signal",,"m","4","10000","15","m","4","5","Operational"
786.00,"15","Physical/chemical constituents","015032","Estimated error in atmospheric path delay",,"m","4","0","10","m","4","4","Operational"
787.00,"15","Physical/chemical constituents","015033","Difference in path delays for limb views at extremes of scan",,"m","5","-10000","15","m","5","5","Operational"
788.00,"15","Physical/chemical constituents","015034","Estimated error in path delay difference",,"m","5","0","14","m","5","5","Operational"
789.00,"15","Physical/chemical constituents","015035","Component of zenith path delay due to water vapour",,"m","4","0","14","m","4","5","Operational"
790.00,"15","Physical/chemical constituents","015036","Atmospheric refractivity","(see Note 5)","N units","3","0","19","N units","3","6","Operational"
791.00,"15","Physical/chemical constituents","015037","Bending angle",,"rad","8","-100000","23","rad","8","7","Operational"
793.00,"15","Physical/chemical constituents","015042","Reflectance",,"%","2","0","14","%","2","5","Operational"
799.00,"15","Physical/chemical constituents","015051","Meteorological optical range",,"m","0","0","18","m","0","6","Operational"
800.00,"15","Physical/chemical constituents","015052","Log_10 of number density of aerosol particles with diameter greater than 5 nm",,"log(m-3)","1","60","6","log(m-3)","1","3","Operational"
801.00,"15","Physical/chemical constituents","015053","Log_10 of number density of aerosol particles with diameter greater than 14 nm",,"log(m-3)","2","600","9","log(m-3)","2","4","Operational"
802.00,"15","Physical/chemical constituents","015054","Log_10 of number density of aerosol particles with diameter between 0.25 and 2.5 μm",,"log(m-3)","2","550","9","log(m-3)","2","4","Operational"
803.00,"15","Physical/chemical constituents","015055","Non volatile aerosol ratio",,"Numeric","2","0","7","Numeric","2","3","Operational"
804.00,"19","Synoptic features","019001","Type of synoptic feature",,"Code table","0","0","6","Code table","0","2","Operational"
805.00,"19","Synoptic features","019002","Effective radius of feature","(see Note 1)","m","-2","0","12","m","-2","4","Operational"
806.00,"19","Synoptic features","019003","Wind speed threshold","(see Note 2)","m/s","0","0","8","m/s","0","3","Operational"
807.00,"19","Synoptic features","019004","Effective radius with respect to wind speeds above threshold","(see Note 2)","m","-2","0","12","m","-2","4","Operational"
808.00,"19","Synoptic features","019005","Direction of motion of feature","(see Note 3)","degree true","0","0","9","degree true","0","3","Operational"
809.00,"19","Synoptic features","019006","Speed of motion of feature","(see Note 3)","m/s","2","0","14","m/s","2","5","Operational"
810.00,"19","Synoptic features","019007","Effective radius of feature",,"m","-3","0","12","m","-3","4","Operational"
811.00,"19","Synoptic features","019008","Vertical extent of circulation",,"Code table","0","0","3","Code table","0","1","Operational"
812.00,"19","Synoptic features","019009","Effective radius with respect to wind speeds above threshold (large storms)",,"m","-3","0","12","m","-3","4","Operational"
813.00,"19","Synoptic features","019010","Method for tracking the centre of synoptic feature",,"Code table","0","0","4","Code table","0","2","Operational"
814.00,"19","Synoptic features","019100","Time interval to calculate the movement of the tropical cyclone",,"Code table","0","0","4","Code table","0","2","Operational"
815.00,"19","Synoptic features","019101","Accuracy of the position of the centre of the tropical cyclone",,"Code table","0","0","4","Code table","0","2","Operational"
816.00,"19","Synoptic features","019102","Shape and definition of the eye of the tropical cyclone",,"Code table","0","0","3","Code table","0","1","Operational"
817.00,"19","Synoptic features","019103","Diameter of major axis of the eye of the tropical cyclone",,"Code table","0","0","4","Code table","0","2","Operational"
818.00,"19","Synoptic features","019104","Change in character of the eye during the 30 minutes",,"Code table","0","0","4","Code table","0","2","Operational"
819.00,"19","Synoptic features","019105","Distance between the end of spiral band and the centre",,"Code table","0","0","4","Code table","0","2","Operational"
820.00,"19","Synoptic features","019106","Identification number of tropical cyclone",,"Numeric","0","0","7","Numeric","0","3","Operational"
821.00,"19","Synoptic features","019107","Time interval over which the movement of the tropical cyclone has been calculated",,"Code table","0","0","4","Code table","0","2","Operational"
822.00,"19","Synoptic features","019108","Accuracy of geographical position of the tropical cyclone",,"Code table","0","0","3","Code table","0","1","Operational"
823.00,"19","Synoptic features","019109","Mean diameter of the overcast cloud of the tropical cyclone",,"Code table","0","0","4","Code table","0","2","Operational"
824.00,"19","Synoptic features","019110","Apparent 24-hour change in intensity of the tropical cyclone",,"Code table","0","0","4","Code table","0","2","Operational"
825.00,"19","Synoptic features","019111","Current Intensity (CI) number of the tropical cyclone",,"Numeric","1","0","7","Numeric","1","3","Operational"
826.00,"19","Synoptic features","019112","Data Tropical (DT) number of the tropical cyclone",,"Numeric","1","0","7","Numeric","1","3","Operational"
827.00,"19","Synoptic features","019113","Cloud pattern type of the DT-number",,"Code table","0","0","4","Code table","0","2","Operational"
828.00,"19","Synoptic features","019114","Model Expected Tropical (MET) number of the tropical cyclone",,"Numeric","1","0","7","Numeric","1","3","Operational"
829.00,"19","Synoptic features","019115","Trend of the past 24-hour change (+: Developed, -: Weakened)",,"Numeric","1","-30","6","Numeric","1","2","Operational"
830.00,"19","Synoptic features","019116","Pattern Tropical (PT) number of the tropical cyclone",,"Numeric","1","0","7","Numeric","1","3","Operational"
831.00,"19","Synoptic features","019117","Cloud picture type of the PT-number",,"Code table","0","0","3","Code table","0","1","Operational"
832.00,"19","Synoptic features","019118","Final Tropical (T) number of the tropical cyclone",,"Numeric","1","0","7","Numeric","1","3","Operational"
833.00,"19","Synoptic features","019119","Type of the final T-number",,"Code table","0","0","3","Code table","0","1","Operational"
834.00,"19","Synoptic features","019150","Typhoon International Common Number (Typhoon Committee)",,"CCITT IA5","0","0","32","Character","0","4","Operational"
835.00,"20","Observed phenomena","020001","Horizontal visibility",,"m","-1","0","13","m","-1","4","Operational"
836.00,"20","Observed phenomena","020002","Vertical visibility",,"m","-1","0","7","m","-1","3","Operational"
837.00,"20","Observed phenomena","020003","Present weather","(see Note 1)","Code table","0","0","9","Code table","0","3","Operational"
838.00,"20","Observed phenomena","020004","Past weather (1)","(see Note 2)","Code table","0","0","5","Code table","0","2","Operational"
839.00,"20","Observed phenomena","020005","Past weather (2)","(see Note 2)","Code table","0","0","5","Code table","0","2","Operational"
840.00,"20","Observed phenomena","020006","Flight rules",,"Code table","0","0","3","Code table","0","1","Operational"
841.00,"20","Observed phenomena","020008","Cloud distribution for aviation",,"Code table","0","0","5","Code table","0","2","Operational"
842.00,"20","Observed phenomena","020009","General weather indicator (TAF/METAR)",,"Code table","0","0","4","Code table","0","2","Operational"
843.00,"20","Observed phenomena","020010","Cloud cover (total)","(see Note 5)","%","0","0","7","%","0","3","Operational"
844.00,"20","Observed phenomena","020011","Cloud amount",,"Code table","0","0","4","Code table","0","2","Operational"
845.00,"20","Observed phenomena","020012","Cloud type",,"Code table","0","0","6","Code table","0","2","Operational"
846.00,"20","Observed phenomena","020013","Height of base of cloud",,"m","-1","-40","11","m","-1","4","Operational"
847.00,"20","Observed phenomena","020014","Height of top of cloud",,"m","-1","-40","11","m","-1","4","Operational"
848.00,"20","Observed phenomena","020015","Pressure at base of cloud",,"Pa","-1","0","14","Pa","-1","5","Operational"
849.00,"20","Observed phenomena","020016","Pressure at top of cloud",,"Pa","-1","0","14","Pa","-1","5","Operational"
850.00,"20","Observed phenomena","020017","Cloud top description",,"Code table","0","0","4","Code table","0","2","Operational"
851.00,"20","Observed phenomena","020018","Tendency of runway visual range",,"Code table","0","0","2","Code table","0","1","Operational"
852.00,"20","Observed phenomena","020019","Significant present or forecast weather","(see Note 15)","CCITT IA5","0","0","72","Character","0","9","Operational"
853.00,"20","Observed phenomena","020020","Significant recent weather phenomena","(see Note 15)","CCITT IA5","0","0","32","Character","0","4","Operational"
854.00,"20","Observed phenomena","020021","Type of precipitation",,"Flag table","0","0","30","Flag table","0","10","Operational"
855.00,"20","Observed phenomena","020022","Character of precipitation",,"Code table","0","0","4","Code table","0","2","Operational"
856.00,"20","Observed phenomena","020023","Other weather phenomena",,"Flag table","0","0","18","Flag table","0","6","Operational"
857.00,"20","Observed phenomena","020024","Intensity of phenomena",,"Code table","0","0","3","Code table","0","1","Operational"
858.00,"20","Observed phenomena","020025","Obscuration",,"Flag table","0","0","21","Flag table","0","7","Operational"
859.00,"20","Observed phenomena","020026","Character of obscuration",,"Code table","0","0","4","Code table","0","2","Operational"
860.00,"20","Observed phenomena","020027","Phenomena occurrence",,"Flag table","0","0","9","Flag table","0","3","Operational"
861.00,"20","Observed phenomena","020028","Expected change in intensity",,"Code table","0","0","3","Code table","0","1","Operational"
862.00,"20","Observed phenomena","020029","Rain flag",,"Code table","0","0","2","Code table","0","1","Operational"
863.00,"20","Observed phenomena","020031","Ice deposit (thickness)",,"m","2","0","7","m","2","3","Operational"
864.00,"20","Observed phenomena","020032","Rate of ice accretion (estimated)",,"Code table","0","0","3","Code table","0","1","Operational"
865.00,"20","Observed phenomena","020033","Cause of ice accretion",,"Flag table","0","0","4","Flag table","0","2","Operational"
866.00,"20","Observed phenomena","020034","Sea ice concentration",,"Code table","0","0","5","Code table","0","2","Operational"
867.00,"20","Observed phenomena","020035","Amount and type of ice",,"Code table","0","0","4","Code table","0","2","Operational"
868.00,"20","Observed phenomena","020036","Ice situation",,"Code table","0","0","5","Code table","0","2","Operational"
869.00,"20","Observed phenomena","020037","Ice development",,"Code table","0","0","5","Code table","0","2","Operational"
870.00,"20","Observed phenomena","020038","Bearing of ice edge","(see Note 3)","degree true","0","0","12","degree true","0","3","Operational"
871.00,"20","Observed phenomena","020039","Ice distance",,"m","-1","0","13","m","-1","4","Operational"
872.00,"20","Observed phenomena","020040","Evolution of drift snow",,"Code table","0","0","4","Code table","0","2","Operational"
873.00,"20","Observed phenomena","020041","Airframe icing",,"Code table","0","0","4","Code table","0","2","Operational"
874.00,"20","Observed phenomena","020042","Airframe icing present",,"Code table","0","0","2","Code table","0","1","Operational"
875.00,"20","Observed phenomena","020043","Peak liquid water content",,"kg m-3","4","0","7","kg m-3","4","2","Operational"
876.00,"20","Observed phenomena","020044","Average liquid water content",,"kg m-3","4","0","7","kg m-3","4","2","Operational"
877.00,"20","Observed phenomena","020045","Supercooled large droplet (SLD) conditions",,"Code table","0","0","2","Code table","0","1","Operational"
878.00,"20","Observed phenomena","020048","Evolution of feature",,"Code table","0","0","4","Code table","0","2","Operational"
879.00,"20","Observed phenomena","020050","Cloud index",,"Code table","0","0","8","Code table","0","3","Operational"
880.00,"20","Observed phenomena","020051","Amount of low clouds",,"%","0","0","7","%","0","3","Operational"
881.00,"20","Observed phenomena","020052","Amount of middle clouds",,"%","0","0","7","%","0","3","Operational"
882.00,"20","Observed phenomena","020053","Amount of high clouds",,"%","0","0","7","%","0","3","Operational"
883.00,"20","Observed phenomena","020054","True direction from which a phenomenon or clouds are moving",,"degree true","0","0","9","degree true","0","3","Operational"
884.00,"20","Observed phenomena","020055","State of sky in the tropics",,"Code table","0","0","4","Code table","0","2","Operational"
885.00,"20","Observed phenomena","020056","Cloud phase",,"Code table","0","0","3","Code table","0","1","Operational"
886.00,"20","Observed phenomena","020058","Visibility seawards from a coastal station",,"m","-1","0","13","m","-1","4","Operational"
887.00,"20","Observed phenomena","020059","Minimum horizontal visibility",,"m","-1","0","9","m","-1","3","Operational"
888.00,"20","Observed phenomena","020060","Prevailing horizontal visibility","(see Note 7)","m","-1","0","10","m","-1","4","Operational"
889.00,"20","Observed phenomena","020061","Runway visual range (RVR)",,"m","0","0","12","m","0","4","Operational"
890.00,"20","Observed phenomena","020062","State of the ground (with or without snow)",,"Code table","0","0","5","Code table","0","2","Operational"
891.00,"20","Observed phenomena","020063","Special phenomena",,"Code table","0","0","10","Code table","0","4","Operational"
892.00,"20","Observed phenomena","020065","Snow cover","(see Note 4)","%","0","0","7","%","0","3","Operational"
893.00,"20","Observed phenomena","020066","Maximum diameter of hailstones",,"m","3","0","8","m","3","3","Operational"
894.00,"20","Observed phenomena","020067","Diameter of deposit",,"m","3","0","9","m","3","3","Operational"
895.00,"20","Observed phenomena","020070","Minimum number of atmospherics",,"Numeric","0","0","7","Numeric","0","3","Operational"
896.00,"20","Observed phenomena","020071","Accuracy of fix and rate of atmospherics",,"Code table","0","0","4","Code table","0","2","Operational"
899.00,"20","Observed phenomena","020081","Cloud amount in segment",,"%","0","0","7","%","0","3","Operational"
900.00,"20","Observed phenomena","020082","Amount segment cloud free",,"%","0","0","7","%","0","3","Operational"
901.00,"20","Observed phenomena","020083","Amount of segment covered by scene",,"%","0","0","7","%","0","3","Operational"
902.00,"20","Observed phenomena","020085","General condition of runway",,"Code table","0","0","4","Code table","0","1","Operational"
903.00,"20","Observed phenomena","020086","Runway deposits",,"Code table","0","0","4","Code table","0","1","Operational"
904.00,"20","Observed phenomena","020087","Runway contamination",,"Code table","0","0","4","Code table","0","1","Operational"
905.00,"20","Observed phenomena","020088","Depth of runway deposits",,"m","3","0","12","m","0","4","Operational"
906.00,"20","Observed phenomena","020089","Runway friction coefficient",,"Code table","0","0","7","Code table","0","2","Operational"
907.00,"20","Observed phenomena","020090","Special clouds",,"Code table","0","0","4","Code table","0","2","Operational"
908.00,"20","Observed phenomena","020091","Vertical visibility",,"ft","-2","0","10","ft","-2","3","Operational"
909.00,"20","Observed phenomena","020092","Height of base of cloud",,"ft","-2","0","10","ft","-2","3","Operational"
910.00,"20","Observed phenomena","020093","Height of inversion",,"m","-1","0","8","m","-1","3","Operational"
911.00,"20","Observed phenomena","020095","Ice probability",,"Numeric","3","0","10","Numeric","3","4","Operational"
912.00,"20","Observed phenomena","020096","Ice age (""A"" parameter)",,"dB","2","-4096","13","dB","2","4","Operational"
913.00,"20","Observed phenomena","020101","Locust (acridian) name",,"Code table","0","0","4","Code table","0","2","Operational"
914.00,"20","Observed phenomena","020102","Locust (maturity) colour",,"Code table","0","0","4","Code table","0","2","Operational"
915.00,"20","Observed phenomena","020103","Stage of development of locusts",,"Code table","0","0","4","Code table","0","2","Operational"
916.00,"20","Observed phenomena","020104","Organization state of swarm or band of locusts",,"Code table","0","0","4","Code table","0","2","Operational"
917.00,"20","Observed phenomena","020105","Size of swarm or band of locusts and duration of passage of swarm",,"Code table","0","0","4","Code table","0","2","Operational"
918.00,"20","Observed phenomena","020106","Locust population density",,"Code table","0","0","4","Code table","0","2","Operational"
919.00,"20","Observed phenomena","020107","Direction of movements of locust swarm",,"Code table","0","0","4","Code table","0","2","Operational"
920.00,"20","Observed phenomena","020108","Extent of vegetation",,"Code table","0","0","4","Code table","0","2","Operational"
921.00,"20","Observed phenomena","020111","x-axis error ellipse major component","(see Notes 8 and 9)","m","-1","0","17","m","-1","6","Operational"
922.00,"20","Observed phenomena","020112","y-axis error ellipse minor component","(see Notes 8 and 9)","m","-1","0","17","m","-1","6","Operational"
923.00,"20","Observed phenomena","020113","z-axis error ellipse component","(see Note 9)","m","-1","0","17","m","-1","6","Operational"
924.00,"20","Observed phenomena","020114","Angle of x-axis in error ellipse","(see Note 10)","deg","2","-18000","16","deg","2","5","Operational"
925.00,"20","Observed phenomena","020115","Angle of z-axis in error ellipse","(see Note 11)","deg","2","-18000","16","deg","2","5","Operational"
926.00,"20","Observed phenomena","020116","Emission height of cloud stroke",,"m","0","0","16","m","0","5","Operational"
927.00,"20","Observed phenomena","020117","Amplitude of lightning strike",,"A","-1","-32000","16","A","-1","5","Operational"
928.00,"20","Observed phenomena","020118","Lightning detection error",,"m","0","0","19","m","0","6","Operational"
929.00,"20","Observed phenomena","020119","Lightning discharge polarity",,"Code table","0","0","2","Code table","0","1","Operational"
930.00,"20","Observed phenomena","020121","Threshold value for polarity decision","(see Note 12)","V","3","0","16","V","3","5","Operational"
931.00,"20","Observed phenomena","020122","Threshold value for polarity decision","(see Note 13)","A","0","0","16","A","0","5","Operational"
932.00,"20","Observed phenomena","020123","Minimum threshold for detection","(see Note 14)","V/m","3","0","16","V/m","3","5","Operational"
933.00,"20","Observed phenomena","020124","Lightning stroke or flash",,"Code table","0","0","2","Code table","0","1","Operational"
934.00,"20","Observed phenomena","020126","Lightning rate of discharge",,"h-1","0","0","23","h-1","0","7","Operational"
935.00,"20","Observed phenomena","020127","Lightning - distance from station",,"m","-3","0","8","m","-3","3","Operational"
936.00,"20","Observed phenomena","020128","Lightning - direction from station",,"degree true","1","0","12","degree true","1","4","Operational"
937.00,"20","Observed phenomena","020130","Cloud hydrometeor concentration",,"Numeric","0","0","10","Numeric","0","3","Operational"
938.00,"20","Observed phenomena","020131","Effective radius of cloud hydrometeors",,"m","5","0","6","m","5","2","Operational"
939.00,"20","Observed phenomena","020132","Cloud liquid water content",,"kg m-3","5","0","11","kg m-3","5","4","Operational"
940.00,"20","Observed phenomena","020133","Hydrometeor radius",,"m","5","0","6","m","5","2","Operational"
941.00,"20","Observed phenomena","020135","Ice mass (on a rod)",,"kg/m","1","0","10","kg/m","1","3","Operational"
942.00,"20","Observed phenomena","020136","Supplementary cloud type",,"Code table","0","0","9","Code table","0","3","Operational"
944.00,"21","Radar data","021001","Horizontal reflectivity",,"dB","0","-64","7","dB","0","3","Operational"
945.00,"21","Radar data","021002","Vertical reflectivity",,"dB","0","-64","7","dB","0","3","Operational"
946.00,"21","Radar data","021003","Differential reflectivity",,"dB","1","-5","7","dB","1","3","Operational"
947.00,"21","Radar data","021005","Linear depolarization ratio",,"dB","0","-65","6","dB","0","2","Operational"
948.00,"21","Radar data","021006","Circular depolarization ratio",,"dB","0","-65","6","dB","0","2","Operational"
949.00,"21","Radar data","021011","Doppler mean velocity in x-direction",,"m/s","0","-128","8","m/s","0","3","Operational"
950.00,"21","Radar data","021012","Doppler mean velocity in y-direction",,"m/s","0","-128","8","m/s","0","3","Operational"
951.00,"21","Radar data","021013","Doppler mean velocity in z-direction",,"m/s","0","-128","8","m/s","0","3","Operational"
952.00,"21","Radar data","021014","Doppler mean velocity (radial)",,"m/s","1","-4096","13","m/s","1","4","Operational"
953.00,"21","Radar data","021017","Doppler velocity spectral width",,"m/s","1","0","8","m/s","1","3","Operational"
954.00,"21","Radar data","021018","Extended NYQUIST velocity",,"m/s","1","0","10","m/s","1","4","Operational"
955.00,"21","Radar data","021019","High NYQUIST velocity",,"m/s","1","0","10","m/s","1","3","Operational"
956.00,"21","Radar data","021021","Echo tops",,"m","-3","0","4","m","-3","2","Operational"
957.00,"21","Radar data","021022","Range bin offset",,"m","1","0","14","m","1","5","Operational"
958.00,"21","Radar data","021023","Range bin size",,"m","0","0","14","m","0","5","Operational"
959.00,"21","Radar data","021024","Azimuth offset",,"deg","1","0","12","deg","1","4","Operational"
960.00,"21","Radar data","021025","Azimuthal resolution",,"deg","1","0","8","deg","1","3","Operational"
961.00,"21","Radar data","021030","Signal to noise ratio",,"dB","0","-32","8","dB","0","3","Operational"
962.00,"21","Radar data","021031","Vertically integrated liquid-water content",,"kg m-2","0","0","7","kg m-2","0","3","Operational"
963.00,"21","Radar data","021036","Radar rainfall intensity",,"m/s","7","0","12","m/s","7","4","Operational"
964.00,"21","Radar data","021041","Bright-band height",,"m","-2","0","8","m","-2","3","Operational"
965.00,"21","Radar data","021051","Signal power above 1 mW",,"dB","0","-256","8","dB","0","3","Operational"
966.00,"21","Radar data","021062","Backscatter",,"dB","2","-5000","13","dB","2","4","Operational"
967.00,"21","Radar data","021063","Radiometric resolution (noise value)",,"%","1","0","10","%","1","4","Operational"
968.00,"21","Radar data","021064","Clutter noise estimate",,"Numeric","0","0","8","Numeric","0","3","Operational"
969.00,"21","Radar data","021065","Missing packet counter",,"Numeric","0","-127","8","Numeric","0","3","Operational"
970.00,"21","Radar data","021066","Wave scatterometer product confidence data",,"Flag table","0","0","12","Flag table","0","4","Operational"
971.00,"21","Radar data","021067","Wind product confidence data",,"Flag table","0","0","13","Flag table","0","5","Operational"
972.00,"21","Radar data","021068","Radar altimeter product confidence data",,"Flag table","0","0","8","Flag table","0","3","Operational"
973.00,"21","Radar data","021069","SST product confidence data",,"Flag table","0","0","10","Flag table","0","4","Operational"
974.00,"21","Radar data","021070","SST product confidence data (SADIST-2)",,"Flag table","0","0","23","Flag table","0","6","Operational"
975.00,"21","Radar data","021071","Peakiness",,"Numeric","0","0","16","Numeric","0","5","Operational"
976.00,"21","Radar data","021072","Satellite altimeter calibration status",,"Flag table","0","0","4","Flag table","0","2","Operational"
977.00,"21","Radar data","021073","Satellite altimeter instrument mode",,"Flag table","0","0","9","Flag table","0","3","Operational"
978.00,"21","Radar data","021075","Image spectrum intensity",,"Numeric","0","0","8","Numeric","0","3","Operational"
979.00,"21","Radar data","021076","Representation of intensities",,"Code table","0","0","3","Code table","0","1","Operational"
980.00,"21","Radar data","021077","Altitude correction (ionosphere)",,"m","3","0","14","m","3","5","Operational"
981.00,"21","Radar data","021078","Altitude correction (dry troposphere)",,"m","3","0","9","m","3","3","Operational"
982.00,"21","Radar data","021079","Altitude correction (wet troposphere)",,"m","3","2000","10","m","3","4","Operational"
983.00,"21","Radar data","021080","Altitude correction (calibration constant)",,"m","3","0","11","m","3","4","Operational"
984.00,"21","Radar data","021081","Open loop correction (height-time loop)",,"m","3","0","10","m","3","4","Operational"
985.00,"21","Radar data","021082","Open loop correction (auto gain control)",,"dB","3","-3000","14","dB","3","5","Operational"
986.00,"21","Radar data","021083","Warm target calibration",,"Numeric","0","0","16","Numeric","0","5","Operational"
987.00,"21","Radar data","021084","Cold target calibration",,"Numeric","0","0","16","Numeric","0","5","Operational"
988.00,"21","Radar data","021085","ATSR sea surface temperature across-track band number",,"Numeric","0","0","4","Numeric","0","2","Operational"
989.00,"21","Radar data","021086","Number of pixels in nadir only, average",,"Numeric","0","0","9","Numeric","0","3","Operational"
990.00,"21","Radar data","021087","Number of pixels in dual view, average",,"Numeric","0","0","9","Numeric","0","3","Operational"
991.00,"21","Radar data","021088","Wet backscatter",,"dB","2","-5000","13","dB","2","4","Operational"
992.00,"21","Radar data","021091","Radar signal Doppler spectrum 0th moment",,"dB","0","-100","8","dB","0","3","Operational"
993.00,"21","Radar data","021092","RASS signal Doppler spectrum 0th moment, referring to RASS signal",,"dB","0","-100","8","dB","0","3","Operational"
994.00,"21","Radar data","021093","Ku band peakiness",,"Numeric","3","0","16","Numeric","3","5","Operational"
995.00,"21","Radar data","021094","S band peakiness",,"Numeric","3","0","16","Numeric","3","5","Operational"
996.00,"21","Radar data","021101","Number of vector ambiguities",,"Numeric","0","0","3","Numeric","0","1","Operational"
997.00,"21","Radar data","021102","Index of selected wind vector",,"Numeric","0","0","3","Numeric","0","1","Operational"
998.00,"21","Radar data","021103","Total number of sigma-0 measurements",,"Numeric","0","0","5","Numeric","0","2","Operational"
999.00,"21","Radar data","021104","Likelihood computed for solution",,"Numeric","3","-30000","15","Numeric","3","5","Operational"
1000.00,"21","Radar data","021105","Normalized radar cross-section",,"dB","2","-10000","14","dB","2","5","Operational"
1001.00,"21","Radar data","021106","Kp variance coefficient (alpha)",,"Numeric","3","0","14","Numeric","3","5","Operational"
1002.00,"21","Radar data","021107","Kp variance coefficient (beta)",,"Numeric","8","0","16","Numeric","8","5","Operational"
1003.00,"21","Radar data","021109","SEAWINDS wind vector cell quality",,"Flag table","0","0","17","Flag table","0","6","Operational"
1004.00,"21","Radar data","021110","Number of inner-beam sigma-0 (forward of satellite)",,"Numeric","0","0","6","Numeric","0","2","Operational"
1005.00,"21","Radar data","021111","Number of outer-beam sigma-0 (forward of satellite)",,"Numeric","0","0","6","Numeric","0","2","Operational"
1006.00,"21","Radar data","021112","Number of inner-beam sigma-0 (aft of satellite)",,"Numeric","0","0","6","Numeric","0","2","Operational"
1007.00,"21","Radar data","021113","Number of outer-beam sigma-0 (aft of satellite)",,"Numeric","0","0","6","Numeric","0","2","Operational"
1008.00,"21","Radar data","021114","Kp variance coefficient (gamma)",,"dB","3","-140000","18","dB","3","6","Operational"
1009.00,"21","Radar data","021115","SEAWINDS sigma-0 quality",,"Flag table","0","0","17","Flag table","0","6","Operational"
1010.00,"21","Radar data","021116","SEAWINDS sigma-0 mode",,"Flag table","0","0","17","Flag table","0","6","Operational"
1011.00,"21","Radar data","021117","Sigma-0 variance quality control",,"Numeric","2","0","16","Numeric","2","5","Operational"
1012.00,"21","Radar data","021118","Attenuation correction on sigma-0",,"dB","2","-10000","14","dB","2","5","Operational"
1013.00,"21","Radar data","021119","Wind scatterometer geophysical model function",,"Code table","0","0","6","Code table","0","2","Operational"
1014.00,"21","Radar data","021120","Probability of rain",,"Numeric","3","0","10","Numeric","3","4","Operational"
1015.00,"21","Radar data","021121","SEAWINDS NOF rain index","*","Numeric","0","0","8","Numeric","0","3","Operational"
1016.00,"21","Radar data","021122","Attenuation correction on sigma-0 (from tB)",,"dB","2","-10000","14","dB","2","5","Operational"
1017.00,"21","Radar data","021123","SEAWINDS normalized radar cross-section",,"dB","2","-30000","15","dB","2","5","Operational"
1018.00,"21","Radar data","021128","Number of valid points per second used to derive previous parameters",,"Numeric","0","0","8","Numeric","0","3","Operational"
1019.00,"21","Radar data","021130","Spectrum total energy",,"Numeric","6","0","28","Numeric","6","9","Operational"
1020.00,"21","Radar data","021131","Spectrum max energy",,"Numeric","6","0","28","Numeric","6","9","Operational"
1021.00,"21","Radar data","021132","Direction of spectrum max on higher resolution grid",,"deg","3","0","19","deg","3","6","Operational"
1022.00,"21","Radar data","021133","Wavelength of spectrum max on higher resolution grid",,"m","3","0","29","m","3","9","Operational"
1023.00,"21","Radar data","021134","Range resolution of cress covariance spectrum",,"rad/m","3","0","19","rad/m","3","6","Operational"
1024.00,"21","Radar data","021135","Real part of cross spectra polar grid number of bins",,"Numeric","3","-524288","20","Numeric","3","7","Operational"
1025.00,"21","Radar data","021136","Imaginary part of cross spectra polar grid number of bins",,"Numeric","3","-524288","20","Numeric","3","7","Operational"
1026.00,"21","Radar data","021137","Ku band corrected ocean backscatter coefficient",,"dB","2","-32768","16","dB","2","5","Operational"
1027.00,"21","Radar data","021138","STD Ku band corrected ocean backscatter coefficient",,"dB","2","-32768","16","dB","2","5","Operational"
1028.00,"21","Radar data","021139","Ku band net instrumental correction for AGC",,"dB","2","-2048","12","dB","2","4","Operational"
1029.00,"21","Radar data","021140","S band corrected ocean backscatter coefficient",,"dB","2","-32768","16","dB","2","5","Operational"
1030.00,"21","Radar data","021141","STD S band corrected ocean backscatter coefficient",,"dB","2","-32768","16","dB","2","5","Operational"
1031.00,"21","Radar data","021142","S band net instrumental correction for AGC",,"dB","2","-1024","11","dB","2","4","Operational"
1032.00,"21","Radar data","021143","Ku band rain attenuation",,"dB","2","-1073741824","31","dB","2","10","Operational"
1033.00,"21","Radar data","021144","Altimeter rain flag",,"Flag table","0","0","2","Flag table","0","1","Operational"
1034.00,"21","Radar data","021145","Ku band automatic gain control",,"dB","2","0","13","dB","2","4","Operational"
1035.00,"21","Radar data","021146","RMS Ku band automatic gain control",,"dB","2","0","8","dB","2","3","Operational"
1036.00,"21","Radar data","021147","Number of valid points for Ku band automatic gain control",,"Numeric","0","0","5","Numeric","0","2","Operational"
1037.00,"21","Radar data","021150","Beam co-location",,"Code table","0","0","2","Code table","0","1","Operational"
1038.00,"21","Radar data","021151","Estimated error in sigma-0 at 40 degrees incidence angle",,"dB","2","0","9","dB","2","3","Operational"
1039.00,"21","Radar data","021152","Slope at 40 degrees incidence angle",,"dB/deg","2","-80","7","dB/deg","2","2","Operational"
1040.00,"21","Radar data","021153","Estimated error in slope at 40 degrees incidence angle",,"dB/deg","2","-40","6","dB/deg","2","2","Operational"
1041.00,"21","Radar data","021154","Soil moisture sensitivity",,"dB","2","0","12","dB","2","4","Operational"
1042.00,"21","Radar data","021155","Wind vector cell quality",,"Flag table","0","0","24","Flag table","0","8","Operational"
1043.00,"21","Radar data","021156","Backscatter distance",,"Numeric","1","-4096","13","Numeric","1","4","Operational"
1044.00,"21","Radar data","021157","Loss per unit length of atmosphere used",,"dB/m","10","0","22","dB/m","10","7","Operational"
1045.00,"21","Radar data","021158","ASCAT Kp quality estimate",,"Code table","0","0","2","Code table","0","1","Operational"
1046.00,"21","Radar data","021159","ASCAT sigma-0 usability",,"Code table","0","0","2","Code table","0","1","Operational"
1047.00,"21","Radar data","021160","ASCAT use of synthetic data",,"Numeric","3","0","10","Numeric","3","4","Operational"
1048.00,"21","Radar data","021161","ASCAT synthetic data quantity",,"Numeric","3","0","10","Numeric","3","4","Operational"
1049.00,"21","Radar data","021162","ASCAT satellite orbit and attitude quality",,"Numeric","3","0","10","Numeric","3","4","Operational"
1050.00,"21","Radar data","021163","ASCAT solar array reflection contamination",,"Numeric","3","0","10","Numeric","3","4","Operational"
1051.00,"21","Radar data","021164","ASCAT telemetry presence and quality",,"Numeric","3","0","10","Numeric","3","4","Operational"
1052.00,"21","Radar data","021165","ASCAT extrapolated reference function presence",,"Numeric","3","0","10","Numeric","3","4","Operational"
1053.00,"21","Radar data","021166","Land fraction",,"Numeric","3","0","10","Numeric","3","4","Operational"
1054.00,"21","Radar data","021169","Ice presence indicator",,"Code table","0","0","2","Code table","0","1","Operational"
1055.00,"21","Radar data","021170","C band corrected ocean backscatter coefficient",,"dB","2","-32768","16","dB","2","5","Operational"
1056.00,"21","Radar data","021171","RMS C band corrected ocean backscatter coefficient",,"dB","2","-32768","16","dB","2","5","Operational"
1057.00,"21","Radar data","021172","C band net instrumental correction for AGC",,"dB","2","-2048","12","dB","2","4","Operational"
1058.00,"21","Radar data","021173","C band automatic gain control",,"dB","2","0","13","dB","2","4","Operational"
1059.00,"21","Radar data","021174","RMS C band automatic gain control",,"dB","2","0","9","dB","2","3","Operational"
1060.00,"21","Radar data","021175","Number of valid points for C band automatic gain control",,"Numeric","0","0","10","Numeric","0","4","Operational"
1061.00,"21","Radar data","021176","High frequency variability correction",,"m","3","0","16","m","3","5","Operational"
1062.00,"21","Radar data","021177","Corrected OCOG backscatter coefficient",,"dB","2","0","16","dB","2","5","Operational"
1063.00,"21","Radar data","021178","STD of 20 Hz OCOG backscatter coefficient",,"dB","2","0","16","dB","2","5","Operational"
1064.00,"21","Radar data","021179","Number of 20 Hz valid points for OCOG backscatter coefficient",,"Numeric","0","0","16","Numeric","0","5","Operational"
1065.00,"21","Radar data","021180","Number of 20 Hz valid points for ocean backscatter coefficient",,"Numeric","0","0","8","Numeric","0","3","Operational"
1066.00,"21","Radar data","021181","20 Hz ocean backscatter coefficient",,"dB","2","0","16","dB","2","5","Operational"
1067.00,"21","Radar data","021182","20 Hz Ku band peakiness",,"Numeric","3","0","16","Numeric","3","5","Operational"
1068.00,"22","Oceanographic elements","022001","Direction of waves",,"degree true","0","0","9","degree true","0","3","Operational"
1069.00,"22","Oceanographic elements","022002","Direction of wind waves",,"degree true","0","0","9","degree true","0","3","Operational"
1070.00,"22","Oceanographic elements","022003","Direction of swell waves",,"degree true","0","0","9","degree true","0","3","Operational"
1071.00,"22","Oceanographic elements","022004","Direction of current","(see Note 7)","degree true","0","0","9","degree true","0","3","Operational"
1072.00,"22","Oceanographic elements","022005","Direction of sea surface current",,"degree true","0","0","9","degree true","0","3","Operational"
1073.00,"22","Oceanographic elements","022011","Period of waves",,"s","0","0","6","s","0","2","Operational"
1074.00,"22","Oceanographic elements","022012","Period of wind waves",,"s","0","0","6","s","0","2","Operational"
1075.00,"22","Oceanographic elements","022013","Period of swell waves",,"s","0","0","6","s","0","2","Operational"
1076.00,"22","Oceanographic elements","022021","Height of waves",,"m","1","0","10","m","1","4","Operational"
1077.00,"22","Oceanographic elements","022022","Height of wind waves",,"m","1","0","10","m","1","4","Operational"
1078.00,"22","Oceanographic elements","022023","Height of swell waves",,"m","1","0","10","m","1","4","Operational"
1079.00,"22","Oceanographic elements","022025","Standard deviation wave height",,"m","2","0","10","m","2","4","Operational"
1080.00,"22","Oceanographic elements","022026","Standard deviation of significant wave height",,"m","2","0","10","m","2","4","Operational"
1081.00,"22","Oceanographic elements","022031","Speed of current",,"m/s","2","0","13","m/s","2","4","Operational"
1082.00,"22","Oceanographic elements","022032","Speed of sea surface current",,"m/s","2","0","13","m/s","2","4","Operational"
1083.00,"22","Oceanographic elements","022035","Tidal elevation with respect to local chart datum",,"m","2","0","14","m","2","4","Operational"
1084.00,"22","Oceanographic elements","022036","Meteorological residual tidal elevation (surge or offset)",,"m","2","0","14","m","2","4","Operational"
1085.00,"22","Oceanographic elements","022037","Tidal elevation with respect to national land datum",,"m","3","-10000","15","m","3","5","Operational"
1086.00,"22","Oceanographic elements","022038","Tidal elevation with respect to local chart datum",,"m","3","-10000","15","m","3","5","Operational"
1087.00,"22","Oceanographic elements","022039","Meteorological residual tidal elevation (surge or offset)","(see Note 4)","m","3","-5000","13","m","3","4","Operational"
1088.00,"22","Oceanographic elements","022040","Meteorological residual tidal elevation (surge or offset)","(see Note 4)","m","3","-5000","14","m","3","5","Operational"
1089.00,"22","Oceanographic elements","022041","Sea-surface temperature (15-day running mean)",,"K","1","0","12","K","1","4","Operational"
1090.00,"22","Oceanographic elements","022042","Sea/water temperature",,"K","1","0","12","K","1","4","Operational"
1091.00,"22","Oceanographic elements","022043","Sea/water temperature",,"K","2","0","15","K","2","5","Operational"
1092.00,"22","Oceanographic elements","022044","Sound velocity",,"m/s","1","0","14","m/s","1","5","Operational"
1093.00,"22","Oceanographic elements","022045","Sea/water temperature",,"K","3","0","19","K","3","6","Operational"
1094.00,"22","Oceanographic elements","022046","Sea ice fraction",,"Numeric","2","0","7","Numeric","2","3","Operational"
1095.00,"22","Oceanographic elements","022049","Sea surface temperature",,"K","2","0","15","K","2","5","Operational"
1096.00,"22","Oceanographic elements","022050","Standard deviation sea-surface temperature",,"K","2","0","8","K","2","3","Operational"
1097.00,"22","Oceanographic elements","022055","Float cycle number",,"Numeric","0","0","10","Numeric","0","3","Operational"
1098.00,"22","Oceanographic elements","022056","Direction of profile",,"Code table","0","0","2","Code table","0","1","Operational"
1099.00,"22","Oceanographic elements","022059","Sea surface salinity",,"0/00","2","0","14","0/00","2","5","Operational"
1100.00,"22","Oceanographic elements","022060","Lagrangian drifter drogue status",,"Code table","0","0","3","Code table","0","1","Operational"
1101.00,"22","Oceanographic elements","022061","State of the sea",,"Code table","0","0","4","Code table","0","2","Operational"
1102.00,"22","Oceanographic elements","022062","Salinity",,"0/00","2","0","14","0/00","2","5","Operational"
1103.00,"22","Oceanographic elements","022063","Total water depth",,"m","0","0","14","m","0","5","Operational"
1104.00,"22","Oceanographic elements","022064","Salinity",,"0/00","3","0","17","0/00","3","6","Operational"
1105.00,"22","Oceanographic elements","022065","Water pressure",,"Pa","-3","0","17","Pa","-3","6","Operational"
1106.00,"22","Oceanographic elements","022066","Water conductivity",,"S/m","6","0","26","S/m","6","8","Operational"
1107.00,"22","Oceanographic elements","022067","Instrument type for water temperature profile measurement",,"Code table","0","0","10","Code table","0","4","Operational"
1108.00,"22","Oceanographic elements","022068","Water temperature profile recorder types",,"Code table","0","0","7","Code table","0","3","Operational"
1109.00,"22","Oceanographic elements","022069","Spectral wave density",,"m2 Hz-1","3","0","22","m2 Hz-1","3","7","Operational"
1110.00,"22","Oceanographic elements","022070","Significant wave height",,"m","2","0","13","m","2","4","Operational"
1111.00,"22","Oceanographic elements","022071","Spectral peak wave period",,"s","1","0","9","s","1","3","Operational"
1112.00,"22","Oceanographic elements","022072","Spectral peak wave length",,"m","0","0","13","m","0","4","Operational"
1113.00,"22","Oceanographic elements","022073","Maximum wave height",,"m","2","0","13","m","2","4","Operational"
1114.00,"22","Oceanographic elements","022074","Average wave period",,"s","1","0","9","s","1","3","Operational"
1115.00,"22","Oceanographic elements","022075","Average wave length",,"m","0","0","13","m","0","4","Operational"
1116.00,"22","Oceanographic elements","022076","Direction from which dominant waves are coming",,"degree true","0","0","9","degree true","0","3","Operational"
1117.00,"22","Oceanographic elements","022077","Directional spread of dominant wave",,"deg","0","0","9","deg","0","3","Operational"
1118.00,"22","Oceanographic elements","022078","Duration of wave record",,"s","0","0","12","s","0","4","Operational"
1119.00,"22","Oceanographic elements","022079","Length of wave record",,"m","0","0","16","m","0","5","Operational"
1120.00,"22","Oceanographic elements","022080","Waveband central frequency",,"Hz","3","0","10","Hz","3","4","Operational"
1121.00,"22","Oceanographic elements","022081","Waveband central wave number",,"m-1","5","0","13","m-1","5","4","Operational"
1122.00,"22","Oceanographic elements","022082","Maximum non-directional spectral wave density",,"m2 s","2","0","20","m2 s","2","7","Operational"
1123.00,"22","Oceanographic elements","022083","Maximum non-directional spectral wave number",,"m3","2","0","20","m3","2","7","Operational"
1124.00,"22","Oceanographic elements","022084","Band containing maximum non-directional spectral wave density",,"Numeric","0","0","7","Numeric","0","3","Operational"
1125.00,"22","Oceanographic elements","022085","Spectral wave density ratio",,"Numeric","0","0","7","Numeric","0","3","Operational"
1126.00,"22","Oceanographic elements","022086","Mean direction from which waves are coming",,"degree true","0","0","9","degree true","0","3","Operational"
1127.00,"22","Oceanographic elements","022087","Principal direction from which waves are coming",,"degree true","0","0","9","degree true","0","3","Operational"
1128.00,"22","Oceanographic elements","022088","First normalized polar coordinate from Fourier coefficients",,"Numeric","2","0","7","Numeric","2","3","Operational"
1129.00,"22","Oceanographic elements","022089","Second normalized polar coordinate from Fourier coefficients",,"Numeric","2","0","7","Numeric","2","3","Operational"
1130.00,"22","Oceanographic elements","022090","Non-directional spectral estimate by wave frequency",,"m2 s","2","0","20","m2 s","2","7","Operational"
1131.00,"22","Oceanographic elements","022091","Non-directional spectral estimate by wave number",,"m3","2","0","20","m3","2","7","Operational"
1132.00,"22","Oceanographic elements","022092","Directional spectral estimate by wave frequency",,"m2 rad-1 s","2","0","20","m2 rad-1 s","2","7","Operational"
1133.00,"22","Oceanographic elements","022093","Directional spectral estimate by wave number",,"m4","2","0","20","m4","2","7","Operational"
1134.00,"22","Oceanographic elements","022094","Total number of wave bands",,"Numeric","0","0","7","Numeric","0","3","Operational"
1135.00,"22","Oceanographic elements","022095","Directional spread of individual waves",,"deg","0","0","8","deg","0","3","Operational"
1136.00,"22","Oceanographic elements","022096","Spectral band width",,"/s","3","0","4","/s","3","2","Operational"
1137.00,"22","Oceanographic elements","022097","Mean wavelength > 731 m of image spectrum at low wave numbers",,"m","0","0","14","m","0","5","Operational"
1138.00,"22","Oceanographic elements","022098","Wavelength spread (wavelength > 731 m) at low wave numbers",,"m","0","0","14","m","0","5","Operational"
1139.00,"22","Oceanographic elements","022099","Mean direction at low wave numbers (wavelength > 731 m)",,"degree true","0","0","9","degree true","0","3","Operational"
1140.00,"22","Oceanographic elements","022100","Direction spread at low wave numbers (wavelength > 731 m)",,"deg","0","0","9","deg","0","3","Operational"
1141.00,"22","Oceanographic elements","022101","Total energy (wavelength > 731m) at low wave numbers",,"Numeric","0","0","31","Numeric","0","10","Operational"
1142.00,"22","Oceanographic elements","022120","Tide station automated water level check",,"Code table","0","0","5","Code table","0","2","Operational"
1143.00,"22","Oceanographic elements","022121","Tide station manual water level check",,"Code table","0","0","5","Code table","0","2","Operational"
1144.00,"22","Oceanographic elements","022122","Tide station automated meteorological data check",,"Code table","0","0","5","Code table","0","2","Operational"
1145.00,"22","Oceanographic elements","022123","Tide station manual meteorological data check",,"Code table","0","0","5","Code table","0","2","Operational"
1146.00,"22","Oceanographic elements","022141","Sea-surface temperature (15-day running mean)",,"K","2","0","15","K","2","5","Operational"
1147.00,"22","Oceanographic elements","022142","Square of significant wave height",,"m2","3","-33554432  ","26","m2","3","8","Operational"
1148.00,"22","Oceanographic elements","022143","STD of 20 Hz SWH squared",,"m2","3","-8388608","24","m2","3","8","Operational"
1149.00,"22","Oceanographic elements","022144","Number of 20 Hz valid points for SWH squared",,"Numeric","0","0","9","Numeric","0","3","Operational"
1150.00,"22","Oceanographic elements","022145","STD of 20 Hz ocean range",,"m","3","-33554432  ","31","m","3","10","Operational"
1151.00,"22","Oceanographic elements","022146","OCOG range",,"m","3","0","31","m","3","10","Operational"
1152.00,"22","Oceanographic elements","022147","STD of 20 Hz OCOG range",,"m","3","-8388608","31","m","3","10","Operational"
1153.00,"22","Oceanographic elements","022148","Number of 20 Hz valid points for ocean range",,"Numeric","0","0","9","Numeric","0","3","Operational"
1154.00,"22","Oceanographic elements","022149","20 Hz significant wave height squared",,"m2","3","-33554432  ","26","m2","3","8","Operational"
1155.00,"22","Oceanographic elements","022150","Number of 18 Hz valid points for Ku band",,"Numeric","0","0","10","Numeric","0","4","Operational"
1156.00,"22","Oceanographic elements","022151","Ku band ocean range",,"m","3","0","31","m","3","10","Operational"
1157.00,"22","Oceanographic elements","022152","STD of 18 Hz Ku band ocean range",,"m","3","0","16","m","3","5","Operational"
1158.00,"22","Oceanographic elements","022153","Number of 18 Hz valid points for S band",,"Numeric","0","0","10","Numeric","0","4","Operational"
1159.00,"22","Oceanographic elements","022154","S band ocean range",,"m","3","0","31","m","3","10","Operational"
1160.00,"22","Oceanographic elements","022155","STD of 18 Hz S band ocean range",,"m","3","0","16","m","3","5","Operational"
1161.00,"22","Oceanographic elements","022156","Ku band significant wave height",,"m","3","0","16","m","3","5","Operational"
1162.00,"22","Oceanographic elements","022157","STD of 18 Hz Ku band ocean range",,"m","3","0","16","m","3","5","Operational"
1163.00,"22","Oceanographic elements","022158","S band significant wave height",,"m","3","0","16","m","3","5","Operational"
1164.00,"22","Oceanographic elements","022159","STD of 18 Hz S band significant wave height",,"m","3","0","16","m","3","5","Operational"
1165.00,"22","Oceanographic elements","022160","Normalized inverse wave age",,"Numeric","6","0","21","Numeric","6","7","Operational"
1166.00,"22","Oceanographic elements","022161","Wave spectra",,"m4","4","0","27","m4","4","9","Operational"
1167.00,"22","Oceanographic elements","022162","RMS of 20 Hz Ku band ocean range",,"m","3","0","16","m","3","5","Operational"
1168.00,"22","Oceanographic elements","022163","Number of 20 Hz valid points for Ku band",,"Numeric","0","0","10","Numeric","0","4","Operational"
1169.00,"22","Oceanographic elements","022164","RMS 20 Hz Ku band significant wave height",,"m","3","0","16","m","3","5","Operational"
1170.00,"22","Oceanographic elements","022165","Number of 20 Hz valid points for Ku band significant wave height",,"Numeric","0","0","10","Numeric","0","4","Operational"
1171.00,"22","Oceanographic elements","022166","Ku band net instrumental correction for significant wave height",,"m","3","-1000","11","m","3","4","Operational"
1172.00,"22","Oceanographic elements","022167","Number of valid points for Ku band backscatter",,"Numeric","0","0","10","Numeric","0","4","Operational"
1173.00,"22","Oceanographic elements","022168","C band ocean range",,"m","3","0","31","m","3","10","Operational"
1174.00,"22","Oceanographic elements","022169","RMS of C band ocean range",,"m","3","0","16","m","3","5","Operational"
1175.00,"22","Oceanographic elements","022170","Number of 20 Hz valid points for C band",,"Numeric","0","0","10","Numeric","0","4","Operational"
1176.00,"22","Oceanographic elements","022171","C band significant wave height",,"m","3","0","16","m","3","5","Operational"
1177.00,"22","Oceanographic elements","022172","RMS 20 Hz C band significant wave height",,"m","3","0","16","m","3","5","Operational"
1178.00,"22","Oceanographic elements","022173","Number of 20 Hz valid points for C band significant wave height",,"Numeric","0","0","10","Numeric","0","4","Operational"
1179.00,"22","Oceanographic elements","022174","C band net instrumental correction for significant wave height",,"m","3","-1000","11","m","3","4","Operational"
1180.00,"22","Oceanographic elements","022175","Number of valid points for C band backscatter",,"Numeric","0","0","10","Numeric","0","4","Operational"
1181.00,"22","Oceanographic elements","022177","Height of XBT/XCTD launcher",,"m","0","0","6","m","0","3","Operational"
1182.00,"22","Oceanographic elements","022178","XBT/XCTD launcher type",,"Code table","0","0","8","Code table","0","3","Operational"
1186.00,"22","Oceanographic elements","022182","Water column height","(see Note 9)","m","3","0","23","m","3","7","Operational"
1187.00,"22","Oceanographic elements","022184","Water column height deviation from the reference value",,"m","3","-2000","12","m","3","4","Operational"
1188.00,"22","Oceanographic elements","022185","BPR transmission count",,"Numeric","0","0","10","Numeric","0","3","Operational"
1191.00,"23","Dispersal and transport","023001","Accident early notification - article applicable",,"Code table","0","0","3","Code table","0","1","Operational"
1192.00,"23","Dispersal and transport","023002","Activity or facility involved in incident",,"Code table","0","0","5","Code table","0","2","Operational"
1193.00,"23","Dispersal and transport","023003","Type of release",,"Code table","0","0","3","Code table","0","1","Operational"
1194.00,"23","Dispersal and transport","023004","Countermeasures taken near border",,"Code table","0","0","3","Code table","0","1","Operational"
1195.00,"23","Dispersal and transport","023005","Cause of incident",,"Code table","0","0","2","Code table","0","1","Operational"
1196.00,"23","Dispersal and transport","023006","Incident situation",,"Code table","0","0","3","Code table","0","1","Operational"
1197.00,"23","Dispersal and transport","023007","Characteristics of release",,"Code table","0","0","3","Code table","0","1","Operational"
1198.00,"23","Dispersal and transport","023008","State of current release",,"Code table","0","0","2","Code table","0","1","Operational"
1199.00,"23","Dispersal and transport","023009","State of expected release",,"Code table","0","0","2","Code table","0","1","Operational"
1200.00,"23","Dispersal and transport","023016","Possibility of significant chemical toxic health effect",,"Code table","0","0","2","Code table","0","1","Operational"
1201.00,"23","Dispersal and transport","023017","Flow discharge of major recipient",,"m3/s","6","0","20","m3/s","6","7","Operational"
1202.00,"23","Dispersal and transport","023018","Release behaviour over time",,"Code table","0","0","3","Code table","0","1","Operational"
1203.00,"23","Dispersal and transport","023019","Actual release height",,"m","0","-15000","17","m","0","6","Operational"
1204.00,"23","Dispersal and transport","023021","Effective release height",,"m","0","-15000","17","m","0","6","Operational"
1205.00,"23","Dispersal and transport","023022","Distance of release point or site of incident",,"m","0","0","24","m","0","8","Operational"
1206.00,"23","Dispersal and transport","023023","Main transport speed in the atmosphere",,"m/s","1","0","12","m/s","1","4","Operational"
1207.00,"23","Dispersal and transport","023024","Main transport speed in water",,"m/s","2","0","13","m/s","2","4","Operational"
1208.00,"23","Dispersal and transport","023025","Main transport speed in ground water",,"m/s","2","0","13","m/s","2","4","Operational"
1209.00,"23","Dispersal and transport","023027","Main transport direction in the atmosphere",,"degree true","0","0","9","degree true","0","3","Operational"
1210.00,"23","Dispersal and transport","023028","Main transport direction in water",,"degree true","0","0","9","degree true","0","3","Operational"
1211.00,"23","Dispersal and transport","023029","Main transport direction in ground water",,"degree true","0","0","9","degree true","0","3","Operational"
1212.00,"23","Dispersal and transport","023031","Possibility that plume will encounter precipitation in State in which incident occurred",,"Code table","0","0","2","Code table","0","1","Operational"
1213.00,"23","Dispersal and transport","023032","Plume will encounter change in wind direction and/or speed flag",,"Code table","0","0","2","Code table","0","1","Operational"
1214.00,"23","Dispersal and transport","023040","Flow discharge - river",,"m3/s","1","0","22","m3/s","1","7","Operational"
1215.00,"23","Dispersal and transport","023041","Flow discharge - well",,"m3/s","3","0","16","m3/s","3","5","Operational"
1216.00,"24","Radiological elements","024001","Estimate of amount of radioactivity released up to specified time","*","Bq","-11","0","28","Bq","-11","9","Operational"
1217.00,"24","Radiological elements","024002","Estimated maximum potential release",,"Bq","-11","0","28","Bq","-11","9","Operational"
1218.00,"24","Radiological elements","024003","Composition of release",,"Code table","0","0","5","Code table","0","2","Operational"
1219.00,"24","Radiological elements","024004","Element name",,"CCITT IA5","0","0","16","Character","0","2","Operational"
1220.00,"24","Radiological elements","024005","Isotope mass",,"Numeric","0","0","9","Numeric","0","3","Operational"
1221.00,"24","Radiological elements","024011","Dose","*","mSv","2","0","32","mSv","2","10","Operational"
1222.00,"24","Radiological elements","024012","Trajectory dose (defined location and expected time of arrival)",,"mSv","2","0","32","mSv","2","10","Operational"
1223.00,"24","Radiological elements","024013","Gamma dose in air along the main transport path (defined location and time period)",,"mSv","2","0","32","mSv","2","10","Operational"
1224.00,"24","Radiological elements","024014","Gamma radiation dose rate",,"nSv/h","1","0","14","nSv/h","1","4","Operational"
1225.00,"24","Radiological elements","024021","Air concentration (of named isotope type including gross beta)",,"Bq m-3","2","0","32","Bq m-3","2","10","Operational"
1226.00,"24","Radiological elements","024022","Concentration in precipitation (of named isotope type)",,"Bq/l","2","0","32","Bq/l","2","10","Operational"
1227.00,"24","Radiological elements","024023","Pulse rate of beta radiation",,"/s","1","0","14","/s","1","4","Operational"
1228.00,"24","Radiological elements","024024","Pulse rate of gamma radiation",,"/s","1","0","14","/s","1","4","Operational"
1229.00,"25","Processing information","025001","Range-gate length",,"m","-1","0","6","m","-1","2","Operational"
1230.00,"25","Processing information","025002","Number of gates averaged",,"Numeric","0","0","4","Numeric","0","2","Operational"
1231.00,"25","Processing information","025003","Number of integrated pulses",,"Numeric","0","0","8","Numeric","0","3","Operational"
1232.00,"25","Processing information","025004","Echo processing",,"Code table","0","0","2","Code table","0","1","Operational"
1233.00,"25","Processing information","025005","Echo integration",,"Code table","0","0","2","Code table","0","1","Operational"
1234.00,"25","Processing information","025006","Z to R conversion",,"Code table","0","0","3","Code table","0","1","Operational"
1235.00,"25","Processing information","025007","Z to R conversion factor",,"Numeric","0","0","12","Numeric","0","4","Operational"
1236.00,"25","Processing information","025008","Z to R conversion exponent",,"Numeric","2","0","9","Numeric","2","3","Operational"
1237.00,"25","Processing information","025009","Calibration method","(see Note 3)","Flag table","0","0","4","Flag table","0","2","Operational"
1238.00,"25","Processing information","025010","Clutter treatment",,"Code table","0","0","4","Code table","0","2","Operational"
1239.00,"25","Processing information","025011","Ground occultation correction (screening)",,"Code table","0","0","2","Code table","0","1","Operational"
1240.00,"25","Processing information","025012","Range attenuation correction",,"Code table","0","0","2","Code table","0","1","Operational"
1241.00,"25","Processing information","025013","Bright-band correction",,"Flag table","0","0","2","Flag table","0","1","Operational"
1242.00,"25","Processing information","025014","Azimuth clutter cut-off","(see Note 1)","Numeric","0","0","12","Numeric","0","4","Operational"
1243.00,"25","Processing information","025015","Radome attenuation correction",,"Flag table","0","0","2","Flag table","0","1","Operational"
1244.00,"25","Processing information","025016","Clear-air attenuation correction",,"dB/m","5","0","6","dB/m","5","2","Operational"
1245.00,"25","Processing information","025017","Precipitation attenuation correction",,"Flag table","0","0","2","Flag table","0","1","Operational"
1246.00,"25","Processing information","025018","A to Z law for attenuation factor",,"Numeric","7","0","6","Numeric","7","2","Operational"
1247.00,"25","Processing information","025019","A to Z law for attenuation exponent",,"Numeric","2","0","7","Numeric","2","3","Operational"
1248.00,"25","Processing information","025020","Mean speed estimation",,"Code table","0","0","2","Code table","0","1","Operational"
1249.00,"25","Processing information","025021","Wind computation enhancement",,"Flag table","0","0","8","Flag table","0","3","Operational"
1250.00,"25","Processing information","025022","GHRSST rejection flag",,"Flag table","0","0","9","Flag table","0","3","Operational"
1251.00,"25","Processing information","025023","GHRSST confidence flag",,"Flag table","0","0","9","Flag table","0","3","Operational"
1252.00,"25","Processing information","025024","GHRSST data quality",,"Code table","0","0","4","Code table","0","2","Operational"
1253.00,"25","Processing information","025025","Battery voltage",,"V","1","0","9","V","1","3","Operational"
1254.00,"25","Processing information","025026","Battery voltage (large range)",,"V","1","0","12","V","1","4","Operational"
1255.00,"25","Processing information","025028","Operator or manufacturer defined parameter",,"Numeric","1","-16384","15","Numeric","1","5","Operational"
1256.00,"25","Processing information","025029","Calibration method","(see Note 3)","Flag table","0","0","6","Flag table","0","2","Operational"
1257.00,"25","Processing information","025030","Running mean sea-surface temperature usage",,"Code table","0","0","2","Code table","0","1","Operational"
1258.00,"25","Processing information","025031","NWP-generated vertical profile thinning method",,"Code table","0","0","3","Code table","0","1","Operational"
1259.00,"25","Processing information","025032","Wind profiler mode information","(see Note 2)","Code table","0","0","2","Code table","0","1","Operational"
1260.00,"25","Processing information","025033","Wind profiler submode information","(see Note 2)","Code table","0","0","2","Code table","0","1","Operational"
1261.00,"25","Processing information","025034","Wind profiler quality control test results","(see Note 2)","Flag table","0","0","4","Flag table","0","2","Operational"
1262.00,"25","Processing information","025035","Decision method for polarity","(see Note 5)","Code table","0","0","3","Code table","0","1","Operational"
1263.00,"25","Processing information","025036","Atmospherics location method",,"Code table","0","0","4","Code table","0","2","Operational"
1264.00,"25","Processing information","025037","SST bias",,"K","2","-127","8","K","2","3","Operational"
1265.00,"25","Processing information","025038","Difference between SST and analysis",,"K","1","-127","8","K","1","3","Operational"
1266.00,"25","Processing information","025040","CO2 wind product derivation",,"Code table","0","0","4","Code table","0","2","Operational"
1267.00,"25","Processing information","025041","Moving platform direction reporting method",,"Code table","0","0","2","Code table","0","1","Operational"
1268.00,"25","Processing information","025042","Moving platform speed reporting method",,"Code table","0","0","2","Code table","0","1","Operational"
1269.00,"25","Processing information","025043","Wave sampling interval (time)",,"s","4","0","15","s","4","5","Operational"
1270.00,"25","Processing information","025044","Wave sampling interval (space)",,"m","2","0","14","m","2","5","Operational"
1271.00,"25","Processing information","025045","HIRS channel combination",,"Flag table","0","0","21","Flag table","0","7","Operational"
1272.00,"25","Processing information","025046","MSU channel combination",,"Flag table","0","0","5","Flag table","0","2","Operational"
1273.00,"25","Processing information","025047","SSU channel combination",,"Flag table","0","0","4","Flag table","0","2","Operational"
1274.00,"25","Processing information","025048","AMSU-A channel combination",,"Flag table","0","0","16","Flag table","0","6","Operational"
1275.00,"25","Processing information","025049","AMSU-B channel combination",,"Flag table","0","0","6","Flag table","0","2","Operational"
1276.00,"25","Processing information","025050","Principal component score",,"Numeric","4","-131072","18","Numeric","4","6","Operational"
1277.00,"25","Processing information","025051","AVHRR channel combination",,"Flag table","0","0","7","Flag table","0","3","Operational"
1278.00,"25","Processing information","025052","Log-10 of principal components normalized fit to data",,"Numeric","4","0","15","Numeric","4","5","Operational"
1279.00,"25","Processing information","025053","Observation quality",,"Flag table","0","0","12","Flag table","0","4","Operational"
1280.00,"25","Processing information","025054","SSMIS subframe ID number",,"Numeric","0","0","5","Numeric","0","2","Operational"
1281.00,"25","Processing information","025055","Multiplexer housekeeping",,"K","2","0","16","K","2","5","Operational"
1282.00,"25","Processing information","025060","Software identification","(see Note 2)","Numeric","0","0","14","Numeric","0","5","Operational"
1283.00,"25","Processing information","025061","Software identification and version number",,"CCITT IA5","0","0","96","Character","0","12","Operational"
1284.00,"25","Processing information","025062","Database identification",,"Numeric","0","0","14","Numeric","0","5","Operational"
1285.00,"25","Processing information","025063","Central processor or system identifier","(see Note 6)","Code table","0","0","8","Code table","0","3","Operational"
1286.00,"25","Processing information","025065","Orientation correction (azimuth)",,"deg","2","-1000","11","deg","2","4","Operational"
1287.00,"25","Processing information","025066","Orientation correction (elevation)",,"deg","2","-1000","11","deg","2","4","Operational"
1288.00,"25","Processing information","025067","Radiosonde release point pressure correction",,"Pa","0","-8000","14","Pa","0","4","Operational"
1289.00,"25","Processing information","025068","Number of archive recomputes",,"Numeric","0","0","7","Numeric","0","3","Operational"
1290.00,"25","Processing information","025069","Flight level pressure corrections",,"Flag table","0","0","8","Flag table","0","3","Operational"
1291.00,"25","Processing information","025070","Major frame count",,"Numeric","0","0","4","Numeric","0","2","Operational"
1292.00,"25","Processing information","025071","Frame count",,"Numeric","0","0","5","Numeric","0","2","Operational"
1293.00,"25","Processing information","025075","Satellite antenna corrections version number",,"Numeric","0","0","5","Numeric","0","2","Operational"
1294.00,"25","Processing information","025076","Log-10 of (temperature-radiance central wave number) for ATOVS",,"log (m-1)","8","0","30","log (m-1)","8","10","Operational"
1295.00,"25","Processing information","025077","Bandwidth correction coefficient 1 for ATOVS",,"Numeric","5","-100000","18","Numeric","5","7","Operational"
1296.00,"25","Processing information","025078","Bandwidth correction coefficient 2 for ATOVS",,"Numeric","5","0","17","Numeric","5","6","Operational"
1297.00,"25","Processing information","025079","Albedo-radiance solar filtered irradiance for ATOVS",,"W m-2","4","0","24","W m-2","4","8","Operational"
1298.00,"25","Processing information","025080","Albedo-radiance equivalent filter width for ATOVS",,"m","10","0","14","m","10","5","Operational"
1299.00,"25","Processing information","025081","Incidence angle",,"deg","3","0","17","deg","3","6","Operational"
1300.00,"25","Processing information","025082","Azimuth angle",,"deg","3","0","19","deg","3","6","Operational"
1301.00,"25","Processing information","025083","Faraday rotational angle",,"deg","3","0","19","deg","3","6","Operational"
1302.00,"25","Processing information","025084","Geometric rotational angle",,"deg","5","0","26","deg","5","8","Operational"
1303.00,"25","Processing information","025085","Fraction of clear pixels in HIRS FOV",,"Numeric","0","0","7","Numeric","0","3","Operational"
1304.00,"25","Processing information","025086","Depth correction indicator",,"Code table","0","0","2","Code table","0","1","Operational"
1305.00,"25","Processing information","025090","Orbit state flag",,"Code table","0","0","4","Code table","0","2","Operational"
1306.00,"25","Processing information","025091","Structure constant of the refraction index (Cn2)",,"dB","3","-18192","13","dB","3","5","Operational"
1307.00,"25","Processing information","025092","Acoustic propagation velocity",,"m/s","2","28000","14","m/s","2","5","Operational"
1308.00,"25","Processing information","025093","RASS computation correction",,"Flag table","0","0","8","Flag table","0","3","Operational"
1309.00,"25","Processing information","025095","Altimeter state flag",,"Flag table","0","0","2","Flag table","0","1","Operational"
1310.00,"25","Processing information","025096","Radiometer state flag",,"Flag table","0","0","5","Flag table","0","2","Operational"
1311.00,"25","Processing information","025097","Three-dimensional error estimate of the navigator orbit",,"Code table","0","0","4","Code table","0","2","Operational"
1312.00,"25","Processing information","025098","Altimeter data quality flag",,"Flag table","0","0","9","Flag table","0","3","Operational"
1313.00,"25","Processing information","025099","Altimeter correction quality flag",,"Flag table","0","0","9","Flag table","0","3","Operational"
1314.00,"25","Processing information","025100","XBT/XCTD fall rate equation coefficient a",,"Numeric","5","0","20","Numeric","5","6","Operational"
1315.00,"25","Processing information","025101","XBT/XCTD fall rate equation coefficient b",,"Numeric","5","-500000","21","Numeric","5","6","Operational"
1316.00,"25","Processing information","025102","Number of missing lines excluding data gaps",,"Numeric","0","0","8","Numeric","0","3","Operational"
1317.00,"25","Processing information","025103","Number of directional bins",,"Numeric","0","0","8","Numeric","0","3","Operational"
1318.00,"25","Processing information","025104","Number of wavelength bins",,"Numeric","0","0","8","Numeric","0","3","Operational"
1319.00,"25","Processing information","025105","First directional bin",,"deg","3","0","19","deg","3","6","Operational"
1320.00,"25","Processing information","025106","Directional bin step",,"deg","3","0","19","deg","3","6","Operational"
1321.00,"25","Processing information","025107","First wavelength bin",,"m","3","0","29","m","3","9","Operational"
1322.00,"25","Processing information","025108","Last wavelength bin",,"m","3","0","29","m","3","9","Operational"
1323.00,"25","Processing information","025110","Image processing summary",,"Flag table","0","0","10","Flag table","0","4","Operational"
1324.00,"25","Processing information","025111","Number of input data gaps",,"Numeric","0","0","8","Numeric","0","3","Operational"
1325.00,"25","Processing information","025120","RA2-L2-processing flag",,"Code table","0","0","2","Code table","0","1","Operational"
1326.00,"25","Processing information","025121","RA2-L2-processing quality",,"%","0","0","7","%","0","3","Operational"
1327.00,"25","Processing information","025122","Hardware configuration for RF",,"Code table","0","0","2","Code table","0","1","Operational"
1328.00,"25","Processing information","025123","Hardware configuration for HPA",,"Code table","0","0","2","Code table","0","1","Operational"
1329.00,"25","Processing information","025124","MWR-L2-processing flag",,"Code table","0","0","2","Code table","0","1","Operational"
1330.00,"25","Processing information","025125","MWR-L2-processing quality",,"%","0","0","7","%","0","3","Operational"
1331.00,"25","Processing information","025126","Model dry tropospheric correction",,"m","3","-32768","16","m","3","5","Operational"
1332.00,"25","Processing information","025127","Inverted barometer correction",,"m","3","-32768","16","m","3","5","Operational"
1333.00,"25","Processing information","025128","Model wet tropospheric correction",,"m","3","-32768","16","m","3","5","Operational"
1334.00,"25","Processing information","025129","MWR derived wet tropospheric correction",,"m","3","-32768","16","m","3","5","Operational"
1335.00,"25","Processing information","025130","RA2 ionospheric correction on Ku band",,"m","3","-32768","16","m","3","5","Operational"
1336.00,"25","Processing information","025131","Ionospheric correction from Doris on Ku band",,"m","3","-32768","16","m","3","5","Operational"
1337.00,"25","Processing information","025132","Ionospheric correction from model on Ku band",,"m","3","-32768","16","m","3","5","Operational"
1338.00,"25","Processing information","025133","Sea state bias correction on Ku band",,"m","3","-32768","16","m","3","5","Operational"
1339.00,"25","Processing information","025134","RA2 ionospheric correction on S band",,"m","3","-32768","16","m","3","5","Operational"
1340.00,"25","Processing information","025135","Ionospheric correction from Doris on S band",,"m","3","-32768","16","m","3","5","Operational"
1341.00,"25","Processing information","025136","Ionospheric correction from model on S band",,"m","3","-32768","16","m","3","5","Operational"
1342.00,"25","Processing information","025137","Sea state bias correction on S band",,"m","3","-32768","16","m","3","5","Operational"
1343.00,"25","Processing information","025138","Average signal-to-noise ratio",,"Numeric","0","-2048","12","Numeric","0","4","Operational"
1344.00,"25","Processing information","025140","Start channel",,"Numeric","0","0","14","Numeric","0","5","Operational"
1345.00,"25","Processing information","025141","End channel",,"Numeric","0","0","14","Numeric","0","5","Operational"
1346.00,"25","Processing information","025142","Channel scale factor",,"Numeric","0","0","6","Numeric","0","2","Operational"
1347.00,"25","Processing information","025143","Linear coefficient",,"Numeric","6","-5000000","24","Numeric","6","8","Operational"
1350.00,"25","Processing information","025150","Method of tropical cyclone intensity analysis using satellite data",,"Code table","0","0","4","Code table","0","2","Operational"
1354.00,"25","Processing information","025160","Ku band net instrumental correction",,"m","4","-120000","18","m","4","6","Operational"
1355.00,"25","Processing information","025161","C band net instrumental correction",,"m","4","-120000","18","m","4","6","Operational"
1356.00,"25","Processing information","025162","Sea state bias correction on C band",,"m","4","-6000","13","m","4","4","Operational"
1357.00,"25","Processing information","025163","Altimeter ionospheric correction on Ku band",,"m","3","-32768","16","m","3","5","Operational"
1358.00,"25","Processing information","025164","Radiometer wet tropospheric correction",,"m","4","-5000","13","m","4","4","Operational"
1359.00,"25","Processing information","025170","Sampling interval (time)",,"s","0","0","10","s","0","4","Operational"
1360.00,"25","Processing information","025171","Sample averaging period",,"s","0","0","10","s","0","4","Operational"
1361.00,"25","Processing information","025172","Number of samples",,"Numeric","0","0","10","Numeric","0","4","Operational"
1362.00,"25","Processing information","025174","SMOS information flag",,"Flag table","0","0","14","Flag table","0","5","Operational"
1363.00,"25","Processing information","025175","Modified residual","(see Note 7)","Numeric","2","0","13","Numeric","2","4","Operational"
1364.00,"25","Processing information","025180","LRM mode per cent",,"%","2","0","16","%","2","5","Operational"
1365.00,"25","Processing information","025181","L2 processing flag",,"Code table","0","0","2","Code table","0","1","Operational"
1366.00,"25","Processing information","025182","L1 processing flag",,"Code table","0","0","2","Code table","0","1","Operational"
1367.00,"25","Processing information","025183","L1 processing quality",,"%","2","0","14","%","2","5","Operational"
1368.00,"25","Processing information","025184","L2 product status",,"Code table","0","0","2","Code table","0","1","Operational"
1369.00,"26","Non-coordinate location (time)","026001","Principal time of daily reading in UTC of maximum temperature",,"h","1","0","12","h","1","3","Operational"
1370.00,"26","Non-coordinate location (time)","026002","Principal time of daily reading in UTC of minimum temperature",,"h","1","0","12","h","1","3","Operational"
1371.00,"26","Non-coordinate location (time)","026003","Time difference",,"min","0","-1440","12","min","0","4","Operational"
1372.00,"26","Non-coordinate location (time)","026010","Hours included",,"Flag table","0","0","26","Flag table","0","9","Operational"
1373.00,"26","Non-coordinate location (time)","026020","Duration of precipitation",,"min","0","0","11","min","0","4","Operational"
1374.00,"26","Non-coordinate location (time)","026021","Year",,"a","0","0","12","a","0","4","Operational"
1375.00,"26","Non-coordinate location (time)","026022","Month",,"mon","0","0","4","mon","0","2","Operational"
1376.00,"26","Non-coordinate location (time)","026023","Day",,"d","0","0","6","d","0","2","Operational"
1377.00,"26","Non-coordinate location (time)","026030","Measurement integration time",,"s","2","0","8","s","2","3","Operational"
1378.00,"27","Non-coordinate location (horizontal - 1)","027001","Latitude (high accuracy)",,"deg","5","-9000000","25","deg","5","7","Operational"
1379.00,"27","Non-coordinate location (horizontal - 1)","027002","Latitude (coarse accuracy)",,"deg","2","-9000","15","deg","2","4","Operational"
1380.00,"27","Non-coordinate location (horizontal - 1)","027003","Alternate latitude (coarse accuracy)",,"deg","2","-9000","15","deg","2","4","Operational"
1381.00,"27","Non-coordinate location (horizontal - 1)","027004","Alternate latitude (high accuracy)",,"deg","5","-9000000","25","deg","5","7","Operational"
1382.00,"27","Non-coordinate location (horizontal - 1)","027010","Footprint axis 1",,"m","-1","0","14","m","-1","5","Operational"
1383.00,"27","Non-coordinate location (horizontal - 1)","027020","Satellite location counter",,"Numeric","0","0","16","Numeric","0","5","Operational"
1384.00,"27","Non-coordinate location (horizontal - 1)","027021","Satellite sublocation dimension",,"Numeric","0","0","16","Numeric","0","5","Operational"
1385.00,"27","Non-coordinate location (horizontal - 1)","027031","In direction of 0 degrees longitude, distance from the Earth's centre",,"m","2","-1073741824","31","m","2","10","Operational"
1386.00,"27","Non-coordinate location (horizontal - 1)","027080","Viewing azimuth angle",,"degree true","2","0","16","degree true","0","5","Operational"
1387.00,"28","Non-coordinate location (horizontal - 2)","028001","Longitude (high accuracy)",,"deg","5","-18000000","26","deg","5","8","Operational"
1388.00,"28","Non-coordinate location (horizontal - 2)","028002","Longitude (coarse accuracy)",,"deg","2","-18000","16","deg","2","5","Operational"
1389.00,"28","Non-coordinate location (horizontal - 2)","028003","Alternate longitude (coarse accuracy)",,"deg","2","-18000","16","deg","2","5","Operational"
1390.00,"28","Non-coordinate location (horizontal - 2)","028004","Alternate longitude (high accuracy)",,"deg","5","-18000000","26","deg","5","8","Operational"
1391.00,"28","Non-coordinate location (horizontal - 2)","028010","Footprint axis 2",,"m","-1","0","14","m","-1","5","Operational"
1392.00,"28","Non-coordinate location (horizontal - 2)","028031","In direction 90 degrees East, distance from the Earth's centre",,"m","2","-1073741824","31","m","2","10","Operational"
1393.00,"29","Map data","029001","Projection type",,"Code table","0","0","3","Code table","0","1","Operational"
1394.00,"29","Map data","029002","Coordinate grid type",,"Code table","0","0","3","Code table","0","1","Operational"
1395.00,"30","Image","030001","Pixel value (4 bits)",,"Numeric","0","0","4","Numeric","0","2","Operational"
1396.00,"30","Image","030002","Pixel value (8 bits)",,"Numeric","0","0","8","Numeric","0","3","Operational"
1397.00,"30","Image","030004","Pixel value (16 bits)",,"Numeric","0","0","16","Numeric","0","5","Operational"
1398.00,"30","Image","030010","Number of grid points",,"Numeric","0","0","13","Numeric","0","4","Operational"
1399.00,"30","Image","030021","Number of pixels per row",,"Numeric","0","0","12","Numeric","0","4","Operational"
1400.00,"30","Image","030022","Number of pixels per column",,"Numeric","0","0","12","Numeric","0","4","Operational"
1401.00,"30","Image","030031","Picture type",,"Code table","0","0","4","Code table","0","2","Operational"
1402.00,"30","Image","030032","Combination with other data",,"Flag table","0","0","16","Flag table","0","6","Operational"
1403.00,"30","Image","030033","Number of bins along the radial",,"Numeric","0","0","12","Numeric","0","4","Operational"
1404.00,"30","Image","030034","Number of azimuths",,"Numeric","0","0","12","Numeric","0","4","Operational"
1405.00,"31","Data description operator qualifiers","031000","Short delayed descriptor replication factor",,"Numeric","0","0","1",,,,"Operational"
1406.00,"31","Data description operator qualifiers","031001","Delayed descriptor replication factor",,"Numeric","0","0","8",,,,"Operational"
1407.00,"31","Data description operator qualifiers","031002","Extended delayed descriptor replication factor",,"Numeric","0","0","16",,,,"Operational"
1408.00,"31","Data description operator qualifiers","031011","Delayed descriptor and data repetition factor",,"Numeric","0","0","8",,,,"Operational"
1409.00,"31","Data description operator qualifiers","031012","Extended delayed descriptor and data repetition factor",,"Numeric","0","0","16",,,,"Operational"
1410.00,"31","Data description operator qualifiers","031021","Associated field significance",,"Code table","0","0","6",,,,"Operational"
1411.00,"31","Data description operator qualifiers","031031","Data present indicator",,"Flag table","0","0","1",,,,"Operational"
1412.00,"33","Quality information","033002","Quality information",,"Code table","0","0","2","Code table","0","1","Operational"
1413.00,"33","Quality information","033003","Quality information",,"Code table","0","0","3","Code table","0","1","Operational"
1414.00,"33","Quality information","033005","Quality information (AWS data)",,"Flag table","0","0","30","Flag table","0","10","Operational"
1415.00,"33","Quality information","033006","Internal measurement status information (AWS)",,"Code table","0","0","3","Code table","0","1","Operational"
1416.00,"33","Quality information","033007","Per cent confidence",,"%","0","0","7","%","0","3","Operational"
1418.00,"33","Quality information","033015","Data quality check indicator",,"Code table","0","0","6","Code table","0","2","Operational"
1419.00,"33","Quality information","033020","Quality control indication of following value",,"Code table","0","0","3","Code table","0","1","Operational"
1420.00,"33","Quality information","033021","Quality of following value",,"Code table","0","0","2","Code table","0","1","Operational"
1421.00,"33","Quality information","033022","Quality of buoy satellite transmission",,"Code table","0","0","2","Code table","0","1","Operational"
1422.00,"33","Quality information","033023","Quality of buoy location",,"Code table","0","0","2","Code table","0","1","Operational"
1423.00,"33","Quality information","033024","Station elevation quality mark (for mobile stations)",,"Code table","0","0","4","Code table","0","2","Operational"
1424.00,"33","Quality information","033025","ACARS interpolated values indicator",,"Code table","0","0","3","Code table","0","1","Operational"
1425.00,"33","Quality information","033026","Moisture quality",,"Code table","0","0","6","Code table","0","2","Operational"
1426.00,"33","Quality information","033027","Location quality class (range of radius of 66 % confidence)",,"Code table","0","0","3","Code table","0","1","Operational"
1427.00,"33","Quality information","033028","Snapshot overall quality",,"Code table","0","0","3","Code table","0","1","Operational"
1428.00,"33","Quality information","033030","Scan line status flags for ATOVS",,"Flag table","0","0","24","Flag table","0","8","Operational"
1429.00,"33","Quality information","033031","Scan line quality flags for ATOVS",,"Flag table","0","0","24","Flag table","0","8","Operational"
1430.00,"33","Quality information","033032","Channel quality flags for ATOVS",,"Flag table","0","0","24","Flag table","0","8","Operational"
1431.00,"33","Quality information","033033","Field of view quality flags for ATOVS",,"Flag table","0","0","24","Flag table","0","8","Operational"
1432.00,"33","Quality information","033035","Manual/automatic quality control",,"Code table","0","0","4","Code table","0","2","Operational"
1433.00,"33","Quality information","033036","Nominal confidence threshold",,"%","0","0","7","%","0","3","Operational"
1434.00,"33","Quality information","033037","Wind correlation error",,"Flag table","0","0","20","Flag table","0","7","Operational"
1435.00,"33","Quality information","033038","Quality flags for ground-based GNSS data",,"Flag table","0","0","10","Flag table","0","4","Operational"
1436.00,"33","Quality information","033039","Quality flags for radio occultation data",,"Flag table","0","0","16","Flag table","0","6","Operational"
1437.00,"33","Quality information","033040","Confidence interval",,"%","0","0","7","%","0","3","Operational"
1438.00,"33","Quality information","033041","Attribute of following value",,"Code table","0","0","2","Code table","0","1","Operational"
1439.00,"33","Quality information","033042","Type of limit represented by following value",,"Code table","0","0","3","Code table","0","1","Operational"
1440.00,"33","Quality information","033043","AST confidence",,"Flag table","0","0","8","Flag table","0","3","Operational"
1441.00,"33","Quality information","033044","ASAR quality information",,"Flag table","0","0","15","Flag table","0","5","Operational"
1442.00,"33","Quality information","033045","Probability of following event","(see Notes 1 and 3)","%","0","0","7","%","0","3","Operational"
1443.00,"33","Quality information","033046","Conditional probability of following event with respect to specified conditioning event","(see Notes 1, 2 and 3)","%","0","0","7","%","0","3","Operational"
1444.00,"33","Quality information","033047","Measurement confidence data",,"Flag table","0","0","31","Flag table","0","11","Operational"
1445.00,"33","Quality information","033048","Confidence measure of SAR inversion",,"Code table","0","0","2","Code table","0","1","Operational"
1446.00,"33","Quality information","033049","Confidence measure of wind retrieval",,"Code table","0","0","2","Code table","0","1","Operational"
1447.00,"33","Quality information","033050","Global GTSPP quality flag",,"Code table","0","0","4","Code table","0","2","Operational"
1448.00,"33","Quality information","033052","S-band ocean retracking quality",,"Flag table","0","0","21","Flag table","0","7","Operational"
1449.00,"33","Quality information","033053","Ku band ocean retracking quality",,"Flag table","0","0","21","Flag table","0","7","Operational"
1450.00,"33","Quality information","033060","GqisFlagQual - individual IASI-System quality flag",,"Code table","0","0","2","Code table","0","1","Operational"
1451.00,"33","Quality information","033061","GqisQualIndex - indicator for instrument noise performance (contributions from spectral and radiometric calibration)",,"%","0","0","7","%","0","3","Operational"
1452.00,"33","Quality information","033062","GqisQualIndexLoc - indicator for geometric quality index",,"%","0","0","7","%","0","3","Operational"
1453.00,"33","Quality information","033063","GqisQualIndexRad - indicator for instrument noise performance (contributions from radiometric calibration)",,"%","0","0","7","%","0","3","Operational"
1454.00,"33","Quality information","033064","GqisQualIndexSpect - indicator for instrument noise performance (contributions from spectral calibration)",,"%","0","0","7","%","0","3","Operational"
1455.00,"33","Quality information","033065","GqisSysTecSondQual - output of system TEC (Technical Expertise Centre) quality function",,"Numeric","0","0","24","Numeric","0","8","Operational"
1456.00,"33","Quality information","033070","Total ozone quality",,"Code table","0","0","4","Code table","0","2","Operational"
1457.00,"33","Quality information","033071","Profile ozone quality",,"Code table","0","0","4","Code table","0","2","Operational"
1458.00,"33","Quality information","033072","Ozone error",,"Code table","0","0","5","Code table","0","2","Operational"
1459.00,"33","Quality information","033075","Scan-level quality flags",,"Flag table","0","0","13","Flag table","0","5","Operational"
1460.00,"33","Quality information","033076","Calibration quality flags",,"Flag table","0","0","9","Flag table","0","3","Operational"
1461.00,"33","Quality information","033077","Field-of-view quality flags",,"Flag table","0","0","19","Flag table","0","7","Operational"
1462.00,"33","Quality information","033078","Geolocation quality",,"Code table","0","0","4","Code table","0","2","Operational"
1463.00,"33","Quality information","033079","Granule level quality flags",,"Flag table","0","0","16","Flag table","0","6","Operational"
1464.00,"33","Quality information","033080","Scan level quality flags",,"Flag table","0","0","20","Flag table","0","7","Operational"
1465.00,"33","Quality information","033081","Channel data quality flags",,"Flag table","0","0","12","Flag table","0","4","Operational"
1466.00,"33","Quality information","033082","Geolocation quality flags",,"Flag table","0","0","16","Flag table","0","6","Operational"
1467.00,"33","Quality information","033083","Radiance data quality flags",,"Flag table","0","0","16","Flag table","0","6","Operational"
1468.00,"33","Quality information","033084","Pixel level quality flags",,"Flag table","0","0","16","Flag table","0","6","Operational"
1470.00,"33","Quality information","033086","Quality of pixel level retrieval",,"Code table","0","0","3","Code table","0","1","Operational"
1472.00,"35","Data monitoring information","035000","FM and Regional Code number",,"Code table","0","0","10","Code table","0","3","Operational"
1473.00,"35","Data monitoring information","035001","Time frame for monitoring",,"Code table","0","0","3","Code table","0","1","Operational"
1474.00,"35","Data monitoring information","035011","Number of reports actually received",,"Numeric","0","0","14","Numeric","0","4","Operational"
1475.00,"35","Data monitoring information","035021","Bulletin being monitored (TTAAii)",,"CCITT IA5","0","0","48","Character","0","6","Operational"
1476.00,"35","Data monitoring information","035022","Bulletin being monitored (YYGGgg)",,"CCITT IA5","0","0","48","Character","0","6","Operational"
1477.00,"35","Data monitoring information","035023","Bulletin being monitored (CCCC)",,"CCITT IA5","0","0","32","Character","0","4","Operational"
1478.00,"35","Data monitoring information","035024","Bulletin being monitored (BBB)",,"CCITT IA5","0","0","24","Character","0","3","Operational"
1479.00,"35","Data monitoring information","035030","Discrepancies in the availability of expected data",,"Code table","0","0","4","Code table","0","1","Operational"
1480.00,"35","Data monitoring information","035031","Qualifier on monitoring results",,"Code table","0","0","7","Code table","0","2","Operational"
1481.00,"35","Data monitoring information","035032","Cause of missing data",,"Code table","0","0","4","Code table","0","1","Operational"
1482.00,"35","Data monitoring information","035033","Observation and collection deficiencies",,"Code table","0","0","7","Code table","0","2","Operational"
1483.00,"35","Data monitoring information","035034","Statistical trends for availability of data (during the survey period(s))",,"Code table","0","0","3","Code table","0","1","Operational"
1484.00,"35","Data monitoring information","035035","Reason for termination",,"Code table","0","0","5","Code table","0","2","Operational"
1485.00,"40","Satellite data","040001","Surface soil moisture (ms)",,"%","1","0","10","%","1","4","Operational"
1486.00,"40","Satellite data","040002","Estimated error in surface soil moisture",,"%","1","0","10","%","1","4","Operational"
1487.00,"40","Satellite data","040003","Mean surface soil moisture",,"Numeric","3","0","10","Numeric","3","4","Operational"
1488.00,"40","Satellite data","040004","Rain fall detection",,"Numeric","3","0","10","Numeric","3","4","Operational"
1489.00,"40","Satellite data","040005","Soil moisture correction flag",,"Flag table","0","0","8","Flag table","0","3","Operational"
1490.00,"40","Satellite data","040006","Soil moisture processing flag",,"Flag table","0","0","16","Flag table","0","6","Operational"
1491.00,"40","Satellite data","040007","Soil moisture quality",,"%","1","0","10","%","1","4","Operational"
1492.00,"40","Satellite data","040008","Frozen land surface fraction",,"%","1","0","10","%","1","4","Operational"
1493.00,"40","Satellite data","040009","Inundation and wetland fraction",,"%","1","0","10","%","1","4","Operational"
1494.00,"40","Satellite data","040010","Topographic complexity",,"%","1","0","10","%","1","4","Operational"
1495.00,"40","Satellite data","040011","Interpolation flag",,"Flag table","0","0","8","Flag table","0","3","Operational"
1496.00,"40","Satellite data","040012","Radiometer data quality flag",,"Flag table","0","0","8","Flag table","0","3","Operational"
1497.00,"40","Satellite data","040013","Radiometer brightness temperature interpretation flag",,"Code table","0","0","3","Code table","0","1","Operational"
1498.00,"40","Satellite data","040014","High-frequency fluctuations of the sea-surface topography correction",,"m","4","-3000","13","m","4","4","Operational"
1499.00,"40","Satellite data","040015","Normalized differential vegetation index (NDVI)",,"Numeric","2","-100","8","Numeric","2","3","Operational"
1500.00,"40","Satellite data","040016","Residual RMS in band",,"Numeric","3","0","14","Numeric","3","5","Operational"
1501.00,"40","Satellite data","040017","Non-normalized principal component score",,"Numeric","0","-1073741824","31","Numeric","0","10","Operational"
1502.00,"40","Satellite data","040018","GIacAvgImagIIS - average of imager measurements",,"W m-2 sr-1 m","6","0","24","W m-2 sr-1 m","6","8","Operational"
1503.00,"40","Satellite data","040019","GIacVarImagIIS - variance of imager measurements",,"W m-2 sr-1 m","6","0","24","W m-2 sr-1 m","6","8","Operational"
1504.00,"40","Satellite data","040020","GqisFlagQualDetailed - quality flag for the system",,"Flag table","0","0","17","Flag table","0","6","Operational"
1505.00,"40","Satellite data","040021","Fraction of weighted AVHRR pixel in IASI FOV covered with snow/ice",,"%","0","0","7","%","0","3","Operational"
1506.00,"40","Satellite data","040022","Number of missing, bad or failed AVHRR pixels",,"Numeric","0","0","7","Numeric","0","3","Operational"
1507.00,"40","Satellite data","040023","Auxiliary altimeter state flags",,"Flag table","0","0","5","Flag table","0","2","Operational"
1508.00,"40","Satellite data","040024","Meteorological map availability",,"Code table","0","0","3","Code table","0","1","Operational"
1509.00,"40","Satellite data","040025","Interpolation flag for mean diurnal tide",,"Code table","0","0","2","Code table","0","1","Operational"
1510.00,"40","Satellite data","040026","Score quantization factor",,"Numeric","2","0","16","Numeric","2","5","Operational"
