"No","Category","CategoryOfSequences_en","FXY1","Title_en","SubTitle_en","FXY2","ElementName_en","ExistingElementName_en","Note_en","Status"
1.00,"00","BUFR table entries sequences","300002",,,"000002","Table A: data category description, line 1","Table A category, line 1",,"Operational"
2.00,"00","BUFR table entries sequences","300002",,,"000003","Table A: data category description, line 2","Table A category, line 2",,"Operational"
3.00,"00","BUFR table entries sequences","300003",,,"000010","F descriptor to be added or defined","F, part descriptor",,"Operational"
4.00,"00","BUFR table entries sequences","300003",,,"000011","X descriptor to be added or defined","X, part descriptor",,"Operational"
5.00,"00","BUFR table entries sequences","300003",,,"000012","Y descriptor to be added or defined","Y, part descriptor",,"Operational"
6.00,"00","BUFR table entries sequences","300004",,,"300003",,,,"Operational"
7.00,"00","BUFR table entries sequences","300004",,,"000013","Element name, line 1","Element name, line 1",,"Operational"
8.00,"00","BUFR table entries sequences","300004",,,"000014","Element name, line 2","Element name, line 2",,"Operational"
9.00,"00","BUFR table entries sequences","300004",,,"000015","Units name","Units name",,"Operational"
10.00,"00","BUFR table entries sequences","300004",,,"000016","Units scale sign","Units scale sign",,"Operational"
11.00,"00","BUFR table entries sequences","300004",,,"000017","Units scale","Units scale",,"Operational"
12.00,"00","BUFR table entries sequences","300004",,,"000018","Units reference sign","Units reference sign",,"Operational"
13.00,"00","BUFR table entries sequences","300004",,,"000019","Units reference value","Units reference value",,"Operational"
14.00,"00","BUFR table entries sequences","300004",,,"000020","Element data width","Element data width",,"Operational"
15.00,"00","BUFR table entries sequences","300010",,,"300003",,"Table D descriptor to be defined",,"Operational"
16.00,"00","BUFR table entries sequences","300010",,,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
17.00,"00","BUFR table entries sequences","300010",,,"031001","Delayed descriptor replication factor","Delayed descriptor replication factor",,"Operational"
18.00,"00","BUFR table entries sequences","300010",,,"000030","Descriptor defining sequence","Descriptor defining sequence",,"Operational"
19.00,"00","BUFR table entries sequences","300015","(Code table definition)",,"000030","Descriptor defining sequence","Descriptor defining sequence (FXY)",,"Operational"
20.00,"00","BUFR table entries sequences","300015","(Code table definition)",,"102000","Replication descriptor","Delayed replication of 2 descriptors",,"Operational"
21.00,"00","BUFR table entries sequences","300015","(Code table definition)",,"031002","Extended delayed descriptor replication factor","Extended delayed descriptor replication factor",,"Operational"
22.00,"00","BUFR table entries sequences","300015","(Code table definition)",,"000024","Code figure","Code figure",,"Operational"
23.00,"00","BUFR table entries sequences","300015","(Code table definition)",,"000025","Code figure meaning","Code figure meaning",,"Operational"
24.00,"00","BUFR table entries sequences","300016","(Flag table definition)",,"000030","Descriptor defining sequence","Descriptor defining sequence (FXY)",,"Operational"
25.00,"00","BUFR table entries sequences","300016","(Flag table definition)",,"102000","Replication descriptor","Delayed replication of 2 descriptors",,"Operational"
26.00,"00","BUFR table entries sequences","300016","(Flag table definition)",,"031001","Delayed descriptor replication factor","Delayed descriptor replication factor",,"Operational"
27.00,"00","BUFR table entries sequences","300016","(Flag table definition)",,"000026","Bit number","Bit number",,"Operational"
28.00,"00","BUFR table entries sequences","300016","(Flag table definition)",,"000027","Bit number meaning","Bit number meaning",,"Operational"
29.00,"01","Location and identification sequences","301001",,,"001001","WMO block number","WMO block number",,"Operational"
30.00,"01","Location and identification sequences","301001",,,"001002","WMO station number","WMO station number",,"Operational"
31.00,"01","Location and identification sequences","301002",,,"001003","WMO Region number/geographical area","WMO Region number",,"Operational"
32.00,"01","Location and identification sequences","301002",,,"001004","WMO Region sub-area","WMO Region sub-area",,"Operational"
33.00,"01","Location and identification sequences","301002",,,"001005","Buoy/platform identifier","Buoy/platform identifier",,"Operational"
34.00,"01","Location and identification sequences","301003",,,"001011","Ship or mobile land station identifier","Ship's call sign",,"Operational"
35.00,"01","Location and identification sequences","301003",,,"001012","Direction of motion of moving observing platform","Direction of motion of moving observing platform",,"Operational"
36.00,"01","Location and identification sequences","301003",,,"001013","Speed of motion of moving observing platform","Speed of motion of moving observing platform",,"Operational"
37.00,"01","Location and identification sequences","301004","(Surface station identification)",,"001001","WMO block number","WMO block number",,"Operational"
38.00,"01","Location and identification sequences","301004","(Surface station identification)",,"001002","WMO station number","WMO station number",,"Operational"
39.00,"01","Location and identification sequences","301004","(Surface station identification)",,"001015","Station or site name","Station or site name",,"Operational"
40.00,"01","Location and identification sequences","301004","(Surface station identification)",,"002001","Type of station","Type of station",,"Operational"
41.00,"01","Location and identification sequences","301005","(Origin and identification sequence)",,"001035","Originating Centre","Originating centre",,"Operational"
42.00,"01","Location and identification sequences","301005","(Origin and identification sequence)",,"001034","Identification of originating/generating sub-centre","Identification of originating/generating sub-centre",,"Operational"
43.00,"01","Location and identification sequences","301011",,,"004001","Year","Year",,"Operational"
44.00,"01","Location and identification sequences","301011",,,"004002","Month","Month",,"Operational"
45.00,"01","Location and identification sequences","301011",,,"004003","Day","Day",,"Operational"
46.00,"01","Location and identification sequences","301012",,,"004004","Hour","Hour",,"Operational"
47.00,"01","Location and identification sequences","301012",,,"004005","Minute","Minute",,"Operational"
48.00,"01","Location and identification sequences","301013",,,"004004","Hour","Hour",,"Operational"
49.00,"01","Location and identification sequences","301013",,,"004005","Minute","Minute",,"Operational"
50.00,"01","Location and identification sequences","301013",,,"004006","Second","Second",,"Operational"
51.00,"01","Location and identification sequences","301014","(Time period)",,"102002","Replication descriptor","Replication of 2 descriptors 2 times",,"Operational"
52.00,"01","Location and identification sequences","301014","(Time period)",,"301011",,"Year, month, day",,"Operational"
53.00,"01","Location and identification sequences","301014","(Time period)",,"301012",,"Hour, minute",,"Operational"
54.00,"01","Location and identification sequences","301021",,,"005001","Latitude (high accuracy)","Latitude (high accuracy)",,"Operational"
55.00,"01","Location and identification sequences","301021",,,"006001","Longitude (high accuracy)","Longitude (high accuracy)",,"Operational"
56.00,"01","Location and identification sequences","301022",,,"005001","Latitude (high accuracy)","Latitude (high accuracy)",,"Operational"
57.00,"01","Location and identification sequences","301022",,,"006001","Longitude (high accuracy)","Longitude (high accuracy)",,"Operational"
58.00,"01","Location and identification sequences","301022",,,"007001","Height of station","Height of station",,"Operational"
59.00,"01","Location and identification sequences","301023",,,"005002","Latitude (coarse accuracy)","Latitude (coarse accuracy)",,"Operational"
60.00,"01","Location and identification sequences","301023",,,"006002","Longitude (coarse accuracy)","Longitude (coarse accuracy)",,"Operational"
61.00,"01","Location and identification sequences","301024",,,"005002","Latitude (coarse accuracy)","Latitude (coarse accuracy)",,"Operational"
62.00,"01","Location and identification sequences","301024",,,"006002","Longitude (coarse accuracy)","Longitude (coarse accuracy)",,"Operational"
63.00,"01","Location and identification sequences","301024",,,"007001","Height of station","Height of station",,"Operational"
64.00,"01","Location and identification sequences","301025",,,"301023",,"Latitude and longitude (coarse accuracy)",,"Operational"
65.00,"01","Location and identification sequences","301025",,,"004003","Day","Day",,"Operational"
66.00,"01","Location and identification sequences","301025",,,"301012",,"Time",,"Operational"
67.00,"01","Location and identification sequences","301026",,,"301021",,"Latitude and longitude (high accuracy)",,"Operational"
68.00,"01","Location and identification sequences","301026",,,"004003","Day","(Time period in days)",,"Operational"
69.00,"01","Location and identification sequences","301026",,,"004003","Day","(Time period in days)",,"Operational"
70.00,"01","Location and identification sequences","301026",,,"004004","Hour","(Time period in hours)",,"Operational"
71.00,"01","Location and identification sequences","301026",,,"004004","Hour","(Time period in hours)",,"Operational"
72.00,"01","Location and identification sequences","301026",,,"004005","Minute","(Time period in minutes)",,"Operational"
73.00,"01","Location and identification sequences","301026",,,"004005","Minute","(Time period in minutes)",,"Operational"
74.00,"01","Location and identification sequences","301027","(Description of a feature in 3-D or 2-D)",,"008007","Dimensional significance","Dimensional significance (0 = Point, 1 = Line, 2 = Area, 3 = Volume)",,"Operational"
75.00,"01","Location and identification sequences","301027","(Description of a feature in 3-D or 2-D)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
76.00,"01","Location and identification sequences","301027","(Description of a feature in 3-D or 2-D)",,"031001","Delayed descriptor replication factor","Replication factor (see Note 5)",,"Operational"
77.00,"01","Location and identification sequences","301027","(Description of a feature in 3-D or 2-D)",,"301028","Horizontal section of a feature described as a polygon, circle, line or point","Description of horizontal section",,"Operational"
78.00,"01","Location and identification sequences","301027","(Description of a feature in 3-D or 2-D)",,"008007","Dimensional significance","Dimensional significance, Missing = Cancel",,"Operational"
79.00,"01","Location and identification sequences","301028","(Horizontal section of a feature described as a polygon, circle, line or point)",,"008040","Flight Level significance","Flight level significance",,"Operational"
80.00,"01","Location and identification sequences","301028","(Horizontal section of a feature described as a polygon, circle, line or point)",,"033042","Type of limit represented by following value","Type of limit represented by following (flight level) value",,"Operational"
81.00,"01","Location and identification sequences","301028","(Horizontal section of a feature described as a polygon, circle, line or point)",,"007010","Flight level","Flight level",,"Operational"
82.00,"01","Location and identification sequences","301028","(Horizontal section of a feature described as a polygon, circle, line or point)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
83.00,"01","Location and identification sequences","301028","(Horizontal section of a feature described as a polygon, circle, line or point)",,"031002","Extended delayed descriptor replication factor","Extended replication factor","(see Note 6)","Operational"
84.00,"01","Location and identification sequences","301028","(Horizontal section of a feature described as a polygon, circle, line or point)",,"301023",,"Location",,"Operational"
85.00,"01","Location and identification sequences","301028","(Horizontal section of a feature described as a polygon, circle, line or point)",,"019007","Effective radius of feature","Radius of feature","(see Note 7)","Operational"
86.00,"01","Location and identification sequences","301028","(Horizontal section of a feature described as a polygon, circle, line or point)",,"008040","Flight Level significance","Flight level significance, Missing = Cancel",,"Operational"
87.00,"01","Location and identification sequences","301031",,,"301001",,"WMO block and station number",,"Operational"
88.00,"01","Location and identification sequences","301031",,,"002001","Type of station","Type of station",,"Operational"
89.00,"01","Location and identification sequences","301031",,,"301011",,"Date",,"Operational"
90.00,"01","Location and identification sequences","301031",,,"301012",,"Time",,"Operational"
91.00,"01","Location and identification sequences","301031",,,"301022",,"Latitude and longitude (high accuracy), height of station",,"Operational"
92.00,"01","Location and identification sequences","301032",,,"301001",,"WMO block and station number",,"Operational"
93.00,"01","Location and identification sequences","301032",,,"002001","Type of station","Type of station",,"Operational"
94.00,"01","Location and identification sequences","301032",,,"301011",,"Date",,"Operational"
95.00,"01","Location and identification sequences","301032",,,"301012",,"Time",,"Operational"
96.00,"01","Location and identification sequences","301032",,,"301024",,"Latitude and longitude (coarse accuracy), height of station",,"Operational"
97.00,"01","Location and identification sequences","301033","(Buoy/platform - fixed)",,"001005","Buoy/platform identifier","Buoy/platform identifier",,"Operational"
98.00,"01","Location and identification sequences","301033","(Buoy/platform - fixed)",,"002001","Type of station","Type of station",,"Operational"
99.00,"01","Location and identification sequences","301033","(Buoy/platform - fixed)",,"301011",,"Date",,"Operational"
100.00,"01","Location and identification sequences","301033","(Buoy/platform - fixed)",,"301012",,"Time",,"Operational"
101.00,"01","Location and identification sequences","301033","(Buoy/platform - fixed)",,"301021",,"Latitude and longitude (high accuracy)",,"Operational"
102.00,"01","Location and identification sequences","301034","(Buoy/platform - fixed)",,"001005","Buoy/platform identifier","Buoy/platform identifier",,"Operational"
103.00,"01","Location and identification sequences","301034","(Buoy/platform - fixed)",,"002001","Type of station","Type of station",,"Operational"
104.00,"01","Location and identification sequences","301034","(Buoy/platform - fixed)",,"301011",,"Date",,"Operational"
105.00,"01","Location and identification sequences","301034","(Buoy/platform - fixed)",,"301012",,"Time",,"Operational"
106.00,"01","Location and identification sequences","301034","(Buoy/platform - fixed)",,"301023",,"Latitude and longitude (coarse accuracy)",,"Operational"
107.00,"01","Location and identification sequences","301035","(Buoy/platform - moving)",,"001005","Buoy/platform identifier","Buoy/platform identifier","(see Note 4)","Operational"
108.00,"01","Location and identification sequences","301035","(Buoy/platform - moving)",,"001012","Direction of motion of moving observing platform","Direction of motion of moving observing platform",,"Operational"
109.00,"01","Location and identification sequences","301035","(Buoy/platform - moving)",,"001013","Speed of motion of moving observing platform","Speed of motion of moving observing platform",,"Operational"
110.00,"01","Location and identification sequences","301035","(Buoy/platform - moving)",,"002001","Type of station","Type of station",,"Operational"
111.00,"01","Location and identification sequences","301035","(Buoy/platform - moving)",,"301011",,"Date",,"Operational"
112.00,"01","Location and identification sequences","301035","(Buoy/platform - moving)",,"301012",,"Time",,"Operational"
113.00,"01","Location and identification sequences","301035","(Buoy/platform - moving)",,"301023",,"Latitude and longitude (coarse accuracy)",,"Operational"
114.00,"01","Location and identification sequences","301036","(Ship)",,"301003",,"Ship's call sign and motion",,"Operational"
115.00,"01","Location and identification sequences","301036","(Ship)",,"002001","Type of station","Type of station",,"Operational"
116.00,"01","Location and identification sequences","301036","(Ship)",,"301011",,"Date",,"Operational"
117.00,"01","Location and identification sequences","301036","(Ship)",,"301012",,"Time",,"Operational"
118.00,"01","Location and identification sequences","301036","(Ship)",,"301023",,"Latitude and longitude (coarse accuracy)",,"Operational"
119.00,"01","Location and identification sequences","301037","(Land station for vertical soundings)",,"301001",,"WMO block and station number",,"Operational"
120.00,"01","Location and identification sequences","301037","(Land station for vertical soundings)",,"002011","Radiosonde type","Radiosonde type",,"Operational"
121.00,"01","Location and identification sequences","301037","(Land station for vertical soundings)",,"002012","Radiosonde computational method","Radiosonde computational method",,"Operational"
122.00,"01","Location and identification sequences","301037","(Land station for vertical soundings)",,"301011",,"Date",,"Operational"
123.00,"01","Location and identification sequences","301037","(Land station for vertical soundings)",,"301012",,"Time",,"Operational"
124.00,"01","Location and identification sequences","301037","(Land station for vertical soundings)",,"301022",,"Latitude and longitude (high accuracy), height of station",,"Operational"
125.00,"01","Location and identification sequences","301038","(Land station for vertical soundings)",,"301001",,"WMO block and station number",,"Operational"
126.00,"01","Location and identification sequences","301038","(Land station for vertical soundings)",,"002011","Radiosonde type","Radiosonde type",,"Operational"
127.00,"01","Location and identification sequences","301038","(Land station for vertical soundings)",,"002012","Radiosonde computational method","Radiosonde computational method",,"Operational"
128.00,"01","Location and identification sequences","301038","(Land station for vertical soundings)",,"301011",,"Date",,"Operational"
129.00,"01","Location and identification sequences","301038","(Land station for vertical soundings)",,"301012",,"Time",,"Operational"
130.00,"01","Location and identification sequences","301038","(Land station for vertical soundings)",,"301024",,"Latitude and longitude (coarse accuracy), height of station",,"Operational"
131.00,"01","Location and identification sequences","301039","(Ship for vertical soundings)",,"301003",,"Ship's call sign and motion",,"Operational"
132.00,"01","Location and identification sequences","301039","(Ship for vertical soundings)",,"002011","Radiosonde type","Radiosonde type",,"Operational"
133.00,"01","Location and identification sequences","301039","(Ship for vertical soundings)",,"002012","Radiosonde computational method","Radiosonde computational method",,"Operational"
134.00,"01","Location and identification sequences","301039","(Ship for vertical soundings)",,"301011",,"Date",,"Operational"
135.00,"01","Location and identification sequences","301039","(Ship for vertical soundings)",,"301012",,"Time",,"Operational"
136.00,"01","Location and identification sequences","301039","(Ship for vertical soundings)",,"301023",,"Latitude and longitude (coarse accuracy)",,"Operational"
137.00,"01","Location and identification sequences","301040",,,"301003",,"Ship's call sign and motion",,"Operational"
138.00,"01","Location and identification sequences","301040",,,"002011","Radiosonde type","Radiosonde type",,"Operational"
139.00,"01","Location and identification sequences","301040",,,"002012","Radiosonde computational method","Radiosonde computational method",,"Operational"
140.00,"01","Location and identification sequences","301040",,,"301011",,"Date",,"Operational"
141.00,"01","Location and identification sequences","301040",,,"301012",,"Time",,"Operational"
142.00,"01","Location and identification sequences","301040",,,"301024",,"Latitude and longitude (coarse accuracy), height of station",,"Operational"
143.00,"01","Location and identification sequences","301041",,,"001007","Satellite identifier","Satellite identifier",,"Operational"
144.00,"01","Location and identification sequences","301041",,,"002021","Satellite instrument data used in processing","Satellite instrument data used in processing",,"Operational"
145.00,"01","Location and identification sequences","301041",,,"002022","Satellite data-processing technique used","Satellite data-processing technique used",,"Operational"
146.00,"01","Location and identification sequences","301041",,,"301011",,"Date",,"Operational"
147.00,"01","Location and identification sequences","301041",,,"301012",,"Time",,"Operational"
148.00,"01","Location and identification sequences","301042",,,"301041",,"Satellite identifier, data used, and data processing technique; date/time",,"Operational"
149.00,"01","Location and identification sequences","301042",,,"301021",,"Latitude, longitude",,"Operational"
150.00,"01","Location and identification sequences","301043",,,"001007","Satellite identifier","Satellite identifier",,"Operational"
151.00,"01","Location and identification sequences","301043",,,"002023","Satellite derived wind computation method","Cloud motion computational method",,"Operational"
152.00,"01","Location and identification sequences","301043",,,"301011",,"Date",,"Operational"
153.00,"01","Location and identification sequences","301043",,,"301013",,"Time",,"Operational"
154.00,"01","Location and identification sequences","301043",,,"301021",,"Latitude, longitude",,"Operational"
155.00,"01","Location and identification sequences","301044",,,"001007","Satellite identifier","Satellite identifier",,"Operational"
156.00,"01","Location and identification sequences","301044",,,"002024","Integrated mean humidity computational method","Integrated mean humidity computational method",,"Operational"
157.00,"01","Location and identification sequences","301044",,,"301011",,"Date",,"Operational"
158.00,"01","Location and identification sequences","301044",,,"301013",,"Time",,"Operational"
159.00,"01","Location and identification sequences","301044",,,"301021",,"Latitude, longitude",,"Operational"
160.00,"01","Location and identification sequences","301045","(Satellite location and velocity)",,"301011",,"Year, month, day",,"Operational"
161.00,"01","Location and identification sequences","301045","(Satellite location and velocity)",,"301012",,"Time (hour, minute)",,"Operational"
162.00,"01","Location and identification sequences","301045","(Satellite location and velocity)",,"201138","Change data width","Change width to 16 bits",,"Operational"
163.00,"01","Location and identification sequences","301045","(Satellite location and velocity)",,"202131","Change scale","Change scale to 3",,"Operational"
164.00,"01","Location and identification sequences","301045","(Satellite location and velocity)",,"004006","Second","Second",,"Operational"
165.00,"01","Location and identification sequences","301045","(Satellite location and velocity)",,"201000","Change data width","Change width back to Table B",,"Operational"
166.00,"01","Location and identification sequences","301045","(Satellite location and velocity)",,"202000","Change scale","Change scale back to Table B",,"Operational"
167.00,"01","Location and identification sequences","301045","(Satellite location and velocity)",,"304030","Location of platform","Location relative to the Earth’s centre",,"Operational"
168.00,"01","Location and identification sequences","301045","(Satellite location and velocity)",,"304031","Speed of platform","Velocity relative to the Earth’s centre",,"Operational"
169.00,"01","Location and identification sequences","301046",,,"001007","Satellite identifier","Satellite identifier",,"Operational"
170.00,"01","Location and identification sequences","301046",,,"001012","Direction of motion of moving observing platform","Direction of motion of moving observing platform",,"Operational"
171.00,"01","Location and identification sequences","301046",,,"002048","Satellite sensor indicator","Satellite sensor indicator",,"Operational"
172.00,"01","Location and identification sequences","301046",,,"021119","Wind scatterometer geophysical model function","Wind scatterometer geophysical model function",,"Operational"
173.00,"01","Location and identification sequences","301046",,,"025060","Software identification","Software identification",,"Operational"
174.00,"01","Location and identification sequences","301046",,,"202124","Change scale","Change scale",,"Operational"
175.00,"01","Location and identification sequences","301046",,,"002026","Cross-track resolution","Cross-track resolution",,"Operational"
176.00,"01","Location and identification sequences","301046",,,"002027","Along-track resolution","Along-tract resolution",,"Operational"
177.00,"01","Location and identification sequences","301046",,,"202000","Change scale","Change scale back to Table B",,"Operational"
178.00,"01","Location and identification sequences","301046",,,"005040","Orbit number","Orbit number",,"Operational"
179.00,"01","Location and identification sequences","301047","(ERS product header)",,"001007","Satellite identifier","Satellite identifier",,"Operational"
180.00,"01","Location and identification sequences","301047","(ERS product header)",,"025060","Software identification","Software identification",,"Operational"
181.00,"01","Location and identification sequences","301047","(ERS product header)",,"001033","Identification of originating/generating centre","Originating/generating centre",,"Operational"
182.00,"01","Location and identification sequences","301047","(ERS product header)",,"001034","Identification of originating/generating sub-centre","Originating/generating sub-centre",,"Operational"
183.00,"01","Location and identification sequences","301047","(ERS product header)",,"001012","Direction of motion of moving observing platform","Direction of motion of moving observation platform",,"Operational"
184.00,"01","Location and identification sequences","301047","(ERS product header)",,"301045","Satellite location and velocity","Satellite location and velocity",,"Operational"
185.00,"01","Location and identification sequences","301047","(ERS product header)",,"002021","Satellite instrument data used in processing","Satellite instrument data used in processing",,"Operational"
186.00,"01","Location and identification sequences","301047","(ERS product header)",,"301011",,"Date (year, month, day)",,"Operational"
187.00,"01","Location and identification sequences","301047","(ERS product header)",,"301012",,"Time (hour, minute)",,"Operational"
188.00,"01","Location and identification sequences","301047","(ERS product header)",,"201138","Change data width","Change bit width to 16 bits",,"Operational"
189.00,"01","Location and identification sequences","301047","(ERS product header)",,"202131","Change scale","Change scale to 3",,"Operational"
190.00,"01","Location and identification sequences","301047","(ERS product header)",,"004006","Second","Second",,"Operational"
191.00,"01","Location and identification sequences","301047","(ERS product header)",,"201000","Change data width","Change width back to Table B",,"Operational"
192.00,"01","Location and identification sequences","301047","(ERS product header)",,"202000","Change scale","Change scale back to Table B",,"Operational"
193.00,"01","Location and identification sequences","301047","(ERS product header)",,"301023",,"Location (latitude, longitude)",,"Operational"
194.00,"01","Location and identification sequences","301048","(Radar parameters)",,"002104","Antenna polarization","Antenna polarization",,"Operational"
195.00,"01","Location and identification sequences","301048","(Radar parameters)",,"002121","Mean frequency","Mean frequency",,"Operational"
196.00,"01","Location and identification sequences","301048","(Radar parameters)",,"002113","Number of azimuth looks","Number of azimuth looks",,"Operational"
197.00,"01","Location and identification sequences","301048","(Radar parameters)",,"002026","Cross-track resolution","Cross-track resolution",,"Operational"
198.00,"01","Location and identification sequences","301048","(Radar parameters)",,"002027","Along-track resolution","Along-track resolution",,"Operational"
199.00,"01","Location and identification sequences","301048","(Radar parameters)",,"002111","Radar incidence angle","Radar incidence angle",,"Operational"
200.00,"01","Location and identification sequences","301048","(Radar parameters)",,"002140","Satellite radar beam azimuth angle","Satellite radar beam azimuth angle",,"Operational"
201.00,"01","Location and identification sequences","301048","(Radar parameters)",,"202127","Change scale","Change scale to -1",,"Operational"
202.00,"01","Location and identification sequences","301048","(Radar parameters)",,"001013","Speed of motion of moving observing platform","Radar platform velocity",,"Operational"
203.00,"01","Location and identification sequences","301048","(Radar parameters)",,"202126","Change scale","Change scale to -2",,"Operational"
204.00,"01","Location and identification sequences","301048","(Radar parameters)",,"007001","Height of station","Radar platform altitude",,"Operational"
205.00,"01","Location and identification sequences","301048","(Radar parameters)",,"202000","Change scale","Change scale to Table B",,"Operational"
206.00,"01","Location and identification sequences","301048","(Radar parameters)",,"025010","Clutter treatment","Clutter treatment",,"Operational"
207.00,"01","Location and identification sequences","301048","(Radar parameters)",,"021064","Clutter noise estimate","Clutter noise estimate",,"Operational"
208.00,"01","Location and identification sequences","301049","(Radar beam data)",,"002111","Radar incidence angle","Radar incidence angle",,"Operational"
209.00,"01","Location and identification sequences","301049","(Radar beam data)",,"002112","Radar look angle","Radar look angle",,"Operational"
210.00,"01","Location and identification sequences","301049","(Radar beam data)",,"021062","Backscatter","Backscatter",,"Operational"
211.00,"01","Location and identification sequences","301049","(Radar beam data)",,"021063","Radiometric resolution (noise value)","Radiometric resolution (Noise value)",,"Operational"
212.00,"01","Location and identification sequences","301049","(Radar beam data)",,"021065","Missing packet counter","Missing packet counter",,"Operational"
213.00,"01","Location and identification sequences","301051",,,"001006","Aircraft flight number","Aircraft flight number",,"Operational"
214.00,"01","Location and identification sequences","301051",,,"002061","Aircraft navigational system","Navigational system",,"Operational"
215.00,"01","Location and identification sequences","301051",,,"301011",,"Date",,"Operational"
216.00,"01","Location and identification sequences","301051",,,"301012",,"Time",,"Operational"
217.00,"01","Location and identification sequences","301051",,,"301021",,"Latitude, longitude",,"Operational"
218.00,"01","Location and identification sequences","301051",,,"008004","Phase of aircraft flight","Phase of aircraft flight",,"Operational"
219.00,"01","Location and identification sequences","301055",,,"001005","Buoy/platform identifier","Buoy/platform identifier",,"Operational"
220.00,"01","Location and identification sequences","301055",,,"002001","Type of station","Type of station",,"Operational"
221.00,"01","Location and identification sequences","301055",,,"301011",,"Date",,"Operational"
222.00,"01","Location and identification sequences","301055",,,"301012",,"Time",,"Operational"
223.00,"01","Location and identification sequences","301055",,,"301021",,"Latitude and longitude (high accuracy)",,"Operational"
224.00,"01","Location and identification sequences","301055",,,"001012","Direction of motion of moving observing platform","Direction of motion of moving observing platform",,"Operational"
225.00,"01","Location and identification sequences","301055",,,"001014","Platform drift speed (high precision)","Platform drift speed (high precision)",,"Operational"
226.00,"01","Location and identification sequences","301058","(Universal lightning event)","Date/time of lightning event","301011",,"Year, month, day",,"Operational"
227.00,"01","Location and identification sequences","301058","(Universal lightning event)","Date/time of lightning event","301012",,"Hour, minute",,"Operational"
228.00,"01","Location and identification sequences","301058","(Universal lightning event)","Date/time of lightning event","201152","Change data width",,,"Operational"
229.00,"01","Location and identification sequences","301058","(Universal lightning event)","Date/time of lightning event","202135","Change scale",,,"Operational"
230.00,"01","Location and identification sequences","301058","(Universal lightning event)","Date/time of lightning event","004006","Second","Seconds",,"Operational"
231.00,"01","Location and identification sequences","301058","(Universal lightning event)","Date/time of lightning event","202000","Change scale",,,"Operational"
232.00,"01","Location and identification sequences","301058","(Universal lightning event)","Date/time of lightning event","201000","Change data width",,,"Operational"
233.00,"01","Location and identification sequences","301058","(Universal lightning event)","Horizontal and vertical coordinates of lightning event","301021",,"Latitude, longitude (high accuracy)",,"Operational"
234.00,"01","Location and identification sequences","301058","(Universal lightning event)","Horizontal and vertical coordinates of lightning event","020111","x-axis error ellipse major component","x-axis error ellipse",,"Operational"
235.00,"01","Location and identification sequences","301058","(Universal lightning event)","Horizontal and vertical coordinates of lightning event","020112","y-axis error ellipse minor component","y-axis error ellipse",,"Operational"
236.00,"01","Location and identification sequences","301058","(Universal lightning event)","Horizontal and vertical coordinates of lightning event","020113","z-axis error ellipse component","z-axis error ellipse",,"Operational"
237.00,"01","Location and identification sequences","301058","(Universal lightning event)","Horizontal and vertical coordinates of lightning event","020114","Angle of x-axis in error ellipse","Angle of x-axis in error ellipse",,"Operational"
238.00,"01","Location and identification sequences","301058","(Universal lightning event)","Horizontal and vertical coordinates of lightning event","020115","Angle of z-axis in error ellipse","Angle of z-axis in error ellipse",,"Operational"
239.00,"01","Location and identification sequences","301058","(Universal lightning event)","Horizontal and vertical coordinates of lightning event","020116","Emission height of cloud stroke","Emission height of cloud stroke",,"Operational"
240.00,"01","Location and identification sequences","301058","(Universal lightning event)","Emission information","020117","Amplitude of lightning strike","Amplitude of lightning strike",,"Operational"
241.00,"01","Location and identification sequences","301058","(Universal lightning event)","Emission information","020118","Lightning detection error","Lightning detection error",,"Operational"
242.00,"01","Location and identification sequences","301058","(Universal lightning event)","Emission information","020119","Lightning discharge polarity","Lightning discharge polarity",,"Operational"
243.00,"01","Location and identification sequences","301058","(Universal lightning event)","Emission information","025035","Decision method for polarity","Decision method for polarity (V or A)",,"Operational"
244.00,"01","Location and identification sequences","301058","(Universal lightning event)","Emission information","020121","Threshold value for polarity decision","Threshold voltage for polarity decision",,"Operational"
245.00,"01","Location and identification sequences","301058","(Universal lightning event)","Emission information","020122","Threshold value for polarity decision","Threshold current for polarity decision",,"Operational"
246.00,"01","Location and identification sequences","301058","(Universal lightning event)","Emission information","020123","Minimum threshold for detection","Minimum threshold for detection",,"Operational"
247.00,"01","Location and identification sequences","301058","(Universal lightning event)","Emission information","020124","Lightning stroke or flash","Lightning stroke or flash",,"Operational"
248.00,"01","Location and identification sequences","301058","(Universal lightning event)","Emission information","025175","Modified residual","Modified residual",,"Operational"
249.00,"01","Location and identification sequences","301058","(Universal lightning event)","Emission information","020023","Other weather phenomena","Other weather (for cloud to ground or cloud to cloud identification)",,"Operational"
250.00,"01","Location and identification sequences","301058","(Universal lightning event)","Sensor processing","025063","Central processor or system identifier","Central processor identifier",,"Operational"
251.00,"01","Location and identification sequences","301058","(Universal lightning event)","Sensor processing","202136","Change scale",,,"Operational"
252.00,"01","Location and identification sequences","301058","(Universal lightning event)","Sensor processing","201136","Change data width",,,"Operational"
253.00,"01","Location and identification sequences","301058","(Universal lightning event)","Sensor processing","002121","Mean frequency","Mean frequency (to define centre frequency, if used)",,"Operational"
254.00,"01","Location and identification sequences","301058","(Universal lightning event)","Sensor processing","201000","Change data width",,,"Operational"
255.00,"01","Location and identification sequences","301058","(Universal lightning event)","Sensor processing","202000","Change scale",,,"Operational"
256.00,"01","Location and identification sequences","301058","(Universal lightning event)","Sensor processing","025061","Software identification and version number","Software identification and version number",,"Operational"
257.00,"01","Location and identification sequences","301058","(Universal lightning event)","Sensor processing","002184","Type of lightning detection sensor","Type of lightning detection sensor",,"Operational"
258.00,"01","Location and identification sequences","301058","(Universal lightning event)","Sensor processing","002189","Capability to discriminate lightning strikes","Capability to discriminate lightning strike",,"Operational"
259.00,"01","Location and identification sequences","301058","(Universal lightning event)","Sensor processing","025036","Atmospherics location method","Atmospherics location method",,"Operational"
260.00,"01","Location and identification sequences","301058","(Universal lightning event)","Sensor processing","101000","Replication descriptor","Delayed replication of 1 descriptor ",,"Operational"
261.00,"01","Location and identification sequences","301058","(Universal lightning event)","Sensor processing","031002","Extended delayed descriptor replication factor","Extended delayed descriptor replication factor - number of sensors contributing",,"Operational"
262.00,"01","Location and identification sequences","301058","(Universal lightning event)","Sensor processing","301059","Identification of sensor site and instrumentation","Identification of sensor site and instrumentation ",,"Operational"
263.00,"01","Location and identification sequences","301059","(Identification of sensor site and instrumentation)",,"301021",,"Latitude, longitude (high accuracy) of sensor",,"Operational"
264.00,"01","Location and identification sequences","301059","(Identification of sensor site and instrumentation)",,"007030","Height of station ground above mean sea level","Height of station ground above mean sea level ",,"Operational"
265.00,"01","Location and identification sequences","301059","(Identification of sensor site and instrumentation)",,"007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above local ground (for lightning)",,"Operational"
266.00,"01","Location and identification sequences","301062","(Radar location(s))",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
267.00,"01","Location and identification sequences","301062","(Radar location(s))",,"031001","Delayed descriptor replication factor","Replication factor",,"Operational"
268.00,"01","Location and identification sequences","301062","(Radar location(s))",,"301001",,"WMO block and station number",,"Operational"
269.00,"01","Location and identification sequences","301065","(ACARS identification)",,"001006","Aircraft flight number","Aircraft flight number","(see Note 1)","Operational"
270.00,"01","Location and identification sequences","301065","(ACARS identification)",,"001008","Aircraft registration number or other identification","Aircraft registration number","(see Note 1)","Operational"
271.00,"01","Location and identification sequences","301065","(ACARS identification)",,"002001","Type of station","Type of station",,"Operational"
272.00,"01","Location and identification sequences","301065","(ACARS identification)",,"002002","Type of instrumentation for wind measurement","Type of instrumentation for wind measurement",,"Operational"
273.00,"01","Location and identification sequences","301065","(ACARS identification)",,"002005","Precision of temperature observation","Precision of temperature observation",,"Operational"
274.00,"01","Location and identification sequences","301065","(ACARS identification)",,"002062","Type of aircraft data relay system","Type of aircraft data relay system",,"Operational"
275.00,"01","Location and identification sequences","301065","(ACARS identification)",,"002070","Original specification of latitude/longitude","Original specification of latitude/longitude",,"Operational"
276.00,"01","Location and identification sequences","301065","(ACARS identification)",,"002065","ACARS ground-receiving station","ACARS ground receiving station",,"Operational"
277.00,"01","Location and identification sequences","301066","(ACARS location)",,"301011",,"Year, month, day",,"Operational"
278.00,"01","Location and identification sequences","301066","(ACARS location)",,"301013",,"Hour, minute, second",,"Operational"
279.00,"01","Location and identification sequences","301066","(ACARS location)",,"301023",,"Latitude and longitude (coarse accuracy)",,"Operational"
280.00,"01","Location and identification sequences","301066","(ACARS location)",,"007004","Pressure","Pressure",,"Operational"
281.00,"01","Location and identification sequences","301066","(ACARS location)",,"002064","Aircraft roll angle quality","Aircraft roll angle quality",,"Operational"
282.00,"01","Location and identification sequences","301066","(ACARS location)",,"008004","Phase of aircraft flight","Phase of aircraft flight",,"Operational"
283.00,"01","Location and identification sequences","301071","(Satellite identifier/Generating resolution)",,"001007","Satellite identifier","Satellite identifier",,"Operational"
284.00,"01","Location and identification sequences","301071","(Satellite identifier/Generating resolution)",,"001031","Identification of originating/generating centre","Generating centre",,"Operational"
285.00,"01","Location and identification sequences","301071","(Satellite identifier/Generating resolution)",,"002020","Satellite classification","Satellite classification",,"Operational"
286.00,"01","Location and identification sequences","301071","(Satellite identifier/Generating resolution)",,"002028","Segment size at nadir in x-direction","Segment size at nadir in X direction",,"Operational"
287.00,"01","Location and identification sequences","301071","(Satellite identifier/Generating resolution)",,"002029","Segment size at nadir in y-direction","Segment size at nadir in Y direction",,"Operational"
288.00,"01","Location and identification sequences","301072","(Satellite identification)",,"301071","Satellite identifier/Generating resolution","Satellite identification, Generation resolution",,"Operational"
289.00,"01","Location and identification sequences","301072","(Satellite identification)",,"301011",,"Date",,"Operational"
290.00,"01","Location and identification sequences","301072","(Satellite identification)",,"301013",,"Time",,"Operational"
291.00,"01","Location and identification sequences","301072","(Satellite identification)",,"301021",,"Latitude, longitude",,"Operational"
292.00,"01","Location and identification sequences","301089","(National station identification)",,"001101","State identifier","State identifier",,"Operational"
293.00,"01","Location and identification sequences","301089","(National station identification)",,"001102","National station number","National station number",,"Operational"
294.00,"01","Location and identification sequences","301090","(Surface station identification; time, horizontal and vertical co-ordinates)",,"301004","Surface station identification","Surface station identification",,"Operational"
295.00,"01","Location and identification sequences","301090","(Surface station identification; time, horizontal and vertical coordinates)",,"301011",,"Year, month, day",,"Operational"
296.00,"01","Location and identification sequences","301090","(Surface station identification; time, horizontal and vertical coordinates)",,"301012",,"Hour, minute",,"Operational"
297.00,"01","Location and identification sequences","301090","(Surface station identification; time, horizontal and vertical coordinates)",,"301021",,"Latitude, longitude (high accuracy)",,"Operational"
298.00,"01","Location and identification sequences","301090","(Surface station identification; time, horizontal and vertical coordinates)",,"007030","Height of station ground above mean sea level","Height of station ground above mean sea level",,"Operational"
299.00,"01","Location and identification sequences","301090","(Surface station identification; time, horizontal and vertical coordinates)",,"007031","Height of barometer above mean sea level","Height of barometer above mean sea level",,"Operational"
300.00,"01","Location and identification sequences","301091","(Surface station instrumentation)",,"002180","Main present weather detecting system","Main present weather detecting system",,"Operational"
301.00,"01","Location and identification sequences","301091","(Surface station instrumentation)",,"002181","Supplementary present weather sensor","Supplementary present weather sensor",,"Operational"
302.00,"01","Location and identification sequences","301091","(Surface station instrumentation)",,"002182","Visibility measurement system","Visibility measurement system",,"Operational"
303.00,"01","Location and identification sequences","301091","(Surface station instrumentation)",,"002183","Cloud detection system","Cloud detection system",,"Operational"
304.00,"01","Location and identification sequences","301091","(Surface station instrumentation)",,"002184","Type of lightning detection sensor","Type of lightning detection sensor",,"Operational"
305.00,"01","Location and identification sequences","301091","(Surface station instrumentation)",,"002179","Type of sky condition algorithm","Type of sky condition algorithm",,"Operational"
306.00,"01","Location and identification sequences","301091","(Surface station instrumentation)",,"002186","Capability to detect precipitation phenomena","Capability to detect precipitation phenomena",,"Operational"
307.00,"01","Location and identification sequences","301091","(Surface station instrumentation)",,"002187","Capability to detect other weather phenomena","Capability to detect other weather phenomena",,"Operational"
308.00,"01","Location and identification sequences","301091","(Surface station instrumentation)",,"002188","Capability to detect obscuration","Capability to detect obscuration",,"Operational"
309.00,"01","Location and identification sequences","301091","(Surface station instrumentation)",,"002189","Capability to discriminate lightning strikes","Capability to discriminate lightning strikes",,"Operational"
310.00,"01","Location and identification sequences","301092","(Mobile surface station identification, date/time, horizontal and vertical coordinates)",,"001011","Ship or mobile land station identifier","Mobile land station identifier",,"Operational"
311.00,"01","Location and identification sequences","301092","(Mobile surface station identification, date/time, horizontal and vertical coordinates)",,"001003","WMO Region number/geographical area","WMO Region number",,"Operational"
312.00,"01","Location and identification sequences","301092","(Mobile surface station identification, date/time, horizontal and vertical coordinates)",,"002001","Type of station","Type of station",,"Operational"
313.00,"01","Location and identification sequences","301092","(Mobile surface station identification, date/time, horizontal and vertical coordinates)",,"301011",,"Year, month, day",,"Operational"
314.00,"01","Location and identification sequences","301092","(Mobile surface station identification, date/time, horizontal and vertical coordinates)",,"301012",,"Hour, minute",,"Operational"
315.00,"01","Location and identification sequences","301092","(Mobile surface station identification, date/time, horizontal and vertical coordinates)",,"301021",,"Latitude (high accuracy), longitude (high accuracy)",,"Operational"
316.00,"01","Location and identification sequences","301092","(Mobile surface station identification, date/time, horizontal and vertical coordinates)",,"007030","Height of station ground above mean sea level","Height of station ground above mean sea level",,"Operational"
317.00,"01","Location and identification sequences","301092","(Mobile surface station identification, date/time, horizontal and vertical coordinates)",,"007031","Height of barometer above mean sea level","Height of barometer above mean sea level",,"Operational"
318.00,"01","Location and identification sequences","301092","(Mobile surface station identification, date/time, horizontal and vertical coordinates)",,"033024","Station elevation quality mark (for mobile stations)","Station elevation quality mark",,"Operational"
319.00,"01","Location and identification sequences","301093","(Ship identification, movement, date/time, horizontal and vertical coordinates)",,"301036","Ship","Ship identification",,"Operational"
320.00,"01","Location and identification sequences","301093","(Ship identification, movement, date/time, horizontal and vertical coordinates)",,"007030","Height of station ground above mean sea level","Height of station platform above mean sea level",,"Operational"
321.00,"01","Location and identification sequences","301093","(Ship identification, movement, date/time, horizontal and vertical coordinates)",,"007031","Height of barometer above mean sea level","Height of barometer above mean sea level",,"Operational"
322.00,"01","Location and identification sequences","301110","(Identification of launch site and instrumentation for wind measurements)",,"301001",,"WMO block number, WMO station number",,"Operational"
323.00,"01","Location and identification sequences","301110","(Identification of launch site and instrumentation for wind measurements)",,"001011","Ship or mobile land station identifier","Ship or mobile land station identifier",,"Operational"
324.00,"01","Location and identification sequences","301110","(Identification of launch site and instrumentation for wind measurements)",,"002011","Radiosonde type","Radiosonde type",,"Operational"
325.00,"01","Location and identification sequences","301110","(Identification of launch site and instrumentation for wind measurements)",,"002014","Tracking technique/status of system used","Tracking technique/status of system used",,"Operational"
326.00,"01","Location and identification sequences","301110","(Identification of launch site and instrumentation for wind measurements)",,"002003","Type of measuring equipment used","Type of measuring equipment used",,"Operational"
327.00,"01","Location and identification sequences","301111","(Identification of launch site and instrumentation for P, T, U and wind measurements)",,"301001",,"WMO block number, WMO station number",,"Operational"
328.00,"01","Location and identification sequences","301111","(Identification of launch site and instrumentation for P, T, U and wind measurements)",,"001011","Ship or mobile land station identifier","Ship or mobile land station identifier",,"Operational"
329.00,"01","Location and identification sequences","301111","(Identification of launch site and instrumentation for P, T, U and wind measurements)",,"002011","Radiosonde type","Radiosonde type",,"Operational"
330.00,"01","Location and identification sequences","301111","(Identification of launch site and instrumentation for P, T, U and wind measurements)",,"002013","Solar and infrared radiation correction","Solar and infrared radiation correction",,"Operational"
331.00,"01","Location and identification sequences","301111","(Identification of launch site and instrumentation for P, T, U and wind measurements)",,"002014","Tracking technique/status of system used","Tracking technique/status of system used",,"Operational"
332.00,"01","Location and identification sequences","301111","(Identification of launch site and instrumentation for P, T, U and wind measurements)",,"002003","Type of measuring equipment used","Type of measuring equipment used",,"Operational"
333.00,"01","Location and identification sequences","301112","(Identification of launch point and instrumentation of dropsonde)",,"001006","Aircraft flight number","Aircraft identifier",,"Operational"
334.00,"01","Location and identification sequences","301112","(Identification of launch point and instrumentation of dropsonde)",,"002011","Radiosonde type","Radiosonde type",,"Operational"
335.00,"01","Location and identification sequences","301112","(Identification of launch point and instrumentation of dropsonde)",,"002013","Solar and infrared radiation correction","Solar and infrared radiation correction",,"Operational"
336.00,"01","Location and identification sequences","301112","(Identification of launch point and instrumentation of dropsonde)",,"002014","Tracking technique/status of system used","Tracking technique/status of system used",,"Operational"
337.00,"01","Location and identification sequences","301112","(Identification of launch point and instrumentation of dropsonde)",,"002003","Type of measuring equipment used","Type of measuring equipment used",,"Operational"
338.00,"01","Location and identification sequences","301113","(Date/time of launch)",,"008021","Time significance","Time significance (= 18 (launch time))","(see Note 3)","Operational"
339.00,"01","Location and identification sequences","301113","(Date/time of launch)",,"301011",,"Year, month, day of launch",,"Operational"
340.00,"01","Location and identification sequences","301113","(Date/time of launch)",,"301013",,"Hour, minute, second of launch",,"Operational"
341.00,"01","Location and identification sequences","301114","(Horizontal and vertical coordinates of launch site)",,"301021",,"Latitude (high accuracy), longitude (high accuracy)",,"Operational"
342.00,"01","Location and identification sequences","301114","(Horizontal and vertical coordinates of launch site)",,"007030","Height of station ground above mean sea level","Height of station ground above mean sea level",,"Operational"
343.00,"01","Location and identification sequences","301114","(Horizontal and vertical coordinates of launch site)",,"007031","Height of barometer above mean sea level","Height of barometer above mean sea level",,"Operational"
344.00,"01","Location and identification sequences","301114","(Horizontal and vertical coordinates of launch site)",,"007007","Height","Height of release of sonde above mean sea level",,"Operational"
345.00,"01","Location and identification sequences","301114","(Horizontal and vertical coordinates of launch site)",,"033024","Station elevation quality mark (for mobile stations)","Station elevation quality mark (for mobile stations)",,"Operational"
346.00,"01","Location and identification sequences","301120","(Radiosonde abbreviated header and launch information)",,"301001",,"WMO block and station number",,"Operational"
347.00,"01","Location and identification sequences","301120","(Radiosonde abbreviated header and launch information)",,"001094","WBAN Number","WBAN number",,"Operational"
348.00,"01","Location and identification sequences","301120","(Radiosonde abbreviated header and launch information)",,"002011","Radiosonde type","Radiosonde type",,"Operational"
349.00,"01","Location and identification sequences","301120","(Radiosonde abbreviated header and launch information)",,"301121","Radiosonde launch point location","Radiosonde launch point location",,"Operational"
350.00,"01","Location and identification sequences","301121","(Radiosonde launch point location)",,"008041","Data significance","Data significance (3 = Balloon launch point)",,"Operational"
351.00,"01","Location and identification sequences","301121","(Radiosonde launch point location)",,"301122","Date/time (to hundredths of second) (see Note 3)","Date/time (to hundredths of second)",,"Operational"
352.00,"01","Location and identification sequences","301121","(Radiosonde launch point location)",,"301021",,"Latitude and longitude (high accuracy)",,"Operational"
353.00,"01","Location and identification sequences","301121","(Radiosonde launch point location)",,"007031",,"Height of barometer above MSL",,"Operational"
354.00,"01","Location and identification sequences","301121","(Radiosonde launch point location)",,"007007","Height","Height (of radiosonde release above MSL)",,"Operational"
355.00,"01","Location and identification sequences","301122","(Date/time (to hundredths of second))",,"301011",,"Date","(see Note 3)","Operational"
356.00,"01","Location and identification sequences","301122","(Date/time (to hundredths of second))",,"301012",,"Time",,"Operational"
357.00,"01","Location and identification sequences","301122","(Date/time (to hundredths of second))",,"201135","Change data width","Change data width",,"Operational"
358.00,"01","Location and identification sequences","301122","(Date/time (to hundredths of second))",,"202130","Change scale","Change scale",,"Operational"
359.00,"01","Location and identification sequences","301122","(Date/time (to hundredths of second))",,"004006","Second","Second",,"Operational"
360.00,"01","Location and identification sequences","301122","(Date/time (to hundredths of second))",,"202000","Change scale","Cancel change scale",,"Operational"
361.00,"01","Location and identification sequences","301122","(Date/time (to hundredths of second))",,"201000","Change data width","Cancel change data width",,"Operational"
362.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"102002","Replication descriptor","Replicate 2 descriptors 2 times",,"Operational"
363.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"008041","Data significance","Data significance (0 = Parent site, 1 = Observation site)",,"Operational"
364.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"001062","Short ICAO location indicator","Short ICAO location identifier",,"Operational"
365.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"301001",,"WMO block and station number",,"Operational"
366.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"001094","WBAN Number","WBAN number",,"Operational"
367.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"002011","Radiosonde type","Radiosonde type",,"Operational"
368.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"001018","Short station or site name","Short station or site name",,"Operational"
369.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"001095","Observer identification","Observer identification",,"Operational"
370.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"025061","Software identification and version number","Software identification",,"Operational"
371.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"025068","Number of archive recomputes","Number of archive recomputes",,"Operational"
372.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"001082","Radiosonde ascension number","Radiosonde ascension number",,"Operational"
373.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"001083","Radiosonde release number","Radiosonde release number",,"Operational"
374.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"001081","Radiosonde serial number","Radiosonde serial number",,"Operational"
375.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"002067","Radiosonde operating frequency","Radiosonde operating frequency",,"Operational"
376.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"002066","Radiosonde ground receiving system","Radiosonde ground receiving system",,"Operational"
377.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"002014","Tracking technique/status of system used","Tracking technique/status of system used",,"Operational"
378.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"025067","Radiosonde release point pressure correction","Release point pressure correction",,"Operational"
379.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"025065","Orientation correction (azimuth)","Orientation correction (azimuth)",,"Operational"
380.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"025066","Orientation correction (elevation)","Orientation correction (elevation)",,"Operational"
381.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"002095","Type of pressure sensor","Type of pressure sensor",,"Operational"
382.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"002096","Type of temperature sensor","Type of temperature sensor",,"Operational"
383.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"002097","Type of humidity sensor","Type of humidity sensor",,"Operational"
384.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"002016","Radiosonde configuration","Radiosonde configuration",,"Operational"
385.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"002083","Type of balloon shelter","Type of balloon shelter",,"Operational"
386.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"002080","Balloon manufacturer","Balloon manufacturer",,"Operational"
387.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"002081","Type of balloon","Type of balloon",,"Operational"
388.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"001093","Balloon lot number","Balloon lot number",,"Operational"
389.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"002084","Type of gas used in balloon","Type of gas used in balloon",,"Operational"
390.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"002085","Amount of gas used in balloon","Amount of gas used in balloon",,"Operational"
391.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"002086","Balloon flight train length","Balloon flight train length",,"Operational"
392.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"002082","Weight of balloon","Weight of balloon",,"Operational"
393.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"008041","Data significance","Data significance (2 = Balloon manufacture date)",,"Operational"
394.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"301011",,"Date",,"Operational"
395.00,"01","Location and identification sequences","301125","(ASCAT header information)",,"001033","Identification of originating/generating centre","Identification of originating/generating centre",,"Operational"
396.00,"01","Location and identification sequences","301125","(ASCAT header information)",,"001034","Identification of originating/generating sub-centre","Identification of originating/generating sub-centre",,"Operational"
397.00,"01","Location and identification sequences","301125","(ASCAT header information)",,"025060","Software identification","Software identification",,"Operational"
398.00,"01","Location and identification sequences","301125","(ASCAT header information)",,"001007","Satellite identifier","Satellite identifier",,"Operational"
399.00,"01","Location and identification sequences","301125","(ASCAT header information)",,"002019","Satellite instruments","Satellite instruments",,"Operational"
400.00,"01","Location and identification sequences","301125","(ASCAT header information)",,"001012","Direction of motion of moving observing platform","Direction of motion of moving observing platform",,"Operational"
401.00,"02","Meteorological sequences common to surface data","302001",,,"010004","Pressure","Pressure (at station level)",,"Operational"
402.00,"02","Meteorological sequences common to surface data","302001",,,"010051","Pressure reduced to mean sea level","Pressure reduced to mean sea level",,"Operational"
403.00,"02","Meteorological sequences common to surface data","302001",,,"010061","3-hour pressure change","3-hour pressure change",,"Operational"
404.00,"02","Meteorological sequences common to surface data","302001",,,"010063","Characteristic of pressure tendency","Characteristic of pressure tendency",,"Operational"
405.00,"02","Meteorological sequences common to surface data","302002","(High altitude station)",,"010004","Pressure","Pressure (at station level)",,"Operational"
406.00,"02","Meteorological sequences common to surface data","302002","(High altitude station)",,"007004","Pressure","Pressure level",,"Operational"
407.00,"02","Meteorological sequences common to surface data","302002","(High altitude station)",,"010003","Geopotential","Geopotential of pressure level",,"Operational"
408.00,"02","Meteorological sequences common to surface data","302002","(High altitude station)",,"010061","3-hour pressure change","3-hour pressure change",,"Operational"
409.00,"02","Meteorological sequences common to surface data","302002","(High altitude station)",,"010063","Characteristic of pressure tendency","Characteristic of pressure tendency",,"Operational"
410.00,"02","Meteorological sequences common to surface data","302003",,,"011011","Wind direction at 10 m","Wind direction (10 m)",,"Operational"
411.00,"02","Meteorological sequences common to surface data","302003",,,"011012","Wind speed at 10 m","Wind speed (10 m)",,"Operational"
412.00,"02","Meteorological sequences common to surface data","302003",,,"012004","Air temperature at 2 m","Temperature (2 m)",,"Operational"
413.00,"02","Meteorological sequences common to surface data","302003",,,"012006","Dew-point temperature at 2 m","Dew point (2 m)",,"Operational"
414.00,"02","Meteorological sequences common to surface data","302003",,,"013003","Relative humidity","Relative humidity",,"Operational"
415.00,"02","Meteorological sequences common to surface data","302003",,,"020001","Horizontal visibility","Horizontal visibility",,"Operational"
416.00,"02","Meteorological sequences common to surface data","302003",,,"020003","Present weather","Present weather",,"Operational"
417.00,"02","Meteorological sequences common to surface data","302003",,,"020004","Past weather (1)","Past weather (1)",,"Operational"
418.00,"02","Meteorological sequences common to surface data","302003",,,"020005","Past weather (2)","Past weather (2)",,"Operational"
419.00,"02","Meteorological sequences common to surface data","302004","(General cloud information)",,"020010","Cloud cover (total)","Cloud cover (total in per cent)",,"Operational"
420.00,"02","Meteorological sequences common to surface data","302004","(General cloud information)",,"008002","Vertical significance (surface observations)","Vertical significance",,"Operational"
421.00,"02","Meteorological sequences common to surface data","302004","(General cloud information)",,"020011","Cloud amount","Cloud amount",,"Operational"
422.00,"02","Meteorological sequences common to surface data","302004","(General cloud information)",,"020013","Height of base of cloud","Height of base of cloud",,"Operational"
423.00,"02","Meteorological sequences common to surface data","302004","(General cloud information)",,"020012","Cloud type","Cloud type",,"Operational"
424.00,"02","Meteorological sequences common to surface data","302004","(General cloud information)",,"020012","Cloud type","Cloud type",,"Operational"
425.00,"02","Meteorological sequences common to surface data","302004","(General cloud information)",,"020012","Cloud type","Cloud type",,"Operational"
426.00,"02","Meteorological sequences common to surface data","302005",,,"008002","Vertical significance (surface observations)","Vertical significance",,"Operational"
427.00,"02","Meteorological sequences common to surface data","302005",,,"020011","Cloud amount","Cloud amount",,"Operational"
428.00,"02","Meteorological sequences common to surface data","302005",,,"020012","Cloud type","Cloud type",,"Operational"
429.00,"02","Meteorological sequences common to surface data","302005",,,"020013","Height of base of cloud","Height of base of cloud",,"Operational"
430.00,"02","Meteorological sequences common to surface data","302006",,,"010004","Pressure","Pressure (at station level)",,"Operational"
431.00,"02","Meteorological sequences common to surface data","302006",,,"010051","Pressure reduced to mean sea level","Pressure reduced to mean sea level",,"Operational"
432.00,"02","Meteorological sequences common to surface data","302006",,,"010062","24-hour pressure change","24-hour pressure change",,"Operational"
433.00,"02","Meteorological sequences common to surface data","302006",,,"010063","Characteristic of pressure tendency","Characteristic of pressure tendency",,"Operational"
434.00,"02","Meteorological sequences common to surface data","302011","(Low altitude station)",,"302001",,"Pressure and pressure change",,"Operational"
435.00,"02","Meteorological sequences common to surface data","302011","(Low altitude station)",,"302003",,"Wind, temperature, humidity, visibility, weather",,"Operational"
436.00,"02","Meteorological sequences common to surface data","302011","(Low altitude station)",,"302004","General cloud information","Significant cloud layer",,"Operational"
437.00,"02","Meteorological sequences common to surface data","302012","(High altitude station)",,"302002","High altitude station","Pressure and pressure change",,"Operational"
438.00,"02","Meteorological sequences common to surface data","302012","(High altitude station)",,"302003",,"Wind, temperature, humidity, visibility, weather",,"Operational"
439.00,"02","Meteorological sequences common to surface data","302012","(High altitude station)",,"302004","General cloud information","Significant cloud information",,"Operational"
440.00,"02","Meteorological sequences common to surface data","302013",,,"302006",,"Pressure and pressure change",,"Operational"
441.00,"02","Meteorological sequences common to surface data","302013",,,"302003",,"Wind, temperature, humidity, visibility, weather",,"Operational"
442.00,"02","Meteorological sequences common to surface data","302013",,,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
443.00,"02","Meteorological sequences common to surface data","302013",,,"031001","Delayed descriptor replication factor","Delayed descriptor replication factor",,"Operational"
444.00,"02","Meteorological sequences common to surface data","302013",,,"302005",,"Cloud layer information",,"Operational"
445.00,"02","Meteorological sequences common to surface data","302021",,,"022001","Direction of waves","Direction of waves",,"Operational"
446.00,"02","Meteorological sequences common to surface data","302021",,,"022011","Period of waves","Period of waves",,"Operational"
447.00,"02","Meteorological sequences common to surface data","302021",,,"022021","Height of waves","Height of waves",,"Operational"
448.00,"02","Meteorological sequences common to surface data","302022",,,"022002","Direction of wind waves","Direction of wind waves",,"Operational"
449.00,"02","Meteorological sequences common to surface data","302022",,,"022012","Period of wind waves","Period of wind waves",,"Operational"
450.00,"02","Meteorological sequences common to surface data","302022",,,"022022","Height of wind waves","Height of wind waves",,"Operational"
451.00,"02","Meteorological sequences common to surface data","302023",,,"022003","Direction of swell waves","Direction of swell waves",,"Operational"
452.00,"02","Meteorological sequences common to surface data","302023",,,"022013","Period of swell waves","Period of swell waves",,"Operational"
453.00,"02","Meteorological sequences common to surface data","302023",,,"022023","Height of swell waves","Height of swell waves",,"Operational"
454.00,"02","Meteorological sequences common to surface data","302024",,,"302022",,"Wind waves",,"Operational"
455.00,"02","Meteorological sequences common to surface data","302024",,,"101002","Replication descriptor","Replicate 1 descriptor 2 times",,"Operational"
456.00,"02","Meteorological sequences common to surface data","302024",,,"302023",,"Swell waves (2 systems of swell)",,"Operational"
457.00,"02","Meteorological sequences common to surface data","302031","(Pressure information)",,"302001",,"Pressure data",,"Operational"
458.00,"02","Meteorological sequences common to surface data","302031","(Pressure information)",,"010062","24-hour pressure change","24-hour pressure change",,"Operational"
459.00,"02","Meteorological sequences common to surface data","302031","(Pressure information)",,"007004","Pressure","Pressure (standard level)",,"Operational"
460.00,"02","Meteorological sequences common to surface data","302031","(Pressure information)",,"010009","Geopotential height","Geopotential height of the standard level",,"Operational"
461.00,"02","Meteorological sequences common to surface data","302032","(Temperature and humidity data)",,"007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above local ground (for temperature and humidity measurement)",,"Operational"
462.00,"02","Meteorological sequences common to surface data","302032","(Temperature and humidity data)",,"012101","Temperature/air temperature","Temperature/air temperature (scale 2)",,"Operational"
463.00,"02","Meteorological sequences common to surface data","302032","(Temperature and humidity data)",,"012103","Dew-point temperature","Dew-point temperature (scale 2)",,"Operational"
464.00,"02","Meteorological sequences common to surface data","302032","(Temperature and humidity data)",,"013003","Relative humidity","Relative humidity",,"Operational"
465.00,"02","Meteorological sequences common to surface data","302033","(Visibility data)",,"007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above local ground (for visibility measurement)",,"Operational"
466.00,"02","Meteorological sequences common to surface data","302033","(Visibility data)",,"020001","Horizontal visibility","Horizontal visibility",,"Operational"
467.00,"02","Meteorological sequences common to surface data","302034","(Precipitation past 24 hours)",,"007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above local ground (for precipitation measurement)",,"Operational"
468.00,"02","Meteorological sequences common to surface data","302034","(Precipitation past 24 hours)",,"013023","Total precipitation past 24 hours","Total precipitation past 24 hours",,"Operational"
469.00,"02","Meteorological sequences common to surface data","302035","(Basic synoptic ""instantaneous"" data)",,"302032","Temperature and humidity data","Temperature and humidity data",,"Operational"
470.00,"02","Meteorological sequences common to surface data","302035","(Basic synoptic ""instantaneous"" data)",,"302033","Visibility data","Visibility data",,"Operational"
471.00,"02","Meteorological sequences common to surface data","302035","(Basic synoptic ""instantaneous"" data)",,"302034","Precipitation past 24 hours","Precipitation past 24 hours",,"Operational"
472.00,"02","Meteorological sequences common to surface data","302035","(Basic synoptic ""instantaneous"" data)",,"007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above local ground (set to missing to cancel the previous value)",,"Operational"
473.00,"02","Meteorological sequences common to surface data","302035","(Basic synoptic ""instantaneous"" data)",,"302004","General cloud information","Cloud data",,"Operational"
474.00,"02","Meteorological sequences common to surface data","302035","(Basic synoptic ""instantaneous"" data)",,"101000","Replication descriptor","Delayed replication",,"Operational"
475.00,"02","Meteorological sequences common to surface data","302035","(Basic synoptic ""instantaneous"" data)",,"031001","Delayed descriptor replication factor","Delayed descriptor replication factor",,"Operational"
476.00,"02","Meteorological sequences common to surface data","302035","(Basic synoptic ""instantaneous"" data)",,"302005",,"Individual cloud layer or mass",,"Operational"
477.00,"02","Meteorological sequences common to surface data","302036","(Clouds with bases below station level)",,"105000","Replication descriptor","Delayed replication of 5 descriptors",,"Operational"
478.00,"02","Meteorological sequences common to surface data","302036","(Clouds with bases below station level)",,"031001","Delayed descriptor replication factor","Delayed descriptor replication factor",,"Operational"
479.00,"02","Meteorological sequences common to surface data","302036","(Clouds with bases below station level)",,"008002","Vertical significance (surface observations)","Vertical significance",,"Operational"
480.00,"02","Meteorological sequences common to surface data","302036","(Clouds with bases below station level)",,"020011","Cloud amount","Cloud amount",,"Operational"
481.00,"02","Meteorological sequences common to surface data","302036","(Clouds with bases below station level)",,"020012","Cloud type","Cloud type",,"Operational"
482.00,"02","Meteorological sequences common to surface data","302036","(Clouds with bases below station level)",,"020014","Height of top of cloud","Height of top of cloud",,"Operational"
483.00,"02","Meteorological sequences common to surface data","302036","(Clouds with bases below station level)",,"020017","Cloud top description","Cloud top description",,"Operational"
484.00,"02","Meteorological sequences common to surface data","302037","(State of ground, snow depth, ground minimum temperature)",,"020062","State of the ground (with or without snow)","State of ground (with or without snow)",,"Operational"
485.00,"02","Meteorological sequences common to surface data","302037","(State of ground, snow depth, ground minimum temperature)",,"013013","Total snow depth","Total snow depth",,"Operational"
486.00,"02","Meteorological sequences common to surface data","302037","(State of ground, snow depth, ground minimum temperature)",,"012113","Ground minimum temperature, past 12 hours","Ground minimum temperature (scale 2), past 12 hours",,"Operational"
487.00,"02","Meteorological sequences common to surface data","302038","(Present and past weather)",,"020003","Present weather","Present weather",,"Operational"
488.00,"02","Meteorological sequences common to surface data","302038","(Present and past weather)",,"004024","Time period or displacement","Time period in hours",,"Operational"
489.00,"02","Meteorological sequences common to surface data","302038","(Present and past weather)",,"020004","Past weather (1)","Past weather (1)",,"Operational"
490.00,"02","Meteorological sequences common to surface data","302038","(Present and past weather)",,"020005","Past weather (2)","Past weather (2)",,"Operational"
491.00,"02","Meteorological sequences common to surface data","302039","(Sunshine data (from 1 hour and 24 hour period))",,"004024","Time period or displacement","Time period in hours",,"Operational"
492.00,"02","Meteorological sequences common to surface data","302039","(Sunshine data (from 1 hour and 24 hour period))",,"014031","Total sunshine","Total sunshine",,"Operational"
493.00,"02","Meteorological sequences common to surface data","302040","(Precipitation measurement)",,"007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above local ground (for precipitation measurement)",,"Operational"
494.00,"02","Meteorological sequences common to surface data","302040","(Precipitation measurement)",,"102002","Replication descriptor","Replicate next 2 descriptors 2 times",,"Operational"
495.00,"02","Meteorological sequences common to surface data","302040","(Precipitation measurement)",,"004024","Time period or displacement","Time period in hours",,"Operational"
496.00,"02","Meteorological sequences common to surface data","302040","(Precipitation measurement)",,"013011","Total precipitation/total water equivalent","Total precipitation / total water equivalent of snow",,"Operational"
497.00,"02","Meteorological sequences common to surface data","302041","(Extreme temperature data)",,"007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above local ground (for temperature measurement)",,"Operational"
498.00,"02","Meteorological sequences common to surface data","302041","(Extreme temperature data)",,"004024","Time period or displacement","Time period or displacement",,"Operational"
499.00,"02","Meteorological sequences common to surface data","302041","(Extreme temperature data)",,"004024","Time period or displacement","Time period or displacement","(see Notes 1 and 2)","Operational"
500.00,"02","Meteorological sequences common to surface data","302041","(Extreme temperature data)",,"012111","Maximum temperature, at height and over period specified","Maximum temperature (scale 2) at height and over period specified",,"Operational"
501.00,"02","Meteorological sequences common to surface data","302041","(Extreme temperature data)",,"004024","Time period or displacement","Time period or displacement",,"Operational"
502.00,"02","Meteorological sequences common to surface data","302041","(Extreme temperature data)",,"004024","Time period or displacement","Time period or displacement","(see Note 2)","Operational"
503.00,"02","Meteorological sequences common to surface data","302041","(Extreme temperature data)",,"012112","Minimum temperature, at height and over period specified","Minimum temperature (scale 2) at height and over period specified",,"Operational"
504.00,"02","Meteorological sequences common to surface data","302042","(Wind data)",,"007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above local ground (for wind measurement)",,"Operational"
505.00,"02","Meteorological sequences common to surface data","302042","(Wind data)",,"002002","Type of instrumentation for wind measurement","Type of instrumentation for wind measurement",,"Operational"
506.00,"02","Meteorological sequences common to surface data","302042","(Wind data)",,"008021","Time significance","Time significance (= 2 (time averaged))",,"Operational"
507.00,"02","Meteorological sequences common to surface data","302042","(Wind data)",,"004025","Time period or displacement","Time period (= -10 minutes, or number of minutes after a significant change of wind)",,"Operational"
508.00,"02","Meteorological sequences common to surface data","302042","(Wind data)",,"011001","Wind direction","Wind direction",,"Operational"
509.00,"02","Meteorological sequences common to surface data","302042","(Wind data)",,"011002","Wind speed","Wind speed",,"Operational"
510.00,"02","Meteorological sequences common to surface data","302042","(Wind data)",,"008021","Time significance","Time significance (= missing value)",,"Operational"
511.00,"02","Meteorological sequences common to surface data","302042","(Wind data)",,"103002","Replication descriptor","Replicate next 3 descriptors 2 times",,"Operational"
512.00,"02","Meteorological sequences common to surface data","302042","(Wind data)",,"004025","Time period or displacement","Time period in minutes",,"Operational"
513.00,"02","Meteorological sequences common to surface data","302042","(Wind data)",,"011043","Maximum wind gust direction","Maximum wind gust direction",,"Operational"
514.00,"02","Meteorological sequences common to surface data","302042","(Wind data)",,"011041","Maximum wind gust speed","Maximum wind gust speed",,"Operational"
515.00,"02","Meteorological sequences common to surface data","302043","(Basic synoptic ""period"" data)",,"302038","Present and past weather","Present and past weather",,"Operational"
516.00,"02","Meteorological sequences common to surface data","302043","(Basic synoptic ""period"" data)",,"101002","Replication descriptor","Replicate 1 descriptor 2 times",,"Operational"
517.00,"02","Meteorological sequences common to surface data","302043","(Basic synoptic ""period"" data)",,"302039","Sunshine data (from 1 hour and 24 hour period)","Sunshine data (from 1 hour and 24 hour period)",,"Operational"
518.00,"02","Meteorological sequences common to surface data","302043","(Basic synoptic ""period"" data)",,"302040","Precipitation measurement","Precipitation measurement",,"Operational"
519.00,"02","Meteorological sequences common to surface data","302043","(Basic synoptic ""period"" data)",,"302041","Extreme temperature data","Extreme temperature data",,"Operational"
520.00,"02","Meteorological sequences common to surface data","302043","(Basic synoptic ""period"" data)",,"302042","Wind data","Wind data",,"Operational"
521.00,"02","Meteorological sequences common to surface data","302043","(Basic synoptic ""period"" data)",,"007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above local ground (set to missing to cancel the previous value)",,"Operational"
522.00,"02","Meteorological sequences common to surface data","302044","(Evaporation data)",,"004024","Time period or displacement","Time period in hours",,"Operational"
523.00,"02","Meteorological sequences common to surface data","302044","(Evaporation data)",,"002004","Type of instrumentation for evaporation measurement or type of crop for which evapotranspiration is reported","Type of instrument for evaporation or crop type for evapotranspiration",,"Operational"
524.00,"02","Meteorological sequences common to surface data","302044","(Evaporation data)",,"013033","Evaporation /evapotranspiration","Evaporation /evapotranspiration",,"Operational"
525.00,"02","Meteorological sequences common to surface data","302045","(Radiation data (from 1 hour and 24 hour period))",,"004024","Time period or displacement","Time period in hours",,"Operational"
526.00,"02","Meteorological sequences common to surface data","302045","(Radiation data (from 1 hour and 24 hour period))",,"014002","Long-wave radiation, integrated over period specified","Long-wave radiation, integrated over period specified",,"Operational"
527.00,"02","Meteorological sequences common to surface data","302045","(Radiation data (from 1 hour and 24 hour period))",,"014004","Short-wave radiation, integrated over period specified","Short-wave radiation, integrated over period specified",,"Operational"
528.00,"02","Meteorological sequences common to surface data","302045","(Radiation data (from 1 hour and 24 hour period))",,"014016","Net radiation, integrated over period specified","Net radiation, integrated over period specified",,"Operational"
529.00,"02","Meteorological sequences common to surface data","302045","(Radiation data (from 1 hour and 24 hour period))",,"014028","Global solar radiation (high accuracy), integrated over period specified","Global solar radiation (high accuracy), integrated over period specified",,"Operational"
530.00,"02","Meteorological sequences common to surface data","302045","(Radiation data (from 1 hour and 24 hour period))",,"014029","Diffuse solar radiation (high accuracy), integrated over period specified","Diffuse solar radiation (high accuracy), integrated over period specified",,"Operational"
531.00,"02","Meteorological sequences common to surface data","302045","(Radiation data (from 1 hour and 24 hour period))",,"014030","Direct solar radiation (high accuracy), integrated over period specified","Direct solar radiation (high accuracy), integrated over period specified",,"Operational"
532.00,"02","Meteorological sequences common to surface data","302046","(Temperature change)",,"004024","Time period or displacement","Time period or displacement",,"Operational"
533.00,"02","Meteorological sequences common to surface data","302046","(Temperature change)",,"004024","Time period or displacement","Time period or displacement","(see Note 3)","Operational"
534.00,"02","Meteorological sequences common to surface data","302046","(Temperature change)",,"012049","Temperature change over specified period","Temperature change over period specified",,"Operational"
535.00,"02","Meteorological sequences common to surface data","302047","(Direction of cloud drift)",,"102003","Replication descriptor","Replicate 2 descriptors 3 times",,"Operational"
536.00,"02","Meteorological sequences common to surface data","302047","(Direction of cloud drift)",,"008002","Vertical significance (surface observations)","Vertical significance",,"Operational"
537.00,"02","Meteorological sequences common to surface data","302047","(Direction of cloud drift)",,"020054","True direction from which a phenomenon or clouds are moving","True direction from which clouds are moving",,"Operational"
538.00,"02","Meteorological sequences common to surface data","302048","(Direction and elevation of cloud)",,"005021","Bearing or azimuth","Bearing or azimuth",,"Operational"
539.00,"02","Meteorological sequences common to surface data","302048","(Direction and elevation of cloud)",,"007021","Elevation","Elevation angle",,"Operational"
540.00,"02","Meteorological sequences common to surface data","302048","(Direction and elevation of cloud)",,"020012","Cloud type","Cloud type",,"Operational"
541.00,"02","Meteorological sequences common to surface data","302048","(Direction and elevation of cloud)",,"005021","Bearing or azimuth","Bearing or azimuth (= missing to cancel the previous value)",,"Operational"
542.00,"02","Meteorological sequences common to surface data","302048","(Direction and elevation of cloud)",,"007021","Elevation","Elevation angle (= missing to cancel the previous value)",,"Operational"
543.00,"02","Meteorological sequences common to surface data","302049","(Cloud information reported with vertical soundings)",,"008002","Vertical significance (surface observations)","Vertical significance",,"Operational"
544.00,"02","Meteorological sequences common to surface data","302049","(Cloud information reported with vertical soundings)",,"020011","Cloud amount","Cloud amount (of low or middle clouds Nh)",,"Operational"
545.00,"02","Meteorological sequences common to surface data","302049","(Cloud information reported with vertical soundings)",,"020013","Height of base of cloud","Height of cloud base (h)",,"Operational"
546.00,"02","Meteorological sequences common to surface data","302049","(Cloud information reported with vertical soundings)",,"020012","Cloud type","Cloud type (low clouds CL)",,"Operational"
547.00,"02","Meteorological sequences common to surface data","302049","(Cloud information reported with vertical soundings)",,"020012","Cloud type","Cloud type (middle clouds CM)",,"Operational"
548.00,"02","Meteorological sequences common to surface data","302049","(Cloud information reported with vertical soundings)",,"020012","Cloud type","Cloud type (high clouds CH)",,"Operational"
549.00,"02","Meteorological sequences common to surface data","302049","(Cloud information reported with vertical soundings)",,"008002","Vertical significance (surface observations)","Vertical significance (= missing value)",,"Operational"
550.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"008041","Data significance","Data significance (5 = sfc ob displacement from launch pt)",,"Operational"
551.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"005021","Bearing or azimuth","Bearing or azimuth",,"Operational"
552.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"007005","Height increment","Height increment",,"Operational"
553.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"202130","Change scale","Change scale",,"Operational"
554.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"006021","Distance","Distance",,"Operational"
555.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"202000","Change scale","Cancel change scale",,"Operational"
556.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"008041","Data significance","Data significance (4 = surface observation)",,"Operational"
557.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"201131","Change data width","Change data width",,"Operational"
558.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"202129","Change scale","Change scale",,"Operational"
559.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"002115","Type of surface observing equipment","Type of surface observing equipment",,"Operational"
560.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"010004","Pressure","Pressure",,"Operational"
561.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"002115","Type of surface observing equipment","Type of surface observing equipment",,"Operational"
562.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"013003","Relative humidity","Relative humidity",,"Operational"
563.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"202000","Change scale","Cancel change scale",,"Operational"
564.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"201000","Change data width","Cancel change data width",,"Operational"
565.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"002115","Type of surface observing equipment","Type of surface observing equipment",,"Operational"
566.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"011001","Wind direction","Wind direction",,"Operational"
567.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"011002","Wind speed","Wind speed",,"Operational"
568.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"002115","Type of surface observing equipment","Type of surface observing equipment",,"Operational"
569.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"102002","Replication descriptor","Replicate 2 descriptors 2 times",,"Operational"
570.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"012101","Temperature/air temperature","Temperature/air temperature",,"Operational"
571.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"004024","Time period or displacement","Time displacement (hour)",,"Operational"
572.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"002115","Type of surface observing equipment","Type of surface observing equipment",,"Operational"
573.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"012103","Dew-point temperature","Dew-point temperature",,"Operational"
574.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"012102","Wet-bulb temperature","Wet bulb temperature",,"Operational"
575.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"101003","Replication descriptor","Replicate 1 descriptor 3 times",,"Operational"
576.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"020012","Cloud type","Cloud type",,"Operational"
577.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"020011","Cloud amount","Cloud amount",,"Operational"
578.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"020013","Height of base of cloud","Height of cloud base",,"Operational"
579.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"101002","Replication descriptor","Replicate 1 descriptor 2 times",,"Operational"
580.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"020003","Present weather","Present weather",,"Operational"
581.00,"02","Meteorological sequences common to surface data","302051",,,"010004","Pressure","Pressure",,"Operational"
582.00,"02","Meteorological sequences common to surface data","302051",,,"010051","Pressure reduced to mean sea level","Pressure reduced to mean sea level",,"Operational"
583.00,"02","Meteorological sequences common to surface data","302051",,,"007004","Pressure","Pressure (vertical location)",,"Operational"
584.00,"02","Meteorological sequences common to surface data","302051",,,"010003","Geopotential","Geopotential",,"Operational"
585.00,"02","Meteorological sequences common to surface data","302051",,,"012004","Air temperature at 2 m","Air temperature at 2 m",,"Operational"
586.00,"02","Meteorological sequences common to surface data","302051",,,"012051","Standard deviation temperature","Standard deviation temperature",,"Operational"
587.00,"02","Meteorological sequences common to surface data","302051",,,"012016","Maximum temperature at 2 m, past 24 hours","Maximum temperature at 2 m, past 24 hours",,"Operational"
588.00,"02","Meteorological sequences common to surface data","302051",,,"012017","Minimum temperature at 2 m, past 24 hours","Minimum temperature at 2 m, past 24 hours",,"Operational"
589.00,"02","Meteorological sequences common to surface data","302051",,,"013004","Vapour pressure","Vapour pressure",,"Operational"
590.00,"02","Meteorological sequences common to surface data","302051",,,"102004","Replication descriptor","Replicate 2 descriptors 4 times",,"Operational"
591.00,"02","Meteorological sequences common to surface data","302051",,,"008051","Qualifier for number of missing values in calculation of statistic","Qualifier for number of missing values in calculation of statistic",,"Operational"
592.00,"02","Meteorological sequences common to surface data","302051",,,"008020","Total number of missing entities (with respect to accumulation or average)","Total number of missing entities (with respect to accumulation or average)",,"Operational"
593.00,"02","Meteorological sequences common to surface data","302052","(Ship temperature and humidity data)",,"007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above marine deck platform (for temperature and humidity measurement)",,"Operational"
594.00,"02","Meteorological sequences common to surface data","302052","(Ship temperature and humidity data)",,"007033","Height of sensor above water surface","Height of sensor above water surface (for temperature and humidity measurement)",,"Operational"
595.00,"02","Meteorological sequences common to surface data","302052","(Ship temperature and humidity data)",,"012101","Temperature/air temperature","Temperature/air temperature (scale 2)",,"Operational"
596.00,"02","Meteorological sequences common to surface data","302052","(Ship temperature and humidity data)",,"002039","Method of wet-bulb temperature measurement","Method of wet-bulb temperature measurement",,"Operational"
597.00,"02","Meteorological sequences common to surface data","302052","(Ship temperature and humidity data)",,"012102","Wet-bulb temperature","Wet-bulb temperature (scale 2)",,"Operational"
598.00,"02","Meteorological sequences common to surface data","302052","(Ship temperature and humidity data)",,"012103","Dew-point temperature","Dew-point temperature (scale 2)",,"Operational"
599.00,"02","Meteorological sequences common to surface data","302052","(Ship temperature and humidity data)",,"013003","Relative humidity","Relative humidity",,"Operational"
600.00,"02","Meteorological sequences common to surface data","302053","(Ship visibility data)",,"007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above marine deck platform (for visibility measurement)",,"Operational"
601.00,"02","Meteorological sequences common to surface data","302053","(Ship visibility data)",,"007033","Height of sensor above water surface","Height of sensor above water surface (for visibility measurement)",,"Operational"
602.00,"02","Meteorological sequences common to surface data","302053","(Ship visibility data)",,"020001","Horizontal visibility","Horizontal visibility",,"Operational"
603.00,"02","Meteorological sequences common to surface data","302054","(Ship ""instantaneous"" data)",,"302052","Ship temperature and humidity data","Temperature and humidity data",,"Operational"
604.00,"02","Meteorological sequences common to surface data","302054","(Ship ""instantaneous"" data)",,"302053","Ship visibility data","Visibility data",,"Operational"
605.00,"02","Meteorological sequences common to surface data","302054","(Ship ""instantaneous"" data)",,"007033","Height of sensor above water surface","Height of sensor above water surface (set to missing to cancel the previous value)",,"Operational"
606.00,"02","Meteorological sequences common to surface data","302054","(Ship ""instantaneous"" data)",,"302034","Precipitation past 24 hours","Precipitation past 24 hours",,"Operational"
607.00,"02","Meteorological sequences common to surface data","302054","(Ship ""instantaneous"" data)",,"007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above marine deck platform (set to missing to cancel the previous value)",,"Operational"
608.00,"02","Meteorological sequences common to surface data","302054","(Ship ""instantaneous"" data)",,"302004","General cloud information","Cloud data",,"Operational"
609.00,"02","Meteorological sequences common to surface data","302054","(Ship ""instantaneous"" data)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
610.00,"02","Meteorological sequences common to surface data","302054","(Ship ""instantaneous"" data)",,"031001","Delayed descriptor replication factor","Delayed descriptor replication factor",,"Operational"
611.00,"02","Meteorological sequences common to surface data","302054","(Ship ""instantaneous"" data)",,"302005",,"Cloud data",,"Operational"
612.00,"02","Meteorological sequences common to surface data","302055","(Icing and ice)",,"020031","Ice deposit (thickness)","Ice deposit (thickness)",,"Operational"
613.00,"02","Meteorological sequences common to surface data","302055","(Icing and ice)",,"020032","Rate of ice accretion","Rate of ice accretion",,"Operational"
614.00,"02","Meteorological sequences common to surface data","302055","(Icing and ice)",,"020033","Cause of ice accretion","Cause of ice accretion",,"Operational"
615.00,"02","Meteorological sequences common to surface data","302055","(Icing and ice)",,"020034","Sea ice concentration","Sea ice concentration",,"Operational"
616.00,"02","Meteorological sequences common to surface data","302055","(Icing and ice)",,"020035","Amount and type of ice","Amount and type of ice",,"Operational"
617.00,"02","Meteorological sequences common to surface data","302055","(Icing and ice)",,"020036","Ice situation","Ice situation",,"Operational"
618.00,"02","Meteorological sequences common to surface data","302055","(Icing and ice)",,"020037","Ice development","Ice development",,"Operational"
619.00,"02","Meteorological sequences common to surface data","302055","(Icing and ice)",,"020038","Bearing of ice edge","Bearing of ice edge",,"Operational"
620.00,"02","Meteorological sequences common to surface data","302056","(Sea/water temperature)",,"002038","Method of water temperature and/or salinity measurement","Method of sea/water temperature measurement",,"Operational"
621.00,"02","Meteorological sequences common to surface data","302056","(Sea/water temperature)",,"007063","Depth below sea/water surface (cm)","Depth below sea/water surface (for sea surface temperature measurement)",,"Operational"
622.00,"02","Meteorological sequences common to surface data","302056","(Sea/water temperature)",,"022043","Sea/water temperature","Sea/water temperature",,"Operational"
623.00,"02","Meteorological sequences common to surface data","302056","(Sea/water temperature)",,"007063","Depth below sea/water surface (cm)","Depth below sea/water surface (set to missing to cancel the previous value)",,"Operational"
624.00,"02","Meteorological sequences common to surface data","302057","(Ship marine data)",,"302056","Sea/water temperature","Sea surface temperature, method of measurement, and depth below sea surface",,"Operational"
625.00,"02","Meteorological sequences common to surface data","302057","(Ship marine data)",,"302021",,"Waves data",,"Operational"
626.00,"02","Meteorological sequences common to surface data","302057","(Ship marine data)",,"302024",,"Wind waves data",,"Operational"
627.00,"02","Meteorological sequences common to surface data","302058","(Ship extreme temperature data)",,"007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above marine deck platform (for temperature measurement)",,"Operational"
628.00,"02","Meteorological sequences common to surface data","302058","(Ship extreme temperature data)",,"007033","Height of sensor above water surface","Height of sensor above water surface (for temperature measurement)",,"Operational"
629.00,"02","Meteorological sequences common to surface data","302058","(Ship extreme temperature data)",,"004024","Time period or displacement","Time period or displacement",,"Operational"
630.00,"02","Meteorological sequences common to surface data","302058","(Ship extreme temperature data)",,"004024","Time period or displacement","Time period or displacement","(see Notes 1 and 2)","Operational"
631.00,"02","Meteorological sequences common to surface data","302058","(Ship extreme temperature data)",,"012111","Maximum temperature, at height and over period specified","Maximum temperature (scale 2) at height and over period specified",,"Operational"
632.00,"02","Meteorological sequences common to surface data","302058","(Ship extreme temperature data)",,"004024","Time period or displacement","Time period or displacement",,"Operational"
633.00,"02","Meteorological sequences common to surface data","302058","(Ship extreme temperature data)",,"004024","Time period or displacement","Time period or displacement","(see Note 2)","Operational"
634.00,"02","Meteorological sequences common to surface data","302058","(Ship extreme temperature data)",,"012112","Minimum temperature, at height and over period specified","Minimum temperature (scale 2) at height and over period specified",,"Operational"
635.00,"02","Meteorological sequences common to surface data","302059","(Ship wind data)",,"007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above marine deck platform (for wind measurement)",,"Operational"
636.00,"02","Meteorological sequences common to surface data","302059","(Ship wind data)",,"007033","Height of sensor above water surface","Height of sensor above water surface (for wind measurement)",,"Operational"
637.00,"02","Meteorological sequences common to surface data","302059","(Ship wind data)",,"002002","Type of instrumentation for wind measurement","Type of instrumentation for wind measurement",,"Operational"
638.00,"02","Meteorological sequences common to surface data","302059","(Ship wind data)",,"008021","Time significance","Time significance (= 2 (time averaged))",,"Operational"
639.00,"02","Meteorological sequences common to surface data","302059","(Ship wind data)",,"004025","Time period or displacement","Time period (= -10 minutes, or number of minutes after a significant change of wind)",,"Operational"
640.00,"02","Meteorological sequences common to surface data","302059","(Ship wind data)",,"011001","Wind direction","Wind direction",,"Operational"
641.00,"02","Meteorological sequences common to surface data","302059","(Ship wind data)",,"011002","Wind speed","Wind speed",,"Operational"
642.00,"02","Meteorological sequences common to surface data","302059","(Ship wind data)",,"008021","Time significance","Time significance (= missing value)",,"Operational"
643.00,"02","Meteorological sequences common to surface data","302059","(Ship wind data)",,"103002","Replication descriptor","Replicate next 3 descriptors 2 times",,"Operational"
644.00,"02","Meteorological sequences common to surface data","302059","(Ship wind data)",,"004025","Time period or displacement","Time period in minutes",,"Operational"
645.00,"02","Meteorological sequences common to surface data","302059","(Ship wind data)",,"011043","Maximum wind gust direction","Maximum wind gust direction",,"Operational"
646.00,"02","Meteorological sequences common to surface data","302059","(Ship wind data)",,"011041","Maximum wind gust speed","Maximum wind gust speed",,"Operational"
647.00,"02","Meteorological sequences common to surface data","302060","(Ship ""period"" data)",,"302038","Present and past weather","Present and past weather",,"Operational"
648.00,"02","Meteorological sequences common to surface data","302060","(Ship ""period"" data)",,"302040","Precipitation measurement","Precipitation measurement",,"Operational"
649.00,"02","Meteorological sequences common to surface data","302060","(Ship ""period"" data)",,"302058","Ship extreme temperature data","Ship extreme temperature data",,"Operational"
650.00,"02","Meteorological sequences common to surface data","302060","(Ship ""period"" data)",,"302059","Ship wind data","Ship wind data",,"Operational"
705.00,"02","Meteorological sequences common to surface data","302066","(Dangerous weather phenomena)",,"020023","Other weather phenomena","Other weather phenomena",,"Operational"
706.00,"02","Meteorological sequences common to surface data","302066","(Dangerous weather phenomena)",,"020024","Intensity of phenomena","Intensity of phenomena",,"Operational"
707.00,"02","Meteorological sequences common to surface data","302066","(Dangerous weather phenomena)",,"020027","Phenomena occurrence","Phenomenon occurrence",,"Operational"
708.00,"02","Meteorological sequences common to surface data","302066","(Dangerous weather phenomena)",,"020054","True direction from which a phenomenon or clouds are moving","True direction from which a phenomenon or clouds are moving",,"Operational"
709.00,"02","Meteorological sequences common to surface data","302066","(Dangerous weather phenomena)",,"020023","Other weather phenomena","Other weather phenomena",,"Operational"
710.00,"02","Meteorological sequences common to surface data","302066","(Dangerous weather phenomena)",,"020027","Phenomena occurrence","Phenomenon occurrence",,"Operational"
711.00,"02","Meteorological sequences common to surface data","302066","(Dangerous weather phenomena)",,"020054","True direction from which a phenomenon or clouds are moving","True direction from which a phenomenon or clouds are moving",,"Operational"
712.00,"02","Meteorological sequences common to surface data","302066","(Dangerous weather phenomena)",,"020025","Obscuration","Obscuration",,"Operational"
713.00,"02","Meteorological sequences common to surface data","302066","(Dangerous weather phenomena)",,"020026","Character of obscuration","Character of obscuration",,"Operational"
714.00,"02","Meteorological sequences common to surface data","302066","(Dangerous weather phenomena)",,"020027","Phenomena occurrence","Phenomenon occurrence",,"Operational"
715.00,"02","Meteorological sequences common to surface data","302066","(Dangerous weather phenomena)",,"020040","Evolution of drift snow","Evolution of drift of snow",,"Operational"
716.00,"02","Meteorological sequences common to surface data","302066","(Dangerous weather phenomena)",,"020066","Maximum diameter of hailstones","Maximum diameter of hailstones",,"Operational"
717.00,"02","Meteorological sequences common to surface data","302066","(Dangerous weather phenomena)",,"020027","Phenomena occurrence","Phenomenon occurrence",,"Operational"
718.00,"02","Meteorological sequences common to surface data","302066","(Dangerous weather phenomena)",,"020021","Type of precipitation","Type of precipitation",,"Operational"
719.00,"02","Meteorological sequences common to surface data","302066","(Dangerous weather phenomena)",,"020067","Diameter of deposit","Diameter of deposit",,"Operational"
720.00,"02","Meteorological sequences common to surface data","302066","(Dangerous weather phenomena)",,"020027","Phenomena occurrence","Phenomenon occurrence",,"Operational"
797.00,"02","Meteorological sequences common to surface data","302069","(Visibility data)",,"007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above local ground",,"Operational"
798.00,"02","Meteorological sequences common to surface data","302069","(Visibility data)",,"007033","Height of sensor above water surface","Height of sensor above water surface",,"Operational"
799.00,"02","Meteorological sequences common to surface data","302069","(Visibility data)",,"033041","Attribute of following value","Attribute of following value",,"Operational"
800.00,"02","Meteorological sequences common to surface data","302069","(Visibility data)",,"020001","Horizontal visibility","Horizontal visibility",,"Operational"
801.00,"02","Meteorological sequences common to surface data","302070","(Wind data)",,"007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above local ground",,"Operational"
802.00,"02","Meteorological sequences common to surface data","302070","(Wind data)",,"007033","Height of sensor above water surface","Height of sensor above water surface",,"Operational"
803.00,"02","Meteorological sequences common to surface data","302070","(Wind data)",,"011001","Wind direction","Wind direction",,"Operational"
804.00,"02","Meteorological sequences common to surface data","302070","(Wind data)",,"011002","Wind speed","Wind speed",,"Operational"
805.00,"02","Meteorological sequences common to surface data","302070","(Wind data)",,"011043","Maximum wind gust direction","Maximum wind gust direction",,"Operational"
806.00,"02","Meteorological sequences common to surface data","302070","(Wind data)",,"011041","Maximum wind gust speed","Maximum wind gust speed",,"Operational"
807.00,"02","Meteorological sequences common to surface data","302070","(Wind data)",,"011016","Extreme counterclockwise wind direction of a variable wind","Extreme counterclockwise wind direction of a variable wind",,"Operational"
808.00,"02","Meteorological sequences common to surface data","302070","(Wind data)",,"011017","Extreme clockwise wind direction of a variable wind","Extreme clockwise wind direction of a variable wind",,"Operational"
809.00,"02","Meteorological sequences common to surface data","302071","(Wind data from one-hour period)",,"007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above local ground",,"Operational"
810.00,"02","Meteorological sequences common to surface data","302071","(Wind data from one-hour period)",,"007033","Height of sensor above water surface","Height of sensor above water surface",,"Operational"
811.00,"02","Meteorological sequences common to surface data","302071","(Wind data from one-hour period)",,"008021","Time significance","Time significance (= 2 (time averaged))",,"Operational"
812.00,"02","Meteorological sequences common to surface data","302071","(Wind data from one-hour period)",,"004025","Time period or displacement","Time period (= -10 minutes, or number of minutes after a significant change of wind, if any)",,"Operational"
813.00,"02","Meteorological sequences common to surface data","302071","(Wind data from one-hour period)",,"011001","Wind direction","Wind direction",,"Operational"
814.00,"02","Meteorological sequences common to surface data","302071","(Wind data from one-hour period)",,"011002","Wind speed","Wind speed",,"Operational"
815.00,"02","Meteorological sequences common to surface data","302071","(Wind data from one-hour period)",,"008021","Time significance","Time significance (= missing value)",,"Operational"
816.00,"02","Meteorological sequences common to surface data","302071","(Wind data from one-hour period)",,"103002","Replication descriptor","Replicate next 3 descriptors 2 times",,"Operational"
817.00,"02","Meteorological sequences common to surface data","302071","(Wind data from one-hour period)",,"004025","Time period or displacement","Time period (= -10 minutes in the first replication, = -60 minutes in the second replication)",,"Operational"
818.00,"02","Meteorological sequences common to surface data","302071","(Wind data from one-hour period)",,"011043","Maximum wind gust direction","Maximum wind gust direction",,"Operational"
819.00,"02","Meteorological sequences common to surface data","302071","(Wind data from one-hour period)",,"011041","Maximum wind gust speed","Maximum wind gust speed",,"Operational"
820.00,"02","Meteorological sequences common to surface data","302071","(Wind data from one-hour period)",,"004025","Time period or displacement","Time period (= -10 minutes)",,"Operational"
821.00,"02","Meteorological sequences common to surface data","302071","(Wind data from one-hour period)",,"011016","Extreme counterclockwise wind direction of a variable wind","Extreme counterclockwise wind direction of a variable wind",,"Operational"
822.00,"02","Meteorological sequences common to surface data","302071","(Wind data from one-hour period)",,"011017","Extreme clockwise wind direction of a variable wind","Extreme clockwise wind direction of a variable wind",,"Operational"
823.00,"02","Meteorological sequences common to surface data","302072","(Temperature and humidity data)",,"007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above local ground",,"Operational"
824.00,"02","Meteorological sequences common to surface data","302072","(Temperature and humidity data)",,"007033","Height of sensor above water surface","Height of sensor above water surface",,"Operational"
825.00,"02","Meteorological sequences common to surface data","302072","(Temperature and humidity data)",,"012101","Temperature/air temperature","Temperature/air temperature (scale 2)",,"Operational"
826.00,"02","Meteorological sequences common to surface data","302072","(Temperature and humidity data)",,"012103","Dew-point temperature","Dew-point temperature  (scale 2)",,"Operational"
827.00,"02","Meteorological sequences common to surface data","302072","(Temperature and humidity data)",,"013003","Relative humidity","Relative humidity",,"Operational"
828.00,"02","Meteorological sequences common to surface data","302073","(Cloud data)",,"020010","Cloud cover (total)","Cloud cover (total)",,"Operational"
829.00,"02","Meteorological sequences common to surface data","302073","(Cloud data)",,"105004","Replication descriptor","Replicate 5 descriptors 4 times",,"Operational"
830.00,"02","Meteorological sequences common to surface data","302073","(Cloud data)",,"008002","Vertical significance (surface observations)","Vertical significance",,"Operational"
831.00,"02","Meteorological sequences common to surface data","302073","(Cloud data)",,"020011","Cloud amount","Cloud amount",,"Operational"
832.00,"02","Meteorological sequences common to surface data","302073","(Cloud data)",,"020012","Cloud type","Cloud type",,"Operational"
833.00,"02","Meteorological sequences common to surface data","302073","(Cloud data)",,"033041","Attribute of following value","Attribute of following value",,"Operational"
834.00,"02","Meteorological sequences common to surface data","302073","(Cloud data)",,"020013","Height of base of cloud","Height of base of cloud",,"Operational"
835.00,"02","Meteorological sequences common to surface data","302074","(Present and past weather)",,"020003","Present weather","Present weather",,"Operational"
836.00,"02","Meteorological sequences common to surface data","302074","(Present and past weather)",,"004025","Time period or displacement","Time period",,"Operational"
837.00,"02","Meteorological sequences common to surface data","302074","(Present and past weather)",,"020004","Past weather (1)","Past weather (1)",,"Operational"
838.00,"02","Meteorological sequences common to surface data","302074","(Present and past weather)",,"020005","Past weather (2)","Past weather (2)",,"Operational"
839.00,"02","Meteorological sequences common to surface data","302075","(Intensity of precipitation, size of precipitation element)",,"008021","Time significance","Time significance (= 2 (time averaged))",,"Operational"
840.00,"02","Meteorological sequences common to surface data","302075","(Intensity of precipitation, size of precipitation element)",,"004025","Time period or displacement","Time period (= -10 minutes)",,"Operational"
841.00,"02","Meteorological sequences common to surface data","302075","(Intensity of precipitation, size of precipitation element)",,"013055","Intensity of precipitation","Intensity of precipitation",,"Operational"
842.00,"02","Meteorological sequences common to surface data","302075","(Intensity of precipitation, size of precipitation element)",,"013058","Size of precipitating element","Size of precipitation element",,"Operational"
843.00,"02","Meteorological sequences common to surface data","302075","(Intensity of precipitation, size of precipitation element)",,"008021","Time significance","Time significance (= missing value)",,"Operational"
844.00,"02","Meteorological sequences common to surface data","302076","(Precipitation, obscuration and other phenomena)",,"020021","Type of precipitation","Type of precipitation",,"Operational"
845.00,"02","Meteorological sequences common to surface data","302076","(Precipitation, obscuration and other phenomena)",,"020022","Character of precipitation","Character of precipitation",,"Operational"
846.00,"02","Meteorological sequences common to surface data","302076","(Precipitation, obscuration and other phenomena)",,"026020","Duration of precipitation","Duration of precipitation",,"Operational"
847.00,"02","Meteorological sequences common to surface data","302076","(Precipitation, obscuration and other phenomena)",,"020023","Other weather phenomena","Other weather phenomena",,"Operational"
848.00,"02","Meteorological sequences common to surface data","302076","(Precipitation, obscuration and other phenomena)",,"020024","Intensity of phenomena","Intensity of phenomena",,"Operational"
849.00,"02","Meteorological sequences common to surface data","302076","(Precipitation, obscuration and other phenomena)",,"020025","Obscuration","Obscuration",,"Operational"
850.00,"02","Meteorological sequences common to surface data","302076","(Precipitation, obscuration and other phenomena)",,"020026","Character of obscuration","Character of obscuration",,"Operational"
851.00,"02","Meteorological sequences common to surface data","302077","(Extreme temperature data)",,"007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above local ground",,"Operational"
852.00,"02","Meteorological sequences common to surface data","302077","(Extreme temperature data)",,"007033","Height of sensor above water surface","Height of sensor above water surface",,"Operational"
853.00,"02","Meteorological sequences common to surface data","302077","(Extreme temperature data)",,"004025","Time period or displacement","Time period",,"Operational"
854.00,"02","Meteorological sequences common to surface data","302077","(Extreme temperature data)",,"012111","Maximum temperature, at height and over period specified","Maximum temperature (scale 2) at height and over period specified",,"Operational"
855.00,"02","Meteorological sequences common to surface data","302077","(Extreme temperature data)",,"012112","Minimum temperature, at height and over period specified","Minimum temperature (scale 2) at height and over period specified",,"Operational"
856.00,"02","Meteorological sequences common to surface data","302077","(Extreme temperature data)",,"007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above local ground (for ground temperature)",,"Operational"
857.00,"02","Meteorological sequences common to surface data","302077","(Extreme temperature data)",,"004025","Time period or displacement","Time period",,"Operational"
858.00,"02","Meteorological sequences common to surface data","302077","(Extreme temperature data)",,"012112","Minimum temperature, at height and over period specified","Minimum temperature (scale 2) at height and over period specified (for ground temperature)",,"Operational"
859.00,"02","Meteorological sequences common to surface data","302078","(State of ground and snow depth measurement)",,"002176","Method of state of ground measurement","Method of state of ground measurement",,"Operational"
860.00,"02","Meteorological sequences common to surface data","302078","(State of ground and snow depth measurement))",,"020062","State of the ground (with or without snow)","State of ground (with or without snow)",,"Operational"
861.00,"02","Meteorological sequences common to surface data","302078","(State of ground and snow depth measurement)",,"002177","Method of snow depth measurement","Method of snow depth measurement",,"Operational"
862.00,"02","Meteorological sequences common to surface data","302078","(State of ground and snow depth measurement)",,"013013","Total snow depth","Total snow depth",,"Operational"
863.00,"02","Meteorological sequences common to surface data","302079","(Precipitation measurement)",,"007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above local ground",,"Operational"
864.00,"02","Meteorological sequences common to surface data","302079","(Precipitation measurement)",,"002175","Method of precipitation measurement","Method of precipitation measurement",,"Operational"
865.00,"02","Meteorological sequences common to surface data","302079","(Precipitation measurement)",,"002178","Method of liquid content measurement of precipitation","Method of liquid water content measurement of precipitation",,"Operational"
866.00,"02","Meteorological sequences common to surface data","302079","(Precipitation measurement)",,"004025","Time period or displacement","Time period",,"Operational"
867.00,"02","Meteorological sequences common to surface data","302079","(Precipitation measurement)",,"013011","Total precipitation/total water equivalent","Total precipitation/total water equivalent of snow",,"Operational"
868.00,"02","Meteorological sequences common to surface data","302080","(Evaporation measurement)",,"002185","Method of evaporation measurement","Method of evaporation measurement",,"Operational"
869.00,"02","Meteorological sequences common to surface data","302080","(Evaporation measurement)",,"004025","Time period or displacement","Time period",,"Operational"
870.00,"02","Meteorological sequences common to surface data","302080","(Evaporation measurement)",,"013033","Evaporation/evapotranspiration","Evaporation/evapotranspiration",,"Operational"
871.00,"02","Meteorological sequences common to surface data","302081","(Total sunshine data)",,"004025","Time period or displacement","Time period",,"Operational"
872.00,"02","Meteorological sequences common to surface data","302081","(Total sunshine data)",,"014031","Total sunshine","Total sunshine",,"Operational"
873.00,"02","Meteorological sequences common to surface data","302082","(Radiation data)",,"004025","Time period or displacement","Time period",,"Operational"
874.00,"02","Meteorological sequences common to surface data","302082","(Radiation data)",,"014002","Long-wave radiation, integrated over period specified","Long-wave radiation, integrated over period specified",,"Operational"
875.00,"02","Meteorological sequences common to surface data","302082","(Radiation data)",,"014004","Short-wave radiation, integrated over period specified","Short-wave radiation, integrated over period specified",,"Operational"
876.00,"02","Meteorological sequences common to surface data","302082","(Radiation data)",,"014016","Net radiation, integrated over period specified","Net radiation, integrated over period specified",,"Operational"
877.00,"02","Meteorological sequences common to surface data","302082","(Radiation data)",,"014028","Global solar radiation (high accuracy), integrated over period specified","Global solar radiation (high accuracy), integrated over period specified",,"Operational"
878.00,"02","Meteorological sequences common to surface data","302082","(Radiation data)",,"014029","Diffuse solar radiation (high accuracy), integrated over period specified","Diffuse solar radiation (high accuracy), integrated over period specified",,"Operational"
879.00,"02","Meteorological sequences common to surface data","302082","(Radiation data)",,"014030","Direct solar radiation (high accuracy), integrated over period specified","Direct solar radiation (high accuracy), integrated over period specified",,"Operational"
880.00,"02","Meteorological sequences common to surface data","302083","(First-order statistics of P, W, T, U data)",,"004025","Time period or displacement","Time period",,"Operational"
881.00,"02","Meteorological sequences common to surface data","302083","(First-order statistics of P, W, T, U data)",,"008023","First-order statistics","First-order statistics",,"Operational"
882.00,"02","Meteorological sequences common to surface data","302083","(First-order statistics of P, W, T, U data)",,"010004","Pressure","Pressure",,"Operational"
883.00,"02","Meteorological sequences common to surface data","302083","(First-order statistics of P, W, T, U data)",,"011001","Wind direction","Wind direction",,"Operational"
884.00,"02","Meteorological sequences common to surface data","302083","(First-order statistics of P, W, T, U data)",,"011002","Wind speed","Wind speed",,"Operational"
885.00,"02","Meteorological sequences common to surface data","302083","(First-order statistics of P, W, T, U data)",,"012101","Temperature/air temperature","Temperature/air temperature (scale 2)",,"Operational"
886.00,"02","Meteorological sequences common to surface data","302083","(First-order statistics of P, W, T, U data)",,"013003","Relative humidity","Relative humidity",,"Operational"
887.00,"02","Meteorological sequences common to surface data","302083","(First-order statistics of P, W, T, U data)",,"008023","First-order statistics","First-order statistics (= missing value)",,"Operational"
888.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)",,"302031","Pressure information","Pressure information",,"Operational"
889.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)",,"302072","Temperature and humidity data","Temperature and humidity data",,"Operational"
890.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)",,"103000","Replication descriptor","Delayed replication of 3 descriptors",,"Operational"
891.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)",,"031000","Short delayed descriptor replication factor","Short delayed descriptor replication factor",,"Operational"
892.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)",,"101005","Replication descriptor","Replicate 1 descriptor 5 times",,"Operational"
893.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)",,"307063",,"Soil temperature",,"Operational"
894.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)",,"007061","Depth below land surface","Depth below land surface (set to missing to cancel the previous value)",,"Operational"
895.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Visibility data","101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
896.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Visibility data","031000","Short delayed descriptor replication factor","Short delayed descriptor replication factor",,"Operational"
897.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Visibility data","302069","Visibility data","Visibility data",,"Operational"
898.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Visibility data","007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above local ground (set to missing to cancel the previous value)",,"Operational"
899.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Visibility data","007033","Height of sensor above water surface","Height of sensor above water surface (set to missing to cancel the previous value)",,"Operational"
900.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Marine data","105000","Replication descriptor","Delayed replication of 5 descriptors",,"Operational"
901.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Marine data","031000","Short delayed descriptor replication factor","Short delayed descriptor replication factor",,"Operational"
902.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Marine data","020031","Ice deposit (thickness)","Ice deposit (thickness)",,"Operational"
903.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Marine data","020032","Rate of ice accretion","Rate of ice accretion",,"Operational"
904.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Marine data","002038","Method of water temperature and/or salinity measurement","Method of sea surface temperature measurement",,"Operational"
905.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Marine data","022043","Sea/water temperature","Sea/water temperature (scale 2)",,"Operational"
906.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Marine data","302021",,"Wave data",,"Operational"
907.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","State of ground and snow depth measurement","101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
908.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","State of ground and snow depth measurement","031000","Short delayed descriptor replication factor","Short delayed descriptor replication factor",,"Operational"
909.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","State of ground and snow depth measurement","302078","State of ground and snow depth measurement","State of ground and snow depth measurement",,"Operational"
910.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","State of ground and snow depth measurement","012113","Ground minimum temperature, past 12 hours","Ground minimum temperature (scale 2), past 12 hours",,"Operational"
911.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Cloud data","101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
912.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Cloud data","031000","Short delayed descriptor replication factor","Short delayed descriptor replication factor",,"Operational"
913.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Cloud data","302004","General cloud information","General cloud information",,"Operational"
914.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Cloud data","105000","Replication descriptor","Delayed replication of 5 descriptors",,"Operational"
915.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Cloud data","031001","Delayed descriptor replication factor","Delayed descriptor replication factor",,"Operational"
916.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Cloud data","008002","Vertical significance (surface observations)","Vertical significance",,"Operational"
917.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Cloud data","020011","Cloud amount","Cloud amount",,"Operational"
918.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Cloud data","020012","Cloud type","Cloud type",,"Operational"
919.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Cloud data","033041","Attribute of following value","Attribute of following value",,"Operational"
920.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Cloud data","020013","Height of base of cloud","Height of base of cloud",,"Operational"
921.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Cloud data","302036","Clouds with bases below station level","Clouds with bases below station level",,"Operational"
922.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Direction of cloud drift 6DLDMDH","101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
923.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Direction of cloud drift 6DLDMDH","031000","Short delayed descriptor replication factor","Short delayed descriptor replication factor",,"Operational"
924.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Direction of cloud drift 6DLDMDH","302047","Direction of cloud drift","Direction of cloud drift",,"Operational"
925.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Direction of cloud drift 6DLDMDH","008002","Vertical significance (surface observations)","Vertical significance (set to missing to cancel the previous value)",,"Operational"
926.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Direction and elevation of cloud 57CDaec","101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
927.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Direction and elevation of cloud 57CDaec","031000","Short delayed descriptor replication factor","Short delayed descriptor replication factor",,"Operational"
928.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Direction and elevation of cloud 57CDaec","302048","Direction and elevation of cloud","Direction and elevation of cloud",,"Operational"
929.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Present and past weather data","105000","Replication descriptor","Delayed replication of 5 descriptors",,"Operational"
930.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Present and past weather data","031000","Short delayed descriptor replication factor","Short delayed descriptor replication factor",,"Operational"
931.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Present and past weather data","020003","Present weather","Present weather",,"Operational"
932.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Present and past weather data","103002","Replication descriptor","Replicate 3 descriptors 2 times",,"Operational"
933.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Present and past weather data","004024","Time period or displacement","Time period (= -1 hour in 1. replication, -x hours in 2. replication,  x corresponding to the time period of W1W2 in the SYNOP report)",,"Operational"
934.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Present and past weather data","020004","Past weather (1)","Past weather (1)",,"Operational"
935.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Present and past weather data","020005","Past weather (2)","Past weather (2)",,"Operational"
936.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Intensity of precipitation, size of precipitation element","101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
937.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Intensity of precipitation, size of precipitation element","031000","Short delayed descriptor replication factor","Short delayed descriptor replication factor",,"Operational"
938.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Intensity of precipitation, size of precipitation element","302175",,"Intensity of precipitation, size of precipitation element",,"Operational"
939.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Precipitation, obscuration and other phenomena","102000","Replication descriptor","Delayed replication of 2 descriptors",,"Operational"
940.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Precipitation, obscuration and other phenomena","031000","Short delayed descriptor replication factor","Short delayed descriptor replication factor",,"Operational"
941.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Precipitation, obscuration and other phenomena","004025","Time period or displacement","Time period (= -10 minutes)",,"Operational"
942.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Precipitation, obscuration and other phenomena","302076","Precipitation, obscuration and other phenomena","Precipitation, obscuration and other phenomena",,"Operational"
943.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Lightning data","102000","Replication descriptor","Delayed replication of 2 descriptors",,"Operational"
944.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Lightning data","031000","Short delayed descriptor replication factor","Short delayed descriptor replication factor",,"Operational"
945.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Lightning data","004025","Time period or displacement","Time period (= -10 minutes)",,"Operational"
946.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Lightning data","013059","Number of flashes (thunderstorm)","Number of flashes",,"Operational"
947.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Wind data","007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above local ground",,"Operational"
948.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Wind data","007033","Height of sensor above water surface","Height of sensor above water surface",,"Operational"
949.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Wind data","008021","Time significance","Time significance (= 2 (time averaged))",,"Operational"
950.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Wind data","004025","Time period or displacement","Time period (= -10 minutes, or number of minutes after a significant change of wind)",,"Operational"
951.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Wind data","011001","Wind direction","Wind direction",,"Operational"
952.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Wind data","011002","Wind speed","Wind speed",,"Operational"
953.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Wind data","008021","Time significance","Time significance (= missing value)",,"Operational"
954.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Wind data","103003","Replication descriptor","Replicate next 3 descriptors 3 times",,"Operational"
955.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Wind data","004025","Time period or displacement","Time period (= -10 minutes in 1. replication,= -60 minutes in 2. replication,= -60x3 or 60x6 minutes in 3. replication)",,"Operational"
956.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Wind data","011043","Maximum wind gust direction","Maximum wind gust direction",,"Operational"
957.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Wind data","011041","Maximum wind gust speed","Maximum wind gust speed",,"Operational"
958.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Wind data","004025","Time period or displacement","Time period (= -10 minutes)",,"Operational"
959.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Wind data","011016","Extreme counterclockwise wind direction of a variable wind","Extreme counterclockwise wind direction of a variable wind",,"Operational"
960.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Wind data","011017","Extreme clockwise wind direction of a variable wind","Extreme clockwise wind direction of a variable wind",,"Operational"
961.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Extreme temperature data","302077","Extreme temperature data","Extreme temperature data",,"Operational"
962.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Extreme temperature data","007033","Height of sensor above water surface","Height of sensor above water surface (set to missing to cancel the previous value)",,"Operational"
963.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Extreme temperature data","302041","Extreme temperature data","Extreme temperature data",,"Operational"
964.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Precipitation measurement","106000","Replication descriptor","Delayed replication of 6 descriptors",,"Operational"
965.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Precipitation measurement","031000","Short delayed descriptor replication factor","Short delayed descriptor replication factor",,"Operational"
966.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Precipitation measurement","007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above local ground",,"Operational"
967.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Precipitation measurement","002175","Method of precipitation measurement","Method of precipitation measurement",,"Operational"
968.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Precipitation measurement","002178","Method of liquid content measurement of precipitation","Method of liquid water content measurement of precipitation",,"Operational"
969.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Precipitation measurement","102005","Replication descriptor","Replicate 2 descriptors 5 times",,"Operational"
970.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Precipitation measurement","004024","Time period or displacement","Time period in hours (= -1 hour in the first replication,= -3, -6, -12 and - 24 hours in the other replications)",,"Operational"
971.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Precipitation measurement","013011","Total precipitation/total water equivalent","Total precipitation / total water equivalent of snow",,"Operational"
972.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Precipitation measurement","007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above local ground (set to missing to cancel the previous value)",,"Operational"
973.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Evaporation data","103000","Replication descriptor","Delayed replication of 3 descriptors",,"Operational"
974.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Evaporation data","031000","Short delayed descriptor replication factor","Short delayed descriptor replication factor",,"Operational"
975.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Evaporation data","002185","Method of evaporation measurement","Method of evaporation measurement",,"Operational"
976.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Evaporation data","101002","Replication descriptor","Replicate 1 descriptor 2 times",,"Operational"
977.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Evaporation data","302044","Evaporation data","Evaporation data",,"Operational"
978.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Total sunshine data","102000","Replication descriptor","Delayed replication of 2 descriptors",,"Operational"
979.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Total sunshine data","031000","Short delayed descriptor replication factor","Short delayed descriptor replication factor",,"Operational"
980.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Total sunshine data","101002","Replication descriptor","Replicate 1 descriptor 2 times",,"Operational"
981.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Total sunshine data","302039","Sunshine data (from 1 hour and 24 hour period)","Sunshine data (from 1 hour and 24 hour period)",,"Operational"
982.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Radiation data","102000","Replication descriptor","Delayed replication of 2 descriptors",,"Operational"
983.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Radiation data","031000","Short delayed descriptor replication factor","Short delayed descriptor replication factor",,"Operational"
984.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Radiation data","101002","Replication descriptor","Replicate 1 descriptor 2 times",,"Operational"
985.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Radiation data","302045","Radiation data (from 1 hour and 24 hour period)","Radiation data (from 1 hour and 24 hour period)",,"Operational"
986.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Temperature change group 54g0sndT","101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
987.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Temperature change group 54g0sndT","031000","Short delayed descriptor replication factor","Short delayed descriptor replication factor",,"Operational"
988.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Temperature change group 54g0sndT","302046","Temperature change","Temperature change",,"Operational"
989.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","First-order statistics of P, W, T, U data","101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
990.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","First-order statistics of P, W, T, U data","031000","Short delayed descriptor replication factor","Short delayed descriptor replication factor",,"Operational"
991.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","First-order statistics of P, W, T, U data","302083","First-order statistics of P, W, T, U data","First-order statistics of P, W, T, U data",,"Operational"
992.00,"02","Meteorological sequences common to surface data","302089","(Locust information)",,"020101","Locust (acridian) name","Locust (acridian) name                                                     Ln",,"Operational"
993.00,"02","Meteorological sequences common to surface data","302089","(Locust information)",,"020102","Locust (maturity) colour","Locust (maturity) colour                                                      Lc",,"Operational"
994.00,"02","Meteorological sequences common to surface data","302089","(Locust information)",,"020103","Stage of development of locusts","Stage of development of locusts                                  Ld",,"Operational"
995.00,"02","Meteorological sequences common to surface data","302089","(Locust information)",,"020104","Organization state of swarm or band of locusts","Organization state of swarm or band of locusts      Lg",,"Operational"
996.00,"02","Meteorological sequences common to surface data","302089","(Locust information)",,"020105","Size of swarm or band of locusts and duration of passage of swarm","Size of swarm or band of locusts and duration of passage of swarm    sL",,"Operational"
997.00,"02","Meteorological sequences common to surface data","302089","(Locust information)",,"020106","Locust population density","Locust population density                                             dL",,"Operational"
998.00,"02","Meteorological sequences common to surface data","302089","(Locust information)",,"020107","Direction of movements of locust swarm","Direction of movements of locust swarm                 DL",,"Operational"
999.00,"02","Meteorological sequences common to surface data","302089","(Locust information)",,"020108","Extent of vegetation","Extent of vegetation                                                        ve",,"Operational"
1004.00,"02","Meteorological sequences common to surface data","302175",,,"008021","Time significance","Time significance",,"Operational"
1005.00,"02","Meteorological sequences common to surface data","302175",,,"004025","Time period or displacement","Time period or displacement",,"Operational"
1006.00,"02","Meteorological sequences common to surface data","302175",,,"013155","Intensity of precipitation (high accuracy)","Intensity of precipitation (high accuracy)",,"Operational"
1007.00,"02","Meteorological sequences common to surface data","302175",,,"013058","Size of precipitating element","Size of precipitating element",,"Operational"
1008.00,"02","Meteorological sequences common to surface data","302175",,,"008021","Time significance","Time significance",,"Operational"
1009.00,"03","Meteorological sequences common to vertical soundings data","303001",,,"007003","Geopotential","Geopotential",,"Operational"
1010.00,"03","Meteorological sequences common to vertical soundings data","303001",,,"011001","Wind direction","Wind direction",,"Operational"
1011.00,"03","Meteorological sequences common to vertical soundings data","303001",,,"011002","Wind speed","Wind speed",,"Operational"
1012.00,"03","Meteorological sequences common to vertical soundings data","303002",,,"007004","Pressure","Pressure",,"Operational"
1013.00,"03","Meteorological sequences common to vertical soundings data","303002",,,"011001","Wind direction","Wind direction",,"Operational"
1014.00,"03","Meteorological sequences common to vertical soundings data","303002",,,"011002","Wind speed","Wind speed",,"Operational"
1015.00,"03","Meteorological sequences common to vertical soundings data","303003",,,"007004","Pressure","Pressure",,"Operational"
1016.00,"03","Meteorological sequences common to vertical soundings data","303003",,,"010003","Geopotential","Geopotential",,"Operational"
1017.00,"03","Meteorological sequences common to vertical soundings data","303003",,,"012001","Temperature/air temperature","Temperature",,"Operational"
1018.00,"03","Meteorological sequences common to vertical soundings data","303003",,,"012003","Dew-point temperature","Dew point",,"Operational"
1019.00,"03","Meteorological sequences common to vertical soundings data","303004",,,"007004","Pressure","Pressure",,"Operational"
1020.00,"03","Meteorological sequences common to vertical soundings data","303004",,,"010003","Geopotential","Geopotential",,"Operational"
1021.00,"03","Meteorological sequences common to vertical soundings data","303004",,,"012001","Temperature/air temperature","Temperature",,"Operational"
1022.00,"03","Meteorological sequences common to vertical soundings data","303004",,,"012003","Dew-point temperature","Dew point",,"Operational"
1023.00,"03","Meteorological sequences common to vertical soundings data","303004",,,"011001","Wind direction","Wind direction",,"Operational"
1024.00,"03","Meteorological sequences common to vertical soundings data","303004",,,"011002","Wind speed","Wind speed",,"Operational"
1025.00,"03","Meteorological sequences common to vertical soundings data","303011",,,"007003","Geopotential","Geopotential",,"Operational"
1026.00,"03","Meteorological sequences common to vertical soundings data","303011",,,"008001","Vertical sounding significance","Vertical sounding significance",,"Operational"
1027.00,"03","Meteorological sequences common to vertical soundings data","303011",,,"011001","Wind direction","Wind direction",,"Operational"
1028.00,"03","Meteorological sequences common to vertical soundings data","303011",,,"011002","Wind speed","Wind speed",,"Operational"
1029.00,"03","Meteorological sequences common to vertical soundings data","303012",,,"007004","Pressure","Pressure",,"Operational"
1030.00,"03","Meteorological sequences common to vertical soundings data","303012",,,"008001","Vertical sounding significance","Vertical sounding significance",,"Operational"
1031.00,"03","Meteorological sequences common to vertical soundings data","303012",,,"011001","Wind direction","Wind direction",,"Operational"
1032.00,"03","Meteorological sequences common to vertical soundings data","303012",,,"011002","Wind speed","Wind speed",,"Operational"
1033.00,"03","Meteorological sequences common to vertical soundings data","303013",,,"007004","Pressure","Pressure",,"Operational"
1034.00,"03","Meteorological sequences common to vertical soundings data","303013",,,"008001","Vertical sounding significance","Vertical sounding significance",,"Operational"
1035.00,"03","Meteorological sequences common to vertical soundings data","303013",,,"010003","Geopotential","Geopotential",,"Operational"
1036.00,"03","Meteorological sequences common to vertical soundings data","303013",,,"012001","Temperature/air temperature","Temperature",,"Operational"
1037.00,"03","Meteorological sequences common to vertical soundings data","303013",,,"013003","Relative humidity","Relative humidity",,"Operational"
1038.00,"03","Meteorological sequences common to vertical soundings data","303013",,,"011001","Wind direction","Wind direction",,"Operational"
1039.00,"03","Meteorological sequences common to vertical soundings data","303013",,,"011002","Wind speed","Wind speed",,"Operational"
1040.00,"03","Meteorological sequences common to vertical soundings data","303014",,,"007004","Pressure","Pressure",,"Operational"
1041.00,"03","Meteorological sequences common to vertical soundings data","303014",,,"008001","Vertical sounding significance","Vertical sounding significance",,"Operational"
1042.00,"03","Meteorological sequences common to vertical soundings data","303014",,,"010003","Geopotential","Geopotential",,"Operational"
1043.00,"03","Meteorological sequences common to vertical soundings data","303014",,,"012001","Temperature/air temperature","Temperature",,"Operational"
1044.00,"03","Meteorological sequences common to vertical soundings data","303014",,,"012003","Dew-point temperature","Dew point",,"Operational"
1045.00,"03","Meteorological sequences common to vertical soundings data","303014",,,"011001","Wind direction","Wind direction",,"Operational"
1046.00,"03","Meteorological sequences common to vertical soundings data","303014",,,"011002","Wind speed","Wind speed",,"Operational"
1047.00,"03","Meteorological sequences common to vertical soundings data","303021",,,"007004","Pressure","Pressure (1)     defines layer",,"Operational"
1048.00,"03","Meteorological sequences common to vertical soundings data","303021",,,"007004","Pressure","Pressure (2)     defines layer",,"Operational"
1049.00,"03","Meteorological sequences common to vertical soundings data","303021",,,"204007","Add associated field","Add associated field of 7 bits",,"Operational"
1050.00,"03","Meteorological sequences common to vertical soundings data","303021",,,"031021","Associated field significance","Additional field significance",,"Operational"
1051.00,"03","Meteorological sequences common to vertical soundings data","303022",,,"303021",,"Layer, quality",,"Operational"
1052.00,"03","Meteorological sequences common to vertical soundings data","303022",,,"010003","Geopotential","Geopotential (layer mean thickness)",,"Operational"
1053.00,"03","Meteorological sequences common to vertical soundings data","303022",,,"204000","Added associated field","Cancel the added associated field",,"Operational"
1054.00,"03","Meteorological sequences common to vertical soundings data","303023",,,"303021",,"Layer, quality",,"Operational"
1055.00,"03","Meteorological sequences common to vertical soundings data","303023",,,"012001","Temperature/air temperature","Temperature (layer mean)",,"Operational"
1056.00,"03","Meteorological sequences common to vertical soundings data","303023",,,"204000","Added associated field","Cancel the added associated field",,"Operational"
1057.00,"03","Meteorological sequences common to vertical soundings data","303024",,,"303021",,"Layer, quality",,"Operational"
1058.00,"03","Meteorological sequences common to vertical soundings data","303024",,,"013016","Precipitable water","Precipitation water",,"Operational"
1059.00,"03","Meteorological sequences common to vertical soundings data","303024",,,"204000","Added associated field","Cancel the added associated field",,"Operational"
1060.00,"03","Meteorological sequences common to vertical soundings data","303025",,,"002025","Satellite channel(s) used in computation","Satellite channel",,"Operational"
1061.00,"03","Meteorological sequences common to vertical soundings data","303025",,,"204007","Add associated field","Add associated field of 7 bits",,"Operational"
1062.00,"03","Meteorological sequences common to vertical soundings data","303025",,,"031021","Associated field significance","Additional field significance",,"Operational"
1063.00,"03","Meteorological sequences common to vertical soundings data","303025",,,"012063","Brightness temperature","Brightness temperature",,"Operational"
1064.00,"03","Meteorological sequences common to vertical soundings data","303025",,,"204000","Added associated field","Cancel the added associated field",,"Operational"
1065.00,"03","Meteorological sequences common to vertical soundings data","303026",,,"007004","Pressure","Pressure",,"Operational"
1066.00,"03","Meteorological sequences common to vertical soundings data","303026",,,"008003","Vertical significance (satellite observations)","Vertical significance",,"Operational"
1067.00,"03","Meteorological sequences common to vertical soundings data","303026",,,"204007","Add associated field","Add associated field of 7 bits",,"Operational"
1068.00,"03","Meteorological sequences common to vertical soundings data","303026",,,"031021","Associated field significance","Additional field significance",,"Operational"
1069.00,"03","Meteorological sequences common to vertical soundings data","303026",,,"012001","Temperature/air temperature","Temperature",,"Operational"
1070.00,"03","Meteorological sequences common to vertical soundings data","303026",,,"204000","Add associated field","Cancel the added associated field",,"Operational"
1071.00,"03","Meteorological sequences common to vertical soundings data","303027",,,"007004","Pressure","Pressure",,"Operational"
1072.00,"03","Meteorological sequences common to vertical soundings data","303027",,,"204007","Add associated field","Add associated field of 7 bits",,"Operational"
1073.00,"03","Meteorological sequences common to vertical soundings data","303027",,,"031021","Associated field significance","Additional field significance",,"Operational"
1074.00,"03","Meteorological sequences common to vertical soundings data","303027",,,"010003","Geopotential","Geopotential",,"Operational"
1075.00,"03","Meteorological sequences common to vertical soundings data","303027",,,"204000","Add associated field","Cancel the added associated field",,"Operational"
1076.00,"03","Meteorological sequences common to vertical soundings data","303031",,,"007004","Pressure","Pressure",,"Operational"
1077.00,"03","Meteorological sequences common to vertical soundings data","303031",,,"008003","Vertical significance (satellite observations)","Vertical significance (base of sounding)",,"Operational"
1078.00,"03","Meteorological sequences common to vertical soundings data","303031",,,"007021","Elevation","Elevation (local zenith)",,"Operational"
1079.00,"03","Meteorological sequences common to vertical soundings data","303031",,,"007022","Solar elevation","Solar elevation (solar zenith)",,"Operational"
1080.00,"03","Meteorological sequences common to vertical soundings data","303031",,,"008012","Land/sea qualifier","Land/sea qualifier",,"Operational"
1081.00,"03","Meteorological sequences common to vertical soundings data","303031",,,"012061","Skin temperature","Skin temperature",,"Operational"
1082.00,"03","Meteorological sequences common to vertical soundings data","303032",,,"020011","Cloud amount","Cloud amount",,"Operational"
1083.00,"03","Meteorological sequences common to vertical soundings data","303032",,,"020016","Pressure at top of cloud","Pressure at top of cloud",,"Operational"
1084.00,"03","Meteorological sequences common to vertical soundings data","303033",,,"020010","Cloud cover (total)","Cloud cover (total)",,"Operational"
1085.00,"03","Meteorological sequences common to vertical soundings data","303033",,,"020016","Pressure at top of cloud","Pressure at the top of cloud",,"Operational"
1086.00,"03","Meteorological sequences common to vertical soundings data","303040","(Radiosonde duration of flight and termination information)",,"008041","Data significance","Data significance (7 = Flight level termination point)",,"Operational"
1087.00,"03","Meteorological sequences common to vertical soundings data","303040","(Radiosonde duration of flight and termination information)",,"004025","Time period or displacement","Time displacement (minute)",,"Operational"
1088.00,"03","Meteorological sequences common to vertical soundings data","303040","(Radiosonde duration of flight and termination information)",,"004026","Time period or displacement","Time displacement (second)",,"Operational"
1089.00,"03","Meteorological sequences common to vertical soundings data","303040","(Radiosonde duration of flight and termination information)",,"301021",,"Latitude and longitude (high accuracy)",,"Operational"
1090.00,"03","Meteorological sequences common to vertical soundings data","303040","(Radiosonde duration of flight and termination information)",,"301122","Date/time (to hundredths of second) (see Note 3)","Date/time (to hundredths of second)",,"Operational"
1091.00,"03","Meteorological sequences common to vertical soundings data","303040","(Radiosonde duration of flight and termination information)",,"201131","Change data width","Change data width",,"Operational"
1092.00,"03","Meteorological sequences common to vertical soundings data","303040","(Radiosonde duration of flight and termination information)",,"202129","Change scale","Change scale",,"Operational"
1093.00,"03","Meteorological sequences common to vertical soundings data","303040","(Radiosonde duration of flight and termination information)",,"025069","Flight level pressure corrections","Flight level pressure correction",,"Operational"
1094.00,"03","Meteorological sequences common to vertical soundings data","303040","(Radiosonde duration of flight and termination information)",,"007004","Pressure","Pressure",,"Operational"
1095.00,"03","Meteorological sequences common to vertical soundings data","303040","(Radiosonde duration of flight and termination information)",,"013003","Relative humidity","Relative humidity",,"Operational"
1096.00,"03","Meteorological sequences common to vertical soundings data","303040","(Radiosonde duration of flight and termination information)",,"202000","Change scale","Cancel change scale",,"Operational"
1097.00,"03","Meteorological sequences common to vertical soundings data","303040","(Radiosonde duration of flight and termination information)",,"201000","Change data width","Cancel change data width",,"Operational"
1098.00,"03","Meteorological sequences common to vertical soundings data","303040","(Radiosonde duration of flight and termination information)",,"002013","Solar and infrared radiation correction","Solar and infrared radiation correction",,"Operational"
1099.00,"03","Meteorological sequences common to vertical soundings data","303040","(Radiosonde duration of flight and termination information)",,"012101","Temperature/air temperature","Temperature/air temperature",,"Operational"
1100.00,"03","Meteorological sequences common to vertical soundings data","303040","(Radiosonde duration of flight and termination information)",,"010009","Geopotential height","Geopotential height",,"Operational"
1101.00,"03","Meteorological sequences common to vertical soundings data","303040","(Radiosonde duration of flight and termination information)",,"102002","Replication descriptor","Replicate 2 descriptors 2 times",,"Operational"
1102.00,"03","Meteorological sequences common to vertical soundings data","303040","(Radiosonde duration of flight and termination information)",,"008040","Flight Level significance","Flight level significance",,"Operational"
1103.00,"03","Meteorological sequences common to vertical soundings data","303040","(Radiosonde duration of flight and termination information)",,"035035","Reason for termination","Reason for termination",,"Operational"
1104.00,"03","Meteorological sequences common to vertical soundings data","303041","(Wind sequence)",,"002152","Satellite instrument used in data processing","Geostationary satellite instrument used",,"Operational"
1105.00,"03","Meteorological sequences common to vertical soundings data","303041","(Wind sequence)",,"002023","Satellite derived wind computation method","Cloud motion computational method",,"Operational"
1106.00,"03","Meteorological sequences common to vertical soundings data","303041","(Wind sequence)",,"007004","Pressure","Pressure",,"Operational"
1107.00,"03","Meteorological sequences common to vertical soundings data","303041","(Wind sequence)",,"011001","Wind direction","Wind direction",,"Operational"
1108.00,"03","Meteorological sequences common to vertical soundings data","303041","(Wind sequence)",,"011002","Wind speed","Wind speed",,"Operational"
1109.00,"03","Meteorological sequences common to vertical soundings data","303041","(Wind sequence)",,"002153","Satellite channel centre frequency","Satellite channel centre frequency",,"Operational"
1110.00,"03","Meteorological sequences common to vertical soundings data","303041","(Wind sequence)",,"002154","Satellite channel band width","Satellite channel band width",,"Operational"
1111.00,"03","Meteorological sequences common to vertical soundings data","303041","(Wind sequence)",,"012071","Coldest cluster temperature","Coldest cluster T",,"Operational"
1112.00,"03","Meteorological sequences common to vertical soundings data","303050","(Wind data at a pressure level with radiosonde position)",,"004086","Long time period or displacement","Long time period or displacement (since launch time)",,"Operational"
1113.00,"03","Meteorological sequences common to vertical soundings data","303050","(Wind data at a pressure level with radiosonde position)",,"008042","Extended vertical sounding significance","Extended vertical sounding significance",,"Operational"
1114.00,"03","Meteorological sequences common to vertical soundings data","303050","(Wind data at a pressure level with radiosonde position)",,"007004","Pressure","Pressure",,"Operational"
1115.00,"03","Meteorological sequences common to vertical soundings data","303050","(Wind data at a pressure level with radiosonde position)",,"005015","Latitude displacement (high accuracy)","Latitude displacement since launch site (high accuracy)",,"Operational"
1116.00,"03","Meteorological sequences common to vertical soundings data","303050","(Wind data at a pressure level with radiosonde position)",,"006015","Longitude displacement (high accuracy)","Longitude displacement since launch site (high accuracy)",,"Operational"
1117.00,"03","Meteorological sequences common to vertical soundings data","303050","(Wind data at a pressure level with radiosonde position)",,"011001","Wind direction","Wind direction",,"Operational"
1118.00,"03","Meteorological sequences common to vertical soundings data","303050","(Wind data at a pressure level with radiosonde position)",,"011002","Wind speed","Wind speed",,"Operational"
1119.00,"03","Meteorological sequences common to vertical soundings data","303051","(Wind shear data at a pressure level with radiosonde position)",,"004086","Long time period or displacement","Long time period or displacement (since launch time)",,"Operational"
1120.00,"03","Meteorological sequences common to vertical soundings data","303051","(Wind shear data at a pressure level with radiosonde position)",,"008042","Extended vertical sounding significance","Extended vertical sounding significance",,"Operational"
1121.00,"03","Meteorological sequences common to vertical soundings data","303051","(Wind shear data at a pressure level with radiosonde position)",,"007004","Pressure","Pressure",,"Operational"
1122.00,"03","Meteorological sequences common to vertical soundings data","303051","(Wind shear data at a pressure level with radiosonde position)",,"005015","Latitude displacement (high accuracy)","Latitude displacement since launch site (high accuracy)",,"Operational"
1123.00,"03","Meteorological sequences common to vertical soundings data","303051","(Wind shear data at a pressure level with radiosonde position)",,"006015","Longitude displacement (high accuracy)","Longitude displacement since launch site (high accuracy)",,"Operational"
1124.00,"03","Meteorological sequences common to vertical soundings data","303051","(Wind shear data at a pressure level with radiosonde position)",,"011061","Absolute wind shear in 1 km layer below","Absolute wind shear in 1 km layer below",,"Operational"
1125.00,"03","Meteorological sequences common to vertical soundings data","303051","(Wind shear data at a pressure level with radiosonde position)",,"011062","Absolute wind shear in 1 km layer above","Absolute wind shear in 1 km layer above",,"Operational"
1126.00,"03","Meteorological sequences common to vertical soundings data","303052","(Wind data at a height level with radiosonde position)",,"004086","Long time period or displacement","Long time period or displacement (since launch time)",,"Operational"
1127.00,"03","Meteorological sequences common to vertical soundings data","303052","(Wind data at a height level with radiosonde position)",,"008042","Extended vertical sounding significance","Extended vertical sounding significance",,"Operational"
1128.00,"03","Meteorological sequences common to vertical soundings data","303052","(Wind data at a height level with radiosonde position)",,"007009","Geopotential height","Geopotential height",,"Operational"
1129.00,"03","Meteorological sequences common to vertical soundings data","303052","(Wind data at a height level with radiosonde position)",,"005015","Latitude displacement (high accuracy)","Latitude displacement since launch site (high accuracy)",,"Operational"
1130.00,"03","Meteorological sequences common to vertical soundings data","303052","(Wind data at a height level with radiosonde position)",,"006015","Longitude displacement (high accuracy)","Longitude displacement since launch site (high accuracy)",,"Operational"
1131.00,"03","Meteorological sequences common to vertical soundings data","303052","(Wind data at a height level with radiosonde position)",,"011001","Wind direction","Wind direction",,"Operational"
1132.00,"03","Meteorological sequences common to vertical soundings data","303052","(Wind data at a height level with radiosonde position)",,"011002","Wind speed","Wind speed",,"Operational"
1133.00,"03","Meteorological sequences common to vertical soundings data","303053","(Wind shear data at a height level with radiosonde position)",,"004086","Long time period or displacement","Long time period or displacement (since launch time)",,"Operational"
1134.00,"03","Meteorological sequences common to vertical soundings data","303053","(Wind shear data at a height level with radiosonde position)",,"008042","Extended vertical sounding significance","Extended vertical sounding significance",,"Operational"
1135.00,"03","Meteorological sequences common to vertical soundings data","303053","(Wind shear data at a height level with radiosonde position)",,"007009","Geopotential height","Geopotential height",,"Operational"
1136.00,"03","Meteorological sequences common to vertical soundings data","303053","(Wind shear data at a height level with radiosonde position)",,"005015","Latitude displacement (high accuracy)","Latitude displacement since launch site (high accuracy)",,"Operational"
1137.00,"03","Meteorological sequences common to vertical soundings data","303053","(Wind shear data at a height level with radiosonde position)",,"006015","Longitude displacement (high accuracy)","Longitude displacement since launch site (high accuracy)",,"Operational"
1138.00,"03","Meteorological sequences common to vertical soundings data","303053","(Wind shear data at a height level with radiosonde position)",,"011061","Absolute wind shear in 1 km layer below","Absolute wind shear in 1 km layer below",,"Operational"
1139.00,"03","Meteorological sequences common to vertical soundings data","303053","(Wind shear data at a height level with radiosonde position)",,"011062","Absolute wind shear in 1 km layer above","Absolute wind shear in 1 km layer above",,"Operational"
1140.00,"03","Meteorological sequences common to vertical soundings data","303054","(Temperature, dew-point and wind data at a pressure level with radiosonde position)",,"004086","Long time period or displacement","Long time period or displacement (since launch time)",,"Operational"
1141.00,"03","Meteorological sequences common to vertical soundings data","303054","(Temperature, dew-point and wind data at a pressure level with radiosonde position)",,"008042","Extended vertical sounding significance","Extended vertical sounding significance",,"Operational"
1142.00,"03","Meteorological sequences common to vertical soundings data","303054","(Temperature, dew-point and wind data at a pressure level with radiosonde position)",,"007004","Pressure","Pressure",,"Operational"
1143.00,"03","Meteorological sequences common to vertical soundings data","303054","(Temperature, dew-point and wind data at a pressure level with radiosonde position)",,"010009","Geopotential height","Geopotential height",,"Operational"
1144.00,"03","Meteorological sequences common to vertical soundings data","303054","(Temperature, dew-point and wind data at a pressure level with radiosonde position)",,"005015","Latitude displacement (high accuracy)","Latitude displacement since launch site (high accuracy)",,"Operational"
1145.00,"03","Meteorological sequences common to vertical soundings data","303054","(Temperature, dew-point and wind data at a pressure level with radiosonde position)",,"006015","Longitude displacement (high accuracy)","Longitude displacement since launch site (high accuracy)",,"Operational"
1146.00,"03","Meteorological sequences common to vertical soundings data","303054","(Temperature, dew-point and wind data at a pressure level with radiosonde position)",,"012101","Temperature/air temperature","Temperature/air temperature (scale 2)",,"Operational"
1147.00,"03","Meteorological sequences common to vertical soundings data","303054","(Temperature, dew-point and wind data at a pressure level with radiosonde position)",,"012103","Dew-point temperature","Dew-point temperature (scale 2)",,"Operational"
1148.00,"03","Meteorological sequences common to vertical soundings data","303054","(Temperature, dew-point and wind data at a pressure level with radiosonde position)",,"011001","Wind direction","Wind direction",,"Operational"
1149.00,"03","Meteorological sequences common to vertical soundings data","303054","(Temperature, dew-point and wind data at a pressure level with radiosonde position)",,"011002","Wind speed","Wind speed",,"Operational"
1150.00,"03","Meteorological sequences common to vertical soundings data","303055","(Temperature, dew-point, relative humidity and wind data at height levels with radiosonde position)",,"004086","Long time period or displacement","Long time period or displacement (since launch time)",,"Operational"
1151.00,"03","Meteorological sequences common to vertical soundings data","303055","(Temperature, dew-point, relative humidity and wind data at height levels with radiosonde position)",,"008042","Extended vertical sounding significance","Extended vertical sounding significance",,"Operational"
1152.00,"03","Meteorological sequences common to vertical soundings data","303055","(Temperature, dew-point, relative humidity and wind data at height levels with radiosonde position)",,"007009","Geopotential height","Geopotential height",,"Operational"
1153.00,"03","Meteorological sequences common to vertical soundings data","303055","(Temperature, dew-point, relative humidity and wind data at height levels with radiosonde position)",,"005015","Latitude displacement (high accuracy)","Latitude displacement since launch site (high accuracy)",,"Operational"
1154.00,"03","Meteorological sequences common to vertical soundings data","303055","(Temperature, dew-point, relative humidity and wind data at height levels with radiosonde position)",,"006015","Longitude displacement (high accuracy)","Longitude displacement since launch site (high accuracy)",,"Operational"
1155.00,"03","Meteorological sequences common to vertical soundings data","303055","(Temperature, dew-point, relative humidity and wind data at height levels with radiosonde position)",,"012101","Temperature/air temperature","Temperature/air temperature (scale 2)",,"Operational"
1156.00,"03","Meteorological sequences common to vertical soundings data","303055","(Temperature, dew-point, relative humidity and wind data at height levels with radiosonde position)",,"013009","Relative humidity","Relative humidity",,"Operational"
1157.00,"03","Meteorological sequences common to vertical soundings data","303055","(Temperature, dew-point, relative humidity and wind data at height levels with radiosonde position)",,"012103","Dew-point temperature","Dew-point temperature (scale 2)",,"Operational"
1158.00,"03","Meteorological sequences common to vertical soundings data","303055","(Temperature, dew-point, relative humidity and wind data at height levels with radiosonde position)",,"011001","Wind direction","Wind direction",,"Operational"
1159.00,"03","Meteorological sequences common to vertical soundings data","303055","(Temperature, dew-point, relative humidity and wind data at height levels with radiosonde position)",,"011002","Wind speed","Wind speed",,"Operational"
1160.00,"04","Meteorological sequences common to satellite observations","304001",,,"008003","Vertical significance (satellite observations)","Vertical significance",,"Operational"
1161.00,"04","Meteorological sequences common to satellite observations","304001",,,"010004","Pressure","Pressure",,"Operational"
1162.00,"04","Meteorological sequences common to satellite observations","304001",,,"012001","Temperature/air temperature","Temperature",,"Operational"
1163.00,"04","Meteorological sequences common to satellite observations","304001",,,"011001","Wind direction","Wind direction",,"Operational"
1164.00,"04","Meteorological sequences common to satellite observations","304001",,,"011002","Wind speed","Wind speed",,"Operational"
1165.00,"04","Meteorological sequences common to satellite observations","304002",,,"008003","Vertical significance (satellite observations)","Vertical significance",,"Operational"
1166.00,"04","Meteorological sequences common to satellite observations","304002",,,"010004","Pressure","Pressure",,"Operational"
1167.00,"04","Meteorological sequences common to satellite observations","304002",,,"011001","Wind direction","Wind direction",,"Operational"
1168.00,"04","Meteorological sequences common to satellite observations","304002",,,"011002","Wind speed","Wind speed",,"Operational"
1169.00,"04","Meteorological sequences common to satellite observations","304003",,,"008003","Vertical significance (satellite observations)","Vertical significance",,"Operational"
1170.00,"04","Meteorological sequences common to satellite observations","304003",,,"012001","Temperature/air temperature","Temperature",,"Operational"
1171.00,"04","Meteorological sequences common to satellite observations","304004",,,"008003","Vertical significance (satellite observations)","Vertical significance",,"Operational"
1172.00,"04","Meteorological sequences common to satellite observations","304004",,,"010004","Pressure","Pressure",,"Operational"
1173.00,"04","Meteorological sequences common to satellite observations","304004",,,"020010","Cloud cover (total)","Cloud cover (total)",,"Operational"
1174.00,"04","Meteorological sequences common to satellite observations","304004",,,"012001","Temperature/air temperature","Temperature",,"Operational"
1175.00,"04","Meteorological sequences common to satellite observations","304005",,,"002024","Integrated mean humidity computational method","Integrated mean humidity computational method",,"Operational"
1176.00,"04","Meteorological sequences common to satellite observations","304005",,,"007004","Pressure","Pressure (1)    defines layer",,"Operational"
1177.00,"04","Meteorological sequences common to satellite observations","304005",,,"007004","Pressure","Pressure (2)    defines layer",,"Operational"
1178.00,"04","Meteorological sequences common to satellite observations","304005",,,"013003","Relative humidity","Relative humidity",,"Operational"
1179.00,"04","Meteorological sequences common to satellite observations","304006",,,"014001","Long-wave radiation, integrated over 24 hours","Outgoing long-wave radiation",,"Operational"
1180.00,"04","Meteorological sequences common to satellite observations","304006",,,"014001","Long-wave radiation, integrated over 24 hours","Incoming long-wave radiation",,"Operational"
1181.00,"04","Meteorological sequences common to satellite observations","304006",,,"014003","Short-wave radiation, integrated over 24 hours","Outgoing short-wave radiation",,"Operational"
1182.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"002163","Height assignment method","Height assignment method",,"Operational"
1183.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"002164","Tracer correlation method","Tracer correlation method",,"Operational"
1184.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"008012","Land/sea qualifier","Land/sea qualifier",,"Operational"
1185.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"007024","Satellite zenith angle","Satellite zenith angle",,"Operational"
1186.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"002057","Origin of first guess information for GOES-I/M soundings","Origin of first guess information",,"Operational"
1187.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"008021","Time significance","Time significance",,"Operational"
1188.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"004001","Year","Year",,"Operational"
1189.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"004002","Month","Month",,"Operational"
1190.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"004003","Day","Day",,"Operational"
1191.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"004004","Hour","Hour",,"Operational"
1192.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"008021","Time significance","Time significance",,"Operational"
1193.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"004024","Time period or displacement","Time period or displacement",,"Operational"
1194.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"110004","Replication descriptor","Replicate 10 descriptors 4 times",,"Operational"
1195.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"008021","Time significance","Time significance",,"Operational"
1196.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"004004","Hour","Hour",,"Operational"
1197.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"004005","Minute","Minute",,"Operational"
1198.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"004006","Second","Second",,"Operational"
1199.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"008021","Time significance","Time significance",,"Operational"
1200.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"004004","Hour","Hour",,"Operational"
1201.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"004005","Minute","Minute",,"Operational"
1202.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"004006","Second","Second",,"Operational"
1203.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"011001","Wind direction","Wind direction",,"Operational"
1204.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"011002","Wind speed","Wind speed",,"Operational"
1205.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"103010","Replication descriptor","Replicate 3 descriptors 10 times",,"Operational"
1206.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"002163","Height assignment method","Height assignment method",,"Operational"
1207.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"007004","Pressure","Pressure",,"Operational"
1208.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"012001","Temperature/air temperature","Temperature",,"Operational"
1209.00,"04","Meteorological sequences common to satellite observations","304030","(Location of platform)",,"027031","In direction of 0 degrees longitude, distance from the Earth's centre","In direction of 0 degree longitude, distance from the Earth’s centre",,"Operational"
1210.00,"04","Meteorological sequences common to satellite observations","304030","(Location of platform)",,"028031","In direction 90 degrees East, distance from the Earth's centre","In direction of 90 degrees East longitude, distance from the Earth’s centre",,"Operational"
1211.00,"04","Meteorological sequences common to satellite observations","304030","(Location of platform)",,"010031","In direction of the North Pole, distance from the Earth's centre","In direction of North Pole, distance from Earth’s centre",,"Operational"
1212.00,"04","Meteorological sequences common to satellite observations","304031","(Speed of platform)",,"001041","Absolute platform velocity - first component","Absolute platform velocity - first component",,"Operational"
1213.00,"04","Meteorological sequences common to satellite observations","304031","(Speed of platform)",,"001042","Absolute platform velocity - second component","Absolute platform velocity - second component",,"Operational"
1214.00,"04","Meteorological sequences common to satellite observations","304031","(Speed of platform)",,"001043","Absolute platform velocity - third component","Absolute platform velocity - third component",,"Operational"
1215.00,"04","Meteorological sequences common to satellite observations","304032","(Cloud fraction)",,"002153","Satellite channel centre frequency","Satellite channel centre frequency",,"Operational"
1216.00,"04","Meteorological sequences common to satellite observations","304032","(Cloud fraction)",,"002154","Satellite channel band width","Satellite channel band width",,"Operational"
1217.00,"04","Meteorological sequences common to satellite observations","304032","(Cloud fraction)",,"020081","Cloud amount in segment","Cloud amount in segment",,"Operational"
1218.00,"04","Meteorological sequences common to satellite observations","304032","(Cloud fraction)",,"020082","Amount segment cloud free","Amount segment cloud free",,"Operational"
1219.00,"04","Meteorological sequences common to satellite observations","304032","(Cloud fraction)",,"020012","Cloud type","Cloud type",,"Operational"
1220.00,"04","Meteorological sequences common to satellite observations","304033","(Clear sky radiance)",,"002152","Satellite instrument used in data processing","Satellite instrument used in data processing",,"Operational"
1221.00,"04","Meteorological sequences common to satellite observations","304033","(Clear sky radiance)",,"002166","Radiance type","Radiance type",,"Operational"
1222.00,"04","Meteorological sequences common to satellite observations","304033","(Clear sky radiance)",,"002167","Radiance computational method","Radiance computational method",,"Operational"
1223.00,"04","Meteorological sequences common to satellite observations","304033","(Clear sky radiance)",,"002153","Satellite channel centre frequency","Satellite channel centre frequency",,"Operational"
1224.00,"04","Meteorological sequences common to satellite observations","304033","(Clear sky radiance)",,"002154","Satellite channel band width","Satellite channel band width",,"Operational"
1225.00,"04","Meteorological sequences common to satellite observations","304033","(Clear sky radiance)",,"012075","Spectral radiance","Spectral radiance",,"Operational"
1226.00,"04","Meteorological sequences common to satellite observations","304033","(Clear sky radiance)",,"012076","Radiance","Radiance",,"Operational"
1227.00,"04","Meteorological sequences common to satellite observations","304033","(Clear sky radiance)",,"012063","Brightness temperature","Brightness temperature",,"Operational"
1228.00,"04","Meteorological sequences common to satellite observations","304034",,,"102004","Replication descriptor","Replicating next two descriptors 4 times",,"Operational"
1229.00,"04","Meteorological sequences common to satellite observations","304034",,,"027001","Latitude (high accuracy)","Latitude (high accuracy)",,"Operational"
1230.00,"04","Meteorological sequences common to satellite observations","304034",,,"028001","Longitude (high accuracy)","Longitude (high accuracy)",,"Operational"
1231.00,"04","Meteorological sequences common to satellite observations","304034",,,"007022","Solar elevation","Solar elevation",,"Operational"
1232.00,"04","Meteorological sequences common to satellite observations","304034",,,"005043","Field of view number","Field of view number",,"Operational"
1233.00,"04","Meteorological sequences common to satellite observations","304034",,,"020010","Cloud cover (total)","Cloud cover (total)",,"Operational"
1234.00,"04","Meteorological sequences common to satellite observations","304034",,,"020016","Pressure at top of cloud","Pressure at top of cloud",,"Operational"
1235.00,"04","Meteorological sequences common to satellite observations","304034",,,"033003","Quality information","Quality information table",,"Operational"
1236.00,"04","Meteorological sequences common to satellite observations","304034",,,"010040","Number of retrieved layers","Number of retrieved layers",,"Operational"
1237.00,"04","Meteorological sequences common to satellite observations","304035","(All sky radiance data)",,"002153","Satellite channel centre frequency","Satellite channel centre frequency",,"Deprecated"
1238.00,"04","Meteorological sequences common to satellite observations","304035","(All sky radiance data)",,"002154","Satellite channel band width","Satellite channel band width",,"Deprecated"
1239.00,"04","Meteorological sequences common to satellite observations","304035","(All sky radiance data)",,"012063","Brightness temperature","Brightness temperature",,"Deprecated"
1240.00,"04","Meteorological sequences common to satellite observations","304035","(All sky radiance data)",,"008001","Meteorological feature","Pixel type: clear",,"Deprecated"
1241.00,"04","Meteorological sequences common to satellite observations","304035","(All sky radiance data)",,"012063","Brightness temperature","Brightness temperature (clear)",,"Deprecated"
1242.00,"04","Meteorological sequences common to satellite observations","304035","(All sky radiance data)",,"008001","Meteorological feature","Pixel type: cloudy",,"Deprecated"
1243.00,"04","Meteorological sequences common to satellite observations","304035","(All sky radiance data)",,"012063","Brightness temperature","Brightness temperature (cloudy)",,"Deprecated"
1244.00,"04","Meteorological sequences common to satellite observations","304035","(All sky radiance data)",,"008001","Meteorological feature","Cancel type",,"Deprecated"
1245.00,"04","Meteorological sequences common to satellite observations","304035","(All sky radiance data)",,"008003","Vertical significance (satellite observations)","Vertical significance: low cloud",,"Deprecated"
1246.00,"04","Meteorological sequences common to satellite observations","304035","(All sky radiance data)",,"012063","Brightness temperature","Brightness temperature (low cloud)",,"Deprecated"
1247.00,"04","Meteorological sequences common to satellite observations","304035","(All sky radiance data)",,"008003","Vertical significance (satellite observations)","vertical significance: mid cloud",,"Deprecated"
1248.00,"04","Meteorological sequences common to satellite observations","304035","(All sky radiance data)",,"012063","Brightness temperature","Brightness temperature (mid cloud)",,"Deprecated"
1249.00,"04","Meteorological sequences common to satellite observations","304035","(All sky radiance data)",,"008003","Vertical significance (satellite observations)","vertical significance: high cloud",,"Deprecated"
1250.00,"04","Meteorological sequences common to satellite observations","304035","(All sky radiance data)",,"012063","Brightness temperature","Brightness temperature (high cloud)",,"Deprecated"
1251.00,"04","Meteorological sequences common to satellite observations","304035","(All sky radiance data)",,"008003","Vertical significance (satellite observations)","Cancel_significance",,"Deprecated"
1252.00,"04","Meteorological sequences common to satellite observations","304036","(Cloud coverage)",,"020082","Amount segment cloud free","Amount of segment cloud free",,"Operational"
1253.00,"04","Meteorological sequences common to satellite observations","304036","(Cloud coverage)",,"008012","Land/sea qualifier","Land-sea qualifier: sea",,"Operational"
1254.00,"04","Meteorological sequences common to satellite observations","304036","(Cloud coverage)",,"020082","Amount segment cloud free","Amount of segment cloud free (sea)",,"Operational"
1255.00,"04","Meteorological sequences common to satellite observations","304036","(Cloud coverage)",,"008012","Land/sea qualifier","Cancel qualifier",,"Operational"
1256.00,"04","Meteorological sequences common to satellite observations","304036","(Cloud coverage)",,"020081","Cloud amount in segment","Cloud amount in segment",,"Operational"
1257.00,"04","Meteorological sequences common to satellite observations","304036","(Cloud coverage)",,"008003","Vertical significance (satellite observations)","Vertical significance: low cloud",,"Operational"
1258.00,"04","Meteorological sequences common to satellite observations","304036","(Cloud coverage)",,"020081","Cloud amount in segment","Cloud amount in segment (low cloud)",,"Operational"
1259.00,"04","Meteorological sequences common to satellite observations","304036","(Cloud coverage)",,"008003","Vertical significance (satellite observations)","Vertical significance: mid cloud",,"Operational"
1260.00,"04","Meteorological sequences common to satellite observations","304036","(Cloud coverage)",,"020081","Cloud amount in segment","Cloud amount in segment (mid cloud)",,"Operational"
1261.00,"04","Meteorological sequences common to satellite observations","304036","(Cloud coverage)",,"008003","Vertical significance (satellite observations)","Vertical significance: high cloud",,"Operational"
1262.00,"04","Meteorological sequences common to satellite observations","304036","(Cloud coverage)",,"020081","Cloud amount in segment","Cloud amount in segment (high cloud)",,"Operational"
1263.00,"04","Meteorological sequences common to satellite observations","304036","(Cloud coverage)",,"008003","Vertical significance (satellite observations)","Cancel significance",,"Operational"
1264.00,"04","Meteorological sequences common to satellite observations","304037","(All sky radiance data)",,"002153","Satellite channel centre frequency","Satellite channel centre frequency",,"Operational"
1265.00,"04","Meteorological sequences common to satellite observations","304037","(All sky radiance data)",,"002154","Satellite channel band width","Satellite channel band width",,"Operational"
1266.00,"04","Meteorological sequences common to satellite observations","304037","(All sky radiance data)",,"012063","Brightness temperature","Brightness temperature",,"Operational"
1267.00,"04","Meteorological sequences common to satellite observations","304037","(All sky radiance data)",,"008011","Meteorological feature","Pixel type: clear",,"Operational"
1268.00,"04","Meteorological sequences common to satellite observations","304037","(All sky radiance data)",,"012063","Brightness temperature","Brightness temperature (clear)",,"Operational"
1269.00,"04","Meteorological sequences common to satellite observations","304037","(All sky radiance data)",,"008011","Meteorological feature","Pixel type: cloudy",,"Operational"
1270.00,"04","Meteorological sequences common to satellite observations","304037","(All sky radiance data)",,"012063","Brightness temperature","Brightness temperature (cloudy)",,"Operational"
1271.00,"04","Meteorological sequences common to satellite observations","304037","(All sky radiance data)",,"008011","Meteorological feature","Cancel type",,"Operational"
1272.00,"04","Meteorological sequences common to satellite observations","304037","(All sky radiance data)",,"008003","Vertical significance (satellite observations)","Vertical significance: low cloud",,"Operational"
1273.00,"04","Meteorological sequences common to satellite observations","304037","(All sky radiance data)",,"012063","Brightness temperature","Brightness temperature (low cloud)",,"Operational"
1274.00,"04","Meteorological sequences common to satellite observations","304037","(All sky radiance data)",,"008003","Vertical significance (satellite observations)","Vertical significance: mid cloud",,"Operational"
1275.00,"04","Meteorological sequences common to satellite observations","304037","(All sky radiance data)",,"012063","Brightness temperature","Brightness temperature (mid cloud)",,"Operational"
1276.00,"04","Meteorological sequences common to satellite observations","304037","(All sky radiance data)",,"008003","Vertical significance (satellite observations)","Vertical significance: high cloud",,"Operational"
1277.00,"04","Meteorological sequences common to satellite observations","304037","(All sky radiance data)",,"012063","Brightness temperature","Brightness temperature",,"Operational"
1278.00,"05","Meteorological or hydrological sequences common to hydrological observations","305003","(SADC-HYCOS measurement array definition)",,"301012",,"Hour, minute of first single measurement minus increment",,"Operational"
1279.00,"05","Meteorological or hydrological sequences common to hydrological observations","305003","(SADC-HYCOS measurement array definition)",,"004065","Short time increment","Short time increment - time interval between measurements",,"Operational"
1280.00,"05","Meteorological or hydrological sequences common to hydrological observations","305003","(SADC-HYCOS measurement array definition)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
1281.00,"05","Meteorological or hydrological sequences common to hydrological observations","305003","(SADC-HYCOS measurement array definition)",,"031001","Delayed descriptor replication factor","Replication factor",,"Operational"
1282.00,"05","Meteorological or hydrological sequences common to hydrological observations","305003","(SADC-HYCOS measurement array definition)",,"305001",,"Single measurement",,"Operational"
1283.00,"05","Meteorological or hydrological sequences common to hydrological observations","305006","(MEDHYCOS measurement)",,"013072","Downstream water level","Downstream water level",,"Operational"
1284.00,"05","Meteorological or hydrological sequences common to hydrological observations","305006","(MEDHYCOS measurement)",,"013082","Water temperature","Water temperature",,"Operational"
1285.00,"05","Meteorological or hydrological sequences common to hydrological observations","305006","(MEDHYCOS measurement)",,"013019","Total precipitation past 1 hour","Precipitation last hour",,"Operational"
1286.00,"05","Meteorological or hydrological sequences common to hydrological observations","305006","(MEDHYCOS measurement)",,"012001","Temperature/air temperature","Air temperature",,"Operational"
1287.00,"05","Meteorological or hydrological sequences common to hydrological observations","305006","(MEDHYCOS measurement)",,"013073","Maximum water level","Maximum water height observed",,"Operational"
1288.00,"05","Meteorological or hydrological sequences common to hydrological observations","305006","(MEDHYCOS measurement)",,"013060","Total accumulated precipitation","Total accumulated precipitation",,"Operational"
1289.00,"05","Meteorological or hydrological sequences common to hydrological observations","305007","(MEDHYCOS report)",,"301029",,"Identification",,"Operational"
1290.00,"05","Meteorological or hydrological sequences common to hydrological observations","305007","(MEDHYCOS report)",,"301012",,"Hour, minute (time of first measurement)",,"Operational"
1291.00,"05","Meteorological or hydrological sequences common to hydrological observations","305007","(MEDHYCOS report)",,"004065","Short time increment","Short time increment - time interval between measurements",,"Operational"
1292.00,"05","Meteorological or hydrological sequences common to hydrological observations","305007","(MEDHYCOS report)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
1293.00,"05","Meteorological or hydrological sequences common to hydrological observations","305007","(MEDHYCOS report)",,"031001","Delayed descriptor replication factor","Replication factor",,"Operational"
1294.00,"05","Meteorological or hydrological sequences common to hydrological observations","305007","(MEDHYCOS report)",,"305006","MEDHYCOS measurement","Single measurement",,"Operational"
1295.00,"05","Meteorological or hydrological sequences common to hydrological observations","305008","(AOCHYCOS - Chad measurement)",,"305006","MEDHYCOS measurement","Same as MEDHYCOS type measurement",,"Operational"
1296.00,"05","Meteorological or hydrological sequences common to hydrological observations","305008","(AOCHYCOS - Chad measurement)",,"012030","Soil temperature","Soil temperature at -50 cm",,"Operational"
1297.00,"05","Meteorological or hydrological sequences common to hydrological observations","305009","(AOCHYCOS - Chad report)",,"301029",,"Identification",,"Operational"
1298.00,"05","Meteorological or hydrological sequences common to hydrological observations","305009","(AOCHYCOS - Chad report)",,"301012",,"Hour, minute (time of first measurement)",,"Operational"
1299.00,"05","Meteorological or hydrological sequences common to hydrological observations","305009","(AOCHYCOS - Chad report)",,"004065","Short time increment","Short time increment - time interval between measurements",,"Operational"
1300.00,"05","Meteorological or hydrological sequences common to hydrological observations","305009","(AOCHYCOS - Chad report)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
1301.00,"05","Meteorological or hydrological sequences common to hydrological observations","305009","(AOCHYCOS - Chad report)",,"031001","Delayed descriptor replication factor","Replication factor",,"Operational"
1302.00,"05","Meteorological or hydrological sequences common to hydrological observations","305009","(AOCHYCOS - Chad report)",,"305008","AOCHYCOS - Chad measurement","Single measurement",,"Operational"
1303.00,"05","Meteorological or hydrological sequences common to hydrological observations","305011","(MEDHYCOS report type 2)",,"301029",,"Identification",,"Operational"
1304.00,"05","Meteorological or hydrological sequences common to hydrological observations","305011","(MEDHYCOS report type 2)",,"301012",,"Hour, minute (time of first measurement)",,"Operational"
1305.00,"05","Meteorological or hydrological sequences common to hydrological observations","305011","(MEDHYCOS report type 2)",,"004065","Short time increment","Short time increment - time interval between measurements",,"Operational"
1306.00,"05","Meteorological or hydrological sequences common to hydrological observations","305011","(MEDHYCOS report type 2)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
1307.00,"05","Meteorological or hydrological sequences common to hydrological observations","305011","(MEDHYCOS report type 2)",,"031001","Delayed descriptor replication factor","Replication factor",,"Operational"
1308.00,"05","Meteorological or hydrological sequences common to hydrological observations","305011","(MEDHYCOS report type 2)",,"305010",,"Single measurement",,"Operational"
1309.00,"05","Meteorological or hydrological sequences common to hydrological observations","305018","(MEDHYCOS report with meteorology and water quality data)",,"301029",,"Identification",,"Operational"
1310.00,"05","Meteorological or hydrological sequences common to hydrological observations","305018","(MEDHYCOS report with meteorology and water quality data)",,"301012",,"Hour, minute (time) of first measurement",,"Operational"
1311.00,"05","Meteorological or hydrological sequences common to hydrological observations","305018","(MEDHYCOS report with meteorology and water quality data)",,"004065","Short time increment","Hour increment",,"Operational"
1312.00,"05","Meteorological or hydrological sequences common to hydrological observations","305018","(MEDHYCOS report with meteorology and water quality data)",,"103000","Replication descriptor","Delayed replications of 3 descriptors",,"Operational"
1313.00,"05","Meteorological or hydrological sequences common to hydrological observations","305018","(MEDHYCOS report with meteorology and water quality data)",,"031001","Delayed descriptor replication factor","Replication factor",,"Operational"
1314.00,"05","Meteorological or hydrological sequences common to hydrological observations","305018","(MEDHYCOS report with meteorology and water quality data)",,"305008","AOCHYCOS - Chad measurement","Same as AOCHYCOS type measurement",,"Operational"
1315.00,"05","Meteorological or hydrological sequences common to hydrological observations","305018","(MEDHYCOS report with meteorology and water quality data)",,"305016",,"Meteorological parameters associated to hydrological data",,"Operational"
1316.00,"05","Meteorological or hydrological sequences common to hydrological observations","305018","(MEDHYCOS report with meteorology and water quality data)",,"305017",,"Water quality measurement",,"Operational"
1317.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306001",,,"002032","Indicator for digitization","Indicator for digitization",,"Operational"
1318.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306001",,,"102000","Replication descriptor","Delayed replication of 2 descriptors",,"Operational"
1319.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306001",,,"031001","Delayed descriptor replication factor","Replication factor",,"Operational"
1320.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306001",,,"007062","Depth below sea/water surface","Depth below sea surface",,"Operational"
1321.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306001",,,"022042","Sea/water temperature","Subsurface sea temperature",,"Operational"
1322.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306002",,,"002031","Duration and time of current measurement","Method of current measurement",,"Operational"
1323.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306002",,,"022004","Direction of current","Direction of current",,"Operational"
1324.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306002",,,"022031","Speed of current","Speed of current",,"Operational"
1325.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306003",,,"002002","Type of instrumentation for wind measurement","Wind instrumentation",,"Operational"
1326.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306003",,,"011011","Wind direction at 10 m","Wind direction (10 m)",,"Operational"
1327.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306003",,,"011012","Wind speed at 10 m","Wind speed (10 m)",,"Operational"
1328.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306003",,,"012004","Air temperature at 2 m","Air temperature (2 m)",,"Operational"
1329.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306004",,,"002032","Indicator for digitization","Indicator for digitization",,"Operational"
1330.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306004",,,"002033","Method of salinity/depth measurement","Method of salinity/depth measurement",,"Operational"
1331.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306004",,,"103000","Replication descriptor","Delayed replication of 3 descriptors",,"Operational"
1332.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306004",,,"031001","Delayed descriptor replication factor","Replication factor",,"Operational"
1333.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306004",,,"007062","Depth below sea/water surface","Depth below sea surface",,"Operational"
1334.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306004",,,"022043","Sea/water temperature","Subsurface sea temperature",,"Operational"
1335.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306004",,,"022062","Salinity","Salinity",,"Operational"
1336.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306005",,,"002031","Duration and time of current measurement","Method of current measurement (duration and time)",,"Operational"
1337.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306005",,,"103000","Replication descriptor","Delayed replication of 3 descriptors",,"Operational"
1338.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306005",,,"031001","Delayed descriptor replication factor","Replication factor",,"Operational"
1339.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306005",,,"007062","Depth below sea/water surface","Depth below sea surface",,"Operational"
1340.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306005",,,"022004","Direction of current","Direction of current",,"Operational"
1341.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306005",,,"022031","Speed of current","Speed of current",,"Operational"
1342.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306006","(Under water sounding (optional) parameters)",,"306003",,"Surface wind and temperature",,"Operational"
1343.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306006","(Under water sounding (optional) parameters)",,"306002",,"Current",,"Operational"
1344.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306006","(Under water sounding (optional) parameters)",,"022063","Total water depth","Total water depth",,"Operational"
1345.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306007","(Buoy spare block parameters)",,"001012","Direction of motion of moving observing platform","Direction of motion of moving observing platform",,"Operational"
1346.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306007","(Buoy spare block parameters)",,"001014","Platform drift speed (high precision)","Platform drift speed (high precision)",,"Operational"
1347.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306007","(Buoy spare block parameters)",,"306008","Buoy instrumentation parameters","Buoy instrumentation",,"Operational"
1348.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306007","(Buoy spare block parameters)",,"004024","Time period or displacement","Time period",,"Operational"
1349.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306007","(Buoy spare block parameters)",,"027003","Alternate latitude (coarse accuracy)","Alternate latitude",,"Operational"
1350.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306007","(Buoy spare block parameters)",,"028003","Alternate longitude (coarse accuracy)","Alternate longitude",,"Operational"
1351.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306008","(Buoy instrumentation parameters)",,"002034","Drogue type","Drogue type",,"Operational"
1352.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306008","(Buoy instrumentation parameters)",,"002035","Cable length","Cable length",,"Operational"
1353.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306008","(Buoy instrumentation parameters)",,"002036","Buoy type","Buoy type",,"Operational"
1389.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306019","(Tide report identification, water level checks, time increments)",,"001075","Tide station identification","Tide station alphanumeric identification",,"Operational"
1390.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306019","(Tide report identification, water level checks, time increments)",,"301011",,"Year, month, day",,"Operational"
1391.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306019","(Tide report identification, water level checks, time increments)",,"301012",,"Hour, minute",,"Operational"
1392.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306019","(Tide report identification, water level checks, time increments)",,"022042","Sea/water temperature","Sea/water temperature",,"Operational"
1393.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306019","(Tide report identification, water level checks, time increments)",,"022120","Tide station automated water level check","Tide station automated water level check",,"Operational"
1394.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306019","(Tide report identification, water level checks, time increments)",,"022121","Tide station manual water level check","Tide station manual water level check",,"Operational"
1395.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306019","(Tide report identification, water level checks, time increments)",,"004015","Time increment","Time increment in minutes","(see Note)","Operational"
1396.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306019","(Tide report identification, water level checks, time increments)",,"004065","Short time increment","Short time increment",,"Operational"
1397.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306023",,,"001015","Station or site name","Station or site name",,"Operational"
1398.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306023",,,"301023",,"Latitude, longitude",,"Operational"
1399.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306023",,,"301011",,"Year, month, day",,"Operational"
1400.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306023",,,"301012",,"Hour, minute",,"Operational"
1401.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306023",,,"022038","Tidal elevation with respect to local chart datum","Tidal level with respect to local chart datum",,"Operational"
1402.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306023",,,"022039","Meteorological residual tidal elevation (surge or offset)","Meteorological residual tidal elevation",,"Operational"
1403.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306023",,,"022120","Tide station automated water level check","Tide station automated water level check",,"Operational"
1404.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306023",,,"022121","Tide station manual water level check","Tide station manual water level check",,"Operational"
1405.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306027","(Sequence for representation of DART buoy identification, transmitter ID, type of tsunameter and the time the message is transmitted to the ground system)",,"001005","Buoy/platform identifier","Buoy/platform identifier",,"Operational"
1406.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306027","(Sequence for representation of DART buoy identification, transmitter ID, type of tsunameter and the time the message is transmitted to the ground system)",,"001052","Platform transmitter ID","Platform transmitter identifier",,"Operational"
1407.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306027","(Sequence for representation of DART buoy identification, transmitter ID, type of tsunameter and the time the message is transmitted to the ground system)",,"002047","Deep-ocean tsunameter type","Deep-ocean tsunameter platform type/manufacturer",,"Operational"
1408.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306027","(Sequence for representation of DART buoy identification, transmitter ID, type of tsunameter and the time the message is transmitted to the ground system)",,"301011",,"Year, month, day (time the message is transmitted to the ground system)",,"Operational"
1409.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306027","(Sequence for representation of DART buoy identification, transmitter ID, type of tsunameter and the time the message is transmitted to the ground system)",,"301013",,"Hour, minute, second",,"Operational"
1410.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306028","(Sequence for representation of time of observation and DART buoy position daily report)",,"306027","Sequence for representation of DART buoy identification, transmitter ID, type of tsunameter and the time the message is transmitted to the ground system","Buoy ID, transmitter ID, platform type, message transmission time",,"Operational"
1411.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306028","(Sequence for representation of time of observation and DART buoy position daily report)",,"301011",,"Year, month, day (observation time)",,"Operational"
1412.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306028","(Sequence for representation of time of observation and DART buoy position daily report)",,"301013",,"Hour, minute, second",,"Operational"
1413.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306028","(Sequence for representation of time of observation and DART buoy position daily report)",,"301021",,"Latitude, longitude (high accuracy)",,"Operational"
1414.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306029","(Sequence for representation of tsunameter sampling information for water column heights in the time series report)",,"025170","Sampling interval (time)","Sampling interval (seconds)",,"Operational"
1415.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306029","(Sequence for representation of tsunameter sampling information for water column heights in the time series report)",,"025171","Sample averaging period","Sample averaging period (seconds)",,"Operational"
1416.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306029","(Sequence for representation of tsunameter sampling information for water column heights in the time series report)",,"025172","Number of samples","Number of samples",,"Operational"
1417.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306030","(Sequence for representation of DART buoy standard hourly report)",,"306027","Sequence for representation of DART buoy identification, transmitter ID, type of tsunameter and the time the message is transmitted to the ground system","Buoy ID, transmitter ID, platform type, message transmission time",,"Operational"
1418.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306030","(Sequence for representation of DART buoy standard hourly report)",,"306029","Sequence for representation of tsunameter sampling information for water column heights in the time series report","Tsunameter sampling information",,"Operational"
1419.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306030","(Sequence for representation of DART buoy standard hourly report)",,"111000","Replication descriptor","Delayed replication of 11 descriptors",,"Operational"
1420.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306030","(Sequence for representation of DART buoy standard hourly report)",,"031001","Delayed descriptor replication factor","Delayed replication factor",,"Operational"
1421.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306030","(Sequence for representation of DART buoy standard hourly report)",,"033002","Quality information","Quality information (for message status)",,"Operational"
1422.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306030","(Sequence for representation of DART buoy standard hourly report)",,"301011",,"Year, month, day (reference date/time for the time series)",,"Operational"
1423.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306030","(Sequence for representation of DART buoy standard hourly report)",,"301013",,"Hour, minute, second",,"Operational"
1424.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306030","(Sequence for representation of DART buoy standard hourly report)",,"025025","Battery voltage","Battery voltage for BPR CPU",,"Operational"
1425.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306030","(Sequence for representation of DART buoy standard hourly report)",,"025025","Battery voltage","Battery voltage for acoustic modem DSP",,"Operational"
1426.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306030","(Sequence for representation of DART buoy standard hourly report)",,"025026","Battery voltage (large range)","Battery voltage for acoustic modem",,"Operational"
1427.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306030","(Sequence for representation of DART buoy standard hourly report)",,"022185","BPR transmission count","BPR transmission count",,"Operational"
1428.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306030","(Sequence for representation of DART buoy standard hourly report)",,"004015","Time increment","Time increment added to reset the reference time",,"Operational"
1429.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306030","(Sequence for representation of DART buoy standard hourly report)",,"004065","Short time increment","Time increment added to each data value in the time series",,"Operational"
1430.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306030","(Sequence for representation of DART buoy standard hourly report)",,"101004","Replication descriptor","Replicate 1 descriptor 4 times",,"Operational"
1431.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306030","(Sequence for representation of DART buoy standard hourly report)",,"022182","Water column height","Water column height",,"Operational"
1432.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306031","(Sequence for representation of DART buoy tsunami event reports and extended tsunami event reports)",,"306027","Sequence for representation of DART buoy identification, transmitter ID, type of tsunameter and the time the message is transmitted to the ground system","Buoy ID, transmitter ID, platform type, message transmission time",,"Operational"
1433.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306031","(Sequence for representation of DART buoy tsunami event reports and extended tsunami event reports)",,"306029","Sequence for representation of tsunameter sampling information for water column heights in the time series report","Tsunameter sampling information",,"Operational"
1434.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306031","(Sequence for representation of DART buoy tsunami event reports and extended tsunami event reports)",,"001053","Tsunameter report sequence number triggered by a tsunami event","Tsunameter report sequence number triggered by a tsunami event",,"Operational"
1435.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306031","(Sequence for representation of DART buoy tsunami event reports and extended tsunami event reports)",,"033002","Quality information","Quality information (for message status)",,"Operational"
1436.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306031","(Sequence for representation of DART buoy tsunami event reports and extended tsunami event reports)",,"301011",,"Year, month, day (time when tsunami is detected)",,"Operational"
1437.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306031","(Sequence for representation of DART buoy tsunami event reports and extended tsunami event reports)",,"301013",,"Hour, minute, second",,"Operational"
1438.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306031","(Sequence for representation of DART buoy tsunami event reports and extended tsunami event reports)",,"301011",,"Year, month, day (reference date/time for the time series)",,"Operational"
1439.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306031","(Sequence for representation of DART buoy tsunami event reports and extended tsunami event reports)",,"301013",,"Hour, minute, second",,"Operational"
1440.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306031","(Sequence for representation of DART buoy tsunami event reports and extended tsunami event reports)",,"022185","BPR transmission count","BPR transmission count",,"Operational"
1441.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306031","(Sequence for representation of DART buoy tsunami event reports and extended tsunami event reports)",,"022182","Water column height","Water column height reference for determination of actual value reported in the time series",,"Operational"
1442.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306031","(Sequence for representation of DART buoy tsunami event reports and extended tsunami event reports)",,"004016","Time increment","Time increment added to reset the reference time",,"Operational"
1443.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306031","(Sequence for representation of DART buoy tsunami event reports and extended tsunami event reports)",,"004066","Short time increment","Time increment added to each data value in the time series",,"Operational"
1444.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306031","(Sequence for representation of DART buoy tsunami event reports and extended tsunami event reports)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
1445.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306031","(Sequence for representation of DART buoy tsunami event reports and extended tsunami event reports)",,"031001","Delayed descriptor replication factor","Delayed replication factor",,"Operational"
1446.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306031","(Sequence for representation of DART buoy tsunami event reports and extended tsunami event reports)",,"022184","Water column height deviation from the reference value","Water column height deviation from the reference value",,"Operational"
1455.00,"07","Surface report sequences (land)","307001","(Low altitude station)",,"301031",,"Identification, type, date/time, position (high accuracy), height",,"Operational"
1456.00,"07","Surface report sequences (land)","307001","(Low altitude station)",,"302011","Low altitude station","Basic surface report",,"Operational"
1457.00,"07","Surface report sequences (land)","307002","(Low altitude station)",,"301032",,"Identification, type, date/time, position (coarse accuracy), height",,"Operational"
1458.00,"07","Surface report sequences (land)","307002","(Low altitude station)",,"302011","Low altitude station","Basic surface report",,"Operational"
1459.00,"07","Surface report sequences (land)","307003","(Low altitude station)",,"307001","Low altitude station","Location (high accuracy) and basic report",,"Operational"
1460.00,"07","Surface report sequences (land)","307003","(Low altitude station)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
1461.00,"07","Surface report sequences (land)","307003","(Low altitude station)",,"031001","Delayed descriptor replication factor","Replication factor",,"Operational"
1462.00,"07","Surface report sequences (land)","307003","(Low altitude station)",,"302005",,"Cloud layer information",,"Operational"
1463.00,"07","Surface report sequences (land)","307004","(Low altitude station)",,"307002","Low altitude station","Location (coarse accuracy) and basic report",,"Operational"
1464.00,"07","Surface report sequences (land)","307004","(Low altitude station)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
1465.00,"07","Surface report sequences (land)","307004","(Low altitude station)",,"031001","Delayed descriptor replication factor","Replication factor",,"Operational"
1466.00,"07","Surface report sequences (land)","307004","(Low altitude station)",,"302005",,"Cloud layer information",,"Operational"
1467.00,"07","Surface report sequences (land)","307005","(Low altitude station)",,"307001","Low altitude station","Location (high accuracy) and basic report",,"Operational"
1468.00,"07","Surface report sequences (land)","307005","(Low altitude station)",,"101004","Replication descriptor","Replicate 1 descriptor 4 times",,"Operational"
1469.00,"07","Surface report sequences (land)","307005","(Low altitude station)",,"302005",,"Cloud layer information (4 layers)",,"Operational"
1470.00,"07","Surface report sequences (land)","307006","(Low altitude station)",,"307002","Low altitude station","Location (coarse accuracy) and basic report",,"Operational"
1471.00,"07","Surface report sequences (land)","307006","(Low altitude station)",,"101004","Replication descriptor","Replicate 1 descriptor 4 times",,"Operational"
1472.00,"07","Surface report sequences (land)","307006","(Low altitude station)",,"302005",,"Cloud layer information (4 layers)",,"Operational"
1473.00,"07","Surface report sequences (land)","307007","(High altitude station)",,"301031",,"Identification, type, date/time, position (high accuracy), height",,"Operational"
1474.00,"07","Surface report sequences (land)","307007","(High altitude station)",,"302012","High altitude station","Basic surface report",,"Operational"
1475.00,"07","Surface report sequences (land)","307008","(High altitude station)",,"301032",,"Identification, type, date/time, position (coarse accuracy), height",,"Operational"
1476.00,"07","Surface report sequences (land)","307008","(High altitude station)",,"302012","High altitude station","Basic surface report",,"Operational"
1477.00,"07","Surface report sequences (land)","307009",,,"301031",,"Identification, type, date/time, position (high accuracy), height",,"Operational"
1478.00,"07","Surface report sequences (land)","307009",,,"302013",,"Basic surface report",,"Operational"
1479.00,"07","Surface report sequences (land)","307011","(Main part of data for representation of METAR/SPECI code in BUFR)",,"001063","ICAO location indicator","ICAO location indicator",,"Operational"
1480.00,"07","Surface report sequences (land)","307011","(Main part of data for representation of METAR/SPECI code in BUFR)",,"002001","Type of station","Type of station",,"Operational"
1481.00,"07","Surface report sequences (land)","307011","(Main part of data for representation of METAR/SPECI code in BUFR)",,"301011",,"Year, month, day (YY)",,"Operational"
1482.00,"07","Surface report sequences (land)","307011","(Main part of data for representation of METAR/SPECI code in BUFR)",,"301012",,"GG, gg",,"Operational"
1483.00,"07","Surface report sequences (land)","307011","(Main part of data for representation of METAR/SPECI code in BUFR)",,"301024",,"Latitude-longitude (coarse accuracy), height of station",,"Operational"
1484.00,"07","Surface report sequences (land)","307011","(Main part of data for representation of METAR/SPECI code in BUFR)",,"007006","Height above station","Height above station (= height of an anemometer)",,"Operational"
1485.00,"07","Surface report sequences (land)","307011","(Main part of data for representation of METAR/SPECI code in BUFR)",,"011001","Wind direction","Wind direction",,"Operational"
1486.00,"07","Surface report sequences (land)","307011","(Main part of data for representation of METAR/SPECI code in BUFR)",,"011016","Extreme counterclockwise wind direction of a variable wind","Extreme counterclockwise wind direction of a variable wind",,"Operational"
1487.00,"07","Surface report sequences (land)","307011","(Main part of data for representation of METAR/SPECI code in BUFR)",,"011017","Extreme clockwise wind direction of a variable wind","Extreme clockwise wind direction of a variable wind",,"Operational"
1488.00,"07","Surface report sequences (land)","307011","(Main part of data for representation of METAR/SPECI code in BUFR)",,"011002","Wind speed","Wind speed",,"Operational"
1489.00,"07","Surface report sequences (land)","307011","(Main part of data for representation of METAR/SPECI code in BUFR)",,"011041","Maximum wind gust speed","Maximum wind speed (gusts)",,"Operational"
1490.00,"07","Surface report sequences (land)","307011","(Main part of data for representation of METAR/SPECI code in BUFR)",,"007006","Height above station","Height above station (= height of a thermometer)",,"Operational"
1491.00,"07","Surface report sequences (land)","307011","(Main part of data for representation of METAR/SPECI code in BUFR)",,"012001","Temperature/air temperature","Temperature",,"Operational"
1492.00,"07","Surface report sequences (land)","307011","(Main part of data for representation of METAR/SPECI code in BUFR)",,"012003","Dew-point temperature","Dew-point temperature",,"Operational"
1493.00,"07","Surface report sequences (land)","307011","(Main part of data for representation of METAR/SPECI code in BUFR)",,"010052","Altimeter setting (QNH)","Altimeter setting (QNH)",,"Operational"
1494.00,"07","Surface report sequences (land)","307011","(Main part of data for representation of METAR/SPECI code in BUFR)",,"020009","General weather indicator (TAF/METAR)","General weather indicator TAF/METAR",,"Operational"
1495.00,"07","Surface report sequences (land)","307012","(DvVVVV)",,"103000","Replication descriptor","Delayed replication of 3 descriptors",,"Operational"
1496.00,"07","Surface report sequences (land)","307012","(DvVVVV)",,"031001","Delayed descriptor replication factor","Number of replication (up to 3)",,"Operational"
1497.00,"07","Surface report sequences (land)","307012","(DvVVVV)",,"008023","First-order statistics","First-order statistics",,"Operational"
1498.00,"07","Surface report sequences (land)","307012","(DvVVVV)",,"005021","Bearing or azimuth","Direction of visibility observed",,"Operational"
1499.00,"07","Surface report sequences (land)","307012","(DvVVVV)",,"020001","Horizontal visibility","Horizontal visibility",,"Operational"
1500.00,"07","Surface report sequences (land)","307013","(DRDR/VRVRVRVR)",,"106000","Replication descriptor","Delayed replication of 6 descriptors",,"Operational"
1501.00,"07","Surface report sequences (land)","307013","(DRDR/VRVRVRVR)",,"031001","Delayed descriptor replication factor","Number of replication (up to 4)",,"Operational"
1502.00,"07","Surface report sequences (land)","307013","(DRDR/VRVRVRVR)",,"001064","Runway designator","Runway designator",,"Operational"
1503.00,"07","Surface report sequences (land)","307013","(DRDR/VRVRVRVR)",,"008014","Qualifier for runway visual range","Qualification for runway visual range",,"Operational"
1504.00,"07","Surface report sequences (land)","307013","(DRDR/VRVRVRVR)",,"020061","Runway visual range (RVR)","Runway visual range",,"Operational"
1505.00,"07","Surface report sequences (land)","307013","(DRDR/VRVRVRVR)",,"008014","Qualifier for runway visual range","Qualification for runway visual range",,"Operational"
1506.00,"07","Surface report sequences (land)","307013","(DRDR/VRVRVRVR)",,"020061","Runway visual range (RVR)","Runway visual range",,"Operational"
1507.00,"07","Surface report sequences (land)","307013","(DRDR/VRVRVRVR)",,"020018","Tendency of runway visual range","Tendency of runway visual range",,"Operational"
1508.00,"07","Surface report sequences (land)","307014","(w´w´)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
1509.00,"07","Surface report sequences (land)","307014","(w´w´)",,"031001","Delayed descriptor replication factor","Number of replication (up to 3)",,"Operational"
1510.00,"07","Surface report sequences (land)","307014","(w´w´)",,"020019","Significant present or forecast weather","Significant present weather",,"Operational"
1511.00,"07","Surface report sequences (land)","307015","(Clouds group(s))",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
1512.00,"07","Surface report sequences (land)","307015","(Clouds group(s))",,"031001","Delayed descriptor replication factor","Number of replication",,"Operational"
1513.00,"07","Surface report sequences (land)","307015","(Clouds group(s))",,"302005",,"(NsNsNs, CC, hshshs)",,"Operational"
1514.00,"07","Surface report sequences (land)","307015","(Clouds group(s))",,"020002","Vertical visibility","Vertical visibility",,"Operational"
1515.00,"07","Surface report sequences (land)","307016","(REw´w´)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
1516.00,"07","Surface report sequences (land)","307016","(REw´w´)",,"031001","Delayed descriptor replication factor","Number of replication (up to 3)",,"Operational"
1517.00,"07","Surface report sequences (land)","307016","(REw´w´)",,"020020","Significant recent weather phenomena","Significant recent weather phenomena",,"Operational"
1518.00,"07","Surface report sequences (land)","307017","(Wind shear on runway(s))",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
1519.00,"07","Surface report sequences (land)","307017","(Wind shear on runway(s))",,"031001","Delayed descriptor replication factor","Number of replication",,"Operational"
1520.00,"07","Surface report sequences (land)","307017","(Wind shear on runway(s))",,"011070","Designator of the runway affected by wind shear (including ALL)","Runway designator of the runway affected by wind shear (including ALL)",,"Operational"
1521.00,"07","Surface report sequences (land)","307018","(Trend-type landing forecast)",,"008016","Change qualifier of a trend-type forecast or an aerodrome forecast","Change qualifier of a trend-type forecast or an aerodrome forecast",,"Operational"
1522.00,"07","Surface report sequences (land)","307018","(Trend-type landing forecast)",,"102000","Replication descriptor","Delayed replication of 2 descriptors",,"Operational"
1523.00,"07","Surface report sequences (land)","307018","(Trend-type landing forecast)",,"031001","Delayed descriptor replication factor","Number of replication (up to 2)",,"Operational"
1524.00,"07","Surface report sequences (land)","307018","(Trend-type landing forecast)",,"008017","Qualifier of the time when the forecast change is expected","Qualifier of the time when the forecast change is expected (FM, TL, AT)",,"Operational"
1525.00,"07","Surface report sequences (land)","307018","(Trend-type landing forecast)",,"301012",,"GG, gg",,"Operational"
1526.00,"07","Surface report sequences (land)","307018","(Trend-type landing forecast)",,"104000","Replication descriptor","Delayed replication of 4 descriptor",,"Operational"
1527.00,"07","Surface report sequences (land)","307018","(Trend-type landing forecast)",,"031001","Delayed descriptor replication factor","Number of replication (up to 1)",,"Operational"
1528.00,"07","Surface report sequences (land)","307018","(Trend-type landing forecast)",,"007006","Height above station","Height above station",,"Operational"
1529.00,"07","Surface report sequences (land)","307018","(Trend-type landing forecast)",,"011001","Wind direction","Wind direction",,"Operational"
1530.00,"07","Surface report sequences (land)","307018","(Trend-type landing forecast)",,"011002","Wind speed","Wind speed",,"Operational"
1531.00,"07","Surface report sequences (land)","307018","(Trend-type landing forecast)",,"011041","Maximum wind gust speed","Maximum wind speed (gusts)",,"Operational"
1532.00,"07","Surface report sequences (land)","307018","(Trend-type landing forecast)",,"020009","General weather indicator (TAF/METAR)","General weather indicator",,"Operational"
1533.00,"07","Surface report sequences (land)","307018","(Trend-type landing forecast)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
1534.00,"07","Surface report sequences (land)","307018","(Trend-type landing forecast)",,"031001","Delayed descriptor replication factor","Number of replication (up to 1)",,"Operational"
1535.00,"07","Surface report sequences (land)","307018","(Trend-type landing forecast)",,"020001","Horizontal visibility","Horizontal visibility",,"Operational"
1536.00,"07","Surface report sequences (land)","307018","(Trend-type landing forecast)",,"307014","w´w´","w´w´",,"Operational"
1537.00,"07","Surface report sequences (land)","307020","(Short METAR/SPECI)",,"307011","Main part of data for representation of METAR/SPECI code in BUFR","Main part of data",,"Operational"
1538.00,"07","Surface report sequences (land)","307020","(Short METAR/SPECI)",,"307014","w´w´","w´w´",,"Operational"
1539.00,"07","Surface report sequences (land)","307020","(Short METAR/SPECI)",,"307016","REw´w´","REw´w´",,"Operational"
1540.00,"07","Surface report sequences (land)","307021","(Total sequence for representation of METAR/SPECI code in BUFR)",,"307011","Main part of data for representation of METAR/SPECI code in BUFR","Main part of data",,"Operational"
1541.00,"07","Surface report sequences (land)","307021","(Total sequence for representation of METAR/SPECI code in BUFR)",,"307012","DvVVVV","DvVVVV",,"Operational"
1542.00,"07","Surface report sequences (land)","307021","(Total sequence for representation of METAR/SPECI code in BUFR)",,"307013","DRDR/VRVRVRVR","DRDR/VRVRVRVR",,"Operational"
1543.00,"07","Surface report sequences (land)","307021","(Total sequence for representation of METAR/SPECI code in BUFR)",,"307014","w´w´","w´w´",,"Operational"
1544.00,"07","Surface report sequences (land)","307021","(Total sequence for representation of METAR/SPECI code in BUFR)",,"307015","Clouds group(s)","Clouds group(s)",,"Operational"
1545.00,"07","Surface report sequences (land)","307021","(Total sequence for representation of METAR/SPECI code in BUFR)",,"307016","REw´w´","REw´w´",,"Operational"
1546.00,"07","Surface report sequences (land)","307021","(Total sequence for representation of METAR/SPECI code in BUFR)",,"307017","Wind shear on runways(s)","Wind shear on runway(s)",,"Operational"
1547.00,"07","Surface report sequences (land)","307021","(Total sequence for representation of METAR/SPECI code in BUFR)",,"307018","Trend-type landing forecast","Trend-type landing forecast",,"Operational"
1548.00,"07","Surface report sequences (land)","307021","(Total sequence for representation of METAR/SPECI code in BUFR)",,"307015","Clouds group(s)","Clouds group(s)",,"Operational"
1549.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"001015","Station or site name","Station or site name",,"Operational"
1550.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"301011",,"Year, month, day",,"Operational"
1551.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"301012",,"Hour, minute",,"Operational"
1552.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"301022",,"Latitude (high accuracy), longitude (high accuracy), height of station",,"Operational"
1553.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"008021","Time significance","Time significance (23 = Monitoring period)",,"Operational"
1554.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"004025","Time period or displacement","Time period or displacement",,"Operational"
1555.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"010004","Pressure","Pressure",,"Operational"
1556.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"012001","Temperature/air temperature","Temperature",,"Operational"
1557.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"013003","Relative humidity","Relative humidity",,"Operational"
1558.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"033038","Quality flags for ground-based GNSS data","Quality flags for ground-based GNSS data",,"Operational"
1559.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"008022","Total number (with respect to accumulation or average)","Total number (Number of GNSS satellites used)",,"Operational"
1560.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"106025","Replication descriptor","Replicate next 6 descriptors 25 times",,"Operational"
1561.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"002020","Satellite classification","Satellite classification",,"Operational"
1562.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"001050","Platform transmitter ID number","Platform transmitter identification number",,"Operational"
1563.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"005021","Bearing or azimuth","Azimuth",,"Operational"
1564.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"007021","Elevation","Elevation",,"Operational"
1565.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"015031","Atmospheric path delay in satellite signal","Atmospheric path delay in satellite signal",,"Operational"
1566.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"015032","Estimated error in atmospheric path delay","Estimated error in atmospheric path delay",,"Operational"
1567.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"008060","Sample scanning mode significance","Sample scanning mode significance (= 5 for north/south)",,"Operational"
1568.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"015033","Difference in path delays for limb views at extremes of scan","Difference in path delays for limb views at extremes of scan",,"Operational"
1569.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"015034","Estimated error in path delay difference","Estimated error in path delay difference",,"Operational"
1570.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"008060","Sample scanning mode significance","Sample scanning mode significance (= 6 for east/west)",,"Operational"
1571.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"015033","Difference in path delays for limb views at extremes of scan","Difference in path delays for limb views at extremes of scan",,"Operational"
1572.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"015034","Estimated error in path delay difference","Estimated error in path delay difference",,"Operational"
1573.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"015035","Component of zenith path delay due to water vapour","Component of zenith path delay due to water vapour",,"Operational"
1574.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"201131","Change data width","Change bit width",,"Operational"
1575.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"202129","Change scale","Change scale",,"Operational"
1576.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"013016","Precipitable water","Precipitable water",,"Operational"
1577.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"202000","Change scale","Reset scale",,"Operational"
1578.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"201000","Change data width","Reset bit width",,"Operational"
1579.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"015011","Log 10 of integrated electron density","Log10 of integrated electron density",,"Operational"
1580.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"001063","ICAO location indicator","ICAO location indicator CCCC",,"Operational"
1581.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"008079","Product status","Aviation product status (routine, special, corrected, not available) METAR SPECI COR",,"Operational"
1582.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"002001","Type of station","Type of station(AUTO)",,"Operational"
1583.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"301011",,"Year, month, day YY",,"Operational"
1584.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"301012",,"Hour, minute GGgg",,"Operational"
1585.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"301023",,"Latitude-longitude (coarse accuracy)",,"Operational"
1586.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"007030","Height of station ground above mean sea level","Height of station ground above mean sea level",,"Operational"
1587.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"007031","Height of barometer above mean sea level","Height of barometer above mean sea level",,"Operational"
1588.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above local ground = 10 m (if the actual value is not available)",,"Operational"
1589.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"011001","Wind direction","Wind direction ddd",,"Operational"
1590.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"011016","Extreme counterclockwise wind direction of a variable wind","Extreme counterclockwise wind direction of a variable wind dndndn",,"Operational"
1591.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"011017","Extreme clockwise wind direction of a variable wind","Extreme clockwise wind direction of a variable wind dxdxdx",,"Operational"
1592.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"008054","Qualifier for wind speed or wind gusts","Qualifier for wind speed or wind gusts P",,"Operational"
1593.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"011083","Wind speed","Wind speed (km/h)     ff","(see Note 5)","Operational"
1594.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"011084","Wind speed","Wind speed (knots)     ff","(see Note 5)","Operational"
1595.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"011002","Wind speed","Wind speed (m/s)     ff","(see Note 5)","Operational"
1596.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"008054","Qualifier for wind speed or wind gusts","Qualifier for wind speed or wind gusts     P",,"Operational"
1597.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"011085","Maximum wind gust speed","Maximum wind speed (gusts) (km/h)     fmfm","(see Note 6)","Operational"
1598.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"011086","Maximum wind gust speed","Maximum wind speed (gusts) (knots)     fmfm","(see Note 6)","Operational"
1599.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"011041","Maximum wind gust speed","Maximum wind speed (gusts) (m/s)     fmfm","(see Note 6)","Operational"
1600.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"008054","Qualifier for wind speed or wind gusts","Qualifier for wind speed or wind gusts = missing (to cancel the previous value)",,"Operational"
1601.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above local ground = 2 m (if the actual value is not available)",,"Operational"
1602.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"012023","Temperature","Temperature (Celsius) TT",,"Operational"
1603.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"012024","Dew point temperature","Dew point (Celsius) TdTd",,"Operational"
1604.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above local ground = missing (to cancel the previous value)",,"Operational"
1605.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"010052","Altimeter setting (QNH)","Altimeter setting (QNH) QPHPHPHPH",,"Operational"
1606.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"020009","General weather indicator (TAF/METAR)","General weather indicator TAF/METAR CAVOK",,"Operational"
1607.00,"07","Surface report sequences (land)","307046","(METAR/SPECI visibility)",,"020060","Prevailing horizontal visibility","Prevailing visibility VVVV or VVVVNDV",,"Operational"
1608.00,"07","Surface report sequences (land)","307046","(METAR/SPECI visibility)",,"102000","Replication descriptor","Delayed replication of two descriptors",,"Operational"
1609.00,"07","Surface report sequences (land)","307046","(METAR/SPECI visibility)",,"031001","Delayed descriptor replication factor","Number of replication (up to 2)",,"Operational"
1610.00,"07","Surface report sequences (land)","307046","(METAR/SPECI visibility)",,"005021","Bearing or azimuth","Bearing or azimuth (direction of minimum visibility observed) Dv",,"Operational"
1611.00,"07","Surface report sequences (land)","307046","(METAR/SPECI visibility)",,"020059","Minimum horizontal visibility","Minimum visibility VNVNVNVN",,"Operational"
1612.00,"07","Surface report sequences (land)","307047","(METAR/SPECI/TAF clouds), replacing 3 07 015",,"105000","Replication descriptor","Delayed replication of 5 descriptor",,"Operational"
1613.00,"07","Surface report sequences (land)","307047","(METAR/SPECI/TAF clouds), replacing 3 07 015",,"031001","Delayed descriptor replication factor","Number of replications",,"Operational"
1614.00,"07","Surface report sequences (land)","307047","(METAR/SPECI/TAF clouds), replacing 3 07 015",,"008002","Vertical significance (surface observations)","Vertical significance",,"Operational"
1615.00,"07","Surface report sequences (land)","307047","(METAR/SPECI/TAF clouds), replacing 3 07 015",,"020011","Cloud amount","Cloud amount NsNsNs",,"Operational"
1616.00,"07","Surface report sequences (land)","307047","(METAR/SPECI/TAF clouds), replacing 3 07 015",,"020012","Cloud type","Cloud type CC",,"Operational"
1617.00,"07","Surface report sequences (land)","307047","(METAR/SPECI/TAF clouds), replacing 3 07 015",,"020013","Height of base of cloud","Height of base of cloud (m) hshshs",,"Operational"
1618.00,"07","Surface report sequences (land)","307047","(METAR/SPECI/TAF clouds), replacing 3 07 015",,"020092","Height of base of cloud","Height of base of cloud (feet) hshshs",,"Operational"
1619.00,"07","Surface report sequences (land)","307047","(METAR/SPECI/TAF clouds), replacing 3 07 015",,"020002","Vertical visibility","Vertical visibility (m) VVhshshs",,"Operational"
1620.00,"07","Surface report sequences (land)","307047","(METAR/SPECI/TAF clouds), replacing 3 07 015",,"020091","Vertical visibility","Vertical visibility (feet) VVhshshs",,"Operational"
1621.00,"07","Surface report sequences (land)","307048","(Trend type forecast), replacing 3 07 018",,"008016","Change qualifier of a trend-type forecast or an aerodrome forecast","Change qualifier for trend type forecast TTTTT NOSIG",,"Operational"
1622.00,"07","Surface report sequences (land)","307048","(Trend type forecast), replacing 3 07 018",,"102000","Replication descriptor","Delayed replication of 2 descriptors",,"Operational"
1623.00,"07","Surface report sequences (land)","307048","(Trend type forecast), replacing 3 07 018",,"031001","Delayed descriptor replication factor","Number of replications (0, 1 or 2)",,"Operational"
1624.00,"07","Surface report sequences (land)","307048","(Trend type forecast), replacing 3 07 018",,"008017","Qualifier of the time when the forecast change is expected","Qualifier for time of forecast change TT",,"Operational"
1625.00,"07","Surface report sequences (land)","307048","(Trend type forecast), replacing 3 07 018",,"301012",,"Time of change GGgg",,"Operational"
1626.00,"07","Surface report sequences (land)","307048","(Trend type forecast), replacing 3 07 018",,"112000","Replication descriptor","Delayed replication of 12 descriptors",,"Operational"
1627.00,"07","Surface report sequences (land)","307048","(Trend type forecast), replacing 3 07 018",,"031000","Short delayed descriptor replication factor","Short delayed replication count (0 or 1)",,"Operational"
1628.00,"07","Surface report sequences (land)","307048","(Trend type forecast), replacing 3 07 018",,"007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above local ground = 10 m (if the actual value is not available)",,"Operational"
1629.00,"07","Surface report sequences (land)","307048","(Trend type forecast), replacing 3 07 018",,"011001","Wind direction","Wind direction ddd",,"Operational"
1630.00,"07","Surface report sequences (land)","307048","(Trend type forecast), replacing 3 07 018",,"008054","Qualifier for wind speed or wind gusts","Qualifier for wind speed or wind gusts     P",,"Operational"
1631.00,"07","Surface report sequences (land)","307048","(Trend type forecast), replacing 3 07 018",,"011083","Wind speed","Wind speed (km/h)     ff","(see Note 5)","Operational"
1632.00,"07","Surface report sequences (land)","307048","(Trend type forecast), replacing 3 07 018",,"011084","Wind speed","Wind speed (knots)     ff","(see Note 5)","Operational"
1633.00,"07","Surface report sequences (land)","307048","(Trend type forecast), replacing 3 07 018",,"011002","Wind speed","Wind speed (m/s)     ff","(see Note 5)","Operational"
1634.00,"07","Surface report sequences (land)","307048","(Trend type forecast), replacing 3 07 018",,"008054","Qualifier for wind speed or wind gusts","Qualifier for wind speed or wind gusts     P",,"Operational"
1635.00,"07","Surface report sequences (land)","307048","(Trend type forecast), replacing 3 07 018",,"011085","Maximum wind gust speed","Maximum wind speed (gusts) (km/h)     fmfm","(see Note 6)","Operational"
1636.00,"07","Surface report sequences (land)","307048","(Trend type forecast), replacing 3 07 018",,"011086","Maximum wind gust speed","Maximum wind speed (gusts) (knots)     fmfm","(see Note 6)","Operational"
1637.00,"07","Surface report sequences (land)","307048","(Trend type forecast), replacing 3 07 018",,"011041","Maximum wind gust speed","Maximum wind speed (gusts) (m/s)     fmfm","(see Note 6)","Operational"
1638.00,"07","Surface report sequences (land)","307048","(Trend type forecast), replacing 3 07 018",,"008054","Qualifier for wind speed or wind gusts","Qualifier for wind speed or wind gusts = missing (to cancel the previous value)",,"Operational"
1639.00,"07","Surface report sequences (land)","307048","(Trend type forecast), replacing 3 07 018",,"007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above local ground = missing (to cancel the previous value)",,"Operational"
1640.00,"07","Surface report sequences (land)","307048","(Trend type forecast), replacing 3 07 018",,"020009","General weather indicator (TAF/METAR)","General weather indicator CAVOK NSW NSC",,"Operational"
1641.00,"07","Surface report sequences (land)","307048","(Trend type forecast), replacing 3 07 018",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
1642.00,"07","Surface report sequences (land)","307048","(Trend type forecast), replacing 3 07 018",,"031000","Short delayed descriptor replication factor","Short delayed replication count (0 or 1)",,"Operational"
1643.00,"07","Surface report sequences (land)","307048","(Trend type forecast), replacing 3 07 018",,"020060","Prevailing horizontal visibility","Prevailing visibility VVVV",,"Operational"
1644.00,"07","Surface report sequences (land)","307048","(Trend type forecast), replacing 3 07 018",,"307014","w´w´","Weather intensity and phenomena w´w´",,"Operational"
1645.00,"07","Surface report sequences (land)","307048","(Trend type forecast), replacing 3 07 018",,"307047","METAR/SPECI/TAF clouds, replacing 3 07 015","METAR/SPECI/TAF clouds NsNsNshshshs",,"Operational"
1646.00,"07","Surface report sequences (land)","307049","(Sea conditions WTsTs/SS’)",,"102000","Replication descriptor","Delayed replication of 2 descriptors",,"Operational"
1647.00,"07","Surface report sequences (land)","307049","(Sea conditions WTsTs/SS’)",,"031000","Short delayed descriptor replication factor","Short delayed replication factor (0 or 1)",,"Operational"
1648.00,"07","Surface report sequences (land)","307049","(Sea conditions WTsTs/SS’)",,"022043","Sea/water temperature","Sea/water temperature TsTs",,"Operational"
1649.00,"07","Surface report sequences (land)","307049","(Sea conditions WTsTs/SS’)",,"022021","Height of waves","Height of waves S´",,"Operational"
1650.00,"07","Surface report sequences (land)","307050","(Runway state RDRDR/ERCReReRBRBR)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
1651.00,"07","Surface report sequences (land)","307050","(Runway state RDRDR/ERCReReRBRBR)",,"031000","Short delayed descriptor replication factor","Short delayed replication factor (0 or 1)",,"Operational"
1652.00,"07","Surface report sequences (land)","307050","(Runway state RDRDR/ERCReReRBRBR)",,"020085","General condition of runway","General condition of runway SNOCLO",,"Operational"
1653.00,"07","Surface report sequences (land)","307050","(Runway state RDRDR/ERCReReRBRBR)",,"102000","Replication descriptor","Delayed replication of 2 descriptors",,"Operational"
1654.00,"07","Surface report sequences (land)","307050","(Runway state RDRDR/ERCReReRBRBR)",,"031001","Delayed descriptor replication factor","Number of replications",,"Operational"
1655.00,"07","Surface report sequences (land)","307050","(Runway state RDRDR/ERCReReRBRBR)",,"001064","Runway designator","Runway designator DRDR",,"Operational"
1656.00,"07","Surface report sequences (land)","307050","(Runway state RDRDR/ERCReReRBRBR)",,"020085","General condition of runway","General condition of runway CLRD//",,"Operational"
1657.00,"07","Surface report sequences (land)","307050","(Runway state RDRDR/ERCReReRBRBR)",,"105000","Replication descriptor","Delayed replication of 5 descriptors",,"Operational"
1658.00,"07","Surface report sequences (land)","307050","(Runway state RDRDR/ERCReReRBRBR)",,"031001","Delayed descriptor replication factor","Number of replications",,"Operational"
1659.00,"07","Surface report sequences (land)","307050","(Runway state RDRDR/ERCReReRBRBR)",,"001064","Runway designator","Runway designator DRDR",,"Operational"
1660.00,"07","Surface report sequences (land)","307050","(Runway state RDRDR/ERCReReRBRBR)",,"020086","Runway deposits","Runway deposits ER",,"Operational"
1661.00,"07","Surface report sequences (land)","307050","(Runway state RDRDR/ERCReReRBRBR)",,"020087","Runway contamination","Runway contamination CR",,"Operational"
1662.00,"07","Surface report sequences (land)","307050","(Runway state RDRDR/ERCReReRBRBR)",,"020088","Depth of runway deposits","Depth of runway deposits eReR",,"Operational"
1663.00,"07","Surface report sequences (land)","307050","(Runway state RDRDR/ERCReReRBRBR)",,"020089","Runway friction coefficient","Runway friction coefficient BRBR",,"Operational"
1664.00,"07","Surface report sequences (land)","307051","(Full METAR/SPECI), replacing 3 07 021",,"307045","Main part of METAR/SPECI, replacing 3 07 011","Main part of METAR/SPECI data",,"Operational"
1665.00,"07","Surface report sequences (land)","307051","(Full METAR/SPECI), replacing 3 07 021",,"307046","METAR/SPECI visibility","Visibility VVVV or VVVVNDV VNVNVVVNDV",,"Operational"
1666.00,"07","Surface report sequences (land)","307051","(Full METAR/SPECI), replacing 3 07 021",,"307013","DRDRVRVRVRVR","Runway visual range RDRDR/VRVRVRVR",,"Operational"
1667.00,"07","Surface report sequences (land)","307051","(Full METAR/SPECI), replacing 3 07 021",,"307014","w´w´","Weather intensity and phenomena w´w´",,"Operational"
1668.00,"07","Surface report sequences (land)","307051","(Full METAR/SPECI), replacing 3 07 021",,"307047","METAR/SPECI/TAF clouds, replacing 3 07 015","Clouds NsNsNshshshs",,"Operational"
1669.00,"07","Surface report sequences (land)","307051","(Full METAR/SPECI), replacing 3 07 021",,"307016","REw´w´","Recent weather phenomena REw´w´",,"Operational"
1670.00,"07","Surface report sequences (land)","307051","(Full METAR/SPECI), replacing 3 07 021",,"307017","Wind shear on runways(s)","Runway shear WS RDRDR",,"Operational"
1671.00,"07","Surface report sequences (land)","307051","(Full METAR/SPECI), replacing 3 07 021",,"307049","Sea conditions WTsTs/SS’","Sea conditions WTsTs/SS´",,"Operational"
1672.00,"07","Surface report sequences (land)","307051","(Full METAR/SPECI), replacing 3 07 021",,"307050","Runway state RDRDR/ERCReReRBRBR","Runway state RDRDR/ERCReReRBRBR",,"Operational"
1673.00,"07","Surface report sequences (land)","307051","(Full METAR/SPECI), replacing 3 07 021",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
1674.00,"07","Surface report sequences (land)","307051","(Full METAR/SPECI), replacing 3 07 021",,"031001","Delayed descriptor replication factor","Replication count (0 to 3 normally)",,"Operational"
1675.00,"07","Surface report sequences (land)","307051","(Full METAR/SPECI), replacing 3 07 021",,"307048","Trend type forecast, replacing 3 07 018","Trend type forecast",,"Operational"
1676.00,"07","Surface report sequences (land)","307052","(Aerodrome forecast identification and time interval)",,"001063","ICAO location indicator","ICAO location identifier CCCC",,"Operational"
1677.00,"07","Surface report sequences (land)","307052","(Aerodrome forecast identification and time interval)",,"008039","Time significance (Aviation forecast)","Time significance = 0 (issue time of forecast)",,"Operational"
1678.00,"07","Surface report sequences (land)","307052","(Aerodrome forecast identification and time interval)",,"301011",,"Year, month, day YY",,"Operational"
1679.00,"07","Surface report sequences (land)","307052","(Aerodrome forecast identification and time interval)",,"301012",,"Hour, minute GGgg",,"Operational"
1680.00,"07","Surface report sequences (land)","307052","(Aerodrome forecast identification and time interval)",,"008079","Product status","Aviation product status COR CNL AMD NIL",,"Operational"
1681.00,"07","Surface report sequences (land)","307052","(Aerodrome forecast identification and time interval)",,"008039","Time significance (Aviation forecast)","Time significance = 1 (time of commencement of period of the forecast)",,"Operational"
1682.00,"07","Surface report sequences (land)","307052","(Aerodrome forecast identification and time interval)",,"301011",,"Year, month, day Y1Y1",,"Operational"
1683.00,"07","Surface report sequences (land)","307052","(Aerodrome forecast identification and time interval)",,"301012",,"Hour, minute G1G1",,"Operational"
1684.00,"07","Surface report sequences (land)","307052","(Aerodrome forecast identification and time interval)",,"008039","Time significance (Aviation forecast)","Time significance = 2 (time of ending of period of the forecast)",,"Operational"
1685.00,"07","Surface report sequences (land)","307052","(Aerodrome forecast identification and time interval)",,"301011",,"Year, month, day Y2Y2",,"Operational"
1686.00,"07","Surface report sequences (land)","307052","(Aerodrome forecast identification and time interval)",,"301012",,"Hour, minute G2G2",,"Operational"
1687.00,"07","Surface report sequences (land)","307052","(Aerodrome forecast identification and time interval)",,"301023",,"Latitude-longitude (coarse accuracy)",,"Operational"
1688.00,"07","Surface report sequences (land)","307052","(Aerodrome forecast identification and time interval)",,"007030","Height of station ground above mean sea level","Height of station ground above mean sea level",,"Operational"
1689.00,"07","Surface report sequences (land)","307052","(Aerodrome forecast identification and time interval)",,"007031","Height of barometer above mean sea level","Height of barometer above mean sea level",,"Operational"
1690.00,"07","Surface report sequences (land)","307053","(Forecast weather at an aerodrome)",,"007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above local ground = 10 m (if the actual value is not available)",,"Operational"
1691.00,"07","Surface report sequences (land)","307053","(Forecast weather at an aerodrome)",,"011001","Wind direction","Wind direction ddd",,"Operational"
1692.00,"07","Surface report sequences (land)","307053","(Forecast weather at an aerodrome)",,"008054","Qualifier for wind speed or wind gusts","Qualifier for wind speed or wind gusts     P",,"Operational"
1693.00,"07","Surface report sequences (land)","307053","(Forecast weather at an aerodrome)",,"011083","Wind speed","Wind speed (km/h)     ff","(see Note 5)","Operational"
1694.00,"07","Surface report sequences (land)","307053","(Forecast weather at an aerodrome)",,"011084","Wind speed","Wind speed (knots)     ff","(see Note 5)","Operational"
1695.00,"07","Surface report sequences (land)","307053","(Forecast weather at an aerodrome)",,"011002","Wind speed","Wind speed (m/s)     ff","(see Note 5)","Operational"
1696.00,"07","Surface report sequences (land)","307053","(Forecast weather at an aerodrome)",,"008054","Qualifier for wind speed or wind gusts","Qualifier for wind speed or wind gusts P",,"Operational"
1697.00,"07","Surface report sequences (land)","307053","(Forecast weather at an aerodrome)",,"011085","Maximum wind gust speed","Maximum wind speed (gusts) (km/h)     fmfm","(see Note 6)","Operational"
1698.00,"07","Surface report sequences (land)","307053","(Forecast weather at an aerodrome)",,"011086","Maximum wind gust speed","Maximum wind speed (gusts) (knots)     fmfm","(see Note 6)","Operational"
1699.00,"07","Surface report sequences (land)","307053","(Forecast weather at an aerodrome)",,"011041","Maximum wind gust speed","Maximum wind speed (gusts) (m/s)     fmfm","(see Note 6)","Operational"
1700.00,"07","Surface report sequences (land)","307053","(Forecast weather at an aerodrome)",,"008054","Qualifier for wind speed or wind gusts","Qualifier for wind speed or wind gusts = missing (to cancel the previous value)",,"Operational"
1701.00,"07","Surface report sequences (land)","307053","(Forecast weather at an aerodrome)",,"007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above local ground = missing (to cancel the previous value)",,"Operational"
1702.00,"07","Surface report sequences (land)","307053","(Forecast weather at an aerodrome)",,"020009","General weather indicator (TAF/METAR)","General weather indicator CAVOK NSW NSC",,"Operational"
1703.00,"07","Surface report sequences (land)","307053","(Forecast weather at an aerodrome)",,"020060","Prevailing horizontal visibility","Prevailing visibility VVVV",,"Operational"
1704.00,"07","Surface report sequences (land)","307053","(Forecast weather at an aerodrome)",,"307014","w´w´","Weather w´w´",,"Operational"
1705.00,"07","Surface report sequences (land)","307053","(Forecast weather at an aerodrome)",,"307047","METAR/SPECI/TAF clouds, replacing 3 07 015","Cloud layer(s) NsNsNshshshs",,"Operational"
1706.00,"07","Surface report sequences (land)","307054","(Forecast of extreme temperatures)",,"007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above local ground = 2 m (if the actual value is not available)",,"Operational"
1707.00,"07","Surface report sequences (land)","307054","(Forecast of extreme temperatures)",,"008039","Time significance (Aviation forecast)","Time significance = 3 (forecast time of maximum temperature)",,"Operational"
1708.00,"07","Surface report sequences (land)","307054","(Forecast of extreme temperatures)",,"004003","Day","Day",,"Operational"
1709.00,"07","Surface report sequences (land)","307054","(Forecast of extreme temperatures)",,"004004","Hour","Hour GFGF",,"Operational"
1710.00,"07","Surface report sequences (land)","307054","(Forecast of extreme temperatures)",,"008023","First-order statistics","First-order statistics = 3 (minimum)",,"Operational"
1711.00,"07","Surface report sequences (land)","307054","(Forecast of extreme temperatures)",,"012023","Temperature","Temperature (Celsius) TFTF",,"Operational"
1712.00,"07","Surface report sequences (land)","307054","(Forecast of extreme temperatures)",,"008039","Time significance (Aviation forecast)","Time significance = 4 (forecast time of minimum temperature)",,"Operational"
1713.00,"07","Surface report sequences (land)","307054","(Forecast of extreme temperatures)",,"004003","Day","Day",,"Operational"
1714.00,"07","Surface report sequences (land)","307054","(Forecast of extreme temperatures)",,"004004","Hour","Hour GFGF",,"Operational"
1715.00,"07","Surface report sequences (land)","307054","(Forecast of extreme temperatures)",,"008023","First-order statistics","First-order statistics = 2 (maximum)",,"Operational"
1716.00,"07","Surface report sequences (land)","307054","(Forecast of extreme temperatures)",,"012023","Temperature","Temperature (Celsius) TFTF",,"Operational"
1717.00,"07","Surface report sequences (land)","307054","(Forecast of extreme temperatures)",,"008023","First-order statistics","First-order statistics = missing (to cancel the previous value)",,"Operational"
1718.00,"07","Surface report sequences (land)","307054","(Forecast of extreme temperatures)",,"007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above local ground = missing (to cancel the previous value)",,"Operational"
1719.00,"07","Surface report sequences (land)","307055","(Change indicator and forecast changes)",,"033045","Probability of following event","Probability of following event C2C2",,"Operational"
1720.00,"07","Surface report sequences (land)","307055","(Change indicator and forecast changes)",,"008016","Change qualifier of a trend-type forecast or an aerodrome forecast","Change qualifier for an aerodrome forecast TTTTTT",,"Operational"
1721.00,"07","Surface report sequences (land)","307055","(Change indicator and forecast changes)",,"008039","Time significance (Aviation forecast)","Time significance = 5 (time of beginning of the forecast change)",,"Operational"
1722.00,"07","Surface report sequences (land)","307055","(Change indicator and forecast changes)",,"004003","Day","Day",,"Operational"
1723.00,"07","Surface report sequences (land)","307055","(Change indicator and forecast changes)",,"301012",,"Hour, minute GGgg",,"Operational"
1724.00,"07","Surface report sequences (land)","307055","(Change indicator and forecast changes)",,"008039","Time significance (Aviation forecast)","Time significance = 6 (time of ending of the forecast change)",,"Operational"
1725.00,"07","Surface report sequences (land)","307055","(Change indicator and forecast changes)",,"004003","Day","Day",,"Operational"
1726.00,"07","Surface report sequences (land)","307055","(Change indicator and forecast changes)",,"301012",,"Hour, minute GeGe",,"Operational"
1727.00,"07","Surface report sequences (land)","307055","(Change indicator and forecast changes)",,"307053","Forecast weather at an aerodrome","Forecast conditions during or after change",,"Operational"
1728.00,"07","Surface report sequences (land)","307056","(Aerodrome forecast - full TAF)",,"307052","Aerodrome forecast identification and time interval","Identification and time interval",,"Operational"
1729.00,"07","Surface report sequences (land)","307056","(Aerodrome forecast - full TAF)",,"307053","Forecast weather at an aerodrome","Forecast",,"Operational"
1730.00,"07","Surface report sequences (land)","307056","(Aerodrome forecast - full TAF)",,"307054","Forecast of extreme temperatures","Extreme temperature forecast",,"Operational"
1731.00,"07","Surface report sequences (land)","307056","(Aerodrome forecast - full TAF)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
1732.00,"07","Surface report sequences (land)","307056","(Aerodrome forecast - full TAF)",,"031001","Delayed descriptor replication factor","Replication factor",,"Operational"
1733.00,"07","Surface report sequences (land)","307056","(Aerodrome forecast - full TAF)",,"307055","Change indicator and forecast changes","Forecast change",,"Operational"
1734.00,"07","Surface report sequences (land)","307063",,,"007061","Depth below land surface","Depth below land surface",,"Operational"
1735.00,"07","Surface report sequences (land)","307063",,,"012130","Soil temperature","Soil temperature (scale 2)",,"Operational"
1736.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)",,"301090","Surface station identification; time, horizontal and vertical co-ordinates","Surface station identification; date and time, horizontal and vertical co-ordinates","(see Note 1)","Operational"
1737.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)",,"004074","Short time period or displacement","Short time displacement (= UTC - LST)","(see Note 1)","Operational"
1738.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)",,"004023","Time period or displacement","Time period (= number of days in the month)",,"Operational"
1739.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Monthly mean values of pressure, temperature, extreme temperatures and vapour pressure:","008023","First-order statistics","First-order statistics (= 4, mean value)",,"Operational"
1740.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Monthly mean values of pressure, temperature, extreme temperatures and vapour pressure:","010004","Pressure","Pressure",,"Operational"
1741.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Monthly mean values of pressure, temperature, extreme temperatures and vapour pressure:","010051","Pressure reduced to mean sea level","Pressure reduced to mean sea level",,"Operational"
1742.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Monthly mean values of pressure, temperature, extreme temperatures and vapour pressure:","007004","Pressure","Pressure (standard level) (for lowland stations = missing value)",,"Operational"
1743.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Monthly mean values of pressure, temperature, extreme temperatures and vapour pressure:","010009","Geopotential height","Geopotential height of the standard level (for lowland stations = missing value)",,"Operational"
1744.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Monthly mean values of pressure, temperature, extreme temperatures and vapour pressure:","007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above local ground","(see Note 3)","Operational"
1745.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Monthly mean values of pressure, temperature, extreme temperatures and vapour pressure:","012101","Temperature/air temperature","Temperature/air temperature",,"Operational"
1746.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Monthly mean values of pressure, temperature, extreme temperatures and vapour pressure:","002051","Indicator to specify observing method for extreme temperatures","Indicator to specify observing method for extreme temperatures",,"Operational"
1747.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Monthly mean values of pressure, temperature, extreme temperatures and vapour pressure:","004051","Principal time of daily reading of maximum temperature","Principal time of daily reading of maximum temperature",,"Operational"
1748.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Monthly mean values of pressure, temperature, extreme temperatures and vapour pressure:","012118","Maximum temperature at height specified, past 24 hours","Maximum temperature at height specified, past 24 hours",,"Operational"
1749.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Monthly mean values of pressure, temperature, extreme temperatures and vapour pressure:","004052","Principal time of daily reading of minimum temperature","Principal time of daily reading of minimum temperature",,"Operational"
1750.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Monthly mean values of pressure, temperature, extreme temperatures and vapour pressure:","012119","Minimum temperature at height specified, past 24 hours","Minimum temperature at height specified, past 24 hours",,"Operational"
1751.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Monthly mean values of pressure, temperature, extreme temperatures and vapour pressure:","013004","Vapour pressure","Vapour pressure",,"Operational"
1752.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Monthly mean values of pressure, temperature, extreme temperatures and vapour pressure:","008023","First-order statistics","First-order statistics (= 63, missing value)",,"Operational"
1753.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Monthly mean values of pressure, temperature, extreme temperatures and vapour pressure:","012151","Standard deviation of daily mean temperature","Standard deviation of daily mean temperature",,"Operational"
1754.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Monthly mean values of pressure, temperature, extreme temperatures and vapour pressure:","007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above local ground (set to missing to cancel the previous value)",,"Operational"
1755.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Monthly mean values of pressure, temperature, extreme temperatures and vapour pressure:","102005","Replication descriptor","Replicate 2 descriptors 5 times",,"Operational"
1756.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Monthly mean values of pressure, temperature, extreme temperatures and vapour pressure:","008050","Qualifier for number of missing values in calculation of statistic","Qualifier for number of missing values in calculation of statistic   = 1 (pressure)   = 2 (temperature)   = 4 (vapour pressure)   = 7 (maximum temperature)   = 8 (minimum temperature)",,"Operational"
1757.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Monthly mean values of pressure, temperature, extreme temperatures and vapour pressure:","008020","Total number of missing entities (with respect to accumulation or average)","Total number of missing entities (days)",,"Operational"
1758.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Sunshine duration","014032","Total sunshine","Total sunshine",,"Operational"
1759.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Sunshine duration","014033","Total sunshine","Total sunshine",,"Operational"
1760.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Sunshine duration","008050","Qualifier for number of missing values in calculation of statistic","Qualifier for number of missing values in calculation of statistic = 6 (sunshine duration)",,"Operational"
1761.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Sunshine duration","008020","Total number of missing entities (with respect to accumulation or average)","Total number of missing entities (days)",,"Operational"
1762.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Numbers of days of occurrence","102018","Replication descriptor","Replicate 2 descriptors 18 times",,"Operational"
1763.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Numbers of days of occurrence","008052","Condition for which number of days of occurrence follows","Conditions for which number of days of occurrence follows",,"Operational"
1764.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Numbers of days of occurrence","008022","Total number (with respect to accumulation or average)","Total number (of days)",,"Operational"
1765.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme values of temperature and wind speed:","007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above local ground","(see Note 3)","Operational"
1766.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme values of temperature and wind speed:","008053","Day of occurrence qualifier","Day of occurrence qualifier = 0 (on 1 day only); = 1 (on 2 or more days)",,"Operational"
1767.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme values of temperature and wind speed:","004003","Day","Day",,"Operational"
1768.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme values of temperature and wind speed:","012152","Highest daily mean temperature","Highest daily mean temperature",,"Operational"
1769.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme values of temperature and wind speed:","008053","Day of occurrence qualifier","Day of occurrence qualifier = 0 (on 1 day only); = 1 (on 2 or more days)",,"Operational"
1770.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme values of temperature and wind speed:","004003","Day","Day",,"Operational"
1771.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme values of temperature and wind speed:","012153","Lowest daily mean temperature","Lowest daily mean temperature",,"Operational"
1772.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme values of temperature and wind speed:","008053","Day of occurrence qualifier","Day of occurrence qualifier = 0 (on 1 day only); = 1 (on 2 or more days)",,"Operational"
1773.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme values of temperature and wind speed:","004003","Day","Day",,"Operational"
1774.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme values of temperature and wind speed:","008023","First-order statistics","First-order statistics (= 2; maximum value)",,"Operational"
1775.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme values of temperature and wind speed:","012101","Temperature/air temperature","Temperature/air temperature",,"Operational"
1776.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme values of temperature and wind speed:","008053","Day of occurrence qualifier","Day of occurrence qualifier = 0 (on 1 day only); = 1 (on 2 or more days)",,"Operational"
1777.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme values of temperature and wind speed:","004003","Day","Day",,"Operational"
1778.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme values of temperature and wind speed:","008023","First-order statistics","First-order statistics (= 3; minimum value)",,"Operational"
1779.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme values of temperature and wind speed:","012101","Temperature/air temperature","Temperature/air temperature",,"Operational"
1780.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme values of temperature and wind speed:","008023","First-order statistics","First-order statistics (= 63; missing value)",,"Operational"
1781.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme values of temperature and wind speed:","007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above local ground","(see Note 3)","Operational"
1782.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme values of temperature and wind speed:","002002","Type of instrumentation for wind measurement","Type of instrumentation for wind measurement",,"Operational"
1783.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme values of temperature and wind speed:","008053","Day of occurrence qualifier","Day of occurrence qualifier = 0 (on 1 day only); = 1 (on 2 or more days)",,"Operational"
1784.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme values of temperature and wind speed:","004003","Day","Day",,"Operational"
1785.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme values of temperature and wind speed:","011046","Maximum instantaneous wind speed","Maximum instantaneous wind speed",,"Operational"
1786.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme values of temperature and wind speed:","008053","Day of occurrence qualifier","Day of occurrence qualifier (set to missing = 3 to cancel the previous value)",,"Operational"
1787.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Precipitation:","004003","Day","Day (= 1)","(see Note 2)","Operational"
1788.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Precipitation:","004004","Hour","Hour (= 6)","(see Note 2)","Operational"
1789.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Precipitation:","004023","Time period or displacement","Time period (= number of days in the month)","(see Note 2)","Operational"
1790.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Precipitation:","007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above local ground","(see Note 3)","Operational"
1791.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Precipitation:","013060","Total accumulated precipitation","Total accumulated precipitation",,"Operational"
1792.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Precipitation:","013051","Frequency group, precipitation","Frequency group; precipitation",,"Operational"
1793.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Precipitation:","004053","Number of days with precipitation equal to or more than 1 mm","Number of days with precipitation equal to or more than 1 mm",,"Operational"
1794.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Precipitation:","008050","Qualifier for number of missing values in calculation of statistic","Qualifier for number of missing values in calculation of statistic = 5 (precipitation)",,"Operational"
1795.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Precipitation:","008020","Total number of missing entities (with respect to accumulation or average)","Total number of missing entities (days)",,"Operational"
1796.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Numbers of days of occurrence:","102006","Replication descriptor","Replicate 2 descriptors 6 times",,"Operational"
1797.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Numbers of days of occurrence:","008052","Condition for which number of days of occurrence follows","Conditions for which number of days of occurrence follows",,"Operational"
1798.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Numbers of days of occurrence:","008022","Total number (with respect to accumulation or average)","Total number (of days)",,"Operational"
1799.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme precipitation:","008053","Day of occurrence qualifier","Day of occurrence qualifier = 0 (on 1 day only); = 1 (on 2 or more days)",,"Operational"
1800.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme precipitation:","004003","Day","Day",,"Operational"
1801.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme precipitation:","013052","Highest daily amount of precipitation","Highest daily amount of precipitation",,"Operational"
1802.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme precipitation:","007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above local ground (set to missing to cancel the previous value)",,"Operational"
1803.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)",,"004001","Year","Year (of beginning of the reference period)",,"Operational"
1804.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)",,"004001","Year","Year (of ending of the reference period)",,"Operational"
1805.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)",,"004002","Month","Month",,"Operational"
1806.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)",,"004003","Day","Day (= 1)","(see Note 1)","Operational"
1807.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)",,"004004","Hour","Hour (= 0)","(see Note 1)","Operational"
1808.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)",,"004074","Short time period or displacement","Short time displacement (= UTC - LST)","(see Note 1)","Operational"
1809.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)",,"004022","Time period or displacement","Time period (= 1)",,"Operational"
1810.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of monthly mean pressure, temperature, vapour pressure and of standard deviation:","008023","First-order statistics","First-order statistics (= 4; mean value)",,"Operational"
1811.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of monthly mean pressure, temperature, vapour pressure and of standard deviation:","010004","Pressure","Pressure",,"Operational"
1812.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of monthly mean pressure, temperature, vapour pressure and of standard deviation:","010051","Pressure reduced to mean sea level","Pressure reduced to mean sea level",,"Operational"
1813.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of monthly mean pressure, temperature, vapour pressure and of standard deviation:","007004","Pressure","Pressure (standard level)",,"Operational"
1814.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of monthly mean pressure, temperature, vapour pressure and of standard deviation:","010009","Geopotential height","Geopotential height of the standard level",,"Operational"
1815.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of monthly mean pressure, temperature, vapour pressure and of standard deviation:","007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above local ground","(see Note 3)","Operational"
1816.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of monthly mean pressure, temperature, vapour pressure and of standard deviation:","012101","Temperature/air temperature","Temperature/air temperature",,"Operational"
1817.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of monthly mean pressure, temperature, vapour pressure and of standard deviation:","002051","Indicator to specify observing method for extreme temperatures","Indicator to specify observing method for extreme temperatures = 2",,"Operational"
1818.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of monthly mean pressure, temperature, vapour pressure and of standard deviation:","004051","Principal time of daily reading of maximum temperature","Principal time of daily reading of maximum temperature",,"Operational"
1819.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of monthly mean pressure, temperature, vapour pressure and of standard deviation:","012118","Maximum temperature at height specified, past 24 hours","Maximum temperature at height specified, past 24 hours",,"Operational"
1820.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of monthly mean pressure, temperature, vapour pressure and of standard deviation:","004052","Principal time of daily reading of minimum temperature","Principal time of daily reading of minimum temperature",,"Operational"
1821.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of monthly mean pressure, temperature, vapour pressure and of standard deviation:","012119","Minimum temperature at height specified, past 24 hours","Minimum temperature at height specified, past 24 hours",,"Operational"
1822.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of monthly mean pressure, temperature, vapour pressure and of standard deviation:","013004","Vapour pressure","Vapour pressure",,"Operational"
1823.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of monthly mean pressure, temperature, vapour pressure and of standard deviation:","012151","Standard deviation of daily mean temperature","Standard deviation of daily mean temperature",,"Operational"
1824.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of monthly mean pressure, temperature, vapour pressure and of standard deviation:","007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above local ground (set to missing to cancel the previous value)",,"Operational"
1825.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normal of sunshine duration:","014032","Total sunshine","Total sunshine",,"Operational"
1826.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normal of sunshine duration:","008023","First-order statistics","First-order statistics (= 63; missing value)",,"Operational"
1827.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of precipitation:","004001","Year","Year (of beginning of the reference period)",,"Operational"
1828.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of precipitation:","004001","Year","Year (of ending of the reference period)",,"Operational"
1829.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of precipitation:","004002","Month","Month",,"Operational"
1830.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of precipitation:","004003","Day","Day (= 1)","(see Note 2)","Operational"
1831.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of precipitation:","004004","Hour","Hour (= 6)","(see Note 2)","Operational"
1832.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of precipitation:","004022","Time period or displacement","Time period (= 1)",,"Operational"
1833.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of precipitation:","007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above local ground","(see Note 3)","Operational"
1834.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of precipitation:","008023","First-order statistics","First-order statistics (= 4; mean value)",,"Operational"
1835.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of precipitation:","013060","Total accumulated precipitation","Total accumulated precipitation",,"Operational"
1836.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of precipitation:","004053","Number of days with precipitation equal to or more than 1 mm","Number of days with precipitation equal to or more than 1 mm",,"Operational"
1837.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of precipitation:","008023","First-order statistics","First-order statistics (= 63; missing value)",,"Operational"
1838.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of precipitation:","102008","Replication descriptor","Replicate 2 descriptors 8 times",,"Operational"
1839.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of precipitation:","008050","Qualifier for number of missing values in calculation of statistic","Qualifier for number of missing values in calculation of statistic   = 1 (pressure)   = 2 (temperature)   = 3 (extreme temperatures)   = 4 (vapour pressure)   = 5 (precipitation)   = 6 (sunshine duration)   = 7 (maximum temperature)  = 8 (minimum temperature)","(see Note 4)","Operational"
1840.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of precipitation:","008020","Total number of missing entities (with respect to accumulation or average)","Total number of missing entities (years)","(see Note 4)","Operational"
1841.00,"07","Surface report sequences (land)","307073","(Representation of CLIMAT data of the actual month and for monthly normals)",,"307071","Monthly values of a land station","Monthly values of a land station",,"Operational"
1842.00,"07","Surface report sequences (land)","307073","(Representation of CLIMAT data of the actual month and for monthly normals)",,"307072","Monthly normals for a land station","Monthly normals for a land station",,"Operational"
1843.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"301090","Surface station identification; time, horizontal and vertical co-ordinates","Fixed surface station identification, time, horizontal and vertical coordinates",,"Operational"
1844.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"302031","Pressure information","Pressure data",,"Operational"
1845.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"302035","Basic synoptic ""instantaneous"" data","Basic synoptic ""instantaneous"" data",,"Operational"
1846.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"302036","Clouds with bases below station level","Clouds with bases below station level",,"Operational"
1847.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
1848.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"031000","Short delayed descriptor replication factor","Short delayed descriptor replication factor",,"Operational"
1849.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"302047","Direction of cloud drift","Direction of cloud drift",,"Operational"
1850.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"008002","Vertical significance (surface observations)","Vertical significance",,"Operational"
1851.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
1852.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"031000","Short delayed descriptor replication factor","Short delayed descriptor replication factor",,"Operational"
1853.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"302048","Direction and elevation of cloud","Direction and elevation of cloud",,"Operational"
1854.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"302037","State of ground, snow depth, ground minimum temperature","State of ground, snow depth, ground minimum temperature",,"Operational"
1855.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"102000","Replication descriptor","Delayed replication of 2 descriptors",,"Operational"
1856.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"031000","Short delayed descriptor replication factor","Short delayed descriptor replication factor",,"Operational"
1857.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"022061","State of the sea","State of the sea",,"Operational"
1858.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"020058","Visibility seawards from a coastal station","Visibility seawards from a coastal station",,"Operational"
1859.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
1860.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"031000","Short delayed descriptor replication factor","Short delayed descriptor replication factor",,"Operational"
1861.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"302056","Sea/water temperature","Sea/water surface temperature, method of measurement, depth below water surface",,"Operational"
1862.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
1863.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"031000","Short delayed descriptor replication factor","Short delayed descriptor replication factor",,"Operational"
1864.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"302055","Icing and ice","Icing and ice",,"Operational"
1865.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"302043","Basic synoptic ""period"" data","Basic synoptic ""period"" data",,"Operational"
1866.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"302044","Evaporation data","Evaporation data",,"Operational"
1867.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
1868.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"031001","Delayed descriptor replication factor","Delayed descriptor replication factor",,"Operational"
1869.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"302045","Radiation data (from 1 hour and 24 hour period)","Radiation data",,"Operational"
1870.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
1871.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"031000","Short delayed descriptor replication factor","Short delayed descriptor replication factor",,"Operational"
1872.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"302046","Temperature change","Temperature change",,"Operational"
1873.00,"07","Surface report sequences (land)","307080","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data)",,"301090","Surface station identification; time, horizontal and vertical co-ordinates","Fixed surface station identification, time, horizontal and vertical coordinates",,"Operational"
1874.00,"07","Surface report sequences (land)","307080","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data)",,"302031","Pressure information","Pressure data",,"Operational"
1875.00,"07","Surface report sequences (land)","307080","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data)",,"302035","Basic synoptic ""instantaneous"" data","Basic synoptic ""instantaneous"" data",,"Operational"
1876.00,"07","Surface report sequences (land)","307080","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data)",,"302036","Clouds with bases below station level","Clouds with bases below station level",,"Operational"
1877.00,"07","Surface report sequences (land)","307080","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data)",,"302047","Direction of cloud drift","Direction of cloud drift",,"Operational"
1878.00,"07","Surface report sequences (land)","307080","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data)",,"008002","Vertical significance (surface observations)","Vertical significance",,"Operational"
1879.00,"07","Surface report sequences (land)","307080","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data)",,"302048","Direction and elevation of cloud","Direction and elevation of cloud",,"Operational"
1880.00,"07","Surface report sequences (land)","307080","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data)",,"302037","State of ground, snow depth, ground minimum temperature","State of ground, snow depth, ground minimum temperature",,"Operational"
1881.00,"07","Surface report sequences (land)","307080","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data)",,"302043","Basic synoptic ""period"" data","Basic synoptic ""period"" data",,"Operational"
1882.00,"07","Surface report sequences (land)","307080","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data)",,"302044","Evaporation data","Evaporation data",,"Operational"
1883.00,"07","Surface report sequences (land)","307080","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data)",,"101002","Replication descriptor","Replicate next descriptor 2 times",,"Operational"
1884.00,"07","Surface report sequences (land)","307080","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data)",,"302045","Radiation data (from 1 hour and 24 hour period)","Radiation data (from 1 hour and/or 24 hour period)",,"Operational"
1885.00,"07","Surface report sequences (land)","307080","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data)",,"302046","Temperature change","Temperature change",,"Operational"
1886.00,"07","Surface report sequences (land)","307081","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA I)",,"301090","Surface station identification; time, horizontal and vertical co-ordinates","Fixed surface station identification, time, horizontal and vertical coordinates",,"Operational"
1887.00,"07","Surface report sequences (land)","307081","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA I)",,"302031","Pressure information","Pressure data",,"Operational"
1888.00,"07","Surface report sequences (land)","307081","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA I)",,"302035","Basic synoptic ""instantaneous"" data","Basic synoptic ""instantaneous"" data",,"Operational"
1889.00,"07","Surface report sequences (land)","307081","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA I)",,"302036","Clouds with bases below station level","Clouds with bases below station level",,"Operational"
1890.00,"07","Surface report sequences (land)","307081","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA I)",,"302047","Direction of cloud drift","Direction of cloud drift",,"Operational"
1891.00,"07","Surface report sequences (land)","307081","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA I)",,"008002","Vertical significance (surface observations)","Vertical significance (= missing to cancel the previous value)",,"Operational"
1892.00,"07","Surface report sequences (land)","307081","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA I)",,"302048","Direction and elevation of cloud","Direction and elevation of cloud",,"Operational"
1893.00,"07","Surface report sequences (land)","307081","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA I)",,"302037","State of ground, snow depth, ground minimum temperature","State of ground, snow depth, ground minimum temperature",,"Operational"
1894.00,"07","Surface report sequences (land)","307081","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA I)",,"012122","Ground minimum temperature of the preceding night","Ground minimum temperature of the preceding night",,"Operational"
1895.00,"07","Surface report sequences (land)","307081","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA I)",,"013056","Character and intensity of precipitation","Character and intensity of precipitation",,"Operational"
1896.00,"07","Surface report sequences (land)","307081","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA I)",,"013057","Time of beginning or end of precipitation","Time of beginning or end of precipitation",,"Operational"
1897.00,"07","Surface report sequences (land)","307081","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA I)",,"020101","Locust (acridian) name","Locust (acridian) name",,"Operational"
1898.00,"07","Surface report sequences (land)","307081","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA I)",,"020102","Locust (maturity) color","Locust (maturity) colour",,"Operational"
1899.00,"07","Surface report sequences (land)","307081","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA I)",,"020103","Stage of development of locusts","Stage of development of locusts",,"Operational"
1900.00,"07","Surface report sequences (land)","307081","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA I)",,"020104","Organization state of swarm or band of locusts","Organization state of swarm or band of locusts",,"Operational"
1901.00,"07","Surface report sequences (land)","307081","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA I)",,"020105","Size of swarm or band of locusts and duration of passage of swarm","Size of swarm or band of locusts and duration of passage of swarm",,"Operational"
1902.00,"07","Surface report sequences (land)","307081","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA I)",,"020106","Locust population density","Locust population density",,"Operational"
1903.00,"07","Surface report sequences (land)","307081","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA I)",,"020107","Direction of movements of locust swarm","Direction of movements of locust swarm",,"Operational"
1904.00,"07","Surface report sequences (land)","307081","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA I)",,"020108","Extent of vegetation","Extent of vegetation",,"Operational"
1905.00,"07","Surface report sequences (land)","307081","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA I)",,"302043","Basic synoptic ""period"" data","Basic synoptic ""period"" data",,"Operational"
1906.00,"07","Surface report sequences (land)","307081","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA I)",,"302044","Evaporation data","Evaporation data",,"Operational"
1907.00,"07","Surface report sequences (land)","307081","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA I)",,"101002","Replication descriptor","Replicate next descriptor 2 times",,"Operational"
1908.00,"07","Surface report sequences (land)","307081","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA I)",,"302045","Radiation data (from 1 hour and 24 hour period)","Radiation data (from 1 hour and/or 24 hour period)",,"Operational"
1909.00,"07","Surface report sequences (land)","307081","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA I)",,"302046","Temperature change","Temperature change",,"Operational"
1910.00,"07","Surface report sequences (land)","307082","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA II)",,"301090","Surface station identification; time, horizontal and vertical co-ordinates","Fixed surface station identification, time, horizontal and vertical coordinates",,"Operational"
1911.00,"07","Surface report sequences (land)","307082","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA II)",,"302031","Pressure information","Pressure data",,"Operational"
1912.00,"07","Surface report sequences (land)","307082","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA II)",,"302035","Basic synoptic ""instantaneous"" data","Basic synoptic ""instantaneous"" data",,"Operational"
1913.00,"07","Surface report sequences (land)","307082","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA II)",,"302036","Clouds with bases below station level","Clouds with bases below station level",,"Operational"
1914.00,"07","Surface report sequences (land)","307082","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA II)",,"302047","Direction of cloud drift","Direction of cloud drift",,"Operational"
1915.00,"07","Surface report sequences (land)","307082","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA II)",,"008002","Vertical significance (surface observations)","Vertical significance (= missing to cancel the previous value)",,"Operational"
1916.00,"07","Surface report sequences (land)","307082","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA II)",,"302048","Direction and elevation of cloud","Direction and elevation of cloud",,"Operational"
1917.00,"07","Surface report sequences (land)","307082","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA II)",,"302037","State of ground, snow depth, ground minimum temperature","State of ground, snow depth, ground minimum temperature",,"Operational"
1918.00,"07","Surface report sequences (land)","307082","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA II)",,"012121","Ground minimum temperature","Ground minimum temperature (at the time of observation)",,"Operational"
1919.00,"07","Surface report sequences (land)","307082","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA II)",,"012122","Ground minimum temperature of the preceding night","Ground minimum temperature of the preceding night",,"Operational"
1920.00,"07","Surface report sequences (land)","307082","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA II)",,"302043","Basic synoptic ""period"" data","Basic synoptic ""period"" data",,"Operational"
1921.00,"07","Surface report sequences (land)","307082","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA II)",,"302044","Evaporation data","Evaporation data",,"Operational"
1922.00,"07","Surface report sequences (land)","307082","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA II)",,"101002","Replication descriptor","Replicate next descriptor 2 times",,"Operational"
1923.00,"07","Surface report sequences (land)","307082","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA II)",,"302045","Radiation data (from 1 hour and 24 hour period)","Radiation data (from 1 hour and/or 24 hour period)",,"Operational"
1924.00,"07","Surface report sequences (land)","307082","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA II)",,"302046","Temperature change","Temperature change",,"Operational"
1925.00,"07","Surface report sequences (land)","307083","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA III)",,"301090","Surface station identification; time, horizontal and vertical co-ordinates","Fixed surface station identification, time, horizontal and vertical coordinates",,"Operational"
1926.00,"07","Surface report sequences (land)","307083","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA III)",,"302031","Pressure information","Pressure data",,"Operational"
1927.00,"07","Surface report sequences (land)","307083","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA III)",,"302035","Basic synoptic ""instantaneous"" data","Basic synoptic ""instantaneous"" data",,"Operational"
1928.00,"07","Surface report sequences (land)","307083","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA III)",,"302036","Clouds with bases below station level","Clouds with bases below station level",,"Operational"
1929.00,"07","Surface report sequences (land)","307083","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA III)",,"302047","Direction of cloud drift","Direction of cloud drift",,"Operational"
1930.00,"07","Surface report sequences (land)","307083","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA III)",,"008002","Vertical significance (surface observations)","Vertical significance (= missing to cancel the previous value)",,"Operational"
1931.00,"07","Surface report sequences (land)","307083","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA III)",,"302048","Direction and elevation of cloud","Direction and elevation of cloud",,"Operational"
1932.00,"07","Surface report sequences (land)","307083","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA III)",,"302037","State of ground, snow depth, ground minimum temperature","State of ground, snow depth, ground minimum temperature",,"Operational"
1933.00,"07","Surface report sequences (land)","307083","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA III)",,"012122","Ground minimum temperature of the preceding night","Ground minimum temperature of the preceding night",,"Operational"
1934.00,"07","Surface report sequences (land)","307083","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA III)",,"302043","Basic synoptic ""period"" data","Basic synoptic ""period"" data",,"Operational"
1935.00,"07","Surface report sequences (land)","307083","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA III)",,"302044","Evaporation data","Evaporation data",,"Operational"
1936.00,"07","Surface report sequences (land)","307083","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA III)",,"101002","Replication descriptor","Replicate next descriptor 2 times",,"Operational"
1937.00,"07","Surface report sequences (land)","307083","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA III)",,"302045","Radiation data (from 1 hour and 24 hour period)","Radiation data (from 1 hour and/or 24 hour period)",,"Operational"
1938.00,"07","Surface report sequences (land)","307083","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA III)",,"302046","Temperature change","Temperature change",,"Operational"
1939.00,"07","Surface report sequences (land)","307084","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA IV)",,"301090","Surface station identification; time, horizontal and vertical co-ordinates","Fixed surface station identification, time, horizontal and vertical coordinates",,"Operational"
1940.00,"07","Surface report sequences (land)","307084","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA IV)",,"302031","Pressure information","Pressure data",,"Operational"
1941.00,"07","Surface report sequences (land)","307084","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA IV)",,"302035","Basic synoptic ""instantaneous"" data","Basic synoptic ""instantaneous"" data",,"Operational"
1942.00,"07","Surface report sequences (land)","307084","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA IV)",,"302036","Clouds with bases below station level","Clouds with bases below station level",,"Operational"
1943.00,"07","Surface report sequences (land)","307084","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA IV)",,"302047","Direction of cloud drift","Direction of cloud drift",,"Operational"
1944.00,"07","Surface report sequences (land)","307084","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA IV)",,"008002","Vertical significance (surface observations)","Vertical significance (= missing to cancel the previous value)",,"Operational"
1945.00,"07","Surface report sequences (land)","307084","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA IV)",,"302048","Direction and elevation of cloud","Direction and elevation of cloud",,"Operational"
1946.00,"07","Surface report sequences (land)","307084","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA IV)",,"302037","State of ground, snow depth, ground minimum temperature","State of ground, snow depth, ground minimum temperature",,"Operational"
1947.00,"07","Surface report sequences (land)","307084","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA IV)",,"020055","State of sky in the tropics","State of sky in tropics",,"Operational"
1948.00,"07","Surface report sequences (land)","307084","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA IV)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
1949.00,"07","Surface report sequences (land)","307084","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA IV)",,"031001","Delayed descriptor replication factor","Delayed descriptor replication factor",,"Operational"
1950.00,"07","Surface report sequences (land)","307084","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA IV)",,"205001","Signify character","Character field of 1 character",,"Operational"
1951.00,"07","Surface report sequences (land)","307084","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA IV)",,"302043","Basic synoptic ""period"" data","Basic synoptic ""period"" data",,"Operational"
1952.00,"07","Surface report sequences (land)","307084","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA IV)",,"302044","Evaporation data","Evaporation data",,"Operational"
1953.00,"07","Surface report sequences (land)","307084","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA IV)",,"101002","Replication descriptor","Replicate next descriptor 2 times",,"Operational"
1954.00,"07","Surface report sequences (land)","307084","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA IV)",,"302045","Radiation data (from 1 hour and 24 hour period)","Radiation data (from 1 hour and/or 24 hour period)",,"Operational"
1955.00,"07","Surface report sequences (land)","307084","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA IV)",,"302046","Temperature change","Temperature change",,"Operational"
1956.00,"07","Surface report sequences (land)","307086","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA VI)",,"301090","Surface station identification; time, horizontal and vertical co-ordinates","Fixed surface station identification, time, horizontal and vertical coordinates",,"Operational"
1957.00,"07","Surface report sequences (land)","307086","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA VI)",,"302031","Pressure information","Pressure data",,"Operational"
1958.00,"07","Surface report sequences (land)","307086","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA VI)",,"302035","Basic synoptic ""instantaneous"" data","Basic synoptic ""instantaneous"" data",,"Operational"
1959.00,"07","Surface report sequences (land)","307086","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA VI)",,"302036","Clouds with bases below station level","Clouds with bases below station level",,"Operational"
1960.00,"07","Surface report sequences (land)","307086","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA VI)",,"008002","Vertical significance (surface observations)","Vertical significance (= missing to cancel the previous value)",,"Operational"
1961.00,"07","Surface report sequences (land)","307086","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA VI)",,"302037","State of ground, snow depth, ground minimum temperature","State of ground, snow depth, ground minimum temperature",,"Operational"
1962.00,"07","Surface report sequences (land)","307086","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA VI)",,"302066","Dangerous weather phenomena","Dangerous weather phenomena",,"Operational"
1963.00,"07","Surface report sequences (land)","307086","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA VI)",,"302043","Basic synoptic ""period"" data","Basic synoptic ""period"" data",,"Operational"
1964.00,"07","Surface report sequences (land)","307086","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA VI)",,"302044","Evaporation data","Evaporation data",,"Operational"
1965.00,"07","Surface report sequences (land)","307086","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA VI)",,"101002","Replication descriptor","Replicate next descriptor 2 times",,"Operational"
1966.00,"07","Surface report sequences (land)","307086","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA VI)",,"302045","Radiation data (from 1 hour and 24 hour period)","Radiation data (from 1 hour and/or 24 hour period)",,"Operational"
1967.00,"07","Surface report sequences (land)","307090","(Sequence for representation of synoptic reports from a mobile land station suitable for SYNOP MOBIL data)",,"301092","Mobile surface station identification,date/time, horizontal and vertical coordinates","Mobile surface station identification, time, horizontal and vertical coordinates",,"Operational"
1968.00,"07","Surface report sequences (land)","307090","(Sequence for representation of synoptic reports from a mobile land station suitable for SYNOP MOBIL data)",,"302031","Pressure information","Pressure data",,"Operational"
1969.00,"07","Surface report sequences (land)","307090","(Sequence for representation of synoptic reports from a mobile land station suitable for SYNOP MOBIL data)",,"302035","Basic synoptic ""instantaneous"" data","Basic synoptic ""instantaneous"" data",,"Operational"
1970.00,"07","Surface report sequences (land)","307090","(Sequence for representation of synoptic reports from a mobile land station suitable for SYNOP MOBIL data)",,"302036","Clouds with bases below station level","Clouds with bases below station level",,"Operational"
1971.00,"07","Surface report sequences (land)","307090","(Sequence for representation of synoptic reports from a mobile land station suitable for SYNOP MOBIL data)",,"302047","Direction of cloud drift","Direction of cloud drift",,"Operational"
1972.00,"07","Surface report sequences (land)","307090","(Sequence for representation of synoptic reports from a mobile land station suitable for SYNOP MOBIL data)",,"008002","Vertical significance (surface observations)","Vertical significance",,"Operational"
1973.00,"07","Surface report sequences (land)","307090","(Sequence for representation of synoptic reports from a mobile land station suitable for SYNOP MOBIL data)",,"302048","Direction and elevation of cloud","Direction and elevation of cloud",,"Operational"
1974.00,"07","Surface report sequences (land)","307090","(Sequence for representation of synoptic reports from a mobile land station suitable for SYNOP MOBIL data)",,"302037","State of ground, snow depth, ground minimum temperature","State of ground, snow depth, ground minimum temperature",,"Operational"
1975.00,"07","Surface report sequences (land)","307090","(Sequence for representation of synoptic reports from a mobile land station suitable for SYNOP MOBIL data)",,"302043","Basic synoptic ""period"" data","Basic synoptic ""period"" data",,"Operational"
1976.00,"07","Surface report sequences (land)","307090","(Sequence for representation of synoptic reports from a mobile land station suitable for SYNOP MOBIL data)",,"302044","Evaporation data","Evaporation data",,"Operational"
1977.00,"07","Surface report sequences (land)","307090","(Sequence for representation of synoptic reports from a mobile land station suitable for SYNOP MOBIL data)",,"101002","Replication descriptor","Replicate next descriptor 2 times",,"Operational"
1978.00,"07","Surface report sequences (land)","307090","(Sequence for representation of synoptic reports from a mobile land station suitable for SYNOP MOBIL data)",,"302045","Radiation data (from 1 hour and 24 hour period)","Radiation data (from 1 hour and/or 24 hour period)",,"Operational"
1979.00,"07","Surface report sequences (land)","307090","(Sequence for representation of synoptic reports from a mobile land station suitable for SYNOP MOBIL data)",,"302046","Temperature change","Temperature change",,"Operational"
1980.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"301089","National station identification","National station identification",,"Operational"
1981.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"301090","Surface station identification; time, horizontal and vertical co-ordinates","Fixed surface station identification; time, horizontal and vertical coordinates",,"Operational"
1982.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"008010","Surface qualifier (temperature data)","Surface qualifier (for temperature data)",,"Operational"
1983.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"301091","Surface station instrumentation","Surface station instrumentation",,"Operational"
1984.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"302001",,"Pressure",,"Operational"
1985.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"007004","Pressure","Pressure (standard level)",,"Operational"
1986.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"010009","Geopotential height","Geopotential height of the standard level",,"Operational"
1987.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"302072","Temperature and humidity data","Temperature and humidity data",,"Operational"
1988.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"103000","Replication descriptor","Delayed replication of 3 descriptors",,"Operational"
1989.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"031000","Short delayed descriptor replication factor","Short delayed descriptor replication factor",,"Operational"
1990.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"101005","Replication descriptor","Replicate 1 descriptor five times",,"Operational"
1991.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"307063",,"Soil temperature",,"Operational"
1992.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"007061","Depth below land surface","Depth below land surface (set to missing to cancel the previous value)",,"Operational"
1993.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
1994.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"031000","Short delayed descriptor replication factor","Short delayed descriptor replication factor",,"Operational"
1995.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"302069","Visibility data","Visibility data",,"Operational"
1996.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above local ground (set to missing to cancel the previous value)",,"Operational"
1997.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"007033","Height of sensor above water surface","Height of sensor above water surface (set to missing to cancel the previous value)",,"Operational"
1998.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"105000","Replication descriptor","Delayed replication of 5 descriptors",,"Operational"
1999.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"031000","Short delayed descriptor replication factor","Short delayed descriptor replication factor",,"Operational"
2000.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"020031","Ice deposit (thickness)","Ice deposit (thickness)",,"Operational"
2001.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"020032","Rate of ice accretion","Rate of ice accretion",,"Operational"
2002.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"002038","Method of water temperature and/or salinity measurement","Method of sea surface temperature measurement",,"Operational"
2003.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"022043","Sea/water temperature","Sea/water temperature (scale 2)",,"Operational"
2004.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"302021",,"Wave data",,"Operational"
2005.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
2006.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"031000","Short delayed descriptor replication factor","Short delayed descriptor replication factor",,"Operational"
2007.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"302078","State of ground and snow depth measurement","State of ground and snow depth measurement",,"Operational"
2008.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
2009.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"031000","Short delayed descriptor replication factor","Short delayed descriptor replication factor",,"Operational"
2010.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"302073","Cloud data","Cloud data",,"Operational"
2011.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
2012.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"031000","Short delayed descriptor replication factor","Short delayed descriptor replication factor",,"Operational"
2013.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"302074","Present and past weather","Present and past weather",,"Operational"
2014.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
2015.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"031000","Short delayed descriptor replication factor","Short delayed descriptor replication factor",,"Operational"
2016.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"302175",,"Intensity of precipitation, size of precipitation element",,"Operational"
2017.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"102000","Replication descriptor","Delayed replication of 2 descriptors",,"Operational"
2018.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"031000","Short delayed descriptor replication factor","Short delayed descriptor replication factor",,"Operational"
2019.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"004025","Time period or displacement","Time period (= -10 minutes)",,"Operational"
2020.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"302076","Precipitation, obscuration and other phenomena","Precipitation, obscuration and other phenomena",,"Operational"
2021.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"302071","Wind data from one-hour period","Wind data from one-hour period",,"Operational"
2022.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"302077","Extreme temperature data","Extreme temperature data",,"Operational"
2023.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"007033","Height of sensor above water surface","Height of sensor above water surface (set to missing to cancel the previous value)",,"Operational"
2024.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
2025.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"031000","Short delayed descriptor replication factor","Short delayed descriptor replication factor",,"Operational"
2026.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"302079","Precipitation measurement","Precipitation measurement",,"Operational"
2027.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above local ground (set to missing to cancel the previous value)",,"Operational"
2028.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
2029.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"031000","Short delayed descriptor replication factor","Short delayed descriptor replication factor",,"Operational"
2030.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"302080","Evaporation measurement","Evaporation measurement",,"Operational"
2031.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
2032.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"031000","Short delayed descriptor replication factor","Short delayed descriptor replication factor",,"Operational"
2033.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"302081","Total sunshine data","Total sunshine data",,"Operational"
2034.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
2035.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"031000","Short delayed descriptor replication factor","Short delayed descriptor replication factor",,"Operational"
2036.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"302082","Radiation data","Radiation data",,"Operational"
2037.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"102000","Replication descriptor","Delayed replication of 2 descriptors",,"Operational"
2038.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"031000","Short delayed descriptor replication factor","Short delayed descriptor replication factor",,"Operational"
2039.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"004025","Time period or displacement","Time period (= -10 minutes)",,"Operational"
2040.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"013059","Number of flashes (thunderstorm)","Number of flashes",,"Operational"
2041.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
2042.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"031000","Short delayed descriptor replication factor","Short delayed descriptor replication factor",,"Operational"
2043.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"302083","First-order statistics of P, W, T, U data","First-order statistics of P, W, T, U data",,"Operational"
2044.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"033005","Quality information (AWS data)","Quality information (AWS data)",,"Operational"
2045.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"033006","Internal measurement status information (AWS)","Internal measurement status information (AWS)",,"Operational"
2134.00,"07","Surface report sequences (land)","307096","(Sequence for representation of SYNOP with supplementary information on one-hour observations)",,"301090","Surface station identification; time, horizontal and vertical co-ordinates","Fixed surface station identification, time, horizontal and vertical coordinates",,"Operational"
2135.00,"07","Surface report sequences (land)","307096","(Sequence for representation of SYNOP with supplementary information on one-hour observations)",,"301089","National station identification","National station identification",,"Operational"
2136.00,"07","Surface report sequences (land)","307096","(Sequence for representation of SYNOP with supplementary information on one-hour observations)",,"008010","Surface qualifier (temperature data)","Surface qualifier (for temperature data)",,"Operational"
2137.00,"07","Surface report sequences (land)","307096","(Sequence for representation of SYNOP with supplementary information on one-hour observations)",,"301091","Surface station instrumentation","Surface station instrumentation",,"Operational"
2138.00,"07","Surface report sequences (land)","307096","(Sequence for representation of SYNOP with supplementary information on one-hour observations)",,"302084","""Instantaneous"" data of sequence 3 07 096","""Instantaneous"" data of sequence 3 07 096",,"Operational"
2139.00,"07","Surface report sequences (land)","307096","(Sequence for representation of SYNOP with supplementary information on one-hour observations)",,"302085","""Period"" data of sequence 3 07 096","""Period"" data of sequence 3 07 096",,"Operational"
2140.00,"07","Surface report sequences (land)","307096","(Sequence for representation of SYNOP with supplementary information on one-hour observations)",,"033005","Quality information (AWS data)","Quality information (AWS data)",,"Operational"
2141.00,"07","Surface report sequences (land)","307096","(Sequence for representation of SYNOP with supplementary information on one-hour observations)",,"033006","Internal measurement status information (AWS)","Internal measurement status information (AWS)",,"Operational"
2142.00,"08","Surface report sequences (sea)","308001","(Buoy/platform - fixed)",,"301033","Buoy/platform - fixed","Identification, type, date/time, position (high accuracy)",,"Operational"
2143.00,"08","Surface report sequences (sea)","308001","(Buoy/platform - fixed)",,"302011","Low altitude station","Basic surface report",,"Operational"
2144.00,"08","Surface report sequences (sea)","308001","(Buoy/platform - fixed)",,"022042","Sea/water temperature","Sea-surface temperature",,"Operational"
2145.00,"08","Surface report sequences (sea)","308002","(Buoy/platform - fixed)",,"301034","Buoy/platform - fixed","Identification, type, date/time, position (coarse accuracy)",,"Operational"
2146.00,"08","Surface report sequences (sea)","308002","(Buoy/platform - fixed)",,"302011","Low altitude station","Basic surface report",,"Operational"
2147.00,"08","Surface report sequences (sea)","308002","(Buoy/platform - fixed)",,"022042","Sea/water temperature","Sea-surface temperature",,"Operational"
2148.00,"08","Surface report sequences (sea)","308003","(Buoy/platform - moving)",,"301035","Buoy/platform - moving","Identification, movement, type, date/time, position (coarse accuracy)","(see Note 4)","Operational"
2149.00,"08","Surface report sequences (sea)","308003","(Buoy/platform - moving)",,"302011","Low altitude station","Basic surface report",,"Operational"
2150.00,"08","Surface report sequences (sea)","308003","(Buoy/platform - moving)",,"022042","Sea/water temperature","Sea-surface temperature",,"Operational"
2151.00,"08","Surface report sequences (sea)","308004","(Ship)",,"301036","Ship","Identification, movement, type, date/time, position (coarse accuracy)",,"Operational"
2152.00,"08","Surface report sequences (sea)","308004","(Ship)",,"302011","Low altitude station","Basic surface report",,"Operational"
2153.00,"08","Surface report sequences (sea)","308004","(Ship)",,"022042","Sea/water temperature","Sea-surface temperature",,"Operational"
2154.00,"08","Surface report sequences (sea)","308005",,,"308004","Ship","Basic ship report",,"Operational"
2155.00,"08","Surface report sequences (sea)","308005",,,"302024",,"Wind waves and swell waves",,"Operational"
2156.00,"08","Surface report sequences (sea)","308006","(Buoy Section 1 optional parameters)",,"010004","Pressure","Pressure",,"Operational"
2157.00,"08","Surface report sequences (sea)","308006","(Buoy Section 1 optional parameters)",,"010061","3-hour pressure change","3-hour pressure change",,"Operational"
2158.00,"08","Surface report sequences (sea)","308006","(Buoy Section 1 optional parameters)",,"010063","Characteristic of pressure tendency","Characteristic of pressure tendency",,"Operational"
2159.00,"08","Surface report sequences (sea)","308006","(Buoy Section 1 optional parameters)",,"011001","Wind direction","Wind direction",,"Operational"
2160.00,"08","Surface report sequences (sea)","308006","(Buoy Section 1 optional parameters)",,"011002","Wind speed","Wind speed",,"Operational"
2161.00,"08","Surface report sequences (sea)","308006","(Buoy Section 1 optional parameters)",,"012004","Air temperature at 2 m","Air temperature at 2 m",,"Operational"
2162.00,"08","Surface report sequences (sea)","308006","(Buoy Section 1 optional parameters)",,"013003","Relative humidity","Relative humidity",,"Operational"
2163.00,"08","Surface report sequences (sea)","308006","(Buoy Section 1 optional parameters)",,"022042","Sea/water temperature","Sea temperature",,"Operational"
2164.00,"08","Surface report sequences (sea)","308007",,,"301055",,"Identification, movement type, date/time, position (high accuracy)",,"Operational"
2165.00,"08","Surface report sequences (sea)","308007",,,"302011","Low altitude station","Basic surface report",,"Operational"
2166.00,"08","Surface report sequences (sea)","308007",,,"007062","Depth below sea/water surface","Depth below sea/water surface",,"Operational"
2167.00,"08","Surface report sequences (sea)","308007",,,"022042","Sea/water temperature","Sea/water temperature",,"Operational"
2171.00,"08","Surface report sequences (sea)","308009","(Sequence for representation of synoptic reports from a sea station suitable for ship data)",,"301093","Ship identification, movement, date/time, horizontal and vertical coordinates","Ship identification, movement, date/time, horizontal and vertical coordinates",,"Operational"
2172.00,"08","Surface report sequences (sea)","308009","(Sequence for representation of synoptic reports from a sea station suitable for ship data)",,"302001",,"Pressure data",,"Operational"
2173.00,"08","Surface report sequences (sea)","308009","(Sequence for representation of synoptic reports from a sea station suitable for ship data)",,"302054","Ship ""instantaneous"" data","Ship ""instantaneous"" data",,"Operational"
2174.00,"08","Surface report sequences (sea)","308009","(Sequence for representation of synoptic reports from a sea station suitable for ship data)",,"008002","Vertical significance (surface observations)","Vertical significance",,"Operational"
2175.00,"08","Surface report sequences (sea)","308009","(Sequence for representation of synoptic reports from a sea station suitable for ship data)",,"302055","Icing and ice","Icing and ice",,"Operational"
2176.00,"08","Surface report sequences (sea)","308009","(Sequence for representation of synoptic reports from a sea station suitable for ship data)",,"302057","Ship marine data","Ship marine data",,"Operational"
2177.00,"08","Surface report sequences (sea)","308009","(Sequence for representation of synoptic reports from a sea station suitable for ship data)",,"302060","Ship ""period"" data","Ship ""period"" data",,"Operational"
2178.00,"08","Surface report sequences (sea)","308010","(TRACKOB Template)",,"001011","Ship or mobile land station identifier","Ship or mobile land station identifier",,"Operational"
2179.00,"08","Surface report sequences (sea)","308010","(TRACKOB Template)",,"113000","Replication descriptor","Delayed replication of 13 descriptors",,"Operational"
2180.00,"08","Surface report sequences (sea)","308010","(TRACKOB Template)",,"031001","Delayed descriptor replication factor","Delayed descriptor replication factor",,"Operational"
2181.00,"08","Surface report sequences (sea)","308010","(TRACKOB Template)",,"301011",,"Date",,"Operational"
2182.00,"08","Surface report sequences (sea)","308010","(TRACKOB Template)",,"301012",,"Time",,"Operational"
2183.00,"08","Surface report sequences (sea)","308010","(TRACKOB Template)",,"301021",,"Latitude/longitude (high accuracy)",,"Operational"
2184.00,"08","Surface report sequences (sea)","308010","(TRACKOB Template)",,"004080","Averaging period for following value","Averaging period for following value",,"Operational"
2185.00,"08","Surface report sequences (sea)","308010","(TRACKOB Template)",,"022049","Sea surface temperature","Sea surface temperature",,"Operational"
2186.00,"08","Surface report sequences (sea)","308010","(TRACKOB Template)",,"004080","Averaging period for following value","Averaging period for following value",,"Operational"
2187.00,"08","Surface report sequences (sea)","308010","(TRACKOB Template)",,"022059","Sea surface salinity","Sea surface salinity",,"Operational"
2188.00,"08","Surface report sequences (sea)","308010","(TRACKOB Template)",,"004080","Averaging period for following value","Averaging period for following value",,"Operational"
2189.00,"08","Surface report sequences (sea)","308010","(TRACKOB Template)",,"022005","Direction of sea surface current","Direction of sea surface current",,"Operational"
2190.00,"08","Surface report sequences (sea)","308010","(TRACKOB Template)",,"002042","Indicator for sea-surface current speed","Indicator for sea surface current speed",,"Operational"
2191.00,"08","Surface report sequences (sea)","308010","(TRACKOB Template)",,"022032","Speed of sea surface current","Speed of sea surface current",,"Operational"
2192.00,"08","Surface report sequences (sea)","308010","(TRACKOB Template)",,"002042","Indicator for sea-surface current speed","Indicator for sea surface current speed (cancel)",,"Operational"
2193.00,"08","Surface report sequences (sea)","308010","(TRACKOB Template)",,"004080","Averaging period for following value","Averaging period for following value (cancel)",,"Operational"
2194.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)",,"001011","Ship or mobile land station identifier","Ship's call sign",,"Operational"
2195.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)",,"002001","Type of station","Type of station",,"Operational"
2196.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)",,"301011",,"Date","(see Note 1)","Operational"
2197.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)",,"301012",,"Time","(see Note 1)","Operational"
2198.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)",,"301023",,"Latitude (coarse accuracy), longitude (coarse accuracy)",,"Operational"
2199.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)",,"007030","Height of station ground above mean sea level","Height of station platform above mean sea level","(see Note 3)","Operational"
2200.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)",,"007031","Height of barometer above mean sea level","Height of barometer above mean sea level","(see Note 3)","Operational"
2201.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)","Monthly mean values of pressure, temperature, vapour pressure and sea/water temperature:","004074","Short time period or displacement","Short time displacement (= UTC - LST)","(see Note 1)","Operational"
2202.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)","Monthly mean values of pressure, temperature, vapour pressure and sea/water temperature:","004023","Time period or displacement","Time period (= number of days in the month)",,"Operational"
2203.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)","Monthly mean values of pressure, temperature, vapour pressure and sea/water temperature:","008023","First-order statistics","First-order statistics (= 4; mean value)",,"Operational"
2204.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)","Monthly mean values of pressure, temperature, vapour pressure and sea/water temperature:","010051","Pressure reduced to mean sea level","Pressure reduced to mean sea level",,"Operational"
2205.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)","Monthly mean values of pressure, temperature, vapour pressure and sea/water temperature:","007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above marine deck platform (for temperature measurement)","(see Note 3)","Operational"
2206.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)","Monthly mean values of pressure, temperature, vapour pressure and sea/water temperature:","007033","Height of sensor above water surface","Height of sensor above water surface (for temperature measurement)","(see Note 3)","Operational"
2207.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)","Monthly mean values of pressure, temperature, vapour pressure and sea/water temperature:","012101","Temperature/air temperature","Temperature/air temperature",,"Operational"
2208.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)","Monthly mean values of pressure, temperature, vapour pressure and sea/water temperature:","013004","Vapour pressure","Vapour pressure",,"Operational"
2209.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)","Monthly mean values of pressure, temperature, vapour pressure and sea/water temperature:","007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above marine deck platform (set to missing to cancel the previous value)",,"Operational"
2210.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)","Monthly mean values of pressure, temperature, vapour pressure and sea/water temperature:","007033","Height of sensor above water surface","Height of sensor above water surface (set to missing to cancel the previous value)",,"Operational"
2211.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)","Monthly mean values of pressure, temperature, vapour pressure and sea/water temperature:","302056","Sea/water temperature","Sea surface temperature, method of measurement, and depth below sea surface",,"Operational"
2212.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)","Monthly mean values of pressure, temperature, vapour pressure and sea/water temperature:","008023","First-order statistics","First-order statistics (= 63; missing value)",,"Operational"
2213.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)","Precipitation","004003","Day","Day (= 1)","(see Note 2)","Operational"
2214.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)","Precipitation","004004","Hour","Hour (= 6)","(see Note 2)","Operational"
2215.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)","Precipitation","004023","Time period or displacement","Time period (= number of days in the month)","(see Note 2)","Operational"
2216.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)","Precipitation","007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above marine deck platform","(see Note 3)","Operational"
2217.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)","Precipitation","013060","Total accumulated precipitation","Total accumulated precipitation",,"Operational"
2218.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)","Precipitation","013051","Frequency group, precipitation","Frequency group; precipitation",,"Operational"
2219.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)","Precipitation","004053","Number of days with precipitation equal to or more than 1 mm","Number of days with precipitation equal to or more than 1 mm",,"Operational"
2220.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)","Precipitation","007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above marine deck platform (set to missing to cancel the previous value)",,"Operational"
2221.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)",,"004001","Year","Year (of beginning of the reference period)",,"Operational"
2222.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)",,"004001","Year","Year (of ending of the reference period)",,"Operational"
2223.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)",,"004002","Month","Month",,"Operational"
2224.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)",,"004003","Day","Day (= 1)","(see Note 1)","Operational"
2225.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)",,"004004","Hour","Hour (= 0)","(see Note 1)","Operational"
2226.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)",,"004074","Short time period or displacement","Short time displacement (= UTC - LST)","(see Note 1)","Operational"
2227.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)",,"004022","Time period or displacement","Time period (= 1)",,"Operational"
2228.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)","Normals of monthly mean pressure, temperature, vapour pressure and sea/water temperature:","008023","First-order statistics","First-order statistics (= 4; mean value)",,"Operational"
2229.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)","Normals of monthly mean pressure, temperature, vapour pressure and sea/water temperature:","010051","Pressure reduced to mean sea level","Pressure reduced to mean sea level",,"Operational"
2230.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)","Normals of monthly mean pressure, temperature, vapour pressure and sea/water temperature:","007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above marine deck platform (for temperature measurement)","(see Note 3)","Operational"
2231.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)","Normals of monthly mean pressure, temperature, vapour pressure and sea/water temperature:","007033","Height of sensor above water surface","Height of sensor above water surface (for temperature measurement)","(see Note 3)","Operational"
2232.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)","Normals of monthly mean pressure, temperature, vapour pressure and sea/water temperature:","012101","Temperature/air temperature","Temperature/air temperature",,"Operational"
2233.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)","Normals of monthly mean pressure, temperature, vapour pressure and sea/water temperature:","013004","Vapour pressure","Vapour pressure",,"Operational"
2234.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)","Normals of monthly mean pressure, temperature, vapour pressure and sea/water temperature:","007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above marine deck platform (set to missing to cancel the previous value)",,"Operational"
2235.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)","Normals of monthly mean pressure, temperature, vapour pressure and sea/water temperature:","007033","Height of sensor above water surface","Height of sensor above water surface (set to missing to cancel the previous value)",,"Operational"
2236.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)","Normals of monthly mean pressure, temperature, vapour pressure and sea/water temperature:","302056","Sea/water temperature","Sea surface temperature, method of measurement, and depth below sea surface",,"Operational"
2237.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)","Normals of monthly mean pressure, temperature, vapour pressure and sea/water temperature:","008023","First-order statistics","First-order statistics (= 63; missing value)",,"Operational"
2238.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)","Normals of monthly mean pressure, temperature, vapour pressure and sea/water temperature:","004001","Year","Year (of beginning of the reference period)",,"Operational"
2239.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)","Normals of monthly mean pressure, temperature, vapour pressure and sea/water temperature:","004001","Year","Year (of ending of the reference period)",,"Operational"
2240.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)","Normals of monthly mean pressure, temperature, vapour pressure and sea/water temperature:","004002","Month","Month",,"Operational"
2241.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)","Normals of monthly mean pressure, temperature, vapour pressure and sea/water temperature:","004003","Day","Day (= 1)","(see Note 2)","Operational"
2242.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)","Normals of monthly mean pressure, temperature, vapour pressure and sea/water temperature:","004004","Hour","Hour (= 6)","(see Note 2)","Operational"
2243.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)","Normals of monthly mean pressure, temperature, vapour pressure and sea/water temperature:","004022","Time period or displacement","Time period (= 1)",,"Operational"
2244.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)","Normals of precipitation:","007032","Height of sensor above local ground (or deck of marine platform)","Height of sensor above marine deck platform (for precipitation measurement)","(see Note 3)","Operational"
2245.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)","Normals of precipitation:","008023","First-order statistics","First-order statistics (= 4; mean value)",,"Operational"
2246.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)","Normals of precipitation:","013060","Total accumulated precipitation","Total accumulated precipitation",,"Operational"
2247.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)","Normals of precipitation:","004053","Number of days with precipitation equal to or more than 1 mm","Number of days with precipitation equal to or more than 1 mm",,"Operational"
2248.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)","Normals of precipitation:","008023","First-order statistics","First-order statistics (= 63; missing value)",,"Operational"
2249.00,"08","Surface report sequences (sea)","308013","(Representation of CLIMAT SHIP data of the actual month and for monthly normals)",,"308011","Monthly values from an ocean weather station - CLIMAT SHIP","Monthly values from an ocean weather station",,"Operational"
2250.00,"08","Surface report sequences (sea)","308013","(Representation of CLIMAT SHIP data of the actual month and for monthly normals)",,"308012","Monthly normals from an ocean weather station","Monthly normals from an ocean weather station",,"Operational"
2352.00,"09","Vertical sounding sequences (conventional data)","309001","(Vertical wind profile)",,"301037","Land station for vertical soundings","Identification, etc. (land station, high accuracy position)",,"Operational"
2353.00,"09","Vertical sounding sequences (conventional data)","309001","(Vertical wind profile)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
2354.00,"09","Vertical sounding sequences (conventional data)","309001","(Vertical wind profile)",,"031001","Delayed descriptor replication factor","Replication factor",,"Operational"
2355.00,"09","Vertical sounding sequences (conventional data)","309001","(Vertical wind profile)",,"303011",,"Winds at heights",,"Operational"
2356.00,"09","Vertical sounding sequences (conventional data)","309002","(Vertical wind profile)",,"301038","Land station for vertical soundings","Identification, etc. (land station, coarse accuracy position)",,"Operational"
2357.00,"09","Vertical sounding sequences (conventional data)","309002","(Vertical wind profile)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
2358.00,"09","Vertical sounding sequences (conventional data)","309002","(Vertical wind profile)",,"031001","Delayed descriptor replication factor","Replication factor",,"Operational"
2359.00,"09","Vertical sounding sequences (conventional data)","309002","(Vertical wind profile)",,"303011",,"Winds at heights",,"Operational"
2360.00,"09","Vertical sounding sequences (conventional data)","309003","(Vertical wind profile)",,"301037","Land station for vertical soundings","Identification, etc. (land station, high accuracy position)",,"Operational"
2361.00,"09","Vertical sounding sequences (conventional data)","309003","(Vertical wind profile)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
2362.00,"09","Vertical sounding sequences (conventional data)","309003","(Vertical wind profile)",,"031001","Delayed descriptor replication factor","Replication factor",,"Operational"
2363.00,"09","Vertical sounding sequences (conventional data)","309003","(Vertical wind profile)",,"303012",,"Winds at pressure levels",,"Operational"
2364.00,"09","Vertical sounding sequences (conventional data)","309004","(Vertical wind profile)",,"301038","Land station for vertical soundings","Identification, etc. (land station, coarse accuracy position)",,"Operational"
2365.00,"09","Vertical sounding sequences (conventional data)","309004","(Vertical wind profile)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
2366.00,"09","Vertical sounding sequences (conventional data)","309004","(Vertical wind profile)",,"031001","Delayed descriptor replication factor","Replication factor",,"Operational"
2367.00,"09","Vertical sounding sequences (conventional data)","309004","(Vertical wind profile)",,"303012",,"Winds at pressure levels",,"Operational"
2368.00,"09","Vertical sounding sequences (conventional data)","309005","(Vertical sounding with relative humidity)",,"301037","Land station for vertical soundings","Identification, etc. (land station, high accuracy position)",,"Operational"
2369.00,"09","Vertical sounding sequences (conventional data)","309005","(Vertical sounding with relative humidity)",,"302004","General cloud information","Significant cloud information",,"Operational"
2370.00,"09","Vertical sounding sequences (conventional data)","309005","(Vertical sounding with relative humidity)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
2371.00,"09","Vertical sounding sequences (conventional data)","309005","(Vertical sounding with relative humidity)",,"031001","Delayed descriptor replication factor","Replication factor",,"Operational"
2372.00,"09","Vertical sounding sequences (conventional data)","309005","(Vertical sounding with relative humidity)",,"303013",,"Pressure, geopotential, temperature and wind data",,"Operational"
2373.00,"09","Vertical sounding sequences (conventional data)","309006","(Vertical sounding with relative humidity)",,"301038","Land station for vertical soundings","Identification, etc. (land station, coarse accuracy position)",,"Operational"
2374.00,"09","Vertical sounding sequences (conventional data)","309006","(Vertical sounding with relative humidity)",,"302004","General cloud information","Significant cloud information",,"Operational"
2375.00,"09","Vertical sounding sequences (conventional data)","309006","(Vertical sounding with relative humidity)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
2376.00,"09","Vertical sounding sequences (conventional data)","309006","(Vertical sounding with relative humidity)",,"031001","Delayed descriptor replication factor","Replication factor",,"Operational"
2377.00,"09","Vertical sounding sequences (conventional data)","309006","(Vertical sounding with relative humidity)",,"303013",,"Pressure, geopotential, temperature and wind data",,"Operational"
2378.00,"09","Vertical sounding sequences (conventional data)","309007","(Vertical sounding with dew-point data)",,"301037","Land station for vertical soundings","Identification, etc. (land station, high accuracy position)",,"Operational"
2379.00,"09","Vertical sounding sequences (conventional data)","309007","(Vertical sounding with dew-point data)",,"302004","General cloud information","Significant cloud information",,"Operational"
2380.00,"09","Vertical sounding sequences (conventional data)","309007","(Vertical sounding with dew-point data)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
2381.00,"09","Vertical sounding sequences (conventional data)","309007","(Vertical sounding with dew-point data)",,"031001","Delayed descriptor replication factor","Replication factor",,"Operational"
2382.00,"09","Vertical sounding sequences (conventional data)","309007","(Vertical sounding with dew-point data)",,"303014",,"Pressure, geopotential, temperature and wind data",,"Operational"
2383.00,"09","Vertical sounding sequences (conventional data)","309008","(Vertical sounding with dew-point data)",,"301038","Land station for vertical soundings","Identification, etc. (land station, coarse accuracy position)",,"Operational"
2384.00,"09","Vertical sounding sequences (conventional data)","309008","(Vertical sounding with dew-point data)",,"302004","General cloud information","Significant cloud information",,"Operational"
2385.00,"09","Vertical sounding sequences (conventional data)","309008","(Vertical sounding with dew-point data)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
2386.00,"09","Vertical sounding sequences (conventional data)","309008","(Vertical sounding with dew-point data)",,"031001","Delayed descriptor replication factor","Replication factor",,"Operational"
2387.00,"09","Vertical sounding sequences (conventional data)","309008","(Vertical sounding with dew-point data)",,"303014",,"Pressure, geopotential, temperature and wind data",,"Operational"
2388.00,"09","Vertical sounding sequences (conventional data)","309011","(Vertical wind profile)",,"301039","Ship for vertical soundings","Ship's identification, etc.",,"Operational"
2389.00,"09","Vertical sounding sequences (conventional data)","309011","(Vertical wind profile)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
2390.00,"09","Vertical sounding sequences (conventional data)","309011","(Vertical wind profile)",,"031001","Delayed descriptor replication factor","Replication factor",,"Operational"
2391.00,"09","Vertical sounding sequences (conventional data)","309011","(Vertical wind profile)",,"303011",,"Winds at heights",,"Operational"
2392.00,"09","Vertical sounding sequences (conventional data)","309012","(Vertical wind profile)",,"301039","Ship for vertical soundings","Ship's identification, etc.",,"Operational"
2393.00,"09","Vertical sounding sequences (conventional data)","309012","(Vertical wind profile)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
2394.00,"09","Vertical sounding sequences (conventional data)","309012","(Vertical wind profile)",,"031001","Delayed descriptor replication factor","Replication factor",,"Operational"
2395.00,"09","Vertical sounding sequences (conventional data)","309012","(Vertical wind profile)",,"303012",,"Winds at pressure levels",,"Operational"
2396.00,"09","Vertical sounding sequences (conventional data)","309013","(Vertical sounding with relative humidity)",,"301039","Ship for vertical soundings","Ship's identification, etc.",,"Operational"
2397.00,"09","Vertical sounding sequences (conventional data)","309013","(Vertical sounding with relative humidity)",,"302004","General cloud information","Significant cloud information",,"Operational"
2398.00,"09","Vertical sounding sequences (conventional data)","309013","(Vertical sounding with relative humidity)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
2399.00,"09","Vertical sounding sequences (conventional data)","309013","(Vertical sounding with relative humidity)",,"031001","Delayed descriptor replication factor","Replication factor",,"Operational"
2400.00,"09","Vertical sounding sequences (conventional data)","309013","(Vertical sounding with relative humidity)",,"303013",,"Pressure, geopotential, temperature and wind data",,"Operational"
2401.00,"09","Vertical sounding sequences (conventional data)","309014","(Vertical sounding with dew-point data)",,"301039","Ship for vertical soundings","Ship's identification, etc.",,"Operational"
2402.00,"09","Vertical sounding sequences (conventional data)","309014","(Vertical sounding with dew-point data)",,"302004","General cloud information","Significant cloud information",,"Operational"
2403.00,"09","Vertical sounding sequences (conventional data)","309014","(Vertical sounding with dew-point data)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
2404.00,"09","Vertical sounding sequences (conventional data)","309014","(Vertical sounding with dew-point data)",,"031001","Delayed descriptor replication factor","Replication factor",,"Operational"
2405.00,"09","Vertical sounding sequences (conventional data)","309014","(Vertical sounding with dew-point data)",,"303014",,"Pressure, geopotential, temperature and wind data",,"Operational"
2406.00,"09","Vertical sounding sequences (conventional data)","309015","(Vertical wind profile)",,"301040",,"Ship's identification, etc.",,"Operational"
2407.00,"09","Vertical sounding sequences (conventional data)","309015","(Vertical wind profile)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
2408.00,"09","Vertical sounding sequences (conventional data)","309015","(Vertical wind profile)",,"031001","Delayed descriptor replication factor","Replication factor",,"Operational"
2409.00,"09","Vertical sounding sequences (conventional data)","309015","(Vertical wind profile)",,"303011",,"Winds at heights",,"Operational"
2410.00,"09","Vertical sounding sequences (conventional data)","309016","(Vertical wind profile)",,"301040",,"Ship's identification, etc.",,"Operational"
2411.00,"09","Vertical sounding sequences (conventional data)","309016","(Vertical wind profile)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
2412.00,"09","Vertical sounding sequences (conventional data)","309016","(Vertical wind profile)",,"031001","Delayed descriptor replication factor","Replication factor",,"Operational"
2413.00,"09","Vertical sounding sequences (conventional data)","309016","(Vertical wind profile)",,"303012",,"Winds at pressure levels",,"Operational"
2414.00,"09","Vertical sounding sequences (conventional data)","309017","(Vertical sounding with relative humidity)",,"301040",,"Ship's identification, etc.",,"Operational"
2415.00,"09","Vertical sounding sequences (conventional data)","309017","(Vertical sounding with relative humidity)",,"302004","General cloud information","Significant cloud information",,"Operational"
2416.00,"09","Vertical sounding sequences (conventional data)","309017","(Vertical sounding with relative humidity)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
2417.00,"09","Vertical sounding sequences (conventional data)","309017","(Vertical sounding with relative humidity)",,"031001","Delayed descriptor replication factor","Replication factor",,"Operational"
2418.00,"09","Vertical sounding sequences (conventional data)","309017","(Vertical sounding with relative humidity)",,"303013",,"Pressure, geopotential, temperature and wind data",,"Operational"
2419.00,"09","Vertical sounding sequences (conventional data)","309018","(Vertical sounding with dew-point data)",,"301040",,"Ship's identification, etc.",,"Operational"
2420.00,"09","Vertical sounding sequences (conventional data)","309018","(Vertical sounding with dew-point data)",,"302004","General cloud information","Significant cloud information",,"Operational"
2421.00,"09","Vertical sounding sequences (conventional data)","309018","(Vertical sounding with dew-point data)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
2422.00,"09","Vertical sounding sequences (conventional data)","309018","(Vertical sounding with dew-point data)",,"031001","Delayed descriptor replication factor","Replication factor",,"Operational"
2423.00,"09","Vertical sounding sequences (conventional data)","309018","(Vertical sounding with dew-point data)",,"303014",,"Pressure, geopotential, temperature and wind data",,"Operational"
2424.00,"09","Vertical sounding sequences (conventional data)","309019","(Wind profiler - wind data sounding)",,"301031",,"Identification, etc.",,"Operational"
2425.00,"09","Vertical sounding sequences (conventional data)","309019","(Wind profiler - wind data sounding)",,"002003","Type of measuring equipment used","Type of measuring equipment used",,"Operational"
2426.00,"09","Vertical sounding sequences (conventional data)","309019","(Wind profiler - wind data sounding)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
2427.00,"09","Vertical sounding sequences (conventional data)","309019","(Wind profiler - wind data sounding)",,"031001","Delayed descriptor replication factor","Replication factor",,"Operational"
2428.00,"09","Vertical sounding sequences (conventional data)","309019","(Wind profiler - wind data sounding)",,"303011",,"Winds at heights",,"Operational"
2429.00,"09","Vertical sounding sequences (conventional data)","309020","(Wind profiler - Cartesian coordinates)",,"301031",,"Identification, etc.",,"Operational"
2430.00,"09","Vertical sounding sequences (conventional data)","309020","(Wind profiler - Cartesian coordinates)",,"002003","Type of measuring equipment used","Type of measuring equipment used",,"Operational"
2431.00,"09","Vertical sounding sequences (conventional data)","309020","(Wind profiler - Cartesian coordinates)",,"104000","Replication descriptor","Delayed replication of 4 descriptors",,"Operational"
2432.00,"09","Vertical sounding sequences (conventional data)","309020","(Wind profiler - Cartesian coordinates)",,"031001","Delayed descriptor replication factor","Replication factor",,"Operational"
2433.00,"09","Vertical sounding sequences (conventional data)","309020","(Wind profiler - Cartesian coordinates)",,"007003","Geopotential","Geopotential",,"Operational"
2434.00,"09","Vertical sounding sequences (conventional data)","309020","(Wind profiler - Cartesian coordinates)",,"011003","u-component","u-component",,"Operational"
2435.00,"09","Vertical sounding sequences (conventional data)","309020","(Wind profiler - Cartesian coordinates)",,"011004","v-component","v-component",,"Operational"
2436.00,"09","Vertical sounding sequences (conventional data)","309020","(Wind profiler - Cartesian coordinates)",,"011005","w-component","w-component",,"Operational"
2437.00,"09","Vertical sounding sequences (conventional data)","309030","(Ozone sonde flight data)",,"015004","Ozone sounding correction factor (CF)","Ozone sounding correction factor",,"Operational"
2438.00,"09","Vertical sounding sequences (conventional data)","309030","(Ozone sonde flight data)",,"015005","Ozone p","Ozone p",,"Operational"
2439.00,"09","Vertical sounding sequences (conventional data)","309030","(Ozone sonde flight data)",,"104000","Replication descriptor","Delayed replication of 4 descriptors",,"Operational"
2440.00,"09","Vertical sounding sequences (conventional data)","309030","(Ozone sonde flight data)",,"031001","Delayed descriptor replication factor","Replication factor",,"Operational"
2441.00,"09","Vertical sounding sequences (conventional data)","309030","(Ozone sonde flight data)",,"004015","Time increment","Time increment since launch time, if needed, in minutes",,"Operational"
2442.00,"09","Vertical sounding sequences (conventional data)","309030","(Ozone sonde flight data)",,"008006","Ozone vertical sounding significance","Ozone vertical sounding significance",,"Operational"
2443.00,"09","Vertical sounding sequences (conventional data)","309030","(Ozone sonde flight data)",,"007004","Pressure","Pressure",,"Operational"
2444.00,"09","Vertical sounding sequences (conventional data)","309030","(Ozone sonde flight data)",,"015003","Measured ozone partial pressure (sounding)","Measured ozone partial pressure",,"Operational"
2445.00,"09","Vertical sounding sequences (conventional data)","309031","(Ozone sonde flight data)",,"015004","Ozone sounding correction factor (CF)","Ozone sounding correction factor",,"Operational"
2446.00,"09","Vertical sounding sequences (conventional data)","309031","(Ozone sonde flight data)",,"015005","Ozone p","Ozone p",,"Operational"
2447.00,"09","Vertical sounding sequences (conventional data)","309031","(Ozone sonde flight data)",,"104000","Replication descriptor","Delayed replication of 4 descriptors",,"Operational"
2448.00,"09","Vertical sounding sequences (conventional data)","309031","(Ozone sonde flight data)",,"031001","Delayed descriptor replication factor","Replication factor",,"Operational"
2449.00,"09","Vertical sounding sequences (conventional data)","309031","(Ozone sonde flight data)",,"004025","Time period or displacement","Time displacement (since launch time) in minutes",,"Operational"
2450.00,"09","Vertical sounding sequences (conventional data)","309031","(Ozone sonde flight data)",,"008006","Ozone vertical sounding significance","Ozone vertical sounding significance",,"Operational"
2451.00,"09","Vertical sounding sequences (conventional data)","309031","(Ozone sonde flight data)",,"007004","Pressure","Pressure",,"Operational"
2452.00,"09","Vertical sounding sequences (conventional data)","309031","(Ozone sonde flight data)",,"015003","Measured ozone partial pressure (sounding)","Measured ozone partial pressure",,"Operational"
2453.00,"09","Vertical sounding sequences (conventional data)","309050","(Sequence for representation of PILOT, PILOT SHIP and PILOT MOBIL observation type data with pressure as the vertical coordinate)",,"301110","Identification of launch site and instrumentation for wind measurements","Identification of launch site and instrumentation for wind measurements",,"Operational"
2454.00,"09","Vertical sounding sequences (conventional data)","309050","(Sequence for representation of PILOT, PILOT SHIP and PILOT MOBIL observation type data with pressure as the vertical coordinate)",,"301113","Date/time of launch (see Note 3)","Date/time of launch",,"Operational"
2455.00,"09","Vertical sounding sequences (conventional data)","309050","(Sequence for representation of PILOT, PILOT SHIP and PILOT MOBIL observation type data with pressure as the vertical coordinate)",,"301114","Horizontal and vertical coordinates of launch site","Horizontal and vertical coordinates of launch site",,"Operational"
2456.00,"09","Vertical sounding sequences (conventional data)","309050","(Sequence for representation of PILOT, PILOT SHIP and PILOT MOBIL observation type data with pressure as the vertical coordinate)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
2457.00,"09","Vertical sounding sequences (conventional data)","309050","(Sequence for representation of PILOT, PILOT SHIP and PILOT MOBIL observation type data with pressure as the vertical coordinate)",,"031002","Extended delayed descriptor replication factor","Extended delayed descriptor replication factor",,"Operational"
2458.00,"09","Vertical sounding sequences (conventional data)","309050","(Sequence for representation of PILOT, PILOT SHIP and PILOT MOBIL observation type data with pressure as the vertical coordinate)",,"303050","Wind data at a pressure level with radiosonde position","Wind data at a pressure level",,"Operational"
2459.00,"09","Vertical sounding sequences (conventional data)","309050","(Sequence for representation of PILOT, PILOT SHIP and PILOT MOBIL observation type data with pressure as the vertical coordinate)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
2460.00,"09","Vertical sounding sequences (conventional data)","309050","(Sequence for representation of PILOT, PILOT SHIP and PILOT MOBIL observation type data with pressure as the vertical coordinate)",,"031001","Delayed descriptor replication factor","Delayed descriptor replication factor",,"Operational"
2461.00,"09","Vertical sounding sequences (conventional data)","309050","(Sequence for representation of PILOT, PILOT SHIP and PILOT MOBIL observation type data with pressure as the vertical coordinate)",,"303051","Wind shear data at a pressure level with radiosonde position","Wind shear data at a pressure level",,"Operational"
2462.00,"09","Vertical sounding sequences (conventional data)","309051","(Sequence for representation of PILOT, PILOT SHIP and PILOT MOBIL observation type data with height as the vertical coordinate)",,"301110","Identification of launch site and instrumentation for wind measurements","Identification of launch site and instrumentation for wind measurements",,"Operational"
2463.00,"09","Vertical sounding sequences (conventional data)","309051","(Sequence for representation of PILOT, PILOT SHIP and PILOT MOBIL observation type data with height as the vertical coordinate)",,"301113","Date/time of launch (see Note 3)","Date/time of launch",,"Operational"
2464.00,"09","Vertical sounding sequences (conventional data)","309051","(Sequence for representation of PILOT, PILOT SHIP and PILOT MOBIL observation type data with height as the vertical coordinate)",,"301114","Horizontal and vertical coordinates of launch site","Horizontal and vertical coordinates of launch site",,"Operational"
2465.00,"09","Vertical sounding sequences (conventional data)","309051","(Sequence for representation of PILOT, PILOT SHIP and PILOT MOBIL observation type data with height as the vertical coordinate)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
2466.00,"09","Vertical sounding sequences (conventional data)","309051","(Sequence for representation of PILOT, PILOT SHIP and PILOT MOBIL observation type data with height as the vertical coordinate)",,"031002","Extended delayed descriptor replication factor","Extended delayed descriptor replication factor",,"Operational"
2467.00,"09","Vertical sounding sequences (conventional data)","309051","(Sequence for representation of PILOT, PILOT SHIP and PILOT MOBIL observation type data with height as the vertical coordinate)",,"303052","Wind data at a height level with radiosonde position","Wind data at a height level",,"Operational"
2468.00,"09","Vertical sounding sequences (conventional data)","309051","(Sequence for representation of PILOT, PILOT SHIP and PILOT MOBIL observation type data with height as the vertical coordinate)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
2469.00,"09","Vertical sounding sequences (conventional data)","309051","(Sequence for representation of PILOT, PILOT SHIP and PILOT MOBIL observation type data with height as the vertical coordinate)",,"031001","Delayed descriptor replication factor","Delayed descriptor replication factor",,"Operational"
2470.00,"09","Vertical sounding sequences (conventional data)","309051","(Sequence for representation of PILOT, PILOT SHIP and PILOT MOBIL observation type data with height as the vertical coordinate)",,"303053","Wind shear data at a height level with radiosonde position","Wind shear data at a height level",,"Operational"
2471.00,"09","Vertical sounding sequences (conventional data)","309052","(Sequence for representation of TEMP, TEMP SHIP and TEMP MOBIL observation type data)",,"301111","Identification of launch site and instrumentation for P, T, U and wind measurements","Identification of launch site and instrumentation for P, T, U and wind measurements",,"Operational"
2472.00,"09","Vertical sounding sequences (conventional data)","309052","(Sequence for representation of TEMP, TEMP SHIP and TEMP MOBIL observation type data)",,"301113","Date/time of launch (see Note 3)","Date/time of launch",,"Operational"
2473.00,"09","Vertical sounding sequences (conventional data)","309052","(Sequence for representation of TEMP, TEMP SHIP and TEMP MOBIL observation type data)",,"301114","Horizontal and vertical coordinates of launch site","Horizontal and vertical coordinates of launch site",,"Operational"
2474.00,"09","Vertical sounding sequences (conventional data)","309052","(Sequence for representation of TEMP, TEMP SHIP and TEMP MOBIL observation type data)",,"302049","Cloud information reported with vertical soundings","Cloud information reported with vertical soundings",,"Operational"
2475.00,"09","Vertical sounding sequences (conventional data)","309052","(Sequence for representation of TEMP, TEMP SHIP and TEMP MOBIL observation type data)",,"022043","Sea/water temperature","Sea water temperature",,"Operational"
2476.00,"09","Vertical sounding sequences (conventional data)","309052","(Sequence for representation of TEMP, TEMP SHIP and TEMP MOBIL observation type data)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
2477.00,"09","Vertical sounding sequences (conventional data)","309052","(Sequence for representation of TEMP, TEMP SHIP and TEMP MOBIL observation type data)",,"031002","Extended delayed descriptor replication factor","Extended delayed descriptor replication factor",,"Operational"
2478.00,"09","Vertical sounding sequences (conventional data)","309052","(Sequence for representation of TEMP, TEMP SHIP and TEMP MOBIL observation type data)",,"303054","Temperature, dew-point and wind data at a pressure level with radiosonde position","Temperature, dew-point and wind data at a pressure level",,"Operational"
2479.00,"09","Vertical sounding sequences (conventional data)","309052","(Sequence for representation of TEMP, TEMP SHIP and TEMP MOBIL observation type data)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
2480.00,"09","Vertical sounding sequences (conventional data)","309052","(Sequence for representation of TEMP, TEMP SHIP and TEMP MOBIL observation type data)",,"031001","Delayed descriptor replication factor","Delayed descriptor replication factor",,"Operational"
2481.00,"09","Vertical sounding sequences (conventional data)","309052","(Sequence for representation of TEMP, TEMP SHIP and TEMP MOBIL observation type data)",,"303051","Wind shear data at a pressure level with radiosonde position","Wind shear data at a pressure level",,"Operational"
2482.00,"09","Vertical sounding sequences (conventional data)","309053","(Sequence for representation of TEMP DROP observation type data)",,"301112","Identification of launch point and instrumentation of dropsonde","Identification of launch point and instrumentation of dropsonde",,"Operational"
2483.00,"09","Vertical sounding sequences (conventional data)","309053","(Sequence for representation of TEMP DROP observation type data)",,"301113","Date/time of launch (see Note 3)","Date/time of launch",,"Operational"
2484.00,"09","Vertical sounding sequences (conventional data)","309053","(Sequence for representation of TEMP DROP observation type data)",,"301114","Horizontal and vertical coordinates of launch site","Horizontal and vertical coordinates of launch site",,"Operational"
2485.00,"09","Vertical sounding sequences (conventional data)","309053","(Sequence for representation of TEMP DROP observation type data)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
2486.00,"09","Vertical sounding sequences (conventional data)","309053","(Sequence for representation of TEMP DROP observation type data)",,"031002","Extended delayed descriptor replication factor","Extended delayed descriptor replication factor",,"Operational"
2487.00,"09","Vertical sounding sequences (conventional data)","309053","(Sequence for representation of TEMP DROP observation type data)",,"303054","Temperature, dew-point and wind data at a pressure level with radiosonde position","Temperature, dew-point and wind data at a pressure level",,"Operational"
2488.00,"09","Vertical sounding sequences (conventional data)","309053","(Sequence for representation of TEMP DROP observation type data)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
2489.00,"09","Vertical sounding sequences (conventional data)","309053","(Sequence for representation of TEMP DROP observation type data)",,"031001","Delayed descriptor replication factor","Delayed descriptor replication factor",,"Operational"
2490.00,"09","Vertical sounding sequences (conventional data)","309053","(Sequence for representation of TEMP DROP observation type data)",,"303051","Wind shear data at a pressure level with radiosonde position","Wind shear data at a pressure level",,"Operational"
2491.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)",,"301001",,"Identification of launch site",,"Operational"
2492.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)",,"001011","Ship or mobile land station identifier","Ship's call sign",,"Operational"
2493.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)",,"301011",,"Date",,"Operational"
2494.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)",,"301012",,"Time",,"Operational"
2495.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)",,"301021",,"Horizontal and vertical coordinates",,"Operational"
2496.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)",,"007030","Height of station ground above mean sea level","Height of station ground above mean sea level",,"Operational"
2497.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)",,"007031","Height of barometer above mean sea level","Height of barometer above mean sea level",,"Operational"
2498.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)",,"007007","Height","Height release of sonde above mean sea level",,"Operational"
2499.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)","Monthly mean data:","004023","Time period or displacement","Time period (= number of days in the month)",,"Operational"
2500.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)","Monthly mean data:","004059","Times of observation used to compute the reported mean values","Times of observations used to compute the reported mean values",,"Operational"
2501.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)","Monthly mean data:","115000","Replication descriptor","Delayed replication of 15 descriptors",,"Operational"
2502.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)","Monthly mean data:","031001","Delayed descriptor replication factor","Delayed descriptor replication factor",,"Operational"
2503.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)","Monthly mean data:","008001","Vertical sounding significance","Vertical sounding significance",,"Operational"
2504.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)","Monthly mean data:","008023","First-order statistics","First-order statistics (= 4; mean value)",,"Operational"
2505.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)","Monthly mean data:","007004","Pressure","Pressure",,"Operational"
2506.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)","Monthly mean data:","010009","Geopotential height","Geopotential height",,"Operational"
2507.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)","Monthly mean data:","012101","Temperature/air temperature","Temperature/air temperature",,"Operational"
2508.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)","Monthly mean data:","012103","Dew-point temperature","Dew-point temperature",,"Operational"
2509.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)","Monthly mean data:","008023","First-order statistics","First-order statistics (= 32; vector mean)",,"Operational"
2510.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)","Monthly mean data:","011001","Wind direction","Wind direction",,"Operational"
2511.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)","Monthly mean data:","011002","Wind speed","Wind speed",,"Operational"
2512.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)","Monthly mean data:","008023","First-order statistics","First-order statistics (= 63; missing value)",,"Operational"
2513.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)","Monthly mean data:","011019","Steadiness of wind","Steadiness of wind",,"Operational"
2514.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)","Monthly mean data:","008050","Qualifier for number of missing values in calculation of statistic","Qualifier for number of missing values in calculation of statistic (= 2; temperature)",,"Operational"
2515.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)","Monthly mean data:","008020","Total number of missing entities (with respect to accumulation or average)","Total number of missing entities (days)",,"Operational"
2516.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)","Monthly mean data:","008050","Qualifier for number of missing values in calculation of statistic","Qualifier for number of missing values in calculation of statistic (= 9; wind)",,"Operational"
2517.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)","Monthly mean data:","008020","Total number of missing entities (with respect to accumulation or average)","Total number of missing entities (days)",,"Operational"
2518.00,"09","Vertical sounding sequences (conventional data)","309060","(Radiosonde complete registration and surface observation)",,"301123","Radiosonde full header information","Radiosonde full header information",,"Operational"
2519.00,"09","Vertical sounding sequences (conventional data)","309060","(Radiosonde complete registration and surface observation)",,"301121","Radiosonde launch point location","Radiosonde launch point location",,"Operational"
2520.00,"09","Vertical sounding sequences (conventional data)","309060","(Radiosonde complete registration and surface observation)",,"302050","Radiosonde surface observation","Radiosonde surface observation",,"Operational"
2521.00,"09","Vertical sounding sequences (conventional data)","309060","(Radiosonde complete registration and surface observation)",,"303040","Radiosonde duration of flight and termination information","Radiosonde duration of flight and termination information",,"Operational"
2522.00,"09","Vertical sounding sequences (conventional data)","309061","(Raw PTU)",,"301120","Radiosonde abbreviated header and launch information","Radiosonde abbreviated header and launch information",,"Operational"
2523.00,"09","Vertical sounding sequences (conventional data)","309061","(Raw PTU)",,"008041","Data significance","Data significance (6 = flight level observation)",,"Operational"
2524.00,"09","Vertical sounding sequences (conventional data)","309061","(Raw PTU)",,"301122","Date/time (to hundredths of second) (see Note 3)","Date/time (to hundredths of second)",,"Operational"
2525.00,"09","Vertical sounding sequences (conventional data)","309061","(Raw PTU)",,"201131","Change data width","Change data width",,"Operational"
2526.00,"09","Vertical sounding sequences (conventional data)","309061","(Raw PTU)",,"202129","Change scale","Change scale",,"Operational"
2527.00,"09","Vertical sounding sequences (conventional data)","309061","(Raw PTU)",,"025069","Flight level pressure corrections","Flight level pressure correction",,"Operational"
2528.00,"09","Vertical sounding sequences (conventional data)","309061","(Raw PTU)",,"007004","Pressure","Pressure",,"Operational"
2529.00,"09","Vertical sounding sequences (conventional data)","309061","(Raw PTU)",,"202000","Change scale","Cancel change scale",,"Operational"
2530.00,"09","Vertical sounding sequences (conventional data)","309061","(Raw PTU)",,"201000","Change data width","Cancel change data width",,"Operational"
2531.00,"09","Vertical sounding sequences (conventional data)","309061","(Raw PTU)",,"033007","Per cent confidence","Per cent confidence (for pressure)",,"Operational"
2532.00,"09","Vertical sounding sequences (conventional data)","309061","(Raw PTU)",,"033035","Manual/automatic quality control","Manual/automatic quality control (for pressure)",,"Operational"
2533.00,"09","Vertical sounding sequences (conventional data)","309061","(Raw PTU)",,"033015","Data quality check indicator","Data quality-check indicator (for pressure)",,"Operational"
2534.00,"09","Vertical sounding sequences (conventional data)","309061","(Raw PTU)",,"013009","Relative humidity","Relative humidity",,"Operational"
2535.00,"09","Vertical sounding sequences (conventional data)","309061","(Raw PTU)",,"033007","Per cent confidence","Per cent confidence (for relative humidity)",,"Operational"
2536.00,"09","Vertical sounding sequences (conventional data)","309061","(Raw PTU)",,"033035","Manual/automatic quality control","Manual/automatic quality control (for relative humidity)",,"Operational"
2537.00,"09","Vertical sounding sequences (conventional data)","309061","(Raw PTU)",,"033015","Data quality check indicator","Data quality-check indicator (for relative humidity)",,"Operational"
2538.00,"09","Vertical sounding sequences (conventional data)","309061","(Raw PTU)",,"002013","Solar and infrared radiation correction","Solar and infrared radiation correction",,"Operational"
2539.00,"09","Vertical sounding sequences (conventional data)","309061","(Raw PTU)",,"012101","Temperature/air temperature","Temperature/air temperature",,"Operational"
2540.00,"09","Vertical sounding sequences (conventional data)","309061","(Raw PTU)",,"033007","Per cent confidence","Per cent confidence (for temperature)",,"Operational"
2541.00,"09","Vertical sounding sequences (conventional data)","309061","(Raw PTU)",,"033035","Manual/automatic quality control","Manual/automatic quality control (for temperature)",,"Operational"
2542.00,"09","Vertical sounding sequences (conventional data)","309061","(Raw PTU)",,"033015","Data quality check indicator","Data quality-check indicator (for temperature)",,"Operational"
2543.00,"09","Vertical sounding sequences (conventional data)","309062","(Raw GPS unsmoothed wind)",,"301120","Radiosonde abbreviated header and launch information","Radiosonde abbreviated header and launch information",,"Operational"
2544.00,"09","Vertical sounding sequences (conventional data)","309062","(Raw GPS unsmoothed wind)",,"008041","Data significance","Data significance (6 = flight level observation)",,"Operational"
2545.00,"09","Vertical sounding sequences (conventional data)","309062","(Raw GPS unsmoothed wind)",,"301122","Date/time (to hundredths of second) (see Note 3)","Date/time (to hundredths of second)",,"Operational"
2546.00,"09","Vertical sounding sequences (conventional data)","309062","(Raw GPS unsmoothed wind)",,"005001","Latitude (high accuracy)","Latitude (high accuracy)",,"Operational"
2547.00,"09","Vertical sounding sequences (conventional data)","309062","(Raw GPS unsmoothed wind)",,"033035","Manual/automatic quality control","Manual/automatic quality control (for latitude)",,"Operational"
2548.00,"09","Vertical sounding sequences (conventional data)","309062","(Raw GPS unsmoothed wind)",,"033015","Data quality check indicator","Data quality-check indicator (for latitude)",,"Operational"
2549.00,"09","Vertical sounding sequences (conventional data)","309062","(Raw GPS unsmoothed wind)",,"006001","Longitude (high accuracy)","Longitude (high accuracy)",,"Operational"
2550.00,"09","Vertical sounding sequences (conventional data)","309062","(Raw GPS unsmoothed wind)",,"033035","Manual/automatic quality control","Manual/automatic quality control (for longitude)",,"Operational"
2551.00,"09","Vertical sounding sequences (conventional data)","309062","(Raw GPS unsmoothed wind)",,"033015","Data quality check indicator","Data quality-check indicator (for longitude)",,"Operational"
2552.00,"09","Vertical sounding sequences (conventional data)","309062","(Raw GPS unsmoothed wind)",,"007007","Height","Height",,"Operational"
2553.00,"09","Vertical sounding sequences (conventional data)","309062","(Raw GPS unsmoothed wind)",,"033035","Manual/automatic quality control","Manual/automatic quality control (for height)",,"Operational"
2554.00,"09","Vertical sounding sequences (conventional data)","309062","(Raw GPS unsmoothed wind)",,"033015","Data quality check indicator","Data quality-check indicator (for height)",,"Operational"
2555.00,"09","Vertical sounding sequences (conventional data)","309062","(Raw GPS unsmoothed wind)",,"011003","u-component","u-component",,"Operational"
2556.00,"09","Vertical sounding sequences (conventional data)","309062","(Raw GPS unsmoothed wind)",,"033035","Manual/automatic quality control","Manual/automatic quality control (for u-component)",,"Operational"
2557.00,"09","Vertical sounding sequences (conventional data)","309062","(Raw GPS unsmoothed wind)",,"033015","Data quality check indicator","Data quality-check indicator (for u-component)",,"Operational"
2558.00,"09","Vertical sounding sequences (conventional data)","309062","(Raw GPS unsmoothed wind)",,"011004","v-component","v-component",,"Operational"
2559.00,"09","Vertical sounding sequences (conventional data)","309062","(Raw GPS unsmoothed wind)",,"033035","Manual/automatic quality control","Manual/automatic quality control (for v-component)",,"Operational"
2560.00,"09","Vertical sounding sequences (conventional data)","309062","(Raw GPS unsmoothed wind)",,"033015","Data quality check indicator","Data quality-check indicator (for v-component)",,"Operational"
2561.00,"09","Vertical sounding sequences (conventional data)","309062","(Raw GPS unsmoothed wind)",,"033007","Per cent confidence","Per cent confidence (for raw GPS unsmoothed wind)",,"Operational"
2562.00,"09","Vertical sounding sequences (conventional data)","309063","(Raw GPS smoothed wind)",,"301120","Radiosonde abbreviated header and launch information","Radiosonde abbreviated header and launch information",,"Operational"
2563.00,"09","Vertical sounding sequences (conventional data)","309063","(Raw GPS smoothed wind)",,"008041","Data significance","Data significance (6 = flight level observation)",,"Operational"
2564.00,"09","Vertical sounding sequences (conventional data)","309063","(Raw GPS smoothed wind)",,"301122","Date/time (to hundredths of second) (see Note 3)","Date/time (to hundredths of second) sequence",,"Operational"
2565.00,"09","Vertical sounding sequences (conventional data)","309063","(Raw GPS smoothed wind)",,"005001","Latitude (high accuracy)","Latitude (high accuracy)",,"Operational"
2566.00,"09","Vertical sounding sequences (conventional data)","309063","(Raw GPS smoothed wind)",,"033035","Manual/automatic quality control","Manual/automatic quality control (for latitude)",,"Operational"
2567.00,"09","Vertical sounding sequences (conventional data)","309063","(Raw GPS smoothed wind)",,"033015","Data quality check indicator","Data quality-check indicator (for latitude)",,"Operational"
2568.00,"09","Vertical sounding sequences (conventional data)","309063","(Raw GPS smoothed wind)",,"006001","Longitude (high accuracy)","Longitude (high accuracy)",,"Operational"
2569.00,"09","Vertical sounding sequences (conventional data)","309063","(Raw GPS smoothed wind)",,"033035","Manual/automatic quality control","Manual/automatic quality control (for longitude)",,"Operational"
2570.00,"09","Vertical sounding sequences (conventional data)","309063","(Raw GPS smoothed wind)",,"033015","Data quality check indicator","Data quality-check indicator (for longitude)",,"Operational"
2571.00,"09","Vertical sounding sequences (conventional data)","309063","(Raw GPS smoothed wind)",,"007007","Height","Height",,"Operational"
2572.00,"09","Vertical sounding sequences (conventional data)","309063","(Raw GPS smoothed wind)",,"033035","Manual/automatic quality control","Manual/automatic quality control (for height)",,"Operational"
2573.00,"09","Vertical sounding sequences (conventional data)","309063","(Raw GPS smoothed wind)",,"033015","Data quality check indicator","Data quality-check indicator (for height)",,"Operational"
2574.00,"09","Vertical sounding sequences (conventional data)","309063","(Raw GPS smoothed wind)",,"011003","u-component","u-component",,"Operational"
2575.00,"09","Vertical sounding sequences (conventional data)","309063","(Raw GPS smoothed wind)",,"033035","Manual/automatic quality control","Manual/automatic quality control (for u-component)",,"Operational"
2576.00,"09","Vertical sounding sequences (conventional data)","309063","(Raw GPS smoothed wind)",,"033015","Data quality check indicator","Data quality-check indicator (for u-component)",,"Operational"
2577.00,"09","Vertical sounding sequences (conventional data)","309063","(Raw GPS smoothed wind)",,"011004","v-component","v-component",,"Operational"
2578.00,"09","Vertical sounding sequences (conventional data)","309063","(Raw GPS smoothed wind)",,"033035","Manual/automatic quality control","Manual/automatic quality control (for v-component)",,"Operational"
2579.00,"09","Vertical sounding sequences (conventional data)","309063","(Raw GPS smoothed wind)",,"033015","Data quality check indicator","Data quality-check indicator (for v-component)",,"Operational"
2580.00,"09","Vertical sounding sequences (conventional data)","309063","(Raw GPS smoothed wind)",,"033007","Per cent confidence","Per cent confidence (for raw GPS smoothed wind)",,"Operational"
2581.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"301120","Radiosonde abbreviated header and launch information","Radiosonde abbreviated header and launch information",,"Operational"
2582.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"008041","Data significance","Data significance (6 = flight level observation)",,"Operational"
2583.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"301122","Date/time (to hundredths of second) (see Note 3)","Date/time (to hundredths of second)",,"Operational"
2584.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"201131","Change data width","Change data width",,"Operational"
2585.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"202129","Change scale","Change scale",,"Operational"
2586.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"104002","Replication descriptor","Replicate 4 descriptors 2 times",,"Operational"
2587.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"025069","Flight level pressure corrections","Flight level pressure correction",,"Operational"
2588.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"007004","Pressure","Pressure",,"Operational"
2589.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"033035","Manual/automatic quality control","Manual/automatic quality control (for pressure)",,"Operational"
2590.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"033015","Data quality check indicator","Data quality-check indicator (for pressure)",,"Operational"
2591.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"013003","Relative humidity","Relative humidity",,"Operational"
2592.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"033035","Manual/automatic quality control","Manual/automatic quality control (for relative humidity)",,"Operational"
2593.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"033015","Data quality check indicator","Data quality-check indicator (for relative humidity)",,"Operational"
2594.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"202000","Change scale","Cancel change scale",,"Operational"
2595.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"201000","Change data width","Cancel change data width",,"Operational"
2596.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"104002","Replication descriptor","Replicate 4 descriptors 2 times",,"Operational"
2597.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"002013","Solar and infrared radiation correction","Solar and infrared radiation correction",,"Operational"
2598.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"012101","Temperature/air temperature","Temperature/air temperature",,"Operational"
2599.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"033035","Manual/automatic quality control","Manual/automatic quality control (for temperature)",,"Operational"
2600.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"033015","Data quality check indicator","Data quality-check indicator (for temperature)",,"Operational"
2601.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"012103","Dew-point temperature","Dew-point temperature",,"Operational"
2602.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"033035","Manual/automatic quality control","Manual/automatic quality control (for dew-point temperature)",,"Operational"
2603.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"033015","Data quality check indicator","Data quality-check indicator (for dew-point temperature)",,"Operational"
2604.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"010009","Geopotential height","Geopotential height",,"Operational"
2605.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"033035","Manual/automatic quality control","Manual/automatic quality control (for geopotential height)",,"Operational"
2606.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"033015","Data quality check indicator","Data quality-check indicator (for geopotential height)",,"Operational"
2607.00,"09","Vertical sounding sequences (conventional data)","309065","(Processed GPS)",,"301120","Radiosonde abbreviated header and launch information","Radiosonde abbreviated header and launch information",,"Operational"
2608.00,"09","Vertical sounding sequences (conventional data)","309065","(Processed GPS)",,"008041","Data significance","Data significance (6 = flight level observation)",,"Operational"
2609.00,"09","Vertical sounding sequences (conventional data)","309065","(Processed GPS)",,"301122","Date/time (to hundredths of second) (see Note 3)","Date/time (to hundredths of second)",,"Operational"
2610.00,"09","Vertical sounding sequences (conventional data)","309065","(Processed GPS)",,"005001","Latitude (high accuracy)","Latitude (high accuracy)",,"Operational"
2611.00,"09","Vertical sounding sequences (conventional data)","309065","(Processed GPS)",,"033035","Manual/automatic quality control","Manual/automatic quality control (for latitude)",,"Operational"
2612.00,"09","Vertical sounding sequences (conventional data)","309065","(Processed GPS)",,"033015","Data quality check indicator","Data quality-check indicator (for latitude)",,"Operational"
2613.00,"09","Vertical sounding sequences (conventional data)","309065","(Processed GPS)",,"006001","Longitude (high accuracy)","Longitude (high accuracy)",,"Operational"
2614.00,"09","Vertical sounding sequences (conventional data)","309065","(Processed GPS)",,"033035","Manual/automatic quality control","Manual/automatic quality control (for longitude)",,"Operational"
2615.00,"09","Vertical sounding sequences (conventional data)","309065","(Processed GPS)",,"033015","Data quality check indicator","Data quality-check indicator (for longitude)",,"Operational"
2616.00,"09","Vertical sounding sequences (conventional data)","309065","(Processed GPS)",,"007007","Height","Height",,"Operational"
2617.00,"09","Vertical sounding sequences (conventional data)","309065","(Processed GPS)",,"033035","Manual/automatic quality control","Manual/automatic quality control (for height)",,"Operational"
2618.00,"09","Vertical sounding sequences (conventional data)","309065","(Processed GPS)",,"033015","Data quality check indicator","Data quality-check indicator (for height)",,"Operational"
2619.00,"09","Vertical sounding sequences (conventional data)","309065","(Processed GPS)",,"011003","u-component","u-component",,"Operational"
2620.00,"09","Vertical sounding sequences (conventional data)","309065","(Processed GPS)",,"033035","Manual/automatic quality control","Manual/automatic quality control (for u-component)",,"Operational"
2621.00,"09","Vertical sounding sequences (conventional data)","309065","(Processed GPS)",,"033015","Data quality check indicator","Data quality-check indicator (for u-component)",,"Operational"
2622.00,"09","Vertical sounding sequences (conventional data)","309065","(Processed GPS)",,"011004","v-component","v-component",,"Operational"
2623.00,"09","Vertical sounding sequences (conventional data)","309065","(Processed GPS)",,"033035","Manual/automatic quality control","Manual/automatic quality control (for v-component)",,"Operational"
2624.00,"09","Vertical sounding sequences (conventional data)","309065","(Processed GPS)",,"033015","Data quality check indicator","Data quality-check indicator (for v-component)",,"Operational"
2625.00,"09","Vertical sounding sequences (conventional data)","309066","(Standard and significant levels)",,"301120","Radiosonde abbreviated header and launch information","Radiosonde abbreviated header and launch information",,"Operational"
2626.00,"09","Vertical sounding sequences (conventional data)","309066","(Standard and significant levels)",,"008041","Data significance","Data significance (6 = flight level observation)",,"Operational"
2627.00,"09","Vertical sounding sequences (conventional data)","309066","(Standard and significant levels)",,"301122","Date/time (to hundredths of second) (see Note 3)","Date/time (to hundredths of second)",,"Operational"
2628.00,"09","Vertical sounding sequences (conventional data)","309066","(Standard and significant levels)",,"008040","Flight Level significance","Flight level significance",,"Operational"
2629.00,"09","Vertical sounding sequences (conventional data)","309066","(Standard and significant levels)",,"201131","Change data width","Change data width",,"Operational"
2630.00,"09","Vertical sounding sequences (conventional data)","309066","(Standard and significant levels)",,"202129","Change scale","Change scale",,"Operational"
2631.00,"09","Vertical sounding sequences (conventional data)","309066","(Standard and significant levels)",,"025069","Flight level pressure corrections","Flight level pressure correction",,"Operational"
2632.00,"09","Vertical sounding sequences (conventional data)","309066","(Standard and significant levels)",,"007004","Pressure","Pressure",,"Operational"
2633.00,"09","Vertical sounding sequences (conventional data)","309066","(Standard and significant levels)",,"013003","Relative humidity","Relative humidity",,"Operational"
2634.00,"09","Vertical sounding sequences (conventional data)","309066","(Standard and significant levels)",,"202000","Change scale","Cancel change scale",,"Operational"
2635.00,"09","Vertical sounding sequences (conventional data)","309066","(Standard and significant levels)",,"201000","Change data width","Cancel change data width",,"Operational"
2636.00,"09","Vertical sounding sequences (conventional data)","309066","(Standard and significant levels)",,"002013","Solar and infrared radiation correction","Solar and infrared radiation correction",,"Operational"
2637.00,"09","Vertical sounding sequences (conventional data)","309066","(Standard and significant levels)",,"012101","Temperature/air temperature","Temperature/air temperature",,"Operational"
2638.00,"09","Vertical sounding sequences (conventional data)","309066","(Standard and significant levels)",,"012103","Dew-point temperature","Dew-point temperature",,"Operational"
2639.00,"09","Vertical sounding sequences (conventional data)","309066","(Standard and significant levels)",,"010009","Geopotential height","Geopotential height",,"Operational"
2640.00,"09","Vertical sounding sequences (conventional data)","309066","(Standard and significant levels)",,"010007","Height","Height",,"Operational"
2641.00,"09","Vertical sounding sequences (conventional data)","309066","(Standard and significant levels)",,"011002","Wind speed","Wind speed",,"Operational"
2642.00,"09","Vertical sounding sequences (conventional data)","309066","(Standard and significant levels)",,"011001","Wind direction","Wind direction",,"Operational"
2643.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Identification","001035","Originating centre","Originating Centre",,"Operational"
2644.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Identification","001032","Generating application","Originating Process",,"Operational"
2645.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Identification","001015","Station or site name","Station name",,"Operational"
2646.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Identification","001063","ICAO location indicator","ICAO location indicator",,"Operational"
2647.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Identification","301001",,"block # stn #",,"Operational"
2648.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Location and reference time","301011",,"yy mm dd",,"Operational"
2649.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Location and reference time","301012",,"hh mm",,"Operational"
2650.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Location and reference time","301021",,"lat long",,"Operational"
2651.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Location and reference time","207001","Increase scale, reference value and data width","Increase scale factor by 1; reference value and data width are recalculated in accordance with the Table C specification of operator 2 07 YYY ",,"Operational"
2652.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Location and reference time","010001","Height of land surface","Station elevation (non coordinate)",,"Operational"
2653.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Location and reference time","207000","Increase scale, reference value and data width","Cancel increase scale factor operator",,"Operational"
2654.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Location and reference time","008086","Vertical significance for NWP","Vertical significance for NWP",,"Operational"
2655.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Location and reference time","007030","Height of station ground above mean sea level","Height of station above mean sea level",,"Operational"
2656.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Vertical profile metadata","025031","NWP - generated vertical profile thinning method","NWP-generated vertical profile thinning method",,"Operational"
2657.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Vertical profile metadata","008021","Time significance","Time significance",,"Operational"
2658.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Vertical profile metadata","004014","Time increment","Time increment in hours",,"Operational"
2659.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Point data at station height (including column-integrated data)","010004","Pressure","Pressure",,"Operational"
2660.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Point data at station height (including column-integrated data)","010051","Pressure reduced to mean sea level","Pressure reduced to MSL",,"Operational"
2661.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Point data at station height (including column-integrated data)","010009","Geopotential height","Geopotential Height ",,"Operational"
2662.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Point data at station height (including column-integrated data)","020010","Cloud cover (total)","Cloud cover (total)",,"Operational"
2663.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Point data at station height (including column-integrated data)","013095","Total column water vapour","Total column water vapour",,"Operational"
2664.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Replication loop for levels","128000","Replication descriptor",,,"Operational"
2665.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Replication loop for levels","031002","Extended delayed descriptor replication factor",,,"Operational"
2666.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data on pressure coordinates","113000","Replication descriptor",,,"Operational"
2667.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data on pressure coordinates","031000","Short delayed descriptor replication factor",,,"Operational"
2668.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data on pressure coordinates","008086","Vertical significance for NWP","Vertical significance for NWP",,"Operational"
2669.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data on pressure coordinates","007004","Pressure","Pressure",,"Operational"
2670.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data on pressure coordinates","011001","Wind direction (degree true)","Wind direction (degrees true)",,"Operational"
2671.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data on pressure coordinates","011002","Wind speed","Wind speed (m/s)",,"Operational"
2672.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data on pressure coordinates","012101","Temperature/air temperature","Temperature",,"Operational"
2673.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data on pressure coordinates","012102","Wet-bulb temperature","Wet Bulb Temperature",,"Operational"
2674.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data on pressure coordinates","012103","Dew-point temperature","Dew Point",,"Operational"
2675.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data on pressure coordinates","010009","Geopotential height","Geopotential Height ",,"Operational"
2676.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data on pressure coordinates","103000","Replication descriptor",,,"Operational"
2677.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data on pressure coordinates","031000","Short delayed descriptor replication factor",,,"Operational"
2678.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data on pressure coordinates","011021","Relative vorticity","Relative vorticity",,"Operational"
2679.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data on pressure coordinates","011022","Divergence","Divergence",,"Operational"
2680.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data on pressure coordinates","011005","w-component","Vertical motion",,"Operational"
2681.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data at 10 metres AGL","104000","Replication descriptor",,,"Operational"
2682.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data at 10 metres AGL","031000","Short delayed descriptor replication factor",,,"Operational"
2683.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data at 10 metres AGL","008086","Vertical significance for NWP","Vertical significance for NWP",,"Operational"
2684.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data at 10 metres AGL","007006","Height above station","Height above station",,"Operational"
2685.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data at 10 metres AGL","011001","Wind direction (degree true)","Wind direction (degrees true)",,"Operational"
2686.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data at 10 metres AGL","011002","Wind speed","Wind speed (m/s)",,"Operational"
2687.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data at 2 metres AGL","105000","Replication descriptor",,,"Operational"
2688.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data at 2 metres AGL","031000","Short delayed descriptor replication factor",,,"Operational"
2689.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data at 2 metres AGL","008086","Vertical significance for NWP","Vertical significance for NWP",,"Operational"
2690.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data at 2 metres AGL","007006","Height above station","Height above station",,"Operational"
2691.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data at 2 metres AGL","012101","Temperature/air temperature","Temperature",,"Operational"
2692.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data at 2 metres AGL","012102","Wet-bulb temperature","Wet Bulb Temperature",,"Operational"
2693.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data at 2 metres AGL","012103","Dew-point temperature","Dew Point Temperature",,"Operational"
2694.00,"10","Vertical sounding sequences (satellite data)","310001","(Satellite - brightness temperature)",,"301042",,"Identification, method, date/time",,"Operational"
2695.00,"10","Vertical sounding sequences (satellite data)","310001","(Satellite - brightness temperature)",,"303031",,"Significance data, land/sea, skin temperature",,"Operational"
2696.00,"10","Vertical sounding sequences (satellite data)","310001","(Satellite - brightness temperature)",,"303032",,"Cloud",,"Operational"
2697.00,"10","Vertical sounding sequences (satellite data)","310001","(Satellite - brightness temperature)",,"101026","Replication descriptor","Replicate 1 descriptor 26 times",,"Operational"
2698.00,"10","Vertical sounding sequences (satellite data)","310001","(Satellite - brightness temperature)",,"303025",,"Satellite channel and brightness temperature",,"Operational"
2699.00,"10","Vertical sounding sequences (satellite data)","310002","(Satellite - low level)",,"301042",,"Identification, method, date/time",,"Operational"
2700.00,"10","Vertical sounding sequences (satellite data)","310002","(Satellite - low level)",,"303031",,"Significance data, land/sea, skin temperature",,"Operational"
2701.00,"10","Vertical sounding sequences (satellite data)","310002","(Satellite - low level)",,"303032",,"Cloud",,"Operational"
2702.00,"10","Vertical sounding sequences (satellite data)","310002","(Satellite - low level)",,"101009","Replication descriptor","Replicate 1 descriptor 9 times",,"Operational"
2703.00,"10","Vertical sounding sequences (satellite data)","310002","(Satellite - low level)",,"303023",,"Layer mean temperature",,"Operational"
2704.00,"10","Vertical sounding sequences (satellite data)","310003","(Satellite - high level)",,"301042",,"Identification, method, date/time",,"Operational"
2705.00,"10","Vertical sounding sequences (satellite data)","310003","(Satellite - high level)",,"303031",,"Significance data, land/sea, skin temperature",,"Operational"
2706.00,"10","Vertical sounding sequences (satellite data)","310003","(Satellite - high level)",,"303032",,"Cloud",,"Operational"
2707.00,"10","Vertical sounding sequences (satellite data)","310003","(Satellite - high level)",,"101006","Replication descriptor","Replicate 1 descriptor 6 times",,"Operational"
2708.00,"10","Vertical sounding sequences (satellite data)","310003","(Satellite - high level)",,"303023",,"Layer mean temperature",,"Operational"
2709.00,"10","Vertical sounding sequences (satellite data)","310004","(Satellite - precipitable water)",,"301042",,"Identification, method, date/time",,"Operational"
2710.00,"10","Vertical sounding sequences (satellite data)","310004","(Satellite - precipitable water)",,"303031",,"Significance data, land/sea, skin temperature",,"Operational"
2711.00,"10","Vertical sounding sequences (satellite data)","310004","(Satellite - precipitable water)",,"303032",,"Cloud",,"Operational"
2712.00,"10","Vertical sounding sequences (satellite data)","310004","(Satellite - precipitable water)",,"101003","Replication descriptor","Replicate 1 descriptor 3 times",,"Operational"
2713.00,"10","Vertical sounding sequences (satellite data)","310004","(Satellite - precipitable water)",,"303024",,"Precipitable water",,"Operational"
2714.00,"10","Vertical sounding sequences (satellite data)","310005",,,"301042",,"Identification, method, date/time",,"Operational"
2715.00,"10","Vertical sounding sequences (satellite data)","310005",,,"303031",,"Significance data, land/sea, skin temperature",,"Operational"
2716.00,"10","Vertical sounding sequences (satellite data)","310005",,,"303033",,"Cloud",,"Operational"
2717.00,"10","Vertical sounding sequences (satellite data)","310005",,,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
2718.00,"10","Vertical sounding sequences (satellite data)","310005",,,"031001","Delayed descriptor replication factor","Delayed descriptor replication factor",,"Operational"
2719.00,"10","Vertical sounding sequences (satellite data)","310005",,,"303025",,"Satellite channel and brightness temperature",,"Operational"
2720.00,"10","Vertical sounding sequences (satellite data)","310006",,,"301042",,"Identification, method, date/time",,"Operational"
2721.00,"10","Vertical sounding sequences (satellite data)","310006",,,"303031",,"Significance data, land/sea, skin temperature",,"Operational"
2722.00,"10","Vertical sounding sequences (satellite data)","310006",,,"303033",,"Cloud",,"Operational"
2723.00,"10","Vertical sounding sequences (satellite data)","310006",,,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
2724.00,"10","Vertical sounding sequences (satellite data)","310006",,,"031001","Delayed descriptor replication factor","Delayed descriptor replication factor",,"Operational"
2725.00,"10","Vertical sounding sequences (satellite data)","310006",,,"303023",,"Layer mean temperature",,"Operational"
2726.00,"10","Vertical sounding sequences (satellite data)","310007",,,"301042",,"Identification, method, date/time",,"Operational"
2727.00,"10","Vertical sounding sequences (satellite data)","310007",,,"303031",,"Significance data, land/sea, skin temperature",,"Operational"
2728.00,"10","Vertical sounding sequences (satellite data)","310007",,,"303033",,"Cloud",,"Operational"
2729.00,"10","Vertical sounding sequences (satellite data)","310007",,,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
2730.00,"10","Vertical sounding sequences (satellite data)","310007",,,"031001","Delayed descriptor replication factor","Delayed descriptor replication factor",,"Operational"
2731.00,"10","Vertical sounding sequences (satellite data)","310007",,,"303024",,"Precipitable water",,"Operational"
2732.00,"10","Vertical sounding sequences (satellite data)","310008","(ATOVS HIRS report)",,"310011","ATOVS field of view variables","ATOVS field of view variables",,"Operational"
2733.00,"10","Vertical sounding sequences (satellite data)","310008","(ATOVS HIRS report)",,"101019","Replication descriptor","Replicate 1 descriptor 19 times",,"Operational"
2734.00,"10","Vertical sounding sequences (satellite data)","310008","(ATOVS HIRS report)",,"310012","ATOVS channel variables","ATOVS channel variables",,"Operational"
2735.00,"10","Vertical sounding sequences (satellite data)","310008","(ATOVS HIRS report)",,"002150","TOVS/ATOVS/AVHRR instrumentation channel number","TOVS/ATOVS/AVHRR instrumentation channel number",,"Operational"
2736.00,"10","Vertical sounding sequences (satellite data)","310008","(ATOVS HIRS report)",,"025079","Albedo-radiance solar filtered irradiance for ATOVS","Albedo-radiance solar filtered irradiance for ATOVS",,"Operational"
2737.00,"10","Vertical sounding sequences (satellite data)","310008","(ATOVS HIRS report)",,"025080","Albedo-radiance equivalent filter width for ATOVS","Albedo-radiance equivalent filter width for ATOVS",,"Operational"
2738.00,"10","Vertical sounding sequences (satellite data)","310008","(ATOVS HIRS report)",,"033032","Channel quality flags for ATOVS","Channel quality flags for ATOVS",,"Operational"
2739.00,"10","Vertical sounding sequences (satellite data)","310008","(ATOVS HIRS report)",,"014045","Channel radiance","Channel radiance",,"Operational"
2740.00,"10","Vertical sounding sequences (satellite data)","310009","(ATOVS AMSU-A report)",,"310011","ATOVS field of view variables","ATOVS field of view variables",,"Operational"
2741.00,"10","Vertical sounding sequences (satellite data)","310009","(ATOVS AMSU-A report)",,"101015","Replication descriptor","Replicate 1 descriptor 15 times",,"Operational"
2742.00,"10","Vertical sounding sequences (satellite data)","310009","(ATOVS AMSU-A report)",,"310012","ATOVS channel variables","ATOVS channel variables",,"Operational"
2743.00,"10","Vertical sounding sequences (satellite data)","310010","(ATOVS AMSU-B/MHS report)",,"310011","ATOVS field of view variables","ATOVS field of view variables",,"Operational"
2744.00,"10","Vertical sounding sequences (satellite data)","310010","(ATOVS AMSU-B/MHS report)",,"101005","Replication descriptor","Replicate 1 descriptor 5 times",,"Operational"
2745.00,"10","Vertical sounding sequences (satellite data)","310010","(ATOVS AMSU-B/MHS report)",,"310012","ATOVS channel variables","ATOVS channel variables",,"Operational"
2746.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"008070","TOVS/ATOVS product qualifier","TOVS/ATOVS product qualifier",,"Operational"
2747.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"001033","Identification of originating/generating centre","Identification of originating/generating centre",,"Operational"
2748.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"001034","Identification of originating/generating sub-centre","Identification of originating/generating sub-centre",,"Operational"
2749.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"008070","TOVS/ATOVS product qualifier","TOVS/ATOVS product qualifier",,"Operational"
2750.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"001033","Identification of originating/generating centre","Identification of originating/generating centre",,"Operational"
2751.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"001034","Identification of originating/generating sub-centre","Identification of originating/generating sub-centre",,"Operational"
2752.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"001007","Satellite identifier","Satellite identifier",,"Operational"
2753.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"002048","Satellite sensor indicator","Satellite sensor indicator",,"Operational"
2754.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"005040","Orbit number","Orbit number",,"Operational"
2755.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"025075","Satellite antenna corrections version number","Satellite antenna corrections version number",,"Operational"
2756.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"201133","Change data width","Change width",,"Operational"
2757.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"005041","Scan line number","Scan line number",,"Operational"
2758.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"201000","Change data width","Change width",,"Operational"
2759.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"005043","Field of view number","Field of view number",,"Operational"
2760.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"025070","Major frame count","Major frame count",,"Operational"
2761.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"033030","Scan line status flags for ATOVS","Scan line status flags for ATOVS",,"Operational"
2762.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"033031","Scan line quality flags for ATOVS","Scan line quality flags for ATOVS",,"Operational"
2763.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"004001","Year","Year",,"Operational"
2764.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"004002","Month","Month",,"Operational"
2765.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"004003","Day","Day",,"Operational"
2766.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"004004","Hour","Hour",,"Operational"
2767.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"004005","Minute","Minute",,"Operational"
2768.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"202131","Change scale","Change scale",,"Operational"
2769.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"201138","Change data width","Change width",,"Operational"
2770.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"004006","Second","Second",,"Operational"
2771.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"201000","Change data width","Change width",,"Operational"
2772.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"202000","Change scale","Change scale",,"Operational"
2773.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"005001","Latitude (high accuracy)","Latitude",,"Operational"
2774.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"006001","Longitude (high accuracy)","Longitude",,"Operational"
2775.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"202126","Change scale","Change scale",,"Operational"
2776.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"007001","Height of station","Height of station",,"Operational"
2777.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"202000","Change scale","Change scale",,"Operational"
2778.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"007024","Satellite zenith angle","Satellite zenith angle",,"Operational"
2779.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"005021","Bearing or azimuth","Satellite azimuth",,"Operational"
2780.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"007025","Solar zenith angle","Solar zenith angle",,"Operational"
2781.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"005022","Solar azimuth","Solar azimuth",,"Operational"
2782.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"033033","Field of view quality flags for ATOVS","Field of view quality flags for ATOVS",,"Operational"
2783.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"002151","Radiometer identifier","Radiometer identifier",,"Operational"
2784.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"012064","Instrument temperature","Instrument temperature",,"Operational"
2785.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"002151","Radiometer identifier","Radiometer identifier",,"Operational"
2786.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"012064","Instrument temperature","Instrument temperature",,"Operational"
2787.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"002151","Radiometer identifier","Radiometer identifier",,"Operational"
2788.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"012064","Instrument temperature","Instrument temperature",,"Operational"
2789.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"002151","Radiometer identifier","Radiometer identifier",,"Operational"
2790.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"012064","Instrument temperature","Instrument temperature",,"Operational"
2791.00,"10","Vertical sounding sequences (satellite data)","310012","(ATOVS channel variables)",,"002150","TOVS/ATOVS/AVHRR instrumentation channel number","TOVS/ATOVS/AVHRR instrumentation channel number",,"Operational"
2792.00,"10","Vertical sounding sequences (satellite data)","310012","(ATOVS channel variables)",,"025076","Log-10 of (Temperature-radiance central wavenumber) for ATOVS","Log-10 of (temperature-radiance central wavenumber) for ATOVS",,"Operational"
2793.00,"10","Vertical sounding sequences (satellite data)","310012","(ATOVS channel variables)",,"025077","Bandwidth correction coefficient 1 for ATOVS","Bandwidth correction coefficient 1 for ATOVS",,"Operational"
2794.00,"10","Vertical sounding sequences (satellite data)","310012","(ATOVS channel variables)",,"025078","Bandwidth correction coefficient 2 for ATOVS","Bandwidth correction coefficient 2 for ATOVS",,"Operational"
2795.00,"10","Vertical sounding sequences (satellite data)","310012","(ATOVS channel variables)",,"033032","Channel quality flags for ATOVS","Channel quality flags for ATOVS",,"Operational"
2796.00,"10","Vertical sounding sequences (satellite data)","310012","(ATOVS channel variables)",,"201132","Change data width","Change width",,"Operational"
2797.00,"10","Vertical sounding sequences (satellite data)","310012","(ATOVS channel variables)",,"202129","Change scale","Change scale",,"Operational"
2798.00,"10","Vertical sounding sequences (satellite data)","310012","(ATOVS channel variables)",,"012063","Brightness temperature","Brightness temperature",,"Operational"
2799.00,"10","Vertical sounding sequences (satellite data)","310012","(ATOVS channel variables)",,"202000","Change scale","Change scale",,"Operational"
2800.00,"10","Vertical sounding sequences (satellite data)","310012","(ATOVS channel variables)",,"201000","Change data width","Change width",,"Operational"
2801.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"001007","Satellite identifier","Satellite ID",,"Operational"
2802.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"005040","Orbit number","Orbit number",,"Operational"
2803.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"004001","Year","Year",,"Operational"
2804.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"004002","Month","Month",,"Operational"
2805.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"004003","Day","Day",,"Operational"
2806.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"004004","Hour","Hour",,"Operational"
2807.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"004005","Minute","Minute",,"Operational"
2808.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"004006","Second","Second",,"Operational"
2809.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"005001","Latitude (high accuracy)","Latitude",,"Operational"
2810.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"006001","Longitude (high accuracy)","Longitude",,"Operational"
2811.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"007025","Solar zenith angle","Solar zenith angle",,"Operational"
2812.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"005043","Field of view number","Field of view number",,"Operational"
2813.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"025085","Fraction of clear pixels in HIRS FOV","Fraction of clear pixels in HIRS field of view",,"Operational"
2814.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"201131","Change data width","Change width",,"Operational"
2815.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"202129","Change scale","Change scale",,"Operational"
2816.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"002150","TOVS/ATOVS/AVHRR instrumentation channel number","TOVS/ATOVS/AVHRR instrumentation channel number",,"Operational"
2817.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"008023","First-order statistics","First-order statistics",,"Operational"
2818.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"008072","Pixel(s) type","Pixel(s) type",,"Operational"
2819.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"014027","Albedo","Albedo",,"Operational"
2820.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"008072","Pixel(s) type","Pixel(s) type",,"Operational"
2821.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"014027","Albedo","Albedo",,"Operational"
2822.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"002150","TOVS/ATOVS/AVHRR instrumentation channel number","TOVS/ATOVS/AVHRR instrumentation channel number",,"Operational"
2823.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"008023","First-order statistics","First-order statistics",,"Operational"
2824.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"008072","Pixel(s) type","Pixel(s) type",,"Operational"
2825.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"014027","Albedo","Albedo",,"Operational"
2826.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"008072","Pixel(s) type","Pixel(s) type",,"Operational"
2827.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"014027","Albedo","Albedo",,"Operational"
2828.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"002150","TOVS/ATOVS/AVHRR instrumentation channel number","TOVS/ATOVS/AVHRR instrumentation channel number",,"Operational"
2829.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"008023","First-order statistics","First-order statistics",,"Operational"
2830.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"008072","Pixel(s) type","Pixel(s) type",,"Operational"
2831.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"014027","Albedo","Albedo",,"Operational"
2832.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"008072","Pixel(s) type","Pixel(s) type",,"Operational"
2833.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"014027","Albedo","Albedo",,"Operational"
2834.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"202000","Change scale","Change scale",,"Operational"
2835.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"201000","Change data width","Change width",,"Operational"
2836.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"201132","Change data width","Change width",,"Operational"
2837.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"202129","Change scale","Change scale",,"Operational"
2838.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"002150","TOVS/ATOVS/AVHRR instrumentation channel number","TOVS/ATOVS/AVHRR instrumentation channel number",,"Operational"
2839.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"008023","First-order statistics","First-order statistics",,"Operational"
2840.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"008072","Pixel(s) type","Pixel(s) type",,"Operational"
2841.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"012063","Brightness temperature","Brightness temperature",,"Operational"
2842.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"008072","Pixel(s) type","Pixel(s) type",,"Operational"
2843.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"012063","Brightness temperature","Brightness temperature",,"Operational"
2844.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"002150","TOVS/ATOVS/AVHRR instrumentation channel number","TOVS/ATOVS/AVHRR instrumentation channel number",,"Operational"
2845.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"008023","First-order statistics","First-order statistics",,"Operational"
2846.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"008072","Pixel(s) type","Pixel(s) type",,"Operational"
2847.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"012063","Brightness temperature","Brightness temperature",,"Operational"
2848.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"008072","Pixel(s) type","Pixel(s) type",,"Operational"
2849.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"012063","Brightness temperature","Brightness temperature",,"Operational"
2850.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"008023","First-order statistics","First-order statistics",,"Operational"
2851.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"008072","Pixel(s) type","Pixel(s) type",,"Operational"
2852.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"012063","Brightness temperature","Brightness temperature",,"Operational"
2853.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"008072","Pixel(s) type","Pixel(s) type",,"Operational"
2854.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"012063","Brightness temperature","Brightness temperature",,"Operational"
2855.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"002150","TOVS/ATOVS/AVHRR instrumentation channel number","TOVS/ATOVS/AVHRR instrumentation channel number",,"Operational"
2856.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"008023","First-order statistics","First-order statistics",,"Operational"
2857.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"008072","Pixel(s) type","Pixel(s) type",,"Operational"
2858.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"012063","Brightness temperature","Brightness temperature",,"Operational"
2859.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"008072","Pixel(s) type","Pixel(s) type",,"Operational"
2860.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"012063","Brightness temperature","Brightness temperature",,"Operational"
2861.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"202000","Change scale","Change scale",,"Operational"
2862.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"201000","Change data width","Change width",,"Operational"
2863.00,"10","Vertical sounding sequences (satellite data)","310014","(Satellite - geostationary wind data)",,"301072","Satellite identification","Satellite identification, date, time, latitude, longitude",,"Operational"
2864.00,"10","Vertical sounding sequences (satellite data)","310014","(Satellite - geostationary wind data)",,"303041","Wind sequence","Wind sequence",,"Operational"
2865.00,"10","Vertical sounding sequences (satellite data)","310014","(Satellite - geostationary wind data)",,"304011","GOES-I/M info","GOES-I/M information",,"Operational"
2866.00,"10","Vertical sounding sequences (satellite data)","310015","(Meteosat radiance data)",,"301072","Satellite identification","Satellite identification",,"Operational"
2867.00,"10","Vertical sounding sequences (satellite data)","310015","(Meteosat radiance data)",,"007024","Satellite zenith angle","Satellite zenith angle",,"Operational"
2868.00,"10","Vertical sounding sequences (satellite data)","310015","(Meteosat radiance data)",,"010002","Height","Height",,"Operational"
2869.00,"10","Vertical sounding sequences (satellite data)","310015","(Meteosat radiance data)",,"303041","Wind sequence","Wind sequence",,"Operational"
2870.00,"10","Vertical sounding sequences (satellite data)","310015","(Meteosat radiance data)",,"101003","Replication descriptor","Replicate next descriptor 3 times",,"Operational"
2871.00,"10","Vertical sounding sequences (satellite data)","310015","(Meteosat radiance data)",,"304032","Cloud fraction","Cloud fraction",,"Operational"
2872.00,"10","Vertical sounding sequences (satellite data)","310015","(Meteosat radiance data)",,"002152","Satellite instrument used in data processing","Satellite instrument used in data processing",,"Operational"
2873.00,"10","Vertical sounding sequences (satellite data)","310015","(Meteosat radiance data)",,"002024","Integrated mean humidity computational method","Integrated mean humidity computational method",,"Operational"
2874.00,"10","Vertical sounding sequences (satellite data)","310015","(Meteosat radiance data)",,"007004","Pressure","Pressure",,"Operational"
2875.00,"10","Vertical sounding sequences (satellite data)","310015","(Meteosat radiance data)",,"007004","Pressure","Pressure",,"Operational"
2876.00,"10","Vertical sounding sequences (satellite data)","310015","(Meteosat radiance data)",,"013003","Relative humidity","Relative humidity",,"Operational"
2877.00,"10","Vertical sounding sequences (satellite data)","310015","(Meteosat radiance data)",,"101003","Replication descriptor","Replicate next descriptor 3 times",,"Operational"
2878.00,"10","Vertical sounding sequences (satellite data)","310015","(Meteosat radiance data)",,"304033","Clear sky radiance","Clear sky radiance",,"Operational"
2879.00,"10","Vertical sounding sequences (satellite data)","310016","(Meteosat Second Generation (MSG) radiance data)",,"301072","Satellite identification","Satellite identification",,"Operational"
2880.00,"10","Vertical sounding sequences (satellite data)","310016","(Meteosat Second Generation (MSG) radiance data)",,"007024","Satellite zenith angle","Satellite zenith angle",,"Operational"
2881.00,"10","Vertical sounding sequences (satellite data)","310016","(Meteosat Second Generation (MSG) radiance data)",,"010002","Height","Height",,"Operational"
2882.00,"10","Vertical sounding sequences (satellite data)","310016","(Meteosat Second Generation (MSG) radiance data)",,"303041","Wind sequence","Wind sequence",,"Operational"
2883.00,"10","Vertical sounding sequences (satellite data)","310016","(Meteosat Second Generation (MSG) radiance data)",,"101012","Replication descriptor","Replicate next descriptor 12 times",,"Operational"
2884.00,"10","Vertical sounding sequences (satellite data)","310016","(Meteosat Second Generation (MSG) radiance data)",,"304032","Cloud fraction","Cloud fraction",,"Operational"
2885.00,"10","Vertical sounding sequences (satellite data)","310016","(Meteosat Second Generation (MSG) radiance data)",,"002152","Satellite instrument used in data processing","Satellite instrument used in data processing",,"Operational"
2886.00,"10","Vertical sounding sequences (satellite data)","310016","(Meteosat Second Generation (MSG) radiance data)",,"002024","Integrated mean humidity computational method","Integrated mean humidity computational method",,"Operational"
2887.00,"10","Vertical sounding sequences (satellite data)","310016","(Meteosat Second Generation (MSG) radiance data)",,"007004","Pressure","Pressure",,"Operational"
2888.00,"10","Vertical sounding sequences (satellite data)","310016","(Meteosat Second Generation (MSG) radiance data)",,"007004","Pressure","Pressure",,"Operational"
2889.00,"10","Vertical sounding sequences (satellite data)","310016","(Meteosat Second Generation (MSG) radiance data)",,"013003","Relative humidity","Relative humidity",,"Operational"
2890.00,"10","Vertical sounding sequences (satellite data)","310016","(Meteosat Second Generation (MSG) radiance data)",,"101012","Replication descriptor","Replicate next descriptor 12 times",,"Operational"
2891.00,"10","Vertical sounding sequences (satellite data)","310016","(Meteosat Second Generation (MSG) radiance data)",,"304033","Clear sky radiance","Clear sky radiance",,"Operational"
2892.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"001007","Satellite identifier","Satellite identifier",,"Operational"
2893.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"005040","Orbit number","Orbit number",,"Operational"
2894.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"004001","Year","Year",,"Operational"
2895.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"004043","Day of the year","Day of year",,"Operational"
2896.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"004004","Hour","Hour",,"Operational"
2897.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"004005","Minute","Minute",,"Operational"
2898.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"004006","Second","Second",,"Operational"
2899.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"207002","Increase scale, reference value and data width","Increase scale, reference value and data width",,"Operational"
2900.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"026030","Measurement integration time","Measurement integration time",,"Operational"
2901.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"207000","Increase scale, reference value and data width","Cancel increase scale, reference value and data width",,"Operational"
2902.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"005002","Latitude (coarse accuracy)","Latitude",,"Operational"
2903.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"006002","Longitude (coarse accuracy)","Longitude",,"Operational"
2904.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"033072","Ozone error","Ozone error",,"Operational"
2905.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"007025","Solar zenith angle","Solar zenith angle",,"Operational"
2906.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"005022","Solar azimuth","Solar azimuth angle",,"Operational"
2907.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"207002","Increase scale, reference value and data width","Increase scale, reference value and data width",,"Operational"
2908.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"015001","Total ozone","Total ozone",,"Operational"
2909.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"207000","Increase scale, reference value and data width","Cancel increase scale, reference value and data width",,"Operational"
2910.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"008003","Vertical significance (satellite observations)","Vertical significance (0 = Surface)",,"Operational"
2911.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"207001","Increase scale, reference value and data width","Increase scale, reference value and data width",,"Operational"
2912.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"010004","Pressure","Pressure (terrain)",,"Operational"
2913.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"207000","Increase scale, reference value and data width","Cancel increase scale, reference value and data width",,"Operational"
2914.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"008003","Vertical significance (satellite observations)","Vertical significance (Missing = Cancel)",,"Operational"
2915.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"008003","Vertical significance (satellite observations)","Vertical significance (2 = Cloud top)",,"Operational"
2916.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"033042","Type of limit represented by following value","Type of limit represented by following value (0 = Exclusive lower limit)",,"Operational"
2917.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"207001","Increase scale, reference value and data width","Increase scale, reference value and data width",,"Operational"
2918.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"007004","Pressure","Pressure",,"Operational"
2919.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"207000","Increase scale, reference value and data width","Cancel increase scale, reference value and data width",,"Operational"
2920.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"207002","Increase scale, reference value and data width","Increase scale, reference value and data width",,"Operational"
2921.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"015001","Total ozone","Total ozone (below cloud top pressure)",,"Operational"
2922.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"207000","Increase scale, reference value and data width","Cancel increase scale, reference value and data width",,"Operational"
2923.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"008003","Vertical significance (satellite observations)","Vertical significance (Missing = Cancel)",,"Operational"
2924.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"207002","Increase scale, reference value and data width","Increase scale, reference value and data width",,"Operational"
2925.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"020081","Cloud amount in segment","Cloud amount in segment (cloud fraction)",,"Operational"
2926.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"207000","Increase scale, reference value and data width","Cancel increase scale, reference value and data width",,"Operational"
2927.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"020065","Snow cover","Snow cover",,"Operational"
2928.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"008029","Surface type","Surface type",,"Operational"
2929.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"207004","Increase scale, reference value and data width","Increase scale, reference value and data width",,"Operational"
2930.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"015030","Aerosol contamination index","Aerosol contamination index",,"Operational"
2931.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"207000","Increase scale, reference value and data width","Cancel increase scale, reference value and data width",,"Operational"
2932.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"008075","Ascending/descending orbit qualifier","Ascending/descending orbit qualifier",,"Operational"
2933.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"001007","Satellite identifier","Satellite identifier",,"Operational"
2934.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"002019","Satellite instruments","Satellite instruments (624 = SBUV/2)",,"Operational"
2935.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"301011",,"Date",,"Operational"
2936.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"301013",,"Time",,"Operational"
2937.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"301023",,"Latitude/longitude",,"Operational"
2938.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"007025","Solar zenith angle","Solar zenith angle",,"Operational"
2939.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"008021","Time significance","Time significance (28 = Start of scan)",,"Operational"
2940.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"007025","Solar zenith angle","Solar zenith angle",,"Operational"
2941.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"008021","Time significance","Time significance (29 = End of scan)",,"Operational"
2942.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"007025","Solar zenith angle","Solar zenith angle",,"Operational"
2943.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"008021","Time significance","Time significance (Missing = Cancel)",,"Operational"
2944.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"008029","Surface type","Surface type",,"Operational"
2945.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"005040","Orbit number","Orbit number",,"Operational"
2946.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"008075","Ascending/descending orbit qualifier","Ascending/descending orbit qualifier",,"Operational"
2947.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"008003","Vertical significance (satellite observations)","Vertical significance (0 = Surface)",,"Operational"
2948.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"010004","Pressure","Pressure (terrain)",,"Operational"
2949.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"008003","Vertical significance (satellite observations)","Vertical significance (Missing = Cancel)",,"Operational"
2950.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"207002","Increase scale, reference value and data width","Increase scale, reference value and data width",,"Operational"
2951.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"015001","Total ozone","Total ozone",,"Operational"
2952.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"207000","Increase scale, reference value and data width","Cancel increase scale, reference value and data width",,"Operational"
2953.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"033070","Total ozone quality","Total ozone quality",,"Operational"
2954.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"015030","Aerosol contamination index","Aerosol contamination index",,"Operational"
2955.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"207002","Increase scale, reference value and data width","Increase scale, reference value and data width",,"Operational"
2956.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"020081","Cloud amount in segment","Cloud amount in segment (cloud fraction)",,"Operational"
2957.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"207000","Increase scale, reference value and data width","Cancel increase scale, reference value and data width",,"Operational"
2958.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"008003","Vertical significance (satellite observations)","Vertical significance (2 = Cloud top)",,"Operational"
2959.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"033042","Type of limit represented by following value","Type of limit represented by following value (0 = Exclusive lower limit)",,"Operational"
2960.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"007004","Pressure","Pressure",,"Operational"
2961.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"207002","Increase scale, reference value and data width","Increase scale, reference value and data width",,"Operational"
2962.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"015001","Total ozone","Total ozone (below cloud top pressure)",,"Operational"
2963.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"207000","Increase scale, reference value and data width","Cancel increase scale, reference value and data width",,"Operational"
2964.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"008003","Vertical significance (satellite observations)","Vertical significance (Missing = Cancel)",,"Operational"
2965.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"113021","Replication descriptor","Repeat next 13 descriptors 21 times",,"Operational"
2966.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"007004","Pressure","Pressure (at bottom of layer)",,"Operational"
2967.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"007004","Pressure","Pressure (at top of layer)",,"Operational"
2968.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"207002","Increase scale, reference value and data width","Increase scale, reference value and data width",,"Operational"
2969.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"008021","Time significance","Time significance (27 = First guess)",,"Operational"
2970.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"015005","Ozone p","Ozone p",,"Operational"
2971.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"008021","Time significance","Time significance (Missing = Cancel)",,"Operational"
2972.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"015005","Ozone p","Ozone p",,"Operational"
2973.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"033007","Per cent confidence","% confidence",,"Operational"
2974.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"207000","Increase scale, reference value and data width","Cancel increase scale, reference value and data width",,"Operational"
2975.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"008026","Matrix significance","Matrix significance (0 = Row of averaging kernel matrix)",,"Operational"
2976.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"101020","Replication descriptor","Repeat next descriptor 20 times",,"Operational"
2977.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"025143","Linear coefficient","Linear coefficient",,"Operational"
2978.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"008026","Matrix significance","Matrix significance (Missing = Cancel)",,"Operational"
2979.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"008043","Atmospheric chemical or physical constituent type","Atmospheric chemical type (0 = Ozone)",,"Operational"
2980.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"109015","Replication descriptor","Repeat next 9 descriptors 15 times",,"Operational"
2981.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"007004","Pressure","Pressure",,"Operational"
2982.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"008090","Decimal scale of following significands","Decimal scale of following Table B values",,"Operational"
2983.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"207006","Increase scale, reference value and data width","Increase scale, reference value and data width",,"Operational"
2984.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"015008","Significand of volumetric mixing ratio","Scaled mixing ratio (volumetric)",,"Operational"
2985.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"207000","Increase scale, reference value and data width","Cancel increase scale, reference value and data width",,"Operational"
2986.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"008090","Decimal scale of following significands","Decimal scale of following Table B values (Missing = Cancel)",,"Operational"
2987.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"207002","Increase scale, reference value and data width","Increase scale, reference value and data width",,"Operational"
2988.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"033007","Per cent confidence","% confidence",,"Operational"
2989.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"207000","Increase scale, reference value and data width","Cancel increase scale, reference value and data width",,"Operational"
2990.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"008043","Atmospheric chemical or physical constituent type","Atmospheric chemical type (Missing = Cancel)",,"Operational"
2991.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"033071","Profile ozone quality","Profile ozone quality",,"Operational"
2992.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"108008","Replication descriptor","Repeat next 8 descriptors 8 times",,"Operational"
2993.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"202124","Change scale","Change scale",,"Operational"
2994.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"201107","Change data width","Change data width",,"Operational"
2995.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"002071","Spectrographic wavelength","Spectrographic wavelength",,"Operational"
2996.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"201000","Change data width","Cancel change data width",,"Operational"
2997.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"202000","Change scale","Cancel change scale",,"Operational"
2998.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"207002","Increase scale, reference value and data width","Increase scale, reference value and data width",,"Operational"
2999.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"020081","Cloud amount in segment","Cloud amount in segment (cloud fraction)",,"Operational"
3000.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"207000","Increase scale, reference value and data width","Cancel increase scale, reference value and data width",,"Operational"
3001.00,"10","Vertical sounding sequences (satellite data)","310020","(Retrieved ozone data)",,"310022",,,,"Operational"
3002.00,"10","Vertical sounding sequences (satellite data)","310020","(Retrieved ozone data)",,"301011",,"Year, month, day",,"Operational"
3003.00,"10","Vertical sounding sequences (satellite data)","310020","(Retrieved ozone data)",,"301013",,"Hour, minute, second",,"Operational"
3004.00,"10","Vertical sounding sequences (satellite data)","310020","(Retrieved ozone data)",,"301021",,"Latitude, longitude (high accuracy)",,"Operational"
3005.00,"10","Vertical sounding sequences (satellite data)","310020","(Retrieved ozone data)",,"304034",,,,"Operational"
3006.00,"10","Vertical sounding sequences (satellite data)","310020","(Retrieved ozone data)",,"310021",,,,"Operational"
3007.00,"10","Vertical sounding sequences (satellite data)","310021",,,"108000","Replication descriptor","Delayed replication of 8 next descriptors",,"Operational"
3008.00,"10","Vertical sounding sequences (satellite data)","310021",,,"031001","Delayed descriptor replication factor","Delayed descriptor replication factor",,"Operational"
3009.00,"10","Vertical sounding sequences (satellite data)","310021",,,"201131","Change data width","Change data width",,"Operational"
3010.00,"10","Vertical sounding sequences (satellite data)","310021",,,"202129","Change scale","Change scale",,"Operational"
3011.00,"10","Vertical sounding sequences (satellite data)","310021",,,"007004","Pressure","Pressure",,"Operational"
3012.00,"10","Vertical sounding sequences (satellite data)","310021",,,"007004","Pressure","Pressure",,"Operational"
3013.00,"10","Vertical sounding sequences (satellite data)","310021",,,"202000","Change scale","Change scale back to Table B",,"Operational"
3014.00,"10","Vertical sounding sequences (satellite data)","310021",,,"201000","Change data width","Change data width back to Table B",,"Operational"
3015.00,"10","Vertical sounding sequences (satellite data)","310021",,,"015020","Integrated ozone density","Integrated ozone density",,"Operational"
3016.00,"10","Vertical sounding sequences (satellite data)","310021",,,"010002","Height","Height",,"Operational"
3017.00,"10","Vertical sounding sequences (satellite data)","310022",,,"001007","Satellite identifier","Satellite identifier",,"Operational"
3018.00,"10","Vertical sounding sequences (satellite data)","310022",,,"002019","Satellite instruments","Satellite instrument used",,"Operational"
3019.00,"10","Vertical sounding sequences (satellite data)","310022",,,"001033","Identification of originating/generating centre","Identification of originating/generating centre",,"Operational"
3020.00,"10","Vertical sounding sequences (satellite data)","310022",,,"002172","Product type for retrieved atmospheric gases","Product type for retrieved atmospheric gases",,"Operational"
3021.00,"10","Vertical sounding sequences (satellite data)","310023","(Geostationary multi-channel satellite radiance data)",,"301072","Satellite identification","Satellite identification",,"Operational"
3022.00,"10","Vertical sounding sequences (satellite data)","310023","(Geostationary multi-channel satellite radiance data)",,"030021","Number of pixels per row","Number of pixels per row",,"Operational"
3023.00,"10","Vertical sounding sequences (satellite data)","310023","(Geostationary multi-channel satellite radiance data)",,"030022","Number of pixels per column","Number of pixels per column",,"Operational"
3024.00,"10","Vertical sounding sequences (satellite data)","310023","(Geostationary multi-channel satellite radiance data)",,"008012","Land/sea qualifier","Land/sea qualifier",,"Operational"
3025.00,"10","Vertical sounding sequences (satellite data)","310023","(Geostationary multi-channel satellite radiance data)",,"007024","Satellite zenith angle","Satellite zenith angle",,"Operational"
3026.00,"10","Vertical sounding sequences (satellite data)","310023","(Geostationary multi-channel satellite radiance data)",,"007025","Solar zenith angle","Solar zenith angle",,"Operational"
3027.00,"10","Vertical sounding sequences (satellite data)","310023","(Geostationary multi-channel satellite radiance data)",,"010002","Height","Height",,"Operational"
3028.00,"10","Vertical sounding sequences (satellite data)","310023","(Geostationary multi-channel satellite radiance data)",,"101012","Replication descriptor","Replicate next descriptor 12 times",,"Operational"
3029.00,"10","Vertical sounding sequences (satellite data)","310023","(Geostationary multi-channel satellite radiance data)",,"304032","Cloud fraction","Cloud fraction",,"Operational"
3030.00,"10","Vertical sounding sequences (satellite data)","310023","(Geostationary multi-channel satellite radiance data)",,"105002","Replication descriptor","Replicate next 5 descriptors 2 times",,"Operational"
3031.00,"10","Vertical sounding sequences (satellite data)","310023","(Geostationary multi-channel satellite radiance data)",,"002152","Satellite instrument used in data processing","Satellite instrument used in data processing",,"Operational"
3032.00,"10","Vertical sounding sequences (satellite data)","310023","(Geostationary multi-channel satellite radiance data)",,"002024","Integrated mean humidity computational method","Integrated mean humidity computational method",,"Operational"
3033.00,"10","Vertical sounding sequences (satellite data)","310023","(Geostationary multi-channel satellite radiance data)",,"007004","Pressure","Pressure",,"Operational"
3034.00,"10","Vertical sounding sequences (satellite data)","310023","(Geostationary multi-channel satellite radiance data)",,"007004","Pressure","Pressure",,"Operational"
3035.00,"10","Vertical sounding sequences (satellite data)","310023","(Geostationary multi-channel satellite radiance data)",,"013003","Relative humidity","Relative humidity",,"Operational"
3036.00,"10","Vertical sounding sequences (satellite data)","310023","(Geostationary multi-channel satellite radiance data)",,"101012","Replication descriptor","Replicate next descriptor 12 times",,"Operational"
3037.00,"10","Vertical sounding sequences (satellite data)","310023","(Geostationary multi-channel satellite radiance data)",,"304033","Clear sky radiance","Radiance",,"Operational"
3038.00,"10","Vertical sounding sequences (satellite data)","310024","(Geostationary three-channel satellite radiance data)",,"301072","Satellite identification","Satellite identification",,"Operational"
3039.00,"10","Vertical sounding sequences (satellite data)","310024","(Geostationary three-channel satellite radiance data)",,"030021","Number of pixels per row","Number of pixels per row",,"Operational"
3040.00,"10","Vertical sounding sequences (satellite data)","310024","(Geostationary three-channel satellite radiance data)",,"030022","Number of pixels per column","Number of pixels per column",,"Operational"
3041.00,"10","Vertical sounding sequences (satellite data)","310024","(Geostationary three-channel satellite radiance data)",,"008012","Land/sea qualifier","Land/sea qualifier",,"Operational"
3042.00,"10","Vertical sounding sequences (satellite data)","310024","(Geostationary three-channel satellite radiance data)",,"007024","Satellite zenith angle","Satellite zenith angle",,"Operational"
3043.00,"10","Vertical sounding sequences (satellite data)","310024","(Geostationary three-channel satellite radiance data)",,"007025","Solar zenith angle","Solar zenith angle",,"Operational"
3044.00,"10","Vertical sounding sequences (satellite data)","310024","(Geostationary three-channel satellite radiance data)",,"010002","Height","Height",,"Operational"
3045.00,"10","Vertical sounding sequences (satellite data)","310024","(Geostationary three-channel satellite radiance data)",,"101003","Replication descriptor","Replicate next descriptor 3 times",,"Operational"
3046.00,"10","Vertical sounding sequences (satellite data)","310024","(Geostationary three-channel satellite radiance data)",,"304032","Cloud fraction","Cloud fraction",,"Operational"
3047.00,"10","Vertical sounding sequences (satellite data)","310024","(Geostationary three-channel satellite radiance data)",,"105002","Replication descriptor","Replicate next 5 descriptors 2 times",,"Operational"
3048.00,"10","Vertical sounding sequences (satellite data)","310024","(Geostationary three-channel satellite radiance data)",,"002152","Satellite instrument used in data processing","Satellite instrument used in data processing",,"Operational"
3049.00,"10","Vertical sounding sequences (satellite data)","310024","(Geostationary three-channel satellite radiance data)",,"002024","Integrated mean humidity computational method","Integrated mean humidity computational method",,"Operational"
3050.00,"10","Vertical sounding sequences (satellite data)","310024","(Geostationary three-channel satellite radiance data)",,"007004","Pressure","Pressure",,"Operational"
3051.00,"10","Vertical sounding sequences (satellite data)","310024","(Geostationary three-channel satellite radiance data)",,"007004","Pressure","Pressure",,"Operational"
3052.00,"10","Vertical sounding sequences (satellite data)","310024","(Geostationary three-channel satellite radiance data)",,"013003","Relative humidity","Relative humidity",,"Operational"
3053.00,"10","Vertical sounding sequences (satellite data)","310024","(Geostationary three-channel satellite radiance data)",,"101003","Replication descriptor","Replicate next descriptor 3 times",,"Operational"
3054.00,"10","Vertical sounding sequences (satellite data)","310024","(Geostationary three-channel satellite radiance data)",,"304033","Clear sky radiance","Radiance",,"Operational"
3055.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"001007","Satellite identifier","Satellite identification",,"Operational"
3056.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"008021","Time significance","Scan start",,"Operational"
3057.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"004001","Year","Year",,"Operational"
3058.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"004002","Month","Month",,"Operational"
3059.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"004003","Day","Day",,"Operational"
3060.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"004004","Hour","Hour",,"Operational"
3061.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"004005","Minute","Minute",,"Operational"
3062.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"201138","Change data width","Milliseconds",,"Operational"
3063.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"202131","Change scale",,,"Operational"
3064.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"004006","Second",,,"Operational"
3065.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"202000","Change scale",,,"Operational"
3066.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"201000","Change data width",,,"Operational"
3067.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"201132","Change data width",,,"Operational"
3068.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"005041","Scan line number","Scan number",,"Operational"
3069.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"201000","Change data width",,,"Operational"
3070.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"201129","Change data width",,,"Operational"
3071.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"005043","Field of view number","Scene number",,"Operational"
3072.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"201000","Change data width",,,"Operational"
3073.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"005002","Latitude (coarse accuracy)","Latitude",,"Operational"
3074.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"006002","Longitude (coarse accuracy)","Longitude",,"Operational"
3075.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"013040","Surface flag","Surface flag",,"Operational"
3076.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"020029","Rain flag","Rain flag",,"Operational"
3077.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"104024","Replication descriptor","Repeat next 4 descriptors 24 times",,"Operational"
3078.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"005042","Channel number","Channel number",,"Operational"
3079.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"012163","Brightness temperature","Temperature",,"Operational"
3080.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"021083","Warm target calibration","Warm target calibration",,"Operational"
3081.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"021084","Cold target calibration","Cold target calibration",,"Operational"
3082.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"115003","Replication descriptor","Replicate Ephemeris data (15 descriptors) 3 times",,"Operational"
3083.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"004001","Year","Year",,"Operational"
3084.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"004002","Month","Month",,"Operational"
3085.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"004003","Day","Day",,"Operational"
3086.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"201142","Change data width","Ephemeris milliseconds",,"Operational"
3087.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"202131","Change scale",,,"Operational"
3088.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"004026","Time period or displacement",,,"Operational"
3089.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"202000","Change scale",,,"Operational"
3090.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"201000","Change data width",,,"Operational"
3091.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"005001","Latitude (high accuracy)","Latitude - Ephemeris",,"Operational"
3092.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"006001","Longitude (high accuracy)","Longitude - Ephemeris",,"Operational"
3093.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"201138","Change data width",,,"Operational"
3094.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"202129","Change scale",,,"Operational"
3095.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"007001","Height of station","Ephemeris height",,"Operational"
3096.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"202000","Change scale",,,"Operational"
3097.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"201000","Change data width",,,"Operational"
3098.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"008021","Time significance","Orbit start",,"Operational"
3099.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"004001","Year","Year",,"Operational"
3100.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"004002","Month","Month",,"Operational"
3101.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"004003","Day","Day",,"Operational"
3102.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"004004","Hour","Hour",,"Operational"
3103.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"004005","Minute","Minute",,"Operational"
3104.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"005040","Orbit number","Orbit number",,"Operational"
3105.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"101003","Replication descriptor","Replicate 3 times",,"Operational"
3106.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"012070","Warm load temperature","Warm load temperature",,"Operational"
3107.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"025054","SSMIS subframe ID nember","SSMIS subframe identification number",,"Operational"
3108.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"101004","Replication descriptor","Replicate 4 times",,"Operational"
3109.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"025055","Multiplexer housekeeping","Multiplexer housekeeping values",,"Operational"
3110.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"008007","Dimensional significance","Dimensional significance (line)",,"Operational"
3111.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"104028","Replication descriptor","Replicate next 4 descriptors 28 times",,"Operational"
3112.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"005002","Latitude (coarse accuracy)","Latitude",,"Operational"
3113.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"006002","Longitude (coarse accuracy)","Longitude",,"Operational"
3114.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"002111","Radar incidence angle","Earth angle",,"Operational"
3115.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"005021","Bearing or azimuth","Azimuth",,"Operational"
3116.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"310022",,"Satellite, instrument and product",,"Operational"
3117.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"025060","Software identification","Software identification",,"Operational"
3118.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"008021","Time significance","Time significance (17 = Start of phenomenon)",,"Operational"
3119.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"301011",,"Year, month, day",,"Operational"
3120.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"301012",,"Hour, minute",,"Operational"
3121.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"201138","Change data width","Change width to 16 bits",,"Operational"
3122.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"202131","Change scale","Change scale to 3",,"Operational"
3123.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"004006","Second","Second",,"Operational"
3124.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"202000","Change scale","Change scale back to Table B",,"Operational"
3125.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"201000","Change data width","Change width back to Table B",,"Operational"
3126.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"033039","Quality flags for radio occultation data","Quality flags for radio occultation data",,"Operational"
3127.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"033007","Per cent confidence","Per cent confidence (for whole message)",,"Operational"
3128.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"304030","Location of platform","Location of platform",,"Operational"
3129.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"304031","Speed of platform","Speed of platform",,"Operational"
3130.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"002020","Satellite classification","Satellite classification",,"Operational"
3131.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"001050","Platform transmitter ID number","Platform transmitter identification number",,"Operational"
3132.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"202127","Change scale","Change scale to 1",,"Operational"
3133.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"304030","Location of platform","Location of platform",,"Operational"
3134.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"202000","Change scale","Change scale back to Table B",,"Operational"
3135.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"304031","Speed of platform","Speed of platform",,"Operational"
3136.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"201133","Change data width","Change width to 18 bits",,"Operational"
3137.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"202131","Change scale","Change scale to 3",,"Operational"
3138.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"004016","Time increment","Time increment",,"Operational"
3139.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"202000","Change scale","Change scale back to Table B",,"Operational"
3140.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"201000","Change data width","Change width back to Table B",,"Operational"
3141.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"301021",,"Latitude, longitude (high accuracy)",,"Operational"
3142.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"304030","Location of platform","Location of point",,"Operational"
3143.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"010035","Earth's local radius of curvature","Earth’s local radius of curvature",,"Operational"
3144.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"005021","Bearing or azimuth","Bearing or azimuth",,"Operational"
3145.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"010036","Geoid undulation","Geoid undulation",,"Operational"
3146.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"113000","Replication descriptor","Delayed replication of 13 descriptors",,"Operational"
3147.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"031002","Extended delayed descriptor replication factor","Replication factor (16 bits)",,"Operational"
3148.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"301021",,"Latitude, longitude (high accuracy)",,"Operational"
3149.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"005021","Bearing or azimuth","Bearing or azimuth",,"Operational"
3150.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"108000","Replication descriptor","Delayed replication of 8 descriptors",,"Operational"
3151.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"031001","Delayed descriptor replication factor","Replication factor",,"Operational"
3152.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"002121","Mean frequency","Mean frequency",,"Operational"
3153.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"007040","Impact parameter","Impact parameter",,"Operational"
3154.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"015037","Bending angle","Bending angle",,"Operational"
3155.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"008023","First-order statistics","First-order statistics (13 = Root-mean-square)",,"Operational"
3156.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"201125","Change data width","Change width to 20 bits",,"Operational"
3157.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"015037","Bending angle","Bending angle",,"Operational"
3158.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"201000","Change data width","Change width back to Table B",,"Operational"
3159.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"008023","First-order statistics","First-order statistics (63 = Missing)",,"Operational"
3160.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"033007","Per cent confidence","Per cent confidence (all data for current replication)",,"Operational"
3161.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"108000","Replication descriptor","Delayed replication of 8 descriptors",,"Operational"
3162.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"031002","Extended delayed descriptor replication factor","Replication factor (16 bits)",,"Operational"
3163.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"007007","Height","Height",,"Operational"
3164.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"015036","Atmospheric refractivity","Atmospheric refractivity",,"Operational"
3165.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"008023","First-order statistics","First-order statistics (13 = Root-mean-square)",,"Operational"
3166.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"201123","Change data width","Change width to 14 bits",,"Operational"
3167.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"015036","Atmospheric refractivity","Atmospheric refractivity",,"Operational"
3168.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"201000","Change data width","Change width back to Table B",,"Operational"
3169.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"008023","First-order statistics","First-order statistics (63 = Missing)",,"Operational"
3170.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"033007","Per cent confidence","Per cent confidence (all data for current height)",,"Operational"
3171.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"116000","Replication descriptor","Delayed replication of 16 descriptors",,"Operational"
3172.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"031002","Extended delayed descriptor replication factor","Replication factor (16 bits)",,"Operational"
3173.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"007009","Geopotential height","Geopotential height",,"Operational"
3174.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"010004","Pressure","Pressure",,"Operational"
3175.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"012001","Temperature/air temperature","Temperature",,"Operational"
3176.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"013001","Specific humidity","Specific humidity",,"Operational"
3177.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"008023","First-order statistics","First-order statistics (13 = Root-mean-square)",,"Operational"
3178.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"201120","Change data width","Change width to 6 bits",,"Operational"
3179.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"010004","Pressure","Pressure",,"Operational"
3180.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"201000","Change data width","Change width back to Table B",,"Operational"
3181.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"201122","Change data width","Change width to 6 bits",,"Operational"
3182.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"012001","Temperature/air temperature","Temperature",,"Operational"
3183.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"201000","Change data width","Change width back to Table B",,"Operational"
3184.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"201123","Change data width","Change width to 9 bits",,"Operational"
3185.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"013001","Specific humidity","Specific humidity",,"Operational"
3186.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"201000","Change data width","Change width back to Table B",,"Operational"
3187.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"008023","First-order statistics","First-order statistics (63 = Missing)",,"Operational"
3188.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"033007","Per cent confidence","Per cent confidence (all data for current height)",,"Operational"
3189.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"008003","Vertical significance (satellite observations)","Vertical significance (0 = surface)",,"Operational"
3190.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"007009","Geopotential height","Geopotential height",,"Operational"
3191.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"010004","Pressure","Pressure",,"Operational"
3192.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"008023","First-order statistics","First-order statistics (13 = Root-mean-square)",,"Operational"
3193.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"201120","Change data width","Change width to 6 bits",,"Operational"
3194.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"010004","Pressure","Pressure",,"Operational"
3195.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"201000","Change data width","Change width back to Table B",,"Operational"
3196.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"008023","First-order statistics","First-order statistics (63 = Missing)",,"Operational"
3197.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"033007","Per cent confidence","Per cent confidence (for surface data)",,"Operational"
3198.00,"10","Vertical sounding sequences (satellite data)","310027","(All sky radiance product main sequence)",,"301071","Satellite identifier/Generating resolution","Product information",,"Deprecated"
3199.00,"10","Vertical sounding sequences (satellite data)","310027","(All sky radiance product main sequence)",,"301011",,"Date",,"Deprecated"
3200.00,"10","Vertical sounding sequences (satellite data)","310027","(All sky radiance product main sequence)",,"301013",,"Time",,"Deprecated"
3201.00,"10","Vertical sounding sequences (satellite data)","310027","(All sky radiance product main sequence)",,"301021",,"Latitude / longitude",,"Deprecated"
3202.00,"10","Vertical sounding sequences (satellite data)","310027","(All sky radiance product main sequence)",,"030021","Number of pixels per row","Number of pixels per row",,"Deprecated"
3203.00,"10","Vertical sounding sequences (satellite data)","310027","(All sky radiance product main sequence)",,"030022","Number of pixels per column","Number of pixels per column",,"Deprecated"
3204.00,"10","Vertical sounding sequences (satellite data)","310027","(All sky radiance product main sequence)",,"010002","Height","Orbit height",,"Deprecated"
3205.00,"10","Vertical sounding sequences (satellite data)","310027","(All sky radiance product main sequence)",,"304036","Cloud coverage","All sky radiance cloud coverage",,"Deprecated"
3206.00,"10","Vertical sounding sequences (satellite data)","310027","(All sky radiance product main sequence)",,"002152","Satellite instrument used in data processing","Satellite instrument used",,"Deprecated"
3207.00,"10","Vertical sounding sequences (satellite data)","310027","(All sky radiance product main sequence)",,"002167","Radiance computational method","Radiance computational method",,"Deprecated"
3208.00,"10","Vertical sounding sequences (satellite data)","310027","(All sky radiance product main sequence)",,"101011","Replication descriptor","Replication operator",,"Deprecated"
3209.00,"10","Vertical sounding sequences (satellite data)","310027","(All sky radiance product main sequence)",,"304035","All sky radiance data","All sky radiance data",,"Deprecated"
3210.00,"10","Vertical sounding sequences (satellite data)","310028","(All sky radiance product main sequence)",,"301071","Satellite identifier/Generating resolution","Product information",,"Operational"
3211.00,"10","Vertical sounding sequences (satellite data)","310028","(All sky radiance product main sequence)",,"301011",,"Date",,"Operational"
3212.00,"10","Vertical sounding sequences (satellite data)","310028","(All sky radiance product main sequence)",,"301013",,"Time",,"Operational"
3213.00,"10","Vertical sounding sequences (satellite data)","310028","(All sky radiance product main sequence)",,"301021",,"Latitude / longitude",,"Operational"
3214.00,"10","Vertical sounding sequences (satellite data)","310028","(All sky radiance product main sequence)",,"030021","Number of pixels per row","Number of pixels per row",,"Operational"
3215.00,"10","Vertical sounding sequences (satellite data)","310028","(All sky radiance product main sequence)",,"030022","Number of pixels per column","Number of pixels per column",,"Operational"
3216.00,"10","Vertical sounding sequences (satellite data)","310028","(All sky radiance product main sequence)",,"010002","Height","Orbit height",,"Operational"
3217.00,"10","Vertical sounding sequences (satellite data)","310028","(All sky radiance product main sequence)",,"304036","Cloud coverage","All sky radiance cloud coverage",,"Operational"
3218.00,"10","Vertical sounding sequences (satellite data)","310028","(All sky radiance product main sequence)",,"002152","Satellite instrument used in data processing","Satellite instrument used",,"Operational"
3219.00,"10","Vertical sounding sequences (satellite data)","310028","(All sky radiance product main sequence)",,"002167","Radiance computational method","Radiance computational method",,"Operational"
3220.00,"10","Vertical sounding sequences (satellite data)","310028","(All sky radiance product main sequence)",,"101011","Replication descriptor","Replication operator",,"Operational"
3221.00,"10","Vertical sounding sequences (satellite data)","310028","(All sky radiance product main sequence)",,"304037","All sky radiance data","All sky radiance data",,"Operational"
3222.00,"10","Vertical sounding sequences (satellite data)","310029","(Layer, ozone, height, temperature and water vapour)",,"110000","Replication descriptor","Delayed replication",,"Operational"
3223.00,"10","Vertical sounding sequences (satellite data)","310029","(Layer, ozone, height, temperature and water vapour)",,"031001","Delayed descriptor replication factor",,,"Operational"
3224.00,"10","Vertical sounding sequences (satellite data)","310029","(Layer, ozone, height, temperature and water vapour)",,"201138","Change data width","Change data width",,"Operational"
3225.00,"10","Vertical sounding sequences (satellite data)","310029","(Layer, ozone, height, temperature and water vapour)",,"202130","Change scale","Change scale",,"Operational"
3226.00,"10","Vertical sounding sequences (satellite data)","310029","(Layer, ozone, height, temperature and water vapour)",,"007004","Pressure","Pressure",,"Operational"
3227.00,"10","Vertical sounding sequences (satellite data)","310029","(Layer, ozone, height, temperature and water vapour)",,"007004","Pressure","Pressure",,"Operational"
3228.00,"10","Vertical sounding sequences (satellite data)","310029","(Layer, ozone, height, temperature and water vapour)",,"202000","Change scale","Cancel operator",,"Operational"
3229.00,"10","Vertical sounding sequences (satellite data)","310029","(Layer, ozone, height, temperature and water vapour)",,"201000","Change data width","Cancel operator",,"Operational"
3230.00,"10","Vertical sounding sequences (satellite data)","310029","(Layer, ozone, height, temperature and water vapour)",,"015020","Integrated ozone density","Integrated ozone density",,"Operational"
3231.00,"10","Vertical sounding sequences (satellite data)","310029","(Layer, ozone, height, temperature and water vapour)",,"010002","Height","Height",,"Operational"
3232.00,"10","Vertical sounding sequences (satellite data)","310029","(Layer, ozone, height, temperature and water vapour)",,"012101","Temperature/air temperature","Temperature",,"Operational"
3233.00,"10","Vertical sounding sequences (satellite data)","310029","(Layer, ozone, height, temperature and water vapour)",,"013098","Integrated water vapour density","Integrated water vapour density",,"Operational"
3234.00,"10","Vertical sounding sequences (satellite data)","310030","(MIPAS or GOMOS instruments reporting)",,"310022",,"Satellite identification, product type",,"Operational"
3235.00,"10","Vertical sounding sequences (satellite data)","310030","(MIPAS or GOMOS instruments reporting)",,"301011",,"Date",,"Operational"
3236.00,"10","Vertical sounding sequences (satellite data)","310030","(MIPAS or GOMOS instruments reporting)",,"301013",,"Time",,"Operational"
3237.00,"10","Vertical sounding sequences (satellite data)","310030","(MIPAS or GOMOS instruments reporting)",,"301021",,"Latitude/longitude",,"Operational"
3238.00,"10","Vertical sounding sequences (satellite data)","310030","(MIPAS or GOMOS instruments reporting)",,"304034",,"Latitude/longitude, solar elevation, number of layers",,"Operational"
3239.00,"10","Vertical sounding sequences (satellite data)","310030","(MIPAS or GOMOS instruments reporting)",,"310029","Layer, ozone, height, temperature and water vapour","Layer, ozone, height, temperature and water vapour",,"Operational"
3240.00,"10","Vertical sounding sequences (satellite data)","310050","(Satellite collocated 1C reports with 3 instruments)",,"310051","Satellite position and instrument temperatures","Satellite position and instrument temperatures",,"Operational"
3241.00,"10","Vertical sounding sequences (satellite data)","310050","(Satellite collocated 1C reports with 3 instruments)",,"310052","Satellite instrument type and position","Satellite instrument type and position (AIRS)",,"Operational"
3242.00,"10","Vertical sounding sequences (satellite data)","310050","(Satellite collocated 1C reports with 3 instruments)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
3243.00,"10","Vertical sounding sequences (satellite data)","310050","(Satellite collocated 1C reports with 3 instruments)",,"031002","Extended delayed descriptor replication factor","Extended delayed descriptor replication factor",,"Operational"
3244.00,"10","Vertical sounding sequences (satellite data)","310050","(Satellite collocated 1C reports with 3 instruments)",,"310053","Satellite channels and brightness temperatures with expanded channel set","Satellite channels and brightness temperatures with expanded channel set (AIRS)",,"Operational"
3245.00,"10","Vertical sounding sequences (satellite data)","310050","(Satellite collocated 1C reports with 3 instruments)",,"101004","Replication descriptor","Replicate 1 descriptor 4 times",,"Operational"
3246.00,"10","Vertical sounding sequences (satellite data)","310050","(Satellite collocated 1C reports with 3 instruments)",,"310054","Satellite visible channels and albedos with expanded channel set","Satellite visible channels and albedos with expanded channel set",,"Operational"
3247.00,"10","Vertical sounding sequences (satellite data)","310050","(Satellite collocated 1C reports with 3 instruments)",,"020010","Cloud cover (total)","Cloud cover (total)",,"Operational"
3248.00,"10","Vertical sounding sequences (satellite data)","310050","(Satellite collocated 1C reports with 3 instruments)",,"310052","Satellite instrument type and position","Satellite instrument type and position (AMSU-A)",,"Operational"
3249.00,"10","Vertical sounding sequences (satellite data)","310050","(Satellite collocated 1C reports with 3 instruments)",,"101015","Replication descriptor","Replicate 1 descriptor 15 times",,"Operational"
3250.00,"10","Vertical sounding sequences (satellite data)","310050","(Satellite collocated 1C reports with 3 instruments)",,"310053","Satellite channels and brightness temperatures with expanded channel set","Satellite channels and brightness temperatures with expanded channel set (AMSU-A)",,"Operational"
3251.00,"10","Vertical sounding sequences (satellite data)","310050","(Satellite collocated 1C reports with 3 instruments)",,"310052","Satellite instrument type and position","Satellite instrument type and position (HSB)",,"Operational"
3252.00,"10","Vertical sounding sequences (satellite data)","310050","(Satellite collocated 1C reports with 3 instruments)",,"101005","Replication descriptor","Replicate 1 descriptor 5 times",,"Operational"
3253.00,"10","Vertical sounding sequences (satellite data)","310050","(Satellite collocated 1C reports with 3 instruments)",,"310053","Satellite channels and brightness temperatures with expanded channel set","Satellite channels and brightness temperatures with expanded channel set (HSB)",,"Operational"
3254.00,"10","Vertical sounding sequences (satellite data)","310051","(Satellite position and instrument temperatures)",,"001007","Satellite identifier","Satellite identifier",,"Operational"
3255.00,"10","Vertical sounding sequences (satellite data)","310051","(Satellite position and instrument temperatures)",,"005040","Orbit number","Orbit number",,"Operational"
3256.00,"10","Vertical sounding sequences (satellite data)","310051","(Satellite position and instrument temperatures)",,"201133","Change data width","Change data width",,"Operational"
3257.00,"10","Vertical sounding sequences (satellite data)","310051","(Satellite position and instrument temperatures)",,"005041","Scan line number","Scan line number",,"Operational"
3258.00,"10","Vertical sounding sequences (satellite data)","310051","(Satellite position and instrument temperatures)",,"201000","Change data width","Cancel change data width",,"Operational"
3259.00,"10","Vertical sounding sequences (satellite data)","310051","(Satellite position and instrument temperatures)",,"201132","Change data width","Change data width",,"Operational"
3260.00,"10","Vertical sounding sequences (satellite data)","310051","(Satellite position and instrument temperatures)",,"025070","Major frame count","Major frame count",,"Operational"
3261.00,"10","Vertical sounding sequences (satellite data)","310051","(Satellite position and instrument temperatures)",,"201000","Change data width","Cancel change data width",,"Operational"
3262.00,"10","Vertical sounding sequences (satellite data)","310051","(Satellite position and instrument temperatures)",,"202126","Change scale","Change scale",,"Operational"
3263.00,"10","Vertical sounding sequences (satellite data)","310051","(Satellite position and instrument temperatures)",,"007001","Height of station","Height of station",,"Operational"
3264.00,"10","Vertical sounding sequences (satellite data)","310051","(Satellite position and instrument temperatures)",,"202000","Change scale","Cancel change scale",,"Operational"
3265.00,"10","Vertical sounding sequences (satellite data)","310051","(Satellite position and instrument temperatures)",,"007025","Solar zenith angle","Solar zenith angle",,"Operational"
3266.00,"10","Vertical sounding sequences (satellite data)","310051","(Satellite position and instrument temperatures)",,"005022","Solar azimuth","Solar azimuth",,"Operational"
3267.00,"10","Vertical sounding sequences (satellite data)","310051","(Satellite position and instrument temperatures)",,"102009","Replication descriptor","Replicate 2 descriptors 9 times",,"Operational"
3268.00,"10","Vertical sounding sequences (satellite data)","310051","(Satellite position and instrument temperatures)",,"002151","Radiometer identifier","Radiometer identifier",,"Operational"
3269.00,"10","Vertical sounding sequences (satellite data)","310051","(Satellite position and instrument temperatures)",,"012064","Instrument temperature","Instrument temperature",,"Operational"
3270.00,"10","Vertical sounding sequences (satellite data)","310052","(Satellite instrument type and position)",,"002019","Satellite instruments","Satellite instruments",,"Operational"
3271.00,"10","Vertical sounding sequences (satellite data)","310052","(Satellite instrument type and position)",,"301011",,"Year, month, day",,"Operational"
3272.00,"10","Vertical sounding sequences (satellite data)","310052","(Satellite instrument type and position)",,"301012",,"Hour, minute",,"Operational"
3273.00,"10","Vertical sounding sequences (satellite data)","310052","(Satellite instrument type and position)",,"202131","Change scale","Change scale",,"Operational"
3274.00,"10","Vertical sounding sequences (satellite data)","310052","(Satellite instrument type and position)",,"201138","Change data width","Change data width",,"Operational"
3275.00,"10","Vertical sounding sequences (satellite data)","310052","(Satellite instrument type and position)",,"004006","Second","Second",,"Operational"
3276.00,"10","Vertical sounding sequences (satellite data)","310052","(Satellite instrument type and position)",,"201000","Change data width","Cancel change data width",,"Operational"
3277.00,"10","Vertical sounding sequences (satellite data)","310052","(Satellite instrument type and position)",,"202000","Change scale","Cancel change scale",,"Operational"
3278.00,"10","Vertical sounding sequences (satellite data)","310052","(Satellite instrument type and position)",,"301021",,"Latitude and longitude (high accuracy)",,"Operational"
3279.00,"10","Vertical sounding sequences (satellite data)","310052","(Satellite instrument type and position)",,"007024","Satellite zenith angle","Satellite zenith angle",,"Operational"
3280.00,"10","Vertical sounding sequences (satellite data)","310052","(Satellite instrument type and position)",,"005021","Bearing or azimuth","Bearing or azimuth",,"Operational"
3281.00,"10","Vertical sounding sequences (satellite data)","310052","(Satellite instrument type and position)",,"005043","Field of view number","Field of view number",,"Operational"
3282.00,"10","Vertical sounding sequences (satellite data)","310053","(Satellite channels and brightness temperatures with expanded channel set)",,"201134","Change data width","Change data width",,"Operational"
3283.00,"10","Vertical sounding sequences (satellite data)","310053","(Satellite channels and brightness temperatures with expanded channel set)",,"005042","Channel number","Channel number",,"Operational"
3284.00,"10","Vertical sounding sequences (satellite data)","310053","(Satellite channels and brightness temperatures with expanded channel set)",,"201000","Change data width","Cancel change data width",,"Operational"
3285.00,"10","Vertical sounding sequences (satellite data)","310053","(Satellite channels and brightness temperatures with expanded channel set)",,"025076","Log-10 of (Temperature-radiance central wavenumber) for ATOVS","Log-10 of temperature-radiance central wave number for ATOVS",,"Operational"
3286.00,"10","Vertical sounding sequences (satellite data)","310053","(Satellite channels and brightness temperatures with expanded channel set)",,"033032","Channel quality flags for ATOVS","Channel quality flags for ATOVS",,"Operational"
3287.00,"10","Vertical sounding sequences (satellite data)","310053","(Satellite channels and brightness temperatures with expanded channel set)",,"012163","Brightness temperature","Brightness temperature (scale 2)",,"Operational"
3288.00,"10","Vertical sounding sequences (satellite data)","310054","(Satellite visible channels and albedos with expanded channel set)",,"201134","Change data width","Change data width",,"Operational"
3289.00,"10","Vertical sounding sequences (satellite data)","310054","(Satellite visible channels and albedos with expanded channel set)",,"005042","Channel number","Channel number",,"Operational"
3290.00,"10","Vertical sounding sequences (satellite data)","310054","(Satellite visible channels and albedos with expanded channel set)",,"201000","Change data width","Cancel change data width",,"Operational"
3291.00,"10","Vertical sounding sequences (satellite data)","310054","(Satellite visible channels and albedos with expanded channel set)",,"025076","Log-10 of (Temperature-radiance central wavenumber) for ATOVS","Log-10 of temperature-radiance central wave number for ATOVS",,"Operational"
3292.00,"10","Vertical sounding sequences (satellite data)","310054","(Satellite visible channels and albedos with expanded channel set)",,"033032","Channel quality flags for ATOVS","Channel quality flags for ATOVS",,"Operational"
3293.00,"10","Vertical sounding sequences (satellite data)","310054","(Satellite visible channels and albedos with expanded channel set)",,"201131","Change data width","Change data width",,"Operational"
3294.00,"10","Vertical sounding sequences (satellite data)","310054","(Satellite visible channels and albedos with expanded channel set)",,"202129","Change scale","Change scale",,"Operational"
3295.00,"10","Vertical sounding sequences (satellite data)","310054","(Satellite visible channels and albedos with expanded channel set)",,"102002","Replication descriptor","Replicate 2 descriptors 2 times",,"Operational"
3296.00,"10","Vertical sounding sequences (satellite data)","310054","(Satellite visible channels and albedos with expanded channel set)",,"008023","First-order statistics","First-order statistics",,"Operational"
3297.00,"10","Vertical sounding sequences (satellite data)","310054","(Satellite visible channels and albedos with expanded channel set)",,"014027","Albedo","Albedo",,"Operational"
3298.00,"10","Vertical sounding sequences (satellite data)","310054","(Satellite visible channels and albedos with expanded channel set)",,"008023","First-order statistics","First-order statistics",,"Operational"
3299.00,"10","Vertical sounding sequences (satellite data)","310054","(Satellite visible channels and albedos with expanded channel set)",,"202000","Change scale","Cancel change scale",,"Operational"
3300.00,"10","Vertical sounding sequences (satellite data)","310054","(Satellite visible channels and albedos with expanded channel set)",,"201000","Change data width","Cancel change data width",,"Operational"
3301.00,"10","Vertical sounding sequences (satellite data)","310055","(Satellite radiance/channel principle components)",,"310051","Satellite position and instrument temperatures","Satellite position and instrument temperatures",,"Operational"
3302.00,"10","Vertical sounding sequences (satellite data)","310055","(Satellite radiance/channel principle components)",,"310052","Satellite instrument type and position","Satellite instrument type and position (AIRS)",,"Operational"
3303.00,"10","Vertical sounding sequences (satellite data)","310055","(Satellite radiance/channel principle components)",,"102020","Replication descriptor","Replicate 2 descriptors 20 times",,"Operational"
3304.00,"10","Vertical sounding sequences (satellite data)","310055","(Satellite radiance/channel principle components)",,"025076","Log-10 of (Temperature-radiance central wavenumber) for ATOVS","Log-10 of temperature-radiance central wave number for ATOVS",,"Operational"
3305.00,"10","Vertical sounding sequences (satellite data)","310055","(Satellite radiance/channel principle components)",,"025052","Log-10 of principal components normalized fit to data","Log-10 of principal components normalized fit to data",,"Operational"
3306.00,"10","Vertical sounding sequences (satellite data)","310055","(Satellite radiance/channel principle components)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
3307.00,"10","Vertical sounding sequences (satellite data)","310055","(Satellite radiance/channel principle components)",,"031002","Extended delayed descriptor replication factor","Extended delayed descriptor replication factor",,"Operational"
3308.00,"10","Vertical sounding sequences (satellite data)","310055","(Satellite radiance/channel principle components)",,"025050","Principal component score","Principal components of satellite radiance",,"Operational"
3309.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"001007","Satellite identifier","Satellite identifier",,"Operational"
3310.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"001033","Identification of originating/generating centre","Identification of originating/generating centre",,"Operational"
3311.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"002019","Satellite instruments","Satellite instruments",,"Operational"
3312.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"002020","Satellite classification","Satellite classification",,"Operational"
3313.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"301011",,"Year, month, day",,"Operational"
3314.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"301012",,"Hour, minute",,"Operational"
3315.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"207003","Increase scale, reference value and data width","Increase scale and bit width",,"Operational"
3316.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"004006","Second","Second",,"Operational"
3317.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"207000","Increase scale, reference value and data width","Cancel increase scale and bit width",,"Operational"
3318.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"304030","Location of platform","Location of satellite platform",,"Operational"
3319.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"301021",,"Latitude, longitude (high accuracy)",,"Operational"
3320.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"007024","Satellite zenith angle","Satellite zenith angle",,"Operational"
3321.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"005021","Bearing or azimuth","Bearing or azimuth",,"Operational"
3322.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"007025","Solar zenith angle","Solar zenith angle",,"Operational"
3323.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"005022","Solar azimuth","Solar azimuth",,"Operational"
3324.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"008075","Ascending/descending orbit qualifier","Ascending/descending orbit qualifier",,"Operational"
3325.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"201133","Change data width","Increase bit width",,"Operational"
3326.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"005041","Scan line number","Scan line number",,"Operational"
3327.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"201000","Change data width","Cancel increase bit width",,"Operational"
3328.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"005045","Field of regard number","Field of regard number",,"Operational"
3329.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"005043","Field of view number","Field of view number",,"Operational"
3330.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"005040","Orbit number","Orbit number",,"Operational"
3331.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"010001","Height of land surface","Height of land surface",,"Operational"
3332.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"201129","Change data width","Increase bit width",,"Operational"
3333.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"007002","Height or altitude","Height or altitude",,"Operational"
3334.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"201000","Change data width","Cancel increase bit width",,"Operational"
3335.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"202127","Change scale","Increase scale",,"Operational"
3336.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"201125","Change data width","Increase bit width",,"Operational"
3337.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"021166","Land fraction","Land fraction",,"Operational"
3338.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"201000","Change data width","Cancel increase bit width",,"Operational"
3339.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"202000","Change scale","Cancel increase scale",,"Operational"
3340.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"008012","Land/sea qualifier","Land/sea qualifier",,"Operational"
3341.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"020010","Cloud cover (total)","Cloud cover (total)",,"Operational"
3342.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"020014","Height of top of cloud","Height of top of cloud",,"Operational"
3343.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"002165","Radiance type flags","Radiance type flags",,"Operational"
3344.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"033075","Scan-level quality flags","Scan-level quality flags",,"Operational"
3345.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"107003","Replication descriptor","Replicate 7 descriptors 3 times",,"Operational"
3346.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"008076","Type of band","Type of band",,"Operational"
3347.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"006029","Wave number","Wave number (start of range)",,"Operational"
3348.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"006029","Wave number","Wave number (end of range)",,"Operational"
3349.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"025140","Start channel","Start channel",,"Operational"
3350.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"025141","End channel","End channel",,"Operational"
3351.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"033076","Calibration quality flags","Calibration quality flags",,"Operational"
3352.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"033077","Field-of-view quality flags","Field of view quality flags",,"Operational"
3353.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"008076","Type of band","Type of band (Missing = Cancel)",,"Operational"
3354.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"033078","Geolocation quality","Geolocation quality",,"Operational"
3355.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"033003","Quality information","Quality information",,"Operational"
3356.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"104000","Replication descriptor","Delayed replication of 4 descriptors",,"Operational"
3357.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"031002","Extended delayed descriptor replication factor","Extended delayed descriptor replication factor",,"Operational"
3358.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"201133","Change data width","Increase bit width",,"Operational"
3359.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"005042","Channel number","Channel number",,"Operational"
3360.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"201000","Change data width","Cancel increase bit width",,"Operational"
3361.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"014044","Channel radiance","Channel radiance",,"Operational"
3362.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"001007","Satellite identifier","Satellite identifier",,"Operational"
3363.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"001033","Identification of originating/generating centre","Identification of originating/generating centre",,"Operational"
3364.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"001034","Identification of originating/generating sub-centre","Identification of originating/generating sub-centre",,"Operational"
3365.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"002019","Satellite instruments","Satellite instruments",,"Operational"
3366.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"002020","Satellite classification","Satellite classification",,"Operational"
3367.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"301011",,"Year, month, day",,"Operational"
3368.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"301012",,"Hour, minute",,"Operational"
3369.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"207003","Increase scale, reference value and data width","Increase scale and bit width",,"Operational"
3370.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"004006","Second","Second",,"Operational"
3371.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"207000","Increase scale, reference value and data width","Cancel increase scale and bit width",,"Operational"
3372.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"005040","Orbit number","Orbit number",,"Operational"
3373.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"005041","Scan line number","Scan line number",,"Operational"
3374.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"005043","Field of view number","Field of view number",,"Operational"
3375.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"033079","Granule level quality flags","Granule level quality flags",,"Operational"
3376.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"033080","Scan level quality flags","Scan level quality flags",,"Operational"
3377.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"033078","Geolocation quality","Geolocation quality",,"Operational"
3378.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"301021",,"Latitude, longitude (high accuracy)",,"Operational"
3379.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"201129","Change data width","Increase bit width",,"Operational"
3380.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"007002","Height or altitude","Height or altitude",,"Operational"
3381.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"201000","Change data width","Cancel increase bit width",,"Operational"
3382.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"007024","Satellite zenith angle","Satellite zenith angle",,"Operational"
3383.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"005021","Bearing or azimuth","Bearing or azimuth",,"Operational"
3384.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"007025","Solar zenith angle","Solar zenith angle",,"Operational"
3385.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"005022","Solar azimuth","Solar azimuth",,"Operational"
3386.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"025075","Satellite antenna corrections version number","Satellite antenna corrections version number",,"Operational"
3387.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"111000","Replication descriptor","Delayed replication of 11 descriptors",,"Operational"
3388.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"031002","Extended delayed descriptor replication factor","Extended delayed descriptor replication factor",,"Operational"
3389.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"005042","Channel number","Channel number",,"Operational"
3390.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"202131","Change scale","Increase scale by 3",,"Operational"
3391.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"002153","Satellite channel centre frequency","Satellite channel centre frequency",,"Operational"
3392.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"002154","Satellite channel band width","Satellite channel band width",,"Operational"
3393.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"202000","Change scale","Cancel increase scale",,"Operational"
3394.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"002104","Antenna polarization","Antenna polarization",,"Operational"
3395.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"012066","Antenna temperature","Antenna temperature",,"Operational"
3396.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"012163","Brightness temperature","Brightness temperature",,"Operational"
3397.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"012158","Noise-equivalent delta temperature while viewing cold target","Noise-equivalent delta temperature while viewing cold target",,"Operational"
3398.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"012159","Noise-equivalent delta temperature while viewing warm target","Noise-equivalent delta temperature while viewing warm target",,"Operational"
3399.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"033081","Channel data quality flags","Channel data quality flags",,"Operational"
3400.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"001007","Satellite identifier","Satellite identifier",,"Operational"
3401.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"001033","Identification of originating/generating centre","Identification of originating/generating centre",,"Operational"
3402.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"001034","Identification of originating/generating sub-centre","Identification of originating/generating sub-centre",,"Operational"
3403.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"002019","Satellite instruments","Satellite instruments",,"Operational"
3404.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"002020","Satellite classification","Satellite classification",,"Operational"
3405.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"301011",,"Year, month, day",,"Operational"
3406.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"301012",,"Hour, minute",,"Operational"
3407.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"207003","Increase scale, reference value and data width","Increase scale and bit width",,"Operational"
3408.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"004006","Second","Second",,"Operational"
3409.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"207000","Increase scale, reference value and data width","Cancel increase scale and bit width",,"Operational"
3410.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"005040","Orbit number","Orbit number",,"Operational"
3411.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"201133","Change data witdth","Increase bit width",,"Operational"
3412.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"005041","Scan line number","Scan line number",,"Operational"
3413.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"005043","Field of view number","Field of view number",,"Operational"
3414.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"201000","Change data witdth","Cancel increase bit width",,"Operational"
3415.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"008076","Type of band","Type of band",,"Operational"
3416.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"033082","Geolocation quality flags","Geolocation quality flags                          ",,"Operational"
3417.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"301021",,"Latitude, longitude (high accuracy)",,"Operational"
3418.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"201129","Change data witdth","Increase bit width",,"Operational"
3419.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"007002","Height or altitude","Height or altitude",,"Operational"
3420.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"201000","Change data witdth","Cancel increase bit width",,"Operational"
3421.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"007024","Satellite zenith angle","Satellite zenith angle",,"Operational"
3422.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"005021","Bearing or azimuth","Bearing or azimuth",,"Operational"
3423.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"007025","Solar zenith angle","Solar zenith angle",,"Operational"
3424.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"005022","Solar azimuth (degree true)","Solar azimuth",,"Operational"
3425.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"008072","Pixel(s) type","Pixel(s) type",,"Operational"
3426.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"008029","Surface type","Surface type",,"Operational"
3427.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"105000","Replication descriptor","Delayed replication of 5 descriptors",,"Operational"
3428.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"031002","Extended delayed descriptor replication factor","Extended delayed descriptor replication factor",,"Operational"
3429.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"005042","Channel number","Channel number",,"Operational"
3430.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"002155","Satellite channel wavelength","Satellite channel wavelength",,"Operational"
3431.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"033083","Radiance data quality flags","Radiance data quality flags",,"Operational"
3432.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"014043","Channel radiance","Channel radiance",,"Operational"
3433.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"015042","Reflectance","Reflectance",,"Operational"
3551.00,"11","Single level report sequences (conventional data)","311001","(Aircraft reports)",,"301051",,"ASDAR aircraft flight number, navigational system, date/time, position, phase of aircraft flight",,"Operational"
3552.00,"11","Single level report sequences (conventional data)","311001","(Aircraft reports)",,"007002","Height or altitude","Altitude",,"Operational"
3553.00,"11","Single level report sequences (conventional data)","311001","(Aircraft reports)",,"012001","Temperature/air temperature","Temperature",,"Operational"
3554.00,"11","Single level report sequences (conventional data)","311001","(Aircraft reports)",,"011001","Wind direction","Wind direction",,"Operational"
3555.00,"11","Single level report sequences (conventional data)","311001","(Aircraft reports)",,"011002","Wind speed","Wind speed",,"Operational"
3556.00,"11","Single level report sequences (conventional data)","311001","(Aircraft reports)",,"011031","Degree of turbulence","Degree of turbulence",,"Operational"
3557.00,"11","Single level report sequences (conventional data)","311001","(Aircraft reports)",,"011032","Height of base of turbulence","Height of base of turbulence",,"Operational"
3558.00,"11","Single level report sequences (conventional data)","311001","(Aircraft reports)",,"011033","Height of top of turbulence","Height of top of turbulence",,"Operational"
3559.00,"11","Single level report sequences (conventional data)","311001","(Aircraft reports)",,"020041","Airframe icing","Airframe icing",,"Operational"
3560.00,"11","Single level report sequences (conventional data)","311002","(ACARS reports)",,"301065","ACARS identification","ACARS identification",,"Operational"
3561.00,"11","Single level report sequences (conventional data)","311002","(ACARS reports)",,"301066","ACARS location","ACARS location",,"Operational"
3562.00,"11","Single level report sequences (conventional data)","311002","(ACARS reports)",,"311003","ACARS standard reported variables","ACARS standard reported variables",,"Operational"
3563.00,"11","Single level report sequences (conventional data)","311002","(ACARS reports)",,"311004","ACARS supplementary reported variables","ACARS supplementary reported variables",,"Operational"
3564.00,"11","Single level report sequences (conventional data)","311003","(ACARS standard reported variables)",,"010070","Indicated aircraft altitude","Indicated aircraft altitude",,"Operational"
3565.00,"11","Single level report sequences (conventional data)","311003","(ACARS standard reported variables)",,"011001","Wind direction","Wind direction",,"Operational"
3566.00,"11","Single level report sequences (conventional data)","311003","(ACARS standard reported variables)",,"011002","Wind speed","Wind speed",,"Operational"
3567.00,"11","Single level report sequences (conventional data)","311003","(ACARS standard reported variables)",,"012001","Temperature/air temperature","Temperature/air temperature",,"Operational"
3568.00,"11","Single level report sequences (conventional data)","311003","(ACARS standard reported variables)",,"013002","Mixing ratio","Mixing ratio",,"Operational"
3569.00,"11","Single level report sequences (conventional data)","311004","(ACARS supplementary reported variables)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
3570.00,"11","Single level report sequences (conventional data)","311004","(ACARS supplementary reported variables)",,"031000","Short delayed descriptor replication factor","Short delayed descriptor replication factor",,"Operational"
3571.00,"11","Single level report sequences (conventional data)","311004","(ACARS supplementary reported variables)",,"011034","Vertical gust velocity","Vertical gust velocity",,"Operational"
3572.00,"11","Single level report sequences (conventional data)","311004","(ACARS supplementary reported variables)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
3573.00,"11","Single level report sequences (conventional data)","311004","(ACARS supplementary reported variables)",,"031000","Short delayed descriptor replication factor","Short delayed descriptor replication factor",,"Operational"
3574.00,"11","Single level report sequences (conventional data)","311004","(ACARS supplementary reported variables)",,"011035","Vertical gust acceleration","Vertical gust acceleration",,"Operational"
3575.00,"11","Single level report sequences (conventional data)","311004","(ACARS supplementary reported variables)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
3576.00,"11","Single level report sequences (conventional data)","311004","(ACARS supplementary reported variables)",,"031000","Short delayed descriptor replication factor","Short delayed descriptor replication factor",,"Operational"
3577.00,"11","Single level report sequences (conventional data)","311004","(ACARS supplementary reported variables)",,"011075","Mean turbulence intensity (eddy dissipation rate)","Mean turbulence intensity (eddy dissipation rate)",,"Operational"
3578.00,"11","Single level report sequences (conventional data)","311004","(ACARS supplementary reported variables)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
3579.00,"11","Single level report sequences (conventional data)","311004","(ACARS supplementary reported variables)",,"031000","Short delayed descriptor replication factor","Short delayed descriptor replication factor",,"Operational"
3580.00,"11","Single level report sequences (conventional data)","311004","(ACARS supplementary reported variables)",,"011076","Peak turbulence intensity (eddy dissipation rate)","Peak turbulence intensity (eddy dissipation rate)",,"Operational"
3581.00,"11","Single level report sequences (conventional data)","311004","(ACARS supplementary reported variables)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
3582.00,"11","Single level report sequences (conventional data)","311004","(ACARS supplementary reported variables)",,"031000","Short delayed descriptor replication factor","Short delayed descriptor replication factor",,"Operational"
3583.00,"11","Single level report sequences (conventional data)","311004","(ACARS supplementary reported variables)",,"033025","ACARS interpolated values indicator","ACARS interpolated values indicator",,"Operational"
3584.00,"11","Single level report sequences (conventional data)","311004","(ACARS supplementary reported variables)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
3585.00,"11","Single level report sequences (conventional data)","311004","(ACARS supplementary reported variables)",,"031000","Short delayed descriptor replication factor","Short delayed descriptor replication factor",,"Operational"
3586.00,"11","Single level report sequences (conventional data)","311004","(ACARS supplementary reported variables)",,"033026","Moisture quality","Moisture quality",,"Operational"
3587.00,"11","Single level report sequences (conventional data)","311005","(Standard AMDAR reports)",,"001008","Aircraft registration number or other identification","Aircraft identification",,"Operational"
3588.00,"11","Single level report sequences (conventional data)","311005","(Standard AMDAR reports)",,"001023","Observation sequence number","Sequence number",,"Operational"
3589.00,"11","Single level report sequences (conventional data)","311005","(Standard AMDAR reports)",,"301021",,"Latitude and longitude",,"Operational"
3590.00,"11","Single level report sequences (conventional data)","311005","(Standard AMDAR reports)",,"301011",,"Year, month, day",,"Operational"
3591.00,"11","Single level report sequences (conventional data)","311005","(Standard AMDAR reports)",,"301013",,"Hour, minute, second",,"Operational"
3592.00,"11","Single level report sequences (conventional data)","311005","(Standard AMDAR reports)",,"007010","Flight level","Flight level",,"Operational"
3593.00,"11","Single level report sequences (conventional data)","311005","(Standard AMDAR reports)",,"008009","Detailed phase of flight","Detailed phase of flight",,"Operational"
3594.00,"11","Single level report sequences (conventional data)","311005","(Standard AMDAR reports)",,"011001","Wind direction","Wind direction",,"Operational"
3595.00,"11","Single level report sequences (conventional data)","311005","(Standard AMDAR reports)",,"011002","Wind speed","Wind speed",,"Operational"
3596.00,"11","Single level report sequences (conventional data)","311005","(Standard AMDAR reports)",,"011031","Degree of turbulence","Degree of turbulence",,"Operational"
3597.00,"11","Single level report sequences (conventional data)","311005","(Standard AMDAR reports)",,"011036","Maximum derived equivalent vertical gust speed","Derived equivalent vertical gust speed",,"Operational"
3598.00,"11","Single level report sequences (conventional data)","311005","(Standard AMDAR reports)",,"012101","Temperature/air temperature","Temperature/air temperature",,"Operational"
3599.00,"11","Single level report sequences (conventional data)","311005","(Standard AMDAR reports)",,"033025","ACARS interpolated values indicator","ACARS interpolated values indicator",,"Operational"
3600.00,"11","Single level report sequences (conventional data)","311006","(AMDAR data or aircraft data for one level without latitude/longitude)",,"007010","Flight level","Flight level",,"Operational"
3601.00,"11","Single level report sequences (conventional data)","311006","(AMDAR data or aircraft data for one level without latitude/longitude)",,"011001","Wind direction","Wind direction",,"Operational"
3602.00,"11","Single level report sequences (conventional data)","311006","(AMDAR data or aircraft data for one level without latitude/longitude)",,"011002","Wind speed","Wind speed",,"Operational"
3603.00,"11","Single level report sequences (conventional data)","311006","(AMDAR data or aircraft data for one level without latitude/longitude)",,"002064","Aircraft roll angle quality","Aircraft roll angle quality",,"Operational"
3604.00,"11","Single level report sequences (conventional data)","311006","(AMDAR data or aircraft data for one level without latitude/longitude)",,"012101","Temperature/air temperature","Temperature/air temperature",,"Operational"
3605.00,"11","Single level report sequences (conventional data)","311006","(AMDAR data or aircraft data for one level without latitude/longitude)",,"012103","Dew-point temperature","Dew-point temperature",,"Operational"
3606.00,"11","Single level report sequences (conventional data)","311007","(Aircraft data for one level with latitude/longitude indicated)",,"007010","Flight level","Flight level",,"Operational"
3607.00,"11","Single level report sequences (conventional data)","311007","(Aircraft data for one level with latitude/longitude indicated)",,"301021",,"Latitude, longitude",,"Operational"
3608.00,"11","Single level report sequences (conventional data)","311007","(Aircraft data for one level with latitude/longitude indicated)",,"011001","Wind direction","Wind direction",,"Operational"
3609.00,"11","Single level report sequences (conventional data)","311007","(Aircraft data for one level with latitude/longitude indicated)",,"011002","Wind speed","Wind speed",,"Operational"
3610.00,"11","Single level report sequences (conventional data)","311007","(Aircraft data for one level with latitude/longitude indicated)",,"002064","Aircraft roll angle quality","Aircraft roll angle quality",,"Operational"
3611.00,"11","Single level report sequences (conventional data)","311007","(Aircraft data for one level with latitude/longitude indicated)",,"012101","Temperature/air temperature","Temperature/air temperature",,"Operational"
3612.00,"11","Single level report sequences (conventional data)","311007","(Aircraft data for one level with latitude/longitude indicated)",,"012103","Dew-point temperature","Dew-point temperature",,"Operational"
3613.00,"11","Single level report sequences (conventional data)","311008","(Aircraft ascent/descent profile without latitude/longitude indicated at each level)",,"001008","Aircraft registration number or other identification","Aircraft identification",,"Operational"
3614.00,"11","Single level report sequences (conventional data)","311008","(Aircraft ascent/descent profile without latitude/longitude indicated at each level)",,"301011",,"Year, month, day",,"Operational"
3615.00,"11","Single level report sequences (conventional data)","311008","(Aircraft ascent/descent profile without latitude/longitude indicated at each level)",,"301013",,"Hour, minute, second",,"Operational"
3616.00,"11","Single level report sequences (conventional data)","311008","(Aircraft ascent/descent profile without latitude/longitude indicated at each level)",,"301021",,"Latitude, longitude",,"Operational"
3617.00,"11","Single level report sequences (conventional data)","311008","(Aircraft ascent/descent profile without latitude/longitude indicated at each level)",,"008004","Phase of aircraft flight","Phase of flight",,"Operational"
3618.00,"11","Single level report sequences (conventional data)","311008","(Aircraft ascent/descent profile without latitude/longitude indicated at each level)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
3619.00,"11","Single level report sequences (conventional data)","311008","(Aircraft ascent/descent profile without latitude/longitude indicated at each level)",,"031001","Delayed descriptor replication factor","Delayed descriptor replication factor",,"Operational"
3620.00,"11","Single level report sequences (conventional data)","311008","(Aircraft ascent/descent profile without latitude/longitude indicated at each level)",,"311006","AMDAR data or aircraft data for one level without latitude/longitude","Aircraft data for one level without latitude/longitude",,"Operational"
3621.00,"11","Single level report sequences (conventional data)","311009","(Aircraft ascent/descent profile with latitude/longitude given for each level)",,"001008","Aircraft registration number or other identification","Aircraft identification",,"Operational"
3622.00,"11","Single level report sequences (conventional data)","311009","(Aircraft ascent/descent profile with latitude/longitude given for each level)",,"301011",,"Year, month, day",,"Operational"
3623.00,"11","Single level report sequences (conventional data)","311009","(Aircraft ascent/descent profile with latitude/longitude given for each level)",,"301013",,"Hour, minute, second",,"Operational"
3624.00,"11","Single level report sequences (conventional data)","311009","(Aircraft ascent/descent profile with latitude/longitude given for each level)",,"301021",,"Latitude, longitude",,"Operational"
3625.00,"11","Single level report sequences (conventional data)","311009","(Aircraft ascent/descent profile with latitude/longitude given for each level)",,"008004","Phase of aircraft flight","Phase of flight",,"Operational"
3626.00,"11","Single level report sequences (conventional data)","311009","(Aircraft ascent/descent profile with latitude/longitude given for each level)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
3627.00,"11","Single level report sequences (conventional data)","311009","(Aircraft ascent/descent profile with latitude/longitude given for each level)",,"031001","Delayed descriptor replication factor","Delayed descriptor replication factor",,"Operational"
3628.00,"11","Single level report sequences (conventional data)","311009","(Aircraft ascent/descent profile with latitude/longitude given for each level)",,"311007","Aircraft data for one level with latitude/longitude indicated","Aircraft data for one level with latitude/longitude indicated",,"Operational"
3629.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"001008","Aircraft registration number or other identification","Aircraft identification",,"Operational"
3630.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"001023","Observation sequence number","Sequence number",,"Operational"
3631.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"001006","Aircraft flight number","Flight number",,"Operational"
3632.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"001110","Aircraft tail number","Aircraft tail number",,"Operational"
3633.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"001111","Origination airport","Origination airport",,"Operational"
3634.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"001112","Destination airport","Destination airport",,"Operational"
3635.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"204002","Add associated field","Add associated field (of 2 bits)",,"Operational"
3636.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"031021","Associated field significance","Associated field significance (= 8 Two bits quality information)",,"Operational"
3637.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"301011",,"Year, month and day",,"Operational"
3638.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"301013",,"Hour, minute and second",,"Operational"
3639.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"301021",,"Latitude and longitude (high accuracy)",,"Operational"
3640.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"007010","Pressure","Pressure altitude (flight level)",,"Operational"
3641.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"010053","Global Navigation Satellite System altitude","GNSS altitude",,"Operational"
3642.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"008009","Detailed phase of flight","Detailed phase of flight",,"Operational"
3643.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"011001","Wind direction","Wind direction",,"Operational"
3644.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"011002","Wind speed","Wind speed",,"Operational"
3645.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"002064","Aircraft roll angle quality","Aircraft roll angle quality",,"Operational"
3646.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"011100","Aircraft true airspeed","Aircraft true airspeed",,"Operational"
3647.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"011101","Aircraft ground speed u-component","Aircraft ground speed (u-component)",,"Operational"
3648.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"011102","Aircraft ground speed v-component","Aircraft ground speed (v-component)",,"Operational"
3649.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"011103","Aircraft ground speed w-component","Aircraft ground speed (w-component)",,"Operational"
3650.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"011104","Aircraft true heading","Aircraft true heading",,"Operational"
3651.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"012101","Temperature/air temperature","Temperature/air temperature",,"Operational"
3652.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"002170","Aircraft humidity sensors","Aircraft humidity sensors",,"Operational"
3653.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"201144","Change data width","Change data width",,"Operational"
3654.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"202133","Change scale","Change scale",,"Operational"
3655.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"013002","Mixing ratio","Mixing ratio",,"Operational"
3656.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"202000","Change scale","Cancel change scale",,"Operational"
3657.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"201000","Change data width","Cancel change data width",,"Operational"
3658.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"201135","Change data width","Change data width",,"Operational"
3659.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"202130","Change scale","Change scale",,"Operational"
3660.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"013003","Relative humidity","Relative humidity",,"Operational"
3661.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"202000","Change scale","Cancel change scale",,"Operational"
3662.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"201000","Change data width","Cancel change data width",,"Operational"
3663.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
3664.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"031000","Short delayed descriptor replication factor","Short delayed descriptor replication factor",,"Operational"
3665.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"012103","Dew-point temperature","Dew-point temperature",,"Operational"
3666.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"033026","Moisture quality","Moisture quality",,"Operational"
3667.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
3668.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"031000","Short delayed descriptor replication factor","Short delayed descriptor replication factor",,"Operational"
3669.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"020042","Airframe icing present","Airframe icing",,"Operational"
3670.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"103000","Replication descriptor","Delayed replication of 3 descriptors",,"Operational"
3671.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"031000","Short delayed descriptor replication factor","Short delayed descriptor replication factor",,"Operational"
3672.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"020043","Peak liquid water content","Peak liquid water content",,"Operational"
3673.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"020044","Average liquid water content","Average liquid water content",,"Operational"
3674.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"020045","Supercooled large droplet (SLD) conditions","Supercooled large droplet (SLD) conditions",,"Operational"
3675.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
3676.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"031000","Short delayed descriptor replication factor","Short delayed descriptor replication factor",,"Operational"
3677.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"033025","ACARS interpolated values indicator","ACARS interpolated values indicator",,"Operational"
3678.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"103000","Replication descriptor","Delayed replication of 3 descriptors",,"Operational"
3679.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"031001","Delayed descriptor replication factor","Delayed descriptor replication factor",,"Operational"
3680.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"011075","Mean turbulence intensity (eddy dissipation rate)","Mean turbulence intensity (EDR)",,"Operational"
3681.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"011076","Peak turbulence intensity (eddy dissipation rate)","Peak turbulence intensity (EDR)",,"Operational"
3682.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"011039","Extended time of occurrence of peak eddy dissipation rate","Extended time of occurrence of peak EDR",,"Operational"
3683.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"102000","Replication descriptor","Delayed replication of 2 descriptors",,"Operational"
3684.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"031000","Short delayed descriptor replication factor","Short delayed descriptor replication factor",,"Operational"
3685.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"011037","Turbulence index","Turbulence index (EDR)",,"Operational"
3686.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"011077","Reporting interval or averaging time for eddy dissipation rate","Reporting interval or averaging time for EDR",,"Operational"
3687.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"103000","Replication descriptor","Delayed replication of 3 descriptors",,"Operational"
3688.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"031000","Short delayed descriptor replication factor","Short delayed descriptor replication factor",,"Operational"
3689.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"011034","Vertical gust velocity","Vertical gust velocity",,"Operational"
3690.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"011035","Vertical gust acceleration","Vertical gust acceleration",,"Operational"
3691.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"011036","Maximum derived equivalent vertical gust speed","Maximum derived equivalent vertical gust speed",,"Operational"
3692.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"204000","Add associated field","Cancel add associated field",,"Operational"
3693.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"119000","Replication descriptor","Delayed replication of 19 descriptors",,"Operational"
3694.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"031001","Delayed descriptor replication factor","Delayed descriptor replication factor",,"Operational"
3695.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"301011",,"Year, month and day",,"Operational"
3696.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"301013",,"Hour, minute and second",,"Operational"
3697.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"301021",,"Latitude and longitude (high accuracy)",,"Operational"
3698.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"007007","Height","Height",,"Operational"
3699.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"011105","EDR algorithm version","EDR algorithm version",,"Operational"
3700.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"204007","Add associated field","Add associated field (of 7 bits)",,"Operational"
3701.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"031021","Associated field significance","Associated field significance (= 7 Percentage confidence)",,"Operational"
3702.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"011076","Peak turbulence intensity (eddy dissipation rate)","Peak turbulence intensity (EDR)",,"Operational"
3703.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"011075","Mean turbulence intensity (eddy dissipation rate)","Mean turbulence intensity (EDR)",,"Operational"
3704.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"204000","Add associated field","Cancel add associated field",,"Operational"
3705.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"011106","Running minimum confidence","Running minimum confidence",,"Operational"
3706.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"011107","Maximum number bad inputs","Maximum number bad inputs",,"Operational"
3707.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"011108","Peak location","Peak location",,"Operational"
3708.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"011109","Number of good EDR","Number of good EDR",,"Operational"
3709.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"012101","Temperature/air temperature","Temperature/air temperature",,"Operational"
3710.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"011001","Wind direction","Wind direction",,"Operational"
3711.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"201130","Change data width","Change data width",,"Operational"
3712.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"011084","Wind speed","Wind speed",,"Operational"
3713.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, 3 11 010, version 7)",,"201000","Change data width","Cancel change data width",,"Operational"
3714.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"001023","Observation sequence number","Observation sequence number ",,"Operational"
3715.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"008004","Phase of aircraft flight","Phase of aircraft flight",,"Operational"
3716.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"301011",,"Year/month/day",,"Operational"
3717.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"301013",,"Hour/minute/second",,"Operational"
3718.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"005002","Latitude (coarse accuracy)","Latitude (coarse accuracy)",,"Operational"
3719.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"006002","Longitude (coarse accuracy)","Longitude (coarse accuracy)",,"Operational"
3720.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"007004","Pressure","Pressure",,"Operational"
3721.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"011001","Wind direction","Wind direction",,"Operational"
3722.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"011002","Wind speed","Wind speed",,"Operational"
3723.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"012101","Temperature/air temperature","Temperature/air temperature",,"Operational"
3724.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"106000","Replication descriptor","Delayed replication of 6 descriptors",,"Operational"
3725.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"031001","Delayed descriptor replication factor","Delayed descriptor replication factor",,"Operational"
3726.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"008046","Atmospheric chemical or physical constituent type","Atmospheric chemical or physical constituent type",,"Operational"
3727.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"201139","Change data width","Increase data width from 9 to 20",,"Operational"
3728.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"202126","Change scale","Decrease scale from 9 to 7",,"Operational"
3729.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"015026","Concentration of pollutant (mol mol-1)","Concentration of pollutant",,"Operational"
3730.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"202000","Change scale","Cancel change scale",,"Operational"
3731.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"201000","Change data width","Cancel change data width",,"Operational"
3732.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"106000","Replication descriptor","Delayed replication of 6 descriptors",,"Operational"
3733.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"031001","Delayed descriptor replication factor","Delayed descriptor replication factor",,"Operational"
3734.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"008046","Atmospheric chemical or physical constituent type","Atmospheric chemical or physical constituent type",,"Operational"
3735.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"201138","Change data width","Increase data width from 9 to 19",,"Operational"
3736.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"202130","Change scale","Increase scale from 9 to 11",,"Operational"
3737.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"015026","Concentration of pollutant (mol mol-1)","Concentration of pollutant",,"Operational"
3738.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"202000","Change scale","Cancel change scale",,"Operational"
3739.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"201000","Change data width","Cancel change data width",,"Operational"
3740.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"015052","Log_10 of Number density of aerosol particles with diameter greater than 5 nm","Log_10 of Number density of aerosol particles with diameter greater than 5 nm",,"Operational"
3741.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"015053","Log_10 of Number density of aerosol particles with diameter greater than 14 nm","Log_10 of Number density of aerosol particles with diameter greater than 14 nm",,"Operational"
3742.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"015054","Log_10 of Number density of aerosol particles with diameter between 0.25 and 2.5 µm","Log_10 of Number density of aerosol particles with diameter between 0.25 and 2.5 µm",,"Operational"
3743.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"015055","Non volatile aerosol ratio","Non volatile aerosol ratio",,"Operational"
3744.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"007004","Pressure","Pressure",,"Operational"
3745.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"007004","Pressure","Pressure",,"Operational"
3746.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"013099","Log_10 of integrated Cloud particle density","Log_10 of integrated Cloud particle density",,"Operational"
3747.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"013100","Log_10 of integrated cloud particle area","Log_10 of integrated cloud particle area",,"Operational"
3748.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"013101","Log_10 of integrated cloud particle volume","Log_10 of integrated cloud particle volume",,"Operational"
3749.00,"12","Single level report sequences (satellite data)","312001",,,"301043",,"Satellite identifier, instrumentation, location, date/time",,"Operational"
3750.00,"12","Single level report sequences (satellite data)","312001",,,"304001",,"Cloud top pressure, temperature, wind",,"Operational"
3751.00,"12","Single level report sequences (satellite data)","312002",,,"301043",,"Satellite identifier, instrumentation, location, date/time",,"Operational"
3752.00,"12","Single level report sequences (satellite data)","312002",,,"304002",,"Cloud top pressure, wind",,"Operational"
3753.00,"12","Single level report sequences (satellite data)","312003",,,"301042",,"Satellite identifier, instrumentation, location, date/time",,"Operational"
3754.00,"12","Single level report sequences (satellite data)","312003",,,"304003",,"Surface temperature",,"Operational"
3755.00,"12","Single level report sequences (satellite data)","312004",,,"301042",,"Satellite identifier, instrumentation, location, date/time",,"Operational"
3756.00,"12","Single level report sequences (satellite data)","312004",,,"304004",,"Cloud cover",,"Operational"
3757.00,"12","Single level report sequences (satellite data)","312005",,,"301042",,"Satellite identifier, instrumentation, location, date/time",,"Operational"
3758.00,"12","Single level report sequences (satellite data)","312005",,,"020014","Height of top of cloud","Height of top of cloud",,"Operational"
3759.00,"12","Single level report sequences (satellite data)","312006",,,"301044",,"Satellite identifier, instrumentation, location, date/time",,"Operational"
3760.00,"12","Single level report sequences (satellite data)","312006",,,"304005",,"Layer mean relative humidity",,"Operational"
3761.00,"12","Single level report sequences (satellite data)","312007",,,"301042",,"Satellite identifier, instrumentation, location, date/time",,"Operational"
3762.00,"12","Single level report sequences (satellite data)","312007",,,"304006",,"Radiation",,"Operational"
3763.00,"12","Single level report sequences (satellite data)","312010","(Orbital information, Part I)",,"001007","Satellite identifier","Satellite identifier",,"Operational"
3764.00,"12","Single level report sequences (satellite data)","312010","(Orbital information, Part I)",,"005040","Orbit number","Orbit number",,"Operational"
3765.00,"12","Single level report sequences (satellite data)","312010","(Orbital information, Part I)",,"002021","Satellite instrument data used in processing","Satellite instrumentation",,"Operational"
3766.00,"12","Single level report sequences (satellite data)","312010","(Orbital information, Part I)",,"005041","Scan line number","Scan line number",,"Operational"
3767.00,"12","Single level report sequences (satellite data)","312010","(Orbital information, Part I)",,"004001","Year","Year",,"Operational"
3768.00,"12","Single level report sequences (satellite data)","312010","(Orbital information, Part I)",,"004043","Day of the year","Day of year",,"Operational"
3769.00,"12","Single level report sequences (satellite data)","312011","(Orbital information, Part II)",,"202131","Change scale","Change scale",,"Operational"
3770.00,"12","Single level report sequences (satellite data)","312011","(Orbital information, Part II)",,"201149","Change data width","Change width",,"Operational"
3771.00,"12","Single level report sequences (satellite data)","312011","(Orbital information, Part II)",,"004006","Second","Second",,"Operational"
3772.00,"12","Single level report sequences (satellite data)","312011","(Orbital information, Part II)",,"201000","Change data width","Change width",,"Operational"
3773.00,"12","Single level report sequences (satellite data)","312011","(Orbital information, Part II)",,"202126","Change scale","Change scale",,"Operational"
3774.00,"12","Single level report sequences (satellite data)","312011","(Orbital information, Part II)",,"010002","Height","Height",,"Operational"
3775.00,"12","Single level report sequences (satellite data)","312011","(Orbital information, Part II)",,"202000","Change scale","Change scale",,"Operational"
3776.00,"12","Single level report sequences (satellite data)","312011","(Orbital information, Part II)",,"005043","Field of view number","Field of view number",,"Operational"
3777.00,"12","Single level report sequences (satellite data)","312011","(Orbital information, Part II)",,"005053","Field of view number increment","Field of view number increment",,"Operational"
3778.00,"12","Single level report sequences (satellite data)","312012","(HIRS brightness temperatures - channels 1-19)",,"202129","Change scale","Change scale",,"Operational"
3779.00,"12","Single level report sequences (satellite data)","312012","(HIRS brightness temperatures - channels 1-19)",,"201132","Change data width","Change width",,"Operational"
3780.00,"12","Single level report sequences (satellite data)","312012","(HIRS brightness temperatures - channels 1-19)",,"101019","Replication descriptor","Replicate 1 descriptor 19 times",,"Operational"
3781.00,"12","Single level report sequences (satellite data)","312012","(HIRS brightness temperatures - channels 1-19)",,"012063","Brightness temperature","Brightness temperature",,"Operational"
3782.00,"12","Single level report sequences (satellite data)","312012","(HIRS brightness temperatures - channels 1-19)",,"201000","Change data width","Change width",,"Operational"
3783.00,"12","Single level report sequences (satellite data)","312012","(HIRS brightness temperatures - channels 1-19)",,"202000","Change scale","Change scale",,"Operational"
3784.00,"12","Single level report sequences (satellite data)","312013","(HIRS brightness temperatures - channel 20)",,"005042","Channel number","Channel number",,"Operational"
3785.00,"12","Single level report sequences (satellite data)","312013","(HIRS brightness temperatures - channel 20)",,"202129","Change scale","Change scale",,"Operational"
3786.00,"12","Single level report sequences (satellite data)","312013","(HIRS brightness temperatures - channel 20)",,"201135","Change data width","Change width",,"Operational"
3787.00,"12","Single level report sequences (satellite data)","312013","(HIRS brightness temperatures - channel 20)",,"012063","Brightness temperature","Brightness temperature",,"Operational"
3788.00,"12","Single level report sequences (satellite data)","312013","(HIRS brightness temperatures - channel 20)",,"201000","Change data width","Change width",,"Operational"
3789.00,"12","Single level report sequences (satellite data)","312013","(HIRS brightness temperatures - channel 20)",,"202000","Change scale","Change scale",,"Operational"
3790.00,"12","Single level report sequences (satellite data)","312014","(HIRS satellite data)",,"312010","Orbital information, Part I","Orbital information, Part I",,"Operational"
3791.00,"12","Single level report sequences (satellite data)","312014","(HIRS satellite data)",,"312011","Orbital information, Part II","Orbital information, Part II",,"Operational"
3792.00,"12","Single level report sequences (satellite data)","312014","(HIRS satellite data)",,"105056","Replication descriptor","Replicate 5 descriptors 56 times",,"Operational"
3793.00,"12","Single level report sequences (satellite data)","312014","(HIRS satellite data)",,"301023",,"Latitude and longitude (coarse accuracy)",,"Operational"
3794.00,"12","Single level report sequences (satellite data)","312014","(HIRS satellite data)",,"005042","Channel number","Channel number",,"Operational"
3795.00,"12","Single level report sequences (satellite data)","312014","(HIRS satellite data)",,"005052","Channel number increment","Channel number increment",,"Operational"
3796.00,"12","Single level report sequences (satellite data)","312014","(HIRS satellite data)",,"312012","HIRS brightness temperatures - channels 1-19","HIRS brightness temperatures - channels 1-19",,"Operational"
3797.00,"12","Single level report sequences (satellite data)","312014","(HIRS satellite data)",,"312013","HIRS brightness temperatures - channels 20","HIRS brightness temperature - channel 20",,"Operational"
3798.00,"12","Single level report sequences (satellite data)","312015","(MSU brightness temperatures - channels 1-4)",,"109011","Replication descriptor","Replicate 9 descriptors 11 times",,"Operational"
3799.00,"12","Single level report sequences (satellite data)","312015","(MSU brightness temperatures - channels 1-4)",,"301023",,"Latitude and longitude (coarse accuracy)",,"Operational"
3800.00,"12","Single level report sequences (satellite data)","312015","(MSU brightness temperatures - channels 1-4)",,"005042","Channel number","Channel number",,"Operational"
3801.00,"12","Single level report sequences (satellite data)","312015","(MSU brightness temperatures - channels 1-4)",,"005052","Channel number increment","Channel number increment",,"Operational"
3802.00,"12","Single level report sequences (satellite data)","312015","(MSU brightness temperatures - channels 1-4)",,"202129","Change scale","Change scale",,"Operational"
3803.00,"12","Single level report sequences (satellite data)","312015","(MSU brightness temperatures - channels 1-4)",,"201132","Change data width","Change width",,"Operational"
3804.00,"12","Single level report sequences (satellite data)","312015","(MSU brightness temperatures - channels 1-4)",,"101004","Replication descriptor","Replicate 1 descriptor 4 times",,"Operational"
3805.00,"12","Single level report sequences (satellite data)","312015","(MSU brightness temperatures - channels 1-4)",,"012063","Brightness temperature","Brightness temperature",,"Operational"
3806.00,"12","Single level report sequences (satellite data)","312015","(MSU brightness temperatures - channels 1-4)",,"202000","Change scale","Change scale",,"Operational"
3807.00,"12","Single level report sequences (satellite data)","312015","(MSU brightness temperatures - channels 1-4)",,"201000","Change data width","Change width",,"Operational"
3808.00,"12","Single level report sequences (satellite data)","312016","(MSU satellite data)",,"312010","Orbital information, Part I","Orbital information, Part I",,"Operational"
3809.00,"12","Single level report sequences (satellite data)","312016","(MSU satellite data)",,"312011","Orbital information, Part II","Orbital information, Part II",,"Operational"
3810.00,"12","Single level report sequences (satellite data)","312016","(MSU satellite data)",,"312015","MSU brightness temperatures - channels 1-4","MSU brightness temperatures - channels 1-4",,"Operational"
3811.00,"12","Single level report sequences (satellite data)","312017","(SSU brightness temperatures - channels 1-3)",,"109008","Replication descriptor","Replicate 9 descriptors 8 times",,"Operational"
3812.00,"12","Single level report sequences (satellite data)","312017","(SSU brightness temperatures - channels 1-3)",,"301023",,"Latitude and longitude (coarse accuracy)",,"Operational"
3813.00,"12","Single level report sequences (satellite data)","312017","(SSU brightness temperatures - channels 1-3)",,"005042","Channel number","Channel number",,"Operational"
3814.00,"12","Single level report sequences (satellite data)","312017","(SSU brightness temperatures - channels 1-3)",,"005052","Channel number increment","Channel number increment",,"Operational"
3815.00,"12","Single level report sequences (satellite data)","312017","(SSU brightness temperatures - channels 1-3)",,"202129","Change scale","Change scale",,"Operational"
3816.00,"12","Single level report sequences (satellite data)","312017","(SSU brightness temperatures - channels 1-3)",,"201132","Change data width","Change width",,"Operational"
3817.00,"12","Single level report sequences (satellite data)","312017","(SSU brightness temperatures - channels 1-3)",,"101003","Replication descriptor","Replicate 1 descriptor 3 times",,"Operational"
3818.00,"12","Single level report sequences (satellite data)","312017","(SSU brightness temperatures - channels 1-3)",,"012063","Brightness temperature","Brightness temperature",,"Operational"
3819.00,"12","Single level report sequences (satellite data)","312017","(SSU brightness temperatures - channels 1-3)",,"202000","Change scale","Change scale",,"Operational"
3820.00,"12","Single level report sequences (satellite data)","312017","(SSU brightness temperatures - channels 1-3)",,"201000","Change data width","Change width",,"Operational"
3821.00,"12","Single level report sequences (satellite data)","312018","(SSU satellite data)",,"312010","Orbital information, Part I","Orbital information, Part I",,"Operational"
3822.00,"12","Single level report sequences (satellite data)","312018","(SSU satellite data)",,"312011","Orbital information, Part II","Orbital information, Part II",,"Operational"
3823.00,"12","Single level report sequences (satellite data)","312018","(SSU satellite data)",,"312017","SSU brightness temperatures - channels 1-3","SSU brightness temperatures - channels 1-3",,"Operational"
3824.00,"12","Single level report sequences (satellite data)","312019","(Wave scatterometer product with width change for wave number (spectral))",,"301047","ERS product header","Product header",,"Operational"
3825.00,"12","Single level report sequences (satellite data)","312019","(Wave scatterometer product with width change for wave number (spectral))",,"301048","Radar parameters","Radar parameters",,"Operational"
3826.00,"12","Single level report sequences (satellite data)","312019","(Wave scatterometer product with width change for wave number (spectral))",,"015015","Maximum image spectral component before normalization","Maximum spectrum composition before normalisation",,"Operational"
3827.00,"12","Single level report sequences (satellite data)","312019","(Wave scatterometer product with width change for wave number (spectral))",,"029002","Co-ordinate grid type","Coordinate grid type",,"Operational"
3828.00,"12","Single level report sequences (satellite data)","312019","(Wave scatterometer product with width change for wave number (spectral))",,"021076","Representation of intensities","Representation of intensities",,"Operational"
3829.00,"12","Single level report sequences (satellite data)","312019","(Wave scatterometer product with width change for wave number (spectral))",,"106012","Replication descriptor","Repeat next 6 descriptors 12 times",,"Operational"
3830.00,"12","Single level report sequences (satellite data)","312019","(Wave scatterometer product with width change for wave number (spectral))",,"201129","Change data width","Change width to 14 bits",,"Operational"
3831.00,"12","Single level report sequences (satellite data)","312019","(Wave scatterometer product with width change for wave number (spectral))",,"006030","Wave number (spectral)","Wave number (spectral)",,"Operational"
3832.00,"12","Single level report sequences (satellite data)","312019","(Wave scatterometer product with width change for wave number (spectral))",,"201000","Change data width","Change width back to Table B",,"Operational"
3833.00,"12","Single level report sequences (satellite data)","312019","(Wave scatterometer product with width change for wave number (spectral))",,"102012","Replication descriptor","Repeat next 2 descriptors 12 times",,"Operational"
3834.00,"12","Single level report sequences (satellite data)","312019","(Wave scatterometer product with width change for wave number (spectral))",,"005030","Direction (spectral)","Direction (spectral)",,"Operational"
3835.00,"12","Single level report sequences (satellite data)","312019","(Wave scatterometer product with width change for wave number (spectral))",,"021075","Image spectrum intensity","Image spectrum intensity",,"Operational"
3836.00,"12","Single level report sequences (satellite data)","312019","(Wave scatterometer product with width change for wave number (spectral))",,"021066","Wave scatterometer product confidence data","Wave scatterometer product confidence data",,"Operational"
3837.00,"12","Single level report sequences (satellite data)","312020","(Wave scatterometer product)",,"301047","ERS product header","Product header",,"Operational"
3838.00,"12","Single level report sequences (satellite data)","312020","(Wave scatterometer product)",,"301048","Radar parameters","Radar parameters",,"Operational"
3839.00,"12","Single level report sequences (satellite data)","312020","(Wave scatterometer product)",,"015015","Maximum image spectral component before normalization","Maximum spectrum composition before normalization",,"Operational"
3840.00,"12","Single level report sequences (satellite data)","312020","(Wave scatterometer product)",,"029002","Co-ordinate grid type","Coordinate grid type",,"Operational"
3841.00,"12","Single level report sequences (satellite data)","312020","(Wave scatterometer product)",,"021076","Representation of intensities","Representation of intensities",,"Operational"
3842.00,"12","Single level report sequences (satellite data)","312020","(Wave scatterometer product)",,"104012","Replication descriptor","Repeat next 4 descriptors 12 times",,"Operational"
3843.00,"12","Single level report sequences (satellite data)","312020","(Wave scatterometer product)",,"006030","Wave number (spectral)","Wave number (spectral)",,"Operational"
3844.00,"12","Single level report sequences (satellite data)","312020","(Wave scatterometer product)",,"102012","Replication descriptor","Repeat next 2 descriptors 12 times",,"Operational"
3845.00,"12","Single level report sequences (satellite data)","312020","(Wave scatterometer product)",,"005030","Direction (spectral)","Direction (spectral)",,"Operational"
3846.00,"12","Single level report sequences (satellite data)","312020","(Wave scatterometer product)",,"021075","Image spectrum intensity","Spectral intensity",,"Operational"
3847.00,"12","Single level report sequences (satellite data)","312020","(Wave scatterometer product)",,"021066","Wave scatterometer product confidence data","Wave scatterometer product confidence data",,"Operational"
3848.00,"12","Single level report sequences (satellite data)","312021","(Wind scatterometer product)",,"301047","ERS product header","Product header",,"Operational"
3849.00,"12","Single level report sequences (satellite data)","312021","(Wind scatterometer product)",,"101003","Replication descriptor","Repeat 1 descriptor 3 times",,"Operational"
3850.00,"12","Single level report sequences (satellite data)","312021","(Wind scatterometer product)",,"301049","Radar beam data","Radar beam data",,"Operational"
3851.00,"12","Single level report sequences (satellite data)","312021","(Wind scatterometer product)",,"011012","Wind speed at 10 m","Wind speed at 10 m",,"Operational"
3852.00,"12","Single level report sequences (satellite data)","312021","(Wind scatterometer product)",,"011011","Wind direction at 10 m","Wind direction at 10 m",,"Operational"
3853.00,"12","Single level report sequences (satellite data)","312021","(Wind scatterometer product)",,"021067","Wind product confidence data","Wind product confidence data",,"Operational"
3854.00,"12","Single level report sequences (satellite data)","312022","(Radar altimeter product)",,"301047","ERS product header","Product header",,"Operational"
3855.00,"12","Single level report sequences (satellite data)","312022","(Radar altimeter product)",,"008022","Total number (with respect to accumulation or average)","Number in average",,"Operational"
3856.00,"12","Single level report sequences (satellite data)","312022","(Radar altimeter product)",,"011012","Wind speed at 10 m","Wind speed",,"Operational"
3857.00,"12","Single level report sequences (satellite data)","312022","(Radar altimeter product)",,"011050","Standard deviation of horizontal wind speed","Standard deviation of horizontal wind speed",,"Operational"
3858.00,"12","Single level report sequences (satellite data)","312022","(Radar altimeter product)",,"022070","Significant wave height","Significant wave height",,"Operational"
3859.00,"12","Single level report sequences (satellite data)","312022","(Radar altimeter product)",,"022026","Standard deviation of significant wave height","Standard deviation of significant wave height",,"Operational"
3860.00,"12","Single level report sequences (satellite data)","312022","(Radar altimeter product)",,"312041","Altitude","Altitude",,"Operational"
3861.00,"12","Single level report sequences (satellite data)","312022","(Radar altimeter product)",,"010050","Standard deviation altitude","Standard deviation of altitude",,"Operational"
3862.00,"12","Single level report sequences (satellite data)","312022","(Radar altimeter product)",,"021068","Radar altimeter product confidence data","Radar altimeter product confidence data",,"Operational"
3863.00,"12","Single level report sequences (satellite data)","312022","(Radar altimeter product)",,"021071","Peakiness","Peakiness",,"Operational"
3864.00,"12","Single level report sequences (satellite data)","312022","(Radar altimeter product)",,"021072","Satellite altimeter calibration status","Altimeter calibration status",,"Operational"
3865.00,"12","Single level report sequences (satellite data)","312022","(Radar altimeter product)",,"021073","Satelllite altimeter instrument mode","Altimeter instrument mode",,"Operational"
3866.00,"12","Single level report sequences (satellite data)","312022","(Radar altimeter product)",,"312042","Altitude corrections","Altitude corrections",,"Operational"
3867.00,"12","Single level report sequences (satellite data)","312022","(Radar altimeter product)",,"021062","Backscatter","Backscatter",,"Operational"
3868.00,"12","Single level report sequences (satellite data)","312022","(Radar altimeter product)",,"015011","Log 10 of integrated electron density","Log 10 of integrated electron density",,"Operational"
3869.00,"12","Single level report sequences (satellite data)","312023","(ATSR sea surface temperature product)",,"301047","ERS product header","Product header",,"Operational"
3870.00,"12","Single level report sequences (satellite data)","312023","(ATSR sea surface temperature product)",,"103003","Replication descriptor","Repeat 3 descriptors 3 times",,"Operational"
3871.00,"12","Single level report sequences (satellite data)","312023","(ATSR sea surface temperature product)",,"008022","Total number (with respect to accumulation or average)","Number in average",,"Operational"
3872.00,"12","Single level report sequences (satellite data)","312023","(ATSR sea surface temperature product)",,"012061","Skin temperature","Skin temperature",,"Operational"
3873.00,"12","Single level report sequences (satellite data)","312023","(ATSR sea surface temperature product)",,"022050","Standard deviation sea-surface temperature","Standard deviation of sea surface temperature",,"Operational"
3874.00,"12","Single level report sequences (satellite data)","312023","(ATSR sea surface temperature product)",,"021069","SST product confidence data","SST product confidence data",,"Operational"
3875.00,"12","Single level report sequences (satellite data)","312023","(ATSR sea surface temperature product)",,"021085","ATSR sea surface temperature across-track band number","ATSR sea surface temperature across-track band number",,"Operational"
3876.00,"12","Single level report sequences (satellite data)","312024","(Wave scatterometer product enhanced)",,"312020","Wave scatterometer product","Wave scatterometer product",,"Operational"
3877.00,"12","Single level report sequences (satellite data)","312024","(Wave scatterometer product enhanced)",,"008060","Sample scanning mode significance","Sample scanning mode significance - range",,"Operational"
3878.00,"12","Single level report sequences (satellite data)","312024","(Wave scatterometer product enhanced)",,"008022","Total number (with respect to accumulation or average)","Number in sample",,"Operational"
3879.00,"12","Single level report sequences (satellite data)","312024","(Wave scatterometer product enhanced)",,"008060","Sample scanning mode significance","Sample scanning mode signification - horizontal",,"Operational"
3880.00,"12","Single level report sequences (satellite data)","312024","(Wave scatterometer product enhanced)",,"008022","Total number (with respect to accumulation or average)","Number in sample",,"Operational"
3881.00,"12","Single level report sequences (satellite data)","312024","(Wave scatterometer product enhanced)",,"025014","Azimuth clutter cut-off","Azimuth clutter cut-off",,"Operational"
3882.00,"12","Single level report sequences (satellite data)","312024","(Wave scatterometer product enhanced)",,"022101","Total energy (wavelength > 731m) at low wave numbers","Total energy (wavelength > 731 m)",,"Operational"
3883.00,"12","Single level report sequences (satellite data)","312024","(Wave scatterometer product enhanced)",,"022097","Mean wavelength > 731 m of image spectrum at low wave numbers","Mean wavelength of image spectrum",,"Operational"
3884.00,"12","Single level report sequences (satellite data)","312024","(Wave scatterometer product enhanced)",,"022098","Wavelength spread (wavelength > 731 m) at low wave numbers","Wavelength spread (wavelength > 731 m)",,"Operational"
3885.00,"12","Single level report sequences (satellite data)","312024","(Wave scatterometer product enhanced)",,"022099","Mean direction at low wave numbers (wavelength > 731 m)","Mean direction (wavelength > 731 m)",,"Operational"
3886.00,"12","Single level report sequences (satellite data)","312024","(Wave scatterometer product enhanced)",,"022100","Direction spread at low wave numbers (wavelength > 731 m)","Direction spread (wavelength > 731 m)",,"Operational"
3887.00,"12","Single level report sequences (satellite data)","312025","(Wave scatterometer enhanced product (with change of width for wave number (spectral))",,"312019","Wave scatterometer product with width change for wave number (spectral)","Wave scatterometer product with width change for wave number (spectral)",,"Operational"
3888.00,"12","Single level report sequences (satellite data)","312025","(Wave scatterometer enhanced product (with change of width for wave number (spectral))",,"008060","Sample scanning mode significance","Sample scanning mode significance - range",,"Operational"
3889.00,"12","Single level report sequences (satellite data)","312025","(Wave scatterometer enhanced product (with change of width for wave number (spectral))",,"008022","Total number (with respect to accumulation or average)","Number in sample",,"Operational"
3890.00,"12","Single level report sequences (satellite data)","312025","(Wave scatterometer enhanced product (with change of width for wave number (spectral))",,"008060","Sample scanning mode significance","Sample scanning mode significance - horizontal",,"Operational"
3891.00,"12","Single level report sequences (satellite data)","312025","(Wave scatterometer enhanced product (with change of width for wave number (spectral))",,"008022","Total number (with respect to accumulation or average)","Number in sample",,"Operational"
3892.00,"12","Single level report sequences (satellite data)","312025","(Wave scatterometer enhanced product (with change of width for wave number (spectral))",,"025014","Azimuth clutter cut-off","Azimuth clutter cut-off",,"Operational"
3893.00,"12","Single level report sequences (satellite data)","312025","(Wave scatterometer enhanced product (with change of width for wave number (spectral))",,"022101","Total energy (wavelength > 731m) at low wave numbers","Total energy (wavelength > 731 m)",,"Operational"
3894.00,"12","Single level report sequences (satellite data)","312025","(Wave scatterometer enhanced product (with change of width for wave number (spectral))",,"022097","Mean wavelength > 731 m of image spectrum at low wave numbers","Mean wavelength of image spectrum",,"Operational"
3895.00,"12","Single level report sequences (satellite data)","312025","(Wave scatterometer enhanced product (with change of width for wave number (spectral))",,"022098","Wavelength spread (wavelength > 731 m) at low wave numbers","Wavelength spread (wavelength > 731 m)",,"Operational"
3896.00,"12","Single level report sequences (satellite data)","312025","(Wave scatterometer enhanced product (with change of width for wave number (spectral))",,"022099","Mean direction at low wave numbers (wavelength > 731 m)","Mean direction (wavelength > 731 m)",,"Operational"
3897.00,"12","Single level report sequences (satellite data)","312025","(Wave scatterometer enhanced product (with change of width for wave number (spectral))",,"022100","Direction spread at low wave numbers (wavelength > 731 m)","Direction spread (wavelength > 731 m)",,"Operational"
3898.00,"12","Single level report sequences (satellite data)","312026","(QUIKSCAT data)",,"301046",,,,"Operational"
3899.00,"12","Single level report sequences (satellite data)","312026","(QUIKSCAT data)",,"301011",,"Date",,"Operational"
3900.00,"12","Single level report sequences (satellite data)","312026","(QUIKSCAT data)",,"301013",,"Time",,"Operational"
3901.00,"12","Single level report sequences (satellite data)","312026","(QUIKSCAT data)",,"301023",,"Location",,"Operational"
3902.00,"12","Single level report sequences (satellite data)","312026","(QUIKSCAT data)",,"312031",,,,"Operational"
3903.00,"12","Single level report sequences (satellite data)","312026","(QUIKSCAT data)",,"101004","Replication descriptor","Replicate 1 descriptor 4 times",,"Operational"
3904.00,"12","Single level report sequences (satellite data)","312026","(QUIKSCAT data)",,"312030",,,,"Operational"
3905.00,"12","Single level report sequences (satellite data)","312026","(QUIKSCAT data)",,"021110","Number of inner-beam sigma-0 (forward of satellite)","Number of inner-beam sigma-0 (forward of satellite)",,"Operational"
3906.00,"12","Single level report sequences (satellite data)","312026","(QUIKSCAT data)",,"301023",,"Location",,"Operational"
3907.00,"12","Single level report sequences (satellite data)","312026","(QUIKSCAT data)",,"321027",,,,"Operational"
3908.00,"12","Single level report sequences (satellite data)","312026","(QUIKSCAT data)",,"021111","Number of outer-beam sigma-0 (forward of satellite)","Number of outer-beam sigma-0 (forward of satellite)",,"Operational"
3909.00,"12","Single level report sequences (satellite data)","312026","(QUIKSCAT data)",,"301023",,"Location",,"Operational"
3910.00,"12","Single level report sequences (satellite data)","312026","(QUIKSCAT data)",,"321027",,,,"Operational"
3911.00,"12","Single level report sequences (satellite data)","312026","(QUIKSCAT data)",,"021112","Number of inner-beam sigma-0 (aft of satellite)","Number of inner-beam sigma-0 (aft of satellite)",,"Operational"
3912.00,"12","Single level report sequences (satellite data)","312026","(QUIKSCAT data)",,"301023",,"Location",,"Operational"
3913.00,"12","Single level report sequences (satellite data)","312026","(QUIKSCAT data)",,"321027",,,,"Operational"
3914.00,"12","Single level report sequences (satellite data)","312026","(QUIKSCAT data)",,"021113","Number of outer-beam sigma-0 (aft of satellite)","Number of outer-beam sigma-0 (aft of satellite)",,"Operational"
3915.00,"12","Single level report sequences (satellite data)","312026","(QUIKSCAT data)",,"301023",,"Location",,"Operational"
3916.00,"12","Single level report sequences (satellite data)","312026","(QUIKSCAT data)",,"321027",,,,"Operational"
3917.00,"12","Single level report sequences (satellite data)","312027","(ATSR SST product (SADIST-2))",,"301047","ERS product header","ERS product header",,"Operational"
3918.00,"12","Single level report sequences (satellite data)","312027","(ATSR SST product (SADIST-2))",,"105009","Replication descriptor","Repeat next 5 descriptors 9 times",,"Operational"
3919.00,"12","Single level report sequences (satellite data)","312027","(ATSR SST product (SADIST-2))",,"301023",,"Location (coarse latitude + longitude) of 10-arcmin cell",,"Operational"
3920.00,"12","Single level report sequences (satellite data)","312027","(ATSR SST product (SADIST-2))",,"007021","Elevation","Elevation: incidence angle Nadir view (set to zero)",,"Operational"
3921.00,"12","Single level report sequences (satellite data)","312027","(ATSR SST product (SADIST-2))",,"012061","Skin temperature","Skin temperature: SST (Nadir-only view)",,"Operational"
3922.00,"12","Single level report sequences (satellite data)","312027","(ATSR SST product (SADIST-2))",,"007021","Elevation","Elevation: incidence angle Dual view (set to ""missing"")",,"Operational"
3923.00,"12","Single level report sequences (satellite data)","312027","(ATSR SST product (SADIST-2))",,"012061","Skin temperature","Skin temperature: SST (Dual view)",,"Operational"
3924.00,"12","Single level report sequences (satellite data)","312027","(ATSR SST product (SADIST-2))",,"021085","ATSR sea surface temperature across-track band number","ATSR SST across-track band number (0-9)",,"Operational"
3925.00,"12","Single level report sequences (satellite data)","312027","(ATSR SST product (SADIST-2))",,"021070","SST product confidence data (SADIST-2)","SST product confidence data (SADIST-2) (23-bit flag)",,"Operational"
3926.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"301046",,,,"Operational"
3927.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"301011",,,,"Operational"
3928.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"301013",,,,"Operational"
3929.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"301023",,,,"Operational"
3930.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"008025","Time difference qualifier","Time difference qualifier",,"Operational"
3931.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"201136","Change data width","Change data width",,"Operational"
3932.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"004006","Second","Second",,"Operational"
3933.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"201000","Change data width","Change data width back to Table B",,"Operational"
3934.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"312031",,,,"Operational"
3935.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"312032",,,,"Operational"
3936.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"101004","Replication descriptor","Next descriptor replicated 4 times",,"Operational"
3937.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"312030",,,,"Operational"
3938.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"101002","Replication descriptor","Next descriptor replicated 2 times",,"Operational"
3939.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"312033",,,,"Operational"
3940.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"021110","Number of inner-beam sigma-0 (forward of satellite)","Number of inner-beam sigma-0 (forward of satellite)",,"Operational"
3941.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"301023",,,,"Operational"
3942.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"321028",,,,"Operational"
3943.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"021111","Number of outer-beam sigma-0 (forward of satellite)","Number of outer-beam sigma-0 (forward of satellite)",,"Operational"
3944.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"301023",,,,"Operational"
3945.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"321028",,,,"Operational"
3946.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"021112","Number of inner-beam sigma-0 (aft of satellite)","Number of inner-beam sigma-0 (aft of satellite)",,"Operational"
3947.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"301023",,,,"Operational"
3948.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"321028",,,,"Operational"
3949.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"021113","Number of outer-beam sigma-0 (aft of satellite)","Number of outer-beam sigma-0 (aft of satellite)",,"Operational"
3950.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"301023",,,,"Operational"
3951.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"321028",,,,"Operational"
3952.00,"12","Single level report sequences (satellite data)","312030",,,"201130","Change data width","Change data width",,"Operational"
3953.00,"12","Single level report sequences (satellite data)","312030",,,"202129","Change scale","Change scale",,"Operational"
3954.00,"12","Single level report sequences (satellite data)","312030",,,"011012","Wind speed at 10 m","Wind speed at 10 m",,"Operational"
3955.00,"12","Single level report sequences (satellite data)","312030",,,"202000","Change scale","Change scale back to Table B",,"Operational"
3956.00,"12","Single level report sequences (satellite data)","312030",,,"201000","Change data width","Change data width back to Table B",,"Operational"
3957.00,"12","Single level report sequences (satellite data)","312030",,,"011052","Formal uncertainty in wind speed","Formal uncertainty in wind speed",,"Operational"
3958.00,"12","Single level report sequences (satellite data)","312030",,,"201135","Change data width","Change data width",,"Operational"
3959.00,"12","Single level report sequences (satellite data)","312030",,,"202130","Change scale","Change scale",,"Operational"
3960.00,"12","Single level report sequences (satellite data)","312030",,,"011011","Wind direction at 10 m","Wind direction at 10 m",,"Operational"
3961.00,"12","Single level report sequences (satellite data)","312030",,,"202000","Change scale","Change scale back to Table B",,"Operational"
3962.00,"12","Single level report sequences (satellite data)","312030",,,"201000","Change data width","Change data width back to Table B",,"Operational"
3963.00,"12","Single level report sequences (satellite data)","312030",,,"011053","Formal uncertainty in wind direction","Formal uncertainty in wind direction",,"Operational"
3964.00,"12","Single level report sequences (satellite data)","312030",,,"021104","Likelihood computed for solution","Likelihood computed for solution",,"Operational"
3965.00,"12","Single level report sequences (satellite data)","312031",,,"005034","Along track row number","Along-track row number",,"Operational"
3966.00,"12","Single level report sequences (satellite data)","312031",,,"006034","Cross-track cell number","Cross-track cell number",,"Operational"
3967.00,"12","Single level report sequences (satellite data)","312031",,,"021109","SEAWINDS wind vector cell quality","SEAWINDS wind vector cell quality",,"Operational"
3968.00,"12","Single level report sequences (satellite data)","312031",,,"011081","Model wind direction at 10m","Model wind direction at 10 m",,"Operational"
3969.00,"12","Single level report sequences (satellite data)","312031",,,"011082","Model wind speed at 10m","Model wind speed at 10 m",,"Operational"
3970.00,"12","Single level report sequences (satellite data)","312031",,,"021101","Number of vector ambiguities","Number of vector ambiguities",,"Operational"
3971.00,"12","Single level report sequences (satellite data)","312031",,,"021102","Index of selected wind vector","Index of selected wind vector",,"Operational"
3972.00,"12","Single level report sequences (satellite data)","312031",,,"021103","Total number of sigma-0 measurements","Total number of sigma-0 measurements",,"Operational"
3973.00,"12","Single level report sequences (satellite data)","312032",,,"021120","Probability of rain","Probability of rain",,"Operational"
3974.00,"12","Single level report sequences (satellite data)","312032",,,"021121","SEAWINDS NOF rain index","SEAWINDS NOF rain index",,"Operational"
3975.00,"12","Single level report sequences (satellite data)","312032",,,"013055","Intensity of precipitation","Intensity of precipitation",,"Operational"
3976.00,"12","Single level report sequences (satellite data)","312032",,,"021122","Attenuation correction of sigma-0 (from tB)","Attenuation correction on sigma-0 (from tB)",,"Operational"
3977.00,"12","Single level report sequences (satellite data)","312033",,,"002104","Antenna polarization","Antenna polarization",,"Operational"
3978.00,"12","Single level report sequences (satellite data)","312033",,,"008022","Total number (with respect to accumulation or average)","Total number (with respect to accumulation)",,"Operational"
3979.00,"12","Single level report sequences (satellite data)","312033",,,"012063","Brightness temperature","Brightness temperature",,"Operational"
3980.00,"12","Single level report sequences (satellite data)","312033",,,"012065","Standard deviation brightness temperature","Standard deviation brightness temperature",,"Operational"
3981.00,"12","Single level report sequences (satellite data)","312041","(Altitude)",,"201141","Change data width","Change width to 28 bits",,"Operational"
3982.00,"12","Single level report sequences (satellite data)","312041","(Altitude)",,"202130","Change scale","Change scale to 2",,"Operational"
3983.00,"12","Single level report sequences (satellite data)","312041","(Altitude)",,"007001","Height of station","Altitude",,"Operational"
3984.00,"12","Single level report sequences (satellite data)","312041","(Altitude)",,"201000","Change data width","Change width back to Table B",,"Operational"
3985.00,"12","Single level report sequences (satellite data)","312041","(Altitude)",,"202000","Change scale","Change scale back to Table B",,"Operational"
3986.00,"12","Single level report sequences (satellite data)","312042","(Altitude corrections)",,"021077","Altitude correction (ionosphere)","Altitude correction, ionosphere",,"Operational"
3987.00,"12","Single level report sequences (satellite data)","312042","(Altitude corrections)",,"021078","Altitude correction (dry troposphere)","Altitude correction, dry troposphere",,"Operational"
3988.00,"12","Single level report sequences (satellite data)","312042","(Altitude corrections)",,"021079","Altitude correction (wet troposphere)","Altitude correction, wet troposphere",,"Operational"
3989.00,"12","Single level report sequences (satellite data)","312042","(Altitude corrections)",,"021080","Altitude correction (calibration constant)","Altitude correction, calibration constant",,"Operational"
3990.00,"12","Single level report sequences (satellite data)","312042","(Altitude corrections)",,"021081","Open loop correction (height-time loop)","Open loop height-time loop calibration correction",,"Operational"
3991.00,"12","Single level report sequences (satellite data)","312042","(Altitude corrections)",,"021082","Open loop correction (auto gain control)","Open loop automatic gain control calibration correction",,"Operational"
3992.00,"12","Single level report sequences (satellite data)","312045","(AATSR sea surface temperatures)",,"001007","Satellite identifier","Satellite identifier",,"Operational"
3993.00,"12","Single level report sequences (satellite data)","312045","(AATSR sea surface temperatures)",,"002019","Satellite instruments","Satellite instruments",,"Operational"
3994.00,"12","Single level report sequences (satellite data)","312045","(AATSR sea surface temperatures)",,"001096","Station acquisition","Station acquisition",,"Operational"
3995.00,"12","Single level report sequences (satellite data)","312045","(AATSR sea surface temperatures)",,"025061","Software identification and version number","Software identification and version number",,"Operational"
3996.00,"12","Single level report sequences (satellite data)","312045","(AATSR sea surface temperatures)",,"005040","Orbit number","Orbit number",,"Operational"
3997.00,"12","Single level report sequences (satellite data)","312045","(AATSR sea surface temperatures)",,"301011",,"Date",,"Operational"
3998.00,"12","Single level report sequences (satellite data)","312045","(AATSR sea surface temperatures)",,"301013",,"Time",,"Operational"
3999.00,"12","Single level report sequences (satellite data)","312045","(AATSR sea surface temperatures)",,"301021",,"Latitude/longitude",,"Operational"
4000.00,"12","Single level report sequences (satellite data)","312045","(AATSR sea surface temperatures)",,"007002","Height or altitude","Height or altitude",,"Operational"
4001.00,"12","Single level report sequences (satellite data)","312045","(AATSR sea surface temperatures)",,"012180","Averaged 12 micron BT for all clear pixels at nadir","Average 12 micron BT for all clear pixels at nadir",,"Operational"
4002.00,"12","Single level report sequences (satellite data)","312045","(AATSR sea surface temperatures)",,"012181","Averaged 11 micron BT for all clear pixels at nadir","Average 11 micron BT for all clear pixels at nadir",,"Operational"
4003.00,"12","Single level report sequences (satellite data)","312045","(AATSR sea surface temperatures)",,"012182","Averaged 3.7 micron BT for all clear pixels at nadir","Average 3.7 micron BT for all clear pixels at nadir",,"Operational"
4004.00,"12","Single level report sequences (satellite data)","312045","(AATSR sea surface temperatures)",,"012183","Averaged 12 micron BT for all clear pixels, forward view","Average 12 micron BT for all clear pixels, forward view",,"Operational"
4005.00,"12","Single level report sequences (satellite data)","312045","(AATSR sea surface temperatures)",,"012184","Averaged 11 micron BT for all clear pixels, forward view","Average 11 micron BT for all clear pixels, forward view",,"Operational"
4006.00,"12","Single level report sequences (satellite data)","312045","(AATSR sea surface temperatures)",,"012185","Averaged 3.7 micron BT for all clear pixels, forward view","Average 3.7 micron BT for all clear pixels, forward view",,"Operational"
4007.00,"12","Single level report sequences (satellite data)","312045","(AATSR sea surface temperatures)",,"002174","Mean across track pixel number","Mean across-track pixel number",,"Operational"
4008.00,"12","Single level report sequences (satellite data)","312045","(AATSR sea surface temperatures)",,"021086","Number of pixels in Nadir only, average","Number of pixels in nadir only, average",,"Operational"
4009.00,"12","Single level report sequences (satellite data)","312045","(AATSR sea surface temperatures)",,"012186","Mean nadir sea surface temperature","Mean nadir sea-surface temperature",,"Operational"
4010.00,"12","Single level report sequences (satellite data)","312045","(AATSR sea surface temperatures)",,"021087","Number of pixels in dual view, average","Number of pixels in dual view, average",,"Operational"
4011.00,"12","Single level report sequences (satellite data)","312045","(AATSR sea surface temperatures)",,"012187","Mean dual view sea-surface temperature","Mean dual view sea-surface temperature",,"Operational"
4012.00,"12","Single level report sequences (satellite data)","312045","(AATSR sea surface temperatures)",,"033043","AST confidence","ATS confidence",,"Operational"
4013.00,"12","Single level report sequences (satellite data)","312050","(MERIS instrument reporting)",,"001007","Satellite identifier","Satellite identifier",,"Operational"
4014.00,"12","Single level report sequences (satellite data)","312050","(MERIS instrument reporting)",,"002019","Satellite instruments","Instrument type",,"Operational"
4015.00,"12","Single level report sequences (satellite data)","312050","(MERIS instrument reporting)",,"001096","Station acquisition","Station acquisition",,"Operational"
4016.00,"12","Single level report sequences (satellite data)","312050","(MERIS instrument reporting)",,"025061","Software identification and version number","Software identification",,"Operational"
4017.00,"12","Single level report sequences (satellite data)","312050","(MERIS instrument reporting)",,"005040","Orbit number","Orbit number",,"Operational"
4018.00,"12","Single level report sequences (satellite data)","312050","(MERIS instrument reporting)",,"301011",,"Date",,"Operational"
4019.00,"12","Single level report sequences (satellite data)","312050","(MERIS instrument reporting)",,"301013",,"Time",,"Operational"
4020.00,"12","Single level report sequences (satellite data)","312050","(MERIS instrument reporting)",,"301021",,"Latitude/longitude",,"Operational"
4021.00,"12","Single level report sequences (satellite data)","312050","(MERIS instrument reporting)",,"007025","Solar zenith angle","Solar zenith angle",,"Operational"
4022.00,"12","Single level report sequences (satellite data)","312050","(MERIS instrument reporting)",,"005022","Solar azimuth","Solar azimuth",,"Operational"
4023.00,"12","Single level report sequences (satellite data)","312050","(MERIS instrument reporting)",,"010080","Viewing zenith angle","Viewing zenith angle",,"Operational"
4024.00,"12","Single level report sequences (satellite data)","312050","(MERIS instrument reporting)",,"027080","Viewing azimuth angle","Viewing azimuth angle",,"Operational"
4025.00,"12","Single level report sequences (satellite data)","312050","(MERIS instrument reporting)",,"008003","Vertical significance (satellite observations)","Vertical significance",,"Operational"
4026.00,"12","Single level report sequences (satellite data)","312050","(MERIS instrument reporting)",,"007004","Pressure","Pressure",,"Operational"
4027.00,"12","Single level report sequences (satellite data)","312050","(MERIS instrument reporting)",,"013093","Cloud optical thickness","Cloud optical thickness",,"Operational"
4028.00,"12","Single level report sequences (satellite data)","312050","(MERIS instrument reporting)",,"008003","Vertical significance (satellite observations)","Vertical significance",,"Operational"
4029.00,"12","Single level report sequences (satellite data)","312050","(MERIS instrument reporting)",,"201131","Change data width","Change data width",,"Operational"
4030.00,"12","Single level report sequences (satellite data)","312050","(MERIS instrument reporting)",,"202129","Change scale","Change scale",,"Operational"
4031.00,"12","Single level report sequences (satellite data)","312050","(MERIS instrument reporting)",,"007004","Pressure","Pressure",,"Operational"
4032.00,"12","Single level report sequences (satellite data)","312050","(MERIS instrument reporting)",,"007004","Pressure","Pressure",,"Operational"
4033.00,"12","Single level report sequences (satellite data)","312050","(MERIS instrument reporting)",,"202000","Change scale","Cancel operator",,"Operational"
4034.00,"12","Single level report sequences (satellite data)","312050","(MERIS instrument reporting)",,"201000","Change data width","Cancel operator",,"Operational"
4035.00,"12","Single level report sequences (satellite data)","312050","(MERIS instrument reporting)",,"013095","Total column water vapour","Total column water vapour",,"Operational"
4036.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"001007","Satellite identifier","Satellite identifier",,"Operational"
4037.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"002019","Satellite instruments","Satellite instrument type",,"Operational"
4038.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"001096","Station acquisition","Station acquisition",,"Operational"
4039.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"025061","Software identification and version number","Software identification",,"Operational"
4040.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"005040","Orbit number","Orbit number",,"Operational"
4041.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"008075","Ascending/descending orbit qualifier","Ascending/descending orbit qualifier",,"Operational"
4042.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"301011",,"Date",,"Operational"
4043.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"301013",,"Time",,"Operational"
4044.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"301021",,"Latitude/longitude",,"Operational"
4045.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"001012","Direction of motion of moving observing platform","Direction of motion of moving observing platform",,"Operational"
4046.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"201131","Change data width","Change data width",,"Operational"
4047.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"001013","Speed of motion of moving observing platform","Speed of motion of moving observing platform",,"Operational"
4048.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"201000","Change data width","Cancel operator",,"Operational"
4049.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"010032","Satellite distance to Earth's centre","Satellite distance to Earth centre",,"Operational"
4050.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"010033","Altitude (platform to ellipsoid)","Altitude (platform to ellipsoid)",,"Operational"
4051.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"010034","Earth radius","Earth radius",,"Operational"
4052.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"007002","Height or altitude","Height",,"Operational"
4053.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"008012","Land/sea qualifier","Land/sea qualifier",,"Operational"
4054.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"025110","Image processing summary","Image processing summary",,"Operational"
4055.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"025111","Number of input data gaps","Number of input data gaps",,"Operational"
4056.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"025102","Number of missing lines excluding data gaps","Number of missing lines excluding data gaps",,"Operational"
4057.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"002104","Antenna polarization","Antenna polarization",,"Operational"
4058.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"025103","Number of directional bins","Number of directional bins",,"Operational"
4059.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"025104","Number of wavelength bins","Number of wavelength bins",,"Operational"
4060.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"025105","First directional bin","First directional bin",,"Operational"
4061.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"025106","Directional bin step","Directional bin step",,"Operational"
4062.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"025107","First wavelength bin","First wavelength bin",,"Operational"
4063.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"025108","Last wavelength bin","Last wavelength bin",,"Operational"
4064.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"002111","Radar incidence angle","Radar incidence angle",,"Operational"
4065.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"002121","Mean frequency","Mean frequency",,"Operational"
4066.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"002026","Cross-track resolution","Cross-track resolution",,"Operational"
4067.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"002027","Along-track resolution","Along-track resolution",,"Operational"
4068.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"021130","Spectrum total energy","Spectrum total energy",,"Operational"
4069.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"021131","Spectrum max energy","Spectrum maximum energy",,"Operational"
4070.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"021132","Direction of spectrum max on higher resolution grid","Direction of spectrum max on higher resolution grid",,"Operational"
4071.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"021133","Wavelength of spectrum max on higher resolution grid","Wavelength of spectrum max on higher resolution grid",,"Operational"
4072.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"021064","Clutter noise estimate","Clutter noise estimate",,"Operational"
4073.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"025014","Azimuth clutter cut-off","Azimuth clutter cut-off",,"Operational"
4074.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"021134","Range resolution of cress covariance spectrum","Range resolution of cross covariance spectrum",,"Operational"
4075.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"107018","Replication descriptor","Replicate next 7 descriptors 18 times",,"Operational"
4076.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"005030","Direction (spectral)","Direction (spectral)",,"Operational"
4077.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"105024","Replication descriptor","Replicate 5 descriptors 24 times",,"Operational"
4078.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"201130","Change data width","Change data width",,"Operational"
4079.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"006030","Wave number (spectral)","Wave number (spectral)",,"Operational"
4080.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"201000","Change data width","Cancel operator",,"Operational"
4081.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"021135","Real part of cross spectra polar grid number of bins","Real part of cross spectra",,"Operational"
4082.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"021136","Imaginary part of cross spectra polar grid number of bins","Imaginary part of cross spectra",,"Operational"
4083.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"033044","ASAR quality information","ASAR quality",,"Operational"
4084.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"001007","Satellite identifier","Satellite identifier",,"Operational"
4085.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"002019","Satellite instruments","Satellite instrument type",,"Operational"
4086.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"001096","Station acquisition","Station acquisition",,"Operational"
4087.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"025061","Software identification and version number","Software identification",,"Operational"
4088.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"005040","Orbit number","Orbit number",,"Operational"
4089.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"025120","RA2-L2-processing flag","RA2 L2 processing flag",,"Operational"
4090.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"025121","RA2-L2-processing quality","RA2 L2 processing quality",,"Operational"
4091.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"025124","MWR-L2-processing flag","MWR L2 processing flag",,"Operational"
4092.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"025125","MWR-L2-processing quality","MWR L2 processing quality",,"Operational"
4093.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"025122","Hardware configuration for RF","Hardware configuration for RF",,"Operational"
4094.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"025123","Hardware configuration for HPA","Hardware configuration for HPA",,"Operational"
4095.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"301011",,"Date",,"Operational"
4096.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"301013",,"Time",,"Operational"
4097.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"301021",,"Latitude/longitude",,"Operational"
4098.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"007002","Height or altitude","Height or altitude",,"Operational"
4099.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"002119","RA-2 instrument operations","Instrument operations",,"Operational"
4100.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"033047","Measurement confidence data","Measurement confidence data",,"Operational"
4101.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"010081","Altitude of COG above reference ellipsoid","Altitude of COG above reference ellipsoid",,"Operational"
4102.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"010082","Instantaneous altitude rate","Instantaneous altitude rate",,"Operational"
4103.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"010083","Squared off nadir angle of the satellite from platform data","Off nadir angle of the satellite from platform data",,"Operational"
4104.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"010084","Squared off nadir angle of the satellite from waveform data","Off nadir angle of the satellite from waveform data",,"Operational"
4105.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"002116","Percentage of 320 MHz band processed","Percentage of 320 MHz band processed",,"Operational"
4106.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"002117","Percentage of 80 MHz band processed","Percentage of 80 MHz band processed",,"Operational"
4107.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"002118","Percentage of 20 MHz band processed","Percentage of 20 MHz band processed",,"Operational"
4108.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"002156","Percentage of valid Ku ocean retracker measurements","Percentage of valid Ku ocean retracker measurements",,"Operational"
4109.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"002157","Percentage of valid S ocean retracker measurements","Percentage of valid S ocean retracker measurements",,"Operational"
4110.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"014055","Solar activity index","Solar activity index",,"Operational"
4111.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"022150","Number of 18 Hz valid points for Ku band","Number of 18 Hz valid points for Ku band",,"Operational"
4112.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"022151","Ku band ocean range","Ku band ocean range",,"Operational"
4113.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"022152","STD of 18 Hz Ku band ocean range","STD of 18 Hz Ku band ocean range",,"Operational"
4114.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"022153","Number of 18 Hz valid points for S band","Number of 18 Hz valid points for S band",,"Operational"
4115.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"022154","S band ocean range","S band ocean range",,"Operational"
4116.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"022155","STD of 18 Hz S band ocean range","STD of 18 Hz S band ocean range",,"Operational"
4117.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"022156","Ku band significant wave height","Ku band significant wave height",,"Operational"
4118.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"022157","STD of 18 Hz Ku band ocean range","STD of 18 Hz Ku band significant wave height",,"Operational"
4119.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"022158","S band significant wave height","S band significant wave height",,"Operational"
4120.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"022159","STD of 18 Hz S band significant wave height","STD 18 Hz S band significant wave height",,"Operational"
4121.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"021137","Ku band corrected ocean backscatter coefficient","Ku band corrected ocean backscatter coefficient",,"Operational"
4122.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"021138","Std Ku band corrected ocean backscatter coefficient","STD Ku band corrected ocean backscatter coefficient",,"Operational"
4123.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"021139","Ku band net instrumental correction for AGC","Ku band net instrumental correction for AGC",,"Operational"
4124.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"021140","S band corrected ocean backscatter coefficient","S band corrected ocean backscatter coefficient",,"Operational"
4125.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"021141","Std S band corrected ocean backscatter coefficient","STD S band corrected ocean backscatter coefficient",,"Operational"
4126.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"021142","S band net instrumental correction for AGC","S band net instrumental correction for AGC",,"Operational"
4127.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"010085","Mean sea surface height","Mean sea-surface height",,"Operational"
4128.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"010086","Geoid's height","Geoid height",,"Operational"
4129.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"010087","Ocean depth/land elevation","Ocean depth/land elevation",,"Operational"
4130.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"010088","Total geocentric ocean tide height (solution 1)","Total geocentric ocean tide height solution 1",,"Operational"
4131.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"010089","Total geocentric ocean tide height (solution 2)","Total geocentric ocean tide height solution 2",,"Operational"
4132.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"010090","Long period tide height","Long period tide height",,"Operational"
4133.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"010091","Tidal loading height","Tidal loading height",,"Operational"
4134.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"010092","Solid Earth tide height","Solid earth tide height",,"Operational"
4135.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"010093","Geocentric pole tide height","Geocentric pole tide height",,"Operational"
4136.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"011002","Wind speed","Wind speed",,"Operational"
4137.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"025126","Model dry tropospheric correction","Model dry tropospheric correction",,"Operational"
4138.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"025127","Inverted barometer correction","Inverted barometer correction",,"Operational"
4139.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"025128","Model wet tropospheric correction","Model wet tropospheric correction",,"Operational"
4140.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"025129","MWR derived wet tropospheric correction","MWR derived wet tropospheric correction",,"Operational"
4141.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"025130","RA2 ionospheric correction on Ku band","RA2 ionospheric correction on Ku band",,"Operational"
4142.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"025131","Ionospheric correction from Doris on Ku band","Ionospheric correction from Doris on Ku band",,"Operational"
4143.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"025132","Ionospheric correction from model on Ku band","Ionospheric correction from model on Ku band",,"Operational"
4144.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"025133","Sea state bias correction on Ku band","Sea state bias correction on Ku band",,"Operational"
4145.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"025134","RA2 ionospheric correction on S band","RA2 ionospheric correction on S band",,"Operational"
4146.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"025135","Ionospheric correction from Doris on S band","Ionospheric correction from Doris on S band",,"Operational"
4147.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"025136","Ionospheric correction from model on S band","Ionospheric correction from model on S band",,"Operational"
4148.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"025137","Sea state bias correction on S band","Sea state bias correction on S band",,"Operational"
4149.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"013096","MWR water vapour content","MWR water vapour content",,"Operational"
4150.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"013097","MWR liquid water content","MWR liquid water content",,"Operational"
4151.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"011095","u component of the model wind vector","u component of model wind vector",,"Operational"
4152.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"011096","v component of the model wind vector","v component of model wind vector",,"Operational"
4153.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"012188","Interpolated 23.8 GHz brightness T from MWR","Interpolated 23.8 GHz brightness temperature from MWR",,"Operational"
4154.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"012189","Interpolated 36.5 GHz brightness T from MWR","Interpolated 36.5 GHz brightness temperature from MWR",,"Operational"
4155.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"002158","RA-2 instrument","RA2 instrument",,"Operational"
4156.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"002159","MWR instrument","MWR instrument",,"Operational"
4157.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"033052","S band ocean retracking quality","S band ocean retracking quality",,"Operational"
4158.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"033053","Ku band ocean retracking quality","Ku band ocean retracking quality",,"Operational"
4159.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"021143","Ku band rain attenuation","Ku band rain attenuation",,"Operational"
4160.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"021144","Altimeter rain flag","Altimeter rain flag",,"Operational"
4161.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"001007","Satellite identifier","Satellite identifier",,"Operational"
4162.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"002019","Satellite instruments","Satellite instrument type",,"Operational"
4163.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"001096","Station acquisition","Station acquisition",,"Operational"
4164.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"025061","Software identification and version number","Software identification and version number",,"Operational"
4165.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"005040","Orbit number","Orbit number",,"Operational"
4166.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"008075","Ascending/descending orbit qualifier","Ascending/descending orbit qualifier",,"Operational"
4167.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"301011",,"Date",,"Operational"
4168.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"301013",,"Time",,"Operational"
4169.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"301021",,"Latitude/longitude",,"Operational"
4170.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"001012","Direction of motion of moving observing platform","Direction of motion of moving observing platform",,"Operational"
4171.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"201131","Change data width","Change data width",,"Operational"
4172.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"001013","Speed of motion of moving observing platform","Speed of motion of moving observing platform",,"Operational"
4173.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"201000","Change data width","Cancel operator",,"Operational"
4174.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"010032","Satellite distance to Earth's centre","Satellite distance to Earth centre",,"Operational"
4175.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"010033","Altitude (platform to ellipsoid)","Altitude (platform to ellipsoid)",,"Operational"
4176.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"010034","Earth radius","Earth radius",,"Operational"
4177.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"007002","Height or altitude","Height or altitude",,"Operational"
4178.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"008012","Land/sea qualifier","Land/sea qualifier",,"Operational"
4179.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"025110","Image processing summary","Image processing summary",,"Operational"
4180.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"025111","Number of input data gaps","Number of input data gaps",,"Operational"
4181.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"025102","Number of missing lines excluding data gaps","Number of missing lines excluding data gaps",,"Operational"
4182.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"002104","Antenna polarization","Antenna polarization",,"Operational"
4183.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"025103","Number of directional bins","Number of directional bins",,"Operational"
4184.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"025104","Number of wave-length bins","Number of wavelength bins",,"Operational"
4185.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"025105","First directional bin","First directional bin",,"Operational"
4186.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"025106","Directional bin step","Directional bin step",,"Operational"
4187.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"025107","First wavelength bin","First wavelength bin",,"Operational"
4188.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"025108","Last wavelength bin","Last wavelength bin",,"Operational"
4189.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"011001","Wind direction","Wind direction",,"Operational"
4190.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"011002","Wind speed","Wind speed",,"Operational"
4191.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"022160","Normalized inverse wave age","Normalized inverse wave age",,"Operational"
4192.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"025138","Average signal-to-noise ratio","Average signal-to-noise ratio",,"Operational"
4193.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"201130","Change data width","Change data width",,"Operational"
4194.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"202129","Change scale","Change scale",,"Operational"
4195.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"022021","Height of waves","Height of waves",,"Operational"
4196.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"202000","Change scale","Cancel operator",,"Operational"
4197.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"201000","Change data width","Cancel operator",,"Operational"
4198.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"033048","Confidence measure of SAR inversion","Confidence measure for SAR inversion",,"Operational"
4199.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"033049","Confidence measure of wind retrieval","Confidence measure for wind retrieval",,"Operational"
4200.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"002026","Cross-track resolution","Cross-track resolution",,"Operational"
4201.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"002027","Along-track resolution","Along-track resolution",,"Operational"
4202.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"021130","Spectrum total energy","Spectrum total energy",,"Operational"
4203.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"021131","Spectrum max energy","Spectrum max energy",,"Operational"
4204.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"021132","Direction of spectrum max on higher resolution grid","Direction of spectrum max",,"Operational"
4205.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"021133","Wavelength of spectrum max on higher resolution grid","Wavelength of spectrum max",,"Operational"
4206.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"025014","Azimuth clutter cut-off","Azimuth clutter cut-off",,"Operational"
4207.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"106036","Replication descriptor","Replicate 6 descriptors 36 times",,"Operational"
4208.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"005030","Direction (spectral)","Direction (spectral)",,"Operational"
4209.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"104024","Replication descriptor","Replicate 4 descriptors 24 times",,"Operational"
4210.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"201130","Change data width","Change data width",,"Operational"
4211.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"006030","Wave number (spectral)","Wave number (spectral)",,"Operational"
4212.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"201000","Change data width","Cancel operator",,"Operational"
4213.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"022161","Wave spectra","Wave spectra",,"Operational"
4214.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"033044","ASAR quality information","ASAR quality",,"Operational"
4215.00,"12","Single level report sequences (satellite data)","312055","(ASCAT level 1b cell information)",,"005033","Pixel size on horizontal - 1","Pixel size on horizontal-1",,"Operational"
4216.00,"12","Single level report sequences (satellite data)","312055","(ASCAT level 1b cell information)",,"005040","Orbit number","Orbit number",,"Operational"
4217.00,"12","Single level report sequences (satellite data)","312055","(ASCAT level 1b cell information)",,"006034","Cross-track cell number","Cross track cell number",,"Operational"
4218.00,"12","Single level report sequences (satellite data)","312055","(ASCAT level 1b cell information)",,"010095","Height of atmosphere used","Height of atmosphere used",,"Operational"
4219.00,"12","Single level report sequences (satellite data)","312055","(ASCAT level 1b cell information)",,"021157","Loss per unit length of atmosphere used","Loss per unit length of atmosphere used",,"Operational"
4220.00,"12","Single level report sequences (satellite data)","312056","(Scatterometer wind cell information)",,"025060","Software identification","Software identification",,"Operational"
4221.00,"12","Single level report sequences (satellite data)","312056","(Scatterometer wind cell information)",,"001032","Generating application","Generating application",,"Operational"
4222.00,"12","Single level report sequences (satellite data)","312056","(Scatterometer wind cell information)",,"011082","Model wind speed at 10m","Model wind speed at 10 m",,"Operational"
4223.00,"12","Single level report sequences (satellite data)","312056","(Scatterometer wind cell information)",,"011081","Model wind direction at 10m","Model wind direction at 10 m",,"Operational"
4224.00,"12","Single level report sequences (satellite data)","312056","(Scatterometer wind cell information)",,"020095","Ice probability","Ice probability",,"Operational"
4225.00,"12","Single level report sequences (satellite data)","312056","(Scatterometer wind cell information)",,"020096","Ice age (""A"" parameter)","Ice age (a-parameter)",,"Operational"
4226.00,"12","Single level report sequences (satellite data)","312056","(Scatterometer wind cell information)",,"021155","Wind vector cell quality","Wind vector cell quality",,"Operational"
4227.00,"12","Single level report sequences (satellite data)","312056","(Scatterometer wind cell information)",,"201133","Change data width","Increase data width by 5 bits",,"Operational"
4228.00,"12","Single level report sequences (satellite data)","312056","(Scatterometer wind cell information)",,"021101","Number of vector ambiguities","Number of vector ambiguities",,"Operational"
4229.00,"12","Single level report sequences (satellite data)","312056","(Scatterometer wind cell information)",,"021102","Index of selected wind vector","Index of selected wind vector",,"Operational"
4230.00,"12","Single level report sequences (satellite data)","312056","(Scatterometer wind cell information)",,"201000","Change data width","Cancel change data width",,"Operational"
4231.00,"12","Single level report sequences (satellite data)","312057","(Ambiguous wind data)",,"201130","Change data width","Increase data width by 2 bits",,"Operational"
4232.00,"12","Single level report sequences (satellite data)","312057","(Ambiguous wind data)",,"202129","Change scale","Increase scaling by 10**1",,"Operational"
4233.00,"12","Single level report sequences (satellite data)","312057","(Ambiguous wind data)",,"011012","Wind speed at 10 m","Wind speed at 10 m",,"Operational"
4234.00,"12","Single level report sequences (satellite data)","312057","(Ambiguous wind data)",,"202000","Change scale","Cancel change scaling",,"Operational"
4235.00,"12","Single level report sequences (satellite data)","312057","(Ambiguous wind data)",,"201000","Change data width","Cancel change data width",,"Operational"
4236.00,"12","Single level report sequences (satellite data)","312057","(Ambiguous wind data)",,"201131","Change data width","Increase data width by 3 bits",,"Operational"
4237.00,"12","Single level report sequences (satellite data)","312057","(Ambiguous wind data)",,"202129","Change scale","Increase scaling by 10**1",,"Operational"
4238.00,"12","Single level report sequences (satellite data)","312057","(Ambiguous wind data)",,"011011","Wind direction at 10 m","Wind direction at 10 m",,"Operational"
4239.00,"12","Single level report sequences (satellite data)","312057","(Ambiguous wind data)",,"202000","Change scale","Cancel change scaling",,"Operational"
4240.00,"12","Single level report sequences (satellite data)","312057","(Ambiguous wind data)",,"201000","Change data width","Cancel change data width",,"Operational"
4241.00,"12","Single level report sequences (satellite data)","312057","(Ambiguous wind data)",,"021156","Backscatter distance","Backscatter distance",,"Operational"
4242.00,"12","Single level report sequences (satellite data)","312057","(Ambiguous wind data)",,"021104","Likelihood computed for solution","Likelihood computed for solution",,"Operational"
4243.00,"12","Single level report sequences (satellite data)","312058","(ASCAT level 1b data)",,"301125","ASCAT header information","ASCAT header information",,"Operational"
4244.00,"12","Single level report sequences (satellite data)","312058","(ASCAT level 1b data)",,"301011",,"Date information",,"Operational"
4245.00,"12","Single level report sequences (satellite data)","312058","(ASCAT level 1b data)",,"301013",,"Time information",,"Operational"
4246.00,"12","Single level report sequences (satellite data)","312058","(ASCAT level 1b data)",,"301021",,"Position information",,"Operational"
4247.00,"12","Single level report sequences (satellite data)","312058","(ASCAT level 1b data)",,"312055","ASCAT level 1b cell information","ASCAT level 1b cell information",,"Operational"
4248.00,"12","Single level report sequences (satellite data)","312058","(ASCAT level 1b data)",,"021150","Beam collocation","Beam co-location",,"Operational"
4249.00,"12","Single level report sequences (satellite data)","312058","(ASCAT level 1b data)",,"101003","Replication descriptor","Repeat next 1 descriptor 3 times",,"Operational"
4250.00,"12","Single level report sequences (satellite data)","312058","(ASCAT level 1b data)",,"321030","ASCAT sigma-0 information","ASCAT sigma-0 information",,"Operational"
4251.00,"12","Single level report sequences (satellite data)","312059","(Scatterometer wind data)",,"312056","Scatterometer wind cell information","Scatterometer wind cell information",,"Operational"
4252.00,"12","Single level report sequences (satellite data)","312059","(Scatterometer wind data)",,"101000","Replication descriptor","Delayed replication of next 1 descriptor",,"Operational"
4253.00,"12","Single level report sequences (satellite data)","312059","(Scatterometer wind data)",,"031001","Delayed descriptor replication factor","Delayed replication factor",,"Operational"
4254.00,"12","Single level report sequences (satellite data)","312059","(Scatterometer wind data)",,"312057","Ambiguous wind data","Ambiguous wind data",,"Operational"
4255.00,"12","Single level report sequences (satellite data)","312060","(Scatterometer soil moisture data)",,"025060","Software identification","Software identification",,"Operational"
4256.00,"12","Single level report sequences (satellite data)","312060","(Scatterometer soil moisture data)",,"025062","Database identification","Database identification",,"Operational"
4257.00,"12","Single level report sequences (satellite data)","312060","(Scatterometer soil moisture data)",,"040001","Surface soil moisture (ms)","Surface soil moisture (ms)",,"Operational"
4258.00,"12","Single level report sequences (satellite data)","312060","(Scatterometer soil moisture data)",,"040002","Estimated error in surface soil moisture","Estimated error in surface soil moisture",,"Operational"
4259.00,"12","Single level report sequences (satellite data)","312060","(Scatterometer soil moisture data)",,"021062","Backscatter","Extrapolated backscatter at 40 deg incidence angle (sigma0_40)",,"Operational"
4260.00,"12","Single level report sequences (satellite data)","312060","(Scatterometer soil moisture data)",,"021151","Estimated error in sigma-0 at 40 degrees incidence angle","Estimated error in sigma 0 at 40 deg incidence angle",,"Operational"
4261.00,"12","Single level report sequences (satellite data)","312060","(Scatterometer soil moisture data)",,"021152","Slope at 40 degrees incidence angle","Slope at 40 deg incidence angle",,"Operational"
4262.00,"12","Single level report sequences (satellite data)","312060","(Scatterometer soil moisture data)",,"021153","Estimated error in slope at 40 degrees incidence angle","Estimated error in slope at 40 deg incidence angle",,"Operational"
4263.00,"12","Single level report sequences (satellite data)","312060","(Scatterometer soil moisture data)",,"021154","Soil moisture sensitivity","Soil moisture sensitivity",,"Operational"
4264.00,"12","Single level report sequences (satellite data)","312060","(Scatterometer soil moisture data)",,"021062","Backscatter","Dry backscatter",,"Operational"
4265.00,"12","Single level report sequences (satellite data)","312060","(Scatterometer soil moisture data)",,"021088","Wet backscatter","Wet backscatter",,"Operational"
4266.00,"12","Single level report sequences (satellite data)","312060","(Scatterometer soil moisture data)",,"040003","Mean surface soil moisture","Mean surface soil moisture",,"Operational"
4267.00,"12","Single level report sequences (satellite data)","312060","(Scatterometer soil moisture data)",,"040004","Rain fall detection","Rain fall detection",,"Operational"
4268.00,"12","Single level report sequences (satellite data)","312060","(Scatterometer soil moisture data)",,"040005","Soil moisture correction flag","Soil moisture correction flag",,"Operational"
4269.00,"12","Single level report sequences (satellite data)","312060","(Scatterometer soil moisture data)",,"040006","Soil moisture processing flag","Soil moisture processing flag",,"Operational"
4270.00,"12","Single level report sequences (satellite data)","312060","(Scatterometer soil moisture data)",,"040007","Soil moisture quality","Soil moisture quality",,"Operational"
4271.00,"12","Single level report sequences (satellite data)","312060","(Scatterometer soil moisture data)",,"020065","Snow cover","Snow cover",,"Operational"
4272.00,"12","Single level report sequences (satellite data)","312060","(Scatterometer soil moisture data)",,"040008","Frozen land surface fraction","Frozen land surface fraction",,"Operational"
4273.00,"12","Single level report sequences (satellite data)","312060","(Scatterometer soil moisture data)",,"040009","Inundation and wetland fraction","Inundation and wetland fraction",,"Operational"
4274.00,"12","Single level report sequences (satellite data)","312060","(Scatterometer soil moisture data)",,"040010","Topographic complexity","Topographic complexity",,"Operational"
4275.00,"12","Single level report sequences (satellite data)","312061","(ASCAT Level 1b and level 2 data)",,"312058","ASCAT level 1b data","ASCAT level 1b data",,"Operational"
4276.00,"12","Single level report sequences (satellite data)","312061","(ASCAT Level 1b and level 2 data)",,"312060","Scatterometer soil moisture data","Scatterometer soil moisture data",,"Operational"
4277.00,"12","Single level report sequences (satellite data)","312061","(ASCAT Level 1b and level 2 data)",,"312059","Scatterometer wind data","Scatterometer wind data",,"Operational"
4278.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"001007","Satellite identifier","Satellite identifier",,"Operational"
4279.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"002019","Satellite instruments","Satellite instruments",,"Operational"
4280.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"001144","Snapshot identifier","Snapshot identifier",,"Operational"
4281.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"001124","Grid point identifier","Grid point identifier",,"Operational"
4282.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"030010","Number of grid points","Number of grid points",,"Operational"
4283.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"301011",,"Year, month, day",,"Operational"
4284.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"301013",,"Hour, minute, second",,"Operational"
4285.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"301021",,"Latitude, longitude (high accuracy)",,"Operational"
4286.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"007012","Grid point altitude","Grid point altitude",,"Operational"
4287.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"015012","Total electron count per square metre","Total electron count per square metre",,"Operational"
4288.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"012165","Direct sun brightness temperature","Direct sun brightness temperature",,"Operational"
4289.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"012166","Snapshot accuracy","Snapshot accuracy",,"Operational"
4290.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"012167","Radiometric accuracy (pure polarization)","Radiometric accuracy (pure polarization)",,"Operational"
4291.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"012168","Radiometric accuracy (cross polarization)","Radiometric accuracy (cross polarization)",,"Operational"
4292.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"027010","Footprint axis 1","Footprint axis 1",,"Operational"
4293.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"028010","Footprint axis 2","Footprint axis 2",,"Operational"
4294.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"002099","Polarization","Polarization",,"Operational"
4295.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"013048","Water fraction","Water fraction",,"Operational"
4296.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"025081","Incidence angle","Incidence angle",,"Operational"
4297.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"025082","Azimuth angle","Azimuth angle",,"Operational"
4298.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"025083","Faraday rotational angle","Faraday rotational angle",,"Operational"
4299.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"025084","Geometric rotational angle","Geometric rotational angle",,"Operational"
4300.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"012080","Brightness temperature real part","Brightness temperature real part",,"Operational"
4301.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"012081","Brightness temperature imaginary part","Brightness temperature imaginary part",,"Operational"
4302.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"012082","Pixel radiometric accuracy","Pixel radiometric accuracy",,"Operational"
4303.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"025174","SMOS information flag","SMOS information flag",,"Operational"
4304.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"033028","Snapshot overall quality","Snapshot overall quality",,"Operational"
4369.00,"13","Sequences common to image data","313009","(Radar reflectivity values)",,"021001","Horizontal reflectivity","Horizontal reflectivity",,"Operational"
4370.00,"13","Sequences common to image data","313009","(Radar reflectivity values)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
4371.00,"13","Sequences common to image data","313009","(Radar reflectivity values)",,"031001","Delayed descriptor replication factor","Replication factor",,"Operational"
4372.00,"13","Sequences common to image data","313009","(Radar reflectivity values)",,"021001","Horizontal reflectivity","Horizontal reflectivity",,"Operational"
4373.00,"13","Sequences common to image data","313010","(Radar rainfall intensities)",,"021036","Radar rainfall intensity","Radar rainfall intensity",,"Operational"
4374.00,"13","Sequences common to image data","313010","(Radar rainfall intensities)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
4375.00,"13","Sequences common to image data","313010","(Radar rainfall intensities)",,"031001","Delayed descriptor replication factor","Replication factor",,"Operational"
4376.00,"13","Sequences common to image data","313010","(Radar rainfall intensities)",,"021036","Radar rainfall intensity","Radar rainfall intensity",,"Operational"
4377.00,"13","Sequences common to image data","313031","(Non run-length encoded row for Pixel value (4 bits))",,"006002","Longitude (coarse accuracy)","First longitude location minus one increment",,"Operational"
4378.00,"13","Sequences common to image data","313031","(Non run-length encoded row for Pixel value (4 bits))",,"006012","Longitude increment (coarse accuracy)","Longitude increment",,"Operational"
4379.00,"13","Sequences common to image data","313031","(Non run-length encoded row for Pixel value (4 bits))",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
4380.00,"13","Sequences common to image data","313031","(Non run-length encoded row for Pixel value (4 bits))",,"031002","Extended delayed descriptor replication factor","Extended replication factor",,"Operational"
4381.00,"13","Sequences common to image data","313031","(Non run-length encoded row for Pixel value (4 bits))",,"030001","Pixel value (4 bits)","Pixel value (4 bits)",,"Operational"
4382.00,"13","Sequences common to image data","313032","(Non run-length encoded picture data for Pixel value (4 bits))",,"005002","Latitude (coarse accuracy)","First latitude location minus one increment",,"Operational"
4383.00,"13","Sequences common to image data","313032","(Non run-length encoded picture data for Pixel value (4 bits))",,"005012","Latitude increment (coarse accuracy)","Latitude increment (signed value so cannot cross pole)",,"Operational"
4384.00,"13","Sequences common to image data","313032","(Non run-length encoded picture data for Pixel value (4 bits))",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
4385.00,"13","Sequences common to image data","313032","(Non run-length encoded picture data for Pixel value (4 bits))",,"031002","Extended delayed descriptor replication factor","Extended replication factor",,"Operational"
4386.00,"13","Sequences common to image data","313032","(Non run-length encoded picture data for Pixel value (4 bits))",,"313031","Non run-length encoded row for Pixel value (4 bits)","Non run-length encoded row",,"Operational"
4387.00,"13","Sequences common to image data","313041","(Run-length encoded row for Pixel value (4 bits))",,"006002","Longitude (coarse accuracy)","First longitude location minus one increment",,"Operational"
4388.00,"13","Sequences common to image data","313041","(Run-length encoded row for Pixel value (4 bits))",,"110000","Replication descriptor","Delayed replication of 10 descriptors",,"Operational"
4389.00,"13","Sequences common to image data","313041","(Run-length encoded row for Pixel value (4 bits))",,"031001","Delayed descriptor replication factor","Replication factor",,"Operational"
4390.00,"13","Sequences common to image data","313041","(Run-length encoded row for Pixel value (4 bits))",,"104000","Replication descriptor","Delayed replication of 4 descriptors",,"Operational"
4391.00,"13","Sequences common to image data","313041","(Run-length encoded row for Pixel value (4 bits))",,"031001","Delayed descriptor replication factor","Replication factor",,"Operational"
4392.00,"13","Sequences common to image data","313041","(Run-length encoded row for Pixel value (4 bits))",,"006012","Longitude increment (coarse accuracy)","Longitude increment",,"Operational"
4393.00,"13","Sequences common to image data","313041","(Run-length encoded row for Pixel value (4 bits))",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
4394.00,"13","Sequences common to image data","313041","(Run-length encoded row for Pixel value (4 bits))",,"031012","Extended delayed descriptor and data repetition factor","Repetition factor",,"Operational"
4395.00,"13","Sequences common to image data","313041","(Run-length encoded row for Pixel value (4 bits))",,"030001","Pixel value (4 bits)","Pixel value (4 bits)",,"Operational"
4396.00,"13","Sequences common to image data","313041","(Run-length encoded row for Pixel value (4 bits))",,"006012","Longitude increment (coarse accuracy)","Longitude increment",,"Operational"
4397.00,"13","Sequences common to image data","313041","(Run-length encoded row for Pixel value (4 bits))",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
4398.00,"13","Sequences common to image data","313041","(Run-length encoded row for Pixel value (4 bits))",,"031001","Delayed descriptor replication factor","Replication factor",,"Operational"
4399.00,"13","Sequences common to image data","313041","(Run-length encoded row for Pixel value (4 bits))",,"030001","Pixel value (4 bits)","Pixel value (4 bits)",,"Operational"
4400.00,"13","Sequences common to image data","313042","(Run-length encoded picture data for Pixel value (4 bits))",,"005002","Latitude (coarse accuracy)","First latitude location minus one increment",,"Operational"
4401.00,"13","Sequences common to image data","313042","(Run-length encoded picture data for Pixel value (4 bits))",,"005012","Latitude increment (coarse accuracy)","Latitude increment (signed value so cannot cross pole)",,"Operational"
4402.00,"13","Sequences common to image data","313042","(Run-length encoded picture data for Pixel value (4 bits))",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
4403.00,"13","Sequences common to image data","313042","(Run-length encoded picture data for Pixel value (4 bits))",,"031002","Extended delayed descriptor replication factor","Extended replication factor",,"Operational"
4404.00,"13","Sequences common to image data","313042","(Run-length encoded picture data for Pixel value (4 bits))",,"313041","Run-length encoded row for Pixel value (4 bits)","Run-length encoded row",,"Operational"
4405.00,"13","Sequences common to image data","313043","(Run-length encoded picture data for pixel value (4 bits), regular grid)",,"006002","Longitude (coarse accuracy)","First longitude location minus one increment",,"Operational"
4406.00,"13","Sequences common to image data","313043","(Run-length encoded picture data for pixel value (4 bits), regular grid)",,"005002","Latitude (coarse accuracy)","First latitude location minus one increment",,"Operational"
4407.00,"13","Sequences common to image data","313043","(Run-length encoded picture data for pixel value (4 bits), regular grid)",,"005012","Latitude increment (coarse accuracy)","Latitude increment",,"Operational"
4408.00,"13","Sequences common to image data","313043","(Run-length encoded picture data for pixel value (4 bits), regular grid)",,"112000","Replication descriptor","Delayed replication of 12 descriptors",,"Operational"
4409.00,"13","Sequences common to image data","313043","(Run-length encoded picture data for pixel value (4 bits), regular grid)",,"031001","Delayed descriptor replication factor","Replication factor",,"Operational"
4410.00,"13","Sequences common to image data","313043","(Run-length encoded picture data for pixel value (4 bits), regular grid)",,"110000","Replication descriptor","Delayed replication of 10 descriptors",,"Operational"
4411.00,"13","Sequences common to image data","313043","(Run-length encoded picture data for pixel value (4 bits), regular grid)",,"031001","Delayed descriptor replication factor","Replication factor",,"Operational"
4412.00,"13","Sequences common to image data","313043","(Run-length encoded picture data for pixel value (4 bits), regular grid)",,"104000","Replication descriptor","Delayed replication of 4 descriptors",,"Operational"
4413.00,"13","Sequences common to image data","313043","(Run-length encoded picture data for pixel value (4 bits), regular grid)",,"031001","Delayed descriptor replication factor","Replication factor",,"Operational"
4414.00,"13","Sequences common to image data","313043","(Run-length encoded picture data for pixel value (4 bits), regular grid)",,"006012","Longitude increment (coarse accuracy)","Longitude increment",,"Operational"
4415.00,"13","Sequences common to image data","313043","(Run-length encoded picture data for pixel value (4 bits), regular grid)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
4416.00,"13","Sequences common to image data","313043","(Run-length encoded picture data for pixel value (4 bits), regular grid)",,"031011","Delayed descriptor and data repetition factor","Repetition factor",,"Operational"
4417.00,"13","Sequences common to image data","313043","(Run-length encoded picture data for pixel value (4 bits), regular grid)",,"030001","Pixel value (4 bits)","Pixel value (4 bits)",,"Operational"
4418.00,"13","Sequences common to image data","313043","(Run-length encoded picture data for pixel value (4 bits), regular grid)",,"006012","Longitude increment (coarse accuracy)","Longitude increment",,"Operational"
4419.00,"13","Sequences common to image data","313043","(Run-length encoded picture data for pixel value (4 bits), regular grid)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
4420.00,"13","Sequences common to image data","313043","(Run-length encoded picture data for pixel value (4 bits), regular grid)",,"031001","Delayed descriptor replication factor","Replication factor",,"Operational"
4421.00,"13","Sequences common to image data","313043","(Run-length encoded picture data for pixel value (4 bits), regular grid)",,"030001","Pixel value (4 bits)","Pixel value (4 bits)",,"Operational"
4422.00,"15","Oceanographic report sequences","315001","(Typically reported underwater sounding without optional fields)",,"001011","Ship or mobile land station identifier","Ship's call sign",,"Operational"
4423.00,"15","Oceanographic report sequences","315001","(Typically reported underwater sounding without optional fields)",,"301011",,"Date",,"Operational"
4424.00,"15","Oceanographic report sequences","315001","(Typically reported underwater sounding without optional fields)",,"301012",,"Time",,"Operational"
4425.00,"15","Oceanographic report sequences","315001","(Typically reported underwater sounding without optional fields)",,"301023",,"Latitude and longitude (coarse accuracy)",,"Operational"
4426.00,"15","Oceanographic report sequences","315001","(Typically reported underwater sounding without optional fields)",,"306001",,"Depth, temperature",,"Operational"
4427.00,"15","Oceanographic report sequences","315002","(Typically reported underwater sounding without optional fields)",,"001011","Ship or mobile land station identifier","Ship's call sign",,"Operational"
4428.00,"15","Oceanographic report sequences","315002","(Typically reported underwater sounding without optional fields)",,"301011",,"Date",,"Operational"
4429.00,"15","Oceanographic report sequences","315002","(Typically reported underwater sounding without optional fields)",,"301012",,"Time",,"Operational"
4430.00,"15","Oceanographic report sequences","315002","(Typically reported underwater sounding without optional fields)",,"301023",,"Latitude and longitude (coarse accuracy)",,"Operational"
4431.00,"15","Oceanographic report sequences","315002","(Typically reported underwater sounding without optional fields)",,"306004",,"Depth, temperature, salinity",,"Operational"
4432.00,"15","Oceanographic report sequences","315003","(Temperature and salinity profile observed by profile floats)",,"001087","WMO Marine observing platform extended identifier","WMO Marine observing platform extended identifier",,"Operational"
4433.00,"15","Oceanographic report sequences","315003","(Temperature and salinity profile observed by profile floats)",,"001085","Observing platform manufacturer's model","Observing platform manufacturers model",,"Operational"
4434.00,"15","Oceanographic report sequences","315003","(Temperature and salinity profile observed by profile floats)",,"001086","Observing platform manufacturer's serial number","Observing platform manufacturers serial number",,"Operational"
4435.00,"15","Oceanographic report sequences","315003","(Temperature and salinity profile observed by profile floats)",,"002036","Buoy type","Buoy type",,"Operational"
4436.00,"15","Oceanographic report sequences","315003","(Temperature and salinity profile observed by profile floats)",,"002148","Data collection and/or location system","Data collection and/or location system",,"Operational"
4437.00,"15","Oceanographic report sequences","315003","(Temperature and salinity profile observed by profile floats)",,"002149","Type of data buoy","Type of data buoy",,"Operational"
4438.00,"15","Oceanographic report sequences","315003","(Temperature and salinity profile observed by profile floats)",,"022055","Float cycle number","Float cycle number",,"Operational"
4439.00,"15","Oceanographic report sequences","315003","(Temperature and salinity profile observed by profile floats)",,"022056","Direction of profile","Direction of profile",,"Operational"
4440.00,"15","Oceanographic report sequences","315003","(Temperature and salinity profile observed by profile floats)",,"022067","Instrument type for water temperature profile measurement","Instrument type for water temperature profile measurement",,"Operational"
4441.00,"15","Oceanographic report sequences","315003","(Temperature and salinity profile observed by profile floats)",,"301011",,"Date",,"Operational"
4442.00,"15","Oceanographic report sequences","315003","(Temperature and salinity profile observed by profile floats)",,"301012",,"Time",,"Operational"
4443.00,"15","Oceanographic report sequences","315003","(Temperature and salinity profile observed by profile floats)",,"301021",,"Latitude and longitude (high accuracy)",,"Operational"
4444.00,"15","Oceanographic report sequences","315003","(Temperature and salinity profile observed by profile floats)",,"008080","Qualifier for GTSPP quality flag","Qualifier for quality class",,"Operational"
4445.00,"15","Oceanographic report sequences","315003","(Temperature and salinity profile observed by profile floats)",,"033050","Global GTSPP quality flag","GTSPP quality class",,"Operational"
4446.00,"15","Oceanographic report sequences","315003","(Temperature and salinity profile observed by profile floats)",,"109000","Replication descriptor","Delayed replication of 9 descriptors",,"Operational"
4447.00,"15","Oceanographic report sequences","315003","(Temperature and salinity profile observed by profile floats)",,"031002","Extended delayed descriptor replication factor","Extended delayed descriptor replication factor",,"Operational"
4448.00,"15","Oceanographic report sequences","315003","(Temperature and salinity profile observed by profile floats)",,"007065","Water pressure","Water pressure",,"Operational"
4449.00,"15","Oceanographic report sequences","315003","(Temperature and salinity profile observed by profile floats)",,"008080","Qualifier for GTSPP quality flag","Qualifier for quality class",,"Operational"
4450.00,"15","Oceanographic report sequences","315003","(Temperature and salinity profile observed by profile floats)",,"033050","Global GTSPP quality flag","GTSPP quality class",,"Operational"
4451.00,"15","Oceanographic report sequences","315003","(Temperature and salinity profile observed by profile floats)",,"022045","Sea/water temperature","Subsurface sea temperature",,"Operational"
4452.00,"15","Oceanographic report sequences","315003","(Temperature and salinity profile observed by profile floats)",,"008080","Qualifier for GTSPP quality flag","Qualifier for quality class",,"Operational"
4453.00,"15","Oceanographic report sequences","315003","(Temperature and salinity profile observed by profile floats)",,"033050","Global GTSPP quality flag","GTSPP quality class",,"Operational"
4454.00,"15","Oceanographic report sequences","315003","(Temperature and salinity profile observed by profile floats)",,"022064","Salinity","Salinity",,"Operational"
4455.00,"15","Oceanographic report sequences","315003","(Temperature and salinity profile observed by profile floats)",,"008080","Qualifier for GTSPP quality flag","Qualifier for quality class",,"Operational"
4456.00,"15","Oceanographic report sequences","315003","(Temperature and salinity profile observed by profile floats)",,"033050","Global GTSPP quality flag","GTSPP quality class",,"Operational"
4517.00,"16","Synoptic feature sequences","316001",,,"301011",,"Year, month, day",,"Operational"
4518.00,"16","Synoptic feature sequences","316001",,,"004004","Hour","Hour",,"Operational"
4519.00,"16","Synoptic feature sequences","316001",,,"301023",,"Latitude and longitude (coarse accuracy)",,"Operational"
4520.00,"16","Synoptic feature sequences","316001",,,"001021","Synoptic feature identifier","Synoptic feature identifier",,"Operational"
4521.00,"16","Synoptic feature sequences","316001",,,"002041","Method for estimating reports related to synoptic features","Method for estimating reports related to synoptic features",,"Operational"
4522.00,"16","Synoptic feature sequences","316001",,,"019001","Type of synoptic feature","Type of synoptic feature",,"Operational"
4523.00,"16","Synoptic feature sequences","316001",,,"010051","Pressure reduced to mean sea level","Pressure reduced to mean sea level",,"Operational"
4524.00,"16","Synoptic feature sequences","316001",,,"019002","Effective radius of feature","Effective radius of feature",,"Operational"
4525.00,"16","Synoptic feature sequences","316001",,,"019003","Wind speed threshold","Wind speed threshold (15 m s**-1 typically)",,"Operational"
4526.00,"16","Synoptic feature sequences","316001",,,"019004","Effective radius with respect to wind speeds above threshold","Effective radius with respect to wind speeds above threshold",,"Operational"
4527.00,"16","Synoptic feature sequences","316002","(Header)",,"008021","Time significance","Data time (analysis)",,"Operational"
4528.00,"16","Synoptic feature sequences","316002","(Header)",,"004001","Year","Year",,"Operational"
4529.00,"16","Synoptic feature sequences","316002","(Header)",,"004002","Month","Month",,"Operational"
4530.00,"16","Synoptic feature sequences","316002","(Header)",,"004003","Day","Day",,"Operational"
4531.00,"16","Synoptic feature sequences","316002","(Header)",,"004004","Hour","Hour",,"Operational"
4532.00,"16","Synoptic feature sequences","316002","(Header)",,"004005","Minute","Minute",,"Operational"
4533.00,"16","Synoptic feature sequences","316002","(Header)",,"001033","Identification of originating/generating centre","Originating/generating centre",,"Operational"
4534.00,"16","Synoptic feature sequences","316002","(Header)",,"008021","Time significance","Validity time (forecast)",,"Operational"
4535.00,"16","Synoptic feature sequences","316002","(Header)",,"004001","Year","Year",,"Operational"
4536.00,"16","Synoptic feature sequences","316002","(Header)",,"004002","Month","Month",,"Operational"
4537.00,"16","Synoptic feature sequences","316002","(Header)",,"004003","Day","Day",,"Operational"
4538.00,"16","Synoptic feature sequences","316002","(Header)",,"004004","Hour","Hour",,"Operational"
4539.00,"16","Synoptic feature sequences","316002","(Header)",,"004005","Minute","Minute",,"Operational"
4540.00,"16","Synoptic feature sequences","316002","(Header)",,"007002","Height or altitude","Flight level (altitude) (base of chart layer)",,"Operational"
4541.00,"16","Synoptic feature sequences","316002","(Header)",,"007002","Height or altitude","Flight level (altitude) (top of chart layer)",,"Operational"
4542.00,"16","Synoptic feature sequences","316003","(Jet stream)",,"110000","Replication descriptor","Delayed replication",,"Operational"
4543.00,"16","Synoptic feature sequences","316003","(Jet stream)",,"031001","Delayed descriptor replication factor","Replication",,"Operational"
4544.00,"16","Synoptic feature sequences","316003","(Jet stream)",,"008011","Meteorological feature","Meteorological feature (jet stream value)",,"Operational"
4545.00,"16","Synoptic feature sequences","316003","(Jet stream)",,"008007","Dimensional significance","Dimensional significance (value for line)",,"Operational"
4546.00,"16","Synoptic feature sequences","316003","(Jet stream)",,"104000","Replication descriptor","Delayed replication",,"Operational"
4547.00,"16","Synoptic feature sequences","316003","(Jet stream)",,"031001","Delayed descriptor replication factor","Replication",,"Operational"
4548.00,"16","Synoptic feature sequences","316003","(Jet stream)",,"005002","Latitude (coarse accuracy)","Latitude (coarse)",,"Operational"
4549.00,"16","Synoptic feature sequences","316003","(Jet stream)",,"006002","Longitude (coarse accuracy)","Longitude (coarse)",,"Operational"
4550.00,"16","Synoptic feature sequences","316003","(Jet stream)",,"010002","Height","Flight level (altitude)",,"Operational"
4551.00,"16","Synoptic feature sequences","316003","(Jet stream)",,"011002","Wind speed","Wind speed",,"Operational"
4552.00,"16","Synoptic feature sequences","316003","(Jet stream)",,"008007","Dimensional significance","Dimensional significance (cancel)",,"Operational"
4553.00,"16","Synoptic feature sequences","316003","(Jet stream)",,"008011","Meteorological feature","Meteorological feature (cancel/end of object)",,"Operational"
4554.00,"16","Synoptic feature sequences","316004","(Turbulence)",,"111000","Replication descriptor","Delayed replication",,"Operational"
4555.00,"16","Synoptic feature sequences","316004","(Turbulence)",,"031001","Delayed descriptor replication factor","Replication",,"Operational"
4556.00,"16","Synoptic feature sequences","316004","(Turbulence)",,"008011","Meteorological feature","Meteorological feature (value for turbulence)",,"Operational"
4557.00,"16","Synoptic feature sequences","316004","(Turbulence)",,"008007","Dimensional significance","Dimensional significance (value for area)",,"Operational"
4558.00,"16","Synoptic feature sequences","316004","(Turbulence)",,"007002","Height or altitude","Flight level (altitude) (base of layer)",,"Operational"
4559.00,"16","Synoptic feature sequences","316004","(Turbulence)",,"007002","Height or altitude","Flight level (altitude) (top of layer)",,"Operational"
4560.00,"16","Synoptic feature sequences","316004","(Turbulence)",,"102000","Replication descriptor","Delayed replication",,"Operational"
4561.00,"16","Synoptic feature sequences","316004","(Turbulence)",,"031001","Delayed descriptor replication factor","Replication",,"Operational"
4562.00,"16","Synoptic feature sequences","316004","(Turbulence)",,"005002","Latitude (coarse accuracy)","Latitude (coarse)",,"Operational"
4563.00,"16","Synoptic feature sequences","316004","(Turbulence)",,"006002","Longitude (coarse accuracy)","Longitude (coarse)",,"Operational"
4564.00,"16","Synoptic feature sequences","316004","(Turbulence)",,"011031","Degree of turbulence","Degree of turbulence","(see Note 1)","Operational"
4565.00,"16","Synoptic feature sequences","316004","(Turbulence)",,"008007","Dimensional significance","Dimensional significance (cancel)",,"Operational"
4566.00,"16","Synoptic feature sequences","316004","(Turbulence)",,"008011","Meteorological feature","Meteorological feature (cancel/end of object)",,"Operational"
4567.00,"16","Synoptic feature sequences","316005","(Storm)",,"108000","Replication descriptor","Delayed replication",,"Operational"
4568.00,"16","Synoptic feature sequences","316005","(Storm)",,"031001","Delayed descriptor replication factor","Replication",,"Operational"
4569.00,"16","Synoptic feature sequences","316005","(Storm)",,"008005","Meteorological attribute significance","Meteorological attribute significance (storm centre)",,"Operational"
4570.00,"16","Synoptic feature sequences","316005","(Storm)",,"008007","Dimensional significance","Dimensional significance (value for point)",,"Operational"
4571.00,"16","Synoptic feature sequences","316005","(Storm)",,"005002","Latitude (coarse accuracy)","Latitude (coarse)",,"Operational"
4572.00,"16","Synoptic feature sequences","316005","(Storm)",,"006002","Longitude (coarse accuracy)","Longitude (coarse)",,"Operational"
4573.00,"16","Synoptic feature sequences","316005","(Storm)",,"001026","WMO storm name","WMO storm name (use ""UNKNOWN"" for a sandstorm)",,"Operational"
4574.00,"16","Synoptic feature sequences","316005","(Storm)",,"019001","Type of synoptic feature","Synoptic features (value for type of storm)",,"Operational"
4575.00,"16","Synoptic feature sequences","316005","(Storm)",,"008007","Dimensional significance","Dimensional significance (cancel)",,"Operational"
4576.00,"16","Synoptic feature sequences","316005","(Storm)",,"008005","Meteorological attribute significance","Meteorological attribute significance (cancel/end of object)",,"Operational"
4577.00,"16","Synoptic feature sequences","316006","(Cloud)",,"112000","Replication descriptor","Delayed replication",,"Operational"
4578.00,"16","Synoptic feature sequences","316006","(Cloud)",,"031001","Delayed descriptor replication factor","Replication",,"Operational"
4579.00,"16","Synoptic feature sequences","316006","(Cloud)",,"008011","Meteorological feature","Meteorological feature (value for cloud)",,"Operational"
4580.00,"16","Synoptic feature sequences","316006","(Cloud)",,"008007","Dimensional significance","Dimensional significance (value for area)",,"Operational"
4581.00,"16","Synoptic feature sequences","316006","(Cloud)",,"007002","Height or altitude","Flight level (altitude) (base of layer)",,"Operational"
4582.00,"16","Synoptic feature sequences","316006","(Cloud)",,"007002","Height or altitude","Flight level (altitude) (top of layer)",,"Operational"
4583.00,"16","Synoptic feature sequences","316006","(Cloud)",,"102000","Replication descriptor","Delayed replication",,"Operational"
4584.00,"16","Synoptic feature sequences","316006","(Cloud)",,"031001","Delayed descriptor replication factor","Replication",,"Operational"
4585.00,"16","Synoptic feature sequences","316006","(Cloud)",,"005002","Latitude (coarse accuracy)","Latitude (coarse)",,"Operational"
4586.00,"16","Synoptic feature sequences","316006","(Cloud)",,"006002","Longitude (coarse accuracy)","Longitude (coarse)",,"Operational"
4587.00,"16","Synoptic feature sequences","316006","(Cloud)",,"020011","Cloud amount","Cloud amount","(see Note 2)","Operational"
4588.00,"16","Synoptic feature sequences","316006","(Cloud)",,"020012","Cloud type","Cloud type",,"Operational"
4589.00,"16","Synoptic feature sequences","316006","(Cloud)",,"008007","Dimensional significance","Dimensional significance (cancel)",,"Operational"
4590.00,"16","Synoptic feature sequences","316006","(Cloud)",,"008011","Meteorological feature","Meteorological feature (cancel/end of object)",,"Operational"
4591.00,"16","Synoptic feature sequences","316007","(Front)",,"110000","Replication descriptor","Delayed replication",,"Operational"
4592.00,"16","Synoptic feature sequences","316007","(Front)",,"031001","Delayed descriptor replication factor","Replication",,"Operational"
4593.00,"16","Synoptic feature sequences","316007","(Front)",,"008011","Meteorological feature","Meteorological feature (value for type of front)","(see Note 3)","Operational"
4594.00,"16","Synoptic feature sequences","316007","(Front)",,"008007","Dimensional significance","Dimensional significance (value for line)",,"Operational"
4595.00,"16","Synoptic feature sequences","316007","(Front)",,"104000","Replication descriptor","Delayed replication",,"Operational"
4596.00,"16","Synoptic feature sequences","316007","(Front)",,"031001","Delayed descriptor replication factor","Replication",,"Operational"
4597.00,"16","Synoptic feature sequences","316007","(Front)",,"005002","Latitude (coarse accuracy)","Latitude (coarse)",,"Operational"
4598.00,"16","Synoptic feature sequences","316007","(Front)",,"006002","Longitude (coarse accuracy)","Longitude (coarse)",,"Operational"
4599.00,"16","Synoptic feature sequences","316007","(Front)",,"019005","Direction of motion of feature","Direction of feature",,"Operational"
4600.00,"16","Synoptic feature sequences","316007","(Front)",,"019006","Speed of motion of feature","Speed of feature",,"Operational"
4601.00,"16","Synoptic feature sequences","316007","(Front)",,"008007","Dimensional significance","Dimensional significance (cancel)",,"Operational"
4602.00,"16","Synoptic feature sequences","316007","(Front)",,"008011","Meteorological feature","Meteorological feature (cancel/end of object)",,"Operational"
4603.00,"16","Synoptic feature sequences","316008","(Tropopause)",,"111000","Replication descriptor","Delayed replication",,"Operational"
4604.00,"16","Synoptic feature sequences","316008","(Tropopause)",,"031001","Delayed descriptor replication factor","Replication",,"Operational"
4605.00,"16","Synoptic feature sequences","316008","(Tropopause)",,"008001","Vertical sounding significance","Vertical significance (bit 3 set for tropopause)",,"Operational"
4606.00,"16","Synoptic feature sequences","316008","(Tropopause)",,"008007","Dimensional significance","Dimensional significance (value for point)",,"Operational"
4607.00,"16","Synoptic feature sequences","316008","(Tropopause)",,"008023","First-order statistics","Statistic (type of tropopause value)","(see Note 4)","Operational"
4608.00,"16","Synoptic feature sequences","316008","(Tropopause)",,"103000","Replication descriptor","Delayed replication",,"Operational"
4609.00,"16","Synoptic feature sequences","316008","(Tropopause)",,"031001","Delayed descriptor replication factor","Replication",,"Operational"
4610.00,"16","Synoptic feature sequences","316008","(Tropopause)",,"005002","Latitude (coarse accuracy)","Latitude (coarse)",,"Operational"
4611.00,"16","Synoptic feature sequences","316008","(Tropopause)",,"006002","Longitude (coarse accuracy)","Longitude (coarse)",,"Operational"
4612.00,"16","Synoptic feature sequences","316008","(Tropopause)",,"010002","Height","Height/altitude",,"Operational"
4613.00,"16","Synoptic feature sequences","316008","(Tropopause)",,"008023","First-order statistics","Statistic (cancel)",,"Operational"
4614.00,"16","Synoptic feature sequences","316008","(Tropopause)",,"008007","Dimensional significance","Dimensional significance (cancel)",,"Operational"
4615.00,"16","Synoptic feature sequences","316008","(Tropopause)",,"008001","Vertical sounding significance","Vertical significance (cancel/end of object)",,"Operational"
4616.00,"16","Synoptic feature sequences","316009","(Airframe icing area)",,"111000","Replication descriptor","Delayed replication",,"Operational"
4617.00,"16","Synoptic feature sequences","316009","(Airframe icing area)",,"031001","Delayed descriptor replication factor","Replication",,"Operational"
4618.00,"16","Synoptic feature sequences","316009","(Airframe icing area)",,"008011","Meteorological feature","Meteorological feature (value for airframe icing)",,"Operational"
4619.00,"16","Synoptic feature sequences","316009","(Airframe icing area)",,"008007","Dimensional significance","Dimensional significance (value for area)",,"Operational"
4620.00,"16","Synoptic feature sequences","316009","(Airframe icing area)",,"007002","Height or altitude","Flight level (altitude) (base of layer)",,"Operational"
4621.00,"16","Synoptic feature sequences","316009","(Airframe icing area)",,"007002","Height or altitude","Flight level (altitude) (top of layer)",,"Operational"
4622.00,"16","Synoptic feature sequences","316009","(Airframe icing area)",,"102000","Replication descriptor","Delayed replication",,"Operational"
4623.00,"16","Synoptic feature sequences","316009","(Airframe icing area)",,"031001","Delayed descriptor replication factor","Replication",,"Operational"
4624.00,"16","Synoptic feature sequences","316009","(Airframe icing area)",,"005002","Latitude (coarse accuracy)","Latitude (coarse)",,"Operational"
4625.00,"16","Synoptic feature sequences","316009","(Airframe icing area)",,"006002","Longitude (coarse accuracy)","Longitude (coarse)",,"Operational"
4626.00,"16","Synoptic feature sequences","316009","(Airframe icing area)",,"020041","Airframe icing","Airframe icing (type of airframe icing)",,"Operational"
4627.00,"16","Synoptic feature sequences","316009","(Airframe icing area)",,"008007","Dimensional significance","Dimensional significance (cancel)",,"Operational"
4628.00,"16","Synoptic feature sequences","316009","(Airframe icing area)",,"008011","Meteorological feature","Meteorological feature (cancel/end of object)",,"Operational"
4629.00,"16","Synoptic feature sequences","316010","(Name of feature)",,"107000","Replication descriptor","Delayed replication",,"Operational"
4630.00,"16","Synoptic feature sequences","316010","(Name of feature)",,"031001","Delayed descriptor replication factor","Replication",,"Operational"
4631.00,"16","Synoptic feature sequences","316010","(Name of feature)",,"008011","Meteorological feature","Meteorological feature",,"Operational"
4632.00,"16","Synoptic feature sequences","316010","(Name of feature)",,"008007","Dimensional significance","Dimensional significance (value for point)",,"Operational"
4633.00,"16","Synoptic feature sequences","316010","(Name of feature)",,"001022","Name of feature","Name of feature",,"Operational"
4634.00,"16","Synoptic feature sequences","316010","(Name of feature)",,"005002","Latitude (coarse accuracy)","Latitude (coarse)",,"Operational"
4635.00,"16","Synoptic feature sequences","316010","(Name of feature)",,"006002","Longitude (coarse accuracy)","Longitude (coarse)",,"Operational"
4636.00,"16","Synoptic feature sequences","316010","(Name of feature)",,"008007","Dimensional significance","Dimensional significance (cancel)",,"Operational"
4637.00,"16","Synoptic feature sequences","316010","(Name of feature)",,"008011","Meteorological feature","Meteorological feature (cancel/end of object)",,"Operational"
4638.00,"16","Synoptic feature sequences","316011","(Volcano erupting)",,"117000","Replication descriptor","Delayed replication",,"Operational"
4639.00,"16","Synoptic feature sequences","316011","(Volcano erupting)",,"031001","Delayed descriptor replication factor","Replication",,"Operational"
4640.00,"16","Synoptic feature sequences","316011","(Volcano erupting)",,"008011","Meteorological feature","Meteorological feature (value for special clouds)",,"Operational"
4641.00,"16","Synoptic feature sequences","316011","(Volcano erupting)",,"001022","Name of feature","Name of feature (volcano name)",,"Operational"
4642.00,"16","Synoptic feature sequences","316011","(Volcano erupting)",,"008007","Dimensional significance","Dimensional significance (value for point)",,"Operational"
4643.00,"16","Synoptic feature sequences","316011","(Volcano erupting)",,"102000","Replication descriptor","Delayed replication",,"Operational"
4644.00,"16","Synoptic feature sequences","316011","(Volcano erupting)",,"031001","Delayed descriptor replication factor","Replication",,"Operational"
4645.00,"16","Synoptic feature sequences","316011","(Volcano erupting)",,"005002","Latitude (coarse accuracy)","Latitude (coarse)",,"Operational"
4646.00,"16","Synoptic feature sequences","316011","(Volcano erupting)",,"006002","Longitude (coarse accuracy)","Longitude (coarse)",,"Operational"
4647.00,"16","Synoptic feature sequences","316011","(Volcano erupting)",,"008021","Time significance","Time significance (eruption starting time)",,"Operational"
4648.00,"16","Synoptic feature sequences","316011","(Volcano erupting)",,"004001","Year","Year",,"Operational"
4649.00,"16","Synoptic feature sequences","316011","(Volcano erupting)",,"004002","Month","Month",,"Operational"
4650.00,"16","Synoptic feature sequences","316011","(Volcano erupting)",,"004003","Day","Day",,"Operational"
4651.00,"16","Synoptic feature sequences","316011","(Volcano erupting)",,"004004","Hour","Hour",,"Operational"
4652.00,"16","Synoptic feature sequences","316011","(Volcano erupting)",,"004005","Minute","Minute",,"Operational"
4653.00,"16","Synoptic feature sequences","316011","(Volcano erupting)",,"020090","Special clouds","Special clouds (clouds from volcanic eruptions)",,"Operational"
4654.00,"16","Synoptic feature sequences","316011","(Volcano erupting)",,"008021","Time significance","Time significance (cancel)",,"Operational"
4655.00,"16","Synoptic feature sequences","316011","(Volcano erupting)",,"008007","Dimensional significance","Dimensional significance (cancel)",,"Operational"
4656.00,"16","Synoptic feature sequences","316011","(Volcano erupting)",,"008011","Meteorological feature","Meteorological feature (cancel/end of object)",,"Operational"
4657.00,"16","Synoptic feature sequences","316022","(Forecast data)",,"001032","Generating application","Generating application (NWP model name, etc. code table defined by originating/generating centre)",,"Operational"
4658.00,"16","Synoptic feature sequences","316022","(Forecast data)",,"002041","Method for estimating reports related to synoptic features","Method for estimating reports related to synoptic feature",,"Operational"
4659.00,"16","Synoptic feature sequences","316022","(Forecast data)",,"019001","Type of synoptic feature","Type of synoptic feature",,"Operational"
4660.00,"16","Synoptic feature sequences","316022","(Forecast data)",,"019010","Method for tracking the centre of synoptic feature","Method for tracing of the centre of synoptic feature",,"Operational"
4661.00,"16","Synoptic feature sequences","316022","(Forecast data)",,"118000","Replication descriptor","Delayed replication of 18 descriptors",,"Operational"
4662.00,"16","Synoptic feature sequences","316022","(Forecast data)",,"031001","Delayed descriptor replication factor","Replication factor",,"Operational"
4663.00,"16","Synoptic feature sequences","316022","(Forecast data)",,"008021","Time significance","Time significance (forecast)",,"Operational"
4664.00,"16","Synoptic feature sequences","316022","(Forecast data)",,"004014","Time increment","Time increment (hour)",,"Operational"
4665.00,"16","Synoptic feature sequences","316022","(Forecast data)",,"008005","Meteorological attribute significance","Surface synoptic feature significance",,"Operational"
4666.00,"16","Synoptic feature sequences","316022","(Forecast data)",,"301023",,"Latitude (coarse accuracy), longitude (coarse accuracy)",,"Operational"
4667.00,"16","Synoptic feature sequences","316022","(Forecast data)",,"019005","Direction of motion of feature","Direction of motion of feature",,"Operational"
4668.00,"16","Synoptic feature sequences","316022","(Forecast data)",,"019006","Speed of motion of feature","Speed of motion of feature",,"Operational"
4669.00,"16","Synoptic feature sequences","316022","(Forecast data)",,"010004","Pressure","Pressure",,"Operational"
4670.00,"16","Synoptic feature sequences","316022","(Forecast data)",,"011041","Maximum wind gust speed","Maximum wind speed (gust: e.g. used in the United States)",,"Operational"
4671.00,"16","Synoptic feature sequences","316022","(Forecast data)",,"008021","Time significance","Time significance (forecast time averaged)",,"Operational"
4672.00,"16","Synoptic feature sequences","316022","(Forecast data)",,"004075","Short time period or displacement","Time period (minutes)",,"Operational"
4673.00,"16","Synoptic feature sequences","316022","(Forecast data)",,"011040","Maximum wind speed (mean wind)","Maximum wind speed (mean wind)",,"Operational"
4674.00,"16","Synoptic feature sequences","316022","(Forecast data)",,"019008","Vertical extent of circulation","Vertical extent of feature",,"Operational"
4675.00,"16","Synoptic feature sequences","316022","(Forecast data)",,"105004","Replication descriptor","Replicate 5 descriptors 4 times",,"Operational"
4676.00,"16","Synoptic feature sequences","316022","(Forecast data)",,"005021","Bearing or azimuth","Starting bearing or azimuth",,"Operational"
4677.00,"16","Synoptic feature sequences","316022","(Forecast data)",,"005021","Bearing or azimuth","Ending bearing or azimuth",,"Operational"
4678.00,"16","Synoptic feature sequences","316022","(Forecast data)",,"102002","Replication descriptor","Replicate 2 descriptors 2 times",,"Operational"
4679.00,"16","Synoptic feature sequences","316022","(Forecast data)",,"019003","Wind speed threshold","Wind speed threshold",,"Operational"
4680.00,"16","Synoptic feature sequences","316022","(Forecast data)",,"019004","Effective radius with respect to wind speeds above threshold","Effective radius with respect to wind speed above threshold",,"Operational"
4681.00,"16","Synoptic feature sequences","316030","(SIGMET header)",,"301014","Time period","Time period (for which SIGMET is valid)",,"Operational"
4682.00,"16","Synoptic feature sequences","316030","(SIGMET header)",,"001037","SIGMET sequence identifier","SIGMET sequence identifier",,"Operational"
4683.00,"16","Synoptic feature sequences","316030","(SIGMET header)",,"010064","SIGMET cruising level","SIGMET cruising level",,"Operational"
4684.00,"16","Synoptic feature sequences","316030","(SIGMET header)",,"008019","Qualifier for following centre identifier","Qualifier for location identifier, 1 = ATS unit serving FIR",,"Operational"
4685.00,"16","Synoptic feature sequences","316030","(SIGMET header)",,"001062","Short ICAO location indicator","Short ICAO location identifier",,"Operational"
4686.00,"16","Synoptic feature sequences","316030","(SIGMET header)",,"008019","Qualifier for following centre identifier","Qualifier for location identifier, 2 = FIR, 3 = UIR, 4 = CTA",,"Operational"
4687.00,"16","Synoptic feature sequences","316030","(SIGMET header)",,"001065","ICAO region identifier","ICAO region identifier",,"Operational"
4688.00,"16","Synoptic feature sequences","316030","(SIGMET header)",,"008019","Qualifier for following centre identifier","Qualifier for location identifier, 6 = MWO",,"Operational"
4689.00,"16","Synoptic feature sequences","316030","(SIGMET header)",,"001062","Short ICAO location indicator","Short ICAO location identifier",,"Operational"
4690.00,"16","Synoptic feature sequences","316030","(SIGMET header)",,"008019","Qualifier for following centre identifier","Qualifier for location identifier, Missing = Cancel",,"Operational"
4691.00,"16","Synoptic feature sequences","316031","(SIGMET, Observed or forecast location and motion)",,"008021","Time significance","Time significance, 16 = Analysis, 4 = Forecast",,"Operational"
4692.00,"16","Synoptic feature sequences","316031","(SIGMET, Observed or forecast location and motion)",,"301011",,"Year, month, day",,"Operational"
4693.00,"16","Synoptic feature sequences","316031","(SIGMET, Observed or forecast location and motion)",,"301012",,"Hour, minute",,"Operational"
4694.00,"16","Synoptic feature sequences","316031","(SIGMET, Observed or forecast location and motion)",,"301027","Description of a feature in 3-D or 2-D","Description of feature",,"Operational"
4695.00,"16","Synoptic feature sequences","316031","(SIGMET, Observed or forecast location and motion)",,"019005","Direction of motion of feature","Direction of motion",,"Operational"
4696.00,"16","Synoptic feature sequences","316031","(SIGMET, Observed or forecast location and motion)",,"019006","Speed of motion of feature","Speed of motion",,"Operational"
4697.00,"16","Synoptic feature sequences","316031","(SIGMET, Observed or forecast location and motion)",,"020028","Expected change in intensity","Expected change in intensity",,"Operational"
4698.00,"16","Synoptic feature sequences","316031","(SIGMET, Observed or forecast location and motion)",,"008021","Time significance","Time significance, Missing = Cancel",,"Operational"
4699.00,"16","Synoptic feature sequences","316032","(SIGMET, Forecast position)",,"008021","Time significance","Time significance, 4 = Forecast",,"Operational"
4700.00,"16","Synoptic feature sequences","316032","(SIGMET, Forecast position)",,"301011",,"Year, month, day",,"Operational"
4701.00,"16","Synoptic feature sequences","316032","(SIGMET, Forecast position)",,"301012",,"Hour, minute",,"Operational"
4702.00,"16","Synoptic feature sequences","316032","(SIGMET, Forecast position)",,"301027","Description of a feature in 3-D or 2-D","Description of feature",,"Operational"
4703.00,"16","Synoptic feature sequences","316032","(SIGMET, Forecast position)",,"008021","Time significance","Time significance, Missing = Cancel",,"Operational"
4704.00,"16","Synoptic feature sequences","316033","(SIGMET, Outlook)",,"008021","Time significance","Time significance, 4 = Forecast",,"Operational"
4705.00,"16","Synoptic feature sequences","316033","(SIGMET, Outlook)",,"301011",,"Year, month, day",,"Operational"
4706.00,"16","Synoptic feature sequences","316033","(SIGMET, Outlook)",,"301012",,"Hour, minute",,"Operational"
4707.00,"16","Synoptic feature sequences","316033","(SIGMET, Outlook)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
4708.00,"16","Synoptic feature sequences","316033","(SIGMET, Outlook)",,"031001","Delayed descriptor replication factor","Replication factor",,"Operational"
4709.00,"16","Synoptic feature sequences","316033","(SIGMET, Outlook)",,"301027","Description of a feature in 3-D or 2-D","Description of feature",,"Operational"
4710.00,"16","Synoptic feature sequences","316033","(SIGMET, Outlook)",,"008021","Time significance","Time significance, Missing = Cancel",,"Operational"
4711.00,"16","Synoptic feature sequences","316034","(Volcanic Ash SIGMET)",,"008079","Product status","Product status, 0 = Normal issue, 1 = Correction",,"Operational"
4712.00,"16","Synoptic feature sequences","316034","(Volcanic Ash SIGMET)",,"316030","SIGMET header","SIGMET header",,"Operational"
4713.00,"16","Synoptic feature sequences","316034","(Volcanic Ash SIGMET)",,"008011","Meteorological feature","Meteorological feature, 17 = Volcano",,"Operational"
4714.00,"16","Synoptic feature sequences","316034","(Volcanic Ash SIGMET)",,"001022","Name of feature","Name of feature",,"Operational"
4715.00,"16","Synoptic feature sequences","316034","(Volcanic Ash SIGMET)",,"008007","Dimensional significance","Dimensional significance, 0 = Point",,"Operational"
4716.00,"16","Synoptic feature sequences","316034","(Volcanic Ash SIGMET)",,"301023",,"Location",,"Operational"
4717.00,"16","Synoptic feature sequences","316034","(Volcanic Ash SIGMET)",,"008007","Dimensional significance","Dimensional significance, Missing = Cancel",,"Operational"
4718.00,"16","Synoptic feature sequences","316034","(Volcanic Ash SIGMET)",,"020090","Special clouds","Special clouds, 5 = Clouds from volcanic eruptions",,"Operational"
4719.00,"16","Synoptic feature sequences","316034","(Volcanic Ash SIGMET)",,"316031","SIGMET, Observed or forecast location and motion","SIGMET observed or forecast location and motion",,"Operational"
4720.00,"16","Synoptic feature sequences","316034","(Volcanic Ash SIGMET)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
4721.00,"16","Synoptic feature sequences","316034","(Volcanic Ash SIGMET)",,"031000","Short delayed descriptor replication factor","Short replication factor",,"Operational"
4722.00,"16","Synoptic feature sequences","316034","(Volcanic Ash SIGMET)",,"316032","SIGMET, Forecast position","SIGMET forecast position",,"Operational"
4723.00,"16","Synoptic feature sequences","316034","(Volcanic Ash SIGMET)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
4724.00,"16","Synoptic feature sequences","316034","(Volcanic Ash SIGMET)",,"031001","Delayed descriptor replication factor","Replication factor",,"Operational"
4725.00,"16","Synoptic feature sequences","316034","(Volcanic Ash SIGMET)",,"316033","SIGMET, Outlook","SIGMET outlook",,"Operational"
4726.00,"16","Synoptic feature sequences","316034","(Volcanic Ash SIGMET)",,"008011","Meteorological feature","Meteorological feature, Missing = Cancel",,"Operational"
4727.00,"16","Synoptic feature sequences","316034","(Volcanic Ash SIGMET)",,"008079","Product status","Product status, Missing = Cancel",,"Operational"
4728.00,"16","Synoptic feature sequences","316035","(Thunderstorm SIGMET)",,"008079","Product status","Product status, 0 = Normal issue, 1 = Correction",,"Operational"
4729.00,"16","Synoptic feature sequences","316035","(Thunderstorm SIGMET)",,"316030","SIGMET header","SIGMET header",,"Operational"
4730.00,"16","Synoptic feature sequences","316035","(Thunderstorm SIGMET)",,"008011","Meteorological feature","Meteorological feature, 21 = Thunderstorm",,"Operational"
4731.00,"16","Synoptic feature sequences","316035","(Thunderstorm SIGMET)",,"020023","Other weather phenomena","Other weather phenomena, bit 2 = Squalls or all 18 bits = Missing",,"Operational"
4732.00,"16","Synoptic feature sequences","316035","(Thunderstorm SIGMET)",,"020021","Type of precipitation","Type of precipitation, bit 14 = Hail or all 30 bits = Missing",,"Operational"
4733.00,"16","Synoptic feature sequences","316035","(Thunderstorm SIGMET)",,"020008","Cloud distribution for aviation","Cloud distribution 15 = OBSC, 16 = EMBD, 12 = FRQ, 31 = Missing",,"Operational"
4734.00,"16","Synoptic feature sequences","316035","(Thunderstorm SIGMET)",,"316031","SIGMET, Observed or forecast location and motion","SIGMET observed or forecast location and motion",,"Operational"
4735.00,"16","Synoptic feature sequences","316035","(Thunderstorm SIGMET)",,"008011","Meteorological feature","Meteorological feature, Missing = Cancel",,"Operational"
4736.00,"16","Synoptic feature sequences","316035","(Thunderstorm SIGMET)",,"008079","Product status","Product status, Missing = Cancel",,"Operational"
4737.00,"16","Synoptic feature sequences","316036","(Tropical cyclone SIGMET)",,"008079","Product status","Product status, 0 = Normal issue, 1 = Correction",,"Operational"
4738.00,"16","Synoptic feature sequences","316036","(Tropical cyclone SIGMET)",,"316030","SIGMET header","SIGMET header",,"Operational"
4739.00,"16","Synoptic feature sequences","316036","(Tropical cyclone SIGMET)",,"008011","Meteorological feature","Meteorological feature, 22 = Tropical cyclone",,"Operational"
4740.00,"16","Synoptic feature sequences","316036","(Tropical cyclone SIGMET)",,"001027","WMO long storm name","WMO long storm name",,"Operational"
4741.00,"16","Synoptic feature sequences","316036","(Tropical cyclone SIGMET)",,"316031","SIGMET, Observed or forecast location and motion","SIGMET observed or forecast location and motion",,"Operational"
4742.00,"16","Synoptic feature sequences","316036","(Tropical cyclone SIGMET)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
4743.00,"16","Synoptic feature sequences","316036","(Tropical cyclone SIGMET)",,"031000","Short delayed descriptor replication factor","Short replication factor",,"Operational"
4744.00,"16","Synoptic feature sequences","316036","(Tropical cyclone SIGMET)",,"316032","SIGMET, Forecast position","SIGMET forecast position",,"Operational"
4745.00,"16","Synoptic feature sequences","316036","(Tropical cyclone SIGMET)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
4746.00,"16","Synoptic feature sequences","316036","(Tropical cyclone SIGMET)",,"031001","Delayed descriptor replication factor","Replication factor",,"Operational"
4747.00,"16","Synoptic feature sequences","316036","(Tropical cyclone SIGMET)",,"316033","SIGMET, Outlook","SIGMET outlook",,"Operational"
4748.00,"16","Synoptic feature sequences","316036","(Tropical cyclone SIGMET)",,"008011","Meteorological feature","Meteorological feature, Missing = Cancel",,"Operational"
4749.00,"16","Synoptic feature sequences","316036","(Tropical cyclone SIGMET)",,"008079","Product status","Product status, Missing = Cancel",,"Operational"
4750.00,"16","Synoptic feature sequences","316037","(Turbulence SIGMET)",,"008079","Product status","Product status, 0 = Normal issue, 1 = Correction",,"Operational"
4751.00,"16","Synoptic feature sequences","316037","(Turbulence SIGMET)",,"316030","SIGMET header","SIGMET header",,"Operational"
4752.00,"16","Synoptic feature sequences","316037","(Turbulence SIGMET)",,"008011","Meteorological feature","Meteorological feature, 13 = Turbulence",,"Operational"
4753.00,"16","Synoptic feature sequences","316037","(Turbulence SIGMET)",,"011031","Degree of turbulence","Degree of turbulence, 10 = Moderate, 11 = Severe",,"Operational"
4754.00,"16","Synoptic feature sequences","316037","(Turbulence SIGMET)",,"316031","SIGMET, Observed or forecast location and motion","SIGMET observed or forecast location and motion",,"Operational"
4755.00,"16","Synoptic feature sequences","316037","(Turbulence SIGMET)",,"008011","Meteorological feature","Meteorological feature, Missing = Cancel",,"Operational"
4756.00,"16","Synoptic feature sequences","316037","(Turbulence SIGMET)",,"008079","Product status","Product status, Missing = Cancel",,"Operational"
4757.00,"16","Synoptic feature sequences","316038","(Icing SIGMET)",,"008079","Product status","Product status, 0 = Normal issue, 1 = Correction",,"Operational"
4758.00,"16","Synoptic feature sequences","316038","(Icing SIGMET)",,"316030","SIGMET header","SIGMET header",,"Operational"
4759.00,"16","Synoptic feature sequences","316038","(Icing SIGMET)",,"008011","Meteorological feature","Meteorological feature, 15 = Airframe icing",,"Operational"
4760.00,"16","Synoptic feature sequences","316038","(Icing SIGMET)",,"020041","Airframe icing","Airframe icing, 7 = Severe",,"Operational"
4761.00,"16","Synoptic feature sequences","316038","(Icing SIGMET)",,"020021","Type of precipitation","Type of precipitation, bit 3 = Liquid freezing or all 30 bits = Missing",,"Operational"
4762.00,"16","Synoptic feature sequences","316038","(Icing SIGMET)",,"316031","SIGMET, Observed or forecast location and motion","SIGMET observed or forecast location and motion",,"Operational"
4763.00,"16","Synoptic feature sequences","316038","(Icing SIGMET)",,"008011","Meteorological feature","Meteorological feature, Missing = Cancel",,"Operational"
4764.00,"16","Synoptic feature sequences","316038","(Icing SIGMET)",,"008079","Product status","Product status, Missing = Cancel",,"Operational"
4765.00,"16","Synoptic feature sequences","316039","(Mountain wave, duststorm or sandstorm SIGMET)",,"008079","Product status","Product status, 0 = Normal issue, 1 = Correction",,"Operational"
4766.00,"16","Synoptic feature sequences","316039","(Mountain wave, duststorm or sandstorm SIGMET)",,"316030","SIGMET header","SIGMET header",,"Operational"
4767.00,"16","Synoptic feature sequences","316039","(Mountain wave, duststorm or sandstorm SIGMET)",,"008011","Meteorological feature","Meteorological feature, 23 = Mountain wave, 24 = Duststorm, 25 = Sandstorm",,"Operational"
4768.00,"16","Synoptic feature sequences","316039","(Mountain wave, duststorm or sandstorm SIGMET)",,"020024","Intensity of phenomena","Intensity of phenomena, 3 = Heavy, 5 = Severe",,"Operational"
4769.00,"16","Synoptic feature sequences","316039","(Mountain wave, duststorm or sandstorm SIGMET)",,"316031","SIGMET, Observed or forecast location and motion","SIGMET observed or forecast location and motion",,"Operational"
4770.00,"16","Synoptic feature sequences","316039","(Mountain wave, duststorm or sandstorm SIGMET)",,"008011","Meteorological feature","Meteorological feature, Missing = Cancel",,"Operational"
4771.00,"16","Synoptic feature sequences","316039","(Mountain wave, duststorm or sandstorm SIGMET)",,"008079","Product status","Product status, Missing = Cancel",,"Operational"
4772.00,"16","Synoptic feature sequences","316040","(Cancellation of SIGMET)",,"316030","SIGMET header","SIGMET header",,"Operational"
4773.00,"16","Synoptic feature sequences","316040","(Cancellation of SIGMET)",,"008079","Product status","Product status, 4 = Cancellation",,"Operational"
4774.00,"16","Synoptic feature sequences","316040","(Cancellation of SIGMET)",,"301014","Time period","Time period (of the SIGMET to be cancelled)",,"Operational"
4775.00,"16","Synoptic feature sequences","316040","(Cancellation of SIGMET)",,"001037","SIGMET sequence identifier","SIGMET sequence identifier (of the SIGMET to be cancelled)",,"Operational"
4776.00,"16","Synoptic feature sequences","316040","(Cancellation of SIGMET)",,"010064","SIGMET cruising level","SIGMET cruising level (of the SIGMET to be cancelled)",,"Operational"
4777.00,"16","Synoptic feature sequences","316040","(Cancellation of SIGMET)",,"008079","Product status","Product status, Missing = Cancel",,"Operational"
4778.00,"16","Synoptic feature sequences","316050","(RADOB template - Part A: Information on tropical cyclone)",,"301001",,"WMO block and station number",,"Operational"
4779.00,"16","Synoptic feature sequences","316050","(RADOB template - Part A: Information on tropical cyclone)",,"301011",,"Date",,"Operational"
4780.00,"16","Synoptic feature sequences","316050","(RADOB template - Part A: Information on tropical cyclone)",,"301012",,"Time",,"Operational"
4781.00,"16","Synoptic feature sequences","316050","(RADOB template - Part A: Information on tropical cyclone)",,"002160","Wave length of the radar","Wave length of the radar",,"Operational"
4782.00,"16","Synoptic feature sequences","316050","(RADOB template - Part A: Information on tropical cyclone)",,"008005","Meteorological attribute significance","Meteorological attribute significance (= 1)",,"Operational"
4783.00,"16","Synoptic feature sequences","316050","(RADOB template - Part A: Information on tropical cyclone)",,"005002","Latitude (coarse accuracy)","Latitude (coarse accuracy)",,"Operational"
4784.00,"16","Synoptic feature sequences","316050","(RADOB template - Part A: Information on tropical cyclone)",,"006002","Longitude (coarse accuracy)","Longitude (coarse accuracy)",,"Operational"
4785.00,"16","Synoptic feature sequences","316050","(RADOB template - Part A: Information on tropical cyclone)",,"008005","Meteorological attribute significance","Cancel meteorological attribute significance",,"Operational"
4786.00,"16","Synoptic feature sequences","316050","(RADOB template - Part A: Information on tropical cyclone)",,"019100","Time interval to calculate the movement of the tropical cyclone","Time interval to calculate the movement of the tropical cyclone",,"Operational"
4787.00,"16","Synoptic feature sequences","316050","(RADOB template - Part A: Information on tropical cyclone)",,"019005","Direction of motion of feature","Direction of motion of feature",,"Operational"
4788.00,"16","Synoptic feature sequences","316050","(RADOB template - Part A: Information on tropical cyclone)",,"019006","Speed of motion of feature","Speed of motion of feature",,"Operational"
4789.00,"16","Synoptic feature sequences","316050","(RADOB template - Part A: Information on tropical cyclone)",,"019101","Accuracy of the position of the centre of the tropical cyclone","Accuracy of the position of the centre of the tropical cyclone",,"Operational"
4790.00,"16","Synoptic feature sequences","316050","(RADOB template - Part A: Information on tropical cyclone)",,"019102","Shape and definition of the eye of the tropical cyclone","Shape and definition of the eye of the tropical cyclone",,"Operational"
4791.00,"16","Synoptic feature sequences","316050","(RADOB template - Part A: Information on tropical cyclone)",,"019103","Diameter of major axis of the eye of the tropical cyclone","Diameter of major axis of the eye of the tropical cyclone",,"Operational"
4792.00,"16","Synoptic feature sequences","316050","(RADOB template - Part A: Information on tropical cyclone)",,"019104","Change in character of the eye during the 30 minutes","Change in character of the eye during the 30 minutes",,"Operational"
4793.00,"16","Synoptic feature sequences","316050","(RADOB template - Part A: Information on tropical cyclone)",,"019105","Distance between the end of spiral band and the centre","Distance between the end of spiral band and the centre",,"Operational"
4794.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"301005","Origin and identification sequence","Originating centre/sub-centre",,"Operational"
4795.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"301011",,"Date",,"Operational"
4796.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"301012",,"Time",,"Operational"
4797.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"001007","Satellite identifier","Satellite identifier",,"Operational"
4798.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"025150","Method of tropical cyclone intensity analysis using satellite data","Method of tropical cyclone intensity analysis using satellite data",,"Operational"
4799.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"122000","Replication descriptor","Delayed replication of 22 descriptors",,"Operational"
4800.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"031001","Delayed descriptor replication factor","Delayed descriptor replication factor",,"Operational"
4801.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"001027","WMO long storm name","WMO long storm name",,"Operational"
4802.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"019150","Typhoon International Common Number (Typhoon Committee)","Typhoon International Common Number (Typhoon Committee)",,"Operational"
4803.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"019106","Identification number of tropical cyclone","Identification number of tropical cyclone",,"Operational"
4804.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"008005","Meteorological attribute significance","Meteorological attribute significance (= 1)",,"Operational"
4805.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"005002","Latitude (coarse accuracy)","Latitude (coarse accuracy)",,"Operational"
4806.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"006002","Longitude (coarse accuracy)","Longitude (coarse accuracy)",,"Operational"
4807.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"008005","Meteorological attribute significance","Cancel meteorological attribute significance",,"Operational"
4808.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"019107","Time interval over which the movement of the tropical cyclone has been calculated","Time interval of the tropical cyclone analysis",,"Operational"
4809.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"019005","Direction of motion of feature","Direction of motion of feature",,"Operational"
4810.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"019006","Speed of motion of feature","Speed of motion of feature",,"Operational"
4811.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"019108","Accuracy of geographical position of the tropical cyclone","Accuracy of geographical position of the tropical cyclone",,"Operational"
4812.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"019109","Mean diameter of the overcast cloud of the tropical cyclone","Mean diameter of the overcast cloud of the tropical cyclone",,"Operational"
4813.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"019110","Apparent 24-hour change in intensity of the tropical cyclone","Apparent 24-hour change in intensity of the tropical cyclone",,"Operational"
4814.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"019111","Current Intensity (CI) number of the tropical cyclone","Current Intensity (CI) number of the tropical cyclone",,"Operational"
4815.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"019112","Data Tropical (DT) number of the tropical cyclone","Data Tropical (DT) number of the tropical cyclone",,"Operational"
4816.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"019113","Cloud pattern type of the DT-number","Cloud pattern type of the DT-number",,"Operational"
4817.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"019114","Model Expected Tropical (MET) number of the tropical cyclone","Model Expected Tropical (MET) number of the tropical cyclone",,"Operational"
4818.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"019115","Trend of the past 24-hour change (+: Developed, -: Weakened)","Trend of the past 24-hour change (+: Developed, -: Weakened)",,"Operational"
4819.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"019116","Pattern Tropical (PT) number of the tropical cyclone","Pattern Tropical (PT) number of the tropical cyclone",,"Operational"
4820.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"019117","Cloud picture type of the PT-number","Cloud picture type of the PT-number",,"Operational"
4821.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"019118","Final Tropical (T) number of the tropical cyclone","Final Tropical (T) number of the tropical cyclone",,"Operational"
4822.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"019119","Type of the final T-number","Type of the final T-number",,"Operational"
4823.00,"16","Synoptic feature sequences","316071","(Graphical AIRMET Sierra)",,"301014","Time period","Time period (for which AIRMET is valid)",,"Operational"
4824.00,"16","Synoptic feature sequences","316071","(Graphical AIRMET Sierra)",,"101000","Replication descriptor","Delayed replication",,"Operational"
4825.00,"16","Synoptic feature sequences","316071","(Graphical AIRMET Sierra)",,"031002","Extended delayed descriptor replication factor","Replication factor",,"Operational"
4826.00,"16","Synoptic feature sequences","316071","(Graphical AIRMET Sierra)",,"316075","GFA IFR Ceiling and Visibility","GFA IFR ceiling and visibility",,"Operational"
4827.00,"16","Synoptic feature sequences","316071","(Graphical AIRMET Sierra)",,"101000","Replication descriptor","Delayed replication",,"Operational"
4828.00,"16","Synoptic feature sequences","316071","(Graphical AIRMET Sierra)",,"031002","Extended delayed descriptor replication factor","Replication factor",,"Operational"
4829.00,"16","Synoptic feature sequences","316071","(Graphical AIRMET Sierra)",,"316076","GFA Mountain Obscuration","GFA mountain obscuration",,"Operational"
4830.00,"16","Synoptic feature sequences","316072","(Graphical AIRMET Tango)",,"301014","Time period","Time period (for which AIRMET is valid)",,"Operational"
4831.00,"16","Synoptic feature sequences","316072","(Graphical AIRMET Tango)",,"101000","Replication descriptor","Delayed replication",,"Operational"
4832.00,"16","Synoptic feature sequences","316072","(Graphical AIRMET Tango)",,"031002","Extended delayed descriptor replication factor","Replication factor",,"Operational"
4833.00,"16","Synoptic feature sequences","316072","(Graphical AIRMET Tango)",,"316077","GFA Turbulence","GFA turbulence",,"Operational"
4834.00,"16","Synoptic feature sequences","316072","(Graphical AIRMET Tango)",,"101000","Replication descriptor","Delayed replication",,"Operational"
4835.00,"16","Synoptic feature sequences","316072","(Graphical AIRMET Tango)",,"031002","Extended delayed descriptor replication factor","Replication factor",,"Operational"
4836.00,"16","Synoptic feature sequences","316072","(Graphical AIRMET Tango)",,"316078","GFA Strong Surface Wind","GFA strong surface wind",,"Operational"
4837.00,"16","Synoptic feature sequences","316072","(Graphical AIRMET Tango)",,"101000","Replication descriptor","Delayed replication",,"Operational"
4838.00,"16","Synoptic feature sequences","316072","(Graphical AIRMET Tango)",,"031002","Extended delayed descriptor replication factor","Replication factor",,"Operational"
4839.00,"16","Synoptic feature sequences","316072","(Graphical AIRMET Tango)",,"316079","GFA Low-Level Wind Shear","GFA low-level wind shear",,"Operational"
4840.00,"16","Synoptic feature sequences","316073","(Graphical AIRMET Zulu)",,"301014","Time period","Time period (for which AIRMET is valid)",,"Operational"
4841.00,"16","Synoptic feature sequences","316073","(Graphical AIRMET Zulu)",,"101000","Replication descriptor","Delayed replication",,"Operational"
4842.00,"16","Synoptic feature sequences","316073","(Graphical AIRMET Zulu)",,"031002","Extended delayed descriptor replication factor","Replication factor",,"Operational"
4843.00,"16","Synoptic feature sequences","316073","(Graphical AIRMET Zulu)",,"316080","GFA Icing","GFA icing",,"Operational"
4844.00,"16","Synoptic feature sequences","316073","(Graphical AIRMET Zulu)",,"101000","Replication descriptor","Delayed replication",,"Operational"
4845.00,"16","Synoptic feature sequences","316073","(Graphical AIRMET Zulu)",,"031002","Extended delayed descriptor replication factor","Replication factor",,"Operational"
4846.00,"16","Synoptic feature sequences","316073","(Graphical AIRMET Zulu)",,"316081","GFA Freezing Level","GFA freezing level",,"Operational"
4847.00,"16","Synoptic feature sequences","316074","(GFA identifier and observed/forecast location)",,"001039","Graphical Area Forecast (GFA) sequence identifier","GFA sequence identifier",,"Operational"
4848.00,"16","Synoptic feature sequences","316074","(GFA identifier and observed/forecast location)",,"008021","Time significance","Time significance, 4 = Forecast, 16 = Analysis",,"Operational"
4849.00,"16","Synoptic feature sequences","316074","(GFA identifier and observed/forecast location)",,"301014","Time period","Time period (for which hazard is being observed/forecast)",,"Operational"
4850.00,"16","Synoptic feature sequences","316074","(GFA identifier and observed/forecast location)",,"301027","Description of a feature in 3-D or 2-D","Description of feature",,"Operational"
4851.00,"16","Synoptic feature sequences","316074","(GFA identifier and observed/forecast location)",,"008021","Time significance","Time significance, Missing = Cancel",,"Operational"
4852.00,"16","Synoptic feature sequences","316075","(GFA IFR ceiling and visibility)",,"008079","Product status","Product status, 0 = Normal, 1 = COR, 2 = AMD, 3 = COR AMD, 4 = CNL",,"Operational"
4853.00,"16","Synoptic feature sequences","316075","(GFA IFR ceiling and visibility)",,"008041","Data significance","Data significance, 8 = IFR ceiling and visibility",,"Operational"
4854.00,"16","Synoptic feature sequences","316075","(GFA IFR ceiling and visibility)",,"316074","GFA Identifier and Observed/Forecast Location","GFA identifier and observed/forecast location",,"Operational"
4855.00,"16","Synoptic feature sequences","316075","(GFA IFR ceiling and visibility)",,"020006","Flight Rules","Flight rules, 1 = IFR",,"Operational"
4856.00,"16","Synoptic feature sequences","316075","(GFA IFR ceiling and visibility)",,"033042","Type of limit represented by following value","Type of limit represented by following (cloud base) value, 2 = Exclusive upper limit, 7 = Missing",,"Operational"
4857.00,"16","Synoptic feature sequences","316075","(GFA IFR ceiling and visibility)",,"020013","Height of base of cloud","Height of base of cloud",,"Operational"
4858.00,"16","Synoptic feature sequences","316075","(GFA IFR ceiling and visibility)",,"033042","Type of limit represented by following value","Type of limit represented by following (visibility) value, 2 = Exclusive upper limit, 7 = Missing",,"Operational"
4859.00,"16","Synoptic feature sequences","316075","(GFA IFR ceiling and visibility)",,"020001","Horizontal visibility","Horizontal visibility",,"Operational"
4860.00,"16","Synoptic feature sequences","316075","(GFA IFR ceiling and visibility)",,"020025","Obscuration","Obscuration",,"Operational"
4861.00,"16","Synoptic feature sequences","316075","(GFA IFR ceiling and visibility)",,"020026","Character of obscuration","Character of obscuration, 6 = Blowing, 15 = Missing",,"Operational"
4862.00,"16","Synoptic feature sequences","316075","(GFA IFR ceiling and visibility)",,"008041","Data significance","Data significance, Missing = Cancel",,"Operational"
4863.00,"16","Synoptic feature sequences","316075","(GFA IFR ceiling and visibility)",,"008079","Product status","Product status, Missing = Cancel",,"Operational"
4864.00,"16","Synoptic feature sequences","316076","(GFA mountain obscuration)",,"008079","Product status","Product status, 0 = Normal, 1 = COR, 2 = AMD, 3 = COR AMD, 4 = CNL",,"Operational"
4865.00,"16","Synoptic feature sequences","316076","(GFA mountain obscuration)",,"008041","Data significance","Data significance, 9 = Mountain obscuration",,"Operational"
4866.00,"16","Synoptic feature sequences","316076","(GFA mountain obscuration)",,"316074","GFA Identifier and Observed/Forecast Location","GFA identifier and observed/forecast location",,"Operational"
4867.00,"16","Synoptic feature sequences","316076","(GFA mountain obscuration)",,"020006","Flight Rules","Flight rules, 1 = IFR",,"Operational"
4868.00,"16","Synoptic feature sequences","316076","(GFA mountain obscuration)",,"020025","Obscuration","Obscuration",,"Operational"
4869.00,"16","Synoptic feature sequences","316076","(GFA mountain obscuration)",,"020026","Character of obscuration","Character of obscuration, 6 = Blowing, 15 = Missing",,"Operational"
4870.00,"16","Synoptic feature sequences","316076","(GFA mountain obscuration)",,"008041","Data significance","Data significance, Missing = Cancel",,"Operational"
4871.00,"16","Synoptic feature sequences","316076","(GFA mountain obscuration)",,"008079","Product status","Product status, Missing = Cancel",,"Operational"
4872.00,"16","Synoptic feature sequences","316077","(GFA turbulence)",,"008079","Product status","Product status, 0 = Normal, 1 = COR, 2 = AMD, 3 = COR AMD, 4 = CNL",,"Operational"
4873.00,"16","Synoptic feature sequences","316077","(GFA turbulence)",,"008011","Meteorological feature","Meteorological feature, 13 = Turbulence",,"Operational"
4874.00,"16","Synoptic feature sequences","316077","(GFA turbulence)",,"316074","GFA Identifier and Observed/Forecast Location","GFA identifier and observed/forecast location",,"Operational"
4875.00,"16","Synoptic feature sequences","316077","(GFA turbulence)",,"011031","Degree of turbulence","Degree of turbulence, 6 = Moderate",,"Operational"
4876.00,"16","Synoptic feature sequences","316077","(GFA turbulence)",,"008011","Meteorological feature","Meteorological feature, Missing = Cancel",,"Operational"
4877.00,"16","Synoptic feature sequences","316077","(GFA turbulence)",,"008079","Product status","Product status, Missing = Cancel",,"Operational"
4878.00,"16","Synoptic feature sequences","316078","(GFA strong surface wind)",,"008079","Product status","Product status, 0 = Normal, 1 = COR, 2 = AMD, 3 = COR AMD, 4 = CNL",,"Operational"
4879.00,"16","Synoptic feature sequences","316078","(GFA strong surface wind)",,"008041","Data significance","Data significance, 10 = Strong surface wind",,"Operational"
4880.00,"16","Synoptic feature sequences","316078","(GFA strong surface wind)",,"316074","GFA Identifier and Observed/Forecast Location","GFA identifier and observed/forecast location",,"Operational"
4881.00,"16","Synoptic feature sequences","316078","(GFA strong surface wind)",,"033042","Type of limit represented by following value","Type of limit represented by following (wind speed) value, 0 = Exclusive lower limit",,"Operational"
4882.00,"16","Synoptic feature sequences","316078","(GFA strong surface wind)",,"011012","Wind speed at 10 m","Wind speed at 10 m",,"Operational"
4883.00,"16","Synoptic feature sequences","316078","(GFA strong surface wind)",,"008041","Data significance","Data significance, Missing = Cancel",,"Operational"
4884.00,"16","Synoptic feature sequences","316078","(GFA strong surface wind)",,"008079","Product status","Product status, Missing = Cancel",,"Operational"
4885.00,"16","Synoptic feature sequences","316079","(GFA Low-Level Wind Shear)",,"008079","Product status","Product status, 0 = Normal, 1 = COR, 2 = AMD, 3 = COR AMD, 4 = CNL",,"Operational"
4886.00,"16","Synoptic feature sequences","316079","(GFA low-level wind shear)",,"008011","Meteorological feature","Meteorological feature, 16 = Phenomenon",,"Operational"
4887.00,"16","Synoptic feature sequences","316079","(GFA low-level wind shear)",,"316074","GFA Identifier and Observed/Forecast Location","GFA identifier and observed/forecast location",,"Operational"
4888.00,"16","Synoptic feature sequences","316079","(GFA low-level wind shear)",,"020023","Other weather phenomena","Other weather phenomena, bit 12 = Wind shear",,"Operational"
4889.00,"16","Synoptic feature sequences","316079","(GFA low-level wind shear)",,"020024","Intensity of phenomena","Intensity of phenomena",,"Operational"
4890.00,"16","Synoptic feature sequences","316079","(GFA low-level wind shear)",,"008011","Meteorological feature","Meteorological feature, Missing = Cancel",,"Operational"
4891.00,"16","Synoptic feature sequences","316079","(GFA low-level wind shear)",,"008079","Product status","Product status, Missing = Cancel",,"Operational"
4892.00,"16","Synoptic feature sequences","316080","(GFA icing)",,"008079","Product status","Product status, 0 = Normal, 1 = COR, 2 = AMD, 3 = COR AMD, 4 = CNL",,"Operational"
4893.00,"16","Synoptic feature sequences","316080","(GFA icing)",,"008011","Meteorological feature","Meteorological feature, 15 = Airframe icing",,"Operational"
4894.00,"16","Synoptic feature sequences","316080","(GFA icing)",,"316074","GFA Identifier and Observed/Forecast Location","GFA identifier and observed/forecast location",,"Operational"
4895.00,"16","Synoptic feature sequences","316080","(GFA icing)",,"020041","Airframe icing","Airframe icing, 4 = Moderate icing",,"Operational"
4896.00,"16","Synoptic feature sequences","316080","(GFA icing)",,"008011","Meteorological feature","Meteorological feature, Missing = Cancel",,"Operational"
4897.00,"16","Synoptic feature sequences","316080","(GFA icing)",,"008079","Product status","Product status, Missing = Cancel",,"Operational"
4898.00,"16","Synoptic feature sequences","316081","(GFA freezing level)",,"008079","Product status","Product status, 0 = Normal, 1 = COR, 2 = AMD, 3 = COR AMD, 4 = CNL",,"Operational"
4899.00,"16","Synoptic feature sequences","316081","(GFA freezing level)",,"008041","Data significance","Data significance, 11 = Freezing level, 12 = Multiple freezing level",,"Operational"
4900.00,"16","Synoptic feature sequences","316081","(GFA freezing level)",,"316074","GFA Identifier and Observed/Forecast Location","GFA identifier and observed/forecast location",,"Operational"
4901.00,"16","Synoptic feature sequences","316081","(GFA freezing level)",,"008041","Data significance","Data significance, Missing = Cancel",,"Operational"
4902.00,"16","Synoptic feature sequences","316081","(GFA freezing level)",,"008079","Product status","Product status, Missing = Cancel",,"Operational"
4903.00,"18","Radiological report sequences","318001",,,"301025",,"Latitude and longitude (coarse accuracy), day and time",,"Operational"
4904.00,"18","Radiological report sequences","318001",,,"024011","Dose","Dose",,"Operational"
4905.00,"18","Radiological report sequences","318003",,,"301026",,"Latitude and longitude (high accuracy), time periods in days, hours and minutes",,"Operational"
4906.00,"18","Radiological report sequences","318003",,,"024005","Isotope mass","Isotope mass",,"Operational"
4907.00,"18","Radiological report sequences","318003",,,"024004","Element name","Element name",,"Operational"
4908.00,"18","Radiological report sequences","318003",,,"024021","Air concentration (of named isotope type including gross beta)","Air concentration",,"Operational"
4909.00,"18","Radiological report sequences","318004",,,"301025",,"Latitude and longitude (coarse accuracy), day and time",,"Operational"
4910.00,"18","Radiological report sequences","318004",,,"004023","Time period or displacement","Time period or displacement",,"Operational"
4911.00,"18","Radiological report sequences","318004",,,"013011","Total precipitation/total water equivalent","Total precipitation/total water equivalent",,"Operational"
4912.00,"18","Radiological report sequences","318004",,,"024005","Isotope mass","Isotope mass",,"Operational"
4913.00,"18","Radiological report sequences","318004",,,"024004","Element name","Element name",,"Operational"
4914.00,"18","Radiological report sequences","318004",,,"024022","Concentration in precipitation (of names isotope type)","Concentration in precipitation",,"Operational"
4915.00,"21","Radar report sequences","321001","(Wind profiler - antenna characteristics)",,"002101","Type of antenna","Type of antenna",,"Operational"
4916.00,"21","Radar report sequences","321001","(Wind profiler - antenna characteristics)",,"002114","Antenna effective surface area","Antenna effective surface area",,"Operational"
4917.00,"21","Radar report sequences","321001","(Wind profiler - antenna characteristics)",,"002105","Maximum antenna gain","Maximum antenna gain",,"Operational"
4918.00,"21","Radar report sequences","321001","(Wind profiler - antenna characteristics)",,"002106","3-dB beamwidth","3-dB beamwidth",,"Operational"
4919.00,"21","Radar report sequences","321001","(Wind profiler - antenna characteristics)",,"002107","Sidelobe suppression","Sidelobe suppression",,"Operational"
4920.00,"21","Radar report sequences","321001","(Wind profiler - antenna characteristics)",,"002121","Mean frequency","Mean frequency",,"Operational"
4921.00,"21","Radar report sequences","321003","(Wind profiler - moment data)",,"021051","Signal power above 1 mW","Signal power above 1 mW",,"Operational"
4922.00,"21","Radar report sequences","321003","(Wind profiler - moment data)",,"021014","Doppler mean velocity (radial)","Doppler mean velocity (radial)",,"Operational"
4923.00,"21","Radar report sequences","321003","(Wind profiler - moment data)",,"021017","Doppler velocity spectral width","Doppler velocity spectral width",,"Operational"
4924.00,"21","Radar report sequences","321003","(Wind profiler - moment data)",,"021030","Signal to noise ratio","Signal to noise ratio",,"Operational"
4925.00,"21","Radar report sequences","321004","(Wind profiler - moment data sounding)",,"301031",,"Identification, type, date/time, position (high accuracy), height",,"Operational"
4926.00,"21","Radar report sequences","321004","(Wind profiler - moment data sounding)",,"002003","Type of measuring equipment used","Type of measuring equipment used",,"Operational"
4927.00,"21","Radar report sequences","321004","(Wind profiler - moment data sounding)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
4928.00,"21","Radar report sequences","321004","(Wind profiler - moment data sounding)",,"031001","Delayed descriptor replication factor","Replication factor",,"Operational"
4929.00,"21","Radar report sequences","321004","(Wind profiler - moment data sounding)",,"321003","Wind profiler - moment data","Wind profiler - moment data",,"Operational"
4930.00,"21","Radar report sequences","321005","(Transmitter-receiver characteristics)",,"025004","Echo processing","Echo processing",,"Operational"
4931.00,"21","Radar report sequences","321005","(Transmitter-receiver characteristics)",,"002121","Mean frequency","Mean frequency",,"Operational"
4932.00,"21","Radar report sequences","321005","(Transmitter-receiver characteristics)",,"002122","Frequency agility range","Frequency agility range",,"Operational"
4933.00,"21","Radar report sequences","321005","(Transmitter-receiver characteristics)",,"002123","Peak power","Peak power",,"Operational"
4934.00,"21","Radar report sequences","321005","(Transmitter-receiver characteristics)",,"002124","Average power","Average power",,"Operational"
4935.00,"21","Radar report sequences","321005","(Transmitter-receiver characteristics)",,"002125","Pulse repetition frequency","Pulse repetition frequency",,"Operational"
4936.00,"21","Radar report sequences","321005","(Transmitter-receiver characteristics)",,"002126","Pulse width","Pulse width",,"Operational"
4937.00,"21","Radar report sequences","321005","(Transmitter-receiver characteristics)",,"002127","Receiver intermediate frequency","Receiver intermediate frequency",,"Operational"
4938.00,"21","Radar report sequences","321005","(Transmitter-receiver characteristics)",,"002128","Intermediate frequency bandwidth","Intermediate frequency bandwidth",,"Operational"
4939.00,"21","Radar report sequences","321005","(Transmitter-receiver characteristics)",,"002129","Minimum detectable signal","Minimum detectable signal",,"Operational"
4940.00,"21","Radar report sequences","321005","(Transmitter-receiver characteristics)",,"002130","Dynamic range","Dynamic range",,"Operational"
4941.00,"21","Radar report sequences","321005","(Transmitter-receiver characteristics)",,"002131","Sensitivity time control (STC)","Sensitivity time control",,"Operational"
4942.00,"21","Radar report sequences","321006","(Integration characteristics)",,"025001","Range-gate length","Range-gate length",,"Operational"
4943.00,"21","Radar report sequences","321006","(Integration characteristics)",,"025002","Number of gates averaged","Number of gates averaged",,"Operational"
4944.00,"21","Radar report sequences","321006","(Integration characteristics)",,"025003","Number of integrated pulses","Number of integrated pulses",,"Operational"
4945.00,"21","Radar report sequences","321006","(Integration characteristics)",,"025005","Echo integration","Echo integration",,"Operational"
4946.00,"21","Radar report sequences","321007","(Corrections)",,"025009","Calibration method","Calibration method",,"Operational"
4947.00,"21","Radar report sequences","321007","(Corrections)",,"025010","Clutter treatment","Clutter treatment",,"Operational"
4948.00,"21","Radar report sequences","321007","(Corrections)",,"025011","Ground occultation correction (screening)","Ground occultation correction",,"Operational"
4949.00,"21","Radar report sequences","321007","(Corrections)",,"025012","Range attenuation correction","Range attenuation correction",,"Operational"
4950.00,"21","Radar report sequences","321007","(Corrections)",,"025013","Bright-band correction","Bright-band correction",,"Operational"
4951.00,"21","Radar report sequences","321007","(Corrections)",,"025015","Radome attenuation correction","Radome attenuation correction",,"Operational"
4952.00,"21","Radar report sequences","321007","(Corrections)",,"025016","Clear-air attenuation correction","Clear-air attenuation correction",,"Operational"
4953.00,"21","Radar report sequences","321007","(Corrections)",,"025017","Precipitation attenuation correction","Precipitation attenuation correction",,"Operational"
4954.00,"21","Radar report sequences","321008","(Z to R conversion)",,"025006","Z to R conversion","Z to R conversion",,"Operational"
4955.00,"21","Radar report sequences","321008","(Z to R conversion)",,"025007","Z to R conversion factor","Z to R conversion factor",,"Operational"
4956.00,"21","Radar report sequences","321008","(Z to R conversion)",,"025008","Z to R conversion exponent","Z to R conversion exponent",,"Operational"
4957.00,"21","Radar report sequences","321009","(A to Z law)",,"025018","A to Z law for attenuation factor","A to Z law for attenuation factor",,"Operational"
4958.00,"21","Radar report sequences","321009","(A to Z law)",,"025019","A to Z law for attenuation exponent","A to Z law for attenuation exponent",,"Operational"
4959.00,"21","Radar report sequences","321010","(Antenna characteristics)",,"002101","Type of antenna","Type of antenna",,"Operational"
4960.00,"21","Radar report sequences","321010","(Antenna characteristics)",,"007002","Height or altitude","Altitude of the tower base",,"Operational"
4961.00,"21","Radar report sequences","321010","(Antenna characteristics)",,"002102","Antenna height above tower base","Antenna height above tower base",,"Operational"
4962.00,"21","Radar report sequences","321010","(Antenna characteristics)",,"002103","Radome","Radome",,"Operational"
4963.00,"21","Radar report sequences","321010","(Antenna characteristics)",,"002104","Antenna polarization","Antenna polarization",,"Operational"
4964.00,"21","Radar report sequences","321010","(Antenna characteristics)",,"002105","Maximum antenna gain","Maximum antenna gain",,"Operational"
4965.00,"21","Radar report sequences","321010","(Antenna characteristics)",,"002106","3-dB beamwidth","3-dB beamwidth",,"Operational"
4966.00,"21","Radar report sequences","321010","(Antenna characteristics)",,"002107","Sidelobe suppression","Sidelobe suppression",,"Operational"
4967.00,"21","Radar report sequences","321010","(Antenna characteristics)",,"002108","Crosspol discrimination (on axis)","Crosspol discrimination (on axis)",,"Operational"
4968.00,"21","Radar report sequences","321010","(Antenna characteristics)",,"002109","Antenna speed (azimuth)","Antenna speed (azimuth)",,"Operational"
4969.00,"21","Radar report sequences","321010","(Antenna characteristics)",,"002110","Antenna speed (elevation)","Antenna speed (elevation)",,"Operational"
4970.00,"21","Radar report sequences","321010","(Antenna characteristics)",,"002132","Azimuth pointing accuracy","Azimuth pointing accuracy",,"Operational"
4971.00,"21","Radar report sequences","321010","(Antenna characteristics)",,"002133","Elevation pointing accuracy","Elevation pointing accuracy",,"Operational"
4972.00,"21","Radar report sequences","321011","(General characteristics)",,"030031","Picture type","Picture type",,"Operational"
4973.00,"21","Radar report sequences","321011","(General characteristics)",,"030032","Combination with other data","Combination with other data",,"Operational"
4974.00,"21","Radar report sequences","321011","(General characteristics)",,"029002","Co-ordinate grid type","Coordinate grid type",,"Operational"
4975.00,"21","Radar report sequences","321012","(Antenna elevations)",,"101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
4976.00,"21","Radar report sequences","321012","(Antenna elevations)",,"031001","Delayed descriptor replication factor","Replication factor",,"Operational"
4977.00,"21","Radar report sequences","321012","(Antenna elevations)",,"002135","Antenna elevation","Antenna elevation",,"Operational"
4978.00,"21","Radar report sequences","321021","(Basic information (system/site header) on wind profiler/RASS)",,"002003","Type of measuring equipment used","Type of measuring equipment used",,"Operational"
4979.00,"21","Radar report sequences","321021","(Basic information (system/site header) on wind profiler/RASS)",,"002101","Type of antenna","Type of antenna",,"Operational"
4980.00,"21","Radar report sequences","321021","(Basic information (system/site header) on wind profiler/RASS)",,"201130","Change data width","Change width to 8 bits",,"Operational"
4981.00,"21","Radar report sequences","321021","(Basic information (system/site header) on wind profiler/RASS)",,"002106","3-dB beamwidth","3-dB beamwidth",,"Operational"
4982.00,"21","Radar report sequences","321021","(Basic information (system/site header) on wind profiler/RASS)",,"201000","Change data width","Change width back to table B",,"Operational"
4983.00,"21","Radar report sequences","321021","(Basic information (system/site header) on wind profiler/RASS)",,"201132","Change data width","Change width to 11 bits",,"Operational"
4984.00,"21","Radar report sequences","321021","(Basic information (system/site header) on wind profiler/RASS)",,"202130","Change scale","Change scale to -6",,"Operational"
4985.00,"21","Radar report sequences","321021","(Basic information (system/site header) on wind profiler/RASS)",,"002121","Mean frequency","Mean frequency",,"Operational"
4986.00,"21","Radar report sequences","321021","(Basic information (system/site header) on wind profiler/RASS)",,"202000","Change scale","Change scale back to table B",,"Operational"
4987.00,"21","Radar report sequences","321021","(Basic information (system/site header) on wind profiler/RASS)",,"201000","Change data width","Change width back to table B",,"Operational"
4988.00,"21","Radar report sequences","321021","(Basic information (system/site header) on wind profiler/RASS)",,"201133","Change data width","Change width to 11 bits",,"Operational"
4989.00,"21","Radar report sequences","321021","(Basic information (system/site header) on wind profiler/RASS)",,"202129","Change scale","Change scale to 0",,"Operational"
4990.00,"21","Radar report sequences","321021","(Basic information (system/site header) on wind profiler/RASS)",,"025001","Range-gate length","Range-gate length",,"Operational"
4991.00,"21","Radar report sequences","321021","(Basic information (system/site header) on wind profiler/RASS)",,"202000","Change scale","Change scale back to table B",,"Operational"
4992.00,"21","Radar report sequences","321021","(Basic information (system/site header) on wind profiler/RASS)",,"201000","Change data width","Change width back to table B",,"Operational"
4993.00,"21","Radar report sequences","321022","(Wind profiler: processed-data winds)",,"007007","Height","Height",,"Operational"
4994.00,"21","Radar report sequences","321022","(Wind profiler: processed-data winds)",,"204001","Add associated field","Add associated field of 1 bit in length",,"Operational"
4995.00,"21","Radar report sequences","321022","(Wind profiler: processed-data winds)",,"031021","Associated field significance","Associated field significance",,"Operational"
4996.00,"21","Radar report sequences","321022","(Wind profiler: processed-data winds)",,"011001","Wind direction","Wind direction",,"Operational"
4997.00,"21","Radar report sequences","321022","(Wind profiler: processed-data winds)",,"204000","Add associated field","Cancel add associated field",,"Operational"
4998.00,"21","Radar report sequences","321022","(Wind profiler: processed-data winds)",,"011002","Wind speed","Wind speed",,"Operational"
4999.00,"21","Radar report sequences","321022","(Wind profiler: processed-data winds)",,"204001","Add associated field","Add associated field of 1 bit in length",,"Operational"
5000.00,"21","Radar report sequences","321022","(Wind profiler: processed-data winds)",,"031021","Associated field significance","Associated field significance",,"Operational"
5001.00,"21","Radar report sequences","321022","(Wind profiler: processed-data winds)",,"011006","w-component","w-component",,"Operational"
5002.00,"21","Radar report sequences","321022","(Wind profiler: processed-data winds)",,"204000","Add associated field","Cancel add associated field",,"Operational"
5003.00,"21","Radar report sequences","321022","(Wind profiler: processed-data winds)",,"021030","Signal to noise ratio","Signal to noise ratio",,"Operational"
5004.00,"21","Radar report sequences","321023","(Wind profiler: raw-data winds)",,"007007","Height","Height",,"Operational"
5005.00,"21","Radar report sequences","321023","(Wind profiler: raw-data winds)",,"021091","Radar signal Doppler spectrum 0th moment","Radar signal Doppler spectrum 0th moment",,"Operational"
5006.00,"21","Radar report sequences","321023","(Wind profiler: raw-data winds)",,"021030","Signal to noise ratio","Signal to noise ratio",,"Operational"
5007.00,"21","Radar report sequences","321023","(Wind profiler: raw-data winds)",,"202129","Change scale","Change scale to 2",,"Operational"
5008.00,"21","Radar report sequences","321023","(Wind profiler: raw-data winds)",,"021014","Doppler mean velocity (radial)","Doppler mean velocity (radial)",,"Operational"
5009.00,"21","Radar report sequences","321023","(Wind profiler: raw-data winds)",,"201129","Change data width","Change width to 9 bits",,"Operational"
5010.00,"21","Radar report sequences","321023","(Wind profiler: raw-data winds)",,"021017","Doppler velocity spectral width","Doppler velocity spectral width",,"Operational"
5011.00,"21","Radar report sequences","321023","(Wind profiler: raw-data winds)",,"202000","Change scale","Change scale back to table B",,"Operational"
5012.00,"21","Radar report sequences","321023","(Wind profiler: raw-data winds)",,"201000","Change data width","Change width back to table B",,"Operational"
5013.00,"21","Radar report sequences","321024","(RASS-mode: processed-data RASS)",,"007007","Height","Height",,"Operational"
5014.00,"21","Radar report sequences","321024","(RASS-mode: processed-data RASS)",,"204001","Add associated field","Add associated field of 1 bit in length",,"Operational"
5015.00,"21","Radar report sequences","321024","(RASS-mode: processed-data RASS)",,"031021","Associated field significance","Associated field significance",,"Operational"
5016.00,"21","Radar report sequences","321024","(RASS-mode: processed-data RASS)",,"012007","Virtual temperature","Virtual temperature",,"Operational"
5017.00,"21","Radar report sequences","321024","(RASS-mode: processed-data RASS)",,"011006","w-component","w-component",,"Operational"
5018.00,"21","Radar report sequences","321024","(RASS-mode: processed-data RASS)",,"204000","Add associated field","Cancel add associated field",,"Operational"
5019.00,"21","Radar report sequences","321024","(RASS-mode: processed-data RASS)",,"021030","Signal to noise ratio","Signal to noise ratio",,"Operational"
5020.00,"21","Radar report sequences","321025","(RASS-mode: raw-data RASS)",,"007007","Height","Height",,"Operational"
5021.00,"21","Radar report sequences","321025","(RASS-mode: raw-data RASS)",,"021091","Radar signal Doppler spectrum 0th moment","Radar signal Doppler spectrum 0th moment",,"Operational"
5022.00,"21","Radar report sequences","321025","(RASS-mode: raw-data RASS)",,"021030","Signal to noise ratio","Signal to noise ratio",,"Operational"
5023.00,"21","Radar report sequences","321025","(RASS-mode: raw-data RASS)",,"202129","Change scale","Change scale to 2",,"Operational"
5024.00,"21","Radar report sequences","321025","(RASS-mode: raw-data RASS)",,"021014","Doppler mean velocity (radial)","Doppler mean velocity (radial)",,"Operational"
5025.00,"21","Radar report sequences","321025","(RASS-mode: raw-data RASS)",,"201129","Change data width","Change width to 9 bits",,"Operational"
5026.00,"21","Radar report sequences","321025","(RASS-mode: raw-data RASS)",,"021017","Doppler velocity spectral width","Doppler velocity spectral width",,"Operational"
5027.00,"21","Radar report sequences","321025","(RASS-mode: raw-data RASS)",,"202000","Change scale","Change scale back to table B",,"Operational"
5028.00,"21","Radar report sequences","321025","(RASS-mode: raw-data RASS)",,"201000","Change data width","Change width back to table B",,"Operational"
5029.00,"21","Radar report sequences","321025","(RASS-mode: raw-data RASS)",,"021092","RASS signal Doppler spectrum 0th moment, referring to RASS signal","RASS signal Doppler spectrum 0th moment, referring to RASS signal",,"Operational"
5030.00,"21","Radar report sequences","321025","(RASS-mode: raw-data RASS)",,"021030","Signal to noise ratio","Signal to noise ratio, referring to RASS signal",,"Operational"
5031.00,"21","Radar report sequences","321025","(RASS-mode: raw-data RASS)",,"025092","Acoustic propagation velocity","Acoustic propagation velocity",,"Operational"
5032.00,"21","Radar report sequences","321025","(RASS-mode: raw-data RASS)",,"201129","Change data width","Change width to 9 bits",,"Operational"
5033.00,"21","Radar report sequences","321025","(RASS-mode: raw-data RASS)",,"202129","Change scale","Change scale to 2",,"Operational"
5034.00,"21","Radar report sequences","321025","(RASS-mode: raw-data RASS)",,"021017","Doppler velocity spectral width","Doppler velocity spectral width, referring to RASS signal",,"Operational"
5035.00,"21","Radar report sequences","321025","(RASS-mode: raw-data RASS)",,"202000","Change scale","Change scale back to table B",,"Operational"
5036.00,"21","Radar report sequences","321025","(RASS-mode: raw-data RASS)",,"201000","Change data width","Change width back to table B",,"Operational"
5037.00,"21","Radar report sequences","321026","(RASS data - fluxes)",,"007007","Height","Height",,"Operational"
5038.00,"21","Radar report sequences","321026","(RASS data - fluxes)",,"204001","Add associated field","Add associated field of 1 bit in length",,"Operational"
5039.00,"21","Radar report sequences","321026","(RASS data - fluxes)",,"031021","Associated field significance","Associated field significance",,"Operational"
5040.00,"21","Radar report sequences","321026","(RASS data - fluxes)",,"012007","Virtual temperature","Virtual temperature",,"Operational"
5041.00,"21","Radar report sequences","321026","(RASS data - fluxes)",,"025091","Structure constant of the refraction index (Cn2)","Structure constant of the refraction index (Cn**2)",,"Operational"
5042.00,"21","Radar report sequences","321026","(RASS data - fluxes)",,"011071","Turbulent vertical momentum flux","Turbulent vertical momentum flux",,"Operational"
5043.00,"21","Radar report sequences","321026","(RASS data - fluxes)",,"011072","Turbulent vertical buoyancy flux","Turbulent vertical buoyancy flux",,"Operational"
5044.00,"21","Radar report sequences","321026","(RASS data - fluxes)",,"011073","Turbulent kinetic energy","Turbulent kinetic energy",,"Operational"
5045.00,"21","Radar report sequences","321026","(RASS data - fluxes)",,"011074","Dissipation energy","Dissipation energy",,"Operational"
5046.00,"21","Radar report sequences","321026","(RASS data - fluxes)",,"204000","Add associated field","Cancel add associated field",,"Operational"
5047.00,"21","Radar report sequences","321027",,,"021118","Attenuation correction on sigma-0","Attenuation correction on sigma-0",,"Operational"
5048.00,"21","Radar report sequences","321027",,,"202129","Change scale","Change scale",,"Operational"
5049.00,"21","Radar report sequences","321027",,,"201132","Change data width","Change data width",,"Operational"
5050.00,"21","Radar report sequences","321027",,,"002112","Radar look angle","Radar look angle",,"Operational"
5051.00,"21","Radar report sequences","321027",,,"201000","Change data width","Change data width back to Table B",,"Operational"
5052.00,"21","Radar report sequences","321027",,,"201131","Change data width","Change data width",,"Operational"
5053.00,"21","Radar report sequences","321027",,,"002111","Radar incidence angle","Radar incidence angle",,"Operational"
5054.00,"21","Radar report sequences","321027",,,"201000","Change data width","Change data width back to Table B",,"Operational"
5055.00,"21","Radar report sequences","321027",,,"202000","Change scale","Change scale back to Table B",,"Operational"
5056.00,"21","Radar report sequences","321027",,,"002104","Antenna polarization","Antenna polarization",,"Operational"
5057.00,"21","Radar report sequences","321027",,,"021105","Normalized radar cross-section","Normalized radar cross-section",,"Operational"
5058.00,"21","Radar report sequences","321027",,,"021106","Kp variance coefficient (alpha)","Kp variance coefficient (alpha)",,"Operational"
5059.00,"21","Radar report sequences","321027",,,"021107","Kp variance coefficient (beta)","Kp variance coefficient (beta)",,"Operational"
5060.00,"21","Radar report sequences","321027",,,"021114","Kp variance coefficent (gamma)","Kp variance coefficient (gamma)",,"Operational"
5061.00,"21","Radar report sequences","321027",,,"021115","SEAWINDS sigma-0 quality","SEAWINDS sigma-0 quality",,"Operational"
5062.00,"21","Radar report sequences","321027",,,"021116","SEAWINDS sigma-0 mode","SEAWINDS sigma-0 mode",,"Operational"
5063.00,"21","Radar report sequences","321027",,,"008018","SEAWINDS land/ice surface type","SEAWINDS land/ice surface type",,"Operational"
5064.00,"21","Radar report sequences","321027",,,"021117","Sigma-0 variance quality control","Sigma-0 variance quality control",,"Operational"
5065.00,"21","Radar report sequences","321028",,,"021118","Attenuation correction on sigma-0","Attenuation correction on sigma-0",,"Operational"
5066.00,"21","Radar report sequences","321028",,,"202129","Change scale","Change scale",,"Operational"
5067.00,"21","Radar report sequences","321028",,,"201132","Change data width","Change data width",,"Operational"
5068.00,"21","Radar report sequences","321028",,,"002112","Radar look angle","Radar look angle",,"Operational"
5069.00,"21","Radar report sequences","321028",,,"201000","Change data width","Change data width back to Table B",,"Operational"
5070.00,"21","Radar report sequences","321028",,,"201131","Change data width","Change data width",,"Operational"
5071.00,"21","Radar report sequences","321028",,,"002111","Radar incidence angle","Radar incidence angle",,"Operational"
5072.00,"21","Radar report sequences","321028",,,"201000","Change data width","Change data width back to Table B",,"Operational"
5073.00,"21","Radar report sequences","321028",,,"202000","Change scale","Change scale back to table B",,"Operational"
5074.00,"21","Radar report sequences","321028",,,"002104","Antenna polarization","Antenna polarization",,"Operational"
5075.00,"21","Radar report sequences","321028",,,"021123","SEAWINDS normalized radar cross-section","SEAWINDS normalized radar cross-section",,"Operational"
5076.00,"21","Radar report sequences","321028",,,"021106","Kp variance coefficient (alpha)","Kp variance coefficient (alpha)",,"Operational"
5077.00,"21","Radar report sequences","321028",,,"021107","Kp variance coefficient (beta)","Kp variance coefficient (beta)",,"Operational"
5078.00,"21","Radar report sequences","321028",,,"021114","Kp variance coefficent (gamma)","Kp variance coefficient (gamma)",,"Operational"
5079.00,"21","Radar report sequences","321028",,,"021115","SEAWINDS sigma-0 quality","SEAWINDS sigma-0 quality flag",,"Operational"
5080.00,"21","Radar report sequences","321028",,,"021116","SEAWINDS sigma-0 mode","SEAWINDS sigma-0 mode flag",,"Operational"
5081.00,"21","Radar report sequences","321028",,,"008018","SEAWINDS land/ice surface type","SEAWINDS land/ice surface flag",,"Operational"
5082.00,"21","Radar report sequences","321028",,,"021117","Sigma-0 variance quality control","Sigma-0 variance quality control",,"Operational"
5083.00,"21","Radar report sequences","321030","(ASCAT sigma-0 information)",,"008085","Beam identifier","Beam identifier",,"Operational"
5084.00,"21","Radar report sequences","321030","(ASCAT sigma-0 information)",,"202129","Change scale","Increase scaling by 10**1",,"Operational"
5085.00,"21","Radar report sequences","321030","(ASCAT sigma-0 information)",,"201131","Change data width","Increase data width by 3 bits",,"Operational"
5086.00,"21","Radar report sequences","321030","(ASCAT sigma-0 information)",,"002111","Radar incidence angle","Radar incidence angle",,"Operational"
5087.00,"21","Radar report sequences","321030","(ASCAT sigma-0 information)",,"201000","Change data width","Cancel change data width",,"Operational"
5088.00,"21","Radar report sequences","321030","(ASCAT sigma-0 information)",,"202000","Change scale","Cancel change scaling",,"Operational"
5089.00,"21","Radar report sequences","321030","(ASCAT sigma-0 information)",,"002134","Antenna beam azimuth","Antenna beam azimuth",,"Operational"
5090.00,"21","Radar report sequences","321030","(ASCAT sigma-0 information)",,"021062","Backscatter","Backscatter",,"Operational"
5091.00,"21","Radar report sequences","321030","(ASCAT sigma-0 information)",,"021063","Radiometric resolution (noise value)","Radiometric resolution (noise value)",,"Operational"
5092.00,"21","Radar report sequences","321030","(ASCAT sigma-0 information)",,"021158","ASCAT kp estimate quality","ASCAT Kp estimate quality",,"Operational"
5093.00,"21","Radar report sequences","321030","(ASCAT sigma-0 information)",,"021159","ASCAT sigma-0 usability","ASCAT sigma-0 usability",,"Operational"
5094.00,"21","Radar report sequences","321030","(ASCAT sigma-0 information)",,"021160","ASCAT use of synthetic data","ASCAT synthetic data quality",,"Operational"
5095.00,"21","Radar report sequences","321030","(ASCAT sigma-0 information)",,"021161","ASCAT synthetic data quality","ASCAT synthetic data quantity",,"Operational"
5096.00,"21","Radar report sequences","321030","(ASCAT sigma-0 information)",,"021162","ASCAT satellite orbit and attitude quality","ASCAT satellite orbit and attitude quality",,"Operational"
5097.00,"21","Radar report sequences","321030","(ASCAT sigma-0 information)",,"021163","ASCAT solar array reflection contamination","ASCAT solar array reflection contamination",,"Operational"
5098.00,"21","Radar report sequences","321030","(ASCAT sigma-0 information)",,"021164","ASCAT telemetry presence and quality","ASCAT telemetry presence and quality",,"Operational"
5099.00,"21","Radar report sequences","321030","(ASCAT sigma-0 information)",,"021165","ASCAT extrapolated reference function presence","ASCAT extrapolated reference function",,"Operational"
5100.00,"21","Radar report sequences","321030","(ASCAT sigma-0 information)",,"021166","Land fraction","Land fraction",,"Operational"
5101.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"001007","Satellite identifier","Satellite identifier",,"Operational"
5102.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"002019","Satellite instruments","Satellite instruments",,"Operational"
5103.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"004001","Year","Year",,"Operational"
5104.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"004002","Month","Month",,"Operational"
5105.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"004003","Day","Day",,"Operational"
5106.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"004004","Hour","Hour",,"Operational"
5107.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"004005","Minute","Minute",,"Operational"
5108.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"004006","Second","Second",,"Operational"
5109.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"005001","Latitude (high accuracy)","Latitude (high accuracy)",,"Operational"
5110.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"006001","Longitude (high accuracy)","Longitude (high accuracy)",,"Operational"
5111.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"027001","Latitude (high accuracy)","Latitude (high accuracy)",,"Operational"
5112.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"028001","Longitude (high accuracy)","Longitude (high accuracy)",,"Operational"
5113.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"027001","Latitude (high accuracy)","Latitude (high accuracy)",,"Operational"
5114.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"028001","Longitude (high accuracy)","Longitude (high accuracy)",,"Operational"
5115.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"027001","Latitude (high accuracy)","Latitude (high accuracy)",,"Operational"
5116.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"028001","Longitude (high accuracy)","Longitude (high accuracy)",,"Operational"
5117.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"027001","Latitude (high accuracy)","Latitude (high accuracy)",,"Operational"
5118.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"028001","Longitude (high accuracy)","Longitude (high accuracy)",,"Operational"
5119.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"010001","Height of land surface","Height of land surface",,"Operational"
5120.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"014019","Surface albedo","Surface albedo",,"Operational"
5121.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"007025","Solar zenith angle","Solar zenith angle",,"Operational"
5122.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"010080","Viewing Zenith angle","Viewing zenith angle",,"Operational"
5123.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"005023","Sun to satellite azimuth difference","Sun to satellite azimuth difference",,"Operational"
5124.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"020010","Cloud cover (total)","Cloud cover (total)",,"Operational"
5125.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"008003","Vertical significance (satellite observations)","Vertical significance (satellite observations)",,"Operational"
5126.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"007004","Pressure","Pressure",,"Operational"
5127.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"014026","Albedo at the top of clouds","Albedo at the top of clouds",,"Operational"
5128.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"020014","Height of top of cloud","Height of top of cloud",,"Operational"
5129.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"013093","Cloud optical thickness","Cloud optical thickness",,"Operational"
5130.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"105000","Replication descriptor","Delayed replication of 5 descriptors",,"Operational"
5131.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"031001","Delayed descriptor replication factor","Delayed descriptor replication factor",,"Operational"
5132.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"007004","Pressure","Pressure",,"Operational"
5133.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"007004","Pressure","Pressure",,"Operational"
5134.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"008043","Atmospheric chemical or physical constituent type","Atmospheric chemical or physical constituent type",,"Operational"
5135.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"008044","CAS registry number","CAS registry number",,"Operational"
5136.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"015021","Integrated mass density","Integrated mass density",,"Operational"
5137.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"001007","Satellite identifier","Satellite identifier",,"Operational"
5138.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"001031","Identification of originating/generating centre","Identification of originating/generating centre",,"Operational"
5139.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"002019","Satellite instruments","Satellite instruments",,"Operational"
5140.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"002020","Satellite classification","Satellite classification",,"Operational"
5141.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"004001","Year","Year",,"Operational"
5142.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"004002","Month","Month",,"Operational"
5143.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"004003","Day","Day",,"Operational"
5144.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"004004","Hour","Hour",,"Operational"
5145.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"004005","Minute","Minute",,"Operational"
5146.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"202131","Change scale","Add 3 to scale",,"Operational"
5147.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"201138","Change data width","Add 10 to width",,"Operational"
5148.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"004006","Second","Second",,"Operational"
5149.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"201000","Change data width","Reset width",,"Operational"
5150.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"202000","Change scale","Reset scale",,"Operational"
5151.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"005001","Latitude (high accuracy)","Latitude (high accuracy)",,"Operational"
5152.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"006001","Longitude (high accuracy)","Longitude (high accuracy)",,"Operational"
5153.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"007024","Satellite zenith angle","Satellite zenith angle",,"Operational"
5154.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"005021","Bearing or azimuth","Bearing or azimuth",,"Operational"
5155.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"007025","Solar zenith angle","Solar zenith angle",,"Operational"
5156.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"005022","Solar azimuth","Solar azimuth",,"Operational"
5157.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"005043","Field of view number","Field of view number",,"Operational"
5158.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"005040","Orbit number","Orbit number",,"Operational"
5159.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"201133","Change data width","Add 5 to width",,"Operational"
5160.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"005041","Scan line number","Scan line number",,"Operational"
5161.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"201000","Change data width","Reset width",,"Operational"
5162.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"201132","Change data width","Add 4 to width",,"Operational"
5163.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"025070","Major frame count","Major frame count",,"Operational"
5164.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"201000","Change data width","Reset width",,"Operational"
5165.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"202126","Change scale","Subtract 2 from scale",,"Operational"
5166.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"007001","Height of station","Height of station",,"Operational"
5167.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"202000","Change scale","Reset scale",,"Operational"
5168.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"033060","GqisFlagQual - individual IASI-System quality flag","GqisFlagQual",,"Operational"
5169.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"033061","GqisQualIndex - indicator for instrument noise performance (contributions from spectral and radiometric calibration)","GqisQualIndex",,"Operational"
5170.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"033062","GqisQualIndexLoc - indicator for geometric quality index","GqisQualIndexLoc",,"Operational"
5171.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"033063","GqisQualIndexRad - indicator for instrument noise performance (contributions from radiometric calibration)","GqisQualIndexRad",,"Operational"
5172.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"033064","GqisQualIndexSpect - indicator for instrument noise performance (contributions from spectral calibration)","GqisQualIndexSpect",,"Operational"
5173.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"033065","GqisSysTecSondQual - output of system TEC (Technical Expertise Centre) quality function","GqisSysTecSondQual",,"Operational"
5174.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"101010","Replication descriptor","Repeat next 1 descriptor 10 times",,"Operational"
5175.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"340002","IASI Level 1c band description","IASI Level 1c band description",,"Operational"
5176.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"101087","Replication descriptor","Repeat next 1 descriptor 87 times",,"Operational"
5177.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"340003","IASI Level 1c 100 channels","IASI Level 1c 100 channel sequence",,"Operational"
5178.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"002019","Satellite instruments","Satellite instruments",,"Operational"
5179.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"025051","AVHRR channel combination","AVHRR channel combination",,"Operational"
5180.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"101007","Replication descriptor","Repeat next 1 descriptor 7 times",,"Operational"
5181.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"340004","IASI Level 1c AVHRR single scene","IASI Level 1c AVHRR single scene sequence",,"Operational"
5182.00,"40","Additional satellite report sequences","340002","(IASI Level 1c band description)",,"025140","Start channel","Start channel",,"Operational"
5183.00,"40","Additional satellite report sequences","340002","(IASI Level 1c band description)",,"025141","End channel","End channel",,"Operational"
5184.00,"40","Additional satellite report sequences","340002","(IASI Level 1c band description)",,"025142","Channel scale factor","Channel scale factor",,"Operational"
5185.00,"40","Additional satellite report sequences","340003","(IASI Level 1c 100 channels)",,"104100","Replication descriptor","Repeat next 4 descriptors 100 times",,"Operational"
5186.00,"40","Additional satellite report sequences","340003","(IASI Level 1c 100 channel)",,"201136","Change data width","Add 8 to width",,"Operational"
5187.00,"40","Additional satellite report sequences","340003","(IASI Level 1c 100 channel)",,"005042","Channel number","Channel number",,"Operational"
5188.00,"40","Additional satellite report sequences","340003","(IASI Level 1c 100 channel)",,"201000","Change data width","Reset width",,"Operational"
5189.00,"40","Additional satellite report sequences","340003","(IASI Level 1c 100 channel)",,"014046","Scaled IASI radiance","Scaled IASI radiance",,"Operational"
5190.00,"40","Additional satellite report sequences","340004","(IASI Level 1c AVHRR single scene)",,"005060","Y angular position from centre of gravity","Y angular position from centre of gravity",,"Operational"
5191.00,"40","Additional satellite report sequences","340004","(IASI Level 1c AVHRR single scene)",,"005061","Z angular position from centre of gravity","Z angular position from centre of gravity",,"Operational"
5192.00,"40","Additional satellite report sequences","340004","(IASI Level 1c AVHRR single scene)",,"025085","Fraction of clear pixels in HIRS FOV","Fraction of clear pixels in HIRS FOV",,"Operational"
5193.00,"40","Additional satellite report sequences","340004","(IASI Level 1c AVHRR single scene)",,"105006","Replication descriptor","Repeat next 5 descriptor 6 times",,"Operational"
5194.00,"40","Additional satellite report sequences","340004","(IASI Level 1c AVHRR single scene)",,"005042","Channel number","Channel number",,"Operational"
5195.00,"40","Additional satellite report sequences","340004","(IASI Level 1c AVHRR single scene)",,"025142","Channel scale factor","Channel scale factor",,"Operational"
5196.00,"40","Additional satellite report sequences","340004","(IASI Level 1c AVHRR single scene)",,"014047","Scaled mean AVHRR radiance","Scaled mean AVHRR radiance",,"Operational"
5197.00,"40","Additional satellite report sequences","340004","(IASI Level 1c AVHRR single scene)",,"025142","Channel scale factor","Channel scale factor",,"Operational"
5198.00,"40","Additional satellite report sequences","340004","(IASI Level 1c AVHRR single scene)",,"014048","Scaled standard deviation AVHRR radiance","Scaled std dev AVHRR radiance",,"Operational"
5199.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)",,"001007","Satellite identifier","Satellite identifier",,"Operational"
5200.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)",,"002019","Satellite instruments","Satellite instruments",,"Operational"
5201.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)",,"001096","Station acquisition","Acquisition station identifier",,"Operational"
5202.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)",,"025061","Software identification and version number","Software identification",,"Operational"
5203.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)",,"005044","Satellite cycle number","Satellite cycle number",,"Operational"
5204.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)",,"005040","Orbit number","Orbit number",,"Operational"
5205.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)",,"001030","Numerical model identifier","Numerical model identifier",,"Operational"
5206.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Datation","004001","Year","Year",,"Operational"
5207.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Datation","004002","Month","Month",,"Operational"
5208.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Datation","004003","Day","Day",,"Operational"
5209.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Datation","004004","Hour","Hour",,"Operational"
5210.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Datation","004005","Minute","Minute",,"Operational"
5211.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Datation","004007","Seconds within a minute (microsecond accuracy)","Seconds within a minute",,"Operational"
5212.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Location and surface type","005001","Latitude (high accuracy)","Latitude (high accuracy)",,"Operational"
5213.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Location and surface type","006001","Longitude (high accuracy)","Longitude (high accuracy)",,"Operational"
5214.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Location and surface type","008029","Surface type","Surface type",,"Operational"
5215.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Location and surface type","008074","Altimeter echo type","Altimeter echo type",,"Operational"
5216.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Location and surface type","008077","Radiometer sensed surface type","Radiometer sensed surface type",,"Operational"
5217.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Flags","040011","Interpolation flag","Interpolation flag",,"Operational"
5218.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Flags","025097","Three-dimensional error estimate of the navigator orbit","Three-dimensional error estimate of the navigator orbit",,"Operational"
5219.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Flags","025095","Altimeter state flag","Altimeter state flag",,"Operational"
5220.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Flags","025098","Altimeter data quality flag","Altimeter data quality flag",,"Operational"
5221.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Flags","025099","Altimeter correction quality flag","Altimeter correction quality flag",,"Operational"
5222.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Flags","021144","Altimeter rain flag","Altimeter rain flag",,"Operational"
5223.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Flags","025096","Radiometer state flag","Radiometer state flag",,"Operational"
5224.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Flags","040012","Radiometer data quality flag","Radiometer data quality flag",,"Operational"
5225.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Flags","040013","Radiometer brightness temperature interpretation flag","Radiometer brightness temperature interpretation flag",,"Operational"
5226.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Flags","021169","Ice presence indicator","Ice presence indicator",,"Operational"
5227.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: Ku band","022151","Ku band ocean range","Ku band ocean range",,"Operational"
5228.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: Ku band","022162","RMS of 20 Hz Ku band ocean range","RMS of 20 Hz Ku band ocean range",,"Operational"
5229.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: Ku band","022163","Number of 20Hz valid points for Ku band","Number of 20 Hz valid points for Ku band",,"Operational"
5230.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: Ku band","025160","Ku band net instrumental correction","Ku band net instrumental correction",,"Operational"
5231.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: Ku band","025133","Sea state bias correction on Ku band","Sea state bias correction on Ku band",,"Operational"
5232.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: Ku band","022156","Ku band significant wave height","Ku band significant wave height",,"Operational"
5233.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: Ku band","022164","RMS 20 Hz Ku band significant wave height","RMS 20 Hz Ku band significant wave height",,"Operational"
5234.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: Ku band","022165","Number of 20Hz valid points for Ku band significant wave height","Number of 20 Hz valid points for Ku band significant wave height",,"Operational"
5235.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: Ku band","022166","Ku band net instrumental correction for significant wave height","Ku band net instrumental correction for significant wave height",,"Operational"
5236.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: Ku band","021137","Ku band corrected ocean backscatter coefficient","Ku band corrected ocean backscatter coefficient",,"Operational"
5237.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: Ku band","021138","Std Ku band corrected ocean backscatter coefficient","STD Ku band corrected ocean backscatter coefficient",,"Operational"
5238.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: Ku band","022167","Number of valid points for Ku band backscatter","Number of valid points for Ku band backscatter",,"Operational"
5239.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: Ku band","021139","Ku band net instrumental correction for AGC","Ku band net instrumental correction for AGC",,"Operational"
5240.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: Ku band","021118","Attenuation correction on sigma-0","Attenuation correction on sigma-0",,"Operational"
5241.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: Ku band","021145","Ku band automatic gain control","Ku band automatic gain control",,"Operational"
5242.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: Ku band","021146","RMS Ku band automatic gain control","RMS Ku band automatic gain control",,"Operational"
5243.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: Ku band","021147","Number of valid points for Ku band automatic gain control","Number of valid points for Ku band automatic gain control",,"Operational"
5244.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: C band","022168","C band ocean range","C band ocean range",,"Operational"
5245.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: C band","022169","RMS of C band ocean range","RMS of C band ocean range",,"Operational"
5246.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: C band","022170","Number of 20Hz valid points for C band","Number of 20 Hz valid points for C band",,"Operational"
5247.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: C band","025161","C band net instrumental correction","C band net instrumental correction",,"Operational"
5248.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: C band","025162","Sea state bias correction on C band","Sea state bias correction on C band",,"Operational"
5249.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: C band","022171","C band significant wave height","C band significant wave height",,"Operational"
5250.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: C band","022172","RMS 20Hz C band significant wave height","RMS 20 Hz C band significant wave height",,"Operational"
5251.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: C band","022173","Number of 20Hz valid points for C band significant wave height","Number of 20 Hz valid points for C band significant wave height",,"Operational"
5252.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: C band","022174","C band net instrumental correction for significant wave height","C band net instrumental correction for significant wave height",,"Operational"
5253.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: C band","021170","C band corrected ocean backscatter coefficient","C band corrected ocean backscatter coefficient",,"Operational"
5254.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: C band","021171","RMS C band corrected ocean backscatter coefficient","RMS C band corrected ocean backscatter coefficient",,"Operational"
5255.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: C band","022175","Number of valid points for C band backscatter","Number of valid points for C band backscatter",,"Operational"
5256.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: C band","021172","C band net instrumental correction for AGC","C band net instrumental correction for AGC",,"Operational"
5257.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: C band","021118","Attenuation correction on sigma-0","Attenuation correction on sigma-0",,"Operational"
5258.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: C band","021173","C band automatic gain control","C band automatic gain control",,"Operational"
5259.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: C band","021174","RMS C band automatic gain control","RMS C band automatic gain control",,"Operational"
5260.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: C band","021175","Number of valid points for C band automatic gain control","Number of valid points for C band automatic gain control",,"Operational"
5261.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Radiometer","002153","Satellite channel centre frequency","Satellite channel centre frequency",,"Operational"
5262.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Radiometer","012063","Brightness temperature","Brightness temperature",,"Operational"
5263.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Radiometer","002153","Satellite channel centre frequency","Satellite channel centre frequency",,"Operational"
5264.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Radiometer","012063","Brightness temperature","Brightness temperature",,"Operational"
5265.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Radiometer","002153","Satellite channel centre frequency","Satellite channel centre frequency",,"Operational"
5266.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Radiometer","012063","Brightness temperature","Brightness temperature",,"Operational"
5267.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Radiometer","013090","Radiometer water vapour content","Radiometer water vapour content",,"Operational"
5268.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Radiometer","013091","Radiometer liquid content","Radiometer liquid content",,"Operational"
5269.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Wind","007002","Height or altitude","Height or altitude",,"Operational"
5270.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Wind","011097","Wind speed from altimeter","Wind speed from altimeter",,"Operational"
5271.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Wind","011098","Wind speed from radiometer","Wind speed from radiometer",,"Operational"
5272.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Wind","007002","Height or altitude","Height or altitude",,"Operational"
5273.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Wind","011095","u component of the model wind vector","u-component of the model wind vector",,"Operational"
5274.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Wind","011096","v component of the model wind vector","v-component of the model wind vector",,"Operational"
5275.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Dynamic topography","010096","Mean dynamic topography","Mean dynamic topography",,"Operational"
5276.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Dynamic topography","010081","Altitude of COG above reference ellipsoid","Altitude of COG above reference ellipsoid",,"Operational"
5277.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Dynamic topography","010082","Instantaneous altitude rate","Instantaneous altitude rate",,"Operational"
5278.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Dynamic topography","010083","Squared off nadir angle of the satellite from platform data","Off nadir angle of the satellite from platform data",,"Operational"
5279.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Dynamic topography","010101","Squared off nadir angle of the satellite from waveform data","Squared off nadir angle of the satellite from waveform data",,"Operational"
5280.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Dynamic topography","025132","Ionospheric correction from model on Ku band","Ionospheric correction from model on Ku band",,"Operational"
5281.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Dynamic topography","025163","Altimeter ionospheric correction on Ku band","Altimeter ionospheric correction on Ku band",,"Operational"
5282.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Dynamic topography","025126","Model dry tropospheric correction","Model dry tropospheric correction",,"Operational"
5283.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Dynamic topography","025128","Model wet tropospheric correction","Model wet tropospheric correction",,"Operational"
5284.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Dynamic topography","025164","Radiometer wet tropospheric correction","Radiometer wet tropospheric correction",,"Operational"
5285.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Dynamic topography","010085","Mean sea surface height","Mean sea surface height",,"Operational"
5286.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Dynamic topography","010097","Mean sea surface height from altimeter only","Mean sea surface height from altimeter only",,"Operational"
5287.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Dynamic topography","010086","Geoid's height","Geoid's height",,"Operational"
5288.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Dynamic topography","010087","Ocean depth/land elevation","Ocean depth/land elevation",,"Operational"
5289.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Dynamic topography","010092","Solid Earth tide height","Solid earth tide height",,"Operational"
5290.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Dynamic topography","010088","Total geocentric ocean tide height (solution 1)","Geocentric ocean tide height solution 1",,"Operational"
5291.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Dynamic topography","010089","Total geocentric ocean tide height (solution 2)","Geocentric ocean tide height solution 2",,"Operational"
5292.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Dynamic topography","010098","Loading tide height geocentric ocean tide solution 1","Loading tide height geocentric ocean tide solution 1",,"Operational"
5293.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Dynamic topography","010099","Loading tide height geocentric ocean tide solution 2","Loading tide height geocentric ocean tide solution 2",,"Operational"
5294.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Dynamic topography","010090","Long period tide height","Long period tide height",,"Operational"
5295.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Dynamic topography","010100","Non-equilibrium long period tide height","Non-equilibrium long period tide height",,"Operational"
5296.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Dynamic topography","010093","Geocentric pole tide height","Geocentric pole tide height",,"Operational"
5297.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Dynamic topography","025127","Inverted barometer correction","Sea surface height correction due to pressure loading",,"Operational"
5298.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Dynamic topography","040014","High frequency fluctuations of the sea surface topography correction","High frequency fluctuations of the sea surface topography correction",,"Operational"
5299.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"001007","Satellite identifier","Satellite identifier",,"Operational"
5300.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"001031","Identification of originating/generating centre","Identification of originating/generating centre",,"Operational"
5301.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"002019","Satellite instruments","Satellite instruments",,"Operational"
5302.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"002020","Satellite classification","Satellite classification",,"Operational"
5303.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"004001","Year","Year",,"Operational"
5304.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"004002","Month","Month",,"Operational"
5305.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"004003","Day","Day",,"Operational"
5306.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"004004","Hour","Hour",,"Operational"
5307.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"004005","Minute","Minute",,"Operational"
5308.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"202131","Change scale","Add 3 to scale",,"Operational"
5309.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"201138","Change data width","Add 10 to width",,"Operational"
5310.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"004006","Second","Second",,"Operational"
5311.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"201000","Change data width","Reset width",,"Operational"
5312.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"202000","Change scale","Reset scale",,"Operational"
5313.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"005001","Latitude (high accuracy)","Latitude (high accuracy)",,"Operational"
5314.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"006001","Longitude (high accuracy)","Longitude (high accuracy)",,"Operational"
5315.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"007024","Satellite zenith angle","Satellite zenith angle",,"Operational"
5316.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"005021","Bearing or azimuth","Bearing or azimuth",,"Operational"
5317.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"007025","Solar zenith angle","Solar zenith angle",,"Operational"
5318.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"005022","Solar azimuth","Solar azimuth",,"Operational"
5319.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"005043","Field of view number","Field of view number",,"Operational"
5320.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"005040","Orbit number","Orbit number",,"Operational"
5321.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"201133","Change data width","Add 5 to width",,"Operational"
5322.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"005041","Scan line number","Scan line number",,"Operational"
5323.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"201000","Change data width","Reset width",,"Operational"
5324.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"201132","Change data width","Add 4 to width",,"Operational"
5325.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"025070","Major frame count","Major frame count",,"Operational"
5326.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"201000","Change data width","Reset width",,"Operational"
5327.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"202126","Change scale","Subtract 2 from scale",,"Operational"
5328.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"007001","Height of station","Height of station",,"Operational"
5329.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"202000","Change scale","Reset scale",,"Operational"
5330.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"103003","Replication descriptor","Repeat next 3 descriptors 3 times",,"Operational"
5331.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"025140","Start channel","Start channel",,"Operational"
5332.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"025141","End channel","End channel",,"Operational"
5333.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"033060","GqisFlagQual - individual IASI-System quality flag","GqisFlagQual",,"Operational"
5334.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"033061","GqisQualIndex - indicator for instrument noise performance (contributions from spectral and radiometric calibration)","GqisQualIndex",,"Operational"
5335.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"033062","GqisQualIndexLoc - indicator for geometric quality index","GqisQualIndexLoc",,"Operational"
5336.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"033063","GqisQualIndexRad - indicator for instrument noise performance","GqisQualIndexRad",,"Operational"
5337.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"033064","GqisQualIndexSpect - indicator for instrument noise performance","GqisQualIndexSpect",,"Operational"
5338.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"033065","GqisSysTecSondQual - output of system TEC (Technical Expertise Centre) quality function","GqisSysTecSondQual",,"Operational"
5339.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"040020","GQisFlagQualDetailed - quality flag for the system","GqisFlagQualDetailed - quality flag for the system",,"Operational"
5340.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"101010","Replication descriptor","Repeat next 1 descriptor 10 times",,"Operational"
5341.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"340002","IASI Level 1c band description","IASI Level 1c band description",,"Operational"
5342.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"101087","Replication descriptor","Repeat next 1 descriptor 87 times",,"Operational"
5343.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"340003","IASI Level 1c 100 channels","IASI Level 1c 100 channel sequence",,"Operational"
5344.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"002019","Satellite instruments","Satellite instruments",,"Operational"
5345.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"025051","AVHRR channel combination","AVHRR channel combination",,"Operational"
5346.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"101007","Replication descriptor","Repeat next 1 descriptor 7 times",,"Operational"
5347.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"340004","IASI Level 1c AVHRR single scene","IASI Level 1c AVHRR single scene sequence",,"Operational"
5348.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"020081","Cloud amount in segment","Cloud amount in segment",,"Operational"
5349.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"008029","Surface type","Surface type",,"Operational"
5350.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"020083","Amount of segment covered by scene","Amount of segment covered by scene",,"Operational"
5351.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"008029","Surface type","Surface type",,"Operational"
5352.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"040018","GIacAvgImagIIS - average of imager measurements","GIacAvgImagIIS -average of imager measurements",,"Operational"
5353.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"040019","GIacVarImagIIS - variance of imager measurements","GIacVarImagIIS -variance of imager measurements",,"Operational"
5354.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"040021","Fraction of weighted AVHRR pixel in IASI FOV covered with snow/ice","Fraction of weighted AVHRR pixel in IASI FOV covered with snow/ice",,"Operational"
5355.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"040022","Number of missing, bad or failed AVHRR pixels","Number of missing, bad or failed AVHRR pixels",,"Operational"
5356.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Satellite processing information","001007","Satellite identifier","Satellite identifier",,"Operational"
5357.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Satellite processing information","001031","Identification of originating/generating centre","Identification of originating/generating centre",,"Operational"
5358.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Satellite processing information","002019","Satellite instruments","Satellite instruments",,"Operational"
5359.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Satellite processing information","002020","Satellite classification","Satellite classification",,"Operational"
5360.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Date and time","004001","Year","Year",,"Operational"
5361.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Date and time","004002","Month","Month",,"Operational"
5362.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Date and time","004003","Day","Day",,"Operational"
5363.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Date and time","004004","Hour","Hour",,"Operational"
5364.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Date and time","004005","Minute","Minute",,"Operational"
5365.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Date and time","202131","Change scale","Add 3 to scale",,"Operational"
5366.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Date and time","201138","Change data width","Add 10 to width",,"Operational"
5367.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Date and time","004006","Second","Second",,"Operational"
5368.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Date and time","201000","Change data width","Reset width",,"Operational"
5369.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Date and time","202000","Change scale","Reset scale",,"Operational"
5370.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Location information","005001","Latitude (high accuracy)","Latitude (high accuracy)",,"Operational"
5371.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Location information","006001","Longitude (high accuracy)","Longitude (high accuracy)",,"Operational"
5372.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Location information","007024","Satellite zenith angle","Satellite zenith angle",,"Operational"
5373.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Location information","005021","Bearing or azimuth","Bearing or azimuth",,"Operational"
5374.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Location information","007025","Solar zenith angle","Solar zenith angle",,"Operational"
5375.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Location information","005022","Solar azimuth","Solar azimuth",,"Operational"
5376.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Location information","005043","Field of view number","Field of view number",,"Operational"
5377.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Location information","005040","Orbit number","Orbit number",,"Operational"
5378.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Location information","201133","Change data width","Add 5 to width",,"Operational"
5379.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Location information","005041","Scan line number","Scan line number",,"Operational"
5380.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Location information","201000","Change data width","Reset width",,"Operational"
5381.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Location information","201132","Change data width","Add 4 to width",,"Operational"
5382.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Location information","025070","Major frame count","Major frame count",,"Operational"
5383.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Location information","201000","Change data width","Reset width",,"Operational"
5384.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Location information","202126","Change scale","Subtract 2 from scale",,"Operational"
5385.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Location information","007001","Height of station","Height of station",,"Operational"
5386.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Location information","202000","Change scale","Reset scale",,"Operational"
5387.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Quality information","103003","Replication descriptor","Repeat next 3 descriptors 3 times",,"Operational"
5388.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Quality information","025140","Start channel","Start channel",,"Operational"
5389.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Quality information","025141","End channel","End channel",,"Operational"
5390.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Quality information","033060","GqisFlagQual - individual IASI-System quality flag","GqisFlagQual",,"Operational"
5391.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Quality information","033061","GqisQualIndex - indicator for instrument noise performance (contributions from spectral and radiometric calibration)","GqisQualIndex",,"Operational"
5392.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Quality information","033062","GqisQualIndexLoc - indicator for geometric quality index","GqisQualIndexLoc",,"Operational"
5393.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Quality information","033063","GqisQualIndexRad - indicator for instrument noise performance (contributions from radiometric calibration)","GqisQualIndexRad",,"Operational"
5394.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Quality information","033064","GqisQualIndexSpect - indicator for instrument noise performance (contributions from spectral calibration)","GqisQualIndexSpect",,"Operational"
5395.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Quality information","033065","GqisSysTecSondQual - output of system TEC (Technical Expertise Centre) quality function","GqisSysTecSondQual",,"Operational"
5396.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Quality information","040020","GqisFlagQualDetailed - quality flag for the system","GqisFlagQualDetailed - quality flag for the system",,"Operational"
5397.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","IASI subset of channels","101010","Replication descriptor","Repeat next 1 descriptor 10 times",,"Operational"
5398.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","IASI subset of channels","340002","IASI Level 1c band description","IASI Level 1c band description",,"Operational"
5399.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","IASI subset of channels","104000","Replication descriptor","Delayed replication of next 4 descriptors",,"Operational"
5400.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","IASI subset of channels","031002","Extended delayed descriptor replication factor","Extended delayed replication factor",,"Operational"
5401.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","IASI subset of channels","201136","Change data width","Add 8 to width",,"Operational"
5402.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","IASI subset of channels","005042","Channel number","Channel number",,"Operational"
5403.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","IASI subset of channels","201000","Change data width","Reset width",,"Operational"
5404.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","IASI subset of channels","014046","Scaled IASI radiance","Scaled IASI radiance",,"Operational"
5405.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Instrument band definition","108003","Replication descriptor","Repeat next 8 descriptors 3 times",,"Operational"
5406.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Instrument band definition","025140","Start channel","Start channel",,"Operational"
5407.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Instrument band definition","025141","End channel","End channel",,"Operational"
5408.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Instrument band definition","040026","Score quantization factor","Quantization factor",,"Operational"
5409.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Instrument band definition","040016","Residual RMS in band","Residual RMS in band",,"Operational"
5410.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Instrument band definition","025062","Database identification","Database identification",,"Operational"
5411.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Principal component scores for band","101000","Replication descriptor","Delayed replication of 1 descriptor",,"Operational"
5412.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Principal component scores for band","031002","Extended delayed descriptor replication factor","Extended delayed replication factor",,"Operational"
5413.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Principal component scores for band","040017","Non-normalized principal component score","Non-normalized principal component score",,"Operational"
5414.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","AVHRR scene analysis","002019","Satellite instruments","Satellite instruments",,"Operational"
5415.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","AVHRR scene analysis","025051","AVHRR channel combination","AVHRR channel combination",,"Operational"
5416.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","AVHRR scene analysis","101007","Replication descriptor","Repeat next 1 descriptor 7 times",,"Operational"
5417.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","AVHRR scene analysis","340004","IASI Level 1c AVHRR single scene","IASI Level 1c AVHRR single scene sequence",,"Operational"
5418.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","AVHRR scene analysis","020081","Cloud amount in segment","Cloud amount in segment",,"Operational"
5419.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","AVHRR scene analysis","008029","Surface type","Surface type",,"Operational"
5420.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","AVHRR scene analysis","020083","Amount of segment covered by scene","Amount of segment covered by scene",,"Operational"
5421.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","AVHRR scene analysis","008029","Surface type","Surface type",,"Operational"
5422.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","AVHRR scene analysis","040018","GIacAvgImagIIS - average of imager measurements","Average of imager measurements",,"Operational"
5423.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","AVHRR scene analysis","040019","GIacVarImagIIS - variance of imager measurements","Variance of imager measurements",,"Operational"
5424.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","AVHRR scene analysis","040021","Fraction of weighted AVHRR pixel in IASI FOV covered with snow/ice","Fraction of weighted AVHRR pixel in IASI FOV covered with snow/ice",,"Operational"
5425.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","AVHRR scene analysis","040022","Number of missing, bad or failed AVHRR pixels","Number of missing, bad or failed AVHRR pixels",,"Operational"
5426.00,"40","Additional satellite report sequences","340009","(Normalized differential vegetation index (NDVI))",,"001007","Satellite identifier","Satellite identifier",,"Operational"
5427.00,"40","Additional satellite report sequences","340009","(Normalized differential vegetation index (NDVI))",,"001031","Identification of originating/generating centre","Generating centre",,"Operational"
5428.00,"40","Additional satellite report sequences","340009","(Normalized differential vegetation index (NDVI))",,"002019","Satellite instruments","Satellite instrument",,"Operational"
5429.00,"40","Additional satellite report sequences","340009","(Normalized differential vegetation index (NDVI))",,"002020","Satellite classification","Satellite classification",,"Operational"
5430.00,"40","Additional satellite report sequences","340009","(Normalized differential vegetation index (NDVI))",,"301011",,"Date",,"Operational"
5431.00,"40","Additional satellite report sequences","340009","(Normalized differential vegetation index (NDVI))",,"301013",,"Time",,"Operational"
5432.00,"40","Additional satellite report sequences","340009","(Normalized differential vegetation index (NDVI))",,"005040","Orbit number","Orbit number",,"Operational"
5433.00,"40","Additional satellite report sequences","340009","(Normalized differential vegetation index (NDVI))",,"201136","Change data width","Add 8 bits to width of next descriptor",,"Operational"
5434.00,"40","Additional satellite report sequences","340009","(Normalized differential vegetation index (NDVI))",,"005041","Scan line number","Scan line number",,"Operational"
5435.00,"40","Additional satellite report sequences","340009","(Normalized differential vegetation index (NDVI))",,"201000","Change data width","Reset descriptor width",,"Operational"
5436.00,"40","Additional satellite report sequences","340009","(Normalized differential vegetation index (NDVI))",,"025071","Frame count","Frame count",,"Operational"
5437.00,"40","Additional satellite report sequences","340009","(Normalized differential vegetation index (NDVI))",,"005001","Latitude (high accuracy)","Latitude (high accuracy)",,"Operational"
5438.00,"40","Additional satellite report sequences","340009","(Normalized differential vegetation index (NDVI))",,"005001","Latitude (high accuracy)","Latitude (high accuracy)",,"Operational"
5439.00,"40","Additional satellite report sequences","340009","(Normalized differential vegetation index (NDVI))",,"006001","Longitude (high accuracy)","Longitude (high accuracy)",,"Operational"
5440.00,"40","Additional satellite report sequences","340009","(Normalized differential vegetation index (NDVI))",,"006001","Longitude (high accuracy)","Longitude (high accuracy)",,"Operational"
5441.00,"40","Additional satellite report sequences","340009","(Normalized differential vegetation index (NDVI))",,"107064","Replication descriptor","Repeat next 7 descriptors 64 times",,"Operational"
5442.00,"40","Additional satellite report sequences","340009","(Normalized differential vegetation index (NDVI))",,"106032","Replication descriptor","Repeat next 6 descriptors 32 times",,"Operational"
5443.00,"40","Additional satellite report sequences","340009","(Normalized differential vegetation index (NDVI))",,"008012","Land/sea qualifier","Land/sea qualifier",,"Operational"
5444.00,"40","Additional satellite report sequences","340009","(Normalized differential vegetation index (NDVI))",,"008013","Day/night qualifier","Day/night qualifier",,"Operational"
5445.00,"40","Additional satellite report sequences","340009","(Normalized differential vegetation index (NDVI))",,"008065","Sun-glint indicator","Sun-glint indicator",,"Operational"
5446.00,"40","Additional satellite report sequences","340009","(Normalized differential vegetation index (NDVI))",,"008072","Pixel(s) type","Pixel(s) type",,"Operational"
5447.00,"40","Additional satellite report sequences","340009","(Normalized differential vegetation index (NDVI))",,"013039","Terrain type (ice/snow)","Terrain type (ice/snow)",,"Operational"
5448.00,"40","Additional satellite report sequences","340009","(Normalized differential vegetation index (NDVI))",,"040015","Normalized differential vegetation index (NDVI)","Normalized differential vegetation index (NDVI)",,"Operational"
5449.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Satellite","001007","Satellite identifier","Satellite identifier",,"Operational"
5450.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Satellite","002019","Satellite instruments","Satellite instruments",,"Operational"
5451.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Satellite","001096","Station acquisition","Acquisition station identifier",,"Operational"
5452.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Satellite","025061","Software identification and version number","Software identification",,"Operational"
5453.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Satellite","005044","Satellite cycle number","Satellite cycle number",,"Operational"
5454.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Satellite","005040","Orbit number","Orbit number",,"Operational"
5455.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Satellite","001030","Numerical model identifier","Numerical model identifier",,"Operational"
5456.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Datation","004001","Year","Year",,"Operational"
5457.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Datation","004002","Month","Month",,"Operational"
5458.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Datation","004003","Day","Day",,"Operational"
5459.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Datation","004004","Hour","Hour",,"Operational"
5460.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Datation","004005","Minute","Minute",,"Operational"
5461.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Datation","004007","Seconds within a minute (microsecond accuracy)","Seconds within a minute",,"Operational"
5462.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Location and surface type","005001","Latitude (high accuracy)","Latitude (high accuracy)",,"Operational"
5463.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Location and surface type","006001","Longitude (high accuracy)","Longitude (high accuracy)",,"Operational"
5464.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Location and surface type","008029","Surface type","Surface type",,"Operational"
5465.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Location and surface type","008074","Altimeter echo type","Altimeter echo type",,"Operational"
5466.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Location and surface type","008077","Radiometer sensed surface type","Radiometer sensed surface type",,"Operational"
5467.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Flags","040011","Interpolation flag","Interpolation flag",,"Operational"
5468.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Flags","025097","Three-dimensional error estimate of the navigator orbit","Three dimensional error estimate of the navigator orbit",,"Operational"
5469.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Flags","025095","Altimeter state flag","Altimeter state flag",,"Operational"
5470.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Flags","025098","Altimeter data quality flag","Altimeter data quality flag",,"Operational"
5471.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Flags","025099","Altimeter correction quality flag","Altimeter correction quality flag",,"Operational"
5472.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Flags","021144","Altimeter rain flag","Altimeter rain flag",,"Operational"
5473.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Flags","025096","Radiometer state flag","Radiometer state flag",,"Operational"
5474.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Flags","040012","Radiometer data quality flag","Radiometer data quality flag",,"Operational"
5475.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Flags","040013","Radiometer brightness temperature interpretation flag","Radiometer brightness temperature interpretation flag",,"Operational"
5476.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Flags","021169","Ice presence indicator","Ice presence indicator",,"Operational"
5477.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Flags","040023","Auxiliary altimeter state flags","Auxiliary altimeter state flags",,"Operational"
5478.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Flags","040024","Meteorological map availability","Meteorological map availability",,"Operational"
5479.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Flags","040025","Interpolation flag for mean diurnal tide","Interpolation flag for mean diurnal tide",,"Operational"
5480.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: Ku band","022151","Ku band ocean range","Ku band ocean range",,"Operational"
5481.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: Ku band","022162","RMS of 20 Hz Ku band ocean range","RMS of 20 Hz Ku band ocean range",,"Operational"
5482.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: Ku band","022163","Number of 20 Hz valid points for Ku band","Number of 20 Hz valid points for Ku band",,"Operational"
5483.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: Ku band","025160","Ku band net instrumental correction","Ku band net instrumental correction",,"Operational"
5484.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: Ku band","025133","Sea state bias correction on Ku band","Sea state bias correction on Ku band",,"Operational"
5485.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: Ku band","022156","Ku band significant wave height","Ku band significant wave height",,"Operational"
5486.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: Ku band","022164","RMS 20 Hz Ku band significant wave height","RMS 20 Hz Ku band significant wave height",,"Operational"
5487.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: Ku band","022165","Number of 20 Hz valid points for Ku band significant wave height","Number of 20 Hz valid points for Ku band significant wave height",,"Operational"
5488.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: Ku band","022166","Ku band net instrumental correction for significant wave height","Ku band net instrumental correction for significant wave height",,"Operational"
5489.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: Ku band","021137","Ku band corrected ocean backscatter coefficient","Ku band corrected ocean backscatter coefficient",,"Operational"
5490.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: Ku band","021138","Std Ku band corrected ocean backscatter coefficient","Std Ku band corrected ocean backscatter coefficient",,"Operational"
5491.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: Ku band","022167","Number of valid points for Ku band backscatter","Number of valid points for Ku band backscatter",,"Operational"
5492.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: Ku band","021139","Ku band net instrumental correction for AGC","Ku band net instrumental correction for AGC",,"Operational"
5493.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: Ku band","021118","Attenuation correction on sigma-0","Attenuation correction on sigma-0",,"Operational"
5494.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: Ku band","021145","Ku band automatic gain control","Ku band automatic gain control",,"Operational"
5495.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: Ku band","021146","RMS Ku band automatic gain control","RMS Ku band automatic gain control",,"Operational"
5496.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: Ku band","021147","Number of valid points for Ku band automatic gain control","Number of valid points for Ku band automatic gain control",,"Operational"
5497.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: C band","022168","C band ocean range","C band ocean range",,"Operational"
5498.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: C band","022169","RMS of C band ocean range","RMS of C band ocean range",,"Operational"
5499.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: C band","022170","Number of 20 Hz valid points for C band","Number of 20 Hz valid points for C band",,"Operational"
5500.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: C band","025161","C band net instrumental correction","C band net instrumental correction",,"Operational"
5501.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: C band","025162","Sea state bias correction on C band","Sea state bias correction on C band",,"Operational"
5502.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: C band","022171","C band significant wave height","C band significant wave height",,"Operational"
5503.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: C band","022172","RMS 20 Hz C band significant wave height","RMS 20 Hz C band significant wave height",,"Operational"
5504.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: C band","022173","Number of 20 Hz valid points for C band significant wave height","Number of 20 Hz valid points for C band significant wave height",,"Operational"
5505.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: C band","022174","C band net instrumental correction for significant wave height","C band net instrumental correction for significant wave height",,"Operational"
5506.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: C band","021170","C band corrected ocean backscatter coefficient","C band corrected ocean backscatter coefficient",,"Operational"
5507.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: C band","021171","RMS C band corrected ocean backscatter coefficient","RMS C band corrected ocean backscatter coefficient",,"Operational"
5508.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: C band","022175","Number of valid points for C band backscatter","Number of valid points for C band backscatter",,"Operational"
5509.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: C band","021172","C band net instrumental correction for AGC","C band net instrumental correction for AGC",,"Operational"
5510.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: C band","021118","Attenuation correction on sigma-0","Attenuation correction on sigma-0",,"Operational"
5511.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: C band","021173","C band automatic gain control","C band automatic gain control",,"Operational"
5512.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: C band","021174","RMS C band automatic gain control","RMS C band automatic gain control",,"Operational"
5513.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: C band","021175","Number of valid points for C band automatic gain control","Number of valid points for C band automatic gain control",,"Operational"
5514.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Radiometer","002153","Satellite channel centre frequency","Satellite channel centre frequency",,"Operational"
5515.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Radiometer","012063","Brightness temperature","Brightness temperature",,"Operational"
5516.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Radiometer","002153","Satellite channel centre frequency","Satellite channel centre frequency",,"Operational"
5517.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Radiometer","012063","Brightness temperature","Brightness temperature",,"Operational"
5518.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Radiometer","002153","Satellite channel centre frequency","Satellite channel centre frequency",,"Operational"
5519.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Radiometer","012063","Brightness temperature","Brightness temperature",,"Operational"
5520.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Radiometer","013090","Radiometer water vapour content","Radiometer water vapour content",,"Operational"
5521.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Radiometer","013091","Radiometer liquid content","Radiometer liquid content",,"Operational"
5522.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Wind","007002","Height or altitude","Height or altitude",,"Operational"
5523.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Wind","011097","Wind speed from altimeter","Wind speed from altimeter",,"Operational"
5524.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Wind","011098","Wind speed from radiometer","Wind speed from radiometer",,"Operational"
5525.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Wind","007002","Height or altitude","Height or altitude",,"Operational"
5526.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Wind","011095","u component of the model wind vector","u component of the model wind vector",,"Operational"
5527.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Wind","011096","v component of the model wind vector","v component of the model wind vector",,"Operational"
5528.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Dynamic topography","010096","Mean dynamic topography","Mean dynamic topography",,"Operational"
5529.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Dynamic topography","010081","Altitude of COG above reference ellipsoid","Altitude of cog above reference ellipsoid",,"Operational"
5530.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Dynamic topography","010082","Instantaneous altitude rate","Instantaneous altitude rate",,"Operational"
5531.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Dynamic topography","010083","Squared off nadir angle of the satellite from platform data","Off nadir angle of the satellite from platform data",,"Operational"
5532.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Dynamic topography","010101","Squared off nadir angle of the satellite from waveform data","Squared off nadir angle of the satellite from waveform data",,"Operational"
5533.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Dynamic topography","025132","Ionospheric correction from model on Ku band","Ionospheric correction from model on Ku band",,"Operational"
5534.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Dynamic topography","025163","Altimeter ionospheric correction on Ku band","Altimeter ionospheric correction on Ku band",,"Operational"
5535.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Dynamic topography","025126","Model dry tropospheric correction","Model dry tropospheric correction",,"Operational"
5536.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Dynamic topography","025128","Model wet tropospheric correction","Model wet tropospheric correction",,"Operational"
5537.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Dynamic topography","025164","Radiometer wet tropospheric correction","Radiometer wet tropospheric correction",,"Operational"
5538.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Dynamic topography","010085","Mean sea surface height","Mean sea surface height",,"Operational"
5539.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Dynamic topography","010097","Mean sea surface height from altimeter only","Mean sea surface height from altimeter only",,"Operational"
5540.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Dynamic topography","010086","Geoid's height","Geoid's height",,"Operational"
5541.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Dynamic topography","010087","Ocean depth/land elevation","Ocean depth/land elevation",,"Operational"
5542.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Dynamic topography","010092","Solid Earth tide height","Solid earth tide height",,"Operational"
5543.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Dynamic topography","010088","Total geocentric ocean tide height (solution 1)","Geocentric ocean tide height solution 1",,"Operational"
5544.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Dynamic topography","010089","Total geocentric ocean tide height (solution 2)","Geocentric ocean tide height solution 2",,"Operational"
5545.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Dynamic topography","010098","Loading tide height geocentric ocean tide solution 1","Loading tide height geocentric ocean tide solution 1",,"Operational"
5546.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Dynamic topography","010099","Loading tide height geocentric ocean tide solution 2","Loading tide height geocentric ocean tide solution 2",,"Operational"
5547.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Dynamic topography","010090","Long period tide height","Long period tide height",,"Operational"
5548.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Dynamic topography","010100","Non-equilibrium long period tide height","Non-equilibrium long period tide height",,"Operational"
5549.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Dynamic topography","010093","Geocentric pole tide height","Geocentric pole tide height",,"Operational"
5550.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Dynamic topography","025127","Inverted barometer correction","Sea surface height correction due to pressure loading",,"Operational"
5551.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Dynamic topography","040014","High frequency fluctuations of the sea surface topography correction","High frequency fluctuations of the sea surface topography correction",,"Operational"
5552.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Dynamic topography","010102","Sea surface height anomaly","Sea surface height anomaly",,"Operational"
