"No","Category","CategoryOfSequences_en","FXY1","Title_en","SubTitle_en","FXY2","ElementName_en","ElementDescription_en","Note_en","Status"
1.00,"00","BUFR table entries sequences","300002",,,"000002","Table A: data category description, line 1",,,"Operational"
2.00,"00","BUFR table entries sequences","300002",,,"000003","Table A: data category description, line 2",,,"Operational"
3.00,"00","BUFR table entries sequences","300003","(F, X, Y of descriptor to be added or defined)",,"000010","F descriptor to be added or defined",,,"Operational"
4.00,"00","BUFR table entries sequences","300003","(F, X, Y of descriptor to be added or defined)",,"000011","X descriptor to be added or defined",,,"Operational"
5.00,"00","BUFR table entries sequences","300003","(F, X, Y of descriptor to be added or defined)",,"000012","Y descriptor to be added or defined",,,"Operational"
6.00,"00","BUFR table entries sequences","300004",,,"300003","F, X, Y of descriptor to be added or defined",,,"Operational"
7.00,"00","BUFR table entries sequences","300004",,,"000013","Element name, line 1",,,"Operational"
8.00,"00","BUFR table entries sequences","300004",,,"000014","Element name, line 2",,,"Operational"
9.00,"00","BUFR table entries sequences","300004",,,"000015","Units name",,,"Operational"
10.00,"00","BUFR table entries sequences","300004",,,"000016","Units scale sign",,,"Operational"
11.00,"00","BUFR table entries sequences","300004",,,"000017","Units scale",,,"Operational"
12.00,"00","BUFR table entries sequences","300004",,,"000018","Units reference sign",,,"Operational"
13.00,"00","BUFR table entries sequences","300004",,,"000019","Units reference value",,,"Operational"
14.00,"00","BUFR table entries sequences","300004",,,"000020","Element data width",,,"Operational"
15.00,"00","BUFR table entries sequences","300010",,,"300003","F, X, Y of descriptor to be added or defined",,,"Operational"
16.00,"00","BUFR table entries sequences","300010",,,"101000","Delayed replication of 1 descriptor",,,"Operational"
17.00,"00","BUFR table entries sequences","300010",,,"031001","Delayed descriptor replication factor",,,"Operational"
18.00,"00","BUFR table entries sequences","300010",,,"000030","Descriptor defining sequence",,,"Operational"
22.00,"00","BUFR table entries sequences","300015","(Code table definition)",,"000030","Descriptor defining sequence",,,"Operational"
23.00,"00","BUFR table entries sequences","300015","(Code table definition)",,"102000","Delayed replication of 2 descriptors",,,"Operational"
24.00,"00","BUFR table entries sequences","300015","(Code table definition)",,"031002","Extended delayed descriptor replication factor",,,"Operational"
25.00,"00","BUFR table entries sequences","300015","(Code table definition)",,"000024","Code figure",,,"Operational"
26.00,"00","BUFR table entries sequences","300015","(Code table definition)",,"000025","Code figure meaning",,,"Operational"
28.00,"00","BUFR table entries sequences","300016","(Flag table definition)",,"000030","Descriptor defining sequence",,,"Operational"
29.00,"00","BUFR table entries sequences","300016","(Flag table definition)",,"102000","Delayed replication of 2 descriptors",,,"Operational"
30.00,"00","BUFR table entries sequences","300016","(Flag table definition)",,"031001","Delayed descriptor replication factor",,,"Operational"
31.00,"00","BUFR table entries sequences","300016","(Flag table definition)",,"000026","Bit number",,,"Operational"
32.00,"00","BUFR table entries sequences","300016","(Flag table definition)",,"000027","Bit number meaning",,,"Operational"
34.00,"01","Location and identification sequences","301001","(WMO block and station numbers)",,"001001","WMO block number",,,"Operational"
35.00,"01","Location and identification sequences","301001","(WMO block and station numbers)",,"001002","WMO station number",,,"Operational"
36.00,"01","Location and identification sequences","301002",,,"001003","WMO Region number/geographical area",,,"Operational"
37.00,"01","Location and identification sequences","301002",,,"001004","WMO Region sub-area",,,"Operational"
38.00,"01","Location and identification sequences","301002",,,"001005","Buoy/platform identifier",,,"Operational"
39.00,"01","Location and identification sequences","301003","(Ship's call sign and motion)",,"001011","Ship or mobile land station identifier","Ship's call sign",,"Operational"
40.00,"01","Location and identification sequences","301003","(Ship's call sign and motion)",,"001012","Direction of motion of moving observing platform",,,"Operational"
41.00,"01","Location and identification sequences","301003","(Ship's call sign and motion)",,"001013","Speed of motion of moving observing platform",,,"Operational"
42.00,"01","Location and identification sequences","301004","(Surface station identification)",,"001001","WMO block number",,,"Operational"
43.00,"01","Location and identification sequences","301004","(Surface station identification)",,"001002","WMO station number",,,"Operational"
44.00,"01","Location and identification sequences","301004","(Surface station identification)",,"001015","Station or site name",,,"Operational"
45.00,"01","Location and identification sequences","301004","(Surface station identification)",,"002001","Type of station",,,"Operational"
46.00,"01","Location and identification sequences","301005","(Originating centre/sub-centre)",,"001035","Originating centre",,,"Operational"
47.00,"01","Location and identification sequences","301005","(Originating centre/sub-centre)",,"001034","Identification of originating/generating sub-centre",,,"Operational"
48.00,"01","Location and identification sequences","301011","(Year, month, day)",,"004001","Year",,,"Operational"
49.00,"01","Location and identification sequences","301011","(Year, month, day)",,"004002","Month",,,"Operational"
50.00,"01","Location and identification sequences","301011","(Year, month, day)",,"004003","Day",,,"Operational"
51.00,"01","Location and identification sequences","301012","(Hour, minute)",,"004004","Hour",,,"Operational"
52.00,"01","Location and identification sequences","301012","(Hour, minute)",,"004005","Minute",,,"Operational"
53.00,"01","Location and identification sequences","301013","(Hour, minute, second)",,"004004","Hour",,,"Operational"
54.00,"01","Location and identification sequences","301013","(Hour, minute, second)",,"004005","Minute",,,"Operational"
55.00,"01","Location and identification sequences","301013","(Hour, minute, second)",,"004006","Second",,,"Operational"
56.00,"01","Location and identification sequences","301014","(Time period)",,"102002","Replicate 2 descriptors 2 times",,,"Operational"
57.00,"01","Location and identification sequences","301014","(Time period)",,"301011","Year, month, day",,,"Operational"
58.00,"01","Location and identification sequences","301014","(Time period)",,"301012","Hour, minute",,,"Operational"
59.00,"01","Location and identification sequences","301021","(Latitude/longitude (high accuracy))",,"005001","Latitude (high accuracy)",,,"Operational"
60.00,"01","Location and identification sequences","301021","(Latitude/longitude (high accuracy))",,"006001","Longitude (high accuracy)",,,"Operational"
61.00,"01","Location and identification sequences","301022","(Latitude/longitude (high accuracy), height of station)",,"005001","Latitude (high accuracy)",,,"Operational"
62.00,"01","Location and identification sequences","301022","(Latitude/longitude (high accuracy), height of station)",,"006001","Longitude (high accuracy)",,,"Operational"
63.00,"01","Location and identification sequences","301022","(Latitude/longitude (high accuracy), height of station)",,"007001","Height of station",,,"Operational"
64.00,"01","Location and identification sequences","301023","(Latitude/longitude (coarse accuracy))",,"005002","Latitude (coarse accuracy)",,,"Operational"
65.00,"01","Location and identification sequences","301023","(Latitude/longitude (coarse accuracy))",,"006002","Longitude (coarse accuracy)",,,"Operational"
66.00,"01","Location and identification sequences","301024","(Latitude/longitude (coarse accuracy), height of station)",,"005002","Latitude (coarse accuracy)",,,"Operational"
67.00,"01","Location and identification sequences","301024","(Latitude/longitude (coarse accuracy), height of station)",,"006002","Longitude (coarse accuracy)",,,"Operational"
68.00,"01","Location and identification sequences","301024","(Latitude/longitude (coarse accuracy), height of station)",,"007001","Height of station",,,"Operational"
69.00,"01","Location and identification sequences","301025","(Latitude/longitude (coarse accuracy), day/time)",,"301023","Latitude/longitude (coarse accuracy)",,,"Operational"
70.00,"01","Location and identification sequences","301025","(Latitude/longitude (coarse accuracy), day/time)",,"004003","Day",,,"Operational"
71.00,"01","Location and identification sequences","301025","(Latitude/longitude (coarse accuracy), day/time)",,"301012","Hour, minute",,,"Operational"
72.00,"01","Location and identification sequences","301026","(Latitude/longitude (high accuracy), time period (day, hour, minute))",,"301021","Latitude/longitude (high accuracy)",,,"Operational"
73.00,"01","Location and identification sequences","301026","(Latitude/longitude (high accuracy), time period (day, hour, minute))",,"004003","Day","Time period in days",,"Operational"
74.00,"01","Location and identification sequences","301026","(Latitude/longitude (high accuracy), time period (day, hour, minute))",,"004003","Day",,,"Operational"
75.00,"01","Location and identification sequences","301026","(Latitude/longitude (high accuracy), time period (day, hour, minute))",,"004004","Hour","Time period in hours",,"Operational"
76.00,"01","Location and identification sequences","301026","(Latitude/longitude (high accuracy), time period (day, hour, minute))",,"004004","Hour",,,"Operational"
77.00,"01","Location and identification sequences","301026","(Latitude/longitude (high accuracy), time period (day, hour, minute))",,"004005","Minute","Time period in minutes",,"Operational"
78.00,"01","Location and identification sequences","301026","(Latitude/longitude (high accuracy), time period (day, hour, minute))",,"004005","Minute",,,"Operational"
79.00,"01","Location and identification sequences","301027","(Description of a feature in 3-D or 2-D)",,"008007","Dimensional significance","= 0 Point, = 1 Line, = 2 Area, = 3 Volume",,"Operational"
80.00,"01","Location and identification sequences","301027","(Description of a feature in 3-D or 2-D)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
81.00,"01","Location and identification sequences","301027","(Description of a feature in 3-D or 2-D)",,"031001","Delayed descriptor replication factor",,"(see Note 5)","Operational"
82.00,"01","Location and identification sequences","301027","(Description of a feature in 3-D or 2-D)",,"301028","Horizontal section of a feature described as a polygon, circle, line or point",,,"Operational"
83.00,"01","Location and identification sequences","301027","(Description of a feature in 3-D or 2-D)",,"008007","Dimensional significance","Set to missing (cancel)",,"Operational"
85.00,"01","Location and identification sequences","301028","(Horizontal section of a feature described as a polygon, circle, line or point)",,"008040","Flight level significance",,,"Operational"
86.00,"01","Location and identification sequences","301028","(Horizontal section of a feature described as a polygon, circle, line or point)",,"033042","Type of limit represented by following value",,,"Operational"
87.00,"01","Location and identification sequences","301028","(Horizontal section of a feature described as a polygon, circle, line or point)",,"007010","Flight level",,,"Operational"
88.00,"01","Location and identification sequences","301028","(Horizontal section of a feature described as a polygon, circle, line or point)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
89.00,"01","Location and identification sequences","301028","(Horizontal section of a feature described as a polygon, circle, line or point)",,"031002","Extended delayed descriptor replication factor",,"(see Note 6)","Operational"
90.00,"01","Location and identification sequences","301028","(Horizontal section of a feature described as a polygon, circle, line or point)",,"301023","Latitude/longitude (coarse accuracy)",,,"Operational"
91.00,"01","Location and identification sequences","301028","(Horizontal section of a feature described as a polygon, circle, line or point)",,"019007","Effective radius of feature",,"(see Note 7)","Operational"
92.00,"01","Location and identification sequences","301028","(Horizontal section of a feature described as a polygon, circle, line or point)",,"008040","Flight level significance","Set to missing (cancel)",,"Operational"
94.00,"01","Location and identification sequences","301029","(Identification)",,"001018","Short station or site name",,,"Operational"
95.00,"01","Location and identification sequences","301029","(Identification)",,"002001","Type of station",,,"Operational"
96.00,"01","Location and identification sequences","301029","(Identification)",,"301011","Year, month, day",,,"Operational"
97.00,"01","Location and identification sequences","301030","(Identification - with physical location)",,"001018","Short station or site name",,,"Operational"
98.00,"01","Location and identification sequences","301030","(Identification - with physical location)",,"002001","Type of station",,,"Operational"
99.00,"01","Location and identification sequences","301030","(Identification - with physical location)",,"301011","Year, month, day",,,"Operational"
100.00,"01","Location and identification sequences","301030","(Identification - with physical location)",,"301024","Latitude/longitude (coarse accuracy), height of station",,,"Operational"
101.00,"01","Location and identification sequences","301031","(Identification and type of station, date/time, location (high accuracy), height of station)",,"301001","WMO block and station numbers",,,"Operational"
102.00,"01","Location and identification sequences","301031","(Identification and type of station, date/time, location (high accuracy), height of station)",,"002001","Type of station",,,"Operational"
103.00,"01","Location and identification sequences","301031","(Identification and type of station, date/time, location (high accuracy), height of station)",,"301011","Year, month, day",,,"Operational"
104.00,"01","Location and identification sequences","301031","(Identification and type of station, date/time, location (high accuracy), height of station)",,"301012","Hour, minute",,,"Operational"
105.00,"01","Location and identification sequences","301031","(Identification and type of station, date/time, location (high accuracy), height of station)",,"301022","Latitude/longitude (high accuracy), height of station",,,"Operational"
106.00,"01","Location and identification sequences","301032","(Identification and type of station, date/time, location (coarse accuracy), height of station)",,"301001","WMO block and station numbers",,,"Operational"
107.00,"01","Location and identification sequences","301032","(Identification and type of station, date/time, location (coarse accuracy), height of station)",,"002001","Type of station",,,"Operational"
108.00,"01","Location and identification sequences","301032","(Identification and type of station, date/time, location (coarse accuracy), height of station)",,"301011","Year, month, day",,,"Operational"
109.00,"01","Location and identification sequences","301032","(Identification and type of station, date/time, location (coarse accuracy), height of station)",,"301012","Hour, minute",,,"Operational"
110.00,"01","Location and identification sequences","301032","(Identification and type of station, date/time, location (coarse accuracy), height of station)",,"301024","Latitude/longitude (coarse accuracy), height of station",,,"Operational"
111.00,"01","Location and identification sequences","301033","(Buoy/platform - fixed)",,"001005","Buoy/platform identifier",,,"Operational"
112.00,"01","Location and identification sequences","301033","(Buoy/platform - fixed)",,"002001","Type of station",,,"Operational"
113.00,"01","Location and identification sequences","301033","(Buoy/platform - fixed)",,"301011","Year, month, day",,,"Operational"
114.00,"01","Location and identification sequences","301033","(Buoy/platform - fixed)",,"301012","Hour, minute",,,"Operational"
115.00,"01","Location and identification sequences","301033","(Buoy/platform - fixed)",,"301021","Latitude/longitude (high accuracy)",,,"Operational"
116.00,"01","Location and identification sequences","301034","(Buoy/platform - fixed)",,"001005","Buoy/platform identifier",,,"Operational"
117.00,"01","Location and identification sequences","301034","(Buoy/platform - fixed)",,"002001","Type of station",,,"Operational"
118.00,"01","Location and identification sequences","301034","(Buoy/platform - fixed)",,"301011","Year, month, day",,,"Operational"
119.00,"01","Location and identification sequences","301034","(Buoy/platform - fixed)",,"301012","Hour, minute",,,"Operational"
120.00,"01","Location and identification sequences","301034","(Buoy/platform - fixed)",,"301023","Latitude/longitude (coarse accuracy)",,,"Operational"
121.00,"01","Location and identification sequences","301035","(Buoy/platform - moving)",,"001005","Buoy/platform identifier",,"<(see Note 4)>","Operational"
122.00,"01","Location and identification sequences","301035","(Buoy/platform - moving)",,"001012","Direction of motion of moving observing platform",,,"Operational"
123.00,"01","Location and identification sequences","301035","(Buoy/platform - moving)",,"001013","Speed of motion of moving observing platform",,,"Operational"
124.00,"01","Location and identification sequences","301035","(Buoy/platform - moving)",,"002001","Type of station",,,"Operational"
125.00,"01","Location and identification sequences","301035","(Buoy/platform - moving)",,"301011","Year, month, day",,,"Operational"
126.00,"01","Location and identification sequences","301035","(Buoy/platform - moving)",,"301012","Hour, minute",,,"Operational"
127.00,"01","Location and identification sequences","301035","(Buoy/platform - moving)",,"301023","Latitude/longitude (coarse accuracy)",,,"Operational"
128.00,"01","Location and identification sequences","301036","(Ship)",,"301003","Ship's call sign and motion",,,"Operational"
129.00,"01","Location and identification sequences","301036","(Ship)",,"002001","Type of station",,,"Operational"
130.00,"01","Location and identification sequences","301036","(Ship)",,"301011","Year, month, day",,,"Operational"
131.00,"01","Location and identification sequences","301036","(Ship)",,"301012","Hour, minute",,,"Operational"
132.00,"01","Location and identification sequences","301036","(Ship)",,"301023","Latitude/longitude (coarse accuracy)",,,"Operational"
133.00,"01","Location and identification sequences","301037","(Land station for vertical soundings)",,"301001","WMO block and station numbers",,,"Operational"
134.00,"01","Location and identification sequences","301037","(Land station for vertical soundings)",,"002011","Radiosonde type",,,"Operational"
135.00,"01","Location and identification sequences","301037","(Land station for vertical soundings)",,"002012","Radiosonde computational method",,,"Operational"
136.00,"01","Location and identification sequences","301037","(Land station for vertical soundings)",,"301011","Year, month, day",,,"Operational"
137.00,"01","Location and identification sequences","301037","(Land station for vertical soundings)",,"301012","Hour, minute",,,"Operational"
138.00,"01","Location and identification sequences","301037","(Land station for vertical soundings)",,"301022","Latitude/longitude (high accuracy), height of station",,,"Operational"
139.00,"01","Location and identification sequences","301038","(Land station for vertical soundings)",,"301001","WMO block and station numbers",,,"Operational"
140.00,"01","Location and identification sequences","301038","(Land station for vertical soundings)",,"002011","Radiosonde type",,,"Operational"
141.00,"01","Location and identification sequences","301038","(Land station for vertical soundings)",,"002012","Radiosonde computational method",,,"Operational"
142.00,"01","Location and identification sequences","301038","(Land station for vertical soundings)",,"301011","Year, month, day",,,"Operational"
143.00,"01","Location and identification sequences","301038","(Land station for vertical soundings)",,"301012","Hour, minute",,,"Operational"
144.00,"01","Location and identification sequences","301038","(Land station for vertical soundings)",,"301024","Latitude/longitude (coarse accuracy), height of station",,,"Operational"
145.00,"01","Location and identification sequences","301039","(Ship for vertical soundings)",,"301003","Ship's call sign and motion",,,"Operational"
146.00,"01","Location and identification sequences","301039","(Ship for vertical soundings)",,"002011","Radiosonde type",,,"Operational"
147.00,"01","Location and identification sequences","301039","(Ship for vertical soundings)",,"002012","Radiosonde computational method",,,"Operational"
148.00,"01","Location and identification sequences","301039","(Ship for vertical soundings)",,"301011","Year, month, day",,,"Operational"
149.00,"01","Location and identification sequences","301039","(Ship for vertical soundings)",,"301012","Hour, minute",,,"Operational"
150.00,"01","Location and identification sequences","301039","(Ship for vertical soundings)",,"301023","Latitude/longitude (coarse accuracy)",,,"Operational"
151.00,"01","Location and identification sequences","301040","(Ship for vertical soundings)",,"301003","Ship's call sign and motion",,,"Operational"
152.00,"01","Location and identification sequences","301040","(Ship for vertical soundings)",,"002011","Radiosonde type",,,"Operational"
153.00,"01","Location and identification sequences","301040","(Ship for vertical soundings)",,"002012","Radiosonde computational method",,,"Operational"
154.00,"01","Location and identification sequences","301040","(Ship for vertical soundings)",,"301011","Year, month, day",,,"Operational"
155.00,"01","Location and identification sequences","301040","(Ship for vertical soundings)",,"301012","Hour, minute",,,"Operational"
156.00,"01","Location and identification sequences","301040","(Ship for vertical soundings)",,"301024","Latitude/longitude (coarse accuracy), height of station",,,"Operational"
157.00,"01","Location and identification sequences","301041","(Satellite identifier, instrument, data-processing technique, date/time)",,"001007","Satellite identifier",,,"Operational"
158.00,"01","Location and identification sequences","301041","(Satellite identifier, instrument, data-processing technique, date/time)",,"002021","Satellite instrument data used in processing",,,"Operational"
159.00,"01","Location and identification sequences","301041","(Satellite identifier, instrument, data-processing technique, date/time)",,"002022","Satellite data-processing technique used",,,"Operational"
160.00,"01","Location and identification sequences","301041","(Satellite identifier, instrument, data-processing technique, date/time)",,"301011","Year, month, day",,,"Operational"
161.00,"01","Location and identification sequences","301041","(Satellite identifier, instrument, data-processing technique, date/time)",,"301012","Hour, minute",,,"Operational"
162.00,"01","Location and identification sequences","301042","(Satellite identifier, instrument, data-processing technique, date/time, location)",,"301041","Satellite identifier, instrument, data-processing technique, date/time",,,"Operational"
163.00,"01","Location and identification sequences","301042","(Satellite identifier, instrument, data-processing technique, date/time, location)",,"301021","Latitude/longitude (high accuracy)",,,"Operational"
164.00,"01","Location and identification sequences","301043","(Satellite identifier, wind computation method, date/time, location)",,"001007","Satellite identifier",,,"Operational"
165.00,"01","Location and identification sequences","301043","(Satellite identifier, wind computation method, date/time, location)",,"002023","Satellite-derived wind computation method",,,"Operational"
166.00,"01","Location and identification sequences","301043","(Satellite identifier, wind computation method, date/time, location)",,"301011","Year, month, day",,,"Operational"
167.00,"01","Location and identification sequences","301043","(Satellite identifier, wind computation method, date/time, location)",,"301013","Hour, minute, second",,,"Operational"
168.00,"01","Location and identification sequences","301043","(Satellite identifier, wind computation method, date/time, location)",,"301021","Latitude/longitude (high accuracy)",,,"Operational"
169.00,"01","Location and identification sequences","301044","(Satellite identifier, humidity computation method, date/time, location)",,"001007","Satellite identifier",,,"Operational"
170.00,"01","Location and identification sequences","301044","(Satellite identifier, humidity computation method, date/time, location)",,"002024","Integrated mean humidity computational method",,,"Operational"
171.00,"01","Location and identification sequences","301044","(Satellite identifier, humidity computation method, date/time, location)",,"301011","Year, month, day",,,"Operational"
172.00,"01","Location and identification sequences","301044","(Satellite identifier, humidity computation method, date/time, location)",,"301013","Hour, minute, second",,,"Operational"
173.00,"01","Location and identification sequences","301044","(Satellite identifier, humidity computation method, date/time, location)",,"301021","Latitude/longitude (high accuracy)",,,"Operational"
174.00,"01","Location and identification sequences","301045","(Satellite location and velocity)",,"301011","Year, month, day",,,"Operational"
175.00,"01","Location and identification sequences","301045","(Satellite location and velocity)",,"301012","Hour, minute",,,"Operational"
176.00,"01","Location and identification sequences","301045","(Satellite location and velocity)",,"201138","Change data width","16 bits long",,"Operational"
177.00,"01","Location and identification sequences","301045","(Satellite location and velocity)",,"202131","Change scale","Scale: 3",,"Operational"
178.00,"01","Location and identification sequences","301045","(Satellite location and velocity)",,"004006","Second",,,"Operational"
179.00,"01","Location and identification sequences","301045","(Satellite location and velocity)",,"201000","Change data width","Cancel",,"Operational"
180.00,"01","Location and identification sequences","301045","(Satellite location and velocity)",,"202000","Change scale","Cancel",,"Operational"
181.00,"01","Location and identification sequences","301045","(Satellite location and velocity)",,"304030","Location of platform","Relative to the Earth’s centre",,"Operational"
182.00,"01","Location and identification sequences","301045","(Satellite location and velocity)",,"304031","Speed of platform","Relative to the Earth’s centre",,"Operational"
184.00,"01","Location and identification sequences","301046","(Satellite identifier, direction of motion, sensor, model function, software, resolution)",,"001007","Satellite identifier",,,"Operational"
185.00,"01","Location and identification sequences","301046","(Satellite identifier, direction of motion, sensor, model function, software, resolution)",,"001012","Direction of motion of moving observing platform",,,"Operational"
186.00,"01","Location and identification sequences","301046","(Satellite identifier, direction of motion, sensor, model function, software, resolution)",,"002048","Satellite sensor indicator",,,"Operational"
187.00,"01","Location and identification sequences","301046","(Satellite identifier, direction of motion, sensor, model function, software, resolution)",,"021119","Wind scatterometer geophysical model function",,,"Operational"
188.00,"01","Location and identification sequences","301046","(Satellite identifier, direction of motion, sensor, model function, software, resolution)",,"025060","Software identification",,,"Operational"
189.00,"01","Location and identification sequences","301046","(Satellite identifier, direction of motion, sensor, model function, software, resolution)",,"202124","Change scale",,,"Operational"
190.00,"01","Location and identification sequences","301046","(Satellite identifier, direction of motion, sensor, model function, software, resolution)",,"002026","Cross-track resolution",,,"Operational"
191.00,"01","Location and identification sequences","301046","(Satellite identifier, direction of motion, sensor, model function, software, resolution)",,"002027","Along-track resolution",,,"Operational"
192.00,"01","Location and identification sequences","301046","(Satellite identifier, direction of motion, sensor, model function, software, resolution)",,"202000","Change scale","Cancel",,"Operational"
193.00,"01","Location and identification sequences","301046","(Satellite identifier, direction of motion, sensor, model function, software, resolution)",,"005040","Orbit number",,,"Operational"
195.00,"01","Location and identification sequences","301047","(ERS product header)",,"001007","Satellite identifier",,,"Operational"
196.00,"01","Location and identification sequences","301047","(ERS product header)",,"025060","Software identification",,,"Operational"
197.00,"01","Location and identification sequences","301047","(ERS product header)",,"001033","Identification of originating/generating centre",,,"Operational"
198.00,"01","Location and identification sequences","301047","(ERS product header)",,"001034","Identification of originating/generating sub-centre",,,"Operational"
199.00,"01","Location and identification sequences","301047","(ERS product header)",,"001012","Direction of motion of moving observing platform",,,"Operational"
200.00,"01","Location and identification sequences","301047","(ERS product header)",,"301045","Satellite location and velocity",,,"Operational"
201.00,"01","Location and identification sequences","301047","(ERS product header)",,"002021","Satellite instrument data used in processing",,,"Operational"
202.00,"01","Location and identification sequences","301047","(ERS product header)",,"301011","Year, month, day",,,"Operational"
203.00,"01","Location and identification sequences","301047","(ERS product header)",,"301012","Hour, minute",,,"Operational"
204.00,"01","Location and identification sequences","301047","(ERS product header)",,"201138","Change data width","16 bits long",,"Operational"
205.00,"01","Location and identification sequences","301047","(ERS product header)",,"202131","Change scale","Scale: 3",,"Operational"
206.00,"01","Location and identification sequences","301047","(ERS product header)",,"004006","Second",,,"Operational"
207.00,"01","Location and identification sequences","301047","(ERS product header)",,"201000","Change data width","Cancel",,"Operational"
208.00,"01","Location and identification sequences","301047","(ERS product header)",,"202000","Change scale","Cancel",,"Operational"
209.00,"01","Location and identification sequences","301047","(ERS product header)",,"301023","Latitude/longitude (coarse accuracy)",,,"Operational"
211.00,"01","Location and identification sequences","301048","(Radar parameters)",,"002104","Antenna polarization",,,"Operational"
212.00,"01","Location and identification sequences","301048","(Radar parameters)",,"002121","Mean frequency",,,"Operational"
213.00,"01","Location and identification sequences","301048","(Radar parameters)",,"002113","Number of azimuth looks",,,"Operational"
214.00,"01","Location and identification sequences","301048","(Radar parameters)",,"002026","Cross-track resolution",,,"Operational"
215.00,"01","Location and identification sequences","301048","(Radar parameters)",,"002027","Along-track resolution",,,"Operational"
216.00,"01","Location and identification sequences","301048","(Radar parameters)",,"002111","Radar incidence angle",,,"Operational"
217.00,"01","Location and identification sequences","301048","(Radar parameters)",,"002140","Satellite radar beam azimuth angle",,,"Operational"
218.00,"01","Location and identification sequences","301048","(Radar parameters)",,"202127","Change scale","Scale: -1",,"Operational"
219.00,"01","Location and identification sequences","301048","(Radar parameters)",,"001013","Speed of motion of moving observing platform","Radar platform velocity",,"Operational"
220.00,"01","Location and identification sequences","301048","(Radar parameters)",,"202126","Change scale","Scale: -2",,"Operational"
221.00,"01","Location and identification sequences","301048","(Radar parameters)",,"007001","Height of station","Radar platform altitude",,"Operational"
222.00,"01","Location and identification sequences","301048","(Radar parameters)",,"202000","Change scale","Cancel",,"Operational"
223.00,"01","Location and identification sequences","301048","(Radar parameters)",,"025010","Clutter treatment",,,"Operational"
224.00,"01","Location and identification sequences","301048","(Radar parameters)",,"021064","Clutter noise estimate",,,"Operational"
226.00,"01","Location and identification sequences","301049","(Radar beam data)",,"002111","Radar incidence angle",,,"Operational"
227.00,"01","Location and identification sequences","301049","(Radar beam data)",,"002112","Radar look angle",,,"Operational"
228.00,"01","Location and identification sequences","301049","(Radar beam data)",,"021062","Backscatter",,,"Operational"
229.00,"01","Location and identification sequences","301049","(Radar beam data)",,"021063","Radiometric resolution (noise value)",,,"Operational"
230.00,"01","Location and identification sequences","301049","(Radar beam data)",,"021065","Missing packet counter",,,"Operational"
231.00,"01","Location and identification sequences","301051","(Flight number, navigational system, date/time, location, phase of flight)",,"001006","Aircraft flight number",,,"Operational"
232.00,"01","Location and identification sequences","301051","(Flight number, navigational system, date/time, location, phase of flight)",,"002061","Aircraft navigational system",,,"Operational"
233.00,"01","Location and identification sequences","301051","(Flight number, navigational system, date/time, location, phase of flight)",,"301011","Year, month, day",,,"Operational"
234.00,"01","Location and identification sequences","301051","(Flight number, navigational system, date/time, location, phase of flight)",,"301012","Hour, minute",,,"Operational"
235.00,"01","Location and identification sequences","301051","(Flight number, navigational system, date/time, location, phase of flight)",,"301021","Latitude/longitude (high accuracy)",,,"Operational"
236.00,"01","Location and identification sequences","301051","(Flight number, navigational system, date/time, location, phase of flight)",,"008004","Phase of aircraft flight",,,"Operational"
237.00,"01","Location and identification sequences","301055","(Identification and type of station, date/time, location (high accuracy), movement)",,"001005","Buoy/platform identifier",,,"Operational"
238.00,"01","Location and identification sequences","301055","(Identification and type of station, date/time, location (high accuracy), movement)",,"002001","Type of station",,,"Operational"
239.00,"01","Location and identification sequences","301055","(Identification and type of station, date/time, location (high accuracy), movement)",,"301011","Year, month, day",,,"Operational"
240.00,"01","Location and identification sequences","301055","(Identification and type of station, date/time, location (high accuracy), movement)",,"301012","Hour, minute",,,"Operational"
241.00,"01","Location and identification sequences","301055","(Identification and type of station, date/time, location (high accuracy), movement)",,"301021","Latitude/longitude (high accuracy)",,,"Operational"
242.00,"01","Location and identification sequences","301055","(Identification and type of station, date/time, location (high accuracy), movement)",,"001012","Direction of motion of moving observing platform",,,"Operational"
243.00,"01","Location and identification sequences","301055","(Identification and type of station, date/time, location (high accuracy), movement)",,"001014","Platform drift speed (high precision)",,,"Operational"
244.00,"01","Location and identification sequences","301058","(Universal lightning event)","Date/time of lightning event","301011","Year, month, day",,,"Operational"
245.00,"01","Location and identification sequences","301058","(Universal lightning event)","Date/time of lightning event","301012","Hour, minute",,,"Operational"
246.00,"01","Location and identification sequences","301058","(Universal lightning event)","Date/time of lightning event","201152","Change data width",,,"Operational"
247.00,"01","Location and identification sequences","301058","(Universal lightning event)","Date/time of lightning event","202135","Change scale",,,"Operational"
248.00,"01","Location and identification sequences","301058","(Universal lightning event)","Date/time of lightning event","004006","Second",,,"Operational"
249.00,"01","Location and identification sequences","301058","(Universal lightning event)","Date/time of lightning event","202000","Change scale",,,"Operational"
250.00,"01","Location and identification sequences","301058","(Universal lightning event)","Date/time of lightning event","201000","Change data width",,,"Operational"
251.00,"01","Location and identification sequences","301058","(Universal lightning event)","Horizontal and vertical coordinates of lightning event","301021","Latitude/longitude (high accuracy)",,,"Operational"
252.00,"01","Location and identification sequences","301058","(Universal lightning event)","Horizontal and vertical coordinates of lightning event","020111","x-axis error ellipse major component",,,"Operational"
253.00,"01","Location and identification sequences","301058","(Universal lightning event)","Horizontal and vertical coordinates of lightning event","020112","y-axis error ellipse minor component",,,"Operational"
254.00,"01","Location and identification sequences","301058","(Universal lightning event)","Horizontal and vertical coordinates of lightning event","020113","z-axis error ellipse component",,,"Operational"
255.00,"01","Location and identification sequences","301058","(Universal lightning event)","Horizontal and vertical coordinates of lightning event","020114","Angle of x-axis in error ellipse",,,"Operational"
256.00,"01","Location and identification sequences","301058","(Universal lightning event)","Horizontal and vertical coordinates of lightning event","020115","Angle of z-axis in error ellipse",,,"Operational"
257.00,"01","Location and identification sequences","301058","(Universal lightning event)","Horizontal and vertical coordinates of lightning event","020116","Emission height of cloud stroke",,,"Operational"
258.00,"01","Location and identification sequences","301058","(Universal lightning event)","Emission information","020117","Amplitude of lightning strike",,,"Operational"
259.00,"01","Location and identification sequences","301058","(Universal lightning event)","Emission information","020118","Lightning detection error",,,"Operational"
260.00,"01","Location and identification sequences","301058","(Universal lightning event)","Emission information","020119","Lightning discharge polarity",,,"Operational"
261.00,"01","Location and identification sequences","301058","(Universal lightning event)","Emission information","025035","Decision method for polarity","V or A",,"Operational"
262.00,"01","Location and identification sequences","301058","(Universal lightning event)","Emission information","020121","Threshold value for polarity decision",,,"Operational"
263.00,"01","Location and identification sequences","301058","(Universal lightning event)","Emission information","020122","Threshold value for polarity decision",,,"Operational"
264.00,"01","Location and identification sequences","301058","(Universal lightning event)","Emission information","020123","Minimum threshold for detection",,,"Operational"
265.00,"01","Location and identification sequences","301058","(Universal lightning event)","Emission information","020124","Lightning stroke or flash",,,"Operational"
266.00,"01","Location and identification sequences","301058","(Universal lightning event)","Emission information","025175","Modified residual",,,"Operational"
267.00,"01","Location and identification sequences","301058","(Universal lightning event)","Emission information","020023","Other weather phenomena","Cloud to ground or cloud to cloud identification",,"Operational"
268.00,"01","Location and identification sequences","301058","(Universal lightning event)","Sensor processing","025063","Central processor or system identifier",,,"Operational"
269.00,"01","Location and identification sequences","301058","(Universal lightning event)","Sensor processing","202136","Change scale",,,"Operational"
270.00,"01","Location and identification sequences","301058","(Universal lightning event)","Sensor processing","201136","Change data width",,,"Operational"
271.00,"01","Location and identification sequences","301058","(Universal lightning event)","Sensor processing","002121","Mean frequency","Define centre frequency, if used",,"Operational"
272.00,"01","Location and identification sequences","301058","(Universal lightning event)","Sensor processing","201000","Change data width",,,"Operational"
273.00,"01","Location and identification sequences","301058","(Universal lightning event)","Sensor processing","202000","Change scale",,,"Operational"
274.00,"01","Location and identification sequences","301058","(Universal lightning event)","Sensor processing","025061","Software identification and version number",,,"Operational"
275.00,"01","Location and identification sequences","301058","(Universal lightning event)","Sensor processing","002184","Type of lightning detection sensor",,,"Operational"
276.00,"01","Location and identification sequences","301058","(Universal lightning event)","Sensor processing","002189","Capability to discriminate lightning strikes",,,"Operational"
277.00,"01","Location and identification sequences","301058","(Universal lightning event)","Sensor processing","025036","Atmospherics location method",,,"Operational"
278.00,"01","Location and identification sequences","301058","(Universal lightning event)","Sensor processing","101000","Delayed replication of 1 descriptor",,,"Operational"
279.00,"01","Location and identification sequences","301058","(Universal lightning event)","Sensor processing","031002","Extended delayed descriptor replication factor","Number of sensors contributing",,"Operational"
280.00,"01","Location and identification sequences","301058","(Universal lightning event)","Sensor processing","301059","Identification of sensor site and instrumentation",,,"Operational"
282.00,"01","Location and identification sequences","301059","(Identification of sensor site and instrumentation)",,"301021","Latitude/longitude (high accuracy)","Sensor",,"Operational"
283.00,"01","Location and identification sequences","301059","(Identification of sensor site and instrumentation)",,"007030","Height of station ground above mean sea level",,,"Operational"
284.00,"01","Location and identification sequences","301059","(Identification of sensor site and instrumentation)",,"007032","Height of sensor above local ground (or deck of marine platform)","Sensor for lightning",,"Operational"
285.00,"01","Location and identification sequences","301062","(Radar location(s))",,"101000","Delayed replication of 1 descriptor",,,"Operational"
286.00,"01","Location and identification sequences","301062","(Radar location(s))",,"031001","Delayed descriptor replication factor",,,"Operational"
287.00,"01","Location and identification sequences","301062","(Radar location(s))",,"301001","WMO block and station numbers",,,"Operational"
289.00,"01","Location and identification sequences","301065","(ACARS identification)",,"001006","Aircraft flight number",,"(see Note 1)","Operational"
290.00,"01","Location and identification sequences","301065","(ACARS identification)",,"001008","Aircraft registration number or other identification",,"(see Note 1)","Operational"
291.00,"01","Location and identification sequences","301065","(ACARS identification)",,"002001","Type of station",,,"Operational"
292.00,"01","Location and identification sequences","301065","(ACARS identification)",,"002002","Type of instrumentation for wind measurement",,,"Operational"
293.00,"01","Location and identification sequences","301065","(ACARS identification)",,"002005","Precision of temperature observation",,,"Operational"
294.00,"01","Location and identification sequences","301065","(ACARS identification)",,"002062","Type of aircraft data relay system",,,"Operational"
295.00,"01","Location and identification sequences","301065","(ACARS identification)",,"002070","Original specification of latitude/longitude",,,"Operational"
296.00,"01","Location and identification sequences","301065","(ACARS identification)",,"002065","ACARS ground-receiving station",,,"Operational"
297.00,"01","Location and identification sequences","301066","(ACARS location)",,"301011","Year, month, day",,,"Operational"
298.00,"01","Location and identification sequences","301066","(ACARS location)",,"301013","Hour, minute, second",,,"Operational"
299.00,"01","Location and identification sequences","301066","(ACARS location)",,"301023","Latitude/longitude (coarse accuracy)",,,"Operational"
300.00,"01","Location and identification sequences","301066","(ACARS location)",,"007004","Pressure",,,"Operational"
301.00,"01","Location and identification sequences","301066","(ACARS location)",,"002064","Aircraft roll angle quality",,,"Operational"
302.00,"01","Location and identification sequences","301066","(ACARS location)",,"008004","Phase of aircraft flight",,,"Operational"
303.00,"01","Location and identification sequences","301070","(Ozone instrumentation - Brewer spectrophotometer)",,"002143","Ozone instrument type",,,"Operational"
304.00,"01","Location and identification sequences","301070","(Ozone instrumentation - Brewer spectrophotometer)",,"002142","Ozone instrument serial number/identification",,,"Operational"
305.00,"01","Location and identification sequences","301070","(Ozone instrumentation - Brewer spectrophotometer)",,"002144","Light source type for Brewer spectrophotometer",,,"Operational"
306.00,"01","Location and identification sequences","301071","(Satellite identifier/Generating resolution)",,"001007","Satellite identifier",,,"Operational"
307.00,"01","Location and identification sequences","301071","(Satellite identifier/Generating resolution)",,"001031","Identification of originating/generating centre",,,"Operational"
308.00,"01","Location and identification sequences","301071","(Satellite identifier/Generating resolution)",,"002020","Satellite classification",,,"Operational"
309.00,"01","Location and identification sequences","301071","(Satellite identifier/Generating resolution)",,"002028","Segment size at nadir in x-direction",,,"Operational"
310.00,"01","Location and identification sequences","301071","(Satellite identifier/Generating resolution)",,"002029","Segment size at nadir in y-direction",,,"Operational"
311.00,"01","Location and identification sequences","301072","(Satellite identification)",,"301071","Satellite identifier/Generating resolution",,,"Operational"
312.00,"01","Location and identification sequences","301072","(Satellite identification)",,"301011","Year, month, day",,,"Operational"
313.00,"01","Location and identification sequences","301072","(Satellite identification)",,"301013","Hour, minute, second",,,"Operational"
314.00,"01","Location and identification sequences","301072","(Satellite identification)",,"301021","Latitude/longitude (high accuracy)",,,"Operational"
315.00,"01","Location and identification sequences","301074","(Ozone instrumentation - Dobson spectrophotometer)",,"002143","Ozone instrument type",,,"Operational"
316.00,"01","Location and identification sequences","301074","(Ozone instrumentation - Dobson spectrophotometer)",,"002142","Ozone instrument serial number/identification",,,"Operational"
317.00,"01","Location and identification sequences","301074","(Ozone instrumentation - Dobson spectrophotometer)",,"002145","Wavelength setting for Dobson instruments",,,"Operational"
318.00,"01","Location and identification sequences","301074","(Ozone instrumentation - Dobson spectrophotometer)",,"002146","Source conditions for Dobson instruments",,,"Operational"
319.00,"01","Location and identification sequences","301075","(Sounding identification)",,"301001","WMO block and station numbers",,,"Operational"
320.00,"01","Location and identification sequences","301075","(Sounding identification)",,"001015","Station or site name",,,"Operational"
321.00,"01","Location and identification sequences","301075","(Sounding identification)",,"301024","Latitude/longitude (coarse accuracy), height of station",,,"Operational"
322.00,"01","Location and identification sequences","301075","(Sounding identification)",,"008021","Time significance","= 18 Launch time",,"Operational"
323.00,"01","Location and identification sequences","301075","(Sounding identification)",,"301011","Year, month, day",,,"Operational"
324.00,"01","Location and identification sequences","301075","(Sounding identification)",,"301012","Hour, minute",,,"Operational"
325.00,"01","Location and identification sequences","301076","(Ozone sounding instrumentation)",,"002011","Radiosonde type",,,"Operational"
326.00,"01","Location and identification sequences","301076","(Ozone sounding instrumentation)",,"002143","Ozone instrument type",,,"Operational"
327.00,"01","Location and identification sequences","301076","(Ozone sounding instrumentation)",,"002142","Ozone instrument serial number/identification",,,"Operational"
328.00,"01","Location and identification sequences","301089","(National station identification)",,"001101","State identifier",,,"Operational"
329.00,"01","Location and identification sequences","301089","(National station identification)",,"001102","National station number",,,"Operational"
330.00,"01","Location and identification sequences","301090","(Surface station identification; time, horizontal and vertical coordinates)",,"301004","Surface station identification",,,"Operational"
331.00,"01","Location and identification sequences","301090","(Surface station identification; time, horizontal and vertical coordinates)",,"301011","Year, month, day",,,"Operational"
332.00,"01","Location and identification sequences","301090","(Surface station identification; time, horizontal and vertical coordinates)",,"301012","Hour, minute",,,"Operational"
333.00,"01","Location and identification sequences","301090","(Surface station identification; time, horizontal and vertical coordinates)",,"301021","Latitude/longitude (high accuracy)",,,"Operational"
334.00,"01","Location and identification sequences","301090","(Surface station identification; time, horizontal and vertical coordinates)",,"007030","Height of station ground above mean sea level",,,"Operational"
335.00,"01","Location and identification sequences","301090","(Surface station identification; time, horizontal and vertical coordinates)",,"007031","Height of barometer above mean sea level",,,"Operational"
336.00,"01","Location and identification sequences","301091","(Surface station instrumentation)",,"002180","Main present weather detecting system",,,"Operational"
337.00,"01","Location and identification sequences","301091","(Surface station instrumentation)",,"002181","Supplementary present weather sensor",,,"Operational"
338.00,"01","Location and identification sequences","301091","(Surface station instrumentation)",,"002182","Visibility measurement system",,,"Operational"
339.00,"01","Location and identification sequences","301091","(Surface station instrumentation)",,"002183","Cloud detection system",,,"Operational"
340.00,"01","Location and identification sequences","301091","(Surface station instrumentation)",,"002184","Type of lightning detection sensor",,,"Operational"
341.00,"01","Location and identification sequences","301091","(Surface station instrumentation)",,"002179","Type of sky condition algorithm",,,"Operational"
342.00,"01","Location and identification sequences","301091","(Surface station instrumentation)",,"002186","Capability to detect precipitation phenomena",,,"Operational"
343.00,"01","Location and identification sequences","301091","(Surface station instrumentation)",,"002187","Capability to detect other weather phenomena",,,"Operational"
344.00,"01","Location and identification sequences","301091","(Surface station instrumentation)",,"002188","Capability to detect obscuration",,,"Operational"
345.00,"01","Location and identification sequences","301091","(Surface station instrumentation)",,"002189","Capability to discriminate lightning strikes",,,"Operational"
346.00,"01","Location and identification sequences","301092","(Mobile surface station identification, date/time, horizontal and vertical coordinates)",,"001011","Ship or mobile land station identifier",,,"Operational"
347.00,"01","Location and identification sequences","301092","(Mobile surface station identification, date/time, horizontal and vertical coordinates)",,"001003","WMO Region number/geographical area",,,"Operational"
348.00,"01","Location and identification sequences","301092","(Mobile surface station identification, date/time, horizontal and vertical coordinates)",,"002001","Type of station",,,"Operational"
349.00,"01","Location and identification sequences","301092","(Mobile surface station identification, date/time, horizontal and vertical coordinates)",,"301011","Year, month, day",,,"Operational"
350.00,"01","Location and identification sequences","301092","(Mobile surface station identification, date/time, horizontal and vertical coordinates)",,"301012","Hour, minute",,,"Operational"
351.00,"01","Location and identification sequences","301092","(Mobile surface station identification, date/time, horizontal and vertical coordinates)",,"301021","Latitude/longitude (high accuracy)",,,"Operational"
352.00,"01","Location and identification sequences","301092","(Mobile surface station identification, date/time, horizontal and vertical coordinates)",,"007030","Height of station ground above mean sea level",,,"Operational"
353.00,"01","Location and identification sequences","301092","(Mobile surface station identification, date/time, horizontal and vertical coordinates)",,"007031","Height of barometer above mean sea level",,,"Operational"
354.00,"01","Location and identification sequences","301092","(Mobile surface station identification, date/time, horizontal and vertical coordinates)",,"033024","Station elevation quality mark (for mobile stations)",,,"Operational"
355.00,"01","Location and identification sequences","301093","(Ship identification, movement, date/time, horizontal and vertical coordinates)",,"301036","Ship","Ship identification",,"Operational"
356.00,"01","Location and identification sequences","301093","(Ship identification, movement, date/time, horizontal and vertical coordinates)",,"007030","Height of station ground above mean sea level",,,"Operational"
357.00,"01","Location and identification sequences","301093","(Ship identification, movement, date/time, horizontal and vertical coordinates)",,"007031","Height of barometer above mean sea level",,,"Operational"
358.00,"01","Location and identification sequences","301110","(Identification of launch site and instrumentation for wind measurements)",,"301001","WMO block and station numbers",,,"Operational"
359.00,"01","Location and identification sequences","301110","(Identification of launch site and instrumentation for wind measurements)",,"001011","Ship or mobile land station identifier",,,"Operational"
360.00,"01","Location and identification sequences","301110","(Identification of launch site and instrumentation for wind measurements)",,"002011","Radiosonde type",,,"Operational"
361.00,"01","Location and identification sequences","301110","(Identification of launch site and instrumentation for wind measurements)",,"002014","Tracking technique/status of system used",,,"Operational"
362.00,"01","Location and identification sequences","301110","(Identification of launch site and instrumentation for wind measurements)",,"002003","Type of measuring equipment used",,,"Operational"
363.00,"01","Location and identification sequences","301111","(Identification of launch site and instrumentation for P, T, U and wind measurements)",,"301001","WMO block and station numbers",,,"Operational"
364.00,"01","Location and identification sequences","301111","(Identification of launch site and instrumentation for P, T, U and wind measurements)",,"001011","Ship or mobile land station identifier",,,"Operational"
365.00,"01","Location and identification sequences","301111","(Identification of launch site and instrumentation for P, T, U and wind measurements)",,"002011","Radiosonde type",,,"Operational"
366.00,"01","Location and identification sequences","301111","(Identification of launch site and instrumentation for P, T, U and wind measurements)",,"002013","Solar and infrared radiation correction",,,"Operational"
367.00,"01","Location and identification sequences","301111","(Identification of launch site and instrumentation for P, T, U and wind measurements)",,"002014","Tracking technique/status of system used",,,"Operational"
368.00,"01","Location and identification sequences","301111","(Identification of launch site and instrumentation for P, T, U and wind measurements)",,"002003","Type of measuring equipment used",,,"Operational"
369.00,"01","Location and identification sequences","301112","(Identification of launch point and instrumentation of dropsonde)",,"001006","Aircraft flight number",,,"Operational"
370.00,"01","Location and identification sequences","301112","(Identification of launch point and instrumentation of dropsonde)",,"002011","Radiosonde type",,,"Operational"
371.00,"01","Location and identification sequences","301112","(Identification of launch point and instrumentation of dropsonde)",,"002013","Solar and infrared radiation correction",,,"Operational"
372.00,"01","Location and identification sequences","301112","(Identification of launch point and instrumentation of dropsonde)",,"002014","Tracking technique/status of system used",,,"Operational"
373.00,"01","Location and identification sequences","301112","(Identification of launch point and instrumentation of dropsonde)",,"002003","Type of measuring equipment used",,,"Operational"
374.00,"01","Location and identification sequences","301113","(Date/time of launch)",,"008021","Time significance","= 18 Launch time","<(see Note 3)>","Operational"
375.00,"01","Location and identification sequences","301113","(Date/time of launch)",,"301011","Year, month, day","Launch time",,"Operational"
376.00,"01","Location and identification sequences","301113","(Date/time of launch)",,"301013","Hour, minute, second","Launch time",,"Operational"
377.00,"01","Location and identification sequences","301114","(Horizontal and vertical coordinates of launch site)",,"301021","Latitude/longitude (high accuracy)",,,"Operational"
378.00,"01","Location and identification sequences","301114","(Horizontal and vertical coordinates of launch site)",,"007030","Height of station ground above mean sea level",,,"Operational"
379.00,"01","Location and identification sequences","301114","(Horizontal and vertical coordinates of launch site)",,"007031","Height of barometer above mean sea level",,,"Operational"
380.00,"01","Location and identification sequences","301114","(Horizontal and vertical coordinates of launch site)",,"007007","Height","Release of sonde above mean sea level",,"Operational"
381.00,"01","Location and identification sequences","301114","(Horizontal and vertical coordinates of launch site)",,"033024","Station elevation quality mark (for mobile stations)",,,"Operational"
382.00,"01","Location and identification sequences","301120","(Radiosonde abbreviated header and launch information)",,"301001","WMO block and station numbers",,,"Operational"
383.00,"01","Location and identification sequences","301120","(Radiosonde abbreviated header and launch information)",,"001094","WBAN number",,,"Operational"
384.00,"01","Location and identification sequences","301120","(Radiosonde abbreviated header and launch information)",,"002011","Radiosonde type",,,"Operational"
385.00,"01","Location and identification sequences","301120","(Radiosonde abbreviated header and launch information)",,"301121","Radiosonde launch point location",,,"Operational"
386.00,"01","Location and identification sequences","301121","(Radiosonde launch point location)",,"008041","Data significance","= 3 Balloon launch point",,"Operational"
387.00,"01","Location and identification sequences","301121","(Radiosonde launch point location)",,"301122","Date/time (to hundredths of second)",,,"Operational"
388.00,"01","Location and identification sequences","301121","(Radiosonde launch point location)",,"301021","Latitude/longitude (high accuracy)",,,"Operational"
389.00,"01","Location and identification sequences","301121","(Radiosonde launch point location)",,"007031","Height of barometer above mean sea level",,,"Operational"
390.00,"01","Location and identification sequences","301121","(Radiosonde launch point location)",,"007007","Height","Release of radiosonde above mean sea level",,"Operational"
391.00,"01","Location and identification sequences","301122","(Date/time (to hundredths of second))",,"301011","Year, month, day",,"<(see Note 3)>","Operational"
392.00,"01","Location and identification sequences","301122","(Date/time (to hundredths of second))",,"301012","Hour, minute",,,"Operational"
393.00,"01","Location and identification sequences","301122","(Date/time (to hundredths of second))",,"201135","Change data width",,,"Operational"
394.00,"01","Location and identification sequences","301122","(Date/time (to hundredths of second))",,"202130","Change scale",,,"Operational"
395.00,"01","Location and identification sequences","301122","(Date/time (to hundredths of second))",,"004006","Second",,,"Operational"
396.00,"01","Location and identification sequences","301122","(Date/time (to hundredths of second))",,"202000","Change scale","Cancel",,"Operational"
397.00,"01","Location and identification sequences","301122","(Date/time (to hundredths of second))",,"201000","Change data width","Cancel",,"Operational"
399.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"102002","Replicate 2 descriptors 2 times",,,"Operational"
400.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"008041","Data significance","= 0 Parent site, = 1 Observation site",,"Operational"
401.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"001062","Short ICAO location indicator",,,"Operational"
402.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"301001","WMO block and station numbers",,,"Operational"
403.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"001094","WBAN number",,,"Operational"
404.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"002011","Radiosonde type",,,"Operational"
405.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"001018","Short station or site name",,,"Operational"
406.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"001095","Observer identification",,,"Operational"
407.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"025061","Software identification and version number",,,"Operational"
408.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"025068","Number of archive recomputes",,,"Operational"
409.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"001082","Radiosonde ascension number",,,"Operational"
410.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"001083","Radiosonde release number",,,"Operational"
411.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"001081","Radiosonde serial number",,,"Operational"
412.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"002067","Radiosonde operating frequency",,,"Operational"
413.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"002066","Radiosonde ground receiving system",,,"Operational"
414.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"002014","Tracking technique/status of system used",,,"Operational"
415.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"025067","Radiosonde release point pressure correction",,,"Operational"
416.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"025065","Orientation correction (azimuth)",,,"Operational"
417.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"025066","Orientation correction (elevation)",,,"Operational"
418.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"002095","Type of pressure sensor",,,"Operational"
419.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"002096","Type of temperature sensor",,,"Operational"
420.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"002097","Type of humidity sensor",,,"Operational"
421.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"002016","Radiosonde configuration",,,"Operational"
422.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"002083","Type of balloon shelter",,,"Operational"
423.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"002080","Balloon manufacturer",,,"Operational"
424.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"002081","Type of balloon",,,"Operational"
425.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"001093","Balloon lot number",,,"Operational"
426.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"002084","Type of gas used in balloon",,,"Operational"
427.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"002085","Amount of gas used in balloon",,,"Operational"
428.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"002086","Balloon flight train length",,,"Operational"
429.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"002082","Weight of balloon",,,"Operational"
430.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"008041","Data significance","= 2 Balloon manufacture date",,"Operational"
431.00,"01","Location and identification sequences","301123","(Radiosonde full header information)",,"301011","Year, month, day",,,"Operational"
432.00,"01","Location and identification sequences","301125","(ASCAT header information)",,"001033","Identification of originating/generating centre",,,"Operational"
433.00,"01","Location and identification sequences","301125","(ASCAT header information)",,"001034","Identification of originating/generating sub-centre",,,"Operational"
434.00,"01","Location and identification sequences","301125","(ASCAT header information)",,"025060","Software identification",,,"Operational"
435.00,"01","Location and identification sequences","301125","(ASCAT header information)",,"001007","Satellite identifier",,,"Operational"
436.00,"01","Location and identification sequences","301125","(ASCAT header information)",,"002019","Satellite instruments",,,"Operational"
437.00,"01","Location and identification sequences","301125","(ASCAT header information)",,"001012","Direction of motion of moving observing platform",,,"Operational"
438.00,"02","Meteorological sequences common to surface data","302001","(Pressure and 3-hour pressure change)",,"010004","Pressure","Station level",,"Operational"
439.00,"02","Meteorological sequences common to surface data","302001","(Pressure and 3-hour pressure change)",,"010051","Pressure reduced to mean sea level",,,"Operational"
440.00,"02","Meteorological sequences common to surface data","302001","(Pressure and 3-hour pressure change)",,"010061","3-hour pressure change",,,"Operational"
441.00,"02","Meteorological sequences common to surface data","302001","(Pressure and 3-hour pressure change)",,"010063","Characteristic of pressure tendency",,,"Operational"
442.00,"02","Meteorological sequences common to surface data","302002","(High altitude station)",,"010004","Pressure","Station level",,"Operational"
443.00,"02","Meteorological sequences common to surface data","302002","(High altitude station)",,"007004","Pressure","Pressure level",,"Operational"
444.00,"02","Meteorological sequences common to surface data","302002","(High altitude station)",,"010003","Geopotential","Pressure level",,"Operational"
445.00,"02","Meteorological sequences common to surface data","302002","(High altitude station)",,"010061","3-hour pressure change",,,"Operational"
446.00,"02","Meteorological sequences common to surface data","302002","(High altitude station)",,"010063","Characteristic of pressure tendency",,,"Operational"
447.00,"02","Meteorological sequences common to surface data","302003","(Wind, temperature, humidity, visibility, weather)",,"011011","Wind direction at 10 m",,,"Operational"
448.00,"02","Meteorological sequences common to surface data","302003","(Wind, temperature, humidity, visibility, weather)",,"011012","Wind speed at 10 m",,,"Operational"
449.00,"02","Meteorological sequences common to surface data","302003","(Wind, temperature, humidity, visibility, weather)",,"012004","Air temperature at 2 m",,,"Operational"
450.00,"02","Meteorological sequences common to surface data","302003","(Wind, temperature, humidity, visibility, weather)",,"012006","Dewpoint temperature at 2 m",,,"Operational"
451.00,"02","Meteorological sequences common to surface data","302003","(Wind, temperature, humidity, visibility, weather)",,"013003","Relative humidity",,,"Operational"
452.00,"02","Meteorological sequences common to surface data","302003","(Wind, temperature, humidity, visibility, weather)",,"020001","Horizontal visibility",,,"Operational"
453.00,"02","Meteorological sequences common to surface data","302003","(Wind, temperature, humidity, visibility, weather)",,"020003","Present weather",,,"Operational"
454.00,"02","Meteorological sequences common to surface data","302003","(Wind, temperature, humidity, visibility, weather)",,"020004","Past weather (1)",,,"Operational"
455.00,"02","Meteorological sequences common to surface data","302003","(Wind, temperature, humidity, visibility, weather)",,"020005","Past weather (2)",,,"Operational"
456.00,"02","Meteorological sequences common to surface data","302004","(General cloud information)",,"020010","Cloud cover (total)",,,"Operational"
457.00,"02","Meteorological sequences common to surface data","302004","(General cloud information)",,"008002","Vertical significance (surface observations)",,,"Operational"
458.00,"02","Meteorological sequences common to surface data","302004","(General cloud information)",,"020011","Cloud amount",,,"Operational"
459.00,"02","Meteorological sequences common to surface data","302004","(General cloud information)",,"020013","Height of base of cloud",,,"Operational"
460.00,"02","Meteorological sequences common to surface data","302004","(General cloud information)",,"020012","Cloud type",,,"Operational"
461.00,"02","Meteorological sequences common to surface data","302004","(General cloud information)",,"020012","Cloud type",,,"Operational"
462.00,"02","Meteorological sequences common to surface data","302004","(General cloud information)",,"020012","Cloud type",,,"Operational"
463.00,"02","Meteorological sequences common to surface data","302005","(Cloud layer)",,"008002","Vertical significance (surface observations)",,,"Operational"
464.00,"02","Meteorological sequences common to surface data","302005","(Cloud layer)",,"020011","Cloud amount",,,"Operational"
465.00,"02","Meteorological sequences common to surface data","302005","(Cloud layer)",,"020012","Cloud type",,,"Operational"
466.00,"02","Meteorological sequences common to surface data","302005","(Cloud layer)",,"020013","Height of base of cloud",,,"Operational"
467.00,"02","Meteorological sequences common to surface data","302006","(Pressure and 24-hour pressure change)",,"010004","Pressure","Station level",,"Operational"
468.00,"02","Meteorological sequences common to surface data","302006","(Pressure and 24-hour pressure change)",,"010051","Pressure reduced to mean sea level",,,"Operational"
469.00,"02","Meteorological sequences common to surface data","302006","(Pressure and 24-hour pressure change)",,"010062","24-hour pressure change",,,"Operational"
470.00,"02","Meteorological sequences common to surface data","302006","(Pressure and 24-hour pressure change)",,"010063","Characteristic of pressure tendency",,,"Operational"
471.00,"02","Meteorological sequences common to surface data","302011","(Low altitude station)",,"302001","Pressure and 3-hour pressure change",,,"Operational"
472.00,"02","Meteorological sequences common to surface data","302011","(Low altitude station)",,"302003","Wind, temperature, humidity, visibility, weather",,,"Operational"
473.00,"02","Meteorological sequences common to surface data","302011","(Low altitude station)",,"302004","General cloud information","Significant cloud layer",,"Operational"
474.00,"02","Meteorological sequences common to surface data","302012","(High altitude station)",,"302002","High altitude station","Pressure and pressure change",,"Operational"
475.00,"02","Meteorological sequences common to surface data","302012","(High altitude station)",,"302003","Wind, temperature, humidity, visibility, weather",,,"Operational"
476.00,"02","Meteorological sequences common to surface data","302012","(High altitude station)",,"302004","General cloud information","Significant cloud layer",,"Operational"
477.00,"02","Meteorological sequences common to surface data","302013","(Basic surface report)",,"302006","Pressure and 24-hour pressure change",,,"Operational"
478.00,"02","Meteorological sequences common to surface data","302013","(Basic surface report)",,"302003","Wind, temperature, humidity, visibility, weather",,,"Operational"
479.00,"02","Meteorological sequences common to surface data","302013","(Basic surface report)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
480.00,"02","Meteorological sequences common to surface data","302013","(Basic surface report)",,"031001","Delayed descriptor replication factor",,,"Operational"
481.00,"02","Meteorological sequences common to surface data","302013","(Basic surface report)",,"302005","Cloud layer",,,"Operational"
486.00,"02","Meteorological sequences common to surface data","302021","(Waves)",,"022001","Direction of waves",,,"Operational"
487.00,"02","Meteorological sequences common to surface data","302021","(Waves)",,"022011","Period of waves",,,"Operational"
488.00,"02","Meteorological sequences common to surface data","302021","(Waves)",,"022021","Height of waves",,,"Operational"
489.00,"02","Meteorological sequences common to surface data","302022","(Wind waves)",,"022002","Direction of wind waves",,,"Operational"
490.00,"02","Meteorological sequences common to surface data","302022","(Wind waves)",,"022012","Period of wind waves",,,"Operational"
491.00,"02","Meteorological sequences common to surface data","302022","(Wind waves)",,"022022","Height of wind waves",,,"Operational"
492.00,"02","Meteorological sequences common to surface data","302023","(Swell waves)",,"022003","Direction of swell waves",,,"Operational"
493.00,"02","Meteorological sequences common to surface data","302023","(Swell waves)",,"022013","Period of swell waves",,,"Operational"
494.00,"02","Meteorological sequences common to surface data","302023","(Swell waves)",,"022023","Height of swell waves",,,"Operational"
495.00,"02","Meteorological sequences common to surface data","302024","(Wind and swell waves)",,"302022","Wind waves",,,"Operational"
496.00,"02","Meteorological sequences common to surface data","302024","(Wind and swell waves)",,"101002","Replicate 1 descriptor 2 times",,,"Operational"
497.00,"02","Meteorological sequences common to surface data","302024","(Wind and swell waves)",,"302023","Swell waves","2 systems of swell",,"Operational"
498.00,"02","Meteorological sequences common to surface data","302031","(Pressure information)",,"302001","Pressure and 3-hour pressure change",,,"Operational"
499.00,"02","Meteorological sequences common to surface data","302031","(Pressure information)",,"010062","24-hour pressure change",,,"Operational"
500.00,"02","Meteorological sequences common to surface data","302031","(Pressure information)",,"007004","Pressure","Standard level",,"Operational"
501.00,"02","Meteorological sequences common to surface data","302031","(Pressure information)",,"010009","Geopotential height",,,"Operational"
502.00,"02","Meteorological sequences common to surface data","302032","(Temperature and humidity data)",,"007032","Height of sensor above local ground (or deck of marine platform)","Temperature and humidity measurement",,"Operational"
503.00,"02","Meteorological sequences common to surface data","302032","(Temperature and humidity data)",,"012101","Temperature/air temperature","Scale: 2",,"Operational"
504.00,"02","Meteorological sequences common to surface data","302032","(Temperature and humidity data)",,"012103","Dewpoint temperature","Scale: 2",,"Operational"
505.00,"02","Meteorological sequences common to surface data","302032","(Temperature and humidity data)",,"013003","Relative humidity",,,"Operational"
506.00,"02","Meteorological sequences common to surface data","302033","(Visibility data)",,"007032","Height of sensor above local ground (or deck of marine platform)","Visibility measurement",,"Operational"
507.00,"02","Meteorological sequences common to surface data","302033","(Visibility data)",,"020001","Horizontal visibility",,,"Operational"
508.00,"02","Meteorological sequences common to surface data","302034","(Precipitation past 24 hours)",,"007032","Height of sensor above local ground (or deck of marine platform)","Precipitation measurement",,"Operational"
509.00,"02","Meteorological sequences common to surface data","302034","(Precipitation past 24 hours)",,"013023","Total precipitation past 24 hours",,,"Operational"
510.00,"02","Meteorological sequences common to surface data","302035","(Basic synoptic ""instantaneous"" data)",,"302032","Temperature and humidity data",,,"Operational"
511.00,"02","Meteorological sequences common to surface data","302035","(Basic synoptic ""instantaneous"" data)",,"302033","Visibility data",,,"Operational"
512.00,"02","Meteorological sequences common to surface data","302035","(Basic synoptic ""instantaneous"" data)",,"302034","Precipitation past 24 hours",,,"Operational"
513.00,"02","Meteorological sequences common to surface data","302035","(Basic synoptic ""instantaneous"" data)",,"007032","Height of sensor above local ground (or deck of marine platform)","Set to missing (cancel)",,"Operational"
514.00,"02","Meteorological sequences common to surface data","302035","(Basic synoptic ""instantaneous"" data)",,"302004","General cloud information",,,"Operational"
515.00,"02","Meteorological sequences common to surface data","302035","(Basic synoptic ""instantaneous"" data)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
516.00,"02","Meteorological sequences common to surface data","302035","(Basic synoptic ""instantaneous"" data)",,"031001","Delayed descriptor replication factor",,,"Operational"
517.00,"02","Meteorological sequences common to surface data","302035","(Basic synoptic ""instantaneous"" data)",,"302005","Cloud layer","Individual cloud layer or mass",,"Operational"
519.00,"02","Meteorological sequences common to surface data","302036","(Clouds with bases below station level)",,"105000","Delayed replication of 5 descriptors",,,"Operational"
520.00,"02","Meteorological sequences common to surface data","302036","(Clouds with bases below station level)",,"031001","Delayed descriptor replication factor",,,"Operational"
521.00,"02","Meteorological sequences common to surface data","302036","(Clouds with bases below station level)",,"008002","Vertical significance (surface observations)",,,"Operational"
522.00,"02","Meteorological sequences common to surface data","302036","(Clouds with bases below station level)",,"020011","Cloud amount",,,"Operational"
523.00,"02","Meteorological sequences common to surface data","302036","(Clouds with bases below station level)",,"020012","Cloud type",,,"Operational"
524.00,"02","Meteorological sequences common to surface data","302036","(Clouds with bases below station level)",,"020014","Height of top of cloud",,,"Operational"
525.00,"02","Meteorological sequences common to surface data","302036","(Clouds with bases below station level)",,"020017","Cloud top description",,,"Operational"
527.00,"02","Meteorological sequences common to surface data","302037","(State of ground, snow depth, ground minimum temperature)",,"020062","State of the ground (with or without snow)",,,"Operational"
528.00,"02","Meteorological sequences common to surface data","302037","(State of ground, snow depth, ground minimum temperature)",,"013013","Total snow depth",,,"Operational"
529.00,"02","Meteorological sequences common to surface data","302037","(State of ground, snow depth, ground minimum temperature)",,"012113","Ground minimum temperature, past 12 hours","Scale: 2",,"Operational"
530.00,"02","Meteorological sequences common to surface data","302038","(Present and past weather)",,"020003","Present weather",,,"Operational"
531.00,"02","Meteorological sequences common to surface data","302038","(Present and past weather)",,"004024","Time period or displacement","Hours",,"Operational"
532.00,"02","Meteorological sequences common to surface data","302038","(Present and past weather)",,"020004","Past weather (1)",,,"Operational"
533.00,"02","Meteorological sequences common to surface data","302038","(Present and past weather)",,"020005","Past weather (2)",,,"Operational"
534.00,"02","Meteorological sequences common to surface data","302039","(Sunshine data (from 1 hour and 24 hour period))",,"004024","Time period or displacement","Hours",,"Operational"
535.00,"02","Meteorological sequences common to surface data","302039","(Sunshine data (from 1 hour and 24 hour period))",,"014031","Total sunshine",,,"Operational"
536.00,"02","Meteorological sequences common to surface data","302040","(Precipitation measurement)",,"007032","Height of sensor above local ground (or deck of marine platform)","Precipitation measurement",,"Operational"
537.00,"02","Meteorological sequences common to surface data","302040","(Precipitation measurement)",,"102002","Replicate 2 descriptors 2 times",,,"Operational"
538.00,"02","Meteorological sequences common to surface data","302040","(Precipitation measurement)",,"004024","Time period or displacement","Hours",,"Operational"
539.00,"02","Meteorological sequences common to surface data","302040","(Precipitation measurement)",,"013011","Total precipitation/total water equivalent",,,"Operational"
540.00,"02","Meteorological sequences common to surface data","302041","(Extreme temperature data)",,"007032","Height of sensor above local ground (or deck of marine platform)","Temperature measurement",,"Operational"
541.00,"02","Meteorological sequences common to surface data","302041","(Extreme temperature data)",,"004024","Time period or displacement",,,"Operational"
542.00,"02","Meteorological sequences common to surface data","302041","(Extreme temperature data)",,"004024","Time period or displacement",,"(see Notes 1 and 2)","Operational"
543.00,"02","Meteorological sequences common to surface data","302041","(Extreme temperature data)",,"012111","Maximum temperature, at height and over period specified","Scale: 2",,"Operational"
544.00,"02","Meteorological sequences common to surface data","302041","(Extreme temperature data)",,"004024","Time period or displacement",,,"Operational"
545.00,"02","Meteorological sequences common to surface data","302041","(Extreme temperature data)",,"004024","Time period or displacement",,"(see Note 2)","Operational"
546.00,"02","Meteorological sequences common to surface data","302041","(Extreme temperature data)",,"012112","Minimum temperature, at height and over period specified","Scale: 2",,"Operational"
547.00,"02","Meteorological sequences common to surface data","302042","(Wind data)",,"007032","Height of sensor above local ground (or deck of marine platform)","Wind measurement",,"Operational"
548.00,"02","Meteorological sequences common to surface data","302042","(Wind data)",,"002002","Type of instrumentation for wind measurement",,,"Operational"
549.00,"02","Meteorological sequences common to surface data","302042","(Wind data)",,"008021","Time significance","= 2 Time averaged",,"Operational"
550.00,"02","Meteorological sequences common to surface data","302042","(Wind data)",,"004025","Time period or displacement","= -10 minutes, or number of minutes after a significant change of wind",,"Operational"
551.00,"02","Meteorological sequences common to surface data","302042","(Wind data)",,"011001","Wind direction",,,"Operational"
552.00,"02","Meteorological sequences common to surface data","302042","(Wind data)",,"011002","Wind speed",,,"Operational"
553.00,"02","Meteorological sequences common to surface data","302042","(Wind data)",,"008021","Time significance","Set to missing",,"Operational"
554.00,"02","Meteorological sequences common to surface data","302042","(Wind data)",,"103002","Replicate 3 descriptors 2 times",,,"Operational"
555.00,"02","Meteorological sequences common to surface data","302042","(Wind data)",,"004025","Time period or displacement","Minutes",,"Operational"
556.00,"02","Meteorological sequences common to surface data","302042","(Wind data)",,"011043","Maximum wind gust direction",,,"Operational"
557.00,"02","Meteorological sequences common to surface data","302042","(Wind data)",,"011041","Maximum wind gust speed",,,"Operational"
558.00,"02","Meteorological sequences common to surface data","302043","(Basic synoptic ""period"" data)",,"302038","Present and past weather",,,"Operational"
559.00,"02","Meteorological sequences common to surface data","302043","(Basic synoptic ""period"" data)",,"101002","Replicate 1 descriptor 2 times",,,"Operational"
560.00,"02","Meteorological sequences common to surface data","302043","(Basic synoptic ""period"" data)",,"302039","Sunshine data (from 1 hour and 24 hour period)",,,"Operational"
561.00,"02","Meteorological sequences common to surface data","302043","(Basic synoptic ""period"" data)",,"302040","Precipitation measurement",,,"Operational"
562.00,"02","Meteorological sequences common to surface data","302043","(Basic synoptic ""period"" data)",,"302041","Extreme temperature data",,,"Operational"
563.00,"02","Meteorological sequences common to surface data","302043","(Basic synoptic ""period"" data)",,"302042","Wind data",,,"Operational"
564.00,"02","Meteorological sequences common to surface data","302043","(Basic synoptic ""period"" data)",,"007032","Height of sensor above local ground (or deck of marine platform)","Set to missing (cancel)",,"Operational"
565.00,"02","Meteorological sequences common to surface data","302044","(Evaporation data)",,"004024","Time period or displacement","Hours",,"Operational"
566.00,"02","Meteorological sequences common to surface data","302044","(Evaporation data)",,"002004","Type of instrumentation for evaporation measurement or type of crop for which evapotranspiration is reported",,,"Operational"
567.00,"02","Meteorological sequences common to surface data","302044","(Evaporation data)",,"013033","Evaporation/evapotranspiration",,,"Operational"
568.00,"02","Meteorological sequences common to surface data","302045","(Radiation data (from 1 hour and 24 hour period))",,"004024","Time period or displacement","Hours",,"Operational"
569.00,"02","Meteorological sequences common to surface data","302045","(Radiation data (from 1 hour and 24 hour period))",,"014002","Long-wave radiation, integrated over period specified",,,"Operational"
570.00,"02","Meteorological sequences common to surface data","302045","(Radiation data (from 1 hour and 24 hour period))",,"014004","Short-wave radiation, integrated over period specified",,,"Operational"
571.00,"02","Meteorological sequences common to surface data","302045","(Radiation data (from 1 hour and 24 hour period))",,"014016","Net radiation, integrated over period specified",,,"Operational"
572.00,"02","Meteorological sequences common to surface data","302045","(Radiation data (from 1 hour and 24 hour period))",,"014028","Global solar radiation (high accuracy), integrated over period specified",,,"Operational"
573.00,"02","Meteorological sequences common to surface data","302045","(Radiation data (from 1 hour and 24 hour period))",,"014029","Diffuse solar radiation (high accuracy), integrated over period specified",,,"Operational"
574.00,"02","Meteorological sequences common to surface data","302045","(Radiation data (from 1 hour and 24 hour period))",,"014030","Direct solar radiation (high accuracy), integrated over period specified",,,"Operational"
575.00,"02","Meteorological sequences common to surface data","302046","(Temperature change)",,"004024","Time period or displacement",,,"Operational"
576.00,"02","Meteorological sequences common to surface data","302046","(Temperature change)",,"004024","Time period or displacement",,"(see Note 3)","Operational"
577.00,"02","Meteorological sequences common to surface data","302046","(Temperature change)",,"012049","Temperature change over specified period",,,"Operational"
578.00,"02","Meteorological sequences common to surface data","302047","(Direction of cloud drift)",,"102003","Replicate 2 descriptors 3 times",,,"Operational"
579.00,"02","Meteorological sequences common to surface data","302047","(Direction of cloud drift)",,"008002","Vertical significance (surface observations)",,,"Operational"
580.00,"02","Meteorological sequences common to surface data","302047","(Direction of cloud drift)",,"020054","True direction from which a phenomenon or clouds are moving",,,"Operational"
581.00,"02","Meteorological sequences common to surface data","302048","(Direction and elevation of cloud)",,"005021","Bearing or azimuth",,,"Operational"
582.00,"02","Meteorological sequences common to surface data","302048","(Direction and elevation of cloud)",,"007021","Elevation","Elevation angle",,"Operational"
583.00,"02","Meteorological sequences common to surface data","302048","(Direction and elevation of cloud)",,"020012","Cloud type",,,"Operational"
584.00,"02","Meteorological sequences common to surface data","302048","(Direction and elevation of cloud)",,"005021","Bearing or azimuth","Set to missing (cancel)",,"Operational"
585.00,"02","Meteorological sequences common to surface data","302048","(Direction and elevation of cloud)",,"007021","Elevation","Set to missing (cancel)",,"Operational"
586.00,"02","Meteorological sequences common to surface data","302049","(Cloud information reported with vertical soundings)",,"008002","Vertical significance (surface observations)",,,"Operational"
587.00,"02","Meteorological sequences common to surface data","302049","(Cloud information reported with vertical soundings)",,"020011","Cloud amount","Low or middle clouds Nh",,"Operational"
588.00,"02","Meteorological sequences common to surface data","302049","(Cloud information reported with vertical soundings)",,"020013","Height of base of cloud","h",,"Operational"
589.00,"02","Meteorological sequences common to surface data","302049","(Cloud information reported with vertical soundings)",,"020012","Cloud type","Low clouds CL",,"Operational"
590.00,"02","Meteorological sequences common to surface data","302049","(Cloud information reported with vertical soundings)",,"020012","Cloud type","Middle clouds CM",,"Operational"
591.00,"02","Meteorological sequences common to surface data","302049","(Cloud information reported with vertical soundings)",,"020012","Cloud type","High clouds CH",,"Operational"
592.00,"02","Meteorological sequences common to surface data","302049","(Cloud information reported with vertical soundings)",,"008002","Vertical significance (surface observations)","Set to missing",,"Operational"
593.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"008041","Data significance","= 5 Surface observation displacement from launch point",,"Operational"
594.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"005021","Bearing or azimuth",,,"Operational"
595.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"007005","Height increment",,,"Operational"
596.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"202130","Change scale",,,"Operational"
597.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"006021","Distance",,,"Operational"
598.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"202000","Change scale","Cancel",,"Operational"
599.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"008041","Data significance","= 4 Surface observation",,"Operational"
600.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"201131","Change data width",,,"Operational"
601.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"202129","Change scale",,,"Operational"
602.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"002115","Type of surface observing equipment",,,"Operational"
603.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"010004","Pressure",,,"Operational"
604.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"002115","Type of surface observing equipment",,,"Operational"
605.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"013003","Relative humidity",,,"Operational"
606.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"202000","Change scale","Cancel",,"Operational"
607.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"201000","Change data width","Cancel",,"Operational"
608.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"002115","Type of surface observing equipment",,,"Operational"
609.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"011001","Wind direction",,,"Operational"
610.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"011002","Wind speed",,,"Operational"
611.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"002115","Type of surface observing equipment",,,"Operational"
612.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"102002","Replicate 2 descriptors 2 times",,,"Operational"
613.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"012101","Temperature/air temperature",,,"Operational"
614.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"004024","Time period or displacement","Hours",,"Operational"
615.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"002115","Type of surface observing equipment",,,"Operational"
616.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"012103","Dewpoint temperature",,,"Operational"
617.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"012102","Wet-bulb temperature",,,"Operational"
618.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"101003","Replicate 1 descriptor 3 times",,,"Operational"
619.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"020012","Cloud type",,,"Operational"
620.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"020011","Cloud amount",,,"Operational"
621.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"020013","Height of base of cloud",,,"Operational"
622.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"101002","Replicate 1 descriptor 2 times",,,"Operational"
623.00,"02","Meteorological sequences common to surface data","302050","(Radiosonde surface observation)",,"020003","Present weather",,,"Operational"
625.00,"02","Meteorological sequences common to surface data","302051",,,"010004","Pressure",,,"Operational"
626.00,"02","Meteorological sequences common to surface data","302051",,,"010051","Pressure reduced to mean sea level",,,"Operational"
627.00,"02","Meteorological sequences common to surface data","302051",,,"007004","Pressure","Vertical location",,"Operational"
628.00,"02","Meteorological sequences common to surface data","302051",,,"010003","Geopotential",,,"Operational"
629.00,"02","Meteorological sequences common to surface data","302051",,,"012004","Air temperature at 2 m",,,"Operational"
630.00,"02","Meteorological sequences common to surface data","302051",,,"012051","Standard deviation temperature",,,"Operational"
631.00,"02","Meteorological sequences common to surface data","302051",,,"012016","Maximum temperature at 2 m, past 24 hours",,,"Operational"
632.00,"02","Meteorological sequences common to surface data","302051",,,"012017","Minimum temperature at 2 m, past 24 hours",,,"Operational"
633.00,"02","Meteorological sequences common to surface data","302051",,,"013004","Vapour pressure",,,"Operational"
634.00,"02","Meteorological sequences common to surface data","302051",,,"102004","Replicate 2 descriptors 4 times",,,"Operational"
635.00,"02","Meteorological sequences common to surface data","302051",,,"008051","Qualifier for number of missing values in calculation of statistic",,,"Operational"
636.00,"02","Meteorological sequences common to surface data","302051",,,"008020","Total number of missing entities (with respect to accumulation or average)",,,"Operational"
637.00,"02","Meteorological sequences common to surface data","302052","(Ship temperature and humidity data)",,"007032","Height of sensor above local ground (or deck of marine platform)","Temperature and humidity measurement",,"Operational"
638.00,"02","Meteorological sequences common to surface data","302052","(Ship temperature and humidity data)",,"007033","Height of sensor above water surface","Temperature and humidity measurement",,"Operational"
639.00,"02","Meteorological sequences common to surface data","302052","(Ship temperature and humidity data)",,"012101","Temperature/air temperature","Scale: 2",,"Operational"
640.00,"02","Meteorological sequences common to surface data","302052","(Ship temperature and humidity data)",,"002039","Method of wet-bulb temperature measurement",,,"Operational"
641.00,"02","Meteorological sequences common to surface data","302052","(Ship temperature and humidity data)",,"012102","Wet-bulb temperature","Scale: 2",,"Operational"
642.00,"02","Meteorological sequences common to surface data","302052","(Ship temperature and humidity data)",,"012103","Dewpoint temperature","Scale: 2",,"Operational"
643.00,"02","Meteorological sequences common to surface data","302052","(Ship temperature and humidity data)",,"013003","Relative humidity",,,"Operational"
644.00,"02","Meteorological sequences common to surface data","302053","(Ship visibility data)",,"007032","Height of sensor above local ground (or deck of marine platform)","Visibility measurement",,"Operational"
645.00,"02","Meteorological sequences common to surface data","302053","(Ship visibility data)",,"007033","Height of sensor above water surface","Visibility measurement",,"Operational"
646.00,"02","Meteorological sequences common to surface data","302053","(Ship visibility data)",,"020001","Horizontal visibility",,,"Operational"
647.00,"02","Meteorological sequences common to surface data","302054","(Ship ""instantaneous"" data)",,"302052","Ship temperature and humidity data",,,"Operational"
648.00,"02","Meteorological sequences common to surface data","302054","(Ship ""instantaneous"" data)",,"302053","Ship visibility data",,,"Operational"
649.00,"02","Meteorological sequences common to surface data","302054","(Ship ""instantaneous"" data)",,"007033","Height of sensor above water surface","Set to missing (cancel)",,"Operational"
650.00,"02","Meteorological sequences common to surface data","302054","(Ship ""instantaneous"" data)",,"302034","Precipitation past 24 hours",,,"Operational"
651.00,"02","Meteorological sequences common to surface data","302054","(Ship ""instantaneous"" data)",,"007032","Height of sensor above local ground (or deck of marine platform)","Set to missing (cancel)",,"Operational"
652.00,"02","Meteorological sequences common to surface data","302054","(Ship ""instantaneous"" data)",,"302004","General cloud information",,,"Operational"
653.00,"02","Meteorological sequences common to surface data","302054","(Ship ""instantaneous"" data)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
654.00,"02","Meteorological sequences common to surface data","302054","(Ship ""instantaneous"" data)",,"031001","Delayed descriptor replication factor",,,"Operational"
655.00,"02","Meteorological sequences common to surface data","302054","(Ship ""instantaneous"" data)",,"302005","Cloud layer",,,"Operational"
657.00,"02","Meteorological sequences common to surface data","302055","(Icing and ice)",,"020031","Ice deposit (thickness)",,,"Operational"
658.00,"02","Meteorological sequences common to surface data","302055","(Icing and ice)",,"020032","Rate of ice accretion (estimated)",,,"Operational"
659.00,"02","Meteorological sequences common to surface data","302055","(Icing and ice)",,"020033","Cause of ice accretion",,,"Operational"
660.00,"02","Meteorological sequences common to surface data","302055","(Icing and ice)",,"020034","Sea ice concentration",,,"Operational"
661.00,"02","Meteorological sequences common to surface data","302055","(Icing and ice)",,"020035","Amount and type of ice",,,"Operational"
662.00,"02","Meteorological sequences common to surface data","302055","(Icing and ice)",,"020036","Ice situation",,,"Operational"
663.00,"02","Meteorological sequences common to surface data","302055","(Icing and ice)",,"020037","Ice development",,,"Operational"
664.00,"02","Meteorological sequences common to surface data","302055","(Icing and ice)",,"020038","Bearing of ice edge",,,"Operational"
665.00,"02","Meteorological sequences common to surface data","302056","(Sea/water temperature)",,"002038","Method of water temperature and/or salinity measurement",,,"Operational"
666.00,"02","Meteorological sequences common to surface data","302056","(Sea/water temperature)",,"007063","Depth below sea/water surface (cm)","Sea-surface temperature measurement",,"Operational"
667.00,"02","Meteorological sequences common to surface data","302056","(Sea/water temperature)",,"022043","Sea/water temperature",,,"Operational"
668.00,"02","Meteorological sequences common to surface data","302056","(Sea/water temperature)",,"007063","Depth below sea/water surface (cm)","Set to missing (cancel)",,"Operational"
669.00,"02","Meteorological sequences common to surface data","302057","(Ship marine data)",,"302056","Sea/water temperature","Sea-surface temperature, method of measurement, and depth below sea surface",,"Operational"
670.00,"02","Meteorological sequences common to surface data","302057","(Ship marine data)",,"302021","Waves",,,"Operational"
671.00,"02","Meteorological sequences common to surface data","302057","(Ship marine data)",,"302024","Wind and swell waves",,,"Operational"
672.00,"02","Meteorological sequences common to surface data","302058","(Ship extreme temperature data)",,"007032","Height of sensor above local ground (or deck of marine platform)","Temperature measurement",,"Operational"
673.00,"02","Meteorological sequences common to surface data","302058","(Ship extreme temperature data)",,"007033","Height of sensor above water surface","Temperature measurement",,"Operational"
674.00,"02","Meteorological sequences common to surface data","302058","(Ship extreme temperature data)",,"004024","Time period or displacement",,,"Operational"
675.00,"02","Meteorological sequences common to surface data","302058","(Ship extreme temperature data)",,"004024","Time period or displacement",,"(see Notes 1 and 2)","Operational"
676.00,"02","Meteorological sequences common to surface data","302058","(Ship extreme temperature data)",,"012111","Maximum temperature, at height and over period specified","Scale: 2",,"Operational"
677.00,"02","Meteorological sequences common to surface data","302058","(Ship extreme temperature data)",,"004024","Time period or displacement",,,"Operational"
678.00,"02","Meteorological sequences common to surface data","302058","(Ship extreme temperature data)",,"004024","Time period or displacement",,"(see Note 2)","Operational"
679.00,"02","Meteorological sequences common to surface data","302058","(Ship extreme temperature data)",,"012112","Minimum temperature, at height and over period specified","Scale: 2",,"Operational"
680.00,"02","Meteorological sequences common to surface data","302059","(Ship wind data)",,"007032","Height of sensor above local ground (or deck of marine platform)","Wind measurement",,"Operational"
681.00,"02","Meteorological sequences common to surface data","302059","(Ship wind data)",,"007033","Height of sensor above water surface","Wind measurement",,"Operational"
682.00,"02","Meteorological sequences common to surface data","302059","(Ship wind data)",,"002002","Type of instrumentation for wind measurement",,,"Operational"
683.00,"02","Meteorological sequences common to surface data","302059","(Ship wind data)",,"008021","Time significance","= 2 Time averaged",,"Operational"
684.00,"02","Meteorological sequences common to surface data","302059","(Ship wind data)",,"004025","Time period or displacement","= -10 minutes, or number of minutes after a significant change of wind",,"Operational"
685.00,"02","Meteorological sequences common to surface data","302059","(Ship wind data)",,"011001","Wind direction",,,"Operational"
686.00,"02","Meteorological sequences common to surface data","302059","(Ship wind data)",,"011002","Wind speed",,,"Operational"
687.00,"02","Meteorological sequences common to surface data","302059","(Ship wind data)",,"008021","Time significance","Set to missing",,"Operational"
688.00,"02","Meteorological sequences common to surface data","302059","(Ship wind data)",,"103002","Replicate 3 descriptors 2 times",,,"Operational"
689.00,"02","Meteorological sequences common to surface data","302059","(Ship wind data)",,"004025","Time period or displacement","Minutes",,"Operational"
690.00,"02","Meteorological sequences common to surface data","302059","(Ship wind data)",,"011043","Maximum wind gust direction",,,"Operational"
691.00,"02","Meteorological sequences common to surface data","302059","(Ship wind data)",,"011041","Maximum wind gust speed",,,"Operational"
692.00,"02","Meteorological sequences common to surface data","302060","(Ship ""period"" data)",,"302038","Present and past weather",,,"Operational"
693.00,"02","Meteorological sequences common to surface data","302060","(Ship ""period"" data)",,"302040","Precipitation measurement",,,"Operational"
694.00,"02","Meteorological sequences common to surface data","302060","(Ship ""period"" data)",,"302058","Ship extreme temperature data",,,"Operational"
695.00,"02","Meteorological sequences common to surface data","302060","(Ship ""period"" data)",,"302059","Ship wind data",,,"Operational"
753.00,"02","Meteorological sequences common to surface data","302066","(Dangerous weather phenomena)",,"020023","Other weather phenomena",,,"Operational"
754.00,"02","Meteorological sequences common to surface data","302066","(Dangerous weather phenomena)",,"020024","Intensity of phenomena",,,"Operational"
755.00,"02","Meteorological sequences common to surface data","302066","(Dangerous weather phenomena)",,"020027","Phenomena occurrence",,,"Operational"
756.00,"02","Meteorological sequences common to surface data","302066","(Dangerous weather phenomena)",,"020054","True direction from which a phenomenon or clouds are moving",,,"Operational"
757.00,"02","Meteorological sequences common to surface data","302066","(Dangerous weather phenomena)",,"020023","Other weather phenomena",,,"Operational"
758.00,"02","Meteorological sequences common to surface data","302066","(Dangerous weather phenomena)",,"020027","Phenomena occurrence",,,"Operational"
759.00,"02","Meteorological sequences common to surface data","302066","(Dangerous weather phenomena)",,"020054","True direction from which a phenomenon or clouds are moving",,,"Operational"
760.00,"02","Meteorological sequences common to surface data","302066","(Dangerous weather phenomena)",,"020025","Obscuration",,,"Operational"
761.00,"02","Meteorological sequences common to surface data","302066","(Dangerous weather phenomena)",,"020026","Character of obscuration",,,"Operational"
762.00,"02","Meteorological sequences common to surface data","302066","(Dangerous weather phenomena)",,"020027","Phenomena occurrence",,,"Operational"
763.00,"02","Meteorological sequences common to surface data","302066","(Dangerous weather phenomena)",,"020040","Evolution of drift snow",,,"Operational"
764.00,"02","Meteorological sequences common to surface data","302066","(Dangerous weather phenomena)",,"020066","Maximum diameter of hailstones",,,"Operational"
765.00,"02","Meteorological sequences common to surface data","302066","(Dangerous weather phenomena)",,"020027","Phenomena occurrence",,,"Operational"
766.00,"02","Meteorological sequences common to surface data","302066","(Dangerous weather phenomena)",,"020021","Type of precipitation",,,"Operational"
767.00,"02","Meteorological sequences common to surface data","302066","(Dangerous weather phenomena)",,"020067","Diameter of deposit",,,"Operational"
768.00,"02","Meteorological sequences common to surface data","302066","(Dangerous weather phenomena)",,"020027","Phenomena occurrence",,,"Operational"
850.00,"02","Meteorological sequences common to surface data","302069","(Visibility data)",,"007032","Height of sensor above local ground (or deck of marine platform)",,,"Operational"
851.00,"02","Meteorological sequences common to surface data","302069","(Visibility data)",,"007033","Height of sensor above water surface",,,"Operational"
852.00,"02","Meteorological sequences common to surface data","302069","(Visibility data)",,"033041","Attribute of following value",,,"Operational"
853.00,"02","Meteorological sequences common to surface data","302069","(Visibility data)",,"020001","Horizontal visibility",,,"Operational"
854.00,"02","Meteorological sequences common to surface data","302070","(Wind data)",,"007032","Height of sensor above local ground (or deck of marine platform)",,,"Operational"
855.00,"02","Meteorological sequences common to surface data","302070","(Wind data)",,"007033","Height of sensor above water surface",,,"Operational"
856.00,"02","Meteorological sequences common to surface data","302070","(Wind data)",,"011001","Wind direction",,,"Operational"
857.00,"02","Meteorological sequences common to surface data","302070","(Wind data)",,"011002","Wind speed",,,"Operational"
858.00,"02","Meteorological sequences common to surface data","302070","(Wind data)",,"011043","Maximum wind gust direction",,,"Operational"
859.00,"02","Meteorological sequences common to surface data","302070","(Wind data)",,"011041","Maximum wind gust speed",,,"Operational"
860.00,"02","Meteorological sequences common to surface data","302070","(Wind data)",,"011016","Extreme counterclockwise wind direction of a variable wind",,,"Operational"
861.00,"02","Meteorological sequences common to surface data","302070","(Wind data)",,"011017","Extreme clockwise wind direction of a variable wind",,,"Operational"
862.00,"02","Meteorological sequences common to surface data","302071","(Wind data from one-hour period)",,"007032","Height of sensor above local ground (or deck of marine platform)",,,"Operational"
863.00,"02","Meteorological sequences common to surface data","302071","(Wind data from one-hour period)",,"007033","Height of sensor above water surface",,,"Operational"
864.00,"02","Meteorological sequences common to surface data","302071","(Wind data from one-hour period)",,"008021","Time significance","= 2 Time averaged",,"Operational"
865.00,"02","Meteorological sequences common to surface data","302071","(Wind data from one-hour period)",,"004025","Time period or displacement","= -10 minutes, or number of minutes after a significant change of wind, if any",,"Operational"
866.00,"02","Meteorological sequences common to surface data","302071","(Wind data from one-hour period)",,"011001","Wind direction",,,"Operational"
867.00,"02","Meteorological sequences common to surface data","302071","(Wind data from one-hour period)",,"011002","Wind speed",,,"Operational"
868.00,"02","Meteorological sequences common to surface data","302071","(Wind data from one-hour period)",,"008021","Time significance","Set to missing",,"Operational"
869.00,"02","Meteorological sequences common to surface data","302071","(Wind data from one-hour period)",,"103002","Replicate 3 descriptors 2 times",,,"Operational"
870.00,"02","Meteorological sequences common to surface data","302071","(Wind data from one-hour period)",,"004025","Time period or displacement","= -10 minutes in the first replication, = -60 minutes in the second replication",,"Operational"
871.00,"02","Meteorological sequences common to surface data","302071","(Wind data from one-hour period)",,"011043","Maximum wind gust direction",,,"Operational"
872.00,"02","Meteorological sequences common to surface data","302071","(Wind data from one-hour period)",,"011041","Maximum wind gust speed",,,"Operational"
873.00,"02","Meteorological sequences common to surface data","302071","(Wind data from one-hour period)",,"004025","Time period or displacement","= -10 minutes",,"Operational"
874.00,"02","Meteorological sequences common to surface data","302071","(Wind data from one-hour period)",,"011016","Extreme counterclockwise wind direction of a variable wind",,,"Operational"
875.00,"02","Meteorological sequences common to surface data","302071","(Wind data from one-hour period)",,"011017","Extreme clockwise wind direction of a variable wind",,,"Operational"
876.00,"02","Meteorological sequences common to surface data","302072","(Temperature and humidity data)",,"007032","Height of sensor above local ground (or deck of marine platform)",,,"Operational"
877.00,"02","Meteorological sequences common to surface data","302072","(Temperature and humidity data)",,"007033","Height of sensor above water surface",,,"Operational"
878.00,"02","Meteorological sequences common to surface data","302072","(Temperature and humidity data)",,"012101","Temperature/air temperature","Scale: 2",,"Operational"
879.00,"02","Meteorological sequences common to surface data","302072","(Temperature and humidity data)",,"012103","Dewpoint temperature","Scale: 2",,"Operational"
880.00,"02","Meteorological sequences common to surface data","302072","(Temperature and humidity data)",,"013003","Relative humidity",,,"Operational"
881.00,"02","Meteorological sequences common to surface data","302073","(Cloud data)",,"020010","Cloud cover (total)",,,"Operational"
882.00,"02","Meteorological sequences common to surface data","302073","(Cloud data)",,"105004","Replicate 5 descriptors 4 times",,,"Operational"
883.00,"02","Meteorological sequences common to surface data","302073","(Cloud data)",,"008002","Vertical significance (surface observations)",,,"Operational"
884.00,"02","Meteorological sequences common to surface data","302073","(Cloud data)",,"020011","Cloud amount",,,"Operational"
885.00,"02","Meteorological sequences common to surface data","302073","(Cloud data)",,"020012","Cloud type",,,"Operational"
886.00,"02","Meteorological sequences common to surface data","302073","(Cloud data)",,"033041","Attribute of following value",,,"Operational"
887.00,"02","Meteorological sequences common to surface data","302073","(Cloud data)",,"020013","Height of base of cloud",,,"Operational"
888.00,"02","Meteorological sequences common to surface data","302074","(Present and past weather)",,"020003","Present weather",,,"Operational"
889.00,"02","Meteorological sequences common to surface data","302074","(Present and past weather)",,"004025","Time period or displacement",,,"Operational"
890.00,"02","Meteorological sequences common to surface data","302074","(Present and past weather)",,"020004","Past weather (1)",,,"Operational"
891.00,"02","Meteorological sequences common to surface data","302074","(Present and past weather)",,"020005","Past weather (2)",,,"Operational"
892.00,"02","Meteorological sequences common to surface data","302075","(Intensity of precipitation, size of precipitation element)",,"008021","Time significance","= 2 Time averaged",,"Operational"
893.00,"02","Meteorological sequences common to surface data","302075","(Intensity of precipitation, size of precipitation element)",,"004025","Time period or displacement","= -10 minutes",,"Operational"
894.00,"02","Meteorological sequences common to surface data","302075","(Intensity of precipitation, size of precipitation element)",,"013055","Intensity of precipitation",,,"Operational"
895.00,"02","Meteorological sequences common to surface data","302075","(Intensity of precipitation, size of precipitation element)",,"013058","Size of precipitating element",,,"Operational"
896.00,"02","Meteorological sequences common to surface data","302075","(Intensity of precipitation, size of precipitation element)",,"008021","Time significance","Set to missing",,"Operational"
897.00,"02","Meteorological sequences common to surface data","302076","(Precipitation, obscuration and other phenomena)",,"020021","Type of precipitation",,,"Operational"
898.00,"02","Meteorological sequences common to surface data","302076","(Precipitation, obscuration and other phenomena)",,"020022","Character of precipitation",,,"Operational"
899.00,"02","Meteorological sequences common to surface data","302076","(Precipitation, obscuration and other phenomena)",,"026020","Duration of precipitation",,,"Operational"
900.00,"02","Meteorological sequences common to surface data","302076","(Precipitation, obscuration and other phenomena)",,"020023","Other weather phenomena",,,"Operational"
901.00,"02","Meteorological sequences common to surface data","302076","(Precipitation, obscuration and other phenomena)",,"020024","Intensity of phenomena",,,"Operational"
902.00,"02","Meteorological sequences common to surface data","302076","(Precipitation, obscuration and other phenomena)",,"020025","Obscuration",,,"Operational"
903.00,"02","Meteorological sequences common to surface data","302076","(Precipitation, obscuration and other phenomena)",,"020026","Character of obscuration",,,"Operational"
904.00,"02","Meteorological sequences common to surface data","302077","(Extreme temperature data)",,"007032","Height of sensor above local ground (or deck of marine platform)",,,"Operational"
905.00,"02","Meteorological sequences common to surface data","302077","(Extreme temperature data)",,"007033","Height of sensor above water surface",,,"Operational"
906.00,"02","Meteorological sequences common to surface data","302077","(Extreme temperature data)",,"004025","Time period or displacement",,,"Operational"
907.00,"02","Meteorological sequences common to surface data","302077","(Extreme temperature data)",,"012111","Maximum temperature, at height and over period specified","Scale: 2",,"Operational"
908.00,"02","Meteorological sequences common to surface data","302077","(Extreme temperature data)",,"012112","Minimum temperature, at height and over period specified","Scale: 2",,"Operational"
909.00,"02","Meteorological sequences common to surface data","302077","(Extreme temperature data)",,"007032","Height of sensor above local ground (or deck of marine platform)","Ground temperature",,"Operational"
910.00,"02","Meteorological sequences common to surface data","302077","(Extreme temperature data)",,"004025","Time period or displacement",,,"Operational"
911.00,"02","Meteorological sequences common to surface data","302077","(Extreme temperature data)",,"012112","Minimum temperature, at height and over period specified","Scale: 2 | Ground temperature",,"Operational"
912.00,"02","Meteorological sequences common to surface data","302078","(State of ground and snow depth measurement)",,"002176","Method of state of ground measurement",,,"Operational"
913.00,"02","Meteorological sequences common to surface data","302078","(State of ground and snow depth measurement))",,"020062","State of the ground (with or without snow)",,,"Operational"
914.00,"02","Meteorological sequences common to surface data","302078","(State of ground and snow depth measurement)",,"002177","Method of snow depth measurement",,,"Operational"
915.00,"02","Meteorological sequences common to surface data","302078","(State of ground and snow depth measurement)",,"013013","Total snow depth",,,"Operational"
916.00,"02","Meteorological sequences common to surface data","302079","(Precipitation measurement)",,"007032","Height of sensor above local ground (or deck of marine platform)",,,"Operational"
917.00,"02","Meteorological sequences common to surface data","302079","(Precipitation measurement)",,"002175","Method of precipitation measurement",,,"Operational"
918.00,"02","Meteorological sequences common to surface data","302079","(Precipitation measurement)",,"002178","Method of liquid content measurement of precipitation",,,"Operational"
919.00,"02","Meteorological sequences common to surface data","302079","(Precipitation measurement)",,"004025","Time period or displacement",,,"Operational"
920.00,"02","Meteorological sequences common to surface data","302079","(Precipitation measurement)",,"013011","Total precipitation/total water equivalent",,,"Operational"
921.00,"02","Meteorological sequences common to surface data","302080","(Evaporation measurement)",,"002185","Method of evaporation measurement",,,"Operational"
922.00,"02","Meteorological sequences common to surface data","302080","(Evaporation measurement)",,"004025","Time period or displacement",,,"Operational"
923.00,"02","Meteorological sequences common to surface data","302080","(Evaporation measurement)",,"013033","Evaporation/evapotranspiration",,,"Operational"
924.00,"02","Meteorological sequences common to surface data","302081","(Total sunshine data)",,"004025","Time period or displacement",,,"Operational"
925.00,"02","Meteorological sequences common to surface data","302081","(Total sunshine data)",,"014031","Total sunshine",,,"Operational"
926.00,"02","Meteorological sequences common to surface data","302082","(Radiation data)",,"004025","Time period or displacement",,,"Operational"
927.00,"02","Meteorological sequences common to surface data","302082","(Radiation data)",,"014002","Long-wave radiation, integrated over period specified",,,"Operational"
928.00,"02","Meteorological sequences common to surface data","302082","(Radiation data)",,"014004","Short-wave radiation, integrated over period specified",,,"Operational"
929.00,"02","Meteorological sequences common to surface data","302082","(Radiation data)",,"014016","Net radiation, integrated over period specified",,,"Operational"
930.00,"02","Meteorological sequences common to surface data","302082","(Radiation data)",,"014028","Global solar radiation (high accuracy), integrated over period specified",,,"Operational"
931.00,"02","Meteorological sequences common to surface data","302082","(Radiation data)",,"014029","Diffuse solar radiation (high accuracy), integrated over period specified",,,"Operational"
932.00,"02","Meteorological sequences common to surface data","302082","(Radiation data)",,"014030","Direct solar radiation (high accuracy), integrated over period specified",,,"Operational"
933.00,"02","Meteorological sequences common to surface data","302083","(First-order statistics of P, W, T, U data)",,"004025","Time period or displacement",,,"Operational"
934.00,"02","Meteorological sequences common to surface data","302083","(First-order statistics of P, W, T, U data)",,"008023","First-order statistics",,,"Operational"
935.00,"02","Meteorological sequences common to surface data","302083","(First-order statistics of P, W, T, U data)",,"010004","Pressure",,,"Operational"
936.00,"02","Meteorological sequences common to surface data","302083","(First-order statistics of P, W, T, U data)",,"011001","Wind direction",,,"Operational"
937.00,"02","Meteorological sequences common to surface data","302083","(First-order statistics of P, W, T, U data)",,"011002","Wind speed",,,"Operational"
938.00,"02","Meteorological sequences common to surface data","302083","(First-order statistics of P, W, T, U data)",,"012101","Temperature/air temperature","Scale: 2",,"Operational"
939.00,"02","Meteorological sequences common to surface data","302083","(First-order statistics of P, W, T, U data)",,"013003","Relative humidity",,,"Operational"
940.00,"02","Meteorological sequences common to surface data","302083","(First-order statistics of P, W, T, U data)",,"008023","First-order statistics","Set to missing",,"Operational"
941.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)",,"302031","Pressure information",,,"Operational"
942.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)",,"302072","Temperature and humidity data",,,"Operational"
943.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)",,"103000","Delayed replication of 3 descriptors",,,"Operational"
944.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)",,"031000","Short delayed descriptor replication factor",,,"Operational"
945.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)",,"101005","Replicate 1 descriptor 5 times",,,"Operational"
946.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)",,"307063","Depth below land surface and soil temperature",,,"Operational"
947.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)",,"007061","Depth below land surface","Set to missing (cancel)",,"Operational"
948.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Visibility data","101000","Delayed replication of 1 descriptor",,,"Operational"
949.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Visibility data","031000","Short delayed descriptor replication factor",,,"Operational"
950.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Visibility data","302069","Visibility data",,,"Operational"
951.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Visibility data","007032","Height of sensor above local ground (or deck of marine platform)","Set to missing (cancel)",,"Operational"
952.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Visibility data","007033","Height of sensor above water surface","Set to missing (cancel)",,"Operational"
953.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Marine data","105000","Delayed replication of 5 descriptors",,,"Operational"
954.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Marine data","031000","Short delayed descriptor replication factor",,,"Operational"
955.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Marine data","020031","Ice deposit (thickness)",,,"Operational"
956.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Marine data","020032","Rate of ice accretion (estimated)",,,"Operational"
957.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Marine data","002038","Method of water temperature and/or salinity measurement",,,"Operational"
958.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Marine data","022043","Sea/water temperature","Scale: 2",,"Operational"
959.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Marine data","302021","Waves",,,"Operational"
960.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","State of ground and snow depth measurement","101000","Delayed replication of 1 descriptor",,,"Operational"
961.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","State of ground and snow depth measurement","031000","Short delayed descriptor replication factor",,,"Operational"
962.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","State of ground and snow depth measurement","302078","State of ground and snow depth measurement",,,"Operational"
963.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","State of ground and snow depth measurement","012113","Ground minimum temperature, past 12 hours","Scale: 2",,"Operational"
964.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Cloud data","101000","Delayed replication of 1 descriptor",,,"Operational"
965.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Cloud data","031000","Short delayed descriptor replication factor",,,"Operational"
966.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Cloud data","302004","General cloud information",,,"Operational"
967.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Cloud data","105000","Delayed replication of 5 descriptors",,,"Operational"
968.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Cloud data","031001","Delayed descriptor replication factor",,,"Operational"
969.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Cloud data","008002","Vertical significance (surface observations)",,,"Operational"
970.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Cloud data","020011","Cloud amount",,,"Operational"
971.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Cloud data","020012","Cloud type",,,"Operational"
972.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Cloud data","033041","Attribute of following value",,,"Operational"
973.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Cloud data","020013","Height of base of cloud",,,"Operational"
974.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Cloud data","302036","Clouds with bases below station level",,,"Operational"
975.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Direction of cloud drift 6DLDMDH","101000","Delayed replication of 1 descriptor",,,"Operational"
976.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Direction of cloud drift 6DLDMDH","031000","Short delayed descriptor replication factor",,,"Operational"
977.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Direction of cloud drift 6DLDMDH","302047","Direction of cloud drift",,,"Operational"
978.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Direction of cloud drift 6DLDMDH","008002","Vertical significance (surface observations)","Set to missing (cancel)",,"Operational"
979.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Direction and elevation of cloud 57CDaec","101000","Delayed replication of 1 descriptor",,,"Operational"
980.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Direction and elevation of cloud 57CDaec","031000","Short delayed descriptor replication factor",,,"Operational"
981.00,"02","Meteorological sequences common to surface data","302084","(""Instantaneous"" data of sequence 3 07 096)","Direction and elevation of cloud 57CDaec","302048","Direction and elevation of cloud",,,"Operational"
983.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Present and past weather data","105000","Delayed replication of 5 descriptors",,,"Operational"
984.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Present and past weather data","031000","Short delayed descriptor replication factor",,,"Operational"
985.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Present and past weather data","020003","Present weather",,,"Operational"
986.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Present and past weather data","103002","Replicate 3 descriptors 2 times",,,"Operational"
987.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Present and past weather data","004024","Time period or displacement","= -1 hour in the first replication, = -x hours in the second replication, x corresponding to the time period of W1W2 in the SYNOP report",,"Operational"
988.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Present and past weather data","020004","Past weather (1)",,,"Operational"
989.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Present and past weather data","020005","Past weather (2)",,,"Operational"
990.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Intensity of precipitation, size of precipitation element","101000","Delayed replication of 1 descriptor",,,"Operational"
991.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Intensity of precipitation, size of precipitation element","031000","Short delayed descriptor replication factor",,,"Operational"
992.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Intensity of precipitation, size of precipitation element","302175","Intensity of precipitation, size of precipitation element",,,"Operational"
993.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Precipitation, obscuration and other phenomena","102000","Delayed replication of 2 descriptors",,,"Operational"
994.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Precipitation, obscuration and other phenomena","031000","Short delayed descriptor replication factor",,,"Operational"
995.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Precipitation, obscuration and other phenomena","004025","Time period or displacement","= -10 minutes",,"Operational"
996.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Precipitation, obscuration and other phenomena","302076","Precipitation, obscuration and other phenomena",,,"Operational"
997.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Lightning data","102000","Delayed replication of 2 descriptors",,,"Operational"
998.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Lightning data","031000","Short delayed descriptor replication factor",,,"Operational"
999.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Lightning data","004025","Time period or displacement","= -10 minutes",,"Operational"
1000.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Lightning data","013059","Number of flashes (thunderstorm)",,,"Operational"
1001.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Wind data","007032","Height of sensor above local ground (or deck of marine platform)",,,"Operational"
1002.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Wind data","007033","Height of sensor above water surface",,,"Operational"
1003.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Wind data","008021","Time significance","= 2 Time averaged",,"Operational"
1004.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Wind data","004025","Time period or displacement","= -10 minutes, or number of minutes after a significant change of wind",,"Operational"
1005.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Wind data","011001","Wind direction",,,"Operational"
1006.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Wind data","011002","Wind speed",,,"Operational"
1007.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Wind data","008021","Time significance","Set to missing",,"Operational"
1008.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Wind data","103003","Replicate 3 descriptors 3 times",,,"Operational"
1009.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Wind data","004025","Time period or displacement","= -10 minutes in the first replication, = -60 minutes in the second replication, = -60x3 or 60x6 minutes in the third replication",,"Operational"
1010.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Wind data","011043","Maximum wind gust direction",,,"Operational"
1011.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Wind data","011041","Maximum wind gust speed",,,"Operational"
1012.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Wind data","004025","Time period or displacement","= -10 minutes",,"Operational"
1013.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Wind data","011016","Extreme counterclockwise wind direction of a variable wind",,,"Operational"
1014.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Wind data","011017","Extreme clockwise wind direction of a variable wind",,,"Operational"
1015.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Extreme temperature data","302077","Extreme temperature data",,,"Operational"
1016.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Extreme temperature data","007033","Height of sensor above water surface","Set to missing (cancel)",,"Operational"
1017.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Extreme temperature data","302041","Extreme temperature data",,,"Operational"
1018.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Precipitation measurement","106000","Delayed replication of 6 descriptors",,,"Operational"
1019.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Precipitation measurement","031000","Short delayed descriptor replication factor",,,"Operational"
1020.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Precipitation measurement","007032","Height of sensor above local ground (or deck of marine platform)",,,"Operational"
1021.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Precipitation measurement","002175","Method of precipitation measurement",,,"Operational"
1022.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Precipitation measurement","002178","Method of liquid content measurement of precipitation",,,"Operational"
1023.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Precipitation measurement","102005","Replicate 2 descriptors 5 times",,,"Operational"
1024.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Precipitation measurement","004024","Time period or displacement","= -1 hour in the first replication, = -3, -6, -12 and -24 hours in the other replications",,"Operational"
1025.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Precipitation measurement","013011","Total precipitation/total water equivalent",,,"Operational"
1026.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Precipitation measurement","007032","Height of sensor above local ground (or deck of marine platform)","Set to missing (cancel)",,"Operational"
1027.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Evaporation data","103000","Delayed replication of 3 descriptors",,,"Operational"
1028.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Evaporation data","031000","Short delayed descriptor replication factor",,,"Operational"
1029.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Evaporation data","002185","Method of evaporation measurement",,,"Operational"
1030.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Evaporation data","101002","Replicate 1 descriptor 2 times",,,"Operational"
1031.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Evaporation data","302044","Evaporation data",,,"Operational"
1032.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Total sunshine data","102000","Delayed replication of 2 descriptors",,,"Operational"
1033.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Total sunshine data","031000","Short delayed descriptor replication factor",,,"Operational"
1034.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Total sunshine data","101002","Replicate 1 descriptor 2 times",,,"Operational"
1035.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Total sunshine data","302039","Sunshine data (from 1 hour and 24 hour period)",,,"Operational"
1036.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Radiation data","102000","Delayed replication of 2 descriptors",,,"Operational"
1037.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Radiation data","031000","Short delayed descriptor replication factor",,,"Operational"
1038.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Radiation data","101002","Replicate 1 descriptor 2 times",,,"Operational"
1039.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Radiation data","302045","Radiation data (from 1 hour and 24 hour period)",,,"Operational"
1040.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Temperature change group 54g0sndT","101000","Delayed replication of 1 descriptor",,,"Operational"
1041.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Temperature change group 54g0sndT","031000","Short delayed descriptor replication factor",,,"Operational"
1042.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","Temperature change group 54g0sndT","302046","Temperature change",,,"Operational"
1043.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","First-order statistics of P, W, T, U data","101000","Delayed replication of 1 descriptor",,,"Operational"
1044.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","First-order statistics of P, W, T, U data","031000","Short delayed descriptor replication factor",,,"Operational"
1045.00,"02","Meteorological sequences common to surface data","302085","(""Period"" data of sequence 3 07 096)","First-order statistics of P, W, T, U data","302083","First-order statistics of P, W, T, U data",,,"Operational"
1047.00,"02","Meteorological sequences common to surface data","302089","(Locust information)",,"020101","Locust (acridian) name","Ln",,"Operational"
1048.00,"02","Meteorological sequences common to surface data","302089","(Locust information)",,"020102","Locust (maturity) colour","Lc",,"Operational"
1049.00,"02","Meteorological sequences common to surface data","302089","(Locust information)",,"020103","Stage of development of locusts","Ld",,"Operational"
1050.00,"02","Meteorological sequences common to surface data","302089","(Locust information)",,"020104","Organization state of swarm or band of locusts","Lg",,"Operational"
1051.00,"02","Meteorological sequences common to surface data","302089","(Locust information)",,"020105","Size of swarm or band of locusts and duration of passage of swarm","sL",,"Operational"
1052.00,"02","Meteorological sequences common to surface data","302089","(Locust information)",,"020106","Locust population density","dL",,"Operational"
1053.00,"02","Meteorological sequences common to surface data","302089","(Locust information)",,"020107","Direction of movements of locust swarm","DL",,"Operational"
1054.00,"02","Meteorological sequences common to surface data","302089","(Locust information)",,"020108","Extent of vegetation","ve",,"Operational"
1055.00,"02","Meteorological sequences common to surface data","302090","(Sea/water temperature high precision)",,"002038","Method of water temperature and/or salinity measurement",,,"Operational"
1056.00,"02","Meteorological sequences common to surface data","302090","(Sea/water temperature high precision)",,"007063","Depth below sea/water surface (cm)","Sea-surface temperature measurement",,"Operational"
1057.00,"02","Meteorological sequences common to surface data","302090","(Sea/water temperature high precision)",,"022045","Sea/water temperature",,,"Operational"
1058.00,"02","Meteorological sequences common to surface data","302175","(Intensity of precipitation, size of precipitation element)",,"008021","Time significance",,,"Operational"
1059.00,"02","Meteorological sequences common to surface data","302175","(Intensity of precipitation, size of precipitation element)",,"004025","Time period or displacement",,,"Operational"
1060.00,"02","Meteorological sequences common to surface data","302175","(Intensity of precipitation, size of precipitation element)",,"013155","Intensity of precipitation (high accuracy)",,,"Operational"
1061.00,"02","Meteorological sequences common to surface data","302175","(Intensity of precipitation, size of precipitation element)",,"013058","Size of precipitating element",,,"Operational"
1062.00,"02","Meteorological sequences common to surface data","302175","(Intensity of precipitation, size of precipitation element)",,"008021","Time significance",,,"Operational"
1063.00,"03","Meteorological sequences common to vertical soundings data","303001",,,"007003","Geopotential",,,"Operational"
1064.00,"03","Meteorological sequences common to vertical soundings data","303001",,,"011001","Wind direction",,,"Operational"
1065.00,"03","Meteorological sequences common to vertical soundings data","303001",,,"011002","Wind speed",,,"Operational"
1066.00,"03","Meteorological sequences common to vertical soundings data","303002","(Wind at pressure level)",,"007004","Pressure",,,"Operational"
1067.00,"03","Meteorological sequences common to vertical soundings data","303002","(Wind at pressure level)",,"011001","Wind direction",,,"Operational"
1068.00,"03","Meteorological sequences common to vertical soundings data","303002","(Wind at pressure level)",,"011002","Wind speed",,,"Operational"
1069.00,"03","Meteorological sequences common to vertical soundings data","303003",,,"007004","Pressure",,,"Operational"
1070.00,"03","Meteorological sequences common to vertical soundings data","303003",,,"010003","Geopotential",,,"Operational"
1071.00,"03","Meteorological sequences common to vertical soundings data","303003",,,"012001","Temperature/air temperature",,,"Operational"
1072.00,"03","Meteorological sequences common to vertical soundings data","303003",,,"012003","Dewpoint temperature",,,"Operational"
1073.00,"03","Meteorological sequences common to vertical soundings data","303004",,,"007004","Pressure",,,"Operational"
1074.00,"03","Meteorological sequences common to vertical soundings data","303004",,,"010003","Geopotential",,,"Operational"
1075.00,"03","Meteorological sequences common to vertical soundings data","303004",,,"012001","Temperature/air temperature",,,"Operational"
1076.00,"03","Meteorological sequences common to vertical soundings data","303004",,,"012003","Dewpoint temperature",,,"Operational"
1077.00,"03","Meteorological sequences common to vertical soundings data","303004",,,"011001","Wind direction",,,"Operational"
1078.00,"03","Meteorological sequences common to vertical soundings data","303004",,,"011002","Wind speed",,,"Operational"
1079.00,"03","Meteorological sequences common to vertical soundings data","303011","(Wind at height)",,"007003","Geopotential",,,"Operational"
1080.00,"03","Meteorological sequences common to vertical soundings data","303011","(Wind at height)",,"008001","Vertical sounding significance",,,"Operational"
1081.00,"03","Meteorological sequences common to vertical soundings data","303011","(Wind at height)",,"011001","Wind direction",,,"Operational"
1082.00,"03","Meteorological sequences common to vertical soundings data","303011","(Wind at height)",,"011002","Wind speed",,,"Operational"
1083.00,"03","Meteorological sequences common to vertical soundings data","303012","(Wind at pressure level)",,"007004","Pressure",,,"Operational"
1084.00,"03","Meteorological sequences common to vertical soundings data","303012","(Wind at pressure level)",,"008001","Vertical sounding significance",,,"Operational"
1085.00,"03","Meteorological sequences common to vertical soundings data","303012","(Wind at pressure level)",,"011001","Wind direction",,,"Operational"
1086.00,"03","Meteorological sequences common to vertical soundings data","303012","(Wind at pressure level)",,"011002","Wind speed",,,"Operational"
1087.00,"03","Meteorological sequences common to vertical soundings data","303013","(Geopotential, temperature, humidity, wind at pressure level)",,"007004","Pressure",,,"Operational"
1088.00,"03","Meteorological sequences common to vertical soundings data","303013","(Geopotential, temperature, humidity, wind at pressure level)",,"008001","Vertical sounding significance",,,"Operational"
1089.00,"03","Meteorological sequences common to vertical soundings data","303013","(Geopotential, temperature, humidity, wind at pressure level)",,"010003","Geopotential",,,"Operational"
1090.00,"03","Meteorological sequences common to vertical soundings data","303013","(Geopotential, temperature, humidity, wind at pressure level)",,"012001","Temperature/air temperature",,,"Operational"
1091.00,"03","Meteorological sequences common to vertical soundings data","303013","(Geopotential, temperature, humidity, wind at pressure level)",,"013003","Relative humidity",,,"Operational"
1092.00,"03","Meteorological sequences common to vertical soundings data","303013","(Geopotential, temperature, humidity, wind at pressure level)",,"011001","Wind direction",,,"Operational"
1093.00,"03","Meteorological sequences common to vertical soundings data","303013","(Geopotential, temperature, humidity, wind at pressure level)",,"011002","Wind speed",,,"Operational"
1094.00,"03","Meteorological sequences common to vertical soundings data","303014","(Geopotential, temperature, dewpoint temperature, wind at pressure level)",,"007004","Pressure",,,"Operational"
1095.00,"03","Meteorological sequences common to vertical soundings data","303014","(Geopotential, temperature, dewpoint temperature, wind at pressure level)",,"008001","Vertical sounding significance",,,"Operational"
1096.00,"03","Meteorological sequences common to vertical soundings data","303014","(Geopotential, temperature, dewpoint temperature, wind at pressure level)",,"010003","Geopotential",,,"Operational"
1097.00,"03","Meteorological sequences common to vertical soundings data","303014","(Geopotential, temperature, dewpoint temperature, wind at pressure level)",,"012001","Temperature/air temperature",,,"Operational"
1098.00,"03","Meteorological sequences common to vertical soundings data","303014","(Geopotential, temperature, dewpoint temperature, wind at pressure level)",,"012003","Dewpoint temperature",,,"Operational"
1099.00,"03","Meteorological sequences common to vertical soundings data","303014","(Geopotential, temperature, dewpoint temperature, wind at pressure level)",,"011001","Wind direction",,,"Operational"
1100.00,"03","Meteorological sequences common to vertical soundings data","303014","(Geopotential, temperature, dewpoint temperature, wind at pressure level)",,"011002","Wind speed",,,"Operational"
1101.00,"03","Meteorological sequences common to vertical soundings data","303021","(Layer, quality)",,"007004","Pressure","Define layer",,"Operational"
1102.00,"03","Meteorological sequences common to vertical soundings data","303021","(Layer, quality)",,"007004","Pressure",,,"Operational"
1103.00,"03","Meteorological sequences common to vertical soundings data","303021","(Layer, quality)",,"204007","Add associated field","7 bits long",,"Operational"
1104.00,"03","Meteorological sequences common to vertical soundings data","303021","(Layer, quality)",,"031021","Associated field significance",,,"Operational"
1106.00,"03","Meteorological sequences common to vertical soundings data","303022",,,"303021","Layer, quality",,,"Operational"
1107.00,"03","Meteorological sequences common to vertical soundings data","303022",,,"010003","Geopotential","Layer mean thickness",,"Operational"
1108.00,"03","Meteorological sequences common to vertical soundings data","303022",,,"204000","Add associated field","Cancel",,"Operational"
1110.00,"03","Meteorological sequences common to vertical soundings data","303023","(Layer mean temperature)",,"303021","Layer, quality",,,"Operational"
1111.00,"03","Meteorological sequences common to vertical soundings data","303023","(Layer mean temperature)",,"012001","Temperature/air temperature","Layer mean",,"Operational"
1112.00,"03","Meteorological sequences common to vertical soundings data","303023","(Layer mean temperature)",,"204000","Add associated field","Cancel",,"Operational"
1114.00,"03","Meteorological sequences common to vertical soundings data","303024","(Precipitable water)",,"303021","Layer, quality",,,"Operational"
1115.00,"03","Meteorological sequences common to vertical soundings data","303024","(Precipitable water)",,"013016","Precipitable water",,,"Operational"
1116.00,"03","Meteorological sequences common to vertical soundings data","303024","(Precipitable water)",,"204000","Add associated field","Cancel",,"Operational"
1118.00,"03","Meteorological sequences common to vertical soundings data","303025","(Satellite channel and brightness temperature)",,"002025","Satellite channel(s) used in computation",,,"Operational"
1119.00,"03","Meteorological sequences common to vertical soundings data","303025","(Satellite channel and brightness temperature)",,"204007","Add associated field","7 bits long",,"Operational"
1120.00,"03","Meteorological sequences common to vertical soundings data","303025","(Satellite channel and brightness temperature)",,"031021","Associated field significance",,,"Operational"
1121.00,"03","Meteorological sequences common to vertical soundings data","303025","(Satellite channel and brightness temperature)",,"012063","Brightness temperature",,,"Operational"
1122.00,"03","Meteorological sequences common to vertical soundings data","303025","(Satellite channel and brightness temperature)",,"204000","Add associated field","Cancel",,"Operational"
1124.00,"03","Meteorological sequences common to vertical soundings data","303026",,,"007004","Pressure",,,"Operational"
1125.00,"03","Meteorological sequences common to vertical soundings data","303026",,,"008003","Vertical significance (satellite observations)",,,"Operational"
1126.00,"03","Meteorological sequences common to vertical soundings data","303026",,,"204007","Add associated field","7 bits long",,"Operational"
1127.00,"03","Meteorological sequences common to vertical soundings data","303026",,,"031021","Associated field significance",,,"Operational"
1128.00,"03","Meteorological sequences common to vertical soundings data","303026",,,"012001","Temperature/air temperature",,,"Operational"
1129.00,"03","Meteorological sequences common to vertical soundings data","303026",,,"204000","Add associated field","Cancel",,"Operational"
1131.00,"03","Meteorological sequences common to vertical soundings data","303027",,,"007004","Pressure",,,"Operational"
1132.00,"03","Meteorological sequences common to vertical soundings data","303027",,,"204007","Add associated field","7 bits long",,"Operational"
1133.00,"03","Meteorological sequences common to vertical soundings data","303027",,,"031021","Associated field significance",,,"Operational"
1134.00,"03","Meteorological sequences common to vertical soundings data","303027",,,"010003","Geopotential",,,"Operational"
1135.00,"03","Meteorological sequences common to vertical soundings data","303027",,,"204000","Add associated field","Cancel",,"Operational"
1137.00,"03","Meteorological sequences common to vertical soundings data","303031","(Significance data, land/sea, skin temperature)",,"007004","Pressure",,,"Operational"
1138.00,"03","Meteorological sequences common to vertical soundings data","303031","(Significance data, land/sea, skin temperature)",,"008003","Vertical significance (satellite observations)","Base of sounding",,"Operational"
1139.00,"03","Meteorological sequences common to vertical soundings data","303031","(Significance data, land/sea, skin temperature)",,"007021","Elevation","Local zenith",,"Operational"
1140.00,"03","Meteorological sequences common to vertical soundings data","303031","(Significance data, land/sea, skin temperature)",,"007022","Solar elevation","Solar zenith",,"Operational"
1141.00,"03","Meteorological sequences common to vertical soundings data","303031","(Significance data, land/sea, skin temperature)",,"008012","Land/sea qualifier",,,"Operational"
1142.00,"03","Meteorological sequences common to vertical soundings data","303031","(Significance data, land/sea, skin temperature)",,"012061","Skin temperature",,,"Operational"
1143.00,"03","Meteorological sequences common to vertical soundings data","303032","(Cloud)",,"020011","Cloud amount",,,"Operational"
1144.00,"03","Meteorological sequences common to vertical soundings data","303032","(Cloud)",,"020016","Pressure at top of cloud",,,"Operational"
1145.00,"03","Meteorological sequences common to vertical soundings data","303033","(Cloud)",,"020010","Cloud cover (total)",,,"Operational"
1146.00,"03","Meteorological sequences common to vertical soundings data","303033","(Cloud)",,"020016","Pressure at top of cloud",,,"Operational"
1147.00,"03","Meteorological sequences common to vertical soundings data","303040","(Radiosonde duration of flight and termination information)",,"008041","Data significance","= 7 Flight level termination point",,"Operational"
1148.00,"03","Meteorological sequences common to vertical soundings data","303040","(Radiosonde duration of flight and termination information)",,"004025","Time period or displacement","Minutes",,"Operational"
1149.00,"03","Meteorological sequences common to vertical soundings data","303040","(Radiosonde duration of flight and termination information)",,"004026","Time period or displacement","Seconds",,"Operational"
1150.00,"03","Meteorological sequences common to vertical soundings data","303040","(Radiosonde duration of flight and termination information)",,"301021","Latitude/longitude (high accuracy)",,,"Operational"
1151.00,"03","Meteorological sequences common to vertical soundings data","303040","(Radiosonde duration of flight and termination information)",,"301122","Date/time (to hundredths of second)",,,"Operational"
1152.00,"03","Meteorological sequences common to vertical soundings data","303040","(Radiosonde duration of flight and termination information)",,"201131","Change data width",,,"Operational"
1153.00,"03","Meteorological sequences common to vertical soundings data","303040","(Radiosonde duration of flight and termination information)",,"202129","Change scale",,,"Operational"
1154.00,"03","Meteorological sequences common to vertical soundings data","303040","(Radiosonde duration of flight and termination information)",,"025069","Flight level pressure corrections",,,"Operational"
1155.00,"03","Meteorological sequences common to vertical soundings data","303040","(Radiosonde duration of flight and termination information)",,"007004","Pressure",,,"Operational"
1156.00,"03","Meteorological sequences common to vertical soundings data","303040","(Radiosonde duration of flight and termination information)",,"013003","Relative humidity",,,"Operational"
1157.00,"03","Meteorological sequences common to vertical soundings data","303040","(Radiosonde duration of flight and termination information)",,"202000","Change scale","Cancel",,"Operational"
1158.00,"03","Meteorological sequences common to vertical soundings data","303040","(Radiosonde duration of flight and termination information)",,"201000","Change data width","Cancel",,"Operational"
1159.00,"03","Meteorological sequences common to vertical soundings data","303040","(Radiosonde duration of flight and termination information)",,"002013","Solar and infrared radiation correction",,,"Operational"
1160.00,"03","Meteorological sequences common to vertical soundings data","303040","(Radiosonde duration of flight and termination information)",,"012101","Temperature/air temperature",,,"Operational"
1161.00,"03","Meteorological sequences common to vertical soundings data","303040","(Radiosonde duration of flight and termination information)",,"010009","Geopotential height",,,"Operational"
1162.00,"03","Meteorological sequences common to vertical soundings data","303040","(Radiosonde duration of flight and termination information)",,"102002","Replicate 2 descriptors 2 times",,,"Operational"
1163.00,"03","Meteorological sequences common to vertical soundings data","303040","(Radiosonde duration of flight and termination information)",,"008040","Flight level significance",,,"Operational"
1164.00,"03","Meteorological sequences common to vertical soundings data","303040","(Radiosonde duration of flight and termination information)",,"035035","Reason for termination",,,"Operational"
1166.00,"03","Meteorological sequences common to vertical soundings data","303041","(Wind sequence)",,"002152","Satellite instrument used in data processing",,,"Operational"
1167.00,"03","Meteorological sequences common to vertical soundings data","303041","(Wind sequence)",,"002023","Satellite-derived wind computation method",,,"Operational"
1168.00,"03","Meteorological sequences common to vertical soundings data","303041","(Wind sequence)",,"007004","Pressure",,,"Operational"
1169.00,"03","Meteorological sequences common to vertical soundings data","303041","(Wind sequence)",,"011001","Wind direction",,,"Operational"
1170.00,"03","Meteorological sequences common to vertical soundings data","303041","(Wind sequence)",,"011002","Wind speed",,,"Operational"
1171.00,"03","Meteorological sequences common to vertical soundings data","303041","(Wind sequence)",,"002153","Satellite channel centre frequency",,,"Operational"
1172.00,"03","Meteorological sequences common to vertical soundings data","303041","(Wind sequence)",,"002154","Satellite channel band width",,,"Operational"
1173.00,"03","Meteorological sequences common to vertical soundings data","303041","(Wind sequence)",,"012071","Coldest cluster temperature",,,"Operational"
1174.00,"03","Meteorological sequences common to vertical soundings data","303050","(Wind data at a pressure level with radiosonde position)",,"004086","Long time period or displacement","Since launch time",,"Operational"
1175.00,"03","Meteorological sequences common to vertical soundings data","303050","(Wind data at a pressure level with radiosonde position)",,"008042","Extended vertical sounding significance",,,"Operational"
1176.00,"03","Meteorological sequences common to vertical soundings data","303050","(Wind data at a pressure level with radiosonde position)",,"007004","Pressure",,,"Operational"
1177.00,"03","Meteorological sequences common to vertical soundings data","303050","(Wind data at a pressure level with radiosonde position)",,"005015","Latitude displacement (high accuracy)","Since launch site",,"Operational"
1178.00,"03","Meteorological sequences common to vertical soundings data","303050","(Wind data at a pressure level with radiosonde position)",,"006015","Longitude displacement (high accuracy)","Since launch site",,"Operational"
1179.00,"03","Meteorological sequences common to vertical soundings data","303050","(Wind data at a pressure level with radiosonde position)",,"011001","Wind direction",,,"Operational"
1180.00,"03","Meteorological sequences common to vertical soundings data","303050","(Wind data at a pressure level with radiosonde position)",,"011002","Wind speed",,,"Operational"
1181.00,"03","Meteorological sequences common to vertical soundings data","303051","(Wind shear data at a pressure level with radiosonde position)",,"004086","Long time period or displacement","Since launch time",,"Operational"
1182.00,"03","Meteorological sequences common to vertical soundings data","303051","(Wind shear data at a pressure level with radiosonde position)",,"008042","Extended vertical sounding significance",,,"Operational"
1183.00,"03","Meteorological sequences common to vertical soundings data","303051","(Wind shear data at a pressure level with radiosonde position)",,"007004","Pressure",,,"Operational"
1184.00,"03","Meteorological sequences common to vertical soundings data","303051","(Wind shear data at a pressure level with radiosonde position)",,"005015","Latitude displacement (high accuracy)","Since launch site",,"Operational"
1185.00,"03","Meteorological sequences common to vertical soundings data","303051","(Wind shear data at a pressure level with radiosonde position)",,"006015","Longitude displacement (high accuracy)","Since launch site",,"Operational"
1186.00,"03","Meteorological sequences common to vertical soundings data","303051","(Wind shear data at a pressure level with radiosonde position)",,"011061","Absolute wind shear in 1 km layer below",,,"Operational"
1187.00,"03","Meteorological sequences common to vertical soundings data","303051","(Wind shear data at a pressure level with radiosonde position)",,"011062","Absolute wind shear in 1 km layer above",,,"Operational"
1188.00,"03","Meteorological sequences common to vertical soundings data","303052","(Wind data at a height level with radiosonde position)",,"004086","Long time period or displacement","Since launch time",,"Operational"
1189.00,"03","Meteorological sequences common to vertical soundings data","303052","(Wind data at a height level with radiosonde position)",,"008042","Extended vertical sounding significance",,,"Operational"
1190.00,"03","Meteorological sequences common to vertical soundings data","303052","(Wind data at a height level with radiosonde position)",,"007009","Geopotential height",,,"Operational"
1191.00,"03","Meteorological sequences common to vertical soundings data","303052","(Wind data at a height level with radiosonde position)",,"005015","Latitude displacement (high accuracy)","Since launch site",,"Operational"
1192.00,"03","Meteorological sequences common to vertical soundings data","303052","(Wind data at a height level with radiosonde position)",,"006015","Longitude displacement (high accuracy)","Since launch site",,"Operational"
1193.00,"03","Meteorological sequences common to vertical soundings data","303052","(Wind data at a height level with radiosonde position)",,"011001","Wind direction",,,"Operational"
1194.00,"03","Meteorological sequences common to vertical soundings data","303052","(Wind data at a height level with radiosonde position)",,"011002","Wind speed",,,"Operational"
1195.00,"03","Meteorological sequences common to vertical soundings data","303053","(Wind shear data at a height level with radiosonde position)",,"004086","Long time period or displacement","Since launch time",,"Operational"
1196.00,"03","Meteorological sequences common to vertical soundings data","303053","(Wind shear data at a height level with radiosonde position)",,"008042","Extended vertical sounding significance",,,"Operational"
1197.00,"03","Meteorological sequences common to vertical soundings data","303053","(Wind shear data at a height level with radiosonde position)",,"007009","Geopotential height",,,"Operational"
1198.00,"03","Meteorological sequences common to vertical soundings data","303053","(Wind shear data at a height level with radiosonde position)",,"005015","Latitude displacement (high accuracy)","Since launch site",,"Operational"
1199.00,"03","Meteorological sequences common to vertical soundings data","303053","(Wind shear data at a height level with radiosonde position)",,"006015","Longitude displacement (high accuracy)","Since launch site",,"Operational"
1200.00,"03","Meteorological sequences common to vertical soundings data","303053","(Wind shear data at a height level with radiosonde position)",,"011061","Absolute wind shear in 1 km layer below",,,"Operational"
1201.00,"03","Meteorological sequences common to vertical soundings data","303053","(Wind shear data at a height level with radiosonde position)",,"011062","Absolute wind shear in 1 km layer above",,,"Operational"
1202.00,"03","Meteorological sequences common to vertical soundings data","303054","(Temperature, dewpoint and wind data at a pressure level with radiosonde position)",,"004086","Long time period or displacement","Since launch time",,"Operational"
1203.00,"03","Meteorological sequences common to vertical soundings data","303054","(Temperature, dewpoint and wind data at a pressure level with radiosonde position)",,"008042","Extended vertical sounding significance",,,"Operational"
1204.00,"03","Meteorological sequences common to vertical soundings data","303054","(Temperature, dewpoint and wind data at a pressure level with radiosonde position)",,"007004","Pressure",,,"Operational"
1205.00,"03","Meteorological sequences common to vertical soundings data","303054","(Temperature, dewpoint and wind data at a pressure level with radiosonde position)",,"010009","Geopotential height",,,"Operational"
1206.00,"03","Meteorological sequences common to vertical soundings data","303054","(Temperature, dewpoint and wind data at a pressure level with radiosonde position)",,"005015","Latitude displacement (high accuracy)","Since launch site",,"Operational"
1207.00,"03","Meteorological sequences common to vertical soundings data","303054","(Temperature, dewpoint and wind data at a pressure level with radiosonde position)",,"006015","Longitude displacement (high accuracy)","Since launch site",,"Operational"
1208.00,"03","Meteorological sequences common to vertical soundings data","303054","(Temperature, dewpoint and wind data at a pressure level with radiosonde position)",,"012101","Temperature/air temperature","Scale: 2",,"Operational"
1209.00,"03","Meteorological sequences common to vertical soundings data","303054","(Temperature, dewpoint and wind data at a pressure level with radiosonde position)",,"012103","Dewpoint temperature","Scale: 2",,"Operational"
1210.00,"03","Meteorological sequences common to vertical soundings data","303054","(Temperature, dewpoint and wind data at a pressure level with radiosonde position)",,"011001","Wind direction",,,"Operational"
1211.00,"03","Meteorological sequences common to vertical soundings data","303054","(Temperature, dewpoint and wind data at a pressure level with radiosonde position)",,"011002","Wind speed",,,"Operational"
1212.00,"03","Meteorological sequences common to vertical soundings data","303055","(Temperature, dewpoint, relative humidity and wind data at a height level with radiosonde position)",,"004086","Long time period or displacement","Since launch time",,"Operational"
1213.00,"03","Meteorological sequences common to vertical soundings data","303055","(Temperature, dewpoint, relative humidity and wind data at a height level with radiosonde position)",,"008042","Extended vertical sounding significance",,,"Operational"
1214.00,"03","Meteorological sequences common to vertical soundings data","303055","(Temperature, dewpoint, relative humidity and wind data at a height level with radiosonde position)",,"007009","Geopotential height",,,"Operational"
1215.00,"03","Meteorological sequences common to vertical soundings data","303055","(Temperature, dewpoint, relative humidity and wind data at a height level with radiosonde position)",,"005015","Latitude displacement (high accuracy)","Since launch site",,"Operational"
1216.00,"03","Meteorological sequences common to vertical soundings data","303055","(Temperature, dewpoint, relative humidity and wind data at a height level with radiosonde position)",,"006015","Longitude displacement (high accuracy)","Since launch site",,"Operational"
1217.00,"03","Meteorological sequences common to vertical soundings data","303055","(Temperature, dewpoint, relative humidity and wind data at a height level with radiosonde position)",,"012101","Temperature/air temperature","Scale: 2",,"Operational"
1218.00,"03","Meteorological sequences common to vertical soundings data","303055","(Temperature, dewpoint, relative humidity and wind data at a height level with radiosonde position)",,"013009","Relative humidity",,,"Operational"
1219.00,"03","Meteorological sequences common to vertical soundings data","303055","(Temperature, dewpoint, relative humidity and wind data at a height level with radiosonde position)",,"012103","Dewpoint temperature","Scale: 2",,"Operational"
1220.00,"03","Meteorological sequences common to vertical soundings data","303055","(Temperature, dewpoint, relative humidity and wind data at a height level with radiosonde position)",,"011001","Wind direction",,,"Operational"
1221.00,"03","Meteorological sequences common to vertical soundings data","303055","(Temperature, dewpoint, relative humidity and wind data at a height level with radiosonde position)",,"011002","Wind speed",,,"Operational"
1222.00,"04","Meteorological sequences common to satellite observations","304001","(Cloud top pressure, temperature, wind)",,"008003","Vertical significance (satellite observations)",,,"Operational"
1223.00,"04","Meteorological sequences common to satellite observations","304001","(Cloud top pressure, temperature, wind)",,"010004","Pressure",,,"Operational"
1224.00,"04","Meteorological sequences common to satellite observations","304001","(Cloud top pressure, temperature, wind)",,"012001","Temperature/air temperature",,,"Operational"
1225.00,"04","Meteorological sequences common to satellite observations","304001","(Cloud top pressure, temperature, wind)",,"011001","Wind direction",,,"Operational"
1226.00,"04","Meteorological sequences common to satellite observations","304001","(Cloud top pressure, temperature, wind)",,"011002","Wind speed",,,"Operational"
1227.00,"04","Meteorological sequences common to satellite observations","304002","(Cloud top pressure, wind)",,"008003","Vertical significance (satellite observations)",,,"Operational"
1228.00,"04","Meteorological sequences common to satellite observations","304002","(Cloud top pressure, wind)",,"010004","Pressure",,,"Operational"
1229.00,"04","Meteorological sequences common to satellite observations","304002","(Cloud top pressure, wind)",,"011001","Wind direction",,,"Operational"
1230.00,"04","Meteorological sequences common to satellite observations","304002","(Cloud top pressure, wind)",,"011002","Wind speed",,,"Operational"
1231.00,"04","Meteorological sequences common to satellite observations","304003","(Surface temperature)",,"008003","Vertical significance (satellite observations)",,,"Operational"
1232.00,"04","Meteorological sequences common to satellite observations","304003","(Surface temperature)",,"012001","Temperature/air temperature",,,"Operational"
1233.00,"04","Meteorological sequences common to satellite observations","304004","(Cloud top pressure, cloud cover, temperature)",,"008003","Vertical significance (satellite observations)",,,"Operational"
1234.00,"04","Meteorological sequences common to satellite observations","304004","(Cloud top pressure, cloud cover, temperature)",,"010004","Pressure",,,"Operational"
1235.00,"04","Meteorological sequences common to satellite observations","304004","(Cloud top pressure, cloud cover, temperature)",,"020010","Cloud cover (total)",,,"Operational"
1236.00,"04","Meteorological sequences common to satellite observations","304004","(Cloud top pressure, cloud cover, temperature)",,"012001","Temperature/air temperature",,,"Operational"
1237.00,"04","Meteorological sequences common to satellite observations","304005","(Layer mean relative humidity)",,"002024","Integrated mean humidity computational method",,,"Operational"
1238.00,"04","Meteorological sequences common to satellite observations","304005","(Layer mean relative humidity)",,"007004","Pressure","Define layer",,"Operational"
1239.00,"04","Meteorological sequences common to satellite observations","304005","(Layer mean relative humidity)",,"007004","Pressure",,,"Operational"
1240.00,"04","Meteorological sequences common to satellite observations","304005","(Layer mean relative humidity)",,"013003","Relative humidity",,,"Operational"
1241.00,"04","Meteorological sequences common to satellite observations","304006","(Radiation)",,"014001","Long-wave radiation, integrated over 24 hours","Outgoing long-wave radiation",,"Operational"
1242.00,"04","Meteorological sequences common to satellite observations","304006","(Radiation)",,"014001","Long-wave radiation, integrated over 24 hours","Incoming long-wave radiation",,"Operational"
1243.00,"04","Meteorological sequences common to satellite observations","304006","(Radiation)",,"014003","Short-wave radiation, integrated over 24 hours","Outgoing short-wave radiation",,"Operational"
1244.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"002163","Height assignment method",,,"Operational"
1245.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"002164","Tracer correlation method",,,"Operational"
1246.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"008012","Land/sea qualifier",,,"Operational"
1247.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"007024","Satellite zenith angle",,,"Operational"
1248.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"002057","Origin of first-guess information for GOES-I/M soundings",,,"Operational"
1249.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"008021","Time significance",,,"Operational"
1250.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"004001","Year",,,"Operational"
1251.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"004002","Month",,,"Operational"
1252.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"004003","Day",,,"Operational"
1253.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"004004","Hour",,,"Operational"
1254.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"008021","Time significance",,,"Operational"
1255.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"004024","Time period or displacement",,,"Operational"
1256.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"110004","Replicate 10 descriptors 4 times",,,"Operational"
1257.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"008021","Time significance",,,"Operational"
1258.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"004004","Hour",,,"Operational"
1259.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"004005","Minute",,,"Operational"
1260.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"004006","Second",,,"Operational"
1261.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"008021","Time significance",,,"Operational"
1262.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"004004","Hour",,,"Operational"
1263.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"004005","Minute",,,"Operational"
1264.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"004006","Second",,,"Operational"
1265.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"011001","Wind direction",,,"Operational"
1266.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"011002","Wind speed",,,"Operational"
1267.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"103010","Replicate 3 descriptors 10 times",,,"Operational"
1268.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"002163","Height assignment method",,,"Operational"
1269.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"007004","Pressure",,,"Operational"
1270.00,"04","Meteorological sequences common to satellite observations","304011","(GOES-I/M info)",,"012001","Temperature/air temperature",,,"Operational"
1271.00,"04","Meteorological sequences common to satellite observations","304030","(Location of platform)",,"027031","In direction of 0 degrees longitude, distance from the Earth's centre",,,"Operational"
1272.00,"04","Meteorological sequences common to satellite observations","304030","(Location of platform)",,"028031","In direction 90 degrees East, distance from the Earth's centre",,,"Operational"
1273.00,"04","Meteorological sequences common to satellite observations","304030","(Location of platform)",,"010031","In direction of the North Pole, distance from the Earth's centre",,,"Operational"
1274.00,"04","Meteorological sequences common to satellite observations","304031","(Speed of platform)",,"001041","Absolute platform velocity - first component",,,"Operational"
1275.00,"04","Meteorological sequences common to satellite observations","304031","(Speed of platform)",,"001042","Absolute platform velocity - second component",,,"Operational"
1276.00,"04","Meteorological sequences common to satellite observations","304031","(Speed of platform)",,"001043","Absolute platform velocity - third component",,,"Operational"
1277.00,"04","Meteorological sequences common to satellite observations","304032","(Cloud fraction)",,"002153","Satellite channel centre frequency",,,"Operational"
1278.00,"04","Meteorological sequences common to satellite observations","304032","(Cloud fraction)",,"002154","Satellite channel band width",,,"Operational"
1279.00,"04","Meteorological sequences common to satellite observations","304032","(Cloud fraction)",,"020081","Cloud amount in segment",,,"Operational"
1280.00,"04","Meteorological sequences common to satellite observations","304032","(Cloud fraction)",,"020082","Amount segment cloud free",,,"Operational"
1281.00,"04","Meteorological sequences common to satellite observations","304032","(Cloud fraction)",,"020012","Cloud type",,,"Operational"
1282.00,"04","Meteorological sequences common to satellite observations","304033","(Clear sky radiance)",,"002152","Satellite instrument used in data processing",,,"Operational"
1283.00,"04","Meteorological sequences common to satellite observations","304033","(Clear sky radiance)",,"002166","Radiance type",,,"Operational"
1284.00,"04","Meteorological sequences common to satellite observations","304033","(Clear sky radiance)",,"002167","Radiance computational method",,,"Operational"
1285.00,"04","Meteorological sequences common to satellite observations","304033","(Clear sky radiance)",,"002153","Satellite channel centre frequency",,,"Operational"
1286.00,"04","Meteorological sequences common to satellite observations","304033","(Clear sky radiance)",,"002154","Satellite channel band width",,,"Operational"
1287.00,"04","Meteorological sequences common to satellite observations","304033","(Clear sky radiance)",,"012075","Spectral radiance",,,"Operational"
1288.00,"04","Meteorological sequences common to satellite observations","304033","(Clear sky radiance)",,"012076","Radiance",,,"Operational"
1289.00,"04","Meteorological sequences common to satellite observations","304033","(Clear sky radiance)",,"012063","Brightness temperature",,,"Operational"
1290.00,"04","Meteorological sequences common to satellite observations","304034","(Latitude/longitude, solar elevation, number of layers)",,"102004","Replicate 2 descriptors 4 times",,,"Operational"
1291.00,"04","Meteorological sequences common to satellite observations","304034","(Latitude/longitude, solar elevation, number of layers)",,"027001","Latitude (high accuracy)",,,"Operational"
1292.00,"04","Meteorological sequences common to satellite observations","304034","(Latitude/longitude, solar elevation, number of layers)",,"028001","Longitude (high accuracy)",,,"Operational"
1293.00,"04","Meteorological sequences common to satellite observations","304034","(Latitude/longitude, solar elevation, number of layers)",,"007022","Solar elevation",,,"Operational"
1294.00,"04","Meteorological sequences common to satellite observations","304034","(Latitude/longitude, solar elevation, number of layers)",,"005043","Field of view number",,,"Operational"
1295.00,"04","Meteorological sequences common to satellite observations","304034","(Latitude/longitude, solar elevation, number of layers)",,"020010","Cloud cover (total)",,,"Operational"
1296.00,"04","Meteorological sequences common to satellite observations","304034","(Latitude/longitude, solar elevation, number of layers)",,"020016","Pressure at top of cloud",,,"Operational"
1297.00,"04","Meteorological sequences common to satellite observations","304034","(Latitude/longitude, solar elevation, number of layers)",,"033003","Quality information",,,"Operational"
1298.00,"04","Meteorological sequences common to satellite observations","304034","(Latitude/longitude, solar elevation, number of layers)",,"010040","Number of retrieved layers",,,"Operational"
1299.00,"04","Meteorological sequences common to satellite observations","304035","(All sky radiance data)",,"002153","Satellite channel centre frequency",,,"Deprecated"
1300.00,"04","Meteorological sequences common to satellite observations","304035","(All sky radiance data)",,"002154","Satellite channel band width",,,"Deprecated"
1301.00,"04","Meteorological sequences common to satellite observations","304035","(All sky radiance data)",,"012063","Brightness temperature",,,"Deprecated"
1302.00,"04","Meteorological sequences common to satellite observations","304035","(All sky radiance data)",,"008001","Meteorological feature","Pixel type: clear",,"Deprecated"
1303.00,"04","Meteorological sequences common to satellite observations","304035","(All sky radiance data)",,"012063","Brightness temperature","Clear",,"Deprecated"
1304.00,"04","Meteorological sequences common to satellite observations","304035","(All sky radiance data)",,"008001","Meteorological feature","Pixel type: cloudy",,"Deprecated"
1305.00,"04","Meteorological sequences common to satellite observations","304035","(All sky radiance data)",,"012063","Brightness temperature","Cloudy",,"Deprecated"
1306.00,"04","Meteorological sequences common to satellite observations","304035","(All sky radiance data)",,"008001","Meteorological feature","Cancel",,"Deprecated"
1307.00,"04","Meteorological sequences common to satellite observations","304035","(All sky radiance data)",,"008003","Vertical significance (satellite observations)","Low cloud",,"Deprecated"
1308.00,"04","Meteorological sequences common to satellite observations","304035","(All sky radiance data)",,"012063","Brightness temperature","Low cloud",,"Deprecated"
1309.00,"04","Meteorological sequences common to satellite observations","304035","(All sky radiance data)",,"008003","Vertical significance (satellite observations)","Mid cloud",,"Deprecated"
1310.00,"04","Meteorological sequences common to satellite observations","304035","(All sky radiance data)",,"012063","Brightness temperature","Mid cloud",,"Deprecated"
1311.00,"04","Meteorological sequences common to satellite observations","304035","(All sky radiance data)",,"008003","Vertical significance (satellite observations)","High cloud",,"Deprecated"
1312.00,"04","Meteorological sequences common to satellite observations","304035","(All sky radiance data)",,"012063","Brightness temperature","High cloud",,"Deprecated"
1313.00,"04","Meteorological sequences common to satellite observations","304035","(All sky radiance data)",,"008003","Vertical significance (satellite observations)","Cancel",,"Deprecated"
1314.00,"04","Meteorological sequences common to satellite observations","304036","(Cloud coverage)",,"020082","Amount segment cloud free",,,"Operational"
1315.00,"04","Meteorological sequences common to satellite observations","304036","(Cloud coverage)",,"008012","Land/sea qualifier","Sea",,"Operational"
1316.00,"04","Meteorological sequences common to satellite observations","304036","(Cloud coverage)",,"020082","Amount segment cloud free","Sea",,"Operational"
1317.00,"04","Meteorological sequences common to satellite observations","304036","(Cloud coverage)",,"008012","Land/sea qualifier","Cancel",,"Operational"
1318.00,"04","Meteorological sequences common to satellite observations","304036","(Cloud coverage)",,"020081","Cloud amount in segment",,,"Operational"
1319.00,"04","Meteorological sequences common to satellite observations","304036","(Cloud coverage)",,"008003","Vertical significance (satellite observations)","Low cloud",,"Operational"
1320.00,"04","Meteorological sequences common to satellite observations","304036","(Cloud coverage)",,"020081","Cloud amount in segment","Low cloud",,"Operational"
1321.00,"04","Meteorological sequences common to satellite observations","304036","(Cloud coverage)",,"008003","Vertical significance (satellite observations)","Mid cloud",,"Operational"
1322.00,"04","Meteorological sequences common to satellite observations","304036","(Cloud coverage)",,"020081","Cloud amount in segment","Mid cloud",,"Operational"
1323.00,"04","Meteorological sequences common to satellite observations","304036","(Cloud coverage)",,"008003","Vertical significance (satellite observations)","High cloud",,"Operational"
1324.00,"04","Meteorological sequences common to satellite observations","304036","(Cloud coverage)",,"020081","Cloud amount in segment","High cloud",,"Operational"
1325.00,"04","Meteorological sequences common to satellite observations","304036","(Cloud coverage)",,"008003","Vertical significance (satellite observations)","Cancel",,"Operational"
1326.00,"04","Meteorological sequences common to satellite observations","304037","(All sky radiance data)",,"002153","Satellite channel centre frequency",,,"Operational"
1327.00,"04","Meteorological sequences common to satellite observations","304037","(All sky radiance data)",,"002154","Satellite channel band width",,,"Operational"
1328.00,"04","Meteorological sequences common to satellite observations","304037","(All sky radiance data)",,"012063","Brightness temperature",,,"Operational"
1329.00,"04","Meteorological sequences common to satellite observations","304037","(All sky radiance data)",,"008011","Meteorological feature","Pixel type: clear",,"Operational"
1330.00,"04","Meteorological sequences common to satellite observations","304037","(All sky radiance data)",,"012063","Brightness temperature","Clear",,"Operational"
1331.00,"04","Meteorological sequences common to satellite observations","304037","(All sky radiance data)",,"008011","Meteorological feature","Pixel type: cloudy",,"Operational"
1332.00,"04","Meteorological sequences common to satellite observations","304037","(All sky radiance data)",,"012063","Brightness temperature","Cloudy",,"Operational"
1333.00,"04","Meteorological sequences common to satellite observations","304037","(All sky radiance data)",,"008011","Meteorological feature","Cancel",,"Operational"
1334.00,"04","Meteorological sequences common to satellite observations","304037","(All sky radiance data)",,"008003","Vertical significance (satellite observations)","Low cloud",,"Operational"
1335.00,"04","Meteorological sequences common to satellite observations","304037","(All sky radiance data)",,"012063","Brightness temperature","Low cloud",,"Operational"
1336.00,"04","Meteorological sequences common to satellite observations","304037","(All sky radiance data)",,"008003","Vertical significance (satellite observations)","Mid cloud",,"Operational"
1337.00,"04","Meteorological sequences common to satellite observations","304037","(All sky radiance data)",,"012063","Brightness temperature","Mid cloud",,"Operational"
1338.00,"04","Meteorological sequences common to satellite observations","304037","(All sky radiance data)",,"008003","Vertical significance (satellite observations)","High cloud",,"Operational"
1339.00,"04","Meteorological sequences common to satellite observations","304037","(All sky radiance data)",,"012063","Brightness temperature","High cloud",,"Operational"
1340.00,"05","Meteorological or hydrological sequences common to hydrological observations","305001","(SADC-HYCOS single measurement)",,"011001","Wind direction",,,"Operational"
1341.00,"05","Meteorological or hydrological sequences common to hydrological observations","305001","(SADC-HYCOS single measurement)",,"011002","Wind speed",,,"Operational"
1342.00,"05","Meteorological or hydrological sequences common to hydrological observations","305001","(SADC-HYCOS single measurement)",,"013060","Total accumulated precipitation",,,"Operational"
1343.00,"05","Meteorological or hydrological sequences common to hydrological observations","305001","(SADC-HYCOS single measurement)",,"013071","Upstream water level",,,"Operational"
1344.00,"05","Meteorological or hydrological sequences common to hydrological observations","305002","(SADC-HYCOS environmental measurement)",,"301012","Hour, minute",,,"Operational"
1345.00,"05","Meteorological or hydrological sequences common to hydrological observations","305002","(SADC-HYCOS environmental measurement)",,"012001","Temperature/air temperature",,,"Operational"
1346.00,"05","Meteorological or hydrological sequences common to hydrological observations","305002","(SADC-HYCOS environmental measurement)",,"013003","Relative humidity",,,"Operational"
1347.00,"05","Meteorological or hydrological sequences common to hydrological observations","305002","(SADC-HYCOS environmental measurement)",,"014051","Direct solar radiation integrated over last hour",,,"Operational"
1348.00,"05","Meteorological or hydrological sequences common to hydrological observations","305002","(SADC-HYCOS environmental measurement)",,"013060","Total accumulated precipitation",,,"Operational"
1349.00,"05","Meteorological or hydrological sequences common to hydrological observations","305002","(SADC-HYCOS environmental measurement)",,"013072","Downstream water level",,,"Operational"
1350.00,"05","Meteorological or hydrological sequences common to hydrological observations","305002","(SADC-HYCOS environmental measurement)",,"013080","Water pH",,,"Operational"
1351.00,"05","Meteorological or hydrological sequences common to hydrological observations","305002","(SADC-HYCOS environmental measurement)",,"013081","Water conductivity",,,"Operational"
1352.00,"05","Meteorological or hydrological sequences common to hydrological observations","305002","(SADC-HYCOS environmental measurement)",,"013082","Water temperature",,,"Operational"
1353.00,"05","Meteorological or hydrological sequences common to hydrological observations","305002","(SADC-HYCOS environmental measurement)",,"013083","Dissolved oxygen",,,"Operational"
1354.00,"05","Meteorological or hydrological sequences common to hydrological observations","305002","(SADC-HYCOS environmental measurement)",,"013084","Turbidity",,,"Operational"
1355.00,"05","Meteorological or hydrological sequences common to hydrological observations","305003","(SADC-HYCOS measurement array definition)",,"301012","Hour, minute","First single measurement minus increment",,"Operational"
1356.00,"05","Meteorological or hydrological sequences common to hydrological observations","305003","(SADC-HYCOS measurement array definition)",,"004065","Short time increment","Time interval between measurements",,"Operational"
1357.00,"05","Meteorological or hydrological sequences common to hydrological observations","305003","(SADC-HYCOS measurement array definition)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
1358.00,"05","Meteorological or hydrological sequences common to hydrological observations","305003","(SADC-HYCOS measurement array definition)",,"031001","Delayed descriptor replication factor",,,"Operational"
1359.00,"05","Meteorological or hydrological sequences common to hydrological observations","305003","(SADC-HYCOS measurement array definition)",,"305001","SADC-HYCOS single measurement",,,"Operational"
1364.00,"05","Meteorological or hydrological sequences common to hydrological observations","305004","(SADC-HYCOS report)",,"301030","Identification - with physical location",,,"Operational"
1365.00,"05","Meteorological or hydrological sequences common to hydrological observations","305004","(SADC-HYCOS report)",,"305002","SADC-HYCOS environmental measurement",,,"Operational"
1366.00,"05","Meteorological or hydrological sequences common to hydrological observations","305004","(SADC-HYCOS report)",,"305003","SADC-HYCOS measurement array definition",,,"Operational"
1367.00,"05","Meteorological or hydrological sequences common to hydrological observations","305006","(MEDHYCOS measurement)",,"013072","Downstream water level",,,"Operational"
1368.00,"05","Meteorological or hydrological sequences common to hydrological observations","305006","(MEDHYCOS measurement)",,"013082","Water temperature",,,"Operational"
1369.00,"05","Meteorological or hydrological sequences common to hydrological observations","305006","(MEDHYCOS measurement)",,"013019","Total precipitation past 1 hour",,,"Operational"
1370.00,"05","Meteorological or hydrological sequences common to hydrological observations","305006","(MEDHYCOS measurement)",,"012001","Temperature/air temperature",,,"Operational"
1371.00,"05","Meteorological or hydrological sequences common to hydrological observations","305006","(MEDHYCOS measurement)",,"013073","Maximum water level",,,"Operational"
1372.00,"05","Meteorological or hydrological sequences common to hydrological observations","305006","(MEDHYCOS measurement)",,"013060","Total accumulated precipitation",,,"Operational"
1381.00,"05","Meteorological or hydrological sequences common to hydrological observations","305007","(MEDHYCOS report)",,"301029","Identification",,,"Operational"
1382.00,"05","Meteorological or hydrological sequences common to hydrological observations","305007","(MEDHYCOS report)",,"301012","Hour, minute","Time of first measurement",,"Operational"
1383.00,"05","Meteorological or hydrological sequences common to hydrological observations","305007","(MEDHYCOS report)",,"004065","Short time increment","Time interval between measurements",,"Operational"
1384.00,"05","Meteorological or hydrological sequences common to hydrological observations","305007","(MEDHYCOS report)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
1385.00,"05","Meteorological or hydrological sequences common to hydrological observations","305007","(MEDHYCOS report)",,"031001","Delayed descriptor replication factor",,,"Operational"
1386.00,"05","Meteorological or hydrological sequences common to hydrological observations","305007","(MEDHYCOS report)",,"305006","MEDHYCOS measurement","Single measurement",,"Operational"
1392.00,"05","Meteorological or hydrological sequences common to hydrological observations","305008","(AOCHYCOS - Chad measurement)",,"305006","MEDHYCOS measurement","Same as MEDHYCOS type measurement",,"Operational"
1393.00,"05","Meteorological or hydrological sequences common to hydrological observations","305008","(AOCHYCOS - Chad measurement)",,"012030","Soil temperature","At -50 cm",,"Operational"
1398.00,"05","Meteorological or hydrological sequences common to hydrological observations","305009","(AOCHYCOS - Chad report)",,"301029","Identification",,,"Operational"
1399.00,"05","Meteorological or hydrological sequences common to hydrological observations","305009","(AOCHYCOS - Chad report)",,"301012","Hour, minute","Time of first measurement",,"Operational"
1400.00,"05","Meteorological or hydrological sequences common to hydrological observations","305009","(AOCHYCOS - Chad report)",,"004065","Short time increment","Time interval between measurements",,"Operational"
1401.00,"05","Meteorological or hydrological sequences common to hydrological observations","305009","(AOCHYCOS - Chad report)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
1402.00,"05","Meteorological or hydrological sequences common to hydrological observations","305009","(AOCHYCOS - Chad report)",,"031001","Delayed descriptor replication factor",,,"Operational"
1403.00,"05","Meteorological or hydrological sequences common to hydrological observations","305009","(AOCHYCOS - Chad report)",,"305008","AOCHYCOS - Chad measurement","Single measurement",,"Operational"
1409.00,"05","Meteorological or hydrological sequences common to hydrological observations","305010","(MEDHYCOS - Measurement type 2)",,"305008","AOCHYCOS - Chad measurement","Same as AOCHYCOS type measurement",,"Operational"
1410.00,"05","Meteorological or hydrological sequences common to hydrological observations","305010","(MEDHYCOS - Measurement type 2)",,"002091","Entry sensor 4/20 mA","No. 1",,"Operational"
1411.00,"05","Meteorological or hydrological sequences common to hydrological observations","305010","(MEDHYCOS - Measurement type 2)",,"002091","Entry sensor 4/20 mA","No. 2",,"Operational"
1412.00,"05","Meteorological or hydrological sequences common to hydrological observations","305011","(MEDHYCOS report type 2)",,"301029","Identification",,,"Operational"
1413.00,"05","Meteorological or hydrological sequences common to hydrological observations","305011","(MEDHYCOS report type 2)",,"301012","Hour, minute","Time of first measurement",,"Operational"
1414.00,"05","Meteorological or hydrological sequences common to hydrological observations","305011","(MEDHYCOS report type 2)",,"004065","Short time increment","Time interval between measurements",,"Operational"
1415.00,"05","Meteorological or hydrological sequences common to hydrological observations","305011","(MEDHYCOS report type 2)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
1416.00,"05","Meteorological or hydrological sequences common to hydrological observations","305011","(MEDHYCOS report type 2)",,"031001","Delayed descriptor replication factor",,,"Operational"
1417.00,"05","Meteorological or hydrological sequences common to hydrological observations","305011","(MEDHYCOS report type 2)",,"305010","MEDHYCOS - Measurement type 2","Single measurement",,"Operational"
1423.00,"05","Meteorological or hydrological sequences common to hydrological observations","305016","(Meteorological parameters associated with hydrological data)",,"014021","Global solar radiation, integrated over period specified",,,"Operational"
1424.00,"05","Meteorological or hydrological sequences common to hydrological observations","305016","(Meteorological parameters associated with hydrological data)",,"007004","Pressure","Atmospheric pressure",,"Operational"
1425.00,"05","Meteorological or hydrological sequences common to hydrological observations","305016","(Meteorological parameters associated with hydrological data)",,"013003","Relative humidity",,,"Operational"
1426.00,"05","Meteorological or hydrological sequences common to hydrological observations","305016","(Meteorological parameters associated with hydrological data)",,"011002","Wind speed",,,"Operational"
1427.00,"05","Meteorological or hydrological sequences common to hydrological observations","305016","(Meteorological parameters associated with hydrological data)",,"011001","Wind direction",,,"Operational"
1428.00,"05","Meteorological or hydrological sequences common to hydrological observations","305016","(Meteorological parameters associated with hydrological data)",,"011041","Maximum wind gust speed",,,"Operational"
1429.00,"05","Meteorological or hydrological sequences common to hydrological observations","305016","(Meteorological parameters associated with hydrological data)",,"011043","Maximum wind gust direction",,,"Operational"
1430.00,"05","Meteorological or hydrological sequences common to hydrological observations","305017","(Water quality measurement)",,"013080","Water pH",,,"Operational"
1431.00,"05","Meteorological or hydrological sequences common to hydrological observations","305017","(Water quality measurement)",,"013081","Water conductivity",,,"Operational"
1432.00,"05","Meteorological or hydrological sequences common to hydrological observations","305017","(Water quality measurement)",,"013083","Dissolved oxygen",,,"Operational"
1433.00,"05","Meteorological or hydrological sequences common to hydrological observations","305017","(Water quality measurement)",,"013085","Oxydation Reduction Potential (ORP)",,,"Operational"
1434.00,"05","Meteorological or hydrological sequences common to hydrological observations","305017","(Water quality measurement)",,"013084","Turbidity",,,"Operational"
1435.00,"05","Meteorological or hydrological sequences common to hydrological observations","305018","(MEDHYCOS report with meteorology and water quality data)",,"301029","Identification",,,"Operational"
1436.00,"05","Meteorological or hydrological sequences common to hydrological observations","305018","(MEDHYCOS report with meteorology and water quality data)",,"301012","Hour, minute","Time of first measurement",,"Operational"
1437.00,"05","Meteorological or hydrological sequences common to hydrological observations","305018","(MEDHYCOS report with meteorology and water quality data)",,"004065","Short time increment","Hour increment",,"Operational"
1438.00,"05","Meteorological or hydrological sequences common to hydrological observations","305018","(MEDHYCOS report with meteorology and water quality data)",,"103000","Delayed replication of 3 descriptors",,,"Operational"
1439.00,"05","Meteorological or hydrological sequences common to hydrological observations","305018","(MEDHYCOS report with meteorology and water quality data)",,"031001","Delayed descriptor replication factor",,,"Operational"
1440.00,"05","Meteorological or hydrological sequences common to hydrological observations","305018","(MEDHYCOS report with meteorology and water quality data)",,"305008","AOCHYCOS - Chad measurement","Same as AOCHYCOS type measurement",,"Operational"
1441.00,"05","Meteorological or hydrological sequences common to hydrological observations","305018","(MEDHYCOS report with meteorology and water quality data)",,"305016","Meteorological parameters associated with hydrological data",,,"Operational"
1442.00,"05","Meteorological or hydrological sequences common to hydrological observations","305018","(MEDHYCOS report with meteorology and water quality data)",,"305017","Water quality measurement",,,"Operational"
1450.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306001","(Depth, temperature)",,"002032","Indicator for digitization",,,"Operational"
1451.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306001","(Depth, temperature)",,"102000","Delayed replication of 2 descriptors",,,"Operational"
1452.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306001","(Depth, temperature)",,"031001","Delayed descriptor replication factor",,,"Operational"
1453.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306001","(Depth, temperature)",,"007062","Depth below sea/water surface",,,"Operational"
1454.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306001","(Depth, temperature)",,"022042","Sea/water temperature",,,"Operational"
1459.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306002","(Current)",,"002031","Duration and time of current measurement",,,"Operational"
1460.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306002","(Current)",,"022004","Direction of current",,,"Operational"
1461.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306002","(Current)",,"022031","Speed of current",,,"Operational"
1462.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306003","(Surface wind and temperature)",,"002002","Type of instrumentation for wind measurement",,,"Operational"
1463.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306003","(Surface wind and temperature)",,"011011","Wind direction at 10 m",,,"Operational"
1464.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306003","(Surface wind and temperature)",,"011012","Wind speed at 10 m",,,"Operational"
1465.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306003","(Surface wind and temperature)",,"012004","Air temperature at 2 m",,,"Operational"
1466.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306004","(Depth, temperature, salinity)",,"002032","Indicator for digitization",,,"Operational"
1467.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306004","(Depth, temperature, salinity)",,"002033","Method of salinity/depth measurement",,,"Operational"
1468.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306004","(Depth, temperature, salinity)",,"103000","Delayed replication of 3 descriptors",,,"Operational"
1469.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306004","(Depth, temperature, salinity)",,"031001","Delayed descriptor replication factor",,,"Operational"
1470.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306004","(Depth, temperature, salinity)",,"007062","Depth below sea/water surface",,,"Operational"
1471.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306004","(Depth, temperature, salinity)",,"022043","Sea/water temperature",,,"Operational"
1472.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306004","(Depth, temperature, salinity)",,"022062","Salinity",,,"Operational"
1479.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306005",,,"002031","Duration and time of current measurement",,,"Operational"
1480.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306005",,,"103000","Delayed replication of 3 descriptors",,,"Operational"
1481.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306005",,,"031001","Delayed descriptor replication factor",,,"Operational"
1482.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306005",,,"007062","Depth below sea/water surface",,,"Operational"
1483.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306005",,,"022004","Direction of current",,,"Operational"
1484.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306005",,,"022031","Speed of current",,,"Operational"
1490.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306006","(Under water sounding (optional) parameters)",,"306003","Surface wind and temperature",,,"Operational"
1491.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306006","(Under water sounding (optional) parameters)",,"306002","Current",,,"Operational"
1492.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306006","(Under water sounding (optional) parameters)",,"022063","Total water depth",,,"Operational"
1493.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306007","(Buoy spare block parameters)",,"001012","Direction of motion of moving observing platform",,,"Operational"
1494.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306007","(Buoy spare block parameters)",,"001014","Platform drift speed (high precision)",,,"Operational"
1495.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306007","(Buoy spare block parameters)",,"306008","Buoy instrumentation parameters",,,"Operational"
1496.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306007","(Buoy spare block parameters)",,"004024","Time period or displacement",,,"Operational"
1497.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306007","(Buoy spare block parameters)",,"027003","Alternate latitude (coarse accuracy)",,,"Operational"
1498.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306007","(Buoy spare block parameters)",,"028003","Alternate longitude (coarse accuracy)",,,"Operational"
1499.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306008","(Buoy instrumentation parameters)",,"002034","Drogue type",,,"Operational"
1500.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306008","(Buoy instrumentation parameters)",,"002035","Cable length",,,"Operational"
1501.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306008","(Buoy instrumentation parameters)",,"002036","Buoy type",,,"Operational"
1539.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306019","(Tide report identification, water level checks, time increments)",,"001075","Tide station identification","Alphanumeric",,"Operational"
1540.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306019","(Tide report identification, water level checks, time increments)",,"301011","Year, month, day",,,"Operational"
1541.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306019","(Tide report identification, water level checks, time increments)",,"301012","Hour, minute",,,"Operational"
1542.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306019","(Tide report identification, water level checks, time increments)",,"022042","Sea/water temperature",,,"Operational"
1543.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306019","(Tide report identification, water level checks, time increments)",,"022120","Tide station automated water level check",,,"Operational"
1544.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306019","(Tide report identification, water level checks, time increments)",,"022121","Tide station manual water level check",,,"Operational"
1545.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306019","(Tide report identification, water level checks, time increments)",,"004015","Time increment","Minutes","(see Note 1)","Operational"
1546.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306019","(Tide report identification, water level checks, time increments)",,"004065","Short time increment",,,"Operational"
1556.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306020","(Tide report identification, water level checks, time period or displacement, time increment)",,"001075","Tide station identification","Alphanumeric","<(see Note 2)>","Operational"
1557.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306020","(Tide report identification, water level checks, time period or displacement, time increment)",,"301011","Year, month, day",,,"Operational"
1558.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306020","(Tide report identification, water level checks, time period or displacement, time increment)",,"301012","Hour, minute",,,"Operational"
1559.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306020","(Tide report identification, water level checks, time period or displacement, time increment)",,"022042","Sea/water temperature",,,"Operational"
1560.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306020","(Tide report identification, water level checks, time period or displacement, time increment)",,"022120","Tide station automated water level check",,,"Operational"
1561.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306020","(Tide report identification, water level checks, time period or displacement, time increment)",,"022121","Tide station manual water level check",,,"Operational"
1562.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306020","(Tide report identification, water level checks, time period or displacement, time increment)",,"004075","Short time period or displacement",,,"Operational"
1563.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306020","(Tide report identification, water level checks, time period or displacement, time increment)",,"004065","Short time increment",,,"Operational"
1564.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306021","(Meteorological parameters in tide station)",,"001075","Tide station identification","Alphanumeric",,"Operational"
1565.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306021","(Meteorological parameters in tide station)",,"301011","Year, month, day",,,"Operational"
1566.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306021","(Meteorological parameters in tide station)",,"301012","Hour, minute",,,"Operational"
1567.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306021","(Meteorological parameters in tide station)",,"022122","Tide station automated meteorological data check",,,"Operational"
1568.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306021","(Meteorological parameters in tide station)",,"022123","Tide station manual meteorological data check",,,"Operational"
1569.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306021","(Meteorological parameters in tide station)",,"012001","Temperature/air temperature",,,"Operational"
1570.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306021","(Meteorological parameters in tide station)",,"303002","Wind at pressure level",,,"Operational"
1571.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306022","(Tidal elevation)",,"001075","Tide station identification",,,"Operational"
1572.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306022","(Tidal elevation)",,"301011","Year, month, day",,,"Operational"
1573.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306022","(Tidal elevation)",,"301012","Hour, minute",,,"Operational"
1574.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306022","(Tidal elevation)",,"022038","Tidal elevation with respect to local chart datum",,,"Operational"
1575.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306022","(Tidal elevation)",,"022039","Meteorological residual tidal elevation (surge or offset)",,,"Operational"
1576.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306023",,,"001015","Station or site name",,,"Operational"
1577.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306023",,,"301023","Latitude/longitude (coarse accuracy)",,,"Operational"
1578.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306023",,,"301011","Year, month, day",,,"Operational"
1579.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306023",,,"301012","Hour, minute",,,"Operational"
1580.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306023",,,"022038","Tidal elevation with respect to local chart datum",,,"Operational"
1581.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306023",,,"022039","Meteorological residual tidal elevation (surge or offset)",,,"Operational"
1582.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306023",,,"022120","Tide station automated water level check",,,"Operational"
1583.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306023",,,"022121","Tide station manual water level check",,,"Operational"
1584.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306024","(Tide elevation series)",,"306020","Tide report identification, water level checks, time period or displacement, time increment",,"<(see Note 3)>","Operational"
1585.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306024","(Tide elevation series)",,"102006","Replicate 2 descriptors 6 times",,,"Operational"
1586.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306024","(Tide elevation series)",,"022038","Tidal elevation with respect to local chart datum",,,"Operational"
1587.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306024","(Tide elevation series)",,"022039","Meteorological residual tidal elevation (surge or offset)",,,"Operational"
1588.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306025","(Tide elevation series)",,"306019","Tide report identification, water level checks, time increments",,,"Operational"
1589.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306025","(Tide elevation series)",,"102006","Replicate 2 descriptors 6 times",,,"Operational"
1590.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306025","(Tide elevation series)",,"022038","Tidal elevation with respect to local chart datum",,,"Operational"
1591.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306025","(Tide elevation series)",,"022039","Meteorological residual tidal elevation (surge or offset)",,,"Operational"
1614.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306027","(Sequence for representation of DART buoy identification, transmitter ID, type of tsunameter and the time the message is transmitted to the ground system)",,"001005","Buoy/platform identifier",,,"Operational"
1615.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306027","(Sequence for representation of DART buoy identification, transmitter ID, type of tsunameter and the time the message is transmitted to the ground system)",,"001052","Platform transmitter ID",,,"Operational"
1616.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306027","(Sequence for representation of DART buoy identification, transmitter ID, type of tsunameter and the time the message is transmitted to the ground system)",,"002047","Deep-ocean tsunameter type",,,"Operational"
1617.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306027","(Sequence for representation of DART buoy identification, transmitter ID, type of tsunameter and the time the message is transmitted to the ground system)",,"301011","Year, month, day","Time the message is transmitted to the ground system",,"Operational"
1618.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306027","(Sequence for representation of DART buoy identification, transmitter ID, type of tsunameter and the time the message is transmitted to the ground system)",,"301013","Hour, minute, second",,,"Operational"
1619.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306028","(Sequence for representation of time of observation and DART buoy position daily report)",,"306027","Sequence for representation of DART buoy identification, transmitter ID, type of tsunameter and the time the message is transmitted to the ground system",,,"Operational"
1620.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306028","(Sequence for representation of time of observation and DART buoy position daily report)",,"301011","Year, month, day","Observation time",,"Operational"
1621.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306028","(Sequence for representation of time of observation and DART buoy position daily report)",,"301013","Hour, minute, second",,,"Operational"
1622.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306028","(Sequence for representation of time of observation and DART buoy position daily report)",,"301021","Latitude/longitude (high accuracy)",,,"Operational"
1623.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306029","(Sequence for representation of tsunameter sampling information for water column heights in the time series report)",,"025170","Sampling interval (time)","Seconds",,"Operational"
1624.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306029","(Sequence for representation of tsunameter sampling information for water column heights in the time series report)",,"025171","Sample averaging period","Seconds",,"Operational"
1625.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306029","(Sequence for representation of tsunameter sampling information for water column heights in the time series report)",,"025172","Number of samples",,,"Operational"
1626.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306030","(Sequence for representation of DART buoy standard hourly report)",,"306027","Sequence for representation of DART buoy identification, transmitter ID, type of tsunameter and the time the message is transmitted to the ground system",,,"Operational"
1627.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306030","(Sequence for representation of DART buoy standard hourly report)",,"306029","Sequence for representation of tsunameter sampling information for water column heights in the time series report",,,"Operational"
1628.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306030","(Sequence for representation of DART buoy standard hourly report)",,"111000","Delayed replication of 11 descriptors",,,"Operational"
1629.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306030","(Sequence for representation of DART buoy standard hourly report)",,"031001","Delayed descriptor replication factor",,,"Operational"
1630.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306030","(Sequence for representation of DART buoy standard hourly report)",,"033002","Quality information","Message status",,"Operational"
1631.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306030","(Sequence for representation of DART buoy standard hourly report)",,"301011","Year, month, day","Reference date/time for the time series",,"Operational"
1632.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306030","(Sequence for representation of DART buoy standard hourly report)",,"301013","Hour, minute, second",,,"Operational"
1633.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306030","(Sequence for representation of DART buoy standard hourly report)",,"025025","Battery voltage","BPR CPU",,"Operational"
1634.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306030","(Sequence for representation of DART buoy standard hourly report)",,"025025","Battery voltage","Acoustic modem DSP",,"Operational"
1635.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306030","(Sequence for representation of DART buoy standard hourly report)",,"025026","Battery voltage (large range)","Acoustic modem",,"Operational"
1636.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306030","(Sequence for representation of DART buoy standard hourly report)",,"022185","BPR transmission count",,,"Operational"
1637.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306030","(Sequence for representation of DART buoy standard hourly report)",,"004015","Time increment","Added to reset the reference time",,"Operational"
1638.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306030","(Sequence for representation of DART buoy standard hourly report)",,"004065","Short time increment","Added to each data value in the time series",,"Operational"
1639.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306030","(Sequence for representation of DART buoy standard hourly report)",,"101004","Replicate 1 descriptor 4 times",,,"Operational"
1640.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306030","(Sequence for representation of DART buoy standard hourly report)",,"022182","Water column height",,,"Operational"
1642.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306031","(Sequence for representation of DART buoy tsunami event reports and extended tsunami event reports)",,"306027","Sequence for representation of DART buoy identification, transmitter ID, type of tsunameter and the time the message is transmitted to the ground system",,,"Operational"
1643.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306031","(Sequence for representation of DART buoy tsunami event reports and extended tsunami event reports)",,"306029","Sequence for representation of tsunameter sampling information for water column heights in the time series report",,,"Operational"
1644.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306031","(Sequence for representation of DART buoy tsunami event reports and extended tsunami event reports)",,"001053","Tsunameter report sequence number triggered by a tsunami event",,,"Operational"
1645.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306031","(Sequence for representation of DART buoy tsunami event reports and extended tsunami event reports)",,"033002","Quality information","Message status",,"Operational"
1646.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306031","(Sequence for representation of DART buoy tsunami event reports and extended tsunami event reports)",,"301011","Year, month, day","Time when tsunami is detected",,"Operational"
1647.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306031","(Sequence for representation of DART buoy tsunami event reports and extended tsunami event reports)",,"301013","Hour, minute, second",,,"Operational"
1648.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306031","(Sequence for representation of DART buoy tsunami event reports and extended tsunami event reports)",,"301011","Year, month, day","Reference date/time for the time series",,"Operational"
1649.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306031","(Sequence for representation of DART buoy tsunami event reports and extended tsunami event reports)",,"301013","Hour, minute, second",,,"Operational"
1650.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306031","(Sequence for representation of DART buoy tsunami event reports and extended tsunami event reports)",,"022185","BPR transmission count",,,"Operational"
1651.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306031","(Sequence for representation of DART buoy tsunami event reports and extended tsunami event reports)",,"022182","Water column height","Determination of actual value reported in the time series",,"Operational"
1652.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306031","(Sequence for representation of DART buoy tsunami event reports and extended tsunami event reports)",,"004016","Time increment","Added to reset the reference time",,"Operational"
1653.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306031","(Sequence for representation of DART buoy tsunami event reports and extended tsunami event reports)",,"004066","Short time increment","Added to each data value in the time series",,"Operational"
1654.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306031","(Sequence for representation of DART buoy tsunami event reports and extended tsunami event reports)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
1655.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306031","(Sequence for representation of DART buoy tsunami event reports and extended tsunami event reports)",,"031001","Delayed descriptor replication factor",,,"Operational"
1656.00,"06","Meteorological or oceanographic sequences common to oceanographic observations","306031","(Sequence for representation of DART buoy tsunami event reports and extended tsunami event reports)",,"022184","Water column height deviation from the reference value",,,"Operational"
1667.00,"07","Surface report sequences (land)","307001","(Low altitude station)",,"301031","Identification and type of station, date/time, location (high accuracy), height of station",,,"Operational"
1668.00,"07","Surface report sequences (land)","307001","(Low altitude station)",,"302011","Low altitude station","Basic surface report",,"Operational"
1669.00,"07","Surface report sequences (land)","307002","(Low altitude station)",,"301032","Identification and type of station, date/time, location (coarse accuracy), height of station",,,"Operational"
1670.00,"07","Surface report sequences (land)","307002","(Low altitude station)",,"302011","Low altitude station","Basic surface report",,"Operational"
1671.00,"07","Surface report sequences (land)","307003","(Low altitude station)",,"307001","Low altitude station","Location (high accuracy) and basic report",,"Operational"
1672.00,"07","Surface report sequences (land)","307003","(Low altitude station)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
1673.00,"07","Surface report sequences (land)","307003","(Low altitude station)",,"031001","Delayed descriptor replication factor",,,"Operational"
1674.00,"07","Surface report sequences (land)","307003","(Low altitude station)",,"302005","Cloud layer",,,"Operational"
1678.00,"07","Surface report sequences (land)","307004","(Low altitude station)",,"307002","Low altitude station","Location (coarse accuracy) and basic report",,"Operational"
1679.00,"07","Surface report sequences (land)","307004","(Low altitude station)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
1680.00,"07","Surface report sequences (land)","307004","(Low altitude station)",,"031001","Delayed descriptor replication factor",,,"Operational"
1681.00,"07","Surface report sequences (land)","307004","(Low altitude station)",,"302005","Cloud layer",,,"Operational"
1685.00,"07","Surface report sequences (land)","307005","(Low altitude station)",,"307001","Low altitude station","Location (high accuracy) and basic report",,"Operational"
1686.00,"07","Surface report sequences (land)","307005","(Low altitude station)",,"101004","Replicate 1 descriptor 4 times",,,"Operational"
1687.00,"07","Surface report sequences (land)","307005","(Low altitude station)",,"302005","Cloud layer","4 layers",,"Operational"
1688.00,"07","Surface report sequences (land)","307006","(Low altitude station)",,"307002","Low altitude station","Location (coarse accuracy) and basic report",,"Operational"
1689.00,"07","Surface report sequences (land)","307006","(Low altitude station)",,"101004","Replicate 1 descriptor 4 times",,,"Operational"
1690.00,"07","Surface report sequences (land)","307006","(Low altitude station)",,"302005","Cloud layer","4 layers",,"Operational"
1691.00,"07","Surface report sequences (land)","307007","(High altitude station)",,"301031","Identification and type of station, date/time, location (high accuracy), height of station",,,"Operational"
1692.00,"07","Surface report sequences (land)","307007","(High altitude station)",,"302012","High altitude station","Basic surface report",,"Operational"
1693.00,"07","Surface report sequences (land)","307008","(High altitude station)",,"301032","Identification and type of station, date/time, location (coarse accuracy), height of station",,,"Operational"
1694.00,"07","Surface report sequences (land)","307008","(High altitude station)",,"302012","High altitude station","Basic surface report",,"Operational"
1695.00,"07","Surface report sequences (land)","307009",,,"301031","Identification and type of station, date/time, location (high accuracy), height of station",,,"Operational"
1696.00,"07","Surface report sequences (land)","307009",,,"302013","Basic surface report",,,"Operational"
1697.00,"07","Surface report sequences (land)","307011","(Main part of data for representation of METAR/SPECI code in BUFR)",,"001063","ICAO location indicator",,,"Operational"
1698.00,"07","Surface report sequences (land)","307011","(Main part of data for representation of METAR/SPECI code in BUFR)",,"002001","Type of station",,,"Operational"
1699.00,"07","Surface report sequences (land)","307011","(Main part of data for representation of METAR/SPECI code in BUFR)",,"301011","Year, month, day","YY",,"Operational"
1700.00,"07","Surface report sequences (land)","307011","(Main part of data for representation of METAR/SPECI code in BUFR)",,"301012","Hour, minute","GG, gg",,"Operational"
1701.00,"07","Surface report sequences (land)","307011","(Main part of data for representation of METAR/SPECI code in BUFR)",,"301024","Latitude/longitude (coarse accuracy), height of station",,,"Operational"
1702.00,"07","Surface report sequences (land)","307011","(Main part of data for representation of METAR/SPECI code in BUFR)",,"007006","Height above station","Height of an anemometer",,"Operational"
1703.00,"07","Surface report sequences (land)","307011","(Main part of data for representation of METAR/SPECI code in BUFR)",,"011001","Wind direction",,,"Operational"
1704.00,"07","Surface report sequences (land)","307011","(Main part of data for representation of METAR/SPECI code in BUFR)",,"011016","Extreme counterclockwise wind direction of a variable wind",,,"Operational"
1705.00,"07","Surface report sequences (land)","307011","(Main part of data for representation of METAR/SPECI code in BUFR)",,"011017","Extreme clockwise wind direction of a variable wind",,,"Operational"
1706.00,"07","Surface report sequences (land)","307011","(Main part of data for representation of METAR/SPECI code in BUFR)",,"011002","Wind speed",,,"Operational"
1707.00,"07","Surface report sequences (land)","307011","(Main part of data for representation of METAR/SPECI code in BUFR)",,"011041","Maximum wind gust speed",,,"Operational"
1708.00,"07","Surface report sequences (land)","307011","(Main part of data for representation of METAR/SPECI code in BUFR)",,"007006","Height above station","Height of a thermometer",,"Operational"
1709.00,"07","Surface report sequences (land)","307011","(Main part of data for representation of METAR/SPECI code in BUFR)",,"012001","Temperature/air temperature",,,"Operational"
1710.00,"07","Surface report sequences (land)","307011","(Main part of data for representation of METAR/SPECI code in BUFR)",,"012003","Dewpoint temperature",,,"Operational"
1711.00,"07","Surface report sequences (land)","307011","(Main part of data for representation of METAR/SPECI code in BUFR)",,"010052","Altimeter setting (QNH)",,,"Operational"
1712.00,"07","Surface report sequences (land)","307011","(Main part of data for representation of METAR/SPECI code in BUFR)",,"020009","General weather indicator (TAF/METAR)",,,"Operational"
1713.00,"07","Surface report sequences (land)","307012","(Horizontal visibility)",,"103000","Delayed replication of 3 descriptors",,,"Operational"
1714.00,"07","Surface report sequences (land)","307012","(Horizontal visibility)",,"031001","Delayed descriptor replication factor","Up to 3",,"Operational"
1715.00,"07","Surface report sequences (land)","307012","(Horizontal visibility)",,"008023","First-order statistics",,,"Operational"
1716.00,"07","Surface report sequences (land)","307012","(Horizontal visibility)",,"005021","Bearing or azimuth","Direction of visibility observed",,"Operational"
1717.00,"07","Surface report sequences (land)","307012","(Horizontal visibility)",,"020001","Horizontal visibility",,,"Operational"
1722.00,"07","Surface report sequences (land)","307013","(Runway visual range)",,"106000","Delayed replication of 6 descriptors",,,"Operational"
1723.00,"07","Surface report sequences (land)","307013","(Runway visual range)",,"031001","Delayed descriptor replication factor","Up to 4",,"Operational"
1724.00,"07","Surface report sequences (land)","307013","(Runway visual range)",,"001064","Runway designator",,,"Operational"
1725.00,"07","Surface report sequences (land)","307013","(Runway visual range)",,"008014","Qualifier for runway visual range",,,"Operational"
1726.00,"07","Surface report sequences (land)","307013","(Runway visual range)",,"020061","Runway visual range (RVR)",,,"Operational"
1727.00,"07","Surface report sequences (land)","307013","(Runway visual range)",,"008014","Qualifier for runway visual range",,,"Operational"
1728.00,"07","Surface report sequences (land)","307013","(Runway visual range)",,"020061","Runway visual range (RVR)",,,"Operational"
1729.00,"07","Surface report sequences (land)","307013","(Runway visual range)",,"020018","Tendency of runway visual range",,,"Operational"
1737.00,"07","Surface report sequences (land)","307014","(Significant present or forecast weather)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
1738.00,"07","Surface report sequences (land)","307014","(Significant present or forecast weather)",,"031001","Delayed descriptor replication factor","Up to 3",,"Operational"
1739.00,"07","Surface report sequences (land)","307014","(Significant present or forecast weather)",,"020019","Significant present or forecast weather",,,"Operational"
1742.00,"07","Surface report sequences (land)","307015","(Clouds group(s))",,"101000","Delayed replication of 1 descriptor",,,"Operational"
1743.00,"07","Surface report sequences (land)","307015","(Clouds group(s))",,"031001","Delayed descriptor replication factor",,,"Operational"
1744.00,"07","Surface report sequences (land)","307015","(Clouds group(s))",,"302005","Cloud layer","NsNsNs, CC, hshshs",,"Operational"
1745.00,"07","Surface report sequences (land)","307015","(Clouds group(s))",,"020002","Vertical visibility",,,"Operational"
1749.00,"07","Surface report sequences (land)","307016","(Significant recent weather phenomena)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
1750.00,"07","Surface report sequences (land)","307016","(Significant recent weather phenomena)",,"031001","Delayed descriptor replication factor","Up to 3",,"Operational"
1751.00,"07","Surface report sequences (land)","307016","(Significant recent weather phenomena)",,"020020","Significant recent weather phenomena",,,"Operational"
1754.00,"07","Surface report sequences (land)","307017","(Wind shear on runway(s))",,"101000","Delayed replication of 1 descriptor",,,"Operational"
1755.00,"07","Surface report sequences (land)","307017","(Wind shear on runway(s))",,"031001","Delayed descriptor replication factor",,,"Operational"
1756.00,"07","Surface report sequences (land)","307017","(Wind shear on runway(s))",,"011070","Designator of the runway affected by wind shear (including ALL)",,,"Operational"
1759.00,"07","Surface report sequences (land)","307018","(Trend-type landing forecast)",,"008016","Change qualifier of a trend-type forecast or an aerodrome forecast",,,"Operational"
1760.00,"07","Surface report sequences (land)","307018","(Trend-type landing forecast)",,"102000","Delayed replication of 2 descriptors",,,"Operational"
1761.00,"07","Surface report sequences (land)","307018","(Trend-type landing forecast)",,"031001","Delayed descriptor replication factor","Up to 2",,"Operational"
1762.00,"07","Surface report sequences (land)","307018","(Trend-type landing forecast)",,"008017","Qualifier of the time when the forecast change is expected","FM, TL, AT",,"Operational"
1763.00,"07","Surface report sequences (land)","307018","(Trend-type landing forecast)",,"301012","Hour, minute","GG, gg",,"Operational"
1764.00,"07","Surface report sequences (land)","307018","(Trend-type landing forecast)",,"104000","Delayed replication of 4 descriptors",,,"Operational"
1765.00,"07","Surface report sequences (land)","307018","(Trend-type landing forecast)",,"031001","Delayed descriptor replication factor","Up to 1",,"Operational"
1766.00,"07","Surface report sequences (land)","307018","(Trend-type landing forecast)",,"007006","Height above station",,,"Operational"
1767.00,"07","Surface report sequences (land)","307018","(Trend-type landing forecast)",,"011001","Wind direction",,,"Operational"
1768.00,"07","Surface report sequences (land)","307018","(Trend-type landing forecast)",,"011002","Wind speed",,,"Operational"
1769.00,"07","Surface report sequences (land)","307018","(Trend-type landing forecast)",,"011041","Maximum wind gust speed",,,"Operational"
1770.00,"07","Surface report sequences (land)","307018","(Trend-type landing forecast)",,"020009","General weather indicator (TAF/METAR)",,,"Operational"
1771.00,"07","Surface report sequences (land)","307018","(Trend-type landing forecast)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
1772.00,"07","Surface report sequences (land)","307018","(Trend-type landing forecast)",,"031001","Delayed descriptor replication factor","Up to 1",,"Operational"
1773.00,"07","Surface report sequences (land)","307018","(Trend-type landing forecast)",,"020001","Horizontal visibility",,,"Operational"
1774.00,"07","Surface report sequences (land)","307018","(Trend-type landing forecast)",,"307014","Significant present or forecast weather","w´w´",,"Operational"
1788.00,"07","Surface report sequences (land)","307020","(Short METAR/SPECI)",,"307011","Main part of data for representation of METAR/SPECI code in BUFR",,,"Operational"
1789.00,"07","Surface report sequences (land)","307020","(Short METAR/SPECI)",,"307014","Significant present or forecast weather","w´w´",,"Operational"
1790.00,"07","Surface report sequences (land)","307020","(Short METAR/SPECI)",,"307016","Significant recent weather phenomena","REw´w´",,"Operational"
1791.00,"07","Surface report sequences (land)","307021","(Total sequence for representation of METAR/SPECI code in BUFR)",,"307011","Main part of data for representation of METAR/SPECI code in BUFR",,,"Operational"
1792.00,"07","Surface report sequences (land)","307021","(Total sequence for representation of METAR/SPECI code in BUFR)",,"307012","Horizontal visibility","DvVVVV",,"Operational"
1793.00,"07","Surface report sequences (land)","307021","(Total sequence for representation of METAR/SPECI code in BUFR)",,"307013","Runway visual range","DRDR/VRVRVRVR",,"Operational"
1794.00,"07","Surface report sequences (land)","307021","(Total sequence for representation of METAR/SPECI code in BUFR)",,"307014","Significant present or forecast weather","w´w´",,"Operational"
1795.00,"07","Surface report sequences (land)","307021","(Total sequence for representation of METAR/SPECI code in BUFR)",,"307015","Clouds group(s)",,,"Operational"
1796.00,"07","Surface report sequences (land)","307021","(Total sequence for representation of METAR/SPECI code in BUFR)",,"307016","Significant recent weather phenomena","REw´w´",,"Operational"
1797.00,"07","Surface report sequences (land)","307021","(Total sequence for representation of METAR/SPECI code in BUFR)",,"307017","Wind shear on runway(s)",,,"Operational"
1798.00,"07","Surface report sequences (land)","307021","(Total sequence for representation of METAR/SPECI code in BUFR)",,"307018","Trend-type landing forecast",,,"Operational"
1799.00,"07","Surface report sequences (land)","307021","(Total sequence for representation of METAR/SPECI code in BUFR)",,"307015","Clouds group(s)",,,"Operational"
1800.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"001015","Station or site name",,,"Operational"
1801.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"301011","Year, month, day",,,"Operational"
1802.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"301012","Hour, minute",,,"Operational"
1803.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"301022","Latitude/longitude (high accuracy), height of station",,,"Operational"
1804.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"008021","Time significance","= 23 Monitoring period",,"Operational"
1805.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"004025","Time period or displacement",,,"Operational"
1806.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"010004","Pressure",,,"Operational"
1807.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"012001","Temperature/air temperature",,,"Operational"
1808.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"013003","Relative humidity",,,"Operational"
1809.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"033038","Quality flags for ground-based GNSS data",,,"Operational"
1810.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"008022","Total number (with respect to accumulation or average)","Number of GNSS satellites used",,"Operational"
1811.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"106025","Replicate 6 descriptors 25 times",,,"Operational"
1812.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"002020","Satellite classification",,,"Operational"
1813.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"001050","Platform transmitter ID number",,,"Operational"
1814.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"005021","Bearing or azimuth",,,"Operational"
1815.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"007021","Elevation",,,"Operational"
1816.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"015031","Atmospheric path delay in satellite signal",,,"Operational"
1817.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"015032","Estimated error in atmospheric path delay",,,"Operational"
1818.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"008060","Sample scanning mode significance","= 5 North/South",,"Operational"
1819.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"015033","Difference in path delays for limb views at extremes of scan",,,"Operational"
1820.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"015034","Estimated error in path delay difference",,,"Operational"
1821.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"008060","Sample scanning mode significance","= 6 East/West",,"Operational"
1822.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"015033","Difference in path delays for limb views at extremes of scan",,,"Operational"
1823.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"015034","Estimated error in path delay difference",,,"Operational"
1824.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"015035","Component of zenith path delay due to water vapour",,,"Operational"
1825.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"201131","Change data width",,,"Operational"
1826.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"202129","Change scale",,,"Operational"
1827.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"013016","Precipitable water",,,"Operational"
1828.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"202000","Change scale","Cancel",,"Operational"
1829.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"201000","Change data width","Cancel",,"Operational"
1830.00,"07","Surface report sequences (land)","307022","(Ground-based GNSS data)",,"015011","Log10 of integrated electron density",,,"Operational"
1832.00,"07","Surface report sequences (land)","307030","(Ozone data - single observation)",,"015001","Total ozone",,,"Operational"
1833.00,"07","Surface report sequences (land)","307030","(Ozone data - single observation)",,"015002","Air mass (slant path at 22 km)",,,"Operational"
1834.00,"07","Surface report sequences (land)","307031","(Ozone data - averaged observations)",,"008022","Total number (with respect to accumulation or average)","Number of measurements",,"Operational"
1835.00,"07","Surface report sequences (land)","307031","(Ozone data - averaged observations)",,"008023","First-order statistics","= 4 Mean value",,"Operational"
1836.00,"07","Surface report sequences (land)","307031","(Ozone data - averaged observations)",,"015001","Total ozone","Average value of ozone measurement",,"Operational"
1837.00,"07","Surface report sequences (land)","307031","(Ozone data - averaged observations)",,"008023","First-order statistics","= 9 Best estimate of standard deviation",,"Operational"
1838.00,"07","Surface report sequences (land)","307031","(Ozone data - averaged observations)",,"015001","Total ozone","Best estimate of standard deviation of the ozone measurement",,"Operational"
1839.00,"07","Surface report sequences (land)","307031","(Ozone data - averaged observations)",,"008023","First-order statistics","= 11 Harmonic mean",,"Operational"
1840.00,"07","Surface report sequences (land)","307031","(Ozone data - averaged observations)",,"015002","Air mass (slant path at 22 km)","Harmonic mean value of the air-mass",,"Operational"
1841.00,"07","Surface report sequences (land)","307041","(Total ozone measurement from a Brewer ground-based spectrophotometer obtained from a single observation)",,"301001","WMO block and station numbers",,,"Operational"
1842.00,"07","Surface report sequences (land)","307041","(Total ozone measurement from a Brewer ground-based spectrophotometer obtained from a single observation)",,"001015","Station or site name",,,"Operational"
1843.00,"07","Surface report sequences (land)","307041","(Total ozone measurement from a Brewer ground-based spectrophotometer obtained from a single observation)",,"301024","Latitude/longitude (coarse accuracy), height of station",,,"Operational"
1844.00,"07","Surface report sequences (land)","307041","(Total ozone measurement from a Brewer ground-based spectrophotometer obtained from a single observation)",,"301011","Year, month, day","Ozone measurement",,"Operational"
1845.00,"07","Surface report sequences (land)","307041","(Total ozone measurement from a Brewer ground-based spectrophotometer obtained from a single observation)",,"301012","Hour, minute","Ozone measurement",,"Operational"
1846.00,"07","Surface report sequences (land)","307041","(Total ozone measurement from a Brewer ground-based spectrophotometer obtained from a single observation)",,"301070","Ozone instrumentation - Brewer spectrophotometer",,,"Operational"
1847.00,"07","Surface report sequences (land)","307041","(Total ozone measurement from a Brewer ground-based spectrophotometer obtained from a single observation)",,"307030","Ozone data - single observation",,,"Operational"
1848.00,"07","Surface report sequences (land)","307042","(Total ozone measurement from a Brewer ground-based spectrophotometer obtained from averaged observations)",,"301001","WMO block and station numbers",,,"Operational"
1849.00,"07","Surface report sequences (land)","307042","(Total ozone measurement from a Brewer ground-based spectrophotometer obtained from averaged observations)",,"001015","Station or site name",,,"Operational"
1850.00,"07","Surface report sequences (land)","307042","(Total ozone measurement from a Brewer ground-based spectrophotometer obtained from averaged observations)",,"301024","Latitude/longitude (coarse accuracy), height of station",,,"Operational"
1851.00,"07","Surface report sequences (land)","307042","(Total ozone measurement from a Brewer ground-based spectrophotometer obtained from averaged observations)",,"301011","Year, month, day","Ozone measurement",,"Operational"
1852.00,"07","Surface report sequences (land)","307042","(Total ozone measurement from a Brewer ground-based spectrophotometer obtained from averaged observations)",,"301012","Hour, minute","Ozone measurement",,"Operational"
1853.00,"07","Surface report sequences (land)","307042","(Total ozone measurement from a Brewer ground-based spectrophotometer obtained from averaged observations)",,"008021","Time significance","= 8 Ensemble mean",,"Operational"
1854.00,"07","Surface report sequences (land)","307042","(Total ozone measurement from a Brewer ground-based spectrophotometer obtained from averaged observations)",,"004025","Time period or displacement","Time period (minutes) for the computation of the average",,"Operational"
1855.00,"07","Surface report sequences (land)","307042","(Total ozone measurement from a Brewer ground-based spectrophotometer obtained from averaged observations)",,"301070","Ozone instrumentation - Brewer spectrophotometer",,,"Operational"
1856.00,"07","Surface report sequences (land)","307042","(Total ozone measurement from a Brewer ground-based spectrophotometer obtained from averaged observations)",,"307031","Ozone data - averaged observations",,,"Operational"
1857.00,"07","Surface report sequences (land)","307043","(Total ozone measurement from a Dobson ground-based spectrophotometer obtained from a single observation)",,"301001","WMO block and station numbers",,,"Operational"
1858.00,"07","Surface report sequences (land)","307043","(Total ozone measurement from a Dobson ground-based spectrophotometer obtained from a single observation)",,"001015","Station or site name",,,"Operational"
1859.00,"07","Surface report sequences (land)","307043","(Total ozone measurement from a Dobson ground-based spectrophotometer obtained from a single observation)",,"301024","Latitude/longitude (coarse accuracy), height of station",,,"Operational"
1860.00,"07","Surface report sequences (land)","307043","(Total ozone measurement from a Dobson ground-based spectrophotometer obtained from a single observation)",,"301011","Year, month, day","Ozone measurement",,"Operational"
1861.00,"07","Surface report sequences (land)","307043","(Total ozone measurement from a Dobson ground-based spectrophotometer obtained from a single observation)",,"301012","Hour, minute","Ozone measurement",,"Operational"
1862.00,"07","Surface report sequences (land)","307043","(Total ozone measurement from a Dobson ground-based spectrophotometer obtained from a single observation)",,"301074","Ozone instrumentation - Dobson spectrophotometer",,,"Operational"
1863.00,"07","Surface report sequences (land)","307043","(Total ozone measurement from a Dobson ground-based spectrophotometer obtained from a single observation)",,"307030","Ozone data - single observation",,,"Operational"
1864.00,"07","Surface report sequences (land)","307044","(Total ozone measurement from a Dobson ground-based spectrophotometer obtained from averaged observations)",,"301001","WMO block and station numbers",,,"Operational"
1865.00,"07","Surface report sequences (land)","307044","(Total ozone measurement from a Dobson ground-based spectrophotometer obtained from averaged observations)",,"001015","Station or site name",,,"Operational"
1866.00,"07","Surface report sequences (land)","307044","(Total ozone measurement from a Dobson ground-based spectrophotometer obtained from averaged observations)",,"301024","Latitude/longitude (coarse accuracy), height of station",,,"Operational"
1867.00,"07","Surface report sequences (land)","307044","(Total ozone measurement from a Dobson ground-based spectrophotometer obtained from averaged observations)",,"301011","Year, month, day","Ozone measurement",,"Operational"
1868.00,"07","Surface report sequences (land)","307044","(Total ozone measurement from a Dobson ground-based spectrophotometer obtained from averaged observations)",,"301012","Hour, minute","Ozone measurement",,"Operational"
1869.00,"07","Surface report sequences (land)","307044","(Total ozone measurement from a Dobson ground-based spectrophotometer obtained from averaged observations)",,"008021","Time significance","= 8 Ensemble mean",,"Operational"
1870.00,"07","Surface report sequences (land)","307044","(Total ozone measurement from a Dobson ground-based spectrophotometer obtained from averaged observations)",,"004025","Time period or displacement","Time period (minutes) for the computation of the average",,"Operational"
1871.00,"07","Surface report sequences (land)","307044","(Total ozone measurement from a Dobson ground-based spectrophotometer obtained from averaged observations)",,"301074","Ozone instrumentation - Dobson spectrophotometer",,,"Operational"
1872.00,"07","Surface report sequences (land)","307044","(Total ozone measurement from a Dobson ground-based spectrophotometer obtained from averaged observations)",,"307031","Ozone data - averaged observations",,,"Operational"
1873.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"001063","ICAO location indicator","CCCC",,"Operational"
1874.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"008079","Product status","METAR SPECI COR",,"Operational"
1875.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"002001","Type of station","AUTO",,"Operational"
1876.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"301011","Year, month, day","YY",,"Operational"
1877.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"301012","Hour, minute","GGgg",,"Operational"
1878.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"301023","Latitude/longitude (coarse accuracy)",,,"Operational"
1879.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"007030","Height of station ground above mean sea level",,,"Operational"
1880.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"007031","Height of barometer above mean sea level",,,"Operational"
1881.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"007032","Height of sensor above local ground (or deck of marine platform)","= 10 m (if the actual value is not available)",,"Operational"
1882.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"011001","Wind direction","ddd",,"Operational"
1883.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"011016","Extreme counterclockwise wind direction of a variable wind","dndndn",,"Operational"
1884.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"011017","Extreme clockwise wind direction of a variable wind","dxdxdx",,"Operational"
1885.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"008054","Qualifier for wind speed or wind gusts","P",,"Operational"
1886.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"011083","Wind speed","ff - km/h","(see Note 5)","Operational"
1887.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"011084","Wind speed","ff - kt","(see Note 5)","Operational"
1888.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"011002","Wind speed","ff - m/s","(see Note 5)","Operational"
1889.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"008054","Qualifier for wind speed or wind gusts","P",,"Operational"
1890.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"011085","Maximum wind gust speed","fmfm - km/h","(see Note 6)","Operational"
1891.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"011086","Maximum wind gust speed","fmfm - kt","(see Note 6)","Operational"
1892.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"011041","Maximum wind gust speed","fmfm - m/s","(see Note 6)","Operational"
1893.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"008054","Qualifier for wind speed or wind gusts","Set to missing (cancel)",,"Operational"
1894.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"007032","Height of sensor above local ground (or deck of marine platform)","= 2 m (if the actual value is not available)",,"Operational"
1895.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"012023","Temperature","TT - Celsius",,"Operational"
1896.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"012024","Dewpoint temperature","TdTd - Celsius",,"Operational"
1897.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"007032","Height of sensor above local ground (or deck of marine platform)","Set to missing (cancel)",,"Operational"
1898.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"010052","Altimeter setting (QNH)","QPHPHPHPH",,"Operational"
1899.00,"07","Surface report sequences (land)","307045","(Main part of METAR/SPECI), replacing 3 07 011",,"020009","General weather indicator (TAF/METAR)","CAVOK",,"Operational"
1900.00,"07","Surface report sequences (land)","307046","(METAR/SPECI visibility)",,"020060","Prevailing horizontal visibility","VVVV or VVVVNDV",,"Operational"
1901.00,"07","Surface report sequences (land)","307046","(METAR/SPECI visibility)",,"102000","Delayed replication of 2 descriptors",,,"Operational"
1902.00,"07","Surface report sequences (land)","307046","(METAR/SPECI visibility)",,"031001","Delayed descriptor replication factor","Up to 2",,"Operational"
1903.00,"07","Surface report sequences (land)","307046","(METAR/SPECI visibility)",,"005021","Bearing or azimuth","Direction of minimum visibility observed Dv",,"Operational"
1904.00,"07","Surface report sequences (land)","307046","(METAR/SPECI visibility)",,"020059","Minimum horizontal visibility","VNVNVNVN",,"Operational"
1906.00,"07","Surface report sequences (land)","307047","(METAR/SPECI/TAF clouds), replacing 3 07 015",,"105000","Delayed replication of 5 descriptors",,,"Operational"
1907.00,"07","Surface report sequences (land)","307047","(METAR/SPECI/TAF clouds), replacing 3 07 015",,"031001","Delayed descriptor replication factor",,,"Operational"
1908.00,"07","Surface report sequences (land)","307047","(METAR/SPECI/TAF clouds), replacing 3 07 015",,"008002","Vertical significance (surface observations)",,,"Operational"
1909.00,"07","Surface report sequences (land)","307047","(METAR/SPECI/TAF clouds), replacing 3 07 015",,"020011","Cloud amount","NsNsNs",,"Operational"
1910.00,"07","Surface report sequences (land)","307047","(METAR/SPECI/TAF clouds), replacing 3 07 015",,"020012","Cloud type","CC",,"Operational"
1911.00,"07","Surface report sequences (land)","307047","(METAR/SPECI/TAF clouds), replacing 3 07 015",,"020013","Height of base of cloud","hshshs - m",,"Operational"
1912.00,"07","Surface report sequences (land)","307047","(METAR/SPECI/TAF clouds), replacing 3 07 015",,"020092","Height of base of cloud","hshshs - ft",,"Operational"
1913.00,"07","Surface report sequences (land)","307047","(METAR/SPECI/TAF clouds), replacing 3 07 015",,"020002","Vertical visibility","VVhshshs - m",,"Operational"
1914.00,"07","Surface report sequences (land)","307047","(METAR/SPECI/TAF clouds), replacing 3 07 015",,"020091","Vertical visibility","VVhshshs - ft",,"Operational"
1916.00,"07","Surface report sequences (land)","307048","(Trend type forecast), replacing 3 07 018",,"008016","Change qualifier of a trend-type forecast or an aerodrome forecast","TTTTT NOSIG",,"Operational"
1917.00,"07","Surface report sequences (land)","307048","(Trend type forecast), replacing 3 07 018",,"102000","Delayed replication of 2 descriptors",,,"Operational"
1918.00,"07","Surface report sequences (land)","307048","(Trend type forecast), replacing 3 07 018",,"031001","Delayed descriptor replication factor","= 0, 1 or 2",,"Operational"
1919.00,"07","Surface report sequences (land)","307048","(Trend type forecast), replacing 3 07 018",,"008017","Qualifier of the time when the forecast change is expected","TT",,"Operational"
1920.00,"07","Surface report sequences (land)","307048","(Trend type forecast), replacing 3 07 018",,"301012","Hour, minute","GGgg",,"Operational"
1921.00,"07","Surface report sequences (land)","307048","(Trend type forecast), replacing 3 07 018",,"112000","Delayed replication of 12 descriptors",,,"Operational"
1922.00,"07","Surface report sequences (land)","307048","(Trend type forecast), replacing 3 07 018",,"031000","Short delayed descriptor replication factor","= 0 or 1",,"Operational"
1923.00,"07","Surface report sequences (land)","307048","(Trend type forecast), replacing 3 07 018",,"007032","Height of sensor above local ground (or deck of marine platform)","= 10 m (if the actual value is not available)",,"Operational"
1924.00,"07","Surface report sequences (land)","307048","(Trend type forecast), replacing 3 07 018",,"011001","Wind direction","ddd",,"Operational"
1925.00,"07","Surface report sequences (land)","307048","(Trend type forecast), replacing 3 07 018",,"008054","Qualifier for wind speed or wind gusts","P",,"Operational"
1926.00,"07","Surface report sequences (land)","307048","(Trend type forecast), replacing 3 07 018",,"011083","Wind speed","ff - km/h","(see Note 5)","Operational"
1927.00,"07","Surface report sequences (land)","307048","(Trend type forecast), replacing 3 07 018",,"011084","Wind speed","ff - kt","(see Note 5)","Operational"
1928.00,"07","Surface report sequences (land)","307048","(Trend type forecast), replacing 3 07 018",,"011002","Wind speed","ff - m/s","(see Note 5)","Operational"
1929.00,"07","Surface report sequences (land)","307048","(Trend type forecast), replacing 3 07 018",,"008054","Qualifier for wind speed or wind gusts","P",,"Operational"
1930.00,"07","Surface report sequences (land)","307048","(Trend type forecast), replacing 3 07 018",,"011085","Maximum wind gust speed","fmfm - km/h","(see Note 6)","Operational"
1931.00,"07","Surface report sequences (land)","307048","(Trend type forecast), replacing 3 07 018",,"011086","Maximum wind gust speed","fmfm - kt","(see Note 6)","Operational"
1932.00,"07","Surface report sequences (land)","307048","(Trend type forecast), replacing 3 07 018",,"011041","Maximum wind gust speed","fmfm - m/s","(see Note 6)","Operational"
1933.00,"07","Surface report sequences (land)","307048","(Trend type forecast), replacing 3 07 018",,"008054","Qualifier for wind speed or wind gusts","Set to missing (cancel)",,"Operational"
1934.00,"07","Surface report sequences (land)","307048","(Trend type forecast), replacing 3 07 018",,"007032","Height of sensor above local ground (or deck of marine platform)","Set to missing (cancel)",,"Operational"
1935.00,"07","Surface report sequences (land)","307048","(Trend type forecast), replacing 3 07 018",,"020009","General weather indicator (TAF/METAR)","CAVOK NSW NSC",,"Operational"
1936.00,"07","Surface report sequences (land)","307048","(Trend type forecast), replacing 3 07 018",,"101000","Delayed replication of 1 descriptor",,,"Operational"
1937.00,"07","Surface report sequences (land)","307048","(Trend type forecast), replacing 3 07 018",,"031000","Short delayed descriptor replication factor","= 0 or 1",,"Operational"
1938.00,"07","Surface report sequences (land)","307048","(Trend type forecast), replacing 3 07 018",,"020060","Prevailing horizontal visibility","VVVV",,"Operational"
1939.00,"07","Surface report sequences (land)","307048","(Trend type forecast), replacing 3 07 018",,"307014","Significant present and forecast weather","Weather intensity and phenomena w´w´",,"Operational"
1940.00,"07","Surface report sequences (land)","307048","(Trend type forecast), replacing 3 07 018",,"307047","METAR/SPECI/TAF clouds, replacing 3 07 015","NsNsNshshshs",,"Operational"
1942.00,"07","Surface report sequences (land)","307049","(Sea conditions)",,"102000","Delayed replication of 2 descriptors",,,"Operational"
1943.00,"07","Surface report sequences (land)","307049","(Sea conditions)",,"031000","Short delayed descriptor replication factor","= 0 or 1",,"Operational"
1944.00,"07","Surface report sequences (land)","307049","(Sea conditions)",,"022043","Sea/water temperature","TsTs",,"Operational"
1945.00,"07","Surface report sequences (land)","307049","(Sea conditions)",,"022021","Height of waves","S´",,"Operational"
1947.00,"07","Surface report sequences (land)","307050","(Runway state)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
1948.00,"07","Surface report sequences (land)","307050","(Runway state)",,"031000","Short delayed descriptor replication factor","= 0 or 1",,"Operational"
1949.00,"07","Surface report sequences (land)","307050","(Runway state)",,"020085","General condition of runway","SNOCLO",,"Operational"
1950.00,"07","Surface report sequences (land)","307050","(Runway state)",,"102000","Delayed replication of 2 descriptors",,,"Operational"
1951.00,"07","Surface report sequences (land)","307050","(Runway state)",,"031001","Delayed descriptor replication factor",,,"Operational"
1952.00,"07","Surface report sequences (land)","307050","(Runway state)",,"001064","Runway designator","DRDR",,"Operational"
1953.00,"07","Surface report sequences (land)","307050","(Runway state)",,"020085","General condition of runway","CLRD//",,"Operational"
1954.00,"07","Surface report sequences (land)","307050","(Runway state)",,"105000","Delayed replication of 5 descriptors",,,"Operational"
1955.00,"07","Surface report sequences (land)","307050","(Runway state)",,"031001","Delayed descriptor replication factor",,,"Operational"
1956.00,"07","Surface report sequences (land)","307050","(Runway state)",,"001064","Runway designator","DRDR",,"Operational"
1957.00,"07","Surface report sequences (land)","307050","(Runway state)",,"020086","Runway deposits","ER",,"Operational"
1958.00,"07","Surface report sequences (land)","307050","(Runway state)",,"020087","Runway contamination","CR",,"Operational"
1959.00,"07","Surface report sequences (land)","307050","(Runway state)",,"020088","Depth of runway deposits","eReR",,"Operational"
1960.00,"07","Surface report sequences (land)","307050","(Runway state)",,"020089","Runway friction coefficient","BRBR",,"Operational"
1962.00,"07","Surface report sequences (land)","307051","(Full METAR/SPECI), replacing 3 07 021",,"307045","Main part of METAR/SPECI, replacing 3 07 011",,,"Operational"
1963.00,"07","Surface report sequences (land)","307051","(Full METAR/SPECI), replacing 3 07 021",,"307046","METAR/SPECI visibility","VVVV or VVVVNDV VNVNVNVNDV",,"Operational"
1964.00,"07","Surface report sequences (land)","307051","(Full METAR/SPECI), replacing 3 07 021",,"307013","Runway visual range","RDRDR/VRVRVRVR",,"Operational"
1965.00,"07","Surface report sequences (land)","307051","(Full METAR/SPECI), replacing 3 07 021",,"307014","Significant present and forecast weather","Weather intensity and phenomena w´w´",,"Operational"
1966.00,"07","Surface report sequences (land)","307051","(Full METAR/SPECI), replacing 3 07 021",,"307047","METAR/SPECI/TAF clouds, replacing 3 07 015","NsNsNshshshs",,"Operational"
1967.00,"07","Surface report sequences (land)","307051","(Full METAR/SPECI), replacing 3 07 021",,"307016","Significant recent weather phenomena","REw´w´",,"Operational"
1968.00,"07","Surface report sequences (land)","307051","(Full METAR/SPECI), replacing 3 07 021",,"307017","Wind shear on runway(s)","WS RDRDR",,"Operational"
1969.00,"07","Surface report sequences (land)","307051","(Full METAR/SPECI), replacing 3 07 021",,"307049","Sea conditions","WTsTs/SS’",,"Operational"
1970.00,"07","Surface report sequences (land)","307051","(Full METAR/SPECI), replacing 3 07 021",,"307050","Runway state","RDRDR/ERCReReRBRBR",,"Operational"
1971.00,"07","Surface report sequences (land)","307051","(Full METAR/SPECI), replacing 3 07 021",,"101000","Delayed replication of 1 descriptor",,,"Operational"
1972.00,"07","Surface report sequences (land)","307051","(Full METAR/SPECI), replacing 3 07 021",,"031001","Delayed descriptor replication factor","= 0 to 3 normally",,"Operational"
1973.00,"07","Surface report sequences (land)","307051","(Full METAR/SPECI), replacing 3 07 021",,"307048","Trend type forecast, replacing 3 07 018",,,"Operational"
1975.00,"07","Surface report sequences (land)","307052","(Aerodrome forecast identification and time interval)",,"001063","ICAO location indicator","CCCC",,"Operational"
1976.00,"07","Surface report sequences (land)","307052","(Aerodrome forecast identification and time interval)",,"008039","Time significance (Aviation forecast)","= 0 Issue time of forecast",,"Operational"
1977.00,"07","Surface report sequences (land)","307052","(Aerodrome forecast identification and time interval)",,"301011","Year, month, day","YY",,"Operational"
1978.00,"07","Surface report sequences (land)","307052","(Aerodrome forecast identification and time interval)",,"301012","Hour, minute","GGgg",,"Operational"
1979.00,"07","Surface report sequences (land)","307052","(Aerodrome forecast identification and time interval)",,"008079","Product status","COR CNL AMD NIL",,"Operational"
1980.00,"07","Surface report sequences (land)","307052","(Aerodrome forecast identification and time interval)",,"008039","Time significance (Aviation forecast)","= 1 Time of commencement of period of the forecast",,"Operational"
1981.00,"07","Surface report sequences (land)","307052","(Aerodrome forecast identification and time interval)",,"301011","Year, month, day","Y1Y1",,"Operational"
1982.00,"07","Surface report sequences (land)","307052","(Aerodrome forecast identification and time interval)",,"301012","Hour, minute","G1G1",,"Operational"
1983.00,"07","Surface report sequences (land)","307052","(Aerodrome forecast identification and time interval)",,"008039","Time significance (Aviation forecast)","= 2 Time of ending of period of the forecast",,"Operational"
1984.00,"07","Surface report sequences (land)","307052","(Aerodrome forecast identification and time interval)",,"301011","Year, month, day","Y2Y2",,"Operational"
1985.00,"07","Surface report sequences (land)","307052","(Aerodrome forecast identification and time interval)",,"301012","Hour, minute","G2G2",,"Operational"
1986.00,"07","Surface report sequences (land)","307052","(Aerodrome forecast identification and time interval)",,"301023","Latitude/longitude (coarse accuracy)",,,"Operational"
1987.00,"07","Surface report sequences (land)","307052","(Aerodrome forecast identification and time interval)",,"007030","Height of station ground above mean sea level",,,"Operational"
1988.00,"07","Surface report sequences (land)","307052","(Aerodrome forecast identification and time interval)",,"007031","Height of barometer above mean sea level",,,"Operational"
1989.00,"07","Surface report sequences (land)","307053","(Forecast weather at an aerodrome)",,"007032","Height of sensor above local ground (or deck of marine platform)","= 10 m (if the actual value is not available)",,"Operational"
1990.00,"07","Surface report sequences (land)","307053","(Forecast weather at an aerodrome)",,"011001","Wind direction","ddd",,"Operational"
1991.00,"07","Surface report sequences (land)","307053","(Forecast weather at an aerodrome)",,"008054","Qualifier for wind speed or wind gusts","P",,"Operational"
1992.00,"07","Surface report sequences (land)","307053","(Forecast weather at an aerodrome)",,"011083","Wind speed","ff - km/h","(see Note 5)","Operational"
1993.00,"07","Surface report sequences (land)","307053","(Forecast weather at an aerodrome)",,"011084","Wind speed","ff - kt","(see Note 5)","Operational"
1994.00,"07","Surface report sequences (land)","307053","(Forecast weather at an aerodrome)",,"011002","Wind speed","ff - m/s","(see Note 5)","Operational"
1995.00,"07","Surface report sequences (land)","307053","(Forecast weather at an aerodrome)",,"008054","Qualifier for wind speed or wind gusts","P",,"Operational"
1996.00,"07","Surface report sequences (land)","307053","(Forecast weather at an aerodrome)",,"011085","Maximum wind gust speed","fmfm - km/h","(see Note 6)","Operational"
1997.00,"07","Surface report sequences (land)","307053","(Forecast weather at an aerodrome)",,"011086","Maximum wind gust speed","fmfm - kt","(see Note 6)","Operational"
1998.00,"07","Surface report sequences (land)","307053","(Forecast weather at an aerodrome)",,"011041","Maximum wind gust speed","fmfm - m/s","(see Note 6)","Operational"
1999.00,"07","Surface report sequences (land)","307053","(Forecast weather at an aerodrome)",,"008054","Qualifier for wind speed or wind gusts","Set to missing (cancel)",,"Operational"
2000.00,"07","Surface report sequences (land)","307053","(Forecast weather at an aerodrome)",,"007032","Height of sensor above local ground (or deck of marine platform)","Set to missing (cancel)",,"Operational"
2001.00,"07","Surface report sequences (land)","307053","(Forecast weather at an aerodrome)",,"020009","General weather indicator (TAF/METAR)","CAVOK NSW NSC",,"Operational"
2002.00,"07","Surface report sequences (land)","307053","(Forecast weather at an aerodrome)",,"020060","Prevailing horizontal visibility","VVVV",,"Operational"
2003.00,"07","Surface report sequences (land)","307053","(Forecast weather at an aerodrome)",,"307014","Significant present and forecast weather","w´w´",,"Operational"
2004.00,"07","Surface report sequences (land)","307053","(Forecast weather at an aerodrome)",,"307047","METAR/SPECI/TAF clouds, replacing 3 07 015","NsNsNshshshs",,"Operational"
2005.00,"07","Surface report sequences (land)","307054","(Forecast of extreme temperatures)",,"007032","Height of sensor above local ground (or deck of marine platform)","= 2 m (if the actual value is not available)",,"Operational"
2006.00,"07","Surface report sequences (land)","307054","(Forecast of extreme temperatures)",,"008039","Time significance (Aviation forecast)","= 3 Forecast time of maximum temperature",,"Operational"
2007.00,"07","Surface report sequences (land)","307054","(Forecast of extreme temperatures)",,"004003","Day",,,"Operational"
2008.00,"07","Surface report sequences (land)","307054","(Forecast of extreme temperatures)",,"004004","Hour","GFGF",,"Operational"
2009.00,"07","Surface report sequences (land)","307054","(Forecast of extreme temperatures)",,"008023","First-order statistics","= 3 Minimum",,"Operational"
2010.00,"07","Surface report sequences (land)","307054","(Forecast of extreme temperatures)",,"012023","Temperature","TFTF - Celsius",,"Operational"
2011.00,"07","Surface report sequences (land)","307054","(Forecast of extreme temperatures)",,"008039","Time significance (Aviation forecast)","= 4 Forecast time of minimum temperature",,"Operational"
2012.00,"07","Surface report sequences (land)","307054","(Forecast of extreme temperatures)",,"004003","Day",,,"Operational"
2013.00,"07","Surface report sequences (land)","307054","(Forecast of extreme temperatures)",,"004004","Hour","GFGF",,"Operational"
2014.00,"07","Surface report sequences (land)","307054","(Forecast of extreme temperatures)",,"008023","First-order statistics","= 2 Maximum",,"Operational"
2015.00,"07","Surface report sequences (land)","307054","(Forecast of extreme temperatures)",,"012023","Temperature","TFTF - Celsius",,"Operational"
2016.00,"07","Surface report sequences (land)","307054","(Forecast of extreme temperatures)",,"008023","First-order statistics","Set to missing (cancel)",,"Operational"
2017.00,"07","Surface report sequences (land)","307054","(Forecast of extreme temperatures)",,"007032","Height of sensor above local ground (or deck of marine platform)","Set to missing (cancel)",,"Operational"
2018.00,"07","Surface report sequences (land)","307055","(Change indicator and forecast changes)",,"033045","Probability of following event","C2C2",,"Operational"
2019.00,"07","Surface report sequences (land)","307055","(Change indicator and forecast changes)",,"008016","Change qualifier of a trend-type forecast or an aerodrome forecast","TTTTTT",,"Operational"
2020.00,"07","Surface report sequences (land)","307055","(Change indicator and forecast changes)",,"008039","Time significance (Aviation forecast)","= 5 Time of beginning of the forecast change",,"Operational"
2021.00,"07","Surface report sequences (land)","307055","(Change indicator and forecast changes)",,"004003","Day",,,"Operational"
2022.00,"07","Surface report sequences (land)","307055","(Change indicator and forecast changes)",,"301012","Hour, minute","GGgg",,"Operational"
2023.00,"07","Surface report sequences (land)","307055","(Change indicator and forecast changes)",,"008039","Time significance (Aviation forecast)","= 6 Time of ending of the forecast change",,"Operational"
2024.00,"07","Surface report sequences (land)","307055","(Change indicator and forecast changes)",,"004003","Day",,,"Operational"
2025.00,"07","Surface report sequences (land)","307055","(Change indicator and forecast changes)",,"301012","Hour, minute","GeGe",,"Operational"
2026.00,"07","Surface report sequences (land)","307055","(Change indicator and forecast changes)",,"307053","Forecast weather at an aerodrome","During or after change",,"Operational"
2027.00,"07","Surface report sequences (land)","307056","(Aerodrome forecast - full TAF)",,"307052","Aerodrome forecast identification and time interval",,,"Operational"
2028.00,"07","Surface report sequences (land)","307056","(Aerodrome forecast - full TAF)",,"307053","Forecast weather at an aerodrome",,,"Operational"
2029.00,"07","Surface report sequences (land)","307056","(Aerodrome forecast - full TAF)",,"307054","Forecast of extreme temperatures",,,"Operational"
2030.00,"07","Surface report sequences (land)","307056","(Aerodrome forecast - full TAF)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
2031.00,"07","Surface report sequences (land)","307056","(Aerodrome forecast - full TAF)",,"031001","Delayed descriptor replication factor",,,"Operational"
2032.00,"07","Surface report sequences (land)","307056","(Aerodrome forecast - full TAF)",,"307055","Change indicator and forecast changes",,,"Operational"
2034.00,"07","Surface report sequences (land)","307060","(Soil temperature below land surface)",,"007061","Depth below land surface",,,"Operational"
2035.00,"07","Surface report sequences (land)","307060","(Soil temperature below land surface)",,"012030","Soil temperature",,,"Operational"
2036.00,"07","Surface report sequences (land)","307061","(Soil temperature data at number of depths not exceeding five - high accuracy position)",,"301031","Identification and type of station, date/time, location (high accuracy), height of station",,,"Operational"
2037.00,"07","Surface report sequences (land)","307061","(Soil temperature data at number of depths not exceeding five - high accuracy position)",,"101005","Replicate 1 descriptor 5 times",,,"Operational"
2038.00,"07","Surface report sequences (land)","307061","(Soil temperature data at number of depths not exceeding five - high accuracy position)",,"307060","Soil temperature below land surface",,,"Operational"
2039.00,"07","Surface report sequences (land)","307062","(Soil temperature data at number of depths not exceeding five - coarse accuracy position)",,"301032","Identification and type of station, date/time, location (coarse accuracy), height of station",,,"Operational"
2040.00,"07","Surface report sequences (land)","307062","(Soil temperature data at number of depths not exceeding five - coarse accuracy position)",,"101005","Replicate 1 descriptor 5 times",,,"Operational"
2041.00,"07","Surface report sequences (land)","307062","(Soil temperature data at number of depths not exceeding five - coarse accuracy position)",,"307060","Soil temperature below land surface",,,"Operational"
2042.00,"07","Surface report sequences (land)","307063","(Depth below land surface and soil temperature)",,"007061","Depth below land surface",,,"Operational"
2043.00,"07","Surface report sequences (land)","307063","(Depth below land surface and soil temperature)",,"012130","Soil temperature","Scale: 2",,"Operational"
2044.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)",,"301090","Surface station identification; time, horizontal and vertical coordinates",,"(see Note 1)","Operational"
2045.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)",,"004074","Short time period or displacement","= UTC - LST","(see Note 1)","Operational"
2046.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)",,"004023","Time period or displacement","Number of days in the month",,"Operational"
2047.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Monthly mean values of pressure, temperature, extreme temperatures and vapour pressure","008023","First-order statistics","= 4 Mean value",,"Operational"
2048.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Monthly mean values of pressure, temperature, extreme temperatures and vapour pressure","010004","Pressure",,,"Operational"
2049.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Monthly mean values of pressure, temperature, extreme temperatures and vapour pressure","010051","Pressure reduced to mean sea level",,,"Operational"
2050.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Monthly mean values of pressure, temperature, extreme temperatures and vapour pressure","007004","Pressure","Standard level | Set to missing for lowland stations",,"Operational"
2051.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Monthly mean values of pressure, temperature, extreme temperatures and vapour pressure","010009","Geopotential height","Standard level | Set to missing for lowland stations",,"Operational"
2052.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Monthly mean values of pressure, temperature, extreme temperatures and vapour pressure","007032","Height of sensor above local ground (or deck of marine platform)",,"(see Note 3)","Operational"
2053.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Monthly mean values of pressure, temperature, extreme temperatures and vapour pressure","012101","Temperature/air temperature",,,"Operational"
2054.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Monthly mean values of pressure, temperature, extreme temperatures and vapour pressure","002051","Indicator to specify observing method for extreme temperatures",,,"Operational"
2055.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Monthly mean values of pressure, temperature, extreme temperatures and vapour pressure","004051","Principal time of daily reading of maximum temperature",,,"Operational"
2056.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Monthly mean values of pressure, temperature, extreme temperatures and vapour pressure","012118","Maximum temperature at height specified, past 24 hours",,,"Operational"
2057.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Monthly mean values of pressure, temperature, extreme temperatures and vapour pressure","004052","Principal time of daily reading of minimum temperature",,,"Operational"
2058.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Monthly mean values of pressure, temperature, extreme temperatures and vapour pressure","012119","Minimum temperature at height specified, past 24 hours",,,"Operational"
2059.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Monthly mean values of pressure, temperature, extreme temperatures and vapour pressure","013004","Vapour pressure",,,"Operational"
2060.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Monthly mean values of pressure, temperature, extreme temperatures and vapour pressure","008023","First-order statistics","Set to missing",,"Operational"
2061.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Monthly mean values of pressure, temperature, extreme temperatures and vapour pressure","012151","Standard deviation of daily mean temperature",,,"Operational"
2062.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Monthly mean values of pressure, temperature, extreme temperatures and vapour pressure","007032","Height of sensor above local ground (or deck of marine platform)","Set to missing (cancel)",,"Operational"
2063.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Monthly mean values of pressure, temperature, extreme temperatures and vapour pressure","102005","Replicate 2 descriptors 5 times",,,"Operational"
2064.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Monthly mean values of pressure, temperature, extreme temperatures and vapour pressure","008050","Qualifier for number of missing values in calculation of statistic","= 1 Pressure, = 2 Temperature, = 4 Vapour pressure, = 7 Maximum temperature, = 8 Minimum temperature",,"Operational"
2065.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Monthly mean values of pressure, temperature, extreme temperatures and vapour pressure","008020","Total number of missing entities (with respect to accumulation or average)","Days",,"Operational"
2066.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Sunshine duration","014032","Total sunshine",,,"Operational"
2067.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Sunshine duration","014033","Total sunshine",,,"Operational"
2068.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Sunshine duration","008050","Qualifier for number of missing values in calculation of statistic","= 6 Sunshine duration",,"Operational"
2069.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Sunshine duration","008020","Total number of missing entities (with respect to accumulation or average)","Days",,"Operational"
2070.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Number of days of occurrence","102018","Replicate 2 descriptors 18 times",,,"Operational"
2071.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Number of days of occurrence","008052","Condition for which number of days of occurrence follows",,,"Operational"
2072.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Number of days of occurrence","008022","Total number (with respect to accumulation or average)","Days",,"Operational"
2073.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme values of temperature and wind speed","007032","Height of sensor above local ground (or deck of marine platform)",,"(see Note 3)","Operational"
2074.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme values of temperature and wind speed","008053","Day of occurrence qualifier","= 0 On 1 day only, = 1 On 2 or more days",,"Operational"
2075.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme values of temperature and wind speed","004003","Day",,,"Operational"
2076.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme values of temperature and wind speed","012152","Highest daily mean temperature",,,"Operational"
2077.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme values of temperature and wind speed","008053","Day of occurrence qualifier","= 0 On 1 day only, = 1 On 2 or more days",,"Operational"
2078.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme values of temperature and wind speed","004003","Day",,,"Operational"
2079.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme values of temperature and wind speed","012153","Lowest daily mean temperature",,,"Operational"
2080.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme values of temperature and wind speed","008053","Day of occurrence qualifier","= 0 On 1 day only, = 1 On 2 or more days",,"Operational"
2081.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme values of temperature and wind speed","004003","Day",,,"Operational"
2082.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme values of temperature and wind speed","008023","First-order statistics","= 2 Maximum value",,"Operational"
2083.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme values of temperature and wind speed","012101","Temperature/air temperature",,,"Operational"
2084.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme values of temperature and wind speed","008053","Day of occurrence qualifier","= 0 On 1 day only, = 1 On 2 or more days",,"Operational"
2085.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme values of temperature and wind speed","004003","Day",,,"Operational"
2086.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme values of temperature and wind speed","008023","First-order statistics","= 3 Minimum value",,"Operational"
2087.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme values of temperature and wind speed","012101","Temperature/air temperature",,,"Operational"
2088.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme values of temperature and wind speed","008023","First-order statistics","Set to missing",,"Operational"
2089.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme values of temperature and wind speed","007032","Height of sensor above local ground (or deck of marine platform)",,"(see Note 3)","Operational"
2090.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme values of temperature and wind speed","002002","Type of instrumentation for wind measurement",,,"Operational"
2091.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme values of temperature and wind speed","008053","Day of occurrence qualifier","= 0 On 1 day only, = 1 On 2 or more days",,"Operational"
2092.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme values of temperature and wind speed","004003","Day",,,"Operational"
2093.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme values of temperature and wind speed","011046","Maximum instantaneous wind speed",,,"Operational"
2094.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme values of temperature and wind speed","008053","Day of occurrence qualifier","Set to missing (cancel)",,"Operational"
2095.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Precipitation","004003","Day","= 1","(see Note 2)","Operational"
2096.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Precipitation","004004","Hour","= 6","(see Note 2)","Operational"
2097.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Precipitation","004023","Time period or displacement","Number of days in the month","(see Note 2)","Operational"
2098.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Precipitation","007032","Height of sensor above local ground (or deck of marine platform)",,"(see Note 3)","Operational"
2099.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Precipitation","013060","Total accumulated precipitation",,,"Operational"
2100.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Precipitation","013051","Frequency group, precipitation",,,"Operational"
2101.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Precipitation","004053","Number of days with precipitation equal to or more than 1 mm",,,"Operational"
2102.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Precipitation","008050","Qualifier for number of missing values in calculation of statistic","= 5 Precipitation",,"Operational"
2103.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Precipitation","008020","Total number of missing entities (with respect to accumulation or average)","Days",,"Operational"
2104.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Numbers of days of occurrence","102006","Replicate 2 descriptors 6 times",,,"Operational"
2105.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Numbers of days of occurrence","008052","Condition for which number of days of occurrence follows",,,"Operational"
2106.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Numbers of days of occurrence","008022","Total number (with respect to accumulation or average)","Days",,"Operational"
2107.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme precipitation","008053","Day of occurrence qualifier","= 0 On 1 day only, = 1 On 2 or more days",,"Operational"
2108.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme precipitation","004003","Day",,,"Operational"
2109.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme precipitation","013052","Highest daily amount of precipitation",,,"Operational"
2110.00,"07","Surface report sequences (land)","307071","(Monthly values of a land station)","Occurrence of extreme precipitation","007032","Height of sensor above local ground (or deck of marine platform)","Set to missing (cancel)",,"Operational"
2111.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)",,"004001","Year","Beginning of the reference period",,"Operational"
2112.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)",,"004001","Year","Ending of the reference period",,"Operational"
2113.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)",,"004002","Month",,,"Operational"
2114.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)",,"004003","Day","= 1","(see Note 1)","Operational"
2115.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)",,"004004","Hour","= 0","(see Note 1)","Operational"
2116.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)",,"004074","Short time period or displacement","= UTC - LST","(see Note 1)","Operational"
2117.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)",,"004022","Time period or displacement","= 1",,"Operational"
2118.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of monthly mean pressure, temperature, vapour pressure and of standard deviation","008023","First-order statistics","= 4 Mean value",,"Operational"
2119.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of monthly mean pressure, temperature, vapour pressure and of standard deviation","010004","Pressure",,,"Operational"
2120.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of monthly mean pressure, temperature, vapour pressure and of standard deviation","010051","Pressure reduced to mean sea level",,,"Operational"
2121.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of monthly mean pressure, temperature, vapour pressure and of standard deviation","007004","Pressure","Standard level",,"Operational"
2122.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of monthly mean pressure, temperature, vapour pressure and of standard deviation","010009","Geopotential height","Standard level",,"Operational"
2123.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of monthly mean pressure, temperature, vapour pressure and of standard deviation","007032","Height of sensor above local ground (or deck of marine platform)",,"(see Note 3)","Operational"
2124.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of monthly mean pressure, temperature, vapour pressure and of standard deviation","012101","Temperature/air temperature",,,"Operational"
2125.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of monthly mean pressure, temperature, vapour pressure and of standard deviation","002051","Indicator to specify observing method for extreme temperatures","= 2",,"Operational"
2126.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of monthly mean pressure, temperature, vapour pressure and of standard deviation","004051","Principal time of daily reading of maximum temperature",,,"Operational"
2127.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of monthly mean pressure, temperature, vapour pressure and of standard deviation","012118","Maximum temperature at height specified, past 24 hours",,,"Operational"
2128.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of monthly mean pressure, temperature, vapour pressure and of standard deviation","004052","Principal time of daily reading of minimum temperature",,,"Operational"
2129.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of monthly mean pressure, temperature, vapour pressure and of standard deviation","012119","Minimum temperature at height specified, past 24 hours",,,"Operational"
2130.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of monthly mean pressure, temperature, vapour pressure and of standard deviation","013004","Vapour pressure",,,"Operational"
2131.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of monthly mean pressure, temperature, vapour pressure and of standard deviation","012151","Standard deviation of daily mean temperature",,,"Operational"
2132.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of monthly mean pressure, temperature, vapour pressure and of standard deviation","007032","Height of sensor above local ground (or deck of marine platform)","Set to missing (cancel)",,"Operational"
2133.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normal of sunshine duration","014032","Total sunshine",,,"Operational"
2134.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normal of sunshine duration","008023","First-order statistics","Set to missing",,"Operational"
2135.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of precipitation","004001","Year","Beginning of the reference period",,"Operational"
2136.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of precipitation","004001","Year","Ending of the reference period",,"Operational"
2137.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of precipitation","004002","Month",,,"Operational"
2138.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of precipitation","004003","Day","= 1","(see Note 2)","Operational"
2139.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of precipitation","004004","Hour","= 6","(see Note 2)","Operational"
2140.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of precipitation","004022","Time period or displacement","= 1",,"Operational"
2141.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of precipitation","007032","Height of sensor above local ground (or deck of marine platform)",,"(see Note 3)","Operational"
2142.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of precipitation","008023","First-order statistics","= 4 Mean value",,"Operational"
2143.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of precipitation","013060","Total accumulated precipitation",,,"Operational"
2144.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of precipitation","004053","Number of days with precipitation equal to or more than 1 mm",,,"Operational"
2145.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of precipitation","008023","First-order statistics","Set to missing",,"Operational"
2146.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of precipitation","102008","Replicate 2 descriptors 8 times",,,"Operational"
2147.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of precipitation","008050","Qualifier for number of missing values in calculation of statistic","= 1 Pressure, = 2 Temperature, = 3 Extreme temperatures, = 4 Vapour pressure, = 5 Precipitation, = 6 Sunshine duration, = 7 Maximum temperature, = 8 Minimum temperature","(see Note 4)","Operational"
2148.00,"07","Surface report sequences (land)","307072","(Monthly normals for a land station)","Normals of precipitation","008020","Total number of missing entities (with respect to accumulation or average)","Years","(see Note 4)","Operational"
2149.00,"07","Surface report sequences (land)","307073","(Representation of CLIMAT data of the actual month and for monthly normals)",,"307071","Monthly values of a land station",,,"Operational"
2150.00,"07","Surface report sequences (land)","307073","(Representation of CLIMAT data of the actual month and for monthly normals)",,"307072","Monthly normals for a land station",,,"Operational"
2151.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"301090","Surface station identification; time, horizontal and vertical coordinates",,,"Operational"
2152.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"302031","Pressure information",,,"Operational"
2153.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"302035","Basic synoptic ""instantaneous"" data",,,"Operational"
2154.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"302036","Clouds with bases below station level",,,"Operational"
2155.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
2156.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"031000","Short delayed descriptor replication factor",,,"Operational"
2157.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"302047","Direction of cloud drift",,,"Operational"
2158.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"008002","Vertical significance (surface observations)",,,"Operational"
2159.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
2160.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"031000","Short delayed descriptor replication factor",,,"Operational"
2161.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"302048","Direction and elevation of cloud",,,"Operational"
2162.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"302037","State of ground, snow depth, ground minimum temperature",,,"Operational"
2163.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"102000","Delayed replication of 2 descriptors",,,"Operational"
2164.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"031000","Short delayed descriptor replication factor",,,"Operational"
2165.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"022061","State of the sea",,,"Operational"
2166.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"020058","Visibility seawards from a coastal station",,,"Operational"
2167.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
2168.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"031000","Short delayed descriptor replication factor",,,"Operational"
2169.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"302056","Sea/water temperature","Sea/water surface temperature, method of measurement, depth below water surface",,"Operational"
2170.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
2171.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"031000","Short delayed descriptor replication factor",,,"Operational"
2172.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"302055","Icing and ice",,,"Operational"
2173.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"302043","Basic synoptic ""period"" data",,,"Operational"
2174.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"302044","Evaporation data",,,"Operational"
2175.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
2176.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"031001","Delayed descriptor replication factor",,,"Operational"
2177.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"302045","Radiation data (from 1 hour and 24-hour period)",,,"Operational"
2178.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
2179.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"031000","Short delayed descriptor replication factor",,,"Operational"
2180.00,"07","Surface report sequences (land)","307079","(Sequence for representation of synoptic reports from fixed land stations suitable for SYNOP data and for maritime data from coastal stations)",,"302046","Temperature change",,,"Operational"
2182.00,"07","Surface report sequences (land)","307080","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data)",,"301090","Surface station identification; time, horizontal and vertical coordinates",,,"Operational"
2183.00,"07","Surface report sequences (land)","307080","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data)",,"302031","Pressure information",,,"Operational"
2184.00,"07","Surface report sequences (land)","307080","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data)",,"302035","Basic synoptic ""instantaneous"" data",,,"Operational"
2185.00,"07","Surface report sequences (land)","307080","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data)",,"302036","Clouds with bases below station level",,,"Operational"
2186.00,"07","Surface report sequences (land)","307080","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data)",,"302047","Direction of cloud drift",,,"Operational"
2187.00,"07","Surface report sequences (land)","307080","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data)",,"008002","Vertical significance (surface observations)",,,"Operational"
2188.00,"07","Surface report sequences (land)","307080","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data)",,"302048","Direction and elevation of cloud",,,"Operational"
2189.00,"07","Surface report sequences (land)","307080","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data)",,"302037","State of ground, snow depth, ground minimum temperature",,,"Operational"
2190.00,"07","Surface report sequences (land)","307080","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data)",,"302043","Basic synoptic ""period"" data",,,"Operational"
2191.00,"07","Surface report sequences (land)","307080","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data)",,"302044","Evaporation data",,,"Operational"
2192.00,"07","Surface report sequences (land)","307080","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data)",,"101002","Replicate 1 descriptor 2 times",,,"Operational"
2193.00,"07","Surface report sequences (land)","307080","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data)",,"302045","Radiation data (from 1 hour and 24-hour period)",,,"Operational"
2194.00,"07","Surface report sequences (land)","307080","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data)",,"302046","Temperature change",,,"Operational"
2195.00,"07","Surface report sequences (land)","307081","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA I)",,"301090","Surface station identification; time, horizontal and vertical coordinates",,,"Operational"
2196.00,"07","Surface report sequences (land)","307081","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA I)",,"302031","Pressure information",,,"Operational"
2197.00,"07","Surface report sequences (land)","307081","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA I)",,"302035","Basic synoptic ""instantaneous"" data",,,"Operational"
2198.00,"07","Surface report sequences (land)","307081","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA I)",,"302036","Clouds with bases below station level",,,"Operational"
2199.00,"07","Surface report sequences (land)","307081","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA I)",,"302047","Direction of cloud drift",,,"Operational"
2200.00,"07","Surface report sequences (land)","307081","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA I)",,"008002","Vertical significance (surface observations)","Set to missing (cancel)",,"Operational"
2201.00,"07","Surface report sequences (land)","307081","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA I)",,"302048","Direction and elevation of cloud",,,"Operational"
2202.00,"07","Surface report sequences (land)","307081","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA I)",,"302037","State of ground, snow depth, ground minimum temperature",,,"Operational"
2203.00,"07","Surface report sequences (land)","307081","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA I)",,"012122","Ground minimum temperature of the preceding night",,,"Operational"
2204.00,"07","Surface report sequences (land)","307081","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA I)",,"013056","Character and intensity of precipitation",,,"Operational"
2205.00,"07","Surface report sequences (land)","307081","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA I)",,"013057","Time of beginning or end of precipitation",,,"Operational"
2206.00,"07","Surface report sequences (land)","307081","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA I)",,"020101","Locust (acridian) name",,,"Operational"
2207.00,"07","Surface report sequences (land)","307081","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA I)",,"020102","Locust (maturity) colour",,,"Operational"
2208.00,"07","Surface report sequences (land)","307081","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA I)",,"020103","Stage of development of locusts",,,"Operational"
2209.00,"07","Surface report sequences (land)","307081","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA I)",,"020104","Organization state of swarm or band of locusts",,,"Operational"
2210.00,"07","Surface report sequences (land)","307081","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA I)",,"020105","Size of swarm or band of locusts and duration of passage of swarm",,,"Operational"
2211.00,"07","Surface report sequences (land)","307081","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA I)",,"020106","Locust population density",,,"Operational"
2212.00,"07","Surface report sequences (land)","307081","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA I)",,"020107","Direction of movements of locust swarm",,,"Operational"
2213.00,"07","Surface report sequences (land)","307081","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA I)",,"020108","Extent of vegetation",,,"Operational"
2214.00,"07","Surface report sequences (land)","307081","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA I)",,"302043","Basic synoptic ""period"" data",,,"Operational"
2215.00,"07","Surface report sequences (land)","307081","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA I)",,"302044","Evaporation data",,,"Operational"
2216.00,"07","Surface report sequences (land)","307081","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA I)",,"101002","Replicate 1 descriptor 2 times",,,"Operational"
2217.00,"07","Surface report sequences (land)","307081","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA I)",,"302045","Radiation data (from 1 hour and 24-hour period)",,,"Operational"
2218.00,"07","Surface report sequences (land)","307081","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA I)",,"302046","Temperature change",,,"Operational"
2219.00,"07","Surface report sequences (land)","307082","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA II)",,"301090","Surface station identification; time, horizontal and vertical coordinates",,,"Operational"
2220.00,"07","Surface report sequences (land)","307082","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA II)",,"302031","Pressure information",,,"Operational"
2221.00,"07","Surface report sequences (land)","307082","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA II)",,"302035","Basic synoptic ""instantaneous"" data",,,"Operational"
2222.00,"07","Surface report sequences (land)","307082","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA II)",,"302036","Clouds with bases below station level",,,"Operational"
2223.00,"07","Surface report sequences (land)","307082","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA II)",,"302047","Direction of cloud drift",,,"Operational"
2224.00,"07","Surface report sequences (land)","307082","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA II)",,"008002","Vertical significance (surface observations)","Set to missing (cancel)",,"Operational"
2225.00,"07","Surface report sequences (land)","307082","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA II)",,"302048","Direction and elevation of cloud",,,"Operational"
2226.00,"07","Surface report sequences (land)","307082","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA II)",,"302037","State of ground, snow depth, ground minimum temperature",,,"Operational"
2227.00,"07","Surface report sequences (land)","307082","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA II)",,"012121","Ground minimum temperature","At the time of observation",,"Operational"
2228.00,"07","Surface report sequences (land)","307082","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA II)",,"012122","Ground minimum temperature of the preceding night",,,"Operational"
2229.00,"07","Surface report sequences (land)","307082","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA II)",,"302043","Basic synoptic ""period"" data",,,"Operational"
2230.00,"07","Surface report sequences (land)","307082","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA II)",,"302044","Evaporation data",,,"Operational"
2231.00,"07","Surface report sequences (land)","307082","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA II)",,"101002","Replicate 1 descriptor 2 times",,,"Operational"
2232.00,"07","Surface report sequences (land)","307082","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA II)",,"302045","Radiation data (from 1 hour and 24-hour period)",,,"Operational"
2233.00,"07","Surface report sequences (land)","307082","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA II)",,"302046","Temperature change",,,"Operational"
2234.00,"07","Surface report sequences (land)","307083","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA III)",,"301090","Surface station identification; time, horizontal and vertical coordinates",,,"Operational"
2235.00,"07","Surface report sequences (land)","307083","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA III)",,"302031","Pressure information",,,"Operational"
2236.00,"07","Surface report sequences (land)","307083","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA III)",,"302035","Basic synoptic ""instantaneous"" data",,,"Operational"
2237.00,"07","Surface report sequences (land)","307083","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA III)",,"302036","Clouds with bases below station level",,,"Operational"
2238.00,"07","Surface report sequences (land)","307083","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA III)",,"302047","Direction of cloud drift",,,"Operational"
2239.00,"07","Surface report sequences (land)","307083","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA III)",,"008002","Vertical significance (surface observations)","Set to missing (cancel)",,"Operational"
2240.00,"07","Surface report sequences (land)","307083","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA III)",,"302048","Direction and elevation of cloud",,,"Operational"
2241.00,"07","Surface report sequences (land)","307083","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA III)",,"302037","State of ground, snow depth, ground minimum temperature",,,"Operational"
2242.00,"07","Surface report sequences (land)","307083","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA III)",,"012122","Ground minimum temperature of the preceding night",,,"Operational"
2243.00,"07","Surface report sequences (land)","307083","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA III)",,"302043","Basic synoptic ""period"" data",,,"Operational"
2244.00,"07","Surface report sequences (land)","307083","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA III)",,"302044","Evaporation data",,,"Operational"
2245.00,"07","Surface report sequences (land)","307083","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA III)",,"101002","Replicate 1 descriptor 2 times",,,"Operational"
2246.00,"07","Surface report sequences (land)","307083","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA III)",,"302045","Radiation data (from 1 hour and 24-hour period)",,,"Operational"
2247.00,"07","Surface report sequences (land)","307083","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA III)",,"302046","Temperature change",,,"Operational"
2248.00,"07","Surface report sequences (land)","307084","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA IV)",,"301090","Surface station identification; time, horizontal and vertical coordinates",,,"Operational"
2249.00,"07","Surface report sequences (land)","307084","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA IV)",,"302031","Pressure information",,,"Operational"
2250.00,"07","Surface report sequences (land)","307084","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA IV)",,"302035","Basic synoptic ""instantaneous"" data",,,"Operational"
2251.00,"07","Surface report sequences (land)","307084","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA IV)",,"302036","Clouds with bases below station level",,,"Operational"
2252.00,"07","Surface report sequences (land)","307084","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA IV)",,"302047","Direction of cloud drift",,,"Operational"
2253.00,"07","Surface report sequences (land)","307084","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA IV)",,"008002","Vertical significance (surface observations)","Set to missing (cancel)",,"Operational"
2254.00,"07","Surface report sequences (land)","307084","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA IV)",,"302048","Direction and elevation of cloud",,,"Operational"
2255.00,"07","Surface report sequences (land)","307084","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA IV)",,"302037","State of ground, snow depth, ground minimum temperature",,,"Operational"
2256.00,"07","Surface report sequences (land)","307084","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA IV)",,"020055","State of sky in the tropics",,,"Operational"
2257.00,"07","Surface report sequences (land)","307084","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA IV)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
2258.00,"07","Surface report sequences (land)","307084","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA IV)",,"031001","Delayed descriptor replication factor",,,"Operational"
2259.00,"07","Surface report sequences (land)","307084","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA IV)",,"205001","Signify character","Character field of 1 character",,"Operational"
2260.00,"07","Surface report sequences (land)","307084","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA IV)",,"302043","Basic synoptic ""period"" data",,,"Operational"
2261.00,"07","Surface report sequences (land)","307084","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA IV)",,"302044","Evaporation data",,,"Operational"
2262.00,"07","Surface report sequences (land)","307084","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA IV)",,"101002","Replicate 1 descriptor 2 times",,,"Operational"
2263.00,"07","Surface report sequences (land)","307084","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA IV)",,"302045","Radiation data (from 1 hour and 24-hour period)",,,"Operational"
2264.00,"07","Surface report sequences (land)","307084","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA IV)",,"302046","Temperature change",,,"Operational"
2266.00,"07","Surface report sequences (land)","307086","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA VI)",,"301090","Surface station identification; time, horizontal and vertical coordinates",,,"Operational"
2267.00,"07","Surface report sequences (land)","307086","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA VI)",,"302031","Pressure information",,,"Operational"
2268.00,"07","Surface report sequences (land)","307086","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA VI)",,"302035","Basic synoptic ""instantaneous"" data",,,"Operational"
2269.00,"07","Surface report sequences (land)","307086","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA VI)",,"302036","Clouds with bases below station level",,,"Operational"
2270.00,"07","Surface report sequences (land)","307086","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA VI)",,"008002","Vertical significance (surface observations)","Set to missing (cancel)",,"Operational"
2271.00,"07","Surface report sequences (land)","307086","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA VI)",,"302037","State of ground, snow depth, ground minimum temperature",,,"Operational"
2272.00,"07","Surface report sequences (land)","307086","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA VI)",,"302066","Dangerous weather phenomena",,,"Operational"
2273.00,"07","Surface report sequences (land)","307086","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA VI)",,"302043","Basic synoptic ""period"" data",,,"Operational"
2274.00,"07","Surface report sequences (land)","307086","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA VI)",,"302044","Evaporation data",,,"Operational"
2275.00,"07","Surface report sequences (land)","307086","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA VI)",,"101002","Replicate 1 descriptor 2 times",,,"Operational"
2276.00,"07","Surface report sequences (land)","307086","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA VI)",,"302045","Radiation data (from 1 hour and 24-hour period)",,,"Operational"
2277.00,"07","Surface report sequences (land)","307087","(""Instantaneous"" parameters of sequence 3 07 089)","Surface station identification, time, horizontal and vertical coordinates","301001","WMO block and station numbers","IIiii",,"Operational"
2278.00,"07","Surface report sequences (land)","307087","(""Instantaneous"" parameters of sequence 3 07 089)","Surface station identification, time, horizontal and vertical coordinates","002001","Type of station","ix",,"Operational"
2279.00,"07","Surface report sequences (land)","307087","(""Instantaneous"" parameters of sequence 3 07 089)","Surface station identification, time, horizontal and vertical coordinates","301011","Year, month, day","YY",,"Operational"
2280.00,"07","Surface report sequences (land)","307087","(""Instantaneous"" parameters of sequence 3 07 089)","Surface station identification, time, horizontal and vertical coordinates","301012","Hour, minute","GG, gg",,"Operational"
2281.00,"07","Surface report sequences (land)","307087","(""Instantaneous"" parameters of sequence 3 07 089)","Surface station identification, time, horizontal and vertical coordinates","301023","Latitude/longitude (coarse accuracy)",,,"Operational"
2282.00,"07","Surface report sequences (land)","307087","(""Instantaneous"" parameters of sequence 3 07 089)","Surface station identification, time, horizontal and vertical coordinates","007030","Height of station ground above mean sea level",,,"Operational"
2283.00,"07","Surface report sequences (land)","307087","(""Instantaneous"" parameters of sequence 3 07 089)","Surface station identification, time, horizontal and vertical coordinates","007031","Height of barometer above mean sea level",,,"Operational"
2284.00,"07","Surface report sequences (land)","307087","(""Instantaneous"" parameters of sequence 3 07 089)","Pressure data","302001","Pressure and 3-hour pressure change","PoPoPoPo, PPPP, ppp, a",,"Operational"
2285.00,"07","Surface report sequences (land)","307087","(""Instantaneous"" parameters of sequence 3 07 089)","Pressure data","010062","24-hour pressure change","p24p24p24",,"Operational"
2286.00,"07","Surface report sequences (land)","307087","(""Instantaneous"" parameters of sequence 3 07 089)","Pressure data","007004","Pressure","Standard level a3 = 925, 850, 700, ..hPa | Set to missing for lowland stations",,"Operational"
2287.00,"07","Surface report sequences (land)","307087","(""Instantaneous"" parameters of sequence 3 07 089)","Pressure data","010009","Geopotential height","Standard level hhh | Set to missing for lowland stations",,"Operational"
2288.00,"07","Surface report sequences (land)","307087","(""Instantaneous"" parameters of sequence 3 07 089)","Temperature and humidity","007032","Height of sensor above local ground (or deck of marine platform)","Temperature measurement",,"Operational"
2289.00,"07","Surface report sequences (land)","307087","(""Instantaneous"" parameters of sequence 3 07 089)","Temperature and humidity","012101","Temperature/air temperature","snTTT | Scale 2",,"Operational"
2290.00,"07","Surface report sequences (land)","307087","(""Instantaneous"" parameters of sequence 3 07 089)","Temperature and humidity","012103","Dewpoint temperature","snTdTdTd | Scale 2",,"Operational"
2291.00,"07","Surface report sequences (land)","307087","(""Instantaneous"" parameters of sequence 3 07 089)","Temperature and humidity","013003","Relative humidity",,,"Operational"
2292.00,"07","Surface report sequences (land)","307087","(""Instantaneous"" parameters of sequence 3 07 089)","Temperature and humidity","007032","Height of sensor above local ground (or deck of marine platform)","Set to missing (cancel)",,"Operational"
2293.00,"07","Surface report sequences (land)","307087","(""Instantaneous"" parameters of sequence 3 07 089)","Visibility","020001","Horizontal visibility","VV",,"Operational"
2294.00,"07","Surface report sequences (land)","307087","(""Instantaneous"" parameters of sequence 3 07 089)","Cloud data","302004","General cloud information","Cloud cover (total) N: If N = 9, then 0 20 010 = 113, if N = /, then 0 20 010 = missing | Vertical significance: If CL are observed, then 0 08 002 = 7 | Low cloud: If CL are not observed and CM are observed, then 0 08 002 = 8 | Middle cloud: If only CH are observed, 0 08 002 = 0, if N = 9, then 0 08 002 = 5, if N = 0, then 0 08 002 = 62, if N = /, then 0 08 002 = missing | Cloud amount (of low or middle clouds) Nh: If N = 0, then 0 20 011 = 0, if N = 9, then 0 20 011 = 9, if N = /, then 0 20 011 = missing | Height of base of cloud h: If N = 0 or /, then 0 20 013 = missing | Cloud type (low clouds) CL: 0 20 012 = CL + 30, if N = 0, then 0 20 012 = 30, if N = 9 or /, then 0 20 012 = 62 | Cloud type (middle clouds) CM: 0 20 012 = CM + 20, if N = 0, then 0 20 012 = 20, if N = 9 or / or CM = /, then 0 20 012 = 61 | Cloud type (high clouds) CH: 0 20 012 = CH + 10, if N = 0, then 0 20 012 = 10, if N = 9 or / or CH = /, then 0 20 012 = 60",,"Operational"
2295.00,"07","Surface report sequences (land)","307087","(""Instantaneous"" parameters of sequence 3 07 089)","Cloud data","101000","Delayed replication of 1 descriptor",,,"Operational"
2296.00,"07","Surface report sequences (land)","307087","(""Instantaneous"" parameters of sequence 3 07 089)","Cloud data","031001","Delayed descriptor replication factor",,,"Operational"
2297.00,"07","Surface report sequences (land)","307087","(""Instantaneous"" parameters of sequence 3 07 089)","Cloud data","302005","Cloud layer","Vertical significance: In any Cb layer, 0 08 002 = 4, else in the first replication, if N = 9, then 0 08 002 = 5, if N = /, then 0 08 002 = missing, else 0 08 002 = 1, in the other replications 0 08 002 = 2, 3, 4 | Cloud amount Ns: In the first replication, if N = /, then 0 20 011 = missing, else 0 20 011 = Ns, in the other replications 0 20 011 = Ns | Cloud type C: If N = 9 or /, then 0 20 012 = missing, else 0 20 012 = C | Height of base of cloud hshs",,"Operational"
2318.00,"07","Surface report sequences (land)","307088","(""Period"" parameters of sequence 3 07 089)","Present and past weather","020003","Present weather","ww",,"Operational"
2319.00,"07","Surface report sequences (land)","307088","(""Period"" parameters of sequence 3 07 089)","Present and past weather","004024","Time period or displacement","= -6 at 00, 06, 12, 18 UTC, = -3 at 03, 09,15, 21 UTC",,"Operational"
2320.00,"07","Surface report sequences (land)","307088","(""Period"" parameters of sequence 3 07 089)","Present and past weather","020004","Past weather (1)","W1",,"Operational"
2321.00,"07","Surface report sequences (land)","307088","(""Period"" parameters of sequence 3 07 089)","Present and past weather","020005","Past weather (2)","W2",,"Operational"
2322.00,"07","Surface report sequences (land)","307088","(""Period"" parameters of sequence 3 07 089)","Evaporation","004024","Time period or displacement","= -24 (hours)",,"Operational"
2323.00,"07","Surface report sequences (land)","307088","(""Period"" parameters of sequence 3 07 089)","Evaporation","002004","Type of instrumentation for evaporation measurement or type of crop for which evapotranspiration is reported","iE",,"Operational"
2324.00,"07","Surface report sequences (land)","307088","(""Period"" parameters of sequence 3 07 089)","Evaporation","013033","Evaporation/evapotranspiration","EEE",,"Operational"
2325.00,"07","Surface report sequences (land)","307088","(""Period"" parameters of sequence 3 07 089)","Sunshine","102002","Replicate 2 descriptors 2 times",,,"Operational"
2326.00,"07","Surface report sequences (land)","307088","(""Period"" parameters of sequence 3 07 089)","Sunshine","004024","Time period or displacement","= -24 (hours) in the first replication, = -1 (hour) in the second replication",,"Operational"
2327.00,"07","Surface report sequences (land)","307088","(""Period"" parameters of sequence 3 07 089)","Sunshine","014031","Total sunshine","SSS in the first replication, SS in the second replication",,"Operational"
2328.00,"07","Surface report sequences (land)","307088","(""Period"" parameters of sequence 3 07 089)","Precipitation","102002","Replicate 2 descriptors 2 times",,,"Operational"
2329.00,"07","Surface report sequences (land)","307088","(""Period"" parameters of sequence 3 07 089)","Precipitation","004024","Time period or displacement","tR",,"Operational"
2330.00,"07","Surface report sequences (land)","307088","(""Period"" parameters of sequence 3 07 089)","Precipitation","013011","Total precipitation/total water equivalent","RRR | = 0 No precipitation, = -0.1 Trace",,"Operational"
2331.00,"07","Surface report sequences (land)","307088","(""Period"" parameters of sequence 3 07 089)","Extreme temperatures","007032","Height of sensor above local ground (or deck of marine platform)","Temperature measurement",,"Operational"
2332.00,"07","Surface report sequences (land)","307088","(""Period"" parameters of sequence 3 07 089)","Extreme temperatures","004024","Time period or displacement","= -12 (hours)",,"Operational"
2333.00,"07","Surface report sequences (land)","307088","(""Period"" parameters of sequence 3 07 089)","Extreme temperatures","012111","Maximum temperature, at height and over period specified","snTxTxTx",,"Operational"
2334.00,"07","Surface report sequences (land)","307088","(""Period"" parameters of sequence 3 07 089)","Extreme temperatures","004024","Time period or displacement","= -12 (hours)",,"Operational"
2335.00,"07","Surface report sequences (land)","307088","(""Period"" parameters of sequence 3 07 089)","Extreme temperatures","012112","Minimum temperature, at height and over period specified","snTnTnTn",,"Operational"
2336.00,"07","Surface report sequences (land)","307088","(""Period"" parameters of sequence 3 07 089)","Wind data","007032","Height of sensor above local ground (or deck of marine platform)","Wind measurement",,"Operational"
2337.00,"07","Surface report sequences (land)","307088","(""Period"" parameters of sequence 3 07 089)","Wind data","002002","Type of instrumentation for wind measurement","iw",,"Operational"
2338.00,"07","Surface report sequences (land)","307088","(""Period"" parameters of sequence 3 07 089)","Wind data","008021","Time significance","= 2 Time averaged",,"Operational"
2339.00,"07","Surface report sequences (land)","307088","(""Period"" parameters of sequence 3 07 089)","Wind data","004025","Time period or displacement","= -10 (minutes) or number of minutes after a significant change of wind, if any",,"Operational"
2340.00,"07","Surface report sequences (land)","307088","(""Period"" parameters of sequence 3 07 089)","Wind data","011001","Wind direction","dd | If dd = 00 Calm or dd = 99 Variable, 0 11 001 = 0",,"Operational"
2341.00,"07","Surface report sequences (land)","307088","(""Period"" parameters of sequence 3 07 089)","Wind data","011002","Wind speed","ff",,"Operational"
2342.00,"07","Surface report sequences (land)","307088","(""Period"" parameters of sequence 3 07 089)","Wind data","008021","Time significance","Set to missing (cancel)",,"Operational"
2343.00,"07","Surface report sequences (land)","307089","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data manually encoded in CREX)",,"307087","""Instantaneous"" parameters of sequence 3 07 089",,,"Operational"
2344.00,"07","Surface report sequences (land)","307089","(Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data manually encoded in CREX)",,"307088","""Period"" parameters of sequence 3 07 089",,,"Operational"
2345.00,"07","Surface report sequences (land)","307090","(Sequence for representation of synoptic reports from a mobile land station suitable for SYNOP MOBIL data)",,"301092","Mobile surface station identification, date/time, horizontal and vertical coordinates",,,"Operational"
2346.00,"07","Surface report sequences (land)","307090","(Sequence for representation of synoptic reports from a mobile land station suitable for SYNOP MOBIL data)",,"302031","Pressure information",,,"Operational"
2347.00,"07","Surface report sequences (land)","307090","(Sequence for representation of synoptic reports from a mobile land station suitable for SYNOP MOBIL data)",,"302035","Basic synoptic ""instantaneous"" data",,,"Operational"
2348.00,"07","Surface report sequences (land)","307090","(Sequence for representation of synoptic reports from a mobile land station suitable for SYNOP MOBIL data)",,"302036","Clouds with bases below station level",,,"Operational"
2349.00,"07","Surface report sequences (land)","307090","(Sequence for representation of synoptic reports from a mobile land station suitable for SYNOP MOBIL data)",,"302047","Direction of cloud drift",,,"Operational"
2350.00,"07","Surface report sequences (land)","307090","(Sequence for representation of synoptic reports from a mobile land station suitable for SYNOP MOBIL data)",,"008002","Vertical significance (surface observations)",,,"Operational"
2351.00,"07","Surface report sequences (land)","307090","(Sequence for representation of synoptic reports from a mobile land station suitable for SYNOP MOBIL data)",,"302048","Direction and elevation of cloud",,,"Operational"
2352.00,"07","Surface report sequences (land)","307090","(Sequence for representation of synoptic reports from a mobile land station suitable for SYNOP MOBIL data)",,"302037","State of ground, snow depth, ground minimum temperature",,,"Operational"
2353.00,"07","Surface report sequences (land)","307090","(Sequence for representation of synoptic reports from a mobile land station suitable for SYNOP MOBIL data)",,"302043","Basic synoptic ""period"" data",,,"Operational"
2354.00,"07","Surface report sequences (land)","307090","(Sequence for representation of synoptic reports from a mobile land station suitable for SYNOP MOBIL data)",,"302044","Evaporation data",,,"Operational"
2355.00,"07","Surface report sequences (land)","307090","(Sequence for representation of synoptic reports from a mobile land station suitable for SYNOP MOBIL data)",,"101002","Replicate 1 descriptor 2 times",,,"Operational"
2356.00,"07","Surface report sequences (land)","307090","(Sequence for representation of synoptic reports from a mobile land station suitable for SYNOP MOBIL data)",,"302045","Radiation data (from 1 hour and 24-hour period)",,,"Operational"
2357.00,"07","Surface report sequences (land)","307090","(Sequence for representation of synoptic reports from a mobile land station suitable for SYNOP MOBIL data)",,"302046","Temperature change",,,"Operational"
2358.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"301089","National station identification",,,"Operational"
2359.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"301090","Surface station identification; time, horizontal and vertical co-ordinates",,,"Operational"
2360.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"008010","Surface qualifier (temperature data)",,,"Operational"
2361.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"301091","Surface station instrumentation",,,"Operational"
2362.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"302001","Pressure and 3-hour pressure change",,,"Operational"
2363.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"007004","Pressure","Standard level",,"Operational"
2364.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"010009","Geopotential height","Standard level",,"Operational"
2365.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"302072","Temperature and humidity data",,,"Operational"
2366.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"103000","Delayed replication of 3 descriptors",,,"Operational"
2367.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"031000","Short delayed descriptor replication factor",,,"Operational"
2368.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"101005","Replicate 1 descriptor 5 times",,,"Operational"
2369.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"307063","Depth below land surface and soil temperature",,,"Operational"
2370.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"007061","Depth below land surface","Set to missing (cancel)",,"Operational"
2371.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
2372.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"031000","Short delayed descriptor replication factor",,,"Operational"
2373.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"302069","Visibility data",,,"Operational"
2374.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"007032","Height of sensor above local ground (or deck of marine platform)","Set to missing (cancel)",,"Operational"
2375.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"007033","Height of sensor above water surface","Set to missing (cancel)",,"Operational"
2376.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"105000","Delayed replication of 5 descriptors",,,"Operational"
2377.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"031000","Short delayed descriptor replication factor",,,"Operational"
2378.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"020031","Ice deposit (thickness)",,,"Operational"
2379.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"020032","Rate of ice accretion (estimated)",,,"Operational"
2380.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"002038","Method of water temperature and/or salinity measurement",,,"Operational"
2381.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"022043","Sea/water temperature","Scale: 2",,"Operational"
2382.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"302021","Waves",,,"Operational"
2383.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
2384.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"031000","Short delayed descriptor replication factor",,,"Operational"
2385.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"302078","State of ground and snow depth measurement",,,"Operational"
2386.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
2387.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"031000","Short delayed descriptor replication factor",,,"Operational"
2388.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"302073","Cloud data",,,"Operational"
2389.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
2390.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"031000","Short delayed descriptor replication factor",,,"Operational"
2391.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"302074","Present and past weather",,,"Operational"
2392.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
2393.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"031000","Short delayed descriptor replication factor",,,"Operational"
2394.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"302175","Intensity of precipitation, size of precipitation element",,,"Operational"
2395.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"102000","Delayed replication of 2 descriptors",,,"Operational"
2396.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"031000","Short delayed descriptor replication factor",,,"Operational"
2397.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"004025","Time period or displacement","= -10 (minutes)",,"Operational"
2398.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"302076","Precipitation, obscuration and other phenomena",,,"Operational"
2399.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"302071","Wind data from one-hour period",,,"Operational"
2400.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"302077","Extreme temperature data",,,"Operational"
2401.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"007033","Height of sensor above water surface","Set to missing (cancel)",,"Operational"
2402.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
2403.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"031000","Short delayed descriptor replication factor",,,"Operational"
2404.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"302079","Precipitation measurement",,,"Operational"
2405.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"007032","Height of sensor above local ground (or deck of marine platform)","Set to missing (cancel)",,"Operational"
2406.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
2407.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"031000","Short delayed descriptor replication factor",,,"Operational"
2408.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"302080","Evaporation measurement",,,"Operational"
2409.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
2410.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"031000","Short delayed descriptor replication factor",,,"Operational"
2411.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"302081","Total sunshine data",,,"Operational"
2412.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
2413.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"031000","Short delayed descriptor replication factor",,,"Operational"
2414.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"302082","Radiation data",,,"Operational"
2415.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"102000","Delayed replication of 2 descriptors",,,"Operational"
2416.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"031000","Short delayed descriptor replication factor",,,"Operational"
2417.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"004025","Time period or displacement","= -10 (minutes)",,"Operational"
2418.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"013059","Number of flashes (thunderstorm)",,,"Operational"
2419.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
2420.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"031000","Short delayed descriptor replication factor",,,"Operational"
2421.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"302083","First-order statistics of P, W, T, U data",,,"Operational"
2422.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"033005","Quality information (AWS data)",,,"Operational"
2423.00,"07","Surface report sequences (land)","307091","(BUFR template for surface observations from one-hour period with national and WMO station identification)",,"033006","Internal measurement status information (AWS)",,,"Operational"
2517.00,"07","Surface report sequences (land)","307096","(Sequence for representation of SYNOP with supplementary information on one-hour observations)",,"301090","Surface station identification; time, horizontal and vertical coordinates",,,"Operational"
2518.00,"07","Surface report sequences (land)","307096","(Sequence for representation of SYNOP with supplementary information on one-hour observations)",,"301089","National station identification",,,"Operational"
2519.00,"07","Surface report sequences (land)","307096","(Sequence for representation of SYNOP with supplementary information on one-hour observations)",,"008010","Surface qualifier (temperature data)",,,"Operational"
2520.00,"07","Surface report sequences (land)","307096","(Sequence for representation of SYNOP with supplementary information on one-hour observations)",,"301091","Surface station instrumentation",,,"Operational"
2521.00,"07","Surface report sequences (land)","307096","(Sequence for representation of SYNOP with supplementary information on one-hour observations)",,"302084","""Instantaneous"" data of sequence 3 07 096",,,"Operational"
2522.00,"07","Surface report sequences (land)","307096","(Sequence for representation of SYNOP with supplementary information on one-hour observations)",,"302085","""Period"" data of sequence 3 07 096",,,"Operational"
2523.00,"07","Surface report sequences (land)","307096","(Sequence for representation of SYNOP with supplementary information on one-hour observations)",,"033005","Quality information (AWS data)",,,"Operational"
2524.00,"07","Surface report sequences (land)","307096","(Sequence for representation of SYNOP with supplementary information on one-hour observations)",,"033006","Internal measurement status information (AWS)",,,"Operational"
2558.00,"08","Surface report sequences (sea)","308001","(Buoy/platform - fixed)",,"301033","Buoy/platform - fixed","Identification, type, date/time, position (high accuracy)",,"Operational"
2559.00,"08","Surface report sequences (sea)","308001","(Buoy/platform - fixed)",,"302011","Low altitude station","Basic surface report",,"Operational"
2560.00,"08","Surface report sequences (sea)","308001","(Buoy/platform - fixed)",,"022042","Sea/water temperature",,,"Operational"
2561.00,"08","Surface report sequences (sea)","308002","(Buoy/platform - fixed)",,"301034","Buoy/platform - fixed","Identification, type, date/time, position (coarse accuracy)",,"Operational"
2562.00,"08","Surface report sequences (sea)","308002","(Buoy/platform - fixed)",,"302011","Low altitude station","Basic surface report",,"Operational"
2563.00,"08","Surface report sequences (sea)","308002","(Buoy/platform - fixed)",,"022042","Sea/water temperature",,,"Operational"
2564.00,"08","Surface report sequences (sea)","308003","(Buoy/platform - moving)",,"301035","Buoy/platform - moving","Identification, movement, type, date/time, position (coarse accuracy)","<(see Note 4)>","Operational"
2565.00,"08","Surface report sequences (sea)","308003","(Buoy/platform - moving)",,"302011","Low altitude station","Basic surface report",,"Operational"
2566.00,"08","Surface report sequences (sea)","308003","(Buoy/platform - moving)",,"022042","Sea/water temperature",,,"Operational"
2567.00,"08","Surface report sequences (sea)","308004","(Ship)",,"301036","Ship","Identification, movement, type, date/time, position (coarse accuracy)",,"Operational"
2568.00,"08","Surface report sequences (sea)","308004","(Ship)",,"302011","Low altitude station","Basic surface report",,"Operational"
2569.00,"08","Surface report sequences (sea)","308004","(Ship)",,"022042","Sea/water temperature",,,"Operational"
2570.00,"08","Surface report sequences (sea)","308005",,,"308004","Ship","Basic ship report",,"Operational"
2571.00,"08","Surface report sequences (sea)","308005",,,"302024","Wind and swell waves",,,"Operational"
2572.00,"08","Surface report sequences (sea)","308006","(Buoy Section 1 optional parameters)",,"010004","Pressure",,,"Operational"
2573.00,"08","Surface report sequences (sea)","308006","(Buoy Section 1 optional parameters)",,"010061","3-hour pressure change",,,"Operational"
2574.00,"08","Surface report sequences (sea)","308006","(Buoy Section 1 optional parameters)",,"010063","Characteristic of pressure tendency",,,"Operational"
2575.00,"08","Surface report sequences (sea)","308006","(Buoy Section 1 optional parameters)",,"011001","Wind direction",,,"Operational"
2576.00,"08","Surface report sequences (sea)","308006","(Buoy Section 1 optional parameters)",,"011002","Wind speed",,,"Operational"
2577.00,"08","Surface report sequences (sea)","308006","(Buoy Section 1 optional parameters)",,"012004","Air temperature at 2 m",,,"Operational"
2578.00,"08","Surface report sequences (sea)","308006","(Buoy Section 1 optional parameters)",,"013003","Relative humidity",,,"Operational"
2579.00,"08","Surface report sequences (sea)","308006","(Buoy Section 1 optional parameters)",,"022042","Sea/water temperature",,,"Operational"
2580.00,"08","Surface report sequences (sea)","308007",,,"301055","Identification and type of station, date/time, location (high accuracy), movement",,,"Operational"
2581.00,"08","Surface report sequences (sea)","308007",,,"302011","Low altitude station","Basic surface report",,"Operational"
2582.00,"08","Surface report sequences (sea)","308007",,,"007062","Depth below sea/water surface",,,"Operational"
2583.00,"08","Surface report sequences (sea)","308007",,,"022042","Sea/water temperature",,,"Operational"
2587.00,"08","Surface report sequences (sea)","308009","(Sequence for representation of synoptic reports from a sea station suitable for ship data)",,"301093","Ship identification, movement, date/time, horizontal and vertical coordinates",,,"Operational"
2588.00,"08","Surface report sequences (sea)","308009","(Sequence for representation of synoptic reports from a sea station suitable for ship data)",,"302001","Pressure and 3-hour pressure change",,,"Operational"
2589.00,"08","Surface report sequences (sea)","308009","(Sequence for representation of synoptic reports from a sea station suitable for ship data)",,"302054","Ship ""instantaneous"" data",,,"Operational"
2590.00,"08","Surface report sequences (sea)","308009","(Sequence for representation of synoptic reports from a sea station suitable for ship data)",,"008002","Vertical significance (surface observations)",,,"Operational"
2591.00,"08","Surface report sequences (sea)","308009","(Sequence for representation of synoptic reports from a sea station suitable for ship data)",,"302055","Icing and ice",,,"Operational"
2592.00,"08","Surface report sequences (sea)","308009","(Sequence for representation of synoptic reports from a sea station suitable for ship data)",,"302057","Ship marine data",,,"Operational"
2593.00,"08","Surface report sequences (sea)","308009","(Sequence for representation of synoptic reports from a sea station suitable for ship data)",,"302060","Ship ""period"" data",,,"Operational"
2594.00,"08","Surface report sequences (sea)","308010","(TRACKOB template)",,"001011","Ship or mobile land station identifier",,,"Operational"
2595.00,"08","Surface report sequences (sea)","308010","(TRACKOB template)",,"113000","Delayed replication of 13 descriptors",,,"Operational"
2596.00,"08","Surface report sequences (sea)","308010","(TRACKOB template)",,"031001","Delayed descriptor replication factor",,,"Operational"
2597.00,"08","Surface report sequences (sea)","308010","(TRACKOB template)",,"301011","Year, month, day",,,"Operational"
2598.00,"08","Surface report sequences (sea)","308010","(TRACKOB template)",,"301012","Hour, minute",,,"Operational"
2599.00,"08","Surface report sequences (sea)","308010","(TRACKOB template)",,"301021","Latitude/longitude (high accuracy)",,,"Operational"
2600.00,"08","Surface report sequences (sea)","308010","(TRACKOB template)",,"004080","Averaging period for following value",,,"Operational"
2601.00,"08","Surface report sequences (sea)","308010","(TRACKOB template)",,"022049","Sea-surface temperature",,,"Operational"
2602.00,"08","Surface report sequences (sea)","308010","(TRACKOB template)",,"004080","Averaging period for following value",,,"Operational"
2603.00,"08","Surface report sequences (sea)","308010","(TRACKOB template)",,"022059","Sea-surface salinity",,,"Operational"
2604.00,"08","Surface report sequences (sea)","308010","(TRACKOB template)",,"004080","Averaging period for following value",,,"Operational"
2605.00,"08","Surface report sequences (sea)","308010","(TRACKOB template)",,"022005","Direction of sea-surface current",,,"Operational"
2606.00,"08","Surface report sequences (sea)","308010","(TRACKOB template)",,"002042","Indicator for sea-surface current speed",,,"Operational"
2607.00,"08","Surface report sequences (sea)","308010","(TRACKOB template)",,"022032","Speed of sea-surface current",,,"Operational"
2608.00,"08","Surface report sequences (sea)","308010","(TRACKOB template)",,"002042","Indicator for sea-surface current speed","Cancel",,"Operational"
2609.00,"08","Surface report sequences (sea)","308010","(TRACKOB template)",,"004080","Averaging period for following value","Cancel",,"Operational"
2625.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)",,"001011","Ship or mobile land station identifier","Ship's call sign",,"Operational"
2626.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)",,"002001","Type of station",,,"Operational"
2627.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)",,"301011","Year, month, day",,"(see Note 1)","Operational"
2628.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)",,"301012","Hour, minute",,"(see Note 1)","Operational"
2629.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)",,"301023","Latitude/longitude (coarse accuracy)",,,"Operational"
2630.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)",,"007030","Height of station ground above mean sea level",,"(see Note 3)","Operational"
2631.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)",,"007031","Height of barometer above mean sea level",,"(see Note 3)","Operational"
2632.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)","Monthly mean values of pressure, temperature, vapour pressure and sea/water temperature","004074","Short time period or displacement","= UTC - LST","(see Note 1)","Operational"
2633.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)","Monthly mean values of pressure, temperature, vapour pressure and sea/water temperature","004023","Time period or displacement","= Number of days in the month",,"Operational"
2634.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)","Monthly mean values of pressure, temperature, vapour pressure and sea/water temperature","008023","First-order statistics","= 4 Mean value",,"Operational"
2635.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)","Monthly mean values of pressure, temperature, vapour pressure and sea/water temperature","010051","Pressure reduced to mean sea level",,,"Operational"
2636.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)","Monthly mean values of pressure, temperature, vapour pressure and sea/water temperature","007032","Height of sensor above local ground (or deck of marine platform)","Temperature measurement","(see Note 3)","Operational"
2637.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)","Monthly mean values of pressure, temperature, vapour pressure and sea/water temperature","007033","Height of sensor above water surface","Temperature measurement","(see Note 3)","Operational"
2638.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)","Monthly mean values of pressure, temperature, vapour pressure and sea/water temperature","012101","Temperature/air temperature",,,"Operational"
2639.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)","Monthly mean values of pressure, temperature, vapour pressure and sea/water temperature","013004","Vapour pressure",,,"Operational"
2640.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)","Monthly mean values of pressure, temperature, vapour pressure and sea/water temperature","007032","Height of sensor above local ground (or deck of marine platform)","Set to missing (cancel)",,"Operational"
2641.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)","Monthly mean values of pressure, temperature, vapour pressure and sea/water temperature","007033","Height of sensor above water surface","Set to missing (cancel)",,"Operational"
2642.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)","Monthly mean values of pressure, temperature, vapour pressure and sea/water temperature","302056","Sea/water temperature","Sea-surface temperature, method of measurement, and depth below sea surface",,"Operational"
2643.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)","Monthly mean values of pressure, temperature, vapour pressure and sea/water temperature","008023","First-order statistics","Set to missing",,"Operational"
2644.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)","Precipitation","004003","Day","= 1","(see Note 2)","Operational"
2645.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)","Precipitation","004004","Hour","= 6","(see Note 2)","Operational"
2646.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)","Precipitation","004023","Time period or displacement","= Number of days in the month","(see Note 2)","Operational"
2647.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)","Precipitation","007032","Height of sensor above local ground (or deck of marine platform)",,"(see Note 3)","Operational"
2648.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)","Precipitation","013060","Total accumulated precipitation",,,"Operational"
2649.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)","Precipitation","013051","Frequency group, precipitation",,,"Operational"
2650.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)","Precipitation","004053","Number of days with precipitation equal to or more than 1 mm",,,"Operational"
2651.00,"08","Surface report sequences (sea)","308011","(Monthly values from an ocean weather station - CLIMAT SHIP)","Precipitation","007032","Height of sensor above local ground (or deck of marine platform)","Set to missing (cancel)",,"Operational"
2652.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)",,"004001","Year","Beginning of the reference period",,"Operational"
2653.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)",,"004001","Year","Ending of the reference period",,"Operational"
2654.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)",,"004002","Month",,,"Operational"
2655.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)",,"004003","Day","= 1","(see Note 1)","Operational"
2656.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)",,"004004","Hour","= 0","(see Note 1)","Operational"
2657.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)",,"004074","Short time period or displacement","= UTC - LST","(see Note 1)","Operational"
2658.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)",,"004022","Time period or displacement","= 1",,"Operational"
2659.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)","Normals of monthly mean pressure, temperature, vapour pressure and sea/water temperature","008023","First-order statistics","= 4 Mean value",,"Operational"
2660.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)","Normals of monthly mean pressure, temperature, vapour pressure and sea/water temperature","010051","Pressure reduced to mean sea level",,,"Operational"
2661.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)","Normals of monthly mean pressure, temperature, vapour pressure and sea/water temperature","007032","Height of sensor above local ground (or deck of marine platform)","Temperature measurement","(see Note 3)","Operational"
2662.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)","Normals of monthly mean pressure, temperature, vapour pressure and sea/water temperature","007033","Height of sensor above water surface","Temperature measurement","(see Note 3)","Operational"
2663.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)","Normals of monthly mean pressure, temperature, vapour pressure and sea/water temperature","012101","Temperature/air temperature",,,"Operational"
2664.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)","Normals of monthly mean pressure, temperature, vapour pressure and sea/water temperature","013004","Vapour pressure",,,"Operational"
2665.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)","Normals of monthly mean pressure, temperature, vapour pressure and sea/water temperature","007032","Height of sensor above local ground (or deck of marine platform)","Set to missing (cancel)",,"Operational"
2666.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)","Normals of monthly mean pressure, temperature, vapour pressure and sea/water temperature","007033","Height of sensor above water surface","Set to missing (cancel)",,"Operational"
2667.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)","Normals of monthly mean pressure, temperature, vapour pressure and sea/water temperature","302056","Sea/water temperature","Sea-surface temperature, method of measurement, and depth below sea surface",,"Operational"
2668.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)","Normals of monthly mean pressure, temperature, vapour pressure and sea/water temperature","008023","First-order statistics","Set to missing",,"Operational"
2669.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)","Normals of monthly mean pressure, temperature, vapour pressure and sea/water temperature","004001","Year","Beginning of the reference period",,"Operational"
2670.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)","Normals of monthly mean pressure, temperature, vapour pressure and sea/water temperature","004001","Year","Ending of the reference period",,"Operational"
2671.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)","Normals of monthly mean pressure, temperature, vapour pressure and sea/water temperature","004002","Month",,,"Operational"
2672.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)","Normals of monthly mean pressure, temperature, vapour pressure and sea/water temperature","004003","Day","= 1","(see Note 2)","Operational"
2673.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)","Normals of monthly mean pressure, temperature, vapour pressure and sea/water temperature","004004","Hour","= 6","(see Note 2)","Operational"
2674.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)","Normals of monthly mean pressure, temperature, vapour pressure and sea/water temperature","004022","Time period or displacement","= 1",,"Operational"
2675.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)","Normals of precipitation","007032","Height of sensor above local ground (or deck of marine platform)","Precipitation measurement","(see Note 3)","Operational"
2676.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)","Normals of precipitation","008023","First-order statistics","= 4 Mean value",,"Operational"
2677.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)","Normals of precipitation","013060","Total accumulated precipitation",,,"Operational"
2678.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)","Normals of precipitation","004053","Number of days with precipitation equal to or more than 1 mm",,,"Operational"
2679.00,"08","Surface report sequences (sea)","308012","(Monthly normals from an ocean weather station)","Normals of precipitation","008023","First-order statistics","Set to missing",,"Operational"
2680.00,"08","Surface report sequences (sea)","308013","(Representation of CLIMAT SHIP data of the actual month and for monthly normals)",,"308011","Monthly values from an ocean weather station - CLIMAT SHIP",,,"Operational"
2681.00,"08","Surface report sequences (sea)","308013","(Representation of CLIMAT SHIP data of the actual month and for monthly normals)",,"308012","Monthly normals from an ocean weather station",,,"Operational"
2785.00,"09","Vertical sounding sequences (conventional data)","309001","(Vertical wind profile)",,"301037","Land station for vertical soundings","Identification, etc. (land station, high accuracy position)",,"Operational"
2786.00,"09","Vertical sounding sequences (conventional data)","309001","(Vertical wind profile)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
2787.00,"09","Vertical sounding sequences (conventional data)","309001","(Vertical wind profile)",,"031001","Delayed descriptor replication factor",,,"Operational"
2788.00,"09","Vertical sounding sequences (conventional data)","309001","(Vertical wind profile)",,"303011","Wind at height",,,"Operational"
2792.00,"09","Vertical sounding sequences (conventional data)","309002","(Vertical wind profile)",,"301038","Land station for vertical soundings","Identification, etc. (land station, coarse accuracy position)",,"Operational"
2793.00,"09","Vertical sounding sequences (conventional data)","309002","(Vertical wind profile)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
2794.00,"09","Vertical sounding sequences (conventional data)","309002","(Vertical wind profile)",,"031001","Delayed descriptor replication factor",,,"Operational"
2795.00,"09","Vertical sounding sequences (conventional data)","309002","(Vertical wind profile)",,"303011","Wind at height",,,"Operational"
2799.00,"09","Vertical sounding sequences (conventional data)","309003","(Vertical wind profile)",,"301037","Land station for vertical soundings","Identification, etc. (land station, high accuracy position)",,"Operational"
2800.00,"09","Vertical sounding sequences (conventional data)","309003","(Vertical wind profile)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
2801.00,"09","Vertical sounding sequences (conventional data)","309003","(Vertical wind profile)",,"031001","Delayed descriptor replication factor",,,"Operational"
2802.00,"09","Vertical sounding sequences (conventional data)","309003","(Vertical wind profile)",,"303012","Wind at pressure level",,,"Operational"
2806.00,"09","Vertical sounding sequences (conventional data)","309004","(Vertical wind profile)",,"301038","Land station for vertical soundings","Identification, etc. (land station, coarse accuracy position)",,"Operational"
2807.00,"09","Vertical sounding sequences (conventional data)","309004","(Vertical wind profile)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
2808.00,"09","Vertical sounding sequences (conventional data)","309004","(Vertical wind profile)",,"031001","Delayed descriptor replication factor",,,"Operational"
2809.00,"09","Vertical sounding sequences (conventional data)","309004","(Vertical wind profile)",,"303012","Wind at pressure level",,,"Operational"
2813.00,"09","Vertical sounding sequences (conventional data)","309005","(Vertical sounding with relative humidity)",,"301037","Land station for vertical soundings","Identification, etc. (land station, high accuracy position)",,"Operational"
2814.00,"09","Vertical sounding sequences (conventional data)","309005","(Vertical sounding with relative humidity)",,"302004","General cloud information","Significant cloud layer",,"Operational"
2815.00,"09","Vertical sounding sequences (conventional data)","309005","(Vertical sounding with relative humidity)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
2816.00,"09","Vertical sounding sequences (conventional data)","309005","(Vertical sounding with relative humidity)",,"031001","Delayed descriptor replication factor",,,"Operational"
2817.00,"09","Vertical sounding sequences (conventional data)","309005","(Vertical sounding with relative humidity)",,"303013","Geopotential, temperature, humidity, wind at pressure level",,,"Operational"
2822.00,"09","Vertical sounding sequences (conventional data)","309006","(Vertical sounding with relative humidity)",,"301038","Land station for vertical soundings","Identification, etc. (land station, coarse accuracy position)",,"Operational"
2823.00,"09","Vertical sounding sequences (conventional data)","309006","(Vertical sounding with relative humidity)",,"302004","General cloud information","Significant cloud layer",,"Operational"
2824.00,"09","Vertical sounding sequences (conventional data)","309006","(Vertical sounding with relative humidity)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
2825.00,"09","Vertical sounding sequences (conventional data)","309006","(Vertical sounding with relative humidity)",,"031001","Delayed descriptor replication factor",,,"Operational"
2826.00,"09","Vertical sounding sequences (conventional data)","309006","(Vertical sounding with relative humidity)",,"303013","Geopotential, temperature, humidity, wind at pressure level",,,"Operational"
2831.00,"09","Vertical sounding sequences (conventional data)","309007","(Vertical sounding with dewpoint data)",,"301037","Land station for vertical soundings","Identification, etc. (land station, high accuracy position)",,"Operational"
2832.00,"09","Vertical sounding sequences (conventional data)","309007","(Vertical sounding with dewpoint data)",,"302004","General cloud information","Significant cloud layer",,"Operational"
2833.00,"09","Vertical sounding sequences (conventional data)","309007","(Vertical sounding with dewpoint data)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
2834.00,"09","Vertical sounding sequences (conventional data)","309007","(Vertical sounding with dewpoint data)",,"031001","Delayed descriptor replication factor",,,"Operational"
2835.00,"09","Vertical sounding sequences (conventional data)","309007","(Vertical sounding with dewpoint data)",,"303014","Geopotential, temperature, dewpoint temperature, wind at pressure level",,,"Operational"
2840.00,"09","Vertical sounding sequences (conventional data)","309008","(Vertical sounding with dewpoint data)",,"301038","Land station for vertical soundings","Identification, etc. (land station, coarse accuracy position)",,"Operational"
2841.00,"09","Vertical sounding sequences (conventional data)","309008","(Vertical sounding with dewpoint data)",,"302004","General cloud information","Significant cloud layer",,"Operational"
2842.00,"09","Vertical sounding sequences (conventional data)","309008","(Vertical sounding with dewpoint data)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
2843.00,"09","Vertical sounding sequences (conventional data)","309008","(Vertical sounding with dewpoint data)",,"031001","Delayed descriptor replication factor",,,"Operational"
2844.00,"09","Vertical sounding sequences (conventional data)","309008","(Vertical sounding with dewpoint data)",,"303014","Geopotential, temperature, dewpoint temperature, wind at pressure level",,,"Operational"
2849.00,"09","Vertical sounding sequences (conventional data)","309011","(Vertical wind profile)",,"301039","Ship for vertical soundings","Ship's identification, etc.",,"Operational"
2850.00,"09","Vertical sounding sequences (conventional data)","309011","(Vertical wind profile)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
2851.00,"09","Vertical sounding sequences (conventional data)","309011","(Vertical wind profile)",,"031001","Delayed descriptor replication factor",,,"Operational"
2852.00,"09","Vertical sounding sequences (conventional data)","309011","(Vertical wind profile)",,"303011","Wind at height",,,"Operational"
2856.00,"09","Vertical sounding sequences (conventional data)","309012","(Vertical wind profile)",,"301039","Ship for vertical soundings","Ship's identification, etc.",,"Operational"
2857.00,"09","Vertical sounding sequences (conventional data)","309012","(Vertical wind profile)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
2858.00,"09","Vertical sounding sequences (conventional data)","309012","(Vertical wind profile)",,"031001","Delayed descriptor replication factor",,,"Operational"
2859.00,"09","Vertical sounding sequences (conventional data)","309012","(Vertical wind profile)",,"303012","Wind at pressure level",,,"Operational"
2863.00,"09","Vertical sounding sequences (conventional data)","309013","(Vertical sounding with relative humidity)",,"301039","Ship for vertical soundings","Ship's identification, etc.",,"Operational"
2864.00,"09","Vertical sounding sequences (conventional data)","309013","(Vertical sounding with relative humidity)",,"302004","General cloud information","Significant cloud layer",,"Operational"
2865.00,"09","Vertical sounding sequences (conventional data)","309013","(Vertical sounding with relative humidity)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
2866.00,"09","Vertical sounding sequences (conventional data)","309013","(Vertical sounding with relative humidity)",,"031001","Delayed descriptor replication factor",,,"Operational"
2867.00,"09","Vertical sounding sequences (conventional data)","309013","(Vertical sounding with relative humidity)",,"303013","Geopotential, temperature, humidity, wind at pressure level",,,"Operational"
2872.00,"09","Vertical sounding sequences (conventional data)","309014","(Vertical sounding with dewpoint data)",,"301039","Ship for vertical soundings","Ship's identification, etc.",,"Operational"
2873.00,"09","Vertical sounding sequences (conventional data)","309014","(Vertical sounding with dewpoint data)",,"302004","General cloud information","Significant cloud layer",,"Operational"
2874.00,"09","Vertical sounding sequences (conventional data)","309014","(Vertical sounding with dewpoint data)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
2875.00,"09","Vertical sounding sequences (conventional data)","309014","(Vertical sounding with dewpoint data)",,"031001","Delayed descriptor replication factor",,,"Operational"
2876.00,"09","Vertical sounding sequences (conventional data)","309014","(Vertical sounding with dewpoint data)",,"303014","Geopotential, temperature, dewpoint temperature, wind at pressure level",,,"Operational"
2881.00,"09","Vertical sounding sequences (conventional data)","309015","(Vertical wind profile)",,"301040","Ship for vertical soundings","Ship's identification, etc.",,"Operational"
2882.00,"09","Vertical sounding sequences (conventional data)","309015","(Vertical wind profile)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
2883.00,"09","Vertical sounding sequences (conventional data)","309015","(Vertical wind profile)",,"031001","Delayed descriptor replication factor",,,"Operational"
2884.00,"09","Vertical sounding sequences (conventional data)","309015","(Vertical wind profile)",,"303011","Wind at height",,,"Operational"
2888.00,"09","Vertical sounding sequences (conventional data)","309016","(Vertical wind profile)",,"301040","Ship for vertical soundings","Ship's identification, etc.",,"Operational"
2889.00,"09","Vertical sounding sequences (conventional data)","309016","(Vertical wind profile)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
2890.00,"09","Vertical sounding sequences (conventional data)","309016","(Vertical wind profile)",,"031001","Delayed descriptor replication factor",,,"Operational"
2891.00,"09","Vertical sounding sequences (conventional data)","309016","(Vertical wind profile)",,"303012","Wind at pressure level",,,"Operational"
2895.00,"09","Vertical sounding sequences (conventional data)","309017","(Vertical sounding with relative humidity)",,"301040","Ship for vertical soundings","Ship's identification, etc.",,"Operational"
2896.00,"09","Vertical sounding sequences (conventional data)","309017","(Vertical sounding with relative humidity)",,"302004","General cloud information","Significant cloud layer",,"Operational"
2897.00,"09","Vertical sounding sequences (conventional data)","309017","(Vertical sounding with relative humidity)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
2898.00,"09","Vertical sounding sequences (conventional data)","309017","(Vertical sounding with relative humidity)",,"031001","Delayed descriptor replication factor",,,"Operational"
2899.00,"09","Vertical sounding sequences (conventional data)","309017","(Vertical sounding with relative humidity)",,"303013","Geopotential, temperature, humidity, wind at pressure level",,,"Operational"
2904.00,"09","Vertical sounding sequences (conventional data)","309018","(Vertical sounding with dewpoint data)",,"301040","Ship for vertical soundings","Ship's identification, etc.",,"Operational"
2905.00,"09","Vertical sounding sequences (conventional data)","309018","(Vertical sounding with dewpoint data)",,"302004","General cloud information","Significant cloud layer",,"Operational"
2906.00,"09","Vertical sounding sequences (conventional data)","309018","(Vertical sounding with dewpoint data)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
2907.00,"09","Vertical sounding sequences (conventional data)","309018","(Vertical sounding with dewpoint data)",,"031001","Delayed descriptor replication factor",,,"Operational"
2908.00,"09","Vertical sounding sequences (conventional data)","309018","(Vertical sounding with dewpoint data)",,"303014","Geopotential, temperature, dewpoint temperature, wind at pressure level",,,"Operational"
2913.00,"09","Vertical sounding sequences (conventional data)","309019","(Wind profiler - wind data sounding)",,"301031","Identification and type of station, date/time, location (high accuracy), height of station",,,"Operational"
2914.00,"09","Vertical sounding sequences (conventional data)","309019","(Wind profiler - wind data sounding)",,"002003","Type of measuring equipment used",,,"Operational"
2915.00,"09","Vertical sounding sequences (conventional data)","309019","(Wind profiler - wind data sounding)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
2916.00,"09","Vertical sounding sequences (conventional data)","309019","(Wind profiler - wind data sounding)",,"031001","Delayed descriptor replication factor",,,"Operational"
2917.00,"09","Vertical sounding sequences (conventional data)","309019","(Wind profiler - wind data sounding)",,"303011","Wind at height",,,"Operational"
2922.00,"09","Vertical sounding sequences (conventional data)","309020","(Wind profiler - Cartesian coordinates)",,"301031","Identification and type of station, date/time, location (high accuracy), height of station",,,"Operational"
2923.00,"09","Vertical sounding sequences (conventional data)","309020","(Wind profiler - Cartesian coordinates)",,"002003","Type of measuring equipment used",,,"Operational"
2924.00,"09","Vertical sounding sequences (conventional data)","309020","(Wind profiler - Cartesian coordinates)",,"104000","Delayed replication of 4 descriptors",,,"Operational"
2925.00,"09","Vertical sounding sequences (conventional data)","309020","(Wind profiler - Cartesian coordinates)",,"031001","Delayed descriptor replication factor",,,"Operational"
2926.00,"09","Vertical sounding sequences (conventional data)","309020","(Wind profiler - Cartesian coordinates)",,"007003","Geopotential",,,"Operational"
2927.00,"09","Vertical sounding sequences (conventional data)","309020","(Wind profiler - Cartesian coordinates)",,"011003","u-component",,,"Operational"
2928.00,"09","Vertical sounding sequences (conventional data)","309020","(Wind profiler - Cartesian coordinates)",,"011004","v-component",,,"Operational"
2929.00,"09","Vertical sounding sequences (conventional data)","309020","(Wind profiler - Cartesian coordinates)",,"011005","w-component",,,"Operational"
2937.00,"09","Vertical sounding sequences (conventional data)","309030","(Ozone sonde flight data)",,"015004","Ozone sounding correction factor (CF)",,"<(see Note 1)>","Operational"
2938.00,"09","Vertical sounding sequences (conventional data)","309030","(Ozone sonde flight data)",,"015005","Ozone p",,,"Operational"
2939.00,"09","Vertical sounding sequences (conventional data)","309030","(Ozone sonde flight data)",,"104000","Delayed replication of 4 descriptors",,,"Operational"
2940.00,"09","Vertical sounding sequences (conventional data)","309030","(Ozone sonde flight data)",,"031001","Delayed descriptor replication factor",,,"Operational"
2941.00,"09","Vertical sounding sequences (conventional data)","309030","(Ozone sonde flight data)",,"004015","Time increment","Since launch time, if needed, in minutes",,"Operational"
2942.00,"09","Vertical sounding sequences (conventional data)","309030","(Ozone sonde flight data)",,"008006","Ozone vertical sounding significance",,,"Operational"
2943.00,"09","Vertical sounding sequences (conventional data)","309030","(Ozone sonde flight data)",,"007004","Pressure",,,"Operational"
2944.00,"09","Vertical sounding sequences (conventional data)","309030","(Ozone sonde flight data)",,"015003","Measured ozone partial pressure (sounding)",,,"Operational"
2952.00,"09","Vertical sounding sequences (conventional data)","309031","(Ozone sonde flight data)",,"015004","Ozone sounding correction factor (CF)",,,"Operational"
2953.00,"09","Vertical sounding sequences (conventional data)","309031","(Ozone sonde flight data)",,"015005","Ozone p",,,"Operational"
2954.00,"09","Vertical sounding sequences (conventional data)","309031","(Ozone sonde flight data)",,"104000","Delayed replication of 4 descriptors",,,"Operational"
2955.00,"09","Vertical sounding sequences (conventional data)","309031","(Ozone sonde flight data)",,"031001","Delayed descriptor replication factor",,,"Operational"
2956.00,"09","Vertical sounding sequences (conventional data)","309031","(Ozone sonde flight data)",,"004025","Time period or displacement","Since launch time in minutes",,"Operational"
2957.00,"09","Vertical sounding sequences (conventional data)","309031","(Ozone sonde flight data)",,"008006","Ozone vertical sounding significance",,,"Operational"
2958.00,"09","Vertical sounding sequences (conventional data)","309031","(Ozone sonde flight data)",,"007004","Pressure",,,"Operational"
2959.00,"09","Vertical sounding sequences (conventional data)","309031","(Ozone sonde flight data)",,"015003","Measured ozone partial pressure (sounding)",,,"Operational"
2967.00,"09","Vertical sounding sequences (conventional data)","309040","(Ozone sounding not coupled to a ground-based spectrophotometer)",,"301075","Sounding identification",,"<(see Note 2)>","Operational"
2968.00,"09","Vertical sounding sequences (conventional data)","309040","(Ozone sounding not coupled to a ground-based spectrophotometer)",,"301076","Ozone sounding instrumentation",,,"Operational"
2969.00,"09","Vertical sounding sequences (conventional data)","309040","(Ozone sounding not coupled to a ground-based spectrophotometer)",,"309030","Ozone sonde flight data",,,"Operational"
2970.00,"09","Vertical sounding sequences (conventional data)","309041","(Ozone sounding coupled to measurements from a Brewer ground-based spectrophotometer; the total ozone obtained from the Brewer is a single value)",,"307041","Total ozone measurement from a Brewer ground-based spectrophotometer obtained from a single observation","Description of the ground-based part","<(see Note 2)>","Operational"
2971.00,"09","Vertical sounding sequences (conventional data)","309041","(Ozone sounding coupled to measurements from a Brewer ground-based spectrophotometer; the total ozone obtained from the Brewer is a single value)",,"301075","Sounding identification","Identification of the ozone sounding part",,"Operational"
2972.00,"09","Vertical sounding sequences (conventional data)","309041","(Ozone sounding coupled to measurements from a Brewer ground-based spectrophotometer; the total ozone obtained from the Brewer is a single value)",,"301076","Ozone sounding instrumentation",,,"Operational"
2973.00,"09","Vertical sounding sequences (conventional data)","309041","(Ozone sounding coupled to measurements from a Brewer ground-based spectrophotometer; the total ozone obtained from the Brewer is a single value)",,"309030","Ozone sonde flight data",,,"Operational"
2974.00,"09","Vertical sounding sequences (conventional data)","309042","(Ozone sounding coupled to measurements from a Brewer ground-based spectrophotometer; the total ozone obtained from the Brewer is an averaged value)",,"307042","Total ozone measurement from a Brewer ground-based spectrophotometer obtained from averaged observations","Description of the ground-based part","<(see Note 2)>","Operational"
2975.00,"09","Vertical sounding sequences (conventional data)","309042","(Ozone sounding coupled to measurements from a Brewer ground-based spectrophotometer; the total ozone obtained from the Brewer is an averaged value)",,"301075","Sounding identification","Identification of the ozone sounding part",,"Operational"
2976.00,"09","Vertical sounding sequences (conventional data)","309042","(Ozone sounding coupled to measurements from a Brewer ground-based spectrophotometer; the total ozone obtained from the Brewer is an averaged value)",,"301076","Ozone sounding instrumentation",,,"Operational"
2977.00,"09","Vertical sounding sequences (conventional data)","309042","(Ozone sounding coupled to measurements from a Brewer ground-based spectrophotometer; the total ozone obtained from the Brewer is an averaged value)",,"309030","Ozone sonde flight data",,,"Operational"
2978.00,"09","Vertical sounding sequences (conventional data)","309043","(Ozone sounding coupled to measurements from a Dobson ground-based spectrophotometer; the total ozone obtained from the Dobson is a single value)",,"307043","Total ozone measurement from a Dobson ground-based spectrophotometer obtained from a single observation","Description of the ground-based part","<(see Note 2)>","Operational"
2979.00,"09","Vertical sounding sequences (conventional data)","309043","(Ozone sounding coupled to measurements from a Dobson ground-based spectrophotometer; the total ozone obtained from the Dobson is a single value)",,"301075","Sounding identification","Identification of the ozone sounding part",,"Operational"
2980.00,"09","Vertical sounding sequences (conventional data)","309043","(Ozone sounding coupled to measurements from a Dobson ground-based spectrophotometer; the total ozone obtained from the Dobson is a single value)",,"301076","Ozone sounding instrumentation",,,"Operational"
2981.00,"09","Vertical sounding sequences (conventional data)","309043","(Ozone sounding coupled to measurements from a Dobson ground-based spectrophotometer; the total ozone obtained from the Dobson is a single value)",,"309030","Ozone sonde flight data",,,"Operational"
2982.00,"09","Vertical sounding sequences (conventional data)","309044","(Ozone sounding coupled to measurements from a Dobson ground-based spectrophotometer; the total ozone obtained from the Dobson is an averaged value)",,"307044","Total ozone measurement from a Dobson ground-based spectrophotometer obtained from averaged observations","Description of the ground-based part","<(see Note 2)>","Operational"
2983.00,"09","Vertical sounding sequences (conventional data)","309044","(Ozone sounding coupled to measurements from a Dobson ground-based spectrophotometer; the total ozone obtained from the Dobson is an averaged value)",,"301075","Sounding identification","Identification of the ozone sounding part",,"Operational"
2984.00,"09","Vertical sounding sequences (conventional data)","309044","(Ozone sounding coupled to measurements from a Dobson ground-based spectrophotometer; the total ozone obtained from the Dobson is an averaged value)",,"301076","Ozone sounding instrumentation",,,"Operational"
2985.00,"09","Vertical sounding sequences (conventional data)","309044","(Ozone sounding coupled to measurements from a Dobson ground-based spectrophotometer; the total ozone obtained from the Dobson is an averaged value)",,"309030","Ozone sonde flight data",,,"Operational"
2986.00,"09","Vertical sounding sequences (conventional data)","309045","(Ozone sounding not coupled to a ground-based spectrophotometer)",,"301075","Sounding identification",,,"Operational"
2987.00,"09","Vertical sounding sequences (conventional data)","309045","(Ozone sounding not coupled to a ground-based spectrophotometer)",,"301076","Ozone sounding instrumentation",,,"Operational"
2988.00,"09","Vertical sounding sequences (conventional data)","309045","(Ozone sounding not coupled to a ground-based spectrophotometer)",,"309031","Ozone sonde flight data",,,"Operational"
2989.00,"09","Vertical sounding sequences (conventional data)","309046","(Ozone sounding coupled to measurements from a Brewer ground-based spectrophotometer; the total ozone obtained from the Brewer is a single value)",,"307041","Total ozone measurement from a Brewer ground-based spectrophotometer obtained from a single observation","Description of the ground-based part",,"Operational"
2990.00,"09","Vertical sounding sequences (conventional data)","309046","(Ozone sounding coupled to measurements from a Brewer ground-based spectrophotometer; the total ozone obtained from the Brewer is a single value)",,"301075","Sounding identification","Identification of the ozone sounding part",,"Operational"
2991.00,"09","Vertical sounding sequences (conventional data)","309046","(Ozone sounding coupled to measurements from a Brewer ground-based spectrophotometer; the total ozone obtained from the Brewer is a single value)",,"301076","Ozone sounding instrumentation",,,"Operational"
2992.00,"09","Vertical sounding sequences (conventional data)","309046","(Ozone sounding coupled to measurements from a Brewer ground-based spectrophotometer; the total ozone obtained from the Brewer is a single value)",,"309031","Ozone sonde flight data",,,"Operational"
2993.00,"09","Vertical sounding sequences (conventional data)","309047","(Ozone sounding coupled to measurements from a Brewer ground-based spectrophotometer; the total ozone obtained from the Brewer is an averaged value)",,"307042","Total ozone measurement from a Brewer ground-based spectrophotometer obtained from averaged observations","Description of the ground-based part",,"Operational"
2994.00,"09","Vertical sounding sequences (conventional data)","309047","(Ozone sounding coupled to measurements from a Brewer ground-based spectrophotometer; the total ozone obtained from the Brewer is an averaged value)",,"301075","Sounding identification","Identification of the ozone sounding part",,"Operational"
2995.00,"09","Vertical sounding sequences (conventional data)","309047","(Ozone sounding coupled to measurements from a Brewer ground-based spectrophotometer; the total ozone obtained from the Brewer is an averaged value)",,"301076","Ozone sounding instrumentation",,,"Operational"
2996.00,"09","Vertical sounding sequences (conventional data)","309047","(Ozone sounding coupled to measurements from a Brewer ground-based spectrophotometer; the total ozone obtained from the Brewer is an averaged value)",,"309031","Ozone sonde flight data",,,"Operational"
2997.00,"09","Vertical sounding sequences (conventional data)","309048","(Ozone sounding coupled to measurements from a Dobson ground-based spectrophotometer; the total ozone obtained from the Dobson is a single value)",,"307043","Total ozone measurement from a Dobson ground-based spectrophotometer obtained from a single observation","Description of the ground-based part",,"Operational"
2998.00,"09","Vertical sounding sequences (conventional data)","309048","(Ozone sounding coupled to measurements from a Dobson ground-based spectrophotometer; the total ozone obtained from the Dobson is a single value)",,"301075","Sounding identification","Identification of the ozone sounding part",,"Operational"
2999.00,"09","Vertical sounding sequences (conventional data)","309048","(Ozone sounding coupled to measurements from a Dobson ground-based spectrophotometer; the total ozone obtained from the Dobson is a single value)",,"301076","Ozone sounding instrumentation",,,"Operational"
3000.00,"09","Vertical sounding sequences (conventional data)","309048","(Ozone sounding coupled to measurements from a Dobson ground-based spectrophotometer; the total ozone obtained from the Dobson is a single value)",,"309031","Ozone sonde flight data",,,"Operational"
3001.00,"09","Vertical sounding sequences (conventional data)","309049","(Ozone sounding coupled to measurements from a Dobson ground-based spectrophotometer; the total ozone obtained from the Dobson is an averaged value)",,"307044","Total ozone measurement from a Dobson ground-based spectrophotometer obtained from averaged observations","Description of the ground-based part",,"Operational"
3002.00,"09","Vertical sounding sequences (conventional data)","309049","(Ozone sounding coupled to measurements from a Dobson ground-based spectrophotometer; the total ozone obtained from the Dobson is an averaged value)",,"301075","Sounding identification","Identification of the ozone sounding part",,"Operational"
3003.00,"09","Vertical sounding sequences (conventional data)","309049","(Ozone sounding coupled to measurements from a Dobson ground-based spectrophotometer; the total ozone obtained from the Dobson is an averaged value)",,"301076","Ozone sounding instrumentation",,,"Operational"
3004.00,"09","Vertical sounding sequences (conventional data)","309049","(Ozone sounding coupled to measurements from a Dobson ground-based spectrophotometer; the total ozone obtained from the Dobson is an averaged value)",,"309031","Ozone sonde flight data",,,"Operational"
3005.00,"09","Vertical sounding sequences (conventional data)","309050","(Sequence for representation of PILOT, PILOT SHIP and PILOT MOBIL observation type data with pressure as the vertical coordinate)",,"301110","Identification of launch site and instrumentation for wind measurements",,,"Operational"
3006.00,"09","Vertical sounding sequences (conventional data)","309050","(Sequence for representation of PILOT, PILOT SHIP and PILOT MOBIL observation type data with pressure as the vertical coordinate)",,"301113","Date/time of launch",,,"Operational"
3007.00,"09","Vertical sounding sequences (conventional data)","309050","(Sequence for representation of PILOT, PILOT SHIP and PILOT MOBIL observation type data with pressure as the vertical coordinate)",,"301114","Horizontal and vertical coordinates of launch site",,,"Operational"
3008.00,"09","Vertical sounding sequences (conventional data)","309050","(Sequence for representation of PILOT, PILOT SHIP and PILOT MOBIL observation type data with pressure as the vertical coordinate)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
3009.00,"09","Vertical sounding sequences (conventional data)","309050","(Sequence for representation of PILOT, PILOT SHIP and PILOT MOBIL observation type data with pressure as the vertical coordinate)",,"031002","Extended delayed descriptor replication factor",,,"Operational"
3010.00,"09","Vertical sounding sequences (conventional data)","309050","(Sequence for representation of PILOT, PILOT SHIP and PILOT MOBIL observation type data with pressure as the vertical coordinate)",,"303050","Wind data at a pressure level with radiosonde position",,,"Operational"
3011.00,"09","Vertical sounding sequences (conventional data)","309050","(Sequence for representation of PILOT, PILOT SHIP and PILOT MOBIL observation type data with pressure as the vertical coordinate)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
3012.00,"09","Vertical sounding sequences (conventional data)","309050","(Sequence for representation of PILOT, PILOT SHIP and PILOT MOBIL observation type data with pressure as the vertical coordinate)",,"031001","Delayed descriptor replication factor",,,"Operational"
3013.00,"09","Vertical sounding sequences (conventional data)","309050","(Sequence for representation of PILOT, PILOT SHIP and PILOT MOBIL observation type data with pressure as the vertical coordinate)",,"303051","Wind shear data at a pressure level with radiosonde position",,,"Operational"
3015.00,"09","Vertical sounding sequences (conventional data)","309051","(Sequence for representation of PILOT, PILOT SHIP and PILOT MOBIL observation type data with height as the vertical coordinate)",,"301110","Identification of launch site and instrumentation for wind measurements",,,"Operational"
3016.00,"09","Vertical sounding sequences (conventional data)","309051","(Sequence for representation of PILOT, PILOT SHIP and PILOT MOBIL observation type data with height as the vertical coordinate)",,"301113","Date/time of launch",,,"Operational"
3017.00,"09","Vertical sounding sequences (conventional data)","309051","(Sequence for representation of PILOT, PILOT SHIP and PILOT MOBIL observation type data with height as the vertical coordinate)",,"301114","Horizontal and vertical coordinates of launch site",,,"Operational"
3018.00,"09","Vertical sounding sequences (conventional data)","309051","(Sequence for representation of PILOT, PILOT SHIP and PILOT MOBIL observation type data with height as the vertical coordinate)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
3019.00,"09","Vertical sounding sequences (conventional data)","309051","(Sequence for representation of PILOT, PILOT SHIP and PILOT MOBIL observation type data with height as the vertical coordinate)",,"031002","Extended delayed descriptor replication factor",,,"Operational"
3020.00,"09","Vertical sounding sequences (conventional data)","309051","(Sequence for representation of PILOT, PILOT SHIP and PILOT MOBIL observation type data with height as the vertical coordinate)",,"303052","Wind data at a height level with radiosonde position",,,"Operational"
3021.00,"09","Vertical sounding sequences (conventional data)","309051","(Sequence for representation of PILOT, PILOT SHIP and PILOT MOBIL observation type data with height as the vertical coordinate)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
3022.00,"09","Vertical sounding sequences (conventional data)","309051","(Sequence for representation of PILOT, PILOT SHIP and PILOT MOBIL observation type data with height as the vertical coordinate)",,"031001","Delayed descriptor replication factor",,,"Operational"
3023.00,"09","Vertical sounding sequences (conventional data)","309051","(Sequence for representation of PILOT, PILOT SHIP and PILOT MOBIL observation type data with height as the vertical coordinate)",,"303053","Wind shear data at a height level with radiosonde position",,,"Operational"
3025.00,"09","Vertical sounding sequences (conventional data)","309052","(Sequence for representation of TEMP, TEMP SHIP and TEMP MOBIL observation type data)",,"301111","Identification of launch site and instrumentation for P, T, U and wind measurements",,,"Operational"
3026.00,"09","Vertical sounding sequences (conventional data)","309052","(Sequence for representation of TEMP, TEMP SHIP and TEMP MOBIL observation type data)",,"301113","Date/time of launch",,,"Operational"
3027.00,"09","Vertical sounding sequences (conventional data)","309052","(Sequence for representation of TEMP, TEMP SHIP and TEMP MOBIL observation type data)",,"301114","Horizontal and vertical coordinates of launch site",,,"Operational"
3028.00,"09","Vertical sounding sequences (conventional data)","309052","(Sequence for representation of TEMP, TEMP SHIP and TEMP MOBIL observation type data)",,"302049","Cloud information reported with vertical soundings",,,"Operational"
3029.00,"09","Vertical sounding sequences (conventional data)","309052","(Sequence for representation of TEMP, TEMP SHIP and TEMP MOBIL observation type data)",,"022043","Sea/water temperature",,,"Operational"
3030.00,"09","Vertical sounding sequences (conventional data)","309052","(Sequence for representation of TEMP, TEMP SHIP and TEMP MOBIL observation type data)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
3031.00,"09","Vertical sounding sequences (conventional data)","309052","(Sequence for representation of TEMP, TEMP SHIP and TEMP MOBIL observation type data)",,"031002","Extended delayed descriptor replication factor",,,"Operational"
3032.00,"09","Vertical sounding sequences (conventional data)","309052","(Sequence for representation of TEMP, TEMP SHIP and TEMP MOBIL observation type data)",,"303054","Temperature, dewpoint and wind data at a pressure level with radiosonde position",,,"Operational"
3033.00,"09","Vertical sounding sequences (conventional data)","309052","(Sequence for representation of TEMP, TEMP SHIP and TEMP MOBIL observation type data)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
3034.00,"09","Vertical sounding sequences (conventional data)","309052","(Sequence for representation of TEMP, TEMP SHIP and TEMP MOBIL observation type data)",,"031001","Delayed descriptor replication factor",,,"Operational"
3035.00,"09","Vertical sounding sequences (conventional data)","309052","(Sequence for representation of TEMP, TEMP SHIP and TEMP MOBIL observation type data)",,"303051","Wind shear data at a pressure level with radiosonde position",,,"Operational"
3037.00,"09","Vertical sounding sequences (conventional data)","309053","(Sequence for representation of TEMP DROP observation type data)",,"301112","Identification of launch point and instrumentation of dropsonde",,,"Operational"
3038.00,"09","Vertical sounding sequences (conventional data)","309053","(Sequence for representation of TEMP DROP observation type data)",,"301113","Date/time of launch",,,"Operational"
3039.00,"09","Vertical sounding sequences (conventional data)","309053","(Sequence for representation of TEMP DROP observation type data)",,"301114","Horizontal and vertical coordinates of launch site",,,"Operational"
3040.00,"09","Vertical sounding sequences (conventional data)","309053","(Sequence for representation of TEMP DROP observation type data)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
3041.00,"09","Vertical sounding sequences (conventional data)","309053","(Sequence for representation of TEMP DROP observation type data)",,"031002","Extended delayed descriptor replication factor",,,"Operational"
3042.00,"09","Vertical sounding sequences (conventional data)","309053","(Sequence for representation of TEMP DROP observation type data)",,"303054","Temperature, dewpoint and wind data at a pressure level with radiosonde position",,,"Operational"
3043.00,"09","Vertical sounding sequences (conventional data)","309053","(Sequence for representation of TEMP DROP observation type data)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
3044.00,"09","Vertical sounding sequences (conventional data)","309053","(Sequence for representation of TEMP DROP observation type data)",,"031001","Delayed descriptor replication factor",,,"Operational"
3045.00,"09","Vertical sounding sequences (conventional data)","309053","(Sequence for representation of TEMP DROP observation type data)",,"303051","Wind shear data at a pressure level with radiosonde position",,,"Operational"
3047.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)",,"301001","WMO block and station numbers","Identification of launch site",,"Operational"
3048.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)",,"001011","Ship or mobile land station identifier","Ship's call sign",,"Operational"
3049.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)",,"301011","Year, month, day",,,"Operational"
3050.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)",,"301012","Hour, minute",,,"Operational"
3051.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)",,"301021","Latitude/longitude (high accuracy)",,,"Operational"
3052.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)",,"007030","Height of station ground above mean sea level",,,"Operational"
3053.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)",,"007031","Height of barometer above mean sea level",,,"Operational"
3054.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)",,"007007","Height","Release of sonde above mean sea level",,"Operational"
3055.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)","Monthly mean data","004023","Time period or displacement","Number of days in the month",,"Operational"
3056.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)","Monthly mean data","004059","Times of observation used to compute the reported mean values",,,"Operational"
3057.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)","Monthly mean data","115000","Delayed replication of 15 descriptors",,,"Operational"
3058.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)","Monthly mean data","031001","Delayed descriptor replication factor",,,"Operational"
3059.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)","Monthly mean data","008001","Vertical sounding significance",,,"Operational"
3060.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)","Monthly mean data","008023","First-order statistics","= 4 Mean value",,"Operational"
3061.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)","Monthly mean data","007004","Pressure",,,"Operational"
3062.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)","Monthly mean data","010009","Geopotential height",,,"Operational"
3063.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)","Monthly mean data","012101","Temperature/air temperature",,,"Operational"
3064.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)","Monthly mean data","012103","Dewpoint temperature",,,"Operational"
3065.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)","Monthly mean data","008023","First-order statistics","= 32 Vector mean",,"Operational"
3066.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)","Monthly mean data","011001","Wind direction",,,"Operational"
3067.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)","Monthly mean data","011002","Wind speed",,,"Operational"
3068.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)","Monthly mean data","008023","First-order statistics","Set to missing",,"Operational"
3069.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)","Monthly mean data","011019","Steadiness of wind",,,"Operational"
3070.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)","Monthly mean data","008050","Qualifier for number of missing values in calculation of statistic","= 2 Temperature",,"Operational"
3071.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)","Monthly mean data","008020","Total number of missing entities (with respect to accumulation or average)","Days",,"Operational"
3072.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)","Monthly mean data","008050","Qualifier for number of missing values in calculation of statistic","= 9 Wind",,"Operational"
3073.00,"09","Vertical sounding sequences (conventional data)","309054","(Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data)","Monthly mean data","008020","Total number of missing entities (with respect to accumulation or average)","Days",,"Operational"
3075.00,"09","Vertical sounding sequences (conventional data)","309055","(Template for the representation of high resolution radiosonde data with geopotential height as the vertical coordinate)",,"301111","Identification of launch site and instrumentation for P, T, U and wind measurements",,,"Operational"
3076.00,"09","Vertical sounding sequences (conventional data)","309055","(Template for the representation of high resolution radiosonde data with geopotential height as the vertical coordinate)",,"025061","Software identification and version number",,,"Operational"
3077.00,"09","Vertical sounding sequences (conventional data)","309055","(Template for the representation of high resolution radiosonde data with geopotential height as the vertical coordinate)",,"001081","Radiosonde serial number",,,"Operational"
3078.00,"09","Vertical sounding sequences (conventional data)","309055","(Template for the representation of high resolution radiosonde data with geopotential height as the vertical coordinate)",,"001082","Radiosonde ascension number",,,"Operational"
3079.00,"09","Vertical sounding sequences (conventional data)","309055","(Template for the representation of high resolution radiosonde data with geopotential height as the vertical coordinate)",,"002067","Radiosonde operating frequency",,,"Operational"
3080.00,"09","Vertical sounding sequences (conventional data)","309055","(Template for the representation of high resolution radiosonde data with geopotential height as the vertical coordinate)",,"002095","Type of pressure sensor",,,"Operational"
3081.00,"09","Vertical sounding sequences (conventional data)","309055","(Template for the representation of high resolution radiosonde data with geopotential height as the vertical coordinate)",,"002096","Type of temperature sensor",,,"Operational"
3082.00,"09","Vertical sounding sequences (conventional data)","309055","(Template for the representation of high resolution radiosonde data with geopotential height as the vertical coordinate)",,"002097","Type of humidity sensor",,,"Operational"
3083.00,"09","Vertical sounding sequences (conventional data)","309055","(Template for the representation of high resolution radiosonde data with geopotential height as the vertical coordinate)",,"002081","Type of balloon",,,"Operational"
3084.00,"09","Vertical sounding sequences (conventional data)","309055","(Template for the representation of high resolution radiosonde data with geopotential height as the vertical coordinate)",,"002082","Weight of balloon",,,"Operational"
3085.00,"09","Vertical sounding sequences (conventional data)","309055","(Template for the representation of high resolution radiosonde data with geopotential height as the vertical coordinate)",,"002084","Type of gas used in balloon",,,"Operational"
3086.00,"09","Vertical sounding sequences (conventional data)","309055","(Template for the representation of high resolution radiosonde data with geopotential height as the vertical coordinate)",,"002191","Geopotential height calculation",,,"Operational"
3087.00,"09","Vertical sounding sequences (conventional data)","309055","(Template for the representation of high resolution radiosonde data with geopotential height as the vertical coordinate)",,"301113","Date/time of launch",,"(see Note 6)","Operational"
3088.00,"09","Vertical sounding sequences (conventional data)","309055","(Template for the representation of high resolution radiosonde data with geopotential height as the vertical coordinate)",,"301114","Horizontal and vertical coordinates of launch site",,,"Operational"
3089.00,"09","Vertical sounding sequences (conventional data)","309055","(Template for the representation of high resolution radiosonde data with geopotential height as the vertical coordinate)",,"010004","Pressure",,,"Operational"
3090.00,"09","Vertical sounding sequences (conventional data)","309055","(Template for the representation of high resolution radiosonde data with geopotential height as the vertical coordinate)",,"302032","Temperature and humidity data",,,"Operational"
3091.00,"09","Vertical sounding sequences (conventional data)","309055","(Template for the representation of high resolution radiosonde data with geopotential height as the vertical coordinate)",,"007032","Height of sensor above local ground (or deck of marine platform)",,,"Operational"
3092.00,"09","Vertical sounding sequences (conventional data)","309055","(Template for the representation of high resolution radiosonde data with geopotential height as the vertical coordinate)",,"002002","Type of instrumentation for wind measurement",,,"Operational"
3093.00,"09","Vertical sounding sequences (conventional data)","309055","(Template for the representation of high resolution radiosonde data with geopotential height as the vertical coordinate)",,"011001","Wind direction",,,"Operational"
3094.00,"09","Vertical sounding sequences (conventional data)","309055","(Template for the representation of high resolution radiosonde data with geopotential height as the vertical coordinate)",,"011002","Wind speed",,,"Operational"
3095.00,"09","Vertical sounding sequences (conventional data)","309055","(Template for the representation of high resolution radiosonde data with geopotential height as the vertical coordinate)",,"007032","Height of sensor above local ground (or deck of marine platform)","Set to missing (cancel)",,"Operational"
3096.00,"09","Vertical sounding sequences (conventional data)","309055","(Template for the representation of high resolution radiosonde data with geopotential height as the vertical coordinate)",,"020003","Present weather",,,"Operational"
3097.00,"09","Vertical sounding sequences (conventional data)","309055","(Template for the representation of high resolution radiosonde data with geopotential height as the vertical coordinate)",,"302049","Cloud information reported with vertical soundings",,,"Operational"
3098.00,"09","Vertical sounding sequences (conventional data)","309055","(Template for the representation of high resolution radiosonde data with geopotential height as the vertical coordinate)",,"022043","Sea/water temperature",,,"Operational"
3099.00,"09","Vertical sounding sequences (conventional data)","309055","(Template for the representation of high resolution radiosonde data with geopotential height as the vertical coordinate)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
3100.00,"09","Vertical sounding sequences (conventional data)","309055","(Template for the representation of high resolution radiosonde data with geopotential height as the vertical coordinate)",,"031002","Extended delayed descriptor replication factor",,,"Operational"
3101.00,"09","Vertical sounding sequences (conventional data)","309055","(Template for the representation of high resolution radiosonde data with geopotential height as the vertical coordinate)",,"303055","Temperature, dewpoint, relative humidity and wind data at a height level with radiosonde position",,"(see Notes 7, 8 and 9)","Operational"
3103.00,"09","Vertical sounding sequences (conventional data)","309060","(Radiosonde complete registration and surface observation)",,"301123","Radiosonde full header information",,,"Operational"
3104.00,"09","Vertical sounding sequences (conventional data)","309060","(Radiosonde complete registration and surface observation)",,"301121","Radiosonde launch point location",,,"Operational"
3105.00,"09","Vertical sounding sequences (conventional data)","309060","(Radiosonde complete registration and surface observation)",,"302050","Radiosonde surface observation",,,"Operational"
3106.00,"09","Vertical sounding sequences (conventional data)","309060","(Radiosonde complete registration and surface observation)",,"303040","Radiosonde duration of flight and termination information",,,"Operational"
3107.00,"09","Vertical sounding sequences (conventional data)","309061","(Raw PTU)",,"301120","Radiosonde abbreviated header and launch information",,,"Operational"
3108.00,"09","Vertical sounding sequences (conventional data)","309061","(Raw PTU)",,"008041","Data significance","= 6 Flight level observation",,"Operational"
3109.00,"09","Vertical sounding sequences (conventional data)","309061","(Raw PTU)",,"301122","Date/time (to hundredths of second)",,,"Operational"
3110.00,"09","Vertical sounding sequences (conventional data)","309061","(Raw PTU)",,"201131","Change data width",,,"Operational"
3111.00,"09","Vertical sounding sequences (conventional data)","309061","(Raw PTU)",,"202129","Change scale",,,"Operational"
3112.00,"09","Vertical sounding sequences (conventional data)","309061","(Raw PTU)",,"025069","Flight level pressure corrections",,,"Operational"
3113.00,"09","Vertical sounding sequences (conventional data)","309061","(Raw PTU)",,"007004","Pressure",,,"Operational"
3114.00,"09","Vertical sounding sequences (conventional data)","309061","(Raw PTU)",,"202000","Change scale","Cancel",,"Operational"
3115.00,"09","Vertical sounding sequences (conventional data)","309061","(Raw PTU)",,"201000","Change data width","Cancel",,"Operational"
3116.00,"09","Vertical sounding sequences (conventional data)","309061","(Raw PTU)",,"033007","Per cent confidence","Pressure",,"Operational"
3117.00,"09","Vertical sounding sequences (conventional data)","309061","(Raw PTU)",,"033035","Manual/automatic quality control","Pressure",,"Operational"
3118.00,"09","Vertical sounding sequences (conventional data)","309061","(Raw PTU)",,"033015","Data quality check indicator","Pressure",,"Operational"
3119.00,"09","Vertical sounding sequences (conventional data)","309061","(Raw PTU)",,"013009","Relative humidity",,,"Operational"
3120.00,"09","Vertical sounding sequences (conventional data)","309061","(Raw PTU)",,"033007","Per cent confidence","Relative humidity",,"Operational"
3121.00,"09","Vertical sounding sequences (conventional data)","309061","(Raw PTU)",,"033035","Manual/automatic quality control","Relative humidity",,"Operational"
3122.00,"09","Vertical sounding sequences (conventional data)","309061","(Raw PTU)",,"033015","Data quality check indicator","Relative humidity",,"Operational"
3123.00,"09","Vertical sounding sequences (conventional data)","309061","(Raw PTU)",,"002013","Solar and infrared radiation correction",,,"Operational"
3124.00,"09","Vertical sounding sequences (conventional data)","309061","(Raw PTU)",,"012101","Temperature/air temperature",,,"Operational"
3125.00,"09","Vertical sounding sequences (conventional data)","309061","(Raw PTU)",,"033007","Per cent confidence","Temperature",,"Operational"
3126.00,"09","Vertical sounding sequences (conventional data)","309061","(Raw PTU)",,"033035","Manual/automatic quality control","Temperature",,"Operational"
3127.00,"09","Vertical sounding sequences (conventional data)","309061","(Raw PTU)",,"033015","Data quality check indicator","Temperature",,"Operational"
3129.00,"09","Vertical sounding sequences (conventional data)","309062","(Raw GPS unsmoothed wind)",,"301120","Radiosonde abbreviated header and launch information",,,"Operational"
3130.00,"09","Vertical sounding sequences (conventional data)","309062","(Raw GPS unsmoothed wind)",,"008041","Data significance","= 6 Flight level observation",,"Operational"
3131.00,"09","Vertical sounding sequences (conventional data)","309062","(Raw GPS unsmoothed wind)",,"301122","Date/time (to hundredths of second)",,,"Operational"
3132.00,"09","Vertical sounding sequences (conventional data)","309062","(Raw GPS unsmoothed wind)",,"005001","Latitude (high accuracy)",,,"Operational"
3133.00,"09","Vertical sounding sequences (conventional data)","309062","(Raw GPS unsmoothed wind)",,"033035","Manual/automatic quality control","Latitude",,"Operational"
3134.00,"09","Vertical sounding sequences (conventional data)","309062","(Raw GPS unsmoothed wind)",,"033015","Data quality check indicator","Latitude",,"Operational"
3135.00,"09","Vertical sounding sequences (conventional data)","309062","(Raw GPS unsmoothed wind)",,"006001","Longitude (high accuracy)",,,"Operational"
3136.00,"09","Vertical sounding sequences (conventional data)","309062","(Raw GPS unsmoothed wind)",,"033035","Manual/automatic quality control","Longitude",,"Operational"
3137.00,"09","Vertical sounding sequences (conventional data)","309062","(Raw GPS unsmoothed wind)",,"033015","Data quality check indicator","Longitude",,"Operational"
3138.00,"09","Vertical sounding sequences (conventional data)","309062","(Raw GPS unsmoothed wind)",,"007007","Height",,,"Operational"
3139.00,"09","Vertical sounding sequences (conventional data)","309062","(Raw GPS unsmoothed wind)",,"033035","Manual/automatic quality control","Height",,"Operational"
3140.00,"09","Vertical sounding sequences (conventional data)","309062","(Raw GPS unsmoothed wind)",,"033015","Data quality check indicator","Height",,"Operational"
3141.00,"09","Vertical sounding sequences (conventional data)","309062","(Raw GPS unsmoothed wind)",,"011003","u-component",,,"Operational"
3142.00,"09","Vertical sounding sequences (conventional data)","309062","(Raw GPS unsmoothed wind)",,"033035","Manual/automatic quality control","u-component",,"Operational"
3143.00,"09","Vertical sounding sequences (conventional data)","309062","(Raw GPS unsmoothed wind)",,"033015","Data quality check indicator","u-component",,"Operational"
3144.00,"09","Vertical sounding sequences (conventional data)","309062","(Raw GPS unsmoothed wind)",,"011004","v-component",,,"Operational"
3145.00,"09","Vertical sounding sequences (conventional data)","309062","(Raw GPS unsmoothed wind)",,"033035","Manual/automatic quality control","v-component",,"Operational"
3146.00,"09","Vertical sounding sequences (conventional data)","309062","(Raw GPS unsmoothed wind)",,"033015","Data quality check indicator","v-component",,"Operational"
3147.00,"09","Vertical sounding sequences (conventional data)","309062","(Raw GPS unsmoothed wind)",,"033007","Per cent confidence","Raw GPS unsmoothed wind",,"Operational"
3148.00,"09","Vertical sounding sequences (conventional data)","309063","(Raw GPS smoothed wind)",,"301120","Radiosonde abbreviated header and launch information",,,"Operational"
3149.00,"09","Vertical sounding sequences (conventional data)","309063","(Raw GPS smoothed wind)",,"008041","Data significance","= 6 Flight level observation",,"Operational"
3150.00,"09","Vertical sounding sequences (conventional data)","309063","(Raw GPS smoothed wind)",,"301122","Date/time (to hundredths of second)",,,"Operational"
3151.00,"09","Vertical sounding sequences (conventional data)","309063","(Raw GPS smoothed wind)",,"005001","Latitude (high accuracy)",,,"Operational"
3152.00,"09","Vertical sounding sequences (conventional data)","309063","(Raw GPS smoothed wind)",,"033035","Manual/automatic quality control","Latitude",,"Operational"
3153.00,"09","Vertical sounding sequences (conventional data)","309063","(Raw GPS smoothed wind)",,"033015","Data quality check indicator","Latitude",,"Operational"
3154.00,"09","Vertical sounding sequences (conventional data)","309063","(Raw GPS smoothed wind)",,"006001","Longitude (high accuracy)",,,"Operational"
3155.00,"09","Vertical sounding sequences (conventional data)","309063","(Raw GPS smoothed wind)",,"033035","Manual/automatic quality control","Longitude",,"Operational"
3156.00,"09","Vertical sounding sequences (conventional data)","309063","(Raw GPS smoothed wind)",,"033015","Data quality check indicator","Longitude",,"Operational"
3157.00,"09","Vertical sounding sequences (conventional data)","309063","(Raw GPS smoothed wind)",,"007007","Height",,,"Operational"
3158.00,"09","Vertical sounding sequences (conventional data)","309063","(Raw GPS smoothed wind)",,"033035","Manual/automatic quality control","Height",,"Operational"
3159.00,"09","Vertical sounding sequences (conventional data)","309063","(Raw GPS smoothed wind)",,"033015","Data quality check indicator","Height",,"Operational"
3160.00,"09","Vertical sounding sequences (conventional data)","309063","(Raw GPS smoothed wind)",,"011003","u-component",,,"Operational"
3161.00,"09","Vertical sounding sequences (conventional data)","309063","(Raw GPS smoothed wind)",,"033035","Manual/automatic quality control","u-component",,"Operational"
3162.00,"09","Vertical sounding sequences (conventional data)","309063","(Raw GPS smoothed wind)",,"033015","Data quality check indicator","u-component",,"Operational"
3163.00,"09","Vertical sounding sequences (conventional data)","309063","(Raw GPS smoothed wind)",,"011004","v-component",,,"Operational"
3164.00,"09","Vertical sounding sequences (conventional data)","309063","(Raw GPS smoothed wind)",,"033035","Manual/automatic quality control","v-component",,"Operational"
3165.00,"09","Vertical sounding sequences (conventional data)","309063","(Raw GPS smoothed wind)",,"033015","Data quality check indicator","v-component",,"Operational"
3166.00,"09","Vertical sounding sequences (conventional data)","309063","(Raw GPS smoothed wind)",,"033007","Per cent confidence","Raw GPS smoothed wind",,"Operational"
3167.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"301120","Radiosonde abbreviated header and launch information",,,"Operational"
3168.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"008041","Data significance","= 6 Flight level observation",,"Operational"
3169.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"301122","Date/time (to hundredths of second)",,,"Operational"
3170.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"201131","Change data width",,,"Operational"
3171.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"202129","Change scale",,,"Operational"
3172.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"104002","Replicate 4 descriptors 2 times",,,"Operational"
3173.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"025069","Flight level pressure corrections",,,"Operational"
3174.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"007004","Pressure",,,"Operational"
3175.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"033035","Manual/automatic quality control","Pressure",,"Operational"
3176.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"033015","Data quality check indicator","Pressure",,"Operational"
3177.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"013003","Relative humidity",,,"Operational"
3178.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"033035","Manual/automatic quality control","Relative humidity",,"Operational"
3179.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"033015","Data quality check indicator","Relative humidity",,"Operational"
3180.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"202000","Change scale","Cancel",,"Operational"
3181.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"201000","Change data width","Cancel",,"Operational"
3182.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"104002","Replicate 4 descriptors 2 times",,,"Operational"
3183.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"002013","Solar and infrared radiation correction",,,"Operational"
3184.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"012101","Temperature/air temperature",,,"Operational"
3185.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"033035","Manual/automatic quality control","Temperature",,"Operational"
3186.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"033015","Data quality check indicator","Temperature",,"Operational"
3187.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"012103","Dewpoint temperature",,,"Operational"
3188.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"033035","Manual/automatic quality control","Dewpoint temperature",,"Operational"
3189.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"033015","Data quality check indicator","Dewpoint temperature",,"Operational"
3190.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"010009","Geopotential height",,,"Operational"
3191.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"033035","Manual/automatic quality control","Geopotential height",,"Operational"
3192.00,"09","Vertical sounding sequences (conventional data)","309064","(Processed PTU)",,"033015","Data quality check indicator","Geopotential height",,"Operational"
3194.00,"09","Vertical sounding sequences (conventional data)","309065","(Processed GPS)",,"301120","Radiosonde abbreviated header and launch information",,,"Operational"
3195.00,"09","Vertical sounding sequences (conventional data)","309065","(Processed GPS)",,"008041","Data significance","= 6 Flight level observation",,"Operational"
3196.00,"09","Vertical sounding sequences (conventional data)","309065","(Processed GPS)",,"301122","Date/time (to hundredths of second)",,,"Operational"
3197.00,"09","Vertical sounding sequences (conventional data)","309065","(Processed GPS)",,"005001","Latitude (high accuracy)",,,"Operational"
3198.00,"09","Vertical sounding sequences (conventional data)","309065","(Processed GPS)",,"033035","Manual/automatic quality control","Latitude",,"Operational"
3199.00,"09","Vertical sounding sequences (conventional data)","309065","(Processed GPS)",,"033015","Data quality check indicator","Latitude",,"Operational"
3200.00,"09","Vertical sounding sequences (conventional data)","309065","(Processed GPS)",,"006001","Longitude (high accuracy)",,,"Operational"
3201.00,"09","Vertical sounding sequences (conventional data)","309065","(Processed GPS)",,"033035","Manual/automatic quality control","Longitude",,"Operational"
3202.00,"09","Vertical sounding sequences (conventional data)","309065","(Processed GPS)",,"033015","Data quality check indicator","Longitude",,"Operational"
3203.00,"09","Vertical sounding sequences (conventional data)","309065","(Processed GPS)",,"007007","Height",,,"Operational"
3204.00,"09","Vertical sounding sequences (conventional data)","309065","(Processed GPS)",,"033035","Manual/automatic quality control","Height",,"Operational"
3205.00,"09","Vertical sounding sequences (conventional data)","309065","(Processed GPS)",,"033015","Data quality check indicator","Height",,"Operational"
3206.00,"09","Vertical sounding sequences (conventional data)","309065","(Processed GPS)",,"011003","u-component",,,"Operational"
3207.00,"09","Vertical sounding sequences (conventional data)","309065","(Processed GPS)",,"033035","Manual/automatic quality control","u-component",,"Operational"
3208.00,"09","Vertical sounding sequences (conventional data)","309065","(Processed GPS)",,"033015","Data quality check indicator","u-component",,"Operational"
3209.00,"09","Vertical sounding sequences (conventional data)","309065","(Processed GPS)",,"011004","v-component",,,"Operational"
3210.00,"09","Vertical sounding sequences (conventional data)","309065","(Processed GPS)",,"033035","Manual/automatic quality control","v-component",,"Operational"
3211.00,"09","Vertical sounding sequences (conventional data)","309065","(Processed GPS)",,"033015","Data quality check indicator","v-component",,"Operational"
3212.00,"09","Vertical sounding sequences (conventional data)","309066","(Standard and significant levels)",,"301120","Radiosonde abbreviated header and launch information",,,"Operational"
3213.00,"09","Vertical sounding sequences (conventional data)","309066","(Standard and significant levels)",,"008041","Data significance","= 6 Flight level observation",,"Operational"
3214.00,"09","Vertical sounding sequences (conventional data)","309066","(Standard and significant levels)",,"301122","Date/time (to hundredths of second)",,,"Operational"
3215.00,"09","Vertical sounding sequences (conventional data)","309066","(Standard and significant levels)",,"008040","Flight level significance",,,"Operational"
3216.00,"09","Vertical sounding sequences (conventional data)","309066","(Standard and significant levels)",,"201131","Change data width",,,"Operational"
3217.00,"09","Vertical sounding sequences (conventional data)","309066","(Standard and significant levels)",,"202129","Change scale",,,"Operational"
3218.00,"09","Vertical sounding sequences (conventional data)","309066","(Standard and significant levels)",,"025069","Flight level pressure corrections",,,"Operational"
3219.00,"09","Vertical sounding sequences (conventional data)","309066","(Standard and significant levels)",,"007004","Pressure",,,"Operational"
3220.00,"09","Vertical sounding sequences (conventional data)","309066","(Standard and significant levels)",,"013003","Relative humidity",,,"Operational"
3221.00,"09","Vertical sounding sequences (conventional data)","309066","(Standard and significant levels)",,"202000","Change scale","Cancel",,"Operational"
3222.00,"09","Vertical sounding sequences (conventional data)","309066","(Standard and significant levels)",,"201000","Change data width","Cancel",,"Operational"
3223.00,"09","Vertical sounding sequences (conventional data)","309066","(Standard and significant levels)",,"002013","Solar and infrared radiation correction",,,"Operational"
3224.00,"09","Vertical sounding sequences (conventional data)","309066","(Standard and significant levels)",,"012101","Temperature/air temperature",,,"Operational"
3225.00,"09","Vertical sounding sequences (conventional data)","309066","(Standard and significant levels)",,"012103","Dewpoint temperature",,,"Operational"
3226.00,"09","Vertical sounding sequences (conventional data)","309066","(Standard and significant levels)",,"010009","Geopotential height",,,"Operational"
3227.00,"09","Vertical sounding sequences (conventional data)","309066","(Standard and significant levels)",,"010007","Height",,,"Operational"
3228.00,"09","Vertical sounding sequences (conventional data)","309066","(Standard and significant levels)",,"011002","Wind speed",,,"Operational"
3229.00,"09","Vertical sounding sequences (conventional data)","309066","(Standard and significant levels)",,"011001","Wind direction",,,"Operational"
3231.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Identification","001035","Originating centre",,,"Operational"
3232.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Identification","001032","Generating application",,,"Operational"
3233.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Identification","001015","Station or site name",,,"Operational"
3234.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Identification","001063","ICAO location indicator",,,"Operational"
3235.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Identification","301001","WMO block and station numbers",,,"Operational"
3236.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Location and reference time","301011","Year, month, day",,,"Operational"
3237.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Location and reference time","301012","Hour, minute","Reference time of the forecast (T-zero)",,"Operational"
3238.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Location and reference time","301021","Latitude/longitude (high accuracy)",,,"Operational"
3239.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Location and reference time","207001","Increase scale, reference value and data width","Increase scale factor by 1; reference value and data width are recalculated in accordance with the Table C specification of operator 2 07 YYY",,"Operational"
3240.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Location and reference time","010001","Height of land surface","Station elevation (non coordinate)","(see Note 3)","Operational"
3241.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Location and reference time","207000","Increase scale, reference value and data width","Cancel",,"Operational"
3242.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Location and reference time","008086","Vertical significance for NWP","Bit 9 set to 1 Virtual station height",,"Operational"
3243.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Location and reference time","007030","Height of station ground above mean sea level","Elevation of model terrain at the lat/lon of station.  As qualified by 0 08 086, this value is both station and model specific.",,"Operational"
3244.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Vertical profile metadata","025031","NWP-generated vertical profile thinning method",,"(see Note 4)","Operational"
3245.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Vertical profile metadata","008021","Time significance","= 4 Forecast, = 16 Analysis, = 27 First guess",,"Operational"
3246.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Vertical profile metadata","004014","Time increment","Validity time of the forecast expressed as a Delta T from reference time. In the case of an analysis or 00 hour forecast, the value is set to zero",,"Operational"
3247.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Point data at station height (including column-integrated data)","010004","Pressure",,,"Operational"
3248.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Point data at station height (including column-integrated data)","010051","Pressure reduced to mean sea level",,,"Operational"
3249.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Point data at station height (including column-integrated data)","010009","Geopotential height",,,"Operational"
3250.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Point data at station height (including column-integrated data)","020010","Cloud cover (total)",,,"Operational"
3251.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Point data at station height (including column-integrated data)","013095","Total column water vapour",,,"Operational"
3252.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Replication loop for levels","128000","Delayed replication of 28 descriptors",,,"Operational"
3253.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Replication loop for levels","031002","Extended delayed descriptor replication factor","The number of levels used in the vertical profile is determined by this replication. The number of levels is discretionary and comprises all agl levels and pressure levels",,"Operational"
3254.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data on pressure coordinates","113000","Delayed replication of 13 descriptors",,,"Operational"
3255.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data on pressure coordinates","031000","Short delayed descriptor replication factor","= 1 Vertical coordinate is pressure, = 0 Otherwise",,"Operational"
3256.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data on pressure coordinates","008086","Vertical significance for NWP","Bit 1 set to 0 and other bits as appropriate",,"Operational"
3257.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data on pressure coordinates","007004","Pressure",,"(see Note 5)","Operational"
3258.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data on pressure coordinates","011001","Wind direction","Degrees true",,"Operational"
3259.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data on pressure coordinates","011002","Wind speed","m/s",,"Operational"
3260.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data on pressure coordinates","012101","Temperature/air temperature",,,"Operational"
3261.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data on pressure coordinates","012102","Wet-bulb temperature",,,"Operational"
3262.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data on pressure coordinates","012103","Dewpoint temperature",,,"Operational"
3263.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data on pressure coordinates","010009","Geopotential height",,,"Operational"
3264.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data on pressure coordinates","103000","Delayed replication of 3 descriptors",,,"Operational"
3265.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data on pressure coordinates","031000","Short delayed descriptor replication factor","= 1 Optional enhanced model data is to be included",,"Operational"
3266.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data on pressure coordinates","011021","Relative vorticity",,,"Operational"
3267.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data on pressure coordinates","011022","Divergence",,,"Operational"
3268.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data on pressure coordinates","011005","w-component","Vertical motion",,"Operational"
3269.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data at 10 metres above ground level","104000","Delayed replication of 4 descriptors",,,"Operational"
3270.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data at 10 metres above ground level","031000","Short delayed descriptor replication factor","= 1 Vertical coordinate is 10 metres above ground level, = 0 Otherwise",,"Operational"
3271.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data at 10 metres above ground level","008086","Vertical significance for NWP","Bit 1 set to 1, bit 8 set to 1",,"Operational"
3272.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data at 10 metres above ground level","007006","Height above station","= 10 m",,"Operational"
3273.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data at 10 metres above ground level","011001","Wind direction","Degrees true",,"Operational"
3274.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data at 10 metres above ground level","011002","Wind speed","m/s",,"Operational"
3275.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data at 2 metres above ground level","105000","Delayed replication of 5 descriptors",,,"Operational"
3276.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data at 2 metres above ground level","031000","Short delayed descriptor replication factor","= 1 Vertical coordinate is 2 metres above ground level, = 0 Otherwise",,"Operational"
3277.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data at 2 metres above ground level","008086","Vertical significance for NWP",,,"Operational"
3278.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data at 2 metres above ground level","007006","Height above station","= 2 m",,"Operational"
3279.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data at 2 metres above ground level","012101","Temperature/air temperature",,,"Operational"
3280.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data at 2 metres above ground level","012102","Wet-bulb temperature",,,"Operational"
3281.00,"09","Vertical sounding sequences (conventional data)","309070","(Vertical profile for numerical weather prediction data)","Data at 2 metres above ground level","012103","Dewpoint temperature",,,"Operational"
3283.00,"09","Vertical sounding sequences (conventional data)","309071","(Sequence for representation of PILOT in the area of ASECNA)",,"301001","WMO block and station numbers",,,"Operational"
3284.00,"09","Vertical sounding sequences (conventional data)","309071","(Sequence for representation of PILOT in the area of ASECNA)",,"002014","Tracking technique/status of system used",,,"Operational"
3285.00,"09","Vertical sounding sequences (conventional data)","309071","(Sequence for representation of PILOT in the area of ASECNA)",,"002003","Type of measuring equipment used",,,"Operational"
3286.00,"09","Vertical sounding sequences (conventional data)","309071","(Sequence for representation of PILOT in the area of ASECNA)",,"301113","Date/time of launch",,,"Operational"
3287.00,"09","Vertical sounding sequences (conventional data)","309071","(Sequence for representation of PILOT in the area of ASECNA)",,"301114","Horizontal and vertical coordinates of launch site",,,"Operational"
3288.00,"09","Vertical sounding sequences (conventional data)","309071","(Sequence for representation of PILOT in the area of ASECNA)",,"301023","Latitude/longitude (coarse accuracy)",,,"Operational"
3289.00,"09","Vertical sounding sequences (conventional data)","309071","(Sequence for representation of PILOT in the area of ASECNA)",,"007030","Height of station ground above mean sea level",,,"Operational"
3290.00,"09","Vertical sounding sequences (conventional data)","309071","(Sequence for representation of PILOT in the area of ASECNA)",,"007007","Height","Release of balloon",,"Operational"
3291.00,"09","Vertical sounding sequences (conventional data)","309071","(Sequence for representation of PILOT in the area of ASECNA)",,"103000","Delayed replication of 3 descriptors",,,"Operational"
3292.00,"09","Vertical sounding sequences (conventional data)","309071","(Sequence for representation of PILOT in the area of ASECNA)",,"031001","Delayed descriptor replication factor",,,"Operational"
3293.00,"09","Vertical sounding sequences (conventional data)","309071","(Sequence for representation of PILOT in the area of ASECNA)",,"007009","Geopotential height",,,"Operational"
3294.00,"09","Vertical sounding sequences (conventional data)","309071","(Sequence for representation of PILOT in the area of ASECNA)",,"011001","Wind direction",,,"Operational"
3295.00,"09","Vertical sounding sequences (conventional data)","309071","(Sequence for representation of PILOT in the area of ASECNA)",,"011002","Wind speed",,,"Operational"
3308.00,"10","Vertical sounding sequences (satellite data)","310001","(Satellite - brightness temperature)",,"301042","Satellite identifier, instrument, data-processing technique, date/time, location",,,"Operational"
3309.00,"10","Vertical sounding sequences (satellite data)","310001","(Satellite - brightness temperature)",,"303031","Significance data, land/sea, skin temperature",,,"Operational"
3310.00,"10","Vertical sounding sequences (satellite data)","310001","(Satellite - brightness temperature)",,"303032","Cloud",,,"Operational"
3311.00,"10","Vertical sounding sequences (satellite data)","310001","(Satellite - brightness temperature)",,"101026","Replicate 1 descriptor 26 times",,,"Operational"
3312.00,"10","Vertical sounding sequences (satellite data)","310001","(Satellite - brightness temperature)",,"303025","Satellite channel and brightness temperature",,,"Operational"
3313.00,"10","Vertical sounding sequences (satellite data)","310002","(Satellite - low level)",,"301042","Satellite identifier, instrument, data-processing technique, date/time, location",,,"Operational"
3314.00,"10","Vertical sounding sequences (satellite data)","310002","(Satellite - low level)",,"303031","Significance data, land/sea, skin temperature",,,"Operational"
3315.00,"10","Vertical sounding sequences (satellite data)","310002","(Satellite - low level)",,"303032","Cloud",,,"Operational"
3316.00,"10","Vertical sounding sequences (satellite data)","310002","(Satellite - low level)",,"101009","Replicate 1 descriptor 9 times",,,"Operational"
3317.00,"10","Vertical sounding sequences (satellite data)","310002","(Satellite - low level)",,"303023","Layer mean temperature",,,"Operational"
3318.00,"10","Vertical sounding sequences (satellite data)","310003","(Satellite - high level)",,"301042","Satellite identifier, instrument, data-processing technique, date/time, location",,,"Operational"
3319.00,"10","Vertical sounding sequences (satellite data)","310003","(Satellite - high level)",,"303031","Significance data, land/sea, skin temperature",,,"Operational"
3320.00,"10","Vertical sounding sequences (satellite data)","310003","(Satellite - high level)",,"303032","Cloud",,,"Operational"
3321.00,"10","Vertical sounding sequences (satellite data)","310003","(Satellite - high level)",,"101006","Replicate 1 descriptor 6 times",,,"Operational"
3322.00,"10","Vertical sounding sequences (satellite data)","310003","(Satellite - high level)",,"303023","Layer mean temperature",,,"Operational"
3323.00,"10","Vertical sounding sequences (satellite data)","310004","(Satellite - precipitable water)",,"301042","Satellite identifier, instrument, data-processing technique, date/time, location",,,"Operational"
3324.00,"10","Vertical sounding sequences (satellite data)","310004","(Satellite - precipitable water)",,"303031","Significance data, land/sea, skin temperature",,,"Operational"
3325.00,"10","Vertical sounding sequences (satellite data)","310004","(Satellite - precipitable water)",,"303032","Cloud",,,"Operational"
3326.00,"10","Vertical sounding sequences (satellite data)","310004","(Satellite - precipitable water)",,"101003","Replicate 1 descriptor 3 times",,,"Operational"
3327.00,"10","Vertical sounding sequences (satellite data)","310004","(Satellite - precipitable water)",,"303024","Precipitable water",,,"Operational"
3328.00,"10","Vertical sounding sequences (satellite data)","310005",,,"301042","Satellite identifier, instrument, data-processing technique, date/time, location",,,"Operational"
3329.00,"10","Vertical sounding sequences (satellite data)","310005",,,"303031","Significance data, land/sea, skin temperature",,,"Operational"
3330.00,"10","Vertical sounding sequences (satellite data)","310005",,,"303033","Cloud",,,"Operational"
3331.00,"10","Vertical sounding sequences (satellite data)","310005",,,"101000","Delayed replication of 1 descriptor",,,"Operational"
3332.00,"10","Vertical sounding sequences (satellite data)","310005",,,"031001","Delayed descriptor replication factor",,,"Operational"
3333.00,"10","Vertical sounding sequences (satellite data)","310005",,,"303025","Satellite channel and brightness temperature",,,"Operational"
3334.00,"10","Vertical sounding sequences (satellite data)","310006",,,"301042","Satellite identifier, instrument, data-processing technique, date/time, location",,,"Operational"
3335.00,"10","Vertical sounding sequences (satellite data)","310006",,,"303031","Significance data, land/sea, skin temperature",,,"Operational"
3336.00,"10","Vertical sounding sequences (satellite data)","310006",,,"303033","Cloud",,,"Operational"
3337.00,"10","Vertical sounding sequences (satellite data)","310006",,,"101000","Delayed replication of 1 descriptor",,,"Operational"
3338.00,"10","Vertical sounding sequences (satellite data)","310006",,,"031001","Delayed descriptor replication factor",,,"Operational"
3339.00,"10","Vertical sounding sequences (satellite data)","310006",,,"303023","Layer mean temperature",,,"Operational"
3340.00,"10","Vertical sounding sequences (satellite data)","310007",,,"301042","Satellite identifier, instrument, data-processing technique, date/time, location",,,"Operational"
3341.00,"10","Vertical sounding sequences (satellite data)","310007",,,"303031","Significance data, land/sea, skin temperature",,,"Operational"
3342.00,"10","Vertical sounding sequences (satellite data)","310007",,,"303033","Cloud",,,"Operational"
3343.00,"10","Vertical sounding sequences (satellite data)","310007",,,"101000","Delayed replication of 1 descriptor",,,"Operational"
3344.00,"10","Vertical sounding sequences (satellite data)","310007",,,"031001","Delayed descriptor replication factor",,,"Operational"
3345.00,"10","Vertical sounding sequences (satellite data)","310007",,,"303024","Precipitable water",,,"Operational"
3346.00,"10","Vertical sounding sequences (satellite data)","310008","(ATOVS HIRS report)",,"310011","ATOVS field of view variables",,,"Operational"
3347.00,"10","Vertical sounding sequences (satellite data)","310008","(ATOVS HIRS report)",,"101019","Replicate 1 descriptor 19 times",,,"Operational"
3348.00,"10","Vertical sounding sequences (satellite data)","310008","(ATOVS HIRS report)",,"310012","ATOVS channel variables",,,"Operational"
3349.00,"10","Vertical sounding sequences (satellite data)","310008","(ATOVS HIRS report)",,"002150","TOVS/ATOVS/AVHRR instrumentation channel number",,,"Operational"
3350.00,"10","Vertical sounding sequences (satellite data)","310008","(ATOVS HIRS report)",,"025079","Albedo-radiance solar filtered irradiance for ATOVS",,,"Operational"
3351.00,"10","Vertical sounding sequences (satellite data)","310008","(ATOVS HIRS report)",,"025080","Albedo-radiance equivalent filter width for ATOVS",,,"Operational"
3352.00,"10","Vertical sounding sequences (satellite data)","310008","(ATOVS HIRS report)",,"033032","Channel quality flags for ATOVS",,,"Operational"
3353.00,"10","Vertical sounding sequences (satellite data)","310008","(ATOVS HIRS report)",,"014045","Channel radiance",,,"Operational"
3354.00,"10","Vertical sounding sequences (satellite data)","310009","(ATOVS AMSU-A report)",,"310011","ATOVS field of view variables",,,"Operational"
3355.00,"10","Vertical sounding sequences (satellite data)","310009","(ATOVS AMSU-A report)",,"101015","Replicate 1 descriptor 15 times",,,"Operational"
3356.00,"10","Vertical sounding sequences (satellite data)","310009","(ATOVS AMSU-A report)",,"310012","ATOVS channel variables",,,"Operational"
3357.00,"10","Vertical sounding sequences (satellite data)","310010","(ATOVS AMSU-B/MHS report)",,"310011","ATOVS field of view variables",,,"Operational"
3358.00,"10","Vertical sounding sequences (satellite data)","310010","(ATOVS AMSU-B/MHS report)",,"101005","Replicate 1 descriptor 5 times",,,"Operational"
3359.00,"10","Vertical sounding sequences (satellite data)","310010","(ATOVS AMSU-B/MHS report)",,"310012","ATOVS channel variables",,,"Operational"
3360.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"008070","TOVS/ATOVS product qualifier",,,"Operational"
3361.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"001033","Identification of originating/generating centre",,,"Operational"
3362.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"001034","Identification of originating/generating sub-centre",,,"Operational"
3363.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"008070","TOVS/ATOVS product qualifier",,,"Operational"
3364.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"001033","Identification of originating/generating centre",,,"Operational"
3365.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"001034","Identification of originating/generating sub-centre",,,"Operational"
3366.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"001007","Satellite identifier",,,"Operational"
3367.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"002048","Satellite sensor indicator",,,"Operational"
3368.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"005040","Orbit number",,,"Operational"
3369.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"025075","Satellite antenna corrections version number",,,"Operational"
3370.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"201133","Change data width",,,"Operational"
3371.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"005041","Scan line number",,,"Operational"
3372.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"201000","Change data width",,,"Operational"
3373.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"005043","Field of view number",,,"Operational"
3374.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"025070","Major frame count",,,"Operational"
3375.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"033030","Scan line status flags for ATOVS",,,"Operational"
3376.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"033031","Scan line quality flags for ATOVS",,,"Operational"
3377.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"004001","Year",,,"Operational"
3378.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"004002","Month",,,"Operational"
3379.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"004003","Day",,,"Operational"
3380.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"004004","Hour",,,"Operational"
3381.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"004005","Minute",,,"Operational"
3382.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"202131","Change scale",,,"Operational"
3383.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"201138","Change data width",,,"Operational"
3384.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"004006","Second",,,"Operational"
3385.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"201000","Change data width",,,"Operational"
3386.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"202000","Change scale",,,"Operational"
3387.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"005001","Latitude (high accuracy)",,,"Operational"
3388.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"006001","Longitude (high accuracy)",,,"Operational"
3389.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"202126","Change scale",,,"Operational"
3390.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"007001","Height of station",,,"Operational"
3391.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"202000","Change scale",,,"Operational"
3392.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"007024","Satellite zenith angle",,,"Operational"
3393.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"005021","Bearing or azimuth","Satellite azimuth",,"Operational"
3394.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"007025","Solar zenith angle",,,"Operational"
3395.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"005022","Solar azimuth",,,"Operational"
3396.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"033033","Field of view quality flags for ATOVS",,,"Operational"
3397.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"002151","Radiometer identifier",,,"Operational"
3398.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"012064","Instrument temperature",,,"Operational"
3399.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"002151","Radiometer identifier",,,"Operational"
3400.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"012064","Instrument temperature",,,"Operational"
3401.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"002151","Radiometer identifier",,,"Operational"
3402.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"012064","Instrument temperature",,,"Operational"
3403.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"002151","Radiometer identifier",,,"Operational"
3404.00,"10","Vertical sounding sequences (satellite data)","310011","(ATOVS field of view variables)",,"012064","Instrument temperature",,,"Operational"
3405.00,"10","Vertical sounding sequences (satellite data)","310012","(ATOVS channel variables)",,"002150","TOVS/ATOVS/AVHRR instrumentation channel number",,,"Operational"
3406.00,"10","Vertical sounding sequences (satellite data)","310012","(ATOVS channel variables)",,"025076","Log10 of (temperature-radiance central wave number) for ATOVS",,,"Operational"
3407.00,"10","Vertical sounding sequences (satellite data)","310012","(ATOVS channel variables)",,"025077","Bandwidth correction coefficient 1 for ATOVS",,,"Operational"
3408.00,"10","Vertical sounding sequences (satellite data)","310012","(ATOVS channel variables)",,"025078","Bandwidth correction coefficient 2 for ATOVS",,,"Operational"
3409.00,"10","Vertical sounding sequences (satellite data)","310012","(ATOVS channel variables)",,"033032","Channel quality flags for ATOVS",,,"Operational"
3410.00,"10","Vertical sounding sequences (satellite data)","310012","(ATOVS channel variables)",,"201132","Change data width",,,"Operational"
3411.00,"10","Vertical sounding sequences (satellite data)","310012","(ATOVS channel variables)",,"202129","Change scale",,,"Operational"
3412.00,"10","Vertical sounding sequences (satellite data)","310012","(ATOVS channel variables)",,"012063","Brightness temperature",,,"Operational"
3413.00,"10","Vertical sounding sequences (satellite data)","310012","(ATOVS channel variables)",,"202000","Change scale",,,"Operational"
3414.00,"10","Vertical sounding sequences (satellite data)","310012","(ATOVS channel variables)",,"201000","Change data width",,,"Operational"
3415.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"001007","Satellite identifier",,,"Operational"
3416.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"005040","Orbit number",,,"Operational"
3417.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"004001","Year",,,"Operational"
3418.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"004002","Month",,,"Operational"
3419.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"004003","Day",,,"Operational"
3420.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"004004","Hour",,,"Operational"
3421.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"004005","Minute",,,"Operational"
3422.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"004006","Second",,,"Operational"
3423.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"005001","Latitude (high accuracy)",,,"Operational"
3424.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"006001","Longitude (high accuracy)",,,"Operational"
3425.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"007025","Solar zenith angle",,,"Operational"
3426.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"005043","Field of view number",,,"Operational"
3427.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"025085","Fraction of clear pixels in HIRS FOV",,,"Operational"
3428.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"201131","Change data width",,,"Operational"
3429.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"202129","Change scale",,,"Operational"
3430.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"002150","TOVS/ATOVS/AVHRR instrumentation channel number",,,"Operational"
3431.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"008023","First-order statistics",,,"Operational"
3432.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"008072","Pixel(s) type",,,"Operational"
3433.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"014027","Albedo",,,"Operational"
3434.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"008072","Pixel(s) type",,,"Operational"
3435.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"014027","Albedo",,,"Operational"
3436.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"002150","TOVS/ATOVS/AVHRR instrumentation channel number",,,"Operational"
3437.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"008023","First-order statistics",,,"Operational"
3438.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"008072","Pixel(s) type",,,"Operational"
3439.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"014027","Albedo",,,"Operational"
3440.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"008072","Pixel(s) type",,,"Operational"
3441.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"014027","Albedo",,,"Operational"
3442.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"002150","TOVS/ATOVS/AVHRR instrumentation channel number",,,"Operational"
3443.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"008023","First-order statistics",,,"Operational"
3444.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"008072","Pixel(s) type",,,"Operational"
3445.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"014027","Albedo",,,"Operational"
3446.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"008072","Pixel(s) type",,,"Operational"
3447.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"014027","Albedo",,,"Operational"
3448.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"202000","Change scale",,,"Operational"
3449.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"201000","Change data width",,,"Operational"
3450.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"201132","Change data width",,,"Operational"
3451.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"202129","Change scale",,,"Operational"
3452.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"002150","TOVS/ATOVS/AVHRR instrumentation channel number",,,"Operational"
3453.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"008023","First-order statistics",,,"Operational"
3454.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"008072","Pixel(s) type",,,"Operational"
3455.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"012063","Brightness temperature",,,"Operational"
3456.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"008072","Pixel(s) type",,,"Operational"
3457.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"012063","Brightness temperature",,,"Operational"
3458.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"002150","TOVS/ATOVS/AVHRR instrumentation channel number",,,"Operational"
3459.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"008023","First-order statistics",,,"Operational"
3460.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"008072","Pixel(s) type",,,"Operational"
3461.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"012063","Brightness temperature",,,"Operational"
3462.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"008072","Pixel(s) type",,,"Operational"
3463.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"012063","Brightness temperature",,,"Operational"
3464.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"008023","First-order statistics",,,"Operational"
3465.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"008072","Pixel(s) type",,,"Operational"
3466.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"012063","Brightness temperature",,,"Operational"
3467.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"008072","Pixel(s) type",,,"Operational"
3468.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"012063","Brightness temperature",,,"Operational"
3469.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"002150","TOVS/ATOVS/AVHRR instrumentation channel number",,,"Operational"
3470.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"008023","First-order statistics",,,"Operational"
3471.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"008072","Pixel(s) type",,,"Operational"
3472.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"012063","Brightness temperature",,,"Operational"
3473.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"008072","Pixel(s) type",,,"Operational"
3474.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"012063","Brightness temperature",,,"Operational"
3475.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"202000","Change scale",,,"Operational"
3476.00,"10","Vertical sounding sequences (satellite data)","310013","(AVHRR (GAC) report)",,"201000","Change data width",,,"Operational"
3477.00,"10","Vertical sounding sequences (satellite data)","310014","(Satellite - geostationary wind data)",,"301072","Satellite identification","Satellite identification, date/time, latitude/longitude",,"Operational"
3478.00,"10","Vertical sounding sequences (satellite data)","310014","(Satellite - geostationary wind data)",,"303041","Wind sequence",,,"Operational"
3479.00,"10","Vertical sounding sequences (satellite data)","310014","(Satellite - geostationary wind data)",,"304011","GOES-I/M info",,,"Operational"
3480.00,"10","Vertical sounding sequences (satellite data)","310015","(Meteosat radiance data)",,"301072","Satellite identification",,,"Operational"
3481.00,"10","Vertical sounding sequences (satellite data)","310015","(Meteosat radiance data)",,"007024","Satellite zenith angle",,,"Operational"
3482.00,"10","Vertical sounding sequences (satellite data)","310015","(Meteosat radiance data)",,"010002","Height",,,"Operational"
3483.00,"10","Vertical sounding sequences (satellite data)","310015","(Meteosat radiance data)",,"303041","Wind sequence",,,"Operational"
3484.00,"10","Vertical sounding sequences (satellite data)","310015","(Meteosat radiance data)",,"101003","Replicate 1 descriptor 3 times",,,"Operational"
3485.00,"10","Vertical sounding sequences (satellite data)","310015","(Meteosat radiance data)",,"304032","Cloud fraction",,,"Operational"
3486.00,"10","Vertical sounding sequences (satellite data)","310015","(Meteosat radiance data)",,"002152","Satellite instrument used in data processing",,,"Operational"
3487.00,"10","Vertical sounding sequences (satellite data)","310015","(Meteosat radiance data)",,"002024","Integrated mean humidity computational method",,,"Operational"
3488.00,"10","Vertical sounding sequences (satellite data)","310015","(Meteosat radiance data)",,"007004","Pressure",,,"Operational"
3489.00,"10","Vertical sounding sequences (satellite data)","310015","(Meteosat radiance data)",,"007004","Pressure",,,"Operational"
3490.00,"10","Vertical sounding sequences (satellite data)","310015","(Meteosat radiance data)",,"013003","Relative humidity",,,"Operational"
3491.00,"10","Vertical sounding sequences (satellite data)","310015","(Meteosat radiance data)",,"101003","Replicate 1 descriptor 3 times",,,"Operational"
3492.00,"10","Vertical sounding sequences (satellite data)","310015","(Meteosat radiance data)",,"304033","Clear sky radiance",,,"Operational"
3493.00,"10","Vertical sounding sequences (satellite data)","310016","(Meteosat Second Generation (MSG) radiance data)",,"301072","Satellite identification",,,"Operational"
3494.00,"10","Vertical sounding sequences (satellite data)","310016","(Meteosat Second Generation (MSG) radiance data)",,"007024","Satellite zenith angle",,,"Operational"
3495.00,"10","Vertical sounding sequences (satellite data)","310016","(Meteosat Second Generation (MSG) radiance data)",,"010002","Height",,,"Operational"
3496.00,"10","Vertical sounding sequences (satellite data)","310016","(Meteosat Second Generation (MSG) radiance data)",,"303041","Wind sequence",,,"Operational"
3497.00,"10","Vertical sounding sequences (satellite data)","310016","(Meteosat Second Generation (MSG) radiance data)",,"101012","Replicate 1 descriptor 12 times",,,"Operational"
3498.00,"10","Vertical sounding sequences (satellite data)","310016","(Meteosat Second Generation (MSG) radiance data)",,"304032","Cloud fraction",,,"Operational"
3499.00,"10","Vertical sounding sequences (satellite data)","310016","(Meteosat Second Generation (MSG) radiance data)",,"002152","Satellite instrument used in data processing",,,"Operational"
3500.00,"10","Vertical sounding sequences (satellite data)","310016","(Meteosat Second Generation (MSG) radiance data)",,"002024","Integrated mean humidity computational method",,,"Operational"
3501.00,"10","Vertical sounding sequences (satellite data)","310016","(Meteosat Second Generation (MSG) radiance data)",,"007004","Pressure",,,"Operational"
3502.00,"10","Vertical sounding sequences (satellite data)","310016","(Meteosat Second Generation (MSG) radiance data)",,"007004","Pressure",,,"Operational"
3503.00,"10","Vertical sounding sequences (satellite data)","310016","(Meteosat Second Generation (MSG) radiance data)",,"013003","Relative humidity",,,"Operational"
3504.00,"10","Vertical sounding sequences (satellite data)","310016","(Meteosat Second Generation (MSG) radiance data)",,"101012","Replicate 1 descriptor 12 times",,,"Operational"
3505.00,"10","Vertical sounding sequences (satellite data)","310016","(Meteosat Second Generation (MSG) radiance data)",,"304033","Clear sky radiance",,,"Operational"
3506.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"001007","Satellite identifier",,,"Operational"
3507.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"005040","Orbit number",,,"Operational"
3508.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"004001","Year",,,"Operational"
3509.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"004043","Day of the year",,,"Operational"
3510.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"004004","Hour",,,"Operational"
3511.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"004005","Minute",,,"Operational"
3512.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"004006","Second",,,"Operational"
3513.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"207002","Increase scale, reference value and data width",,,"Operational"
3514.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"026030","Measurement integration time",,,"Operational"
3515.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"207000","Increase scale, reference value and data width","Cancel",,"Operational"
3516.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"005002","Latitude (coarse accuracy)",,,"Operational"
3517.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"006002","Longitude (coarse accuracy)",,,"Operational"
3518.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"033072","Ozone error",,,"Operational"
3519.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"007025","Solar zenith angle",,,"Operational"
3520.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"005022","Solar azimuth",,,"Operational"
3521.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"207002","Increase scale, reference value and data width",,,"Operational"
3522.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"015001","Total ozone",,,"Operational"
3523.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"207000","Increase scale, reference value and data width","Cancel",,"Operational"
3524.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"008003","Vertical significance (satellite observations)","= 0 Surface",,"Operational"
3525.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"207001","Increase scale, reference value and data width",,,"Operational"
3526.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"010004","Pressure","Terrain",,"Operational"
3527.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"207000","Increase scale, reference value and data width","Cancel",,"Operational"
3528.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"008003","Vertical significance (satellite observations)","Set to missing (cancel)",,"Operational"
3529.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"008003","Vertical significance (satellite observations)","= 2 Cloud top",,"Operational"
3530.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"033042","Type of limit represented by following value","= 0 Exclusive lower limit",,"Operational"
3531.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"207001","Increase scale, reference value and data width",,,"Operational"
3532.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"007004","Pressure",,,"Operational"
3533.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"207000","Increase scale, reference value and data width","Cancel",,"Operational"
3534.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"207002","Increase scale, reference value and data width",,,"Operational"
3535.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"015001","Total ozone","Below cloud top pressure",,"Operational"
3536.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"207000","Increase scale, reference value and data width","Cancel",,"Operational"
3537.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"008003","Vertical significance (satellite observations)","Set to missing (cancel)",,"Operational"
3538.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"207002","Increase scale, reference value and data width",,,"Operational"
3539.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"020081","Cloud amount in segment","Cloud fraction",,"Operational"
3540.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"207000","Increase scale, reference value and data width","Cancel",,"Operational"
3541.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"020065","Snow cover",,,"Operational"
3542.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"008029","Surface type",,,"Operational"
3543.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"207004","Increase scale, reference value and data width",,,"Operational"
3544.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"015030","Aerosol contamination index",,,"Operational"
3545.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"207000","Increase scale, reference value and data width","Cancel",,"Operational"
3546.00,"10","Vertical sounding sequences (satellite data)","310018","(Ozone data)",,"008075","Ascending/descending orbit qualifier",,,"Operational"
3547.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"001007","Satellite identifier",,,"Operational"
3548.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"002019","Satellite instruments","= 624 SBUV/2",,"Operational"
3549.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"301011","Year, month, day",,,"Operational"
3550.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"301013","Hour, minute, second",,,"Operational"
3551.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"301023","Latitude/longitude (coarse accuracy)",,,"Operational"
3552.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"007025","Solar zenith angle",,,"Operational"
3553.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"008021","Time significance","= 28 Start of scan",,"Operational"
3554.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"007025","Solar zenith angle",,,"Operational"
3555.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"008021","Time significance","= 29 End of scan",,"Operational"
3556.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"007025","Solar zenith angle",,,"Operational"
3557.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"008021","Time significance","Set to missing (cancel)",,"Operational"
3558.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"008029","Surface type",,,"Operational"
3559.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"005040","Orbit number",,,"Operational"
3560.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"008075","Ascending/descending orbit qualifier",,,"Operational"
3561.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"008003","Vertical significance (satellite observations)","= 0 Surface",,"Operational"
3562.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"010004","Pressure","= Terrain",,"Operational"
3563.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"008003","Vertical significance (satellite observations)","Set to missing (cancel)",,"Operational"
3564.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"207002","Increase scale, reference value and data width",,,"Operational"
3565.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"015001","Total ozone",,,"Operational"
3566.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"207000","Increase scale, reference value and data width","Cancel",,"Operational"
3567.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"033070","Total ozone quality",,,"Operational"
3568.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"015030","Aerosol contamination index",,,"Operational"
3569.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"207002","Increase scale, reference value and data width",,,"Operational"
3570.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"020081","Cloud amount in segment","Cloud fraction",,"Operational"
3571.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"207000","Increase scale, reference value and data width","Cancel",,"Operational"
3572.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"008003","Vertical significance (satellite observations)","= 2 Cloud top",,"Operational"
3573.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"033042","Type of limit represented by following value","= 0 Exclusive lower limit",,"Operational"
3574.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"007004","Pressure",,,"Operational"
3575.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"207002","Increase scale, reference value and data width",,,"Operational"
3576.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"015001","Total ozone","Below cloud top pressure",,"Operational"
3577.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"207000","Increase scale, reference value and data width","Cancel",,"Operational"
3578.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"008003","Vertical significance (satellite observations)","Set to missing (cancel)",,"Operational"
3579.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"113021","Replicate 13 descriptors 21 times",,,"Operational"
3580.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"007004","Pressure","Bottom of layer",,"Operational"
3581.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"007004","Pressure","Top of layer",,"Operational"
3582.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"207002","Increase scale, reference value and data width",,,"Operational"
3583.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"008021","Time significance","= 27 First guess",,"Operational"
3584.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"015005","Ozone p",,,"Operational"
3585.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"008021","Time significance","Set to missing (cancel)",,"Operational"
3586.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"015005","Ozone p",,,"Operational"
3587.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"033007","Per cent confidence",,,"Operational"
3588.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"207000","Increase scale, reference value and data width","Cancel",,"Operational"
3589.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"008026","Matrix significance","= 0 Row of averaging kernel matrix",,"Operational"
3590.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"101020","Replicate 1 descriptor 20 times",,,"Operational"
3591.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"025143","Linear coefficient",,,"Operational"
3592.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"008026","Matrix significance","Set to missing (cancel)",,"Operational"
3593.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"008043","Atmospheric chemical or physical constituent type","= 0 Ozone",,"Operational"
3594.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"109015","Replicate 9 descriptors 15 times",,,"Operational"
3595.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"007004","Pressure",,,"Operational"
3596.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"008090","Decimal scale of following significands",,,"Operational"
3597.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"207006","Increase scale, reference value and data width",,,"Operational"
3598.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"015008","Significand of volumetric mixing ratio",,,"Operational"
3599.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"207000","Increase scale, reference value and data width","Cancel",,"Operational"
3600.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"008090","Decimal scale of following significands","Set to missing (cancel)",,"Operational"
3601.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"207002","Increase scale, reference value and data width",,,"Operational"
3602.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"033007","Per cent confidence",,,"Operational"
3603.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"207000","Increase scale, reference value and data width","Cancel",,"Operational"
3604.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"008043","Atmospheric chemical or physical constituent type","Set to missing (cancel)",,"Operational"
3605.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"033071","Profile ozone quality",,,"Operational"
3606.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"108008","Replicate 8 descriptors 8 times",,,"Operational"
3607.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"202124","Change scale",,,"Operational"
3608.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"201107","Change data width",,,"Operational"
3609.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"002071","Spectrographic wavelength",,,"Operational"
3610.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"201000","Change data width","Cancel",,"Operational"
3611.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"202000","Change scale","Cancel",,"Operational"
3612.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"207002","Increase scale, reference value and data width",,,"Operational"
3613.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"020081","Cloud amount in segment","Cloud fraction",,"Operational"
3614.00,"10","Vertical sounding sequences (satellite data)","310019","(Ozone data)",,"207000","Increase scale, reference value and data width","Cancel",,"Operational"
3615.00,"10","Vertical sounding sequences (satellite data)","310020","(Retrieved ozone data)",,"310022","Satellite identifier, instrument and product type",,,"Operational"
3616.00,"10","Vertical sounding sequences (satellite data)","310020","(Retrieved ozone data)",,"301011","Year, month, day",,,"Operational"
3617.00,"10","Vertical sounding sequences (satellite data)","310020","(Retrieved ozone data)",,"301013","Hour, minute, second",,,"Operational"
3618.00,"10","Vertical sounding sequences (satellite data)","310020","(Retrieved ozone data)",,"301021","Latitude/longitude (high accuracy)",,,"Operational"
3619.00,"10","Vertical sounding sequences (satellite data)","310020","(Retrieved ozone data)",,"304034","Latitude/longitude, solar elevation, number of layers",,,"Operational"
3620.00,"10","Vertical sounding sequences (satellite data)","310020","(Retrieved ozone data)",,"310021","Integrated ozone density, height of defined layer",,,"Operational"
3621.00,"10","Vertical sounding sequences (satellite data)","310021","(Integrated ozone density, height of defined layer)",,"108000","Delayed replication of 8 descriptors",,,"Operational"
3622.00,"10","Vertical sounding sequences (satellite data)","310021","(Integrated ozone density, height of defined layer)",,"031001","Delayed descriptor replication factor",,,"Operational"
3623.00,"10","Vertical sounding sequences (satellite data)","310021","(Integrated ozone density, height of defined layer)",,"201131","Change data width",,,"Operational"
3624.00,"10","Vertical sounding sequences (satellite data)","310021","(Integrated ozone density, height of defined layer)",,"202129","Change scale",,,"Operational"
3625.00,"10","Vertical sounding sequences (satellite data)","310021","(Integrated ozone density, height of defined layer)",,"007004","Pressure",,,"Operational"
3626.00,"10","Vertical sounding sequences (satellite data)","310021","(Integrated ozone density, height of defined layer)",,"007004","Pressure",,,"Operational"
3627.00,"10","Vertical sounding sequences (satellite data)","310021","(Integrated ozone density, height of defined layer)",,"202000","Change scale","Cancel",,"Operational"
3628.00,"10","Vertical sounding sequences (satellite data)","310021","(Integrated ozone density, height of defined layer)",,"201000","Change data width","Cancel",,"Operational"
3629.00,"10","Vertical sounding sequences (satellite data)","310021","(Integrated ozone density, height of defined layer)",,"015020","Integrated ozone density",,,"Operational"
3630.00,"10","Vertical sounding sequences (satellite data)","310021","(Integrated ozone density, height of defined layer)",,"010002","Height",,,"Operational"
3631.00,"10","Vertical sounding sequences (satellite data)","310022","(Satellite identifier, instrument and product type)",,"001007","Satellite identifier",,,"Operational"
3632.00,"10","Vertical sounding sequences (satellite data)","310022","(Satellite identifier, instrument and product type)",,"002019","Satellite instruments",,,"Operational"
3633.00,"10","Vertical sounding sequences (satellite data)","310022","(Satellite identifier, instrument and product type)",,"001033","Identification of originating/generating centre",,,"Operational"
3634.00,"10","Vertical sounding sequences (satellite data)","310022","(Satellite identifier, instrument and product type)",,"002172","Product type for retrieved atmospheric gases",,,"Operational"
3635.00,"10","Vertical sounding sequences (satellite data)","310023","(Geostationary multi-channel satellite radiance data)",,"301072","Satellite identification",,,"Operational"
3636.00,"10","Vertical sounding sequences (satellite data)","310023","(Geostationary multi-channel satellite radiance data)",,"030021","Number of pixels per row",,,"Operational"
3637.00,"10","Vertical sounding sequences (satellite data)","310023","(Geostationary multi-channel satellite radiance data)",,"030022","Number of pixels per column",,,"Operational"
3638.00,"10","Vertical sounding sequences (satellite data)","310023","(Geostationary multi-channel satellite radiance data)",,"008012","Land/sea qualifier",,,"Operational"
3639.00,"10","Vertical sounding sequences (satellite data)","310023","(Geostationary multi-channel satellite radiance data)",,"007024","Satellite zenith angle",,,"Operational"
3640.00,"10","Vertical sounding sequences (satellite data)","310023","(Geostationary multi-channel satellite radiance data)",,"007025","Solar zenith angle",,,"Operational"
3641.00,"10","Vertical sounding sequences (satellite data)","310023","(Geostationary multi-channel satellite radiance data)",,"010002","Height",,,"Operational"
3642.00,"10","Vertical sounding sequences (satellite data)","310023","(Geostationary multi-channel satellite radiance data)",,"101012","Replicate 1 descriptor 12 times",,,"Operational"
3643.00,"10","Vertical sounding sequences (satellite data)","310023","(Geostationary multi-channel satellite radiance data)",,"304032","Cloud fraction",,,"Operational"
3644.00,"10","Vertical sounding sequences (satellite data)","310023","(Geostationary multi-channel satellite radiance data)",,"105002","Replicate 5 descriptors 2 times",,,"Operational"
3645.00,"10","Vertical sounding sequences (satellite data)","310023","(Geostationary multi-channel satellite radiance data)",,"002152","Satellite instrument used in data processing",,,"Operational"
3646.00,"10","Vertical sounding sequences (satellite data)","310023","(Geostationary multi-channel satellite radiance data)",,"002024","Integrated mean humidity computational method",,,"Operational"
3647.00,"10","Vertical sounding sequences (satellite data)","310023","(Geostationary multi-channel satellite radiance data)",,"007004","Pressure",,,"Operational"
3648.00,"10","Vertical sounding sequences (satellite data)","310023","(Geostationary multi-channel satellite radiance data)",,"007004","Pressure",,,"Operational"
3649.00,"10","Vertical sounding sequences (satellite data)","310023","(Geostationary multi-channel satellite radiance data)",,"013003","Relative humidity",,,"Operational"
3650.00,"10","Vertical sounding sequences (satellite data)","310023","(Geostationary multi-channel satellite radiance data)",,"101012","Replicate 1 descriptor 12 times",,,"Operational"
3651.00,"10","Vertical sounding sequences (satellite data)","310023","(Geostationary multi-channel satellite radiance data)",,"304033","Clear sky radiance",,,"Operational"
3652.00,"10","Vertical sounding sequences (satellite data)","310024","(Geostationary three-channel satellite radiance data)",,"301072","Satellite identification",,,"Operational"
3653.00,"10","Vertical sounding sequences (satellite data)","310024","(Geostationary three-channel satellite radiance data)",,"030021","Number of pixels per row",,,"Operational"
3654.00,"10","Vertical sounding sequences (satellite data)","310024","(Geostationary three-channel satellite radiance data)",,"030022","Number of pixels per column",,,"Operational"
3655.00,"10","Vertical sounding sequences (satellite data)","310024","(Geostationary three-channel satellite radiance data)",,"008012","Land/sea qualifier",,,"Operational"
3656.00,"10","Vertical sounding sequences (satellite data)","310024","(Geostationary three-channel satellite radiance data)",,"007024","Satellite zenith angle",,,"Operational"
3657.00,"10","Vertical sounding sequences (satellite data)","310024","(Geostationary three-channel satellite radiance data)",,"007025","Solar zenith angle",,,"Operational"
3658.00,"10","Vertical sounding sequences (satellite data)","310024","(Geostationary three-channel satellite radiance data)",,"010002","Height",,,"Operational"
3659.00,"10","Vertical sounding sequences (satellite data)","310024","(Geostationary three-channel satellite radiance data)",,"101003","Replicate 1 descriptor 3 times",,,"Operational"
3660.00,"10","Vertical sounding sequences (satellite data)","310024","(Geostationary three-channel satellite radiance data)",,"304032","Cloud fraction",,,"Operational"
3661.00,"10","Vertical sounding sequences (satellite data)","310024","(Geostationary three-channel satellite radiance data)",,"105002","Replicate 5 descriptors 2 times",,,"Operational"
3662.00,"10","Vertical sounding sequences (satellite data)","310024","(Geostationary three-channel satellite radiance data)",,"002152","Satellite instrument used in data processing",,,"Operational"
3663.00,"10","Vertical sounding sequences (satellite data)","310024","(Geostationary three-channel satellite radiance data)",,"002024","Integrated mean humidity computational method",,,"Operational"
3664.00,"10","Vertical sounding sequences (satellite data)","310024","(Geostationary three-channel satellite radiance data)",,"007004","Pressure",,,"Operational"
3665.00,"10","Vertical sounding sequences (satellite data)","310024","(Geostationary three-channel satellite radiance data)",,"007004","Pressure",,,"Operational"
3666.00,"10","Vertical sounding sequences (satellite data)","310024","(Geostationary three-channel satellite radiance data)",,"013003","Relative humidity",,,"Operational"
3667.00,"10","Vertical sounding sequences (satellite data)","310024","(Geostationary three-channel satellite radiance data)",,"101003","Replicate 1 descriptor 3 times",,,"Operational"
3668.00,"10","Vertical sounding sequences (satellite data)","310024","(Geostationary three-channel satellite radiance data)",,"304033","Clear sky radiance",,,"Operational"
3669.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"001007","Satellite identifier",,,"Operational"
3670.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"008021","Time significance","Scan start",,"Operational"
3671.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"004001","Year",,,"Operational"
3672.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"004002","Month",,,"Operational"
3673.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"004003","Day",,,"Operational"
3674.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"004004","Hour",,,"Operational"
3675.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"004005","Minute",,,"Operational"
3676.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"201138","Change data width",,,"Operational"
3677.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"202131","Change scale",,,"Operational"
3678.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"004006","Second","Milliseconds",,"Operational"
3679.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"202000","Change scale",,,"Operational"
3680.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"201000","Change data width",,,"Operational"
3681.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"201132","Change data width",,,"Operational"
3682.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"005041","Scan line number","Scan number",,"Operational"
3683.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"201000","Change data width",,,"Operational"
3684.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"201129","Change data width",,,"Operational"
3685.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"005043","Field of view number","Scene number",,"Operational"
3686.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"201000","Change data width",,,"Operational"
3687.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"005002","Latitude (coarse accuracy)",,,"Operational"
3688.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"006002","Longitude (coarse accuracy)",,,"Operational"
3689.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"013040","Surface flag",,,"Operational"
3690.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"020029","Rain flag",,,"Operational"
3691.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"104024","Replicate 4 descriptors 24 times",,,"Operational"
3692.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"005042","Channel number",,,"Operational"
3693.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"012163","Brightness temperature",,,"Operational"
3694.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"021083","Warm target calibration",,,"Operational"
3695.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"021084","Cold target calibration",,,"Operational"
3696.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"115003","Replicate 15 descriptors 3 times",,,"Operational"
3697.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"004001","Year",,,"Operational"
3698.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"004002","Month",,,"Operational"
3699.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"004003","Day",,,"Operational"
3700.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"201142","Change data width",,,"Operational"
3701.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"202131","Change scale",,,"Operational"
3702.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"004026","Time period or displacement","Ephemeris milliseconds",,"Operational"
3703.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"202000","Change scale",,,"Operational"
3704.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"201000","Change data width",,,"Operational"
3705.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"005001","Latitude (high accuracy)","Ephemeris",,"Operational"
3706.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"006001","Longitude (high accuracy)","Ephemeris",,"Operational"
3707.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"201138","Change data width",,,"Operational"
3708.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"202129","Change scale",,,"Operational"
3709.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"007001","Height of station","Ephemeris",,"Operational"
3710.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"202000","Change scale",,,"Operational"
3711.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"201000","Change data width",,,"Operational"
3712.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"008021","Time significance","Orbit start",,"Operational"
3713.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"004001","Year",,,"Operational"
3714.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"004002","Month",,,"Operational"
3715.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"004003","Day",,,"Operational"
3716.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"004004","Hour",,,"Operational"
3717.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"004005","Minute",,,"Operational"
3718.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"005040","Orbit number",,,"Operational"
3719.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"101003","Replicate 1 descriptor 3 times",,,"Operational"
3720.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"012070","Warm load temperature",,,"Operational"
3721.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"025054","SSMIS subframe ID number",,,"Operational"
3722.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"101004","Replicate 1 descriptor 4 times",,,"Operational"
3723.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"025055","Multiplexer housekeeping",,,"Operational"
3724.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"008007","Dimensional significance","Line",,"Operational"
3725.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"104028","Replicate 4 descriptors 28 times",,,"Operational"
3726.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"005002","Latitude (coarse accuracy)",,,"Operational"
3727.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"006002","Longitude (coarse accuracy)",,,"Operational"
3728.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"002111","Radar incidence angle","Earth angle",,"Operational"
3729.00,"10","Vertical sounding sequences (satellite data)","310025","(SSMIS temperature data record)",,"005021","Bearing or azimuth",,,"Operational"
3730.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"310022","Satellite identifier, instrument and product type",,,"Operational"
3731.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"025060","Software identification",,,"Operational"
3732.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"008021","Time significance","= 17 Start of phenomenon",,"Operational"
3733.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"301011","Year, month, day",,,"Operational"
3734.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"301012","Hour, minute",,,"Operational"
3735.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"201138","Change data width","16 bits long",,"Operational"
3736.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"202131","Change scale","Scale: 3",,"Operational"
3737.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"004006","Second",,,"Operational"
3738.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"202000","Change scale","Cancel",,"Operational"
3739.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"201000","Change data width","Cancel",,"Operational"
3740.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"033039","Quality flags for radio occultation data",,,"Operational"
3741.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"033007","Per cent confidence","Whole message",,"Operational"
3742.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"304030","Location of platform",,,"Operational"
3743.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"304031","Speed of platform",,,"Operational"
3744.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"002020","Satellite classification",,,"Operational"
3745.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"001050","Platform transmitter ID number",,,"Operational"
3746.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"202127","Change scale","Scale: 1",,"Operational"
3747.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"304030","Location of platform",,,"Operational"
3748.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"202000","Change scale","Cancel",,"Operational"
3749.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"304031","Speed of platform",,,"Operational"
3750.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"201133","Change data width","18 bits long",,"Operational"
3751.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"202131","Change scale","Scale: 3",,"Operational"
3752.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"004016","Time increment",,,"Operational"
3753.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"202000","Change scale","Cancel",,"Operational"
3754.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"201000","Change data width","Cancel",,"Operational"
3755.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"301021","Latitude/longitude (high accuracy)",,,"Operational"
3756.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"304030","Location of platform",,,"Operational"
3757.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"010035","Earth's local radius of curvature",,,"Operational"
3758.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"005021","Bearing or azimuth",,,"Operational"
3759.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"010036","Geoid undulation",,,"Operational"
3760.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"113000","Delayed replication of 13 descriptors",,,"Operational"
3761.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"031002","Extended delayed descriptor replication factor",,,"Operational"
3762.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"301021","Latitude/longitude (high accuracy)",,,"Operational"
3763.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"005021","Bearing or azimuth",,,"Operational"
3764.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"108000","Delayed replication of 8 descriptors",,,"Operational"
3765.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"031001","Delayed descriptor replication factor",,,"Operational"
3766.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"002121","Mean frequency",,,"Operational"
3767.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"007040","Impact parameter",,,"Operational"
3768.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"015037","Bending angle",,,"Operational"
3769.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"008023","First-order statistics","= 13 Root-mean-square",,"Operational"
3770.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"201125","Change data width","20 bits long",,"Operational"
3771.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"015037","Bending angle",,,"Operational"
3772.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"201000","Change data width","Cancel",,"Operational"
3773.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"008023","First-order statistics","Set to missing",,"Operational"
3774.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"033007","Per cent confidence","All data for current replication",,"Operational"
3775.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"108000","Delayed replication of 8 descriptors",,,"Operational"
3776.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"031002","Extended delayed descriptor replication factor",,,"Operational"
3777.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"007007","Height",,,"Operational"
3778.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"015036","Atmospheric refractivity",,,"Operational"
3779.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"008023","First-order statistics","= 13 Root-mean-square",,"Operational"
3780.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"201123","Change data width","14 bits long",,"Operational"
3781.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"015036","Atmospheric refractivity",,,"Operational"
3782.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"201000","Change data width","Cancel",,"Operational"
3783.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"008023","First-order statistics","Set to missing",,"Operational"
3784.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"033007","Per cent confidence","All data for current height",,"Operational"
3785.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"116000","Delayed replication of 16 descriptors",,,"Operational"
3786.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"031002","Extended delayed descriptor replication factor",,,"Operational"
3787.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"007009","Geopotential height",,,"Operational"
3788.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"010004","Pressure",,,"Operational"
3789.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"012001","Temperature/air temperature",,,"Operational"
3790.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"013001","Specific humidity",,,"Operational"
3791.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"008023","First-order statistics","= 13 Root-mean-square",,"Operational"
3792.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"201120","Change data width","6 bits long",,"Operational"
3793.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"010004","Pressure",,,"Operational"
3794.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"201000","Change data width","Cancel",,"Operational"
3795.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"201122","Change data width","6 bits long",,"Operational"
3796.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"012001","Temperature/air temperature",,,"Operational"
3797.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"201000","Change data width","Cancel",,"Operational"
3798.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"201123","Change data width","9 bits long",,"Operational"
3799.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"013001","Specific humidity",,,"Operational"
3800.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"201000","Change data width","Cancel",,"Operational"
3801.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"008023","First-order statistics","Set to missing",,"Operational"
3802.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"033007","Per cent confidence","All data for current height",,"Operational"
3803.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"008003","Vertical significance (satellite observations)","= 0 Surface",,"Operational"
3804.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"007009","Geopotential height",,,"Operational"
3805.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"010004","Pressure",,,"Operational"
3806.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"008023","First-order statistics","= 13 Root-mean-square",,"Operational"
3807.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"201120","Change data width","6 bits long",,"Operational"
3808.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"010004","Pressure",,,"Operational"
3809.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"201000","Change data width","Cancel",,"Operational"
3810.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"008023","First-order statistics","Set to missing",,"Operational"
3811.00,"10","Vertical sounding sequences (satellite data)","310026","(Satellite radio occultation data)",,"033007","Per cent confidence","Surface data",,"Operational"
3812.00,"10","Vertical sounding sequences (satellite data)","310027","(All sky radiance product main sequence)",,"301071","Satellite identifier/Generating resolution","Product information",,"Deprecated"
3813.00,"10","Vertical sounding sequences (satellite data)","310027","(All sky radiance product main sequence)",,"301011","Year, month, day",,,"Deprecated"
3814.00,"10","Vertical sounding sequences (satellite data)","310027","(All sky radiance product main sequence)",,"301013","Hour, minute, second",,,"Deprecated"
3815.00,"10","Vertical sounding sequences (satellite data)","310027","(All sky radiance product main sequence)",,"301021","Latitude/longitude (high accuracy)",,,"Deprecated"
3816.00,"10","Vertical sounding sequences (satellite data)","310027","(All sky radiance product main sequence)",,"030021","Number of pixels per row",,,"Deprecated"
3817.00,"10","Vertical sounding sequences (satellite data)","310027","(All sky radiance product main sequence)",,"030022","Number of pixels per column",,,"Deprecated"
3818.00,"10","Vertical sounding sequences (satellite data)","310027","(All sky radiance product main sequence)",,"010002","Height","Orbit height",,"Deprecated"
3819.00,"10","Vertical sounding sequences (satellite data)","310027","(All sky radiance product main sequence)",,"304036","Cloud coverage",,,"Deprecated"
3820.00,"10","Vertical sounding sequences (satellite data)","310027","(All sky radiance product main sequence)",,"002152","Satellite instrument used in data processing",,,"Deprecated"
3821.00,"10","Vertical sounding sequences (satellite data)","310027","(All sky radiance product main sequence)",,"002167","Radiance computational method",,,"Deprecated"
3822.00,"10","Vertical sounding sequences (satellite data)","310027","(All sky radiance product main sequence)",,"101011","Replicate 1 descriptor 11 times",,,"Deprecated"
3823.00,"10","Vertical sounding sequences (satellite data)","310027","(All sky radiance product main sequence)",,"304035","All sky radiance data",,,"Deprecated"
3824.00,"10","Vertical sounding sequences (satellite data)","310028","(All sky radiance product main sequence)",,"301071","Satellite identifier/Generating resolution","Product information",,"Operational"
3825.00,"10","Vertical sounding sequences (satellite data)","310028","(All sky radiance product main sequence)",,"301011","Year, month, day",,,"Operational"
3826.00,"10","Vertical sounding sequences (satellite data)","310028","(All sky radiance product main sequence)",,"301013","Hour, minute, second",,,"Operational"
3827.00,"10","Vertical sounding sequences (satellite data)","310028","(All sky radiance product main sequence)",,"301021","Latitude/longitude (high accuracy)",,,"Operational"
3828.00,"10","Vertical sounding sequences (satellite data)","310028","(All sky radiance product main sequence)",,"030021","Number of pixels per row",,,"Operational"
3829.00,"10","Vertical sounding sequences (satellite data)","310028","(All sky radiance product main sequence)",,"030022","Number of pixels per column",,,"Operational"
3830.00,"10","Vertical sounding sequences (satellite data)","310028","(All sky radiance product main sequence)",,"010002","Height","Orbit height",,"Operational"
3831.00,"10","Vertical sounding sequences (satellite data)","310028","(All sky radiance product main sequence)",,"304036","Cloud coverage",,,"Operational"
3832.00,"10","Vertical sounding sequences (satellite data)","310028","(All sky radiance product main sequence)",,"002152","Satellite instrument used in data processing",,,"Operational"
3833.00,"10","Vertical sounding sequences (satellite data)","310028","(All sky radiance product main sequence)",,"002167","Radiance computational method",,,"Operational"
3834.00,"10","Vertical sounding sequences (satellite data)","310028","(All sky radiance product main sequence)",,"101011","Replicate 1 descriptor 11 times",,,"Operational"
3835.00,"10","Vertical sounding sequences (satellite data)","310028","(All sky radiance product main sequence)",,"304037","All sky radiance data",,,"Operational"
3836.00,"10","Vertical sounding sequences (satellite data)","310029","(Layer, ozone, height, temperature and water vapour)",,"110000","Delayed replication of 10 descriptors",,,"Operational"
3837.00,"10","Vertical sounding sequences (satellite data)","310029","(Layer, ozone, height, temperature and water vapour)",,"031001","Delayed descriptor replication factor",,,"Operational"
3838.00,"10","Vertical sounding sequences (satellite data)","310029","(Layer, ozone, height, temperature and water vapour)",,"201138","Change data width",,,"Operational"
3839.00,"10","Vertical sounding sequences (satellite data)","310029","(Layer, ozone, height, temperature and water vapour)",,"202130","Change scale",,,"Operational"
3840.00,"10","Vertical sounding sequences (satellite data)","310029","(Layer, ozone, height, temperature and water vapour)",,"007004","Pressure",,,"Operational"
3841.00,"10","Vertical sounding sequences (satellite data)","310029","(Layer, ozone, height, temperature and water vapour)",,"007004","Pressure",,,"Operational"
3842.00,"10","Vertical sounding sequences (satellite data)","310029","(Layer, ozone, height, temperature and water vapour)",,"202000","Change scale","Cancel",,"Operational"
3843.00,"10","Vertical sounding sequences (satellite data)","310029","(Layer, ozone, height, temperature and water vapour)",,"201000","Change data width","Cancel",,"Operational"
3844.00,"10","Vertical sounding sequences (satellite data)","310029","(Layer, ozone, height, temperature and water vapour)",,"015020","Integrated ozone density",,,"Operational"
3845.00,"10","Vertical sounding sequences (satellite data)","310029","(Layer, ozone, height, temperature and water vapour)",,"010002","Height",,,"Operational"
3846.00,"10","Vertical sounding sequences (satellite data)","310029","(Layer, ozone, height, temperature and water vapour)",,"012101","Temperature/air temperature",,,"Operational"
3847.00,"10","Vertical sounding sequences (satellite data)","310029","(Layer, ozone, height, temperature and water vapour)",,"013098","Integrated water vapour density",,,"Operational"
3848.00,"10","Vertical sounding sequences (satellite data)","310030","(MIPAS or GOMOS instruments reporting)",,"310022","Satellite identifier, instrument and product type",,,"Operational"
3849.00,"10","Vertical sounding sequences (satellite data)","310030","(MIPAS or GOMOS instruments reporting)",,"301011","Year, month, day",,,"Operational"
3850.00,"10","Vertical sounding sequences (satellite data)","310030","(MIPAS or GOMOS instruments reporting)",,"301013","Hour, minute, second",,,"Operational"
3851.00,"10","Vertical sounding sequences (satellite data)","310030","(MIPAS or GOMOS instruments reporting)",,"301021","Latitude/longitude (high accuracy)",,,"Operational"
3852.00,"10","Vertical sounding sequences (satellite data)","310030","(MIPAS or GOMOS instruments reporting)",,"304034","Latitude/longitude, solar elevation, number of layers",,,"Operational"
3853.00,"10","Vertical sounding sequences (satellite data)","310030","(MIPAS or GOMOS instruments reporting)",,"310029","Layer, ozone, height, temperature and water vapour",,,"Operational"
3854.00,"10","Vertical sounding sequences (satellite data)","310050","(Satellite collocated 1C reports with 3 instruments)",,"310051","Satellite position and instrument temperatures",,,"Operational"
3855.00,"10","Vertical sounding sequences (satellite data)","310050","(Satellite collocated 1C reports with 3 instruments)",,"310052","Satellite instrument type and position","AIRS",,"Operational"
3856.00,"10","Vertical sounding sequences (satellite data)","310050","(Satellite collocated 1C reports with 3 instruments)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
3857.00,"10","Vertical sounding sequences (satellite data)","310050","(Satellite collocated 1C reports with 3 instruments)",,"031002","Extended delayed descriptor replication factor",,,"Operational"
3858.00,"10","Vertical sounding sequences (satellite data)","310050","(Satellite collocated 1C reports with 3 instruments)",,"310053","Satellite channels and brightness temperatures with expanded channel set","AIRS",,"Operational"
3859.00,"10","Vertical sounding sequences (satellite data)","310050","(Satellite collocated 1C reports with 3 instruments)",,"101004","Replicate 1 descriptor 4 times",,,"Operational"
3860.00,"10","Vertical sounding sequences (satellite data)","310050","(Satellite collocated 1C reports with 3 instruments)",,"310054","Satellite visible channels and albedos with expanded channel set",,,"Operational"
3861.00,"10","Vertical sounding sequences (satellite data)","310050","(Satellite collocated 1C reports with 3 instruments)",,"020010","Cloud cover (total)",,,"Operational"
3862.00,"10","Vertical sounding sequences (satellite data)","310050","(Satellite collocated 1C reports with 3 instruments)",,"310052","Satellite instrument type and position","AMSU-A",,"Operational"
3863.00,"10","Vertical sounding sequences (satellite data)","310050","(Satellite collocated 1C reports with 3 instruments)",,"101015","Replicate 1 descriptor 15 times",,,"Operational"
3864.00,"10","Vertical sounding sequences (satellite data)","310050","(Satellite collocated 1C reports with 3 instruments)",,"310053","Satellite channels and brightness temperatures with expanded channel set","AMSU-A",,"Operational"
3865.00,"10","Vertical sounding sequences (satellite data)","310050","(Satellite collocated 1C reports with 3 instruments)",,"310052","Satellite instrument type and position","HSB",,"Operational"
3866.00,"10","Vertical sounding sequences (satellite data)","310050","(Satellite collocated 1C reports with 3 instruments)",,"101005","Replicate 1 descriptor 5 times",,,"Operational"
3867.00,"10","Vertical sounding sequences (satellite data)","310050","(Satellite collocated 1C reports with 3 instruments)",,"310053","Satellite channels and brightness temperatures with expanded channel set","HSB",,"Operational"
3868.00,"10","Vertical sounding sequences (satellite data)","310051","(Satellite position and instrument temperatures)",,"001007","Satellite identifier",,,"Operational"
3869.00,"10","Vertical sounding sequences (satellite data)","310051","(Satellite position and instrument temperatures)",,"005040","Orbit number",,,"Operational"
3870.00,"10","Vertical sounding sequences (satellite data)","310051","(Satellite position and instrument temperatures)",,"201133","Change data width",,,"Operational"
3871.00,"10","Vertical sounding sequences (satellite data)","310051","(Satellite position and instrument temperatures)",,"005041","Scan line number",,,"Operational"
3872.00,"10","Vertical sounding sequences (satellite data)","310051","(Satellite position and instrument temperatures)",,"201000","Change data width","Cancel",,"Operational"
3873.00,"10","Vertical sounding sequences (satellite data)","310051","(Satellite position and instrument temperatures)",,"201132","Change data width",,,"Operational"
3874.00,"10","Vertical sounding sequences (satellite data)","310051","(Satellite position and instrument temperatures)",,"025070","Major frame count",,,"Operational"
3875.00,"10","Vertical sounding sequences (satellite data)","310051","(Satellite position and instrument temperatures)",,"201000","Change data width","Cancel",,"Operational"
3876.00,"10","Vertical sounding sequences (satellite data)","310051","(Satellite position and instrument temperatures)",,"202126","Change scale",,,"Operational"
3877.00,"10","Vertical sounding sequences (satellite data)","310051","(Satellite position and instrument temperatures)",,"007001","Height of station",,,"Operational"
3878.00,"10","Vertical sounding sequences (satellite data)","310051","(Satellite position and instrument temperatures)",,"202000","Change scale","Cancel",,"Operational"
3879.00,"10","Vertical sounding sequences (satellite data)","310051","(Satellite position and instrument temperatures)",,"007025","Solar zenith angle",,,"Operational"
3880.00,"10","Vertical sounding sequences (satellite data)","310051","(Satellite position and instrument temperatures)",,"005022","Solar azimuth",,,"Operational"
3881.00,"10","Vertical sounding sequences (satellite data)","310051","(Satellite position and instrument temperatures)",,"102009","Replicate 2 descriptors 9 times",,,"Operational"
3882.00,"10","Vertical sounding sequences (satellite data)","310051","(Satellite position and instrument temperatures)",,"002151","Radiometer identifier",,,"Operational"
3883.00,"10","Vertical sounding sequences (satellite data)","310051","(Satellite position and instrument temperatures)",,"012064","Instrument temperature",,,"Operational"
3884.00,"10","Vertical sounding sequences (satellite data)","310052","(Satellite instrument type and position)",,"002019","Satellite instruments",,,"Operational"
3885.00,"10","Vertical sounding sequences (satellite data)","310052","(Satellite instrument type and position)",,"301011","Year, month, day",,,"Operational"
3886.00,"10","Vertical sounding sequences (satellite data)","310052","(Satellite instrument type and position)",,"301012","Hour, minute",,,"Operational"
3887.00,"10","Vertical sounding sequences (satellite data)","310052","(Satellite instrument type and position)",,"202131","Change scale",,,"Operational"
3888.00,"10","Vertical sounding sequences (satellite data)","310052","(Satellite instrument type and position)",,"201138","Change data width",,,"Operational"
3889.00,"10","Vertical sounding sequences (satellite data)","310052","(Satellite instrument type and position)",,"004006","Second",,,"Operational"
3890.00,"10","Vertical sounding sequences (satellite data)","310052","(Satellite instrument type and position)",,"201000","Change data width","Cancel",,"Operational"
3891.00,"10","Vertical sounding sequences (satellite data)","310052","(Satellite instrument type and position)",,"202000","Change scale","Cancel",,"Operational"
3892.00,"10","Vertical sounding sequences (satellite data)","310052","(Satellite instrument type and position)",,"301021","Latitude/longitude (high accuracy)",,,"Operational"
3893.00,"10","Vertical sounding sequences (satellite data)","310052","(Satellite instrument type and position)",,"007024","Satellite zenith angle",,,"Operational"
3894.00,"10","Vertical sounding sequences (satellite data)","310052","(Satellite instrument type and position)",,"005021","Bearing or azimuth",,,"Operational"
3895.00,"10","Vertical sounding sequences (satellite data)","310052","(Satellite instrument type and position)",,"005043","Field of view number",,,"Operational"
3896.00,"10","Vertical sounding sequences (satellite data)","310053","(Satellite channels and brightness temperatures with expanded channel set)",,"201134","Change data width",,,"Operational"
3897.00,"10","Vertical sounding sequences (satellite data)","310053","(Satellite channels and brightness temperatures with expanded channel set)",,"005042","Channel number",,,"Operational"
3898.00,"10","Vertical sounding sequences (satellite data)","310053","(Satellite channels and brightness temperatures with expanded channel set)",,"201000","Change data width","Cancel",,"Operational"
3899.00,"10","Vertical sounding sequences (satellite data)","310053","(Satellite channels and brightness temperatures with expanded channel set)",,"025076","Log10 of (temperature-radiance central wave number) for ATOVS",,,"Operational"
3900.00,"10","Vertical sounding sequences (satellite data)","310053","(Satellite channels and brightness temperatures with expanded channel set)",,"033032","Channel quality flags for ATOVS",,,"Operational"
3901.00,"10","Vertical sounding sequences (satellite data)","310053","(Satellite channels and brightness temperatures with expanded channel set)",,"012163","Brightness temperature","Scale: 2",,"Operational"
3902.00,"10","Vertical sounding sequences (satellite data)","310054","(Satellite visible channels and albedos with expanded channel set)",,"201134","Change data width",,,"Operational"
3903.00,"10","Vertical sounding sequences (satellite data)","310054","(Satellite visible channels and albedos with expanded channel set)",,"005042","Channel number",,,"Operational"
3904.00,"10","Vertical sounding sequences (satellite data)","310054","(Satellite visible channels and albedos with expanded channel set)",,"201000","Change data width","Cancel",,"Operational"
3905.00,"10","Vertical sounding sequences (satellite data)","310054","(Satellite visible channels and albedos with expanded channel set)",,"025076","Log10 of (temperature-radiance central wave number) for ATOVS",,,"Operational"
3906.00,"10","Vertical sounding sequences (satellite data)","310054","(Satellite visible channels and albedos with expanded channel set)",,"033032","Channel quality flags for ATOVS",,,"Operational"
3907.00,"10","Vertical sounding sequences (satellite data)","310054","(Satellite visible channels and albedos with expanded channel set)",,"201131","Change data width",,,"Operational"
3908.00,"10","Vertical sounding sequences (satellite data)","310054","(Satellite visible channels and albedos with expanded channel set)",,"202129","Change scale",,,"Operational"
3909.00,"10","Vertical sounding sequences (satellite data)","310054","(Satellite visible channels and albedos with expanded channel set)",,"102002","Replicate 2 descriptors 2 times",,,"Operational"
3910.00,"10","Vertical sounding sequences (satellite data)","310054","(Satellite visible channels and albedos with expanded channel set)",,"008023","First-order statistics",,,"Operational"
3911.00,"10","Vertical sounding sequences (satellite data)","310054","(Satellite visible channels and albedos with expanded channel set)",,"014027","Albedo",,,"Operational"
3912.00,"10","Vertical sounding sequences (satellite data)","310054","(Satellite visible channels and albedos with expanded channel set)",,"008023","First-order statistics",,,"Operational"
3913.00,"10","Vertical sounding sequences (satellite data)","310054","(Satellite visible channels and albedos with expanded channel set)",,"202000","Change scale","Cancel",,"Operational"
3914.00,"10","Vertical sounding sequences (satellite data)","310054","(Satellite visible channels and albedos with expanded channel set)",,"201000","Change data width","Cancel",,"Operational"
3915.00,"10","Vertical sounding sequences (satellite data)","310055","(Satellite radiance/channel principal components)",,"310051","Satellite position and instrument temperatures",,,"Operational"
3916.00,"10","Vertical sounding sequences (satellite data)","310055","(Satellite radiance/channel principal components)",,"310052","Satellite instrument type and position","AIRS",,"Operational"
3917.00,"10","Vertical sounding sequences (satellite data)","310055","(Satellite radiance/channel principal components)",,"102020","Replicate 2 descriptors 20 times",,,"Operational"
3918.00,"10","Vertical sounding sequences (satellite data)","310055","(Satellite radiance/channel principal components)",,"025076","Log10 of (temperature-radiance central wave number) for ATOVS",,,"Operational"
3919.00,"10","Vertical sounding sequences (satellite data)","310055","(Satellite radiance/channel principal components)",,"025052","Log10 of principal components normalized fit to data",,,"Operational"
3920.00,"10","Vertical sounding sequences (satellite data)","310055","(Satellite radiance/channel principal components)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
3921.00,"10","Vertical sounding sequences (satellite data)","310055","(Satellite radiance/channel principal components)",,"031002","Extended delayed descriptor replication factor",,,"Operational"
3922.00,"10","Vertical sounding sequences (satellite data)","310055","(Satellite radiance/channel principal components)",,"025050","Principal component score","Satellite radiance",,"Operational"
3923.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"001007","Satellite identifier",,,"Operational"
3924.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"001033","Identification of originating/generating centre",,,"Operational"
3925.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"002019","Satellite instruments",,,"Operational"
3926.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"002020","Satellite classification",,,"Operational"
3927.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"301011","Year, month, day",,,"Operational"
3928.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"301012","Hour, minute",,,"Operational"
3929.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"207003","Increase scale, reference value and data width",,,"Operational"
3930.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"004006","Second",,,"Operational"
3931.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"207000","Increase scale, reference value and data width","Cancel",,"Operational"
3932.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"304030","Location of platform",,,"Operational"
3933.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"301021","Latitude/longitude (high accuracy)",,,"Operational"
3934.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"007024","Satellite zenith angle",,,"Operational"
3935.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"005021","Bearing or azimuth",,,"Operational"
3936.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"007025","Solar zenith angle",,,"Operational"
3937.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"005022","Solar azimuth",,,"Operational"
3938.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"008075","Ascending/descending orbit qualifier",,,"Operational"
3939.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"201133","Change data width","Increase bit width",,"Operational"
3940.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"005041","Scan line number",,,"Operational"
3941.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"201000","Change data width","Cancel increase bit width",,"Operational"
3942.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"005045","Field of regard number",,,"Operational"
3943.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"005043","Field of view number",,,"Operational"
3944.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"005040","Orbit number",,,"Operational"
3945.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"010001","Height of land surface",,,"Operational"
3946.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"201129","Change data width","Increase bit width",,"Operational"
3947.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"007002","Height or altitude",,,"Operational"
3948.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"201000","Change data width","Cancel increase bit width",,"Operational"
3949.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"202127","Change scale","Increase scale",,"Operational"
3950.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"201125","Change data width","Increase bit width",,"Operational"
3951.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"021166","Land fraction",,,"Operational"
3952.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"201000","Change data width","Cancel increase bit width",,"Operational"
3953.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"202000","Change scale","Cancel increase scale",,"Operational"
3954.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"008012","Land/sea qualifier",,,"Operational"
3955.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"020010","Cloud cover (total)",,,"Operational"
3956.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"020014","Height of top of cloud",,,"Operational"
3957.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"002165","Radiance type flags",,,"Operational"
3958.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"033075","Scan-level quality flags",,,"Operational"
3959.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"107003","Replicate 7 descriptors 3 times",,,"Operational"
3960.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"008076","Type of band",,,"Operational"
3961.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"006029","Wave number","Start of range",,"Operational"
3962.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"006029","Wave number","End of range",,"Operational"
3963.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"025140","Start channel",,,"Operational"
3964.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"025141","End channel",,,"Operational"
3965.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"033076","Calibration quality flags",,,"Operational"
3966.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"033077","Field-of-view quality flags",,,"Operational"
3967.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"008076","Type of band","Set to missing (cancel)",,"Operational"
3968.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"033078","Geolocation quality",,,"Operational"
3969.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"033003","Quality information",,,"Operational"
3970.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"104000","Delayed replication of 4 descriptors",,,"Operational"
3971.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"031002","Extended delayed descriptor replication factor",,,"Operational"
3972.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"201133","Change data width","Increase bit width",,"Operational"
3973.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"005042","Channel number",,,"Operational"
3974.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"201000","Change data width","Cancel increase bit width",,"Operational"
3975.00,"10","Vertical sounding sequences (satellite data)","310060","(CrIS (Cross-Track Infrared Sounder) radiance data)",,"014044","Channel radiance",,,"Operational"
3976.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"001007","Satellite identifier",,,"Operational"
3977.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"001033","Identification of originating/generating centre",,,"Operational"
3978.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"001034","Identification of originating/generating sub-centre",,,"Operational"
3979.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"002019","Satellite instruments",,,"Operational"
3980.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"002020","Satellite classification",,,"Operational"
3981.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"301011","Year, month, day",,,"Operational"
3982.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"301012","Hour, minute",,,"Operational"
3983.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"207003","Increase scale, reference value and data width",,,"Operational"
3984.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"004006","Second",,,"Operational"
3985.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"207000","Increase scale, reference value and data width","Cancel",,"Operational"
3986.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"005040","Orbit number",,,"Operational"
3987.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"005041","Scan line number",,,"Operational"
3988.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"005043","Field of view number",,,"Operational"
3989.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"033079","Granule level quality flags",,,"Operational"
3990.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"033080","Scan level quality flags",,,"Operational"
3991.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"033078","Geolocation quality",,,"Operational"
3992.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"301021","Latitude/longitude (high accuracy)",,,"Operational"
3993.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"201129","Change data width","Increase bit width",,"Operational"
3994.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"007002","Height or altitude",,,"Operational"
3995.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"201000","Change data width","Cancel increase bit width",,"Operational"
3996.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"007024","Satellite zenith angle",,,"Operational"
3997.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"005021","Bearing or azimuth",,,"Operational"
3998.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"007025","Solar zenith angle",,,"Operational"
3999.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"005022","Solar azimuth",,,"Operational"
4000.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"025075","Satellite antenna corrections version number",,,"Operational"
4001.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"111000","Delayed replication of 11 descriptors",,,"Operational"
4002.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"031002","Extended delayed descriptor replication factor",,,"Operational"
4003.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"005042","Channel number",,,"Operational"
4004.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"202131","Change scale","Increase scale by 3",,"Operational"
4005.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"002153","Satellite channel centre frequency",,,"Operational"
4006.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"002154","Satellite channel band width",,,"Operational"
4007.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"202000","Change scale","Cancel increase scale",,"Operational"
4008.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"002104","Antenna polarization",,,"Operational"
4009.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"012066","Antenna temperature",,,"Operational"
4010.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"012163","Brightness temperature",,,"Operational"
4011.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"012158","Noise-equivalent delta temperature while viewing cold target",,,"Operational"
4012.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"012159","Noise-equivalent delta temperature while viewing warm target",,,"Operational"
4013.00,"10","Vertical sounding sequences (satellite data)","310061","(ATMS (Advanced Technology Microwave Sounder) data)",,"033081","Channel data quality flags",,,"Operational"
4014.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"001007","Satellite identifier",,,"Operational"
4015.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"001033","Identification of originating/generating centre",,,"Operational"
4016.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"001034","Identification of originating/generating sub-centre",,,"Operational"
4017.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"002019","Satellite instruments",,,"Operational"
4018.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"002020","Satellite classification",,,"Operational"
4019.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"301011","Year, month, day",,,"Operational"
4020.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"301012","Hour, minute",,,"Operational"
4021.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"207003","Increase scale, reference value and data width",,,"Operational"
4022.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"004006","Second",,,"Operational"
4023.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"207000","Increase scale, reference value and data width","Cancel",,"Operational"
4024.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"005040","Orbit number",,,"Operational"
4025.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"201133","Change data width","Increase bit width",,"Operational"
4026.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"005041","Scan line number",,,"Operational"
4027.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"005043","Field of view number",,,"Operational"
4028.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"201000","Change data width","Cancel increase bit width",,"Operational"
4029.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"008076","Type of band",,,"Operational"
4030.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"033082","Geolocation quality flags",,,"Operational"
4031.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"301021","Latitude/longitude (high accuracy)",,,"Operational"
4032.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"201129","Change data width","Increase bit width",,"Operational"
4033.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"007002","Height or altitude",,,"Operational"
4034.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"201000","Change data width","Cancel increase bit width",,"Operational"
4035.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"007024","Satellite zenith angle",,,"Operational"
4036.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"005021","Bearing or azimuth",,,"Operational"
4037.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"007025","Solar zenith angle",,,"Operational"
4038.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"005022","Solar azimuth",,,"Operational"
4039.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"008072","Pixel(s) type",,,"Operational"
4040.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"008029","Surface type",,,"Operational"
4041.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"105000","Delayed replication of 5 descriptors",,,"Operational"
4042.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"031002","Extended delayed descriptor replication factor",,,"Operational"
4043.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"005042","Channel number",,,"Operational"
4044.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"002155","Satellite channel wavelength",,,"Operational"
4045.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"033083","Radiance data quality flags",,,"Operational"
4046.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"014043","Channel radiance",,,"Operational"
4047.00,"10","Vertical sounding sequences (satellite data)","310062","(VIIRS (Visible/Infrared Imager Radiometer Suite) data)",,"015042","Reflectance",,,"Operational"
4048.00,"10","Vertical sounding sequences (satellite data)","310063","(SST (Sea-surface temperature) data)",,"001007","Satellite identifier",,,"Operational"
4049.00,"10","Vertical sounding sequences (satellite data)","310063","(SST (Sea-surface temperature) data)",,"001033","Identification of originating/generating centre",,,"Operational"
4050.00,"10","Vertical sounding sequences (satellite data)","310063","(SST (Sea-surface temperature) data)",,"001034","Identification of originating/generating sub-centre",,,"Operational"
4051.00,"10","Vertical sounding sequences (satellite data)","310063","(SST (Sea-surface temperature) data)",,"002019","Satellite instruments",,,"Operational"
4052.00,"10","Vertical sounding sequences (satellite data)","310063","(SST (Sea-surface temperature) data)",,"002020","Satellite classification",,,"Operational"
4053.00,"10","Vertical sounding sequences (satellite data)","310063","(SST (Sea-surface temperature) data)",,"301011","Year, month, day",,,"Operational"
4054.00,"10","Vertical sounding sequences (satellite data)","310063","(SST (Sea-surface temperature) data)",,"301012","Hour, minute",,,"Operational"
4055.00,"10","Vertical sounding sequences (satellite data)","310063","(SST (Sea-surface temperature) data)",,"207003","Increase scale, reference value and data width",,,"Operational"
4056.00,"10","Vertical sounding sequences (satellite data)","310063","(SST (Sea-surface temperature) data)",,"004006","Second",,,"Operational"
4057.00,"10","Vertical sounding sequences (satellite data)","310063","(SST (Sea-surface temperature) data)",,"207000","Increase scale, reference value and data width","Cancel",,"Operational"
4058.00,"10","Vertical sounding sequences (satellite data)","310063","(SST (Sea-surface temperature) data)",,"005040","Orbit number",,,"Operational"
4059.00,"10","Vertical sounding sequences (satellite data)","310063","(SST (Sea-surface temperature) data)",,"201133","Change data width","Increase bit width",,"Operational"
4060.00,"10","Vertical sounding sequences (satellite data)","310063","(SST (Sea-surface temperature) data)",,"005041","Scan line number",,,"Operational"
4061.00,"10","Vertical sounding sequences (satellite data)","310063","(SST (Sea-surface temperature) data)",,"005043","Field of view number",,,"Operational"
4062.00,"10","Vertical sounding sequences (satellite data)","310063","(SST (Sea-surface temperature) data)",,"201000","Change data width","Cancel increase bit width",,"Operational"
4063.00,"10","Vertical sounding sequences (satellite data)","310063","(SST (Sea-surface temperature) data)",,"033082","Geolocation quality flags",,,"Operational"
4064.00,"10","Vertical sounding sequences (satellite data)","310063","(SST (Sea-surface temperature) data)",,"301021","Latitude/longitude (high accuracy)",,,"Operational"
4065.00,"10","Vertical sounding sequences (satellite data)","310063","(SST (Sea-surface temperature) data)",,"201129","Change data width","Increase bit width",,"Operational"
4066.00,"10","Vertical sounding sequences (satellite data)","310063","(SST (Sea-surface temperature) data)",,"007002","Height or altitude",,,"Operational"
4067.00,"10","Vertical sounding sequences (satellite data)","310063","(SST (Sea-surface temperature) data)",,"201000","Change data width","Cancel increase bit width",,"Operational"
4068.00,"10","Vertical sounding sequences (satellite data)","310063","(SST (Sea-surface temperature) data)",,"007024","Satellite zenith angle",,,"Operational"
4069.00,"10","Vertical sounding sequences (satellite data)","310063","(SST (Sea-surface temperature) data)",,"005021","Bearing or azimuth",,,"Operational"
4070.00,"10","Vertical sounding sequences (satellite data)","310063","(SST (Sea-surface temperature) data)",,"007025","Solar zenith angle",,,"Operational"
4071.00,"10","Vertical sounding sequences (satellite data)","310063","(SST (Sea-surface temperature) data)",,"005022","Solar azimuth",,,"Operational"
4072.00,"10","Vertical sounding sequences (satellite data)","310063","(SST (Sea-surface temperature) data)",,"008075","Ascending/descending orbit qualifier",,,"Operational"
4073.00,"10","Vertical sounding sequences (satellite data)","310063","(SST (Sea-surface temperature) data)",,"008013","Day/night qualifier",,,"Operational"
4074.00,"10","Vertical sounding sequences (satellite data)","310063","(SST (Sea-surface temperature) data)",,"008072","Pixel(s) type",,,"Operational"
4075.00,"10","Vertical sounding sequences (satellite data)","310063","(SST (Sea-surface temperature) data)",,"033084","Pixel level quality flags",,,"Operational"
4076.00,"10","Vertical sounding sequences (satellite data)","310063","(SST (Sea-surface temperature) data)",,"007062","Depth below sea/water surface",,,"Operational"
4077.00,"10","Vertical sounding sequences (satellite data)","310063","(SST (Sea-surface temperature) data)",,"033086","Quality of pixel level retrieval",,,"Operational"
4078.00,"10","Vertical sounding sequences (satellite data)","310063","(SST (Sea-surface temperature) data)",,"022043","Sea/water temperature",,,"Operational"
4079.00,"10","Vertical sounding sequences (satellite data)","310063","(SST (Sea-surface temperature) data)",,"007062","Depth below sea/water surface","Top of layer",,"Operational"
4080.00,"10","Vertical sounding sequences (satellite data)","310063","(SST (Sea-surface temperature) data)",,"007062","Depth below sea/water surface","Bottom of layer",,"Operational"
4081.00,"10","Vertical sounding sequences (satellite data)","310063","(SST (Sea-surface temperature) data)",,"033086","Quality of pixel level retrieval",,,"Operational"
4082.00,"10","Vertical sounding sequences (satellite data)","310063","(SST (Sea-surface temperature) data)",,"022043","Sea/water temperature",,,"Operational"
4083.00,"10","Vertical sounding sequences (satellite data)","310064","(AOT (Aerosol optical thickness) data)",,"001007","Satellite identifier",,,"Operational"
4084.00,"10","Vertical sounding sequences (satellite data)","310064","(AOT (Aerosol optical thickness) data)",,"001033","Identification of originating/generating centre",,,"Operational"
4085.00,"10","Vertical sounding sequences (satellite data)","310064","(AOT (Aerosol optical thickness) data)",,"001034","Identification of originating/generating sub-centre",,,"Operational"
4086.00,"10","Vertical sounding sequences (satellite data)","310064","(AOT (Aerosol optical thickness) data)",,"002019","Satellite instruments",,,"Operational"
4087.00,"10","Vertical sounding sequences (satellite data)","310064","(AOT (Aerosol optical thickness) data)",,"002020","Satellite classification",,,"Operational"
4088.00,"10","Vertical sounding sequences (satellite data)","310064","(AOT (Aerosol optical thickness) data)",,"301011","Year, month, day",,,"Operational"
4089.00,"10","Vertical sounding sequences (satellite data)","310064","(AOT (Aerosol optical thickness) data)",,"301012","Hour, minute",,,"Operational"
4090.00,"10","Vertical sounding sequences (satellite data)","310064","(AOT (Aerosol optical thickness) data)",,"207003","Increase scale, reference value and data width",,,"Operational"
4091.00,"10","Vertical sounding sequences (satellite data)","310064","(AOT (Aerosol optical thickness) data)",,"004006","Second",,,"Operational"
4092.00,"10","Vertical sounding sequences (satellite data)","310064","(AOT (Aerosol optical thickness) data)",,"207000","Increase scale, reference value and data width","Cancel",,"Operational"
4093.00,"10","Vertical sounding sequences (satellite data)","310064","(AOT (Aerosol optical thickness) data)",,"005040","Orbit number",,,"Operational"
4094.00,"10","Vertical sounding sequences (satellite data)","310064","(AOT (Aerosol optical thickness) data)",,"201133","Change data width",,,"Operational"
4095.00,"10","Vertical sounding sequences (satellite data)","310064","(AOT (Aerosol optical thickness) data)",,"005041","Scan line number",,,"Operational"
4096.00,"10","Vertical sounding sequences (satellite data)","310064","(AOT (Aerosol optical thickness) data)",,"005043","Field of view number",,,"Operational"
4097.00,"10","Vertical sounding sequences (satellite data)","310064","(AOT (Aerosol optical thickness) data)",,"201000","Change data width","Cancel",,"Operational"
4098.00,"10","Vertical sounding sequences (satellite data)","310064","(AOT (Aerosol optical thickness) data)",,"033082","Geolocation quality flags",,,"Operational"
4099.00,"10","Vertical sounding sequences (satellite data)","310064","(AOT (Aerosol optical thickness) data)",,"301021","Latitude/longitude (high accuracy)",,,"Operational"
4100.00,"10","Vertical sounding sequences (satellite data)","310064","(AOT (Aerosol optical thickness) data)",,"201129","Change data width",,,"Operational"
4101.00,"10","Vertical sounding sequences (satellite data)","310064","(AOT (Aerosol optical thickness) data)",,"007002","Height or altitude",,,"Operational"
4102.00,"10","Vertical sounding sequences (satellite data)","310064","(AOT (Aerosol optical thickness) data)",,"201000","Change data width","Cancel",,"Operational"
4103.00,"10","Vertical sounding sequences (satellite data)","310064","(AOT (Aerosol optical thickness) data)",,"007024","Satellite zenith angle",,,"Operational"
4104.00,"10","Vertical sounding sequences (satellite data)","310064","(AOT (Aerosol optical thickness) data)",,"005021","Bearing or azimuth",,,"Operational"
4105.00,"10","Vertical sounding sequences (satellite data)","310064","(AOT (Aerosol optical thickness) data)",,"007025","Solar zenith angle",,,"Operational"
4106.00,"10","Vertical sounding sequences (satellite data)","310064","(AOT (Aerosol optical thickness) data)",,"005022","Solar azimuth",,,"Operational"
4107.00,"10","Vertical sounding sequences (satellite data)","310064","(AOT (Aerosol optical thickness) data)",,"008075","Ascending/descending orbit qualifier",,,"Operational"
4108.00,"10","Vertical sounding sequences (satellite data)","310064","(AOT (Aerosol optical thickness) data)",,"008029","Surface type",,,"Operational"
4109.00,"10","Vertical sounding sequences (satellite data)","310064","(AOT (Aerosol optical thickness) data)",,"008046","Atmospheric chemical or physical constituent type",,,"Operational"
4110.00,"10","Vertical sounding sequences (satellite data)","310064","(AOT (Aerosol optical thickness) data)",,"033085","Aerosol optical thickness quality flags",,,"Operational"
4111.00,"10","Vertical sounding sequences (satellite data)","310064","(AOT (Aerosol optical thickness) data)",,"033086","Quality of pixel level retrieval",,,"Operational"
4112.00,"10","Vertical sounding sequences (satellite data)","310064","(AOT (Aerosol optical thickness) data)",,"015049","Aerosol Angstrom wavelength exponent",,,"Operational"
4113.00,"10","Vertical sounding sequences (satellite data)","310064","(AOT (Aerosol optical thickness) data)",,"033086","Quality of pixel level retrieval",,,"Operational"
4114.00,"10","Vertical sounding sequences (satellite data)","310064","(AOT (Aerosol optical thickness) data)",,"102011","Replicate 2 descriptors 11 times",,,"Operational"
4115.00,"10","Vertical sounding sequences (satellite data)","310064","(AOT (Aerosol optical thickness) data)",,"002155","Satellite channel wavelength",,,"Operational"
4116.00,"10","Vertical sounding sequences (satellite data)","310064","(AOT (Aerosol optical thickness) data)",,"015062","Aerosol optical thickness",,,"Operational"
4118.00,"10","Vertical sounding sequences (satellite data)","310065","(OMPS (Ozone mapping and profiler suite) nadir profile data)",,"001007","Satellite identifier",,,"Operational"
4119.00,"10","Vertical sounding sequences (satellite data)","310065","(OMPS (Ozone mapping and profiler suite) nadir profile data)",,"001033","Identification of originating/generating centre",,,"Operational"
4120.00,"10","Vertical sounding sequences (satellite data)","310065","(OMPS (Ozone mapping and profiler suite) nadir profile data)",,"001034","Identification of originating/generating sub-centre",,,"Operational"
4121.00,"10","Vertical sounding sequences (satellite data)","310065","(OMPS (Ozone mapping and profiler suite) nadir profile data)",,"002019","Satellite instruments",,,"Operational"
4122.00,"10","Vertical sounding sequences (satellite data)","310065","(OMPS (Ozone mapping and profiler suite) nadir profile data)",,"002020","Satellite classification",,,"Operational"
4123.00,"10","Vertical sounding sequences (satellite data)","310065","(OMPS (Ozone mapping and profiler suite) nadir profile data)",,"301011","Year, month, day",,,"Operational"
4124.00,"10","Vertical sounding sequences (satellite data)","310065","(OMPS (Ozone mapping and profiler suite) nadir profile data)",,"301012","Hour, minute",,,"Operational"
4125.00,"10","Vertical sounding sequences (satellite data)","310065","(OMPS (Ozone mapping and profiler suite) nadir profile data)",,"207003","Increase scale, reference value and data width",,,"Operational"
4126.00,"10","Vertical sounding sequences (satellite data)","310065","(OMPS (Ozone mapping and profiler suite) nadir profile data)",,"004006","Second",,,"Operational"
4127.00,"10","Vertical sounding sequences (satellite data)","310065","(OMPS (Ozone mapping and profiler suite) nadir profile data)",,"207000","Increase scale, reference value and data width","Cancel",,"Operational"
4128.00,"10","Vertical sounding sequences (satellite data)","310065","(OMPS (Ozone mapping and profiler suite) nadir profile data)",,"005040","Orbit number",,,"Operational"
4129.00,"10","Vertical sounding sequences (satellite data)","310065","(OMPS (Ozone mapping and profiler suite) nadir profile data)",,"033082","Geolocation quality flags",,,"Operational"
4130.00,"10","Vertical sounding sequences (satellite data)","310065","(OMPS (Ozone mapping and profiler suite) nadir profile data)",,"301021","Latitude/longitude (high accuracy)",,,"Operational"
4131.00,"10","Vertical sounding sequences (satellite data)","310065","(OMPS (Ozone mapping and profiler suite) nadir profile data)",,"201129","Change data width",,,"Operational"
4132.00,"10","Vertical sounding sequences (satellite data)","310065","(OMPS (Ozone mapping and profiler suite) nadir profile data)",,"007002","Height or altitude",,,"Operational"
4133.00,"10","Vertical sounding sequences (satellite data)","310065","(OMPS (Ozone mapping and profiler suite) nadir profile data)",,"201000","Change data width","Cancel",,"Operational"
4134.00,"10","Vertical sounding sequences (satellite data)","310065","(OMPS (Ozone mapping and profiler suite) nadir profile data)",,"007024","Satellite zenith angle",,,"Operational"
4135.00,"10","Vertical sounding sequences (satellite data)","310065","(OMPS (Ozone mapping and profiler suite) nadir profile data)",,"005021","Bearing or azimuth",,,"Operational"
4136.00,"10","Vertical sounding sequences (satellite data)","310065","(OMPS (Ozone mapping and profiler suite) nadir profile data)",,"007025","Solar zenith angle",,,"Operational"
4137.00,"10","Vertical sounding sequences (satellite data)","310065","(OMPS (Ozone mapping and profiler suite) nadir profile data)",,"005022","Solar azimuth",,,"Operational"
4138.00,"10","Vertical sounding sequences (satellite data)","310065","(OMPS (Ozone mapping and profiler suite) nadir profile data)",,"008075","Ascending/descending orbit qualifier",,,"Operational"
4139.00,"10","Vertical sounding sequences (satellite data)","310065","(OMPS (Ozone mapping and profiler suite) nadir profile data)",,"033071","Profile ozone quality",,,"Operational"
4140.00,"10","Vertical sounding sequences (satellite data)","310065","(OMPS (Ozone mapping and profiler suite) nadir profile data)",,"033070","Total ozone quality",,,"Operational"
4141.00,"10","Vertical sounding sequences (satellite data)","310065","(OMPS (Ozone mapping and profiler suite) nadir profile data)",,"020021","Type of precipitation",,,"Operational"
4142.00,"10","Vertical sounding sequences (satellite data)","310065","(OMPS (Ozone mapping and profiler suite) nadir profile data)",,"015045","Sulphur dioxide",,,"Operational"
4143.00,"10","Vertical sounding sequences (satellite data)","310065","(OMPS (Ozone mapping and profiler suite) nadir profile data)",,"015046","Volcano contamination index",,,"Operational"
4144.00,"10","Vertical sounding sequences (satellite data)","310065","(OMPS (Ozone mapping and profiler suite) nadir profile data)",,"008065","Sun-glint indicator",,,"Operational"
4145.00,"10","Vertical sounding sequences (satellite data)","310065","(OMPS (Ozone mapping and profiler suite) nadir profile data)",,"033087","Extent of satellite within South Atlantic anomaly (based on climatological data)",,,"Operational"
4146.00,"10","Vertical sounding sequences (satellite data)","310065","(OMPS (Ozone mapping and profiler suite) nadir profile data)",,"008003","Vertical significance (satellite observations)",,,"Operational"
4147.00,"10","Vertical sounding sequences (satellite data)","310065","(OMPS (Ozone mapping and profiler suite) nadir profile data)",,"010004","Pressure",,,"Operational"
4148.00,"10","Vertical sounding sequences (satellite data)","310065","(OMPS (Ozone mapping and profiler suite) nadir profile data)",,"008003","Vertical significance (satellite observations)",,,"Operational"
4149.00,"10","Vertical sounding sequences (satellite data)","310065","(OMPS (Ozone mapping and profiler suite) nadir profile data)",,"207002","Increase scale, reference value and data width",,,"Operational"
4150.00,"10","Vertical sounding sequences (satellite data)","310065","(OMPS (Ozone mapping and profiler suite) nadir profile data)",,"015001","Total ozone",,,"Operational"
4151.00,"10","Vertical sounding sequences (satellite data)","310065","(OMPS (Ozone mapping and profiler suite) nadir profile data)",,"207000","Increase scale, reference value and data width","Cancel",,"Operational"
4152.00,"10","Vertical sounding sequences (satellite data)","310065","(OMPS (Ozone mapping and profiler suite) nadir profile data)",,"105012","Replicate 5 descriptors 12 times",,,"Operational"
4153.00,"10","Vertical sounding sequences (satellite data)","310065","(OMPS (Ozone mapping and profiler suite) nadir profile data)",,"010040","Number of retrieved layers",,,"Operational"
4154.00,"10","Vertical sounding sequences (satellite data)","310065","(OMPS (Ozone mapping and profiler suite) nadir profile data)",,"010004","Pressure",,,"Operational"
4155.00,"10","Vertical sounding sequences (satellite data)","310065","(OMPS (Ozone mapping and profiler suite) nadir profile data)",,"207003","Increase scale, reference value and data width",,,"Operational"
4156.00,"10","Vertical sounding sequences (satellite data)","310065","(OMPS (Ozone mapping and profiler suite) nadir profile data)",,"015005","Ozone p",,,"Operational"
4157.00,"10","Vertical sounding sequences (satellite data)","310065","(OMPS (Ozone mapping and profiler suite) nadir profile data)",,"207000","Increase scale, reference value and data width","Cancel",,"Operational"
4158.00,"10","Vertical sounding sequences (satellite data)","310065","(OMPS (Ozone mapping and profiler suite) nadir profile data)",,"008046","Atmospheric chemical or physical constituent type",,,"Operational"
4159.00,"10","Vertical sounding sequences (satellite data)","310065","(OMPS (Ozone mapping and profiler suite) nadir profile data)",,"107019","Replicate 7 descriptors 19 times",,,"Operational"
4160.00,"10","Vertical sounding sequences (satellite data)","310065","(OMPS (Ozone mapping and profiler suite) nadir profile data)",,"010040","Number of retrieved layers",,,"Operational"
4161.00,"10","Vertical sounding sequences (satellite data)","310065","(OMPS (Ozone mapping and profiler suite) nadir profile data)",,"010004","Pressure",,,"Operational"
4162.00,"10","Vertical sounding sequences (satellite data)","310065","(OMPS (Ozone mapping and profiler suite) nadir profile data)",,"008090","Decimal scale of following significands",,,"Operational"
4163.00,"10","Vertical sounding sequences (satellite data)","310065","(OMPS (Ozone mapping and profiler suite) nadir profile data)",,"207006","Increase scale, reference value and data width",,,"Operational"
4164.00,"10","Vertical sounding sequences (satellite data)","310065","(OMPS (Ozone mapping and profiler suite) nadir profile data)",,"015008","Significand of volumetric mixing ratio",,,"Operational"
4165.00,"10","Vertical sounding sequences (satellite data)","310065","(OMPS (Ozone mapping and profiler suite) nadir profile data)",,"207000","Increase scale, reference value and data width","Cancel",,"Operational"
4166.00,"10","Vertical sounding sequences (satellite data)","310065","(OMPS (Ozone mapping and profiler suite) nadir profile data)",,"008090","Decimal scale of following significands","Set to missing (cancel)",,"Operational"
4168.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"001007","Satellite identifier",,,"Operational"
4169.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"001033","Identification of originating/generating centre",,,"Operational"
4170.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"001034","Identification of originating/generating sub-centre",,,"Operational"
4171.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"002019","Satellite instruments",,,"Operational"
4172.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"002020","Satellite classification",,,"Operational"
4173.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"301011","Year, month, day",,,"Operational"
4174.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"301012","Hour, minute",,,"Operational"
4175.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"207003","Increase scale, reference value and data width",,,"Operational"
4176.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"004006","Second",,,"Operational"
4177.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"207000","Increase scale, reference value and data width","Cancel",,"Operational"
4178.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"005040","Orbit number",,,"Operational"
4179.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"033082","Geolocation quality flags                          ",,,"Operational"
4180.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"301021","Latitude/longitude (high accuracy)",,,"Operational"
4181.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"201129","Change data width",,,"Operational"
4182.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"007002","Height or altitude",,,"Operational"
4183.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"201000","Change data width","Cancel",,"Operational"
4184.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"007024","Satellite zenith angle",,,"Operational"
4185.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"005021","Bearing or azimuth",,,"Operational"
4186.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"007025","Solar zenith angle",,,"Operational"
4187.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"005022","Solar azimuth",,,"Operational"
4188.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"008075","Ascending/descending orbit qualifier",,,"Operational"
4189.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"020081","Cloud amount in segment","Cloud fraction",,"Operational"
4190.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"207004","Increase scale, reference value and data width",,,"Operational"
4191.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"015030","Aerosol contamination index",,,"Operational"
4192.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"207000","Increase scale, reference value and data width","Cancel",,"Operational"
4193.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"020065","Snow cover",,,"Operational"
4194.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"015041","Sulphur dioxide index  ",,,"Operational"
4195.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"033086","Quality of pixel level retrieval",,,"Operational"
4196.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"033087","Extent of satellite within South Atlantic anomaly",,,"Operational"
4197.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"033088","Ozone total column quality flag",,,"Operational"
4198.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"008003","Vertical significance (satellite observations)","= 0 Surface",,"Operational"
4199.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"207001","Increase scale, reference value and data width",,,"Operational"
4200.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"007004","Pressure",,,"Operational"
4201.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"207000","Increase scale, reference value and data width","Cancel",,"Operational"
4202.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"008003","Vertical significance (satellite observations)","Set to missing (cancel)",,"Operational"
4203.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"207002","Increase scale, reference value and data width",,,"Operational"
4204.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"015001","Total ozone",,,"Operational"
4205.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"207000","Increase scale, reference value and data width","Cancel",,"Operational"
4206.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"008003","Vertical significance (satellite observations)","= 2 Cloud top",,"Operational"
4207.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"033042","Type of limit represented by following value","= 0 Exclusive lower limit (>)",,"Operational"
4208.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"207001","Increase scale, reference value and data width",,,"Operational"
4209.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"007004","Pressure","Cloud top pressure",,"Operational"
4210.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"207000","Increase scale, reference value and data width","Cancel",,"Operational"
4211.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"207002","Increase scale, reference value and data width",,,"Operational"
4212.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"015001","Total ozone","Below cloud",,"Operational"
4213.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"207000","Increase scale, reference value and data width","Cancel",,"Operational"
4214.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"008003","Vertical significance (satellite observations)","Set to missing (cancel)",,"Operational"
4215.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"001032","Generating application","= 0 First guess | Defined by local generating centre",,"Operational"
4216.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"207002","Increase scale, reference value and data width",,,"Operational"
4217.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"015001","Total ozone","First guess total column ozone",,"Operational"
4218.00,"10","Vertical sounding sequences (satellite data)","310066","(OMPS (Ozone mapping and profiler suite) total column data)",,"207000","Increase scale, reference value and data width","Cancel",,"Operational"
4220.00,"11","Single level report sequences (conventional data)","311001","(Aircraft reports)",,"301051","Flight number, navigational system, date/time, location, phase of flight","ASDAR",,"Operational"
4221.00,"11","Single level report sequences (conventional data)","311001","(Aircraft reports)",,"007002","Height or altitude",,,"Operational"
4222.00,"11","Single level report sequences (conventional data)","311001","(Aircraft reports)",,"012001","Temperature/air temperature",,,"Operational"
4223.00,"11","Single level report sequences (conventional data)","311001","(Aircraft reports)",,"011001","Wind direction",,,"Operational"
4224.00,"11","Single level report sequences (conventional data)","311001","(Aircraft reports)",,"011002","Wind speed",,,"Operational"
4225.00,"11","Single level report sequences (conventional data)","311001","(Aircraft reports)",,"011031","Degree of turbulence",,,"Operational"
4226.00,"11","Single level report sequences (conventional data)","311001","(Aircraft reports)",,"011032","Height of base of turbulence",,,"Operational"
4227.00,"11","Single level report sequences (conventional data)","311001","(Aircraft reports)",,"011033","Height of top of turbulence",,,"Operational"
4228.00,"11","Single level report sequences (conventional data)","311001","(Aircraft reports)",,"020041","Airframe icing",,,"Operational"
4229.00,"11","Single level report sequences (conventional data)","311002","(ACARS reports)",,"301065","ACARS identification",,,"Operational"
4230.00,"11","Single level report sequences (conventional data)","311002","(ACARS reports)",,"301066","ACARS location",,,"Operational"
4231.00,"11","Single level report sequences (conventional data)","311002","(ACARS reports)",,"311003","ACARS standard reported variables",,,"Operational"
4232.00,"11","Single level report sequences (conventional data)","311002","(ACARS reports)",,"311004","ACARS supplementary reported variables",,,"Operational"
4233.00,"11","Single level report sequences (conventional data)","311003","(ACARS standard reported variables)",,"010070","Indicated aircraft altitude",,,"Operational"
4234.00,"11","Single level report sequences (conventional data)","311003","(ACARS standard reported variables)",,"011001","Wind direction",,,"Operational"
4235.00,"11","Single level report sequences (conventional data)","311003","(ACARS standard reported variables)",,"011002","Wind speed",,,"Operational"
4236.00,"11","Single level report sequences (conventional data)","311003","(ACARS standard reported variables)",,"012001","Temperature/air temperature",,,"Operational"
4237.00,"11","Single level report sequences (conventional data)","311003","(ACARS standard reported variables)",,"013002","Mixing ratio",,,"Operational"
4238.00,"11","Single level report sequences (conventional data)","311004","(ACARS supplementary reported variables)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
4239.00,"11","Single level report sequences (conventional data)","311004","(ACARS supplementary reported variables)",,"031000","Short delayed descriptor replication factor",,,"Operational"
4240.00,"11","Single level report sequences (conventional data)","311004","(ACARS supplementary reported variables)",,"011034","Vertical gust velocity",,,"Operational"
4241.00,"11","Single level report sequences (conventional data)","311004","(ACARS supplementary reported variables)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
4242.00,"11","Single level report sequences (conventional data)","311004","(ACARS supplementary reported variables)",,"031000","Short delayed descriptor replication factor",,,"Operational"
4243.00,"11","Single level report sequences (conventional data)","311004","(ACARS supplementary reported variables)",,"011035","Vertical gust acceleration",,,"Operational"
4244.00,"11","Single level report sequences (conventional data)","311004","(ACARS supplementary reported variables)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
4245.00,"11","Single level report sequences (conventional data)","311004","(ACARS supplementary reported variables)",,"031000","Short delayed descriptor replication factor",,,"Operational"
4246.00,"11","Single level report sequences (conventional data)","311004","(ACARS supplementary reported variables)",,"011075","Mean turbulence intensity (eddy dissipation rate)",,,"Operational"
4247.00,"11","Single level report sequences (conventional data)","311004","(ACARS supplementary reported variables)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
4248.00,"11","Single level report sequences (conventional data)","311004","(ACARS supplementary reported variables)",,"031000","Short delayed descriptor replication factor",,,"Operational"
4249.00,"11","Single level report sequences (conventional data)","311004","(ACARS supplementary reported variables)",,"011076","Peak turbulence intensity (eddy dissipation rate)",,,"Operational"
4250.00,"11","Single level report sequences (conventional data)","311004","(ACARS supplementary reported variables)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
4251.00,"11","Single level report sequences (conventional data)","311004","(ACARS supplementary reported variables)",,"031000","Short delayed descriptor replication factor",,,"Operational"
4252.00,"11","Single level report sequences (conventional data)","311004","(ACARS supplementary reported variables)",,"033025","ACARS interpolated values indicator",,,"Operational"
4253.00,"11","Single level report sequences (conventional data)","311004","(ACARS supplementary reported variables)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
4254.00,"11","Single level report sequences (conventional data)","311004","(ACARS supplementary reported variables)",,"031000","Short delayed descriptor replication factor",,,"Operational"
4255.00,"11","Single level report sequences (conventional data)","311004","(ACARS supplementary reported variables)",,"033026","Moisture quality",,,"Operational"
4268.00,"11","Single level report sequences (conventional data)","311005","(Standard AMDAR reports)",,"001008","Aircraft registration number or other identification",,,"Operational"
4269.00,"11","Single level report sequences (conventional data)","311005","(Standard AMDAR reports)",,"001023","Observation sequence number",,,"Operational"
4270.00,"11","Single level report sequences (conventional data)","311005","(Standard AMDAR reports)",,"301021","Latitude/longitude (high accuracy)",,,"Operational"
4271.00,"11","Single level report sequences (conventional data)","311005","(Standard AMDAR reports)",,"301011","Year, month, day",,,"Operational"
4272.00,"11","Single level report sequences (conventional data)","311005","(Standard AMDAR reports)",,"301013","Hour, minute, second",,,"Operational"
4273.00,"11","Single level report sequences (conventional data)","311005","(Standard AMDAR reports)",,"007010","Flight level",,,"Operational"
4274.00,"11","Single level report sequences (conventional data)","311005","(Standard AMDAR reports)",,"008009","Detailed phase of flight",,,"Operational"
4275.00,"11","Single level report sequences (conventional data)","311005","(Standard AMDAR reports)",,"011001","Wind direction",,,"Operational"
4276.00,"11","Single level report sequences (conventional data)","311005","(Standard AMDAR reports)",,"011002","Wind speed",,,"Operational"
4277.00,"11","Single level report sequences (conventional data)","311005","(Standard AMDAR reports)",,"011031","Degree of turbulence",,,"Operational"
4278.00,"11","Single level report sequences (conventional data)","311005","(Standard AMDAR reports)",,"011036","Maximum derived equivalent vertical gust speed",,,"Operational"
4279.00,"11","Single level report sequences (conventional data)","311005","(Standard AMDAR reports)",,"012101","Temperature/air temperature",,,"Operational"
4280.00,"11","Single level report sequences (conventional data)","311005","(Standard AMDAR reports)",,"033025","ACARS interpolated values indicator",,,"Operational"
4281.00,"11","Single level report sequences (conventional data)","311006","(AMDAR data or aircraft data for one level without latitude/longitude)",,"007010","Flight level",,,"Operational"
4282.00,"11","Single level report sequences (conventional data)","311006","(AMDAR data or aircraft data for one level without latitude/longitude)",,"011001","Wind direction",,,"Operational"
4283.00,"11","Single level report sequences (conventional data)","311006","(AMDAR data or aircraft data for one level without latitude/longitude)",,"011002","Wind speed",,,"Operational"
4284.00,"11","Single level report sequences (conventional data)","311006","(AMDAR data or aircraft data for one level without latitude/longitude)",,"002064","Aircraft roll angle quality",,,"Operational"
4285.00,"11","Single level report sequences (conventional data)","311006","(AMDAR data or aircraft data for one level without latitude/longitude)",,"012101","Temperature/air temperature",,,"Operational"
4286.00,"11","Single level report sequences (conventional data)","311006","(AMDAR data or aircraft data for one level without latitude/longitude)",,"012103","Dewpoint temperature",,,"Operational"
4287.00,"11","Single level report sequences (conventional data)","311007","(Aircraft data for one level with latitude/longitude indicated)",,"007010","Flight level",,,"Operational"
4288.00,"11","Single level report sequences (conventional data)","311007","(Aircraft data for one level with latitude/longitude indicated)",,"301021","Latitude/longitude (high accuracy)",,,"Operational"
4289.00,"11","Single level report sequences (conventional data)","311007","(Aircraft data for one level with latitude/longitude indicated)",,"011001","Wind direction",,,"Operational"
4290.00,"11","Single level report sequences (conventional data)","311007","(Aircraft data for one level with latitude/longitude indicated)",,"011002","Wind speed",,,"Operational"
4291.00,"11","Single level report sequences (conventional data)","311007","(Aircraft data for one level with latitude/longitude indicated)",,"002064","Aircraft roll angle quality",,,"Operational"
4292.00,"11","Single level report sequences (conventional data)","311007","(Aircraft data for one level with latitude/longitude indicated)",,"012101","Temperature/air temperature",,,"Operational"
4293.00,"11","Single level report sequences (conventional data)","311007","(Aircraft data for one level with latitude/longitude indicated)",,"012103","Dewpoint temperature",,,"Operational"
4294.00,"11","Single level report sequences (conventional data)","311008","(Aircraft ascent/descent profile without latitude/longitude indicated at each level)",,"001008","Aircraft registration number or other identification",,,"Operational"
4295.00,"11","Single level report sequences (conventional data)","311008","(Aircraft ascent/descent profile without latitude/longitude indicated at each level)",,"301011","Year, month, day",,,"Operational"
4296.00,"11","Single level report sequences (conventional data)","311008","(Aircraft ascent/descent profile without latitude/longitude indicated at each level)",,"301013","Hour, minute, second",,,"Operational"
4297.00,"11","Single level report sequences (conventional data)","311008","(Aircraft ascent/descent profile without latitude/longitude indicated at each level)",,"301021","Latitude/longitude (high accuracy)",,,"Operational"
4298.00,"11","Single level report sequences (conventional data)","311008","(Aircraft ascent/descent profile without latitude/longitude indicated at each level)",,"008004","Phase of aircraft flight",,,"Operational"
4299.00,"11","Single level report sequences (conventional data)","311008","(Aircraft ascent/descent profile without latitude/longitude indicated at each level)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
4300.00,"11","Single level report sequences (conventional data)","311008","(Aircraft ascent/descent profile without latitude/longitude indicated at each level)",,"031001","Delayed descriptor replication factor",,,"Operational"
4301.00,"11","Single level report sequences (conventional data)","311008","(Aircraft ascent/descent profile without latitude/longitude indicated at each level)",,"311006","AMDAR data or aircraft data for one level without latitude/longitude",,,"Operational"
4309.00,"11","Single level report sequences (conventional data)","311009","(Aircraft ascent/descent profile with latitude/longitude given for each level)",,"001008","Aircraft registration number or other identification",,,"Operational"
4310.00,"11","Single level report sequences (conventional data)","311009","(Aircraft ascent/descent profile with latitude/longitude given for each level)",,"301011","Year, month, day",,,"Operational"
4311.00,"11","Single level report sequences (conventional data)","311009","(Aircraft ascent/descent profile with latitude/longitude given for each level)",,"301013","Hour, minute, second",,,"Operational"
4312.00,"11","Single level report sequences (conventional data)","311009","(Aircraft ascent/descent profile with latitude/longitude given for each level)",,"301021","Latitude/longitude (high accuracy)",,,"Operational"
4313.00,"11","Single level report sequences (conventional data)","311009","(Aircraft ascent/descent profile with latitude/longitude given for each level)",,"008004","Phase of aircraft flight",,,"Operational"
4314.00,"11","Single level report sequences (conventional data)","311009","(Aircraft ascent/descent profile with latitude/longitude given for each level)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
4315.00,"11","Single level report sequences (conventional data)","311009","(Aircraft ascent/descent profile with latitude/longitude given for each level)",,"031001","Delayed descriptor replication factor",,,"Operational"
4316.00,"11","Single level report sequences (conventional data)","311009","(Aircraft ascent/descent profile with latitude/longitude given for each level)",,"311007","Aircraft data for one level with latitude/longitude indicated",,,"Operational"
4324.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"001008","Aircraft registration number or other identification",,,"Operational"
4325.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"001023","Observation sequence number",,,"Operational"
4326.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"001006","Aircraft flight number",,,"Operational"
4327.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"001110","Aircraft tail number",,,"Operational"
4328.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"001111","Origination airport",,,"Operational"
4329.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"001112","Destination airport",,,"Operational"
4330.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"204002","Add associated field","2 bits long",,"Operational"
4331.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"031021","Associated field significance","= 8 Two bits quality information",,"Operational"
4332.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"301011","Year, month, day",,,"Operational"
4333.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"301013","Hour, minute, second",,,"Operational"
4334.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"301021","Latitude/longitude (high accuracy)",,,"Operational"
4335.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"007010","Flight level","Pressure altitude",,"Operational"
4336.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"010053","Global navigation satellite system altitude",,,"Operational"
4337.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"008009","Detailed phase of flight",,,"Operational"
4338.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"011001","Wind direction",,,"Operational"
4339.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"011002","Wind speed",,,"Operational"
4340.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"002064","Aircraft roll angle quality",,,"Operational"
4341.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"011100","Aircraft true airspeed",,,"Operational"
4342.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"011101","Aircraft ground speed u-component",,,"Operational"
4343.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"011102","Aircraft ground speed v-component",,,"Operational"
4344.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"011103","Aircraft ground speed w-component",,,"Operational"
4345.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"011104","Aircraft true heading",,,"Operational"
4346.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"012101","Temperature/air temperature",,,"Operational"
4347.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"002170","Aircraft humidity sensors",,,"Operational"
4348.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"201144","Change data width",,,"Operational"
4349.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"202133","Change scale",,,"Operational"
4350.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"013002","Mixing ratio",,,"Operational"
4351.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"202000","Change scale","Cancel",,"Operational"
4352.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"201000","Change data width","Cancel",,"Operational"
4353.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"201135","Change data width",,,"Operational"
4354.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"202130","Change scale",,,"Operational"
4355.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"013003","Relative humidity",,,"Operational"
4356.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"202000","Change scale","Cancel",,"Operational"
4357.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"201000","Change data width","Cancel",,"Operational"
4358.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
4359.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"031000","Short delayed descriptor replication factor",,,"Operational"
4360.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"012103","Dewpoint temperature",,,"Operational"
4361.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"033026","Moisture quality",,,"Operational"
4362.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
4363.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"031000","Short delayed descriptor replication factor",,,"Operational"
4364.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"020042","Airframe icing present",,,"Operational"
4365.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"103000","Delayed replication of 3 descriptors",,,"Operational"
4366.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"031000","Short delayed descriptor replication factor",,,"Operational"
4367.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"020043","Peak liquid water content",,,"Operational"
4368.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"020044","Average liquid water content",,,"Operational"
4369.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"020045","Supercooled large droplet (SLD) conditions",,,"Operational"
4370.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
4371.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"031000","Short delayed descriptor replication factor",,,"Operational"
4372.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"033025","ACARS interpolated values indicator",,,"Operational"
4373.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"103000","Delayed replication of 3 descriptors",,,"Operational"
4374.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"031001","Delayed descriptor replication factor",,,"Operational"
4375.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"011075","Mean turbulence intensity (eddy dissipation rate)",,,"Operational"
4376.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"011076","Peak turbulence intensity (eddy dissipation rate)",,,"Operational"
4377.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"011039","Extended time of occurrence of peak eddy dissipation rate",,,"Operational"
4378.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"102000","Delayed replication of 2 descriptors",,,"Operational"
4379.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"031000","Short delayed descriptor replication factor",,,"Operational"
4380.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"011037","Turbulence index","EDR",,"Operational"
4381.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"011077","Reporting interval or averaging time for eddy dissipation rate",,,"Operational"
4382.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"103000","Delayed replication of 3 descriptors",,,"Operational"
4383.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"031000","Short delayed descriptor replication factor",,,"Operational"
4384.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"011034","Vertical gust velocity",,,"Operational"
4385.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"011035","Vertical gust acceleration",,,"Operational"
4386.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"011036","Maximum derived equivalent vertical gust speed",,,"Operational"
4387.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"204000","Add associated field","Cancel",,"Operational"
4388.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"119000","Delayed replication of 19 descriptors",,,"Operational"
4389.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"031001","Delayed descriptor replication factor",,,"Operational"
4390.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"301011","Year, month, day",,,"Operational"
4391.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"301013","Hour, minute, second",,,"Operational"
4392.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"301021","Latitude/longitude (high accuracy)",,,"Operational"
4393.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"007007","Height",,,"Operational"
4394.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"011105","EDR algorithm version",,,"Operational"
4395.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"204007","Add associated field","7 bits long",,"Operational"
4396.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"031021","Associated field significance","= 7 Percentage confidence",,"Operational"
4397.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"011076","Peak turbulence intensity (eddy dissipation rate)",,,"Operational"
4398.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"011075","Mean turbulence intensity (eddy dissipation rate)",,,"Operational"
4399.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"204000","Add associated field","Cancel",,"Operational"
4400.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"011106","Running minimum confidence",,,"Operational"
4401.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"011107","Maximum number bad inputs",,,"Operational"
4402.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"011108","Peak location",,,"Operational"
4403.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"011109","Number of good EDR",,,"Operational"
4404.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"012101","Temperature/air temperature",,,"Operational"
4405.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"011001","Wind direction",,,"Operational"
4406.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"201130","Change data width",,,"Operational"
4407.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"011084","Wind speed",,,"Operational"
4408.00,"11","Single level report sequences (conventional data)","311010","(BUFR template for AMDAR, version 7)",,"201000","Change data width","Cancel",,"Operational"
4410.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"001023","Observation sequence number",,,"Operational"
4411.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"008004","Phase of aircraft flight",,,"Operational"
4412.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"301011","Year, month, day",,,"Operational"
4413.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"301013","Hour, minute, second",,,"Operational"
4414.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"005002","Latitude (coarse accuracy)",,,"Operational"
4415.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"006002","Longitude (coarse accuracy)",,,"Operational"
4416.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"007004","Pressure",,,"Operational"
4417.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"011001","Wind direction",,,"Operational"
4418.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"011002","Wind speed",,,"Operational"
4419.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"012101","Temperature/air temperature",,,"Operational"
4420.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"106000","Delayed replication of 6 descriptors",,,"Operational"
4421.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"031001","Delayed descriptor replication factor",,,"Operational"
4422.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"008046","Atmospheric chemical or physical constituent type",,,"Operational"
4423.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"201139","Change data width","20 bits long",,"Operational"
4424.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"202126","Change scale","Scale: 7",,"Operational"
4425.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"015026","Concentration of pollutant (mol mol-1)",,,"Operational"
4426.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"202000","Change scale","Cancel",,"Operational"
4427.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"201000","Change data width","Cancel",,"Operational"
4428.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"106000","Delayed replication of 6 descriptors",,,"Operational"
4429.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"031001","Delayed descriptor replication factor",,,"Operational"
4430.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"008046","Atmospheric chemical or physical constituent type",,,"Operational"
4431.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"201138","Change data width","19 bits long",,"Operational"
4432.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"202130","Change scale","Scale: 11",,"Operational"
4433.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"015026","Concentration of pollutant (mol mol-1)",,,"Operational"
4434.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"202000","Change scale","Cancel",,"Operational"
4435.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"201000","Change data width","Cancel",,"Operational"
4436.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"015052","Log10 of number density of aerosol particles with diameter greater than 5 nm",,,"Operational"
4437.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"015053","Log10 of number density of aerosol particles with diameter greater than 14 nm",,,"Operational"
4438.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"015054","Log10 of number density of aerosol particles with diameter between 0.25 and 2.5 μm",,,"Operational"
4439.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"015055","Non volatile aerosol ratio",,,"Operational"
4440.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"007004","Pressure",,,"Operational"
4441.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"007004","Pressure",,,"Operational"
4442.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"013099","Log10 of integrated cloud particle density",,,"Operational"
4443.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"013100","Log10 of integrated cloud particle area",,,"Operational"
4444.00,"11","Single level report sequences (conventional data)","311011","(IAGOS template for a single observation), version 2",,"013101","Log10 of integrated cloud particle volume",,,"Operational"
4446.00,"12","Single level report sequences (satellite data)","312001",,,"301043","Satellite identifier, wind computation method, date/time, location",,,"Operational"
4447.00,"12","Single level report sequences (satellite data)","312001",,,"304001","Cloud top pressure, temperature, wind",,,"Operational"
4448.00,"12","Single level report sequences (satellite data)","312002",,,"301043","Satellite identifier, wind computation method, date/time, location",,,"Operational"
4449.00,"12","Single level report sequences (satellite data)","312002",,,"304002","Cloud top pressure, wind",,,"Operational"
4450.00,"12","Single level report sequences (satellite data)","312003",,,"301042","Satellite identifier, instrument, data-processing technique, date/time, location",,,"Operational"
4451.00,"12","Single level report sequences (satellite data)","312003",,,"304003","Surface temperature",,,"Operational"
4452.00,"12","Single level report sequences (satellite data)","312004",,,"301042","Satellite identifier, instrument, data-processing technique, date/time, location",,,"Operational"
4453.00,"12","Single level report sequences (satellite data)","312004",,,"304004","Cloud top pressure, cloud cover, temperature",,,"Operational"
4454.00,"12","Single level report sequences (satellite data)","312005",,,"301042","Satellite identifier, instrument, data-processing technique, date/time, location",,,"Operational"
4455.00,"12","Single level report sequences (satellite data)","312005",,,"020014","Height of top of cloud",,,"Operational"
4456.00,"12","Single level report sequences (satellite data)","312006",,,"301044","Satellite identifier, humidity computation method, date/time, location",,,"Operational"
4457.00,"12","Single level report sequences (satellite data)","312006",,,"304005","Layer mean relative humidity",,,"Operational"
4458.00,"12","Single level report sequences (satellite data)","312007",,,"301042","Satellite identifier, instrument, data-processing technique, date/time, location",,,"Operational"
4459.00,"12","Single level report sequences (satellite data)","312007",,,"304006","Radiation",,,"Operational"
4460.00,"12","Single level report sequences (satellite data)","312010","(Orbital information, Part I)",,"001007","Satellite identifier",,,"Operational"
4461.00,"12","Single level report sequences (satellite data)","312010","(Orbital information, Part I)",,"005040","Orbit number",,,"Operational"
4462.00,"12","Single level report sequences (satellite data)","312010","(Orbital information, Part I)",,"002021","Satellite instrument data used in processing",,,"Operational"
4463.00,"12","Single level report sequences (satellite data)","312010","(Orbital information, Part I)",,"005041","Scan line number",,,"Operational"
4464.00,"12","Single level report sequences (satellite data)","312010","(Orbital information, Part I)",,"004001","Year",,,"Operational"
4465.00,"12","Single level report sequences (satellite data)","312010","(Orbital information, Part I)",,"004043","Day of the year",,,"Operational"
4466.00,"12","Single level report sequences (satellite data)","312011","(Orbital information, Part II)",,"202131","Change scale",,,"Operational"
4467.00,"12","Single level report sequences (satellite data)","312011","(Orbital information, Part II)",,"201149","Change data width",,,"Operational"
4468.00,"12","Single level report sequences (satellite data)","312011","(Orbital information, Part II)",,"004006","Second",,,"Operational"
4469.00,"12","Single level report sequences (satellite data)","312011","(Orbital information, Part II)",,"201000","Change data width",,,"Operational"
4470.00,"12","Single level report sequences (satellite data)","312011","(Orbital information, Part II)",,"202126","Change scale",,,"Operational"
4471.00,"12","Single level report sequences (satellite data)","312011","(Orbital information, Part II)",,"010002","Height",,,"Operational"
4472.00,"12","Single level report sequences (satellite data)","312011","(Orbital information, Part II)",,"202000","Change scale",,,"Operational"
4473.00,"12","Single level report sequences (satellite data)","312011","(Orbital information, Part II)",,"005043","Field of view number",,,"Operational"
4474.00,"12","Single level report sequences (satellite data)","312011","(Orbital information, Part II)",,"005053","Field of view number increment",,,"Operational"
4475.00,"12","Single level report sequences (satellite data)","312012","(HIRS brightness temperatures - channels 1-19)",,"202129","Change scale",,,"Operational"
4476.00,"12","Single level report sequences (satellite data)","312012","(HIRS brightness temperatures - channels 1-19)",,"201132","Change data width",,,"Operational"
4477.00,"12","Single level report sequences (satellite data)","312012","(HIRS brightness temperatures - channels 1-19)",,"101019","Replicate 1 descriptor 19 times",,,"Operational"
4478.00,"12","Single level report sequences (satellite data)","312012","(HIRS brightness temperatures - channels 1-19)",,"012063","Brightness temperature",,,"Operational"
4479.00,"12","Single level report sequences (satellite data)","312012","(HIRS brightness temperatures - channels 1-19)",,"201000","Change data width",,,"Operational"
4480.00,"12","Single level report sequences (satellite data)","312012","(HIRS brightness temperatures - channels 1-19)",,"202000","Change scale",,,"Operational"
4481.00,"12","Single level report sequences (satellite data)","312013","(HIRS brightness temperatures - channel 20)",,"005042","Channel number",,,"Operational"
4482.00,"12","Single level report sequences (satellite data)","312013","(HIRS brightness temperatures - channel 20)",,"202129","Change scale",,,"Operational"
4483.00,"12","Single level report sequences (satellite data)","312013","(HIRS brightness temperatures - channel 20)",,"201135","Change data width",,,"Operational"
4484.00,"12","Single level report sequences (satellite data)","312013","(HIRS brightness temperatures - channel 20)",,"012063","Brightness temperature",,,"Operational"
4485.00,"12","Single level report sequences (satellite data)","312013","(HIRS brightness temperatures - channel 20)",,"201000","Change data width",,,"Operational"
4486.00,"12","Single level report sequences (satellite data)","312013","(HIRS brightness temperatures - channel 20)",,"202000","Change scale",,,"Operational"
4487.00,"12","Single level report sequences (satellite data)","312014","(HIRS satellite data)",,"312010","Orbital information, Part I",,,"Operational"
4488.00,"12","Single level report sequences (satellite data)","312014","(HIRS satellite data)",,"312011","Orbital information, Part II",,,"Operational"
4489.00,"12","Single level report sequences (satellite data)","312014","(HIRS satellite data)",,"105056","Replicate 5 descriptors 56 times",,,"Operational"
4490.00,"12","Single level report sequences (satellite data)","312014","(HIRS satellite data)",,"301023","Latitude/longitude (coarse accuracy)",,,"Operational"
4491.00,"12","Single level report sequences (satellite data)","312014","(HIRS satellite data)",,"005042","Channel number",,,"Operational"
4492.00,"12","Single level report sequences (satellite data)","312014","(HIRS satellite data)",,"005052","Channel number increment",,,"Operational"
4493.00,"12","Single level report sequences (satellite data)","312014","(HIRS satellite data)",,"312012","HIRS brightness temperatures - channels 1-19",,,"Operational"
4494.00,"12","Single level report sequences (satellite data)","312014","(HIRS satellite data)",,"312013","HIRS brightness temperatures - channel 20",,,"Operational"
4495.00,"12","Single level report sequences (satellite data)","312015","(MSU brightness temperatures - channels 1-4)",,"109011","Replicate 9 descriptors 11 times",,,"Operational"
4496.00,"12","Single level report sequences (satellite data)","312015","(MSU brightness temperatures - channels 1-4)",,"301023","Latitude/longitude (coarse accuracy)",,,"Operational"
4497.00,"12","Single level report sequences (satellite data)","312015","(MSU brightness temperatures - channels 1-4)",,"005042","Channel number",,,"Operational"
4498.00,"12","Single level report sequences (satellite data)","312015","(MSU brightness temperatures - channels 1-4)",,"005052","Channel number increment",,,"Operational"
4499.00,"12","Single level report sequences (satellite data)","312015","(MSU brightness temperatures - channels 1-4)",,"202129","Change scale",,,"Operational"
4500.00,"12","Single level report sequences (satellite data)","312015","(MSU brightness temperatures - channels 1-4)",,"201132","Change data width",,,"Operational"
4501.00,"12","Single level report sequences (satellite data)","312015","(MSU brightness temperatures - channels 1-4)",,"101004","Replicate 1 descriptor 4 times",,,"Operational"
4502.00,"12","Single level report sequences (satellite data)","312015","(MSU brightness temperatures - channels 1-4)",,"012063","Brightness temperature",,,"Operational"
4503.00,"12","Single level report sequences (satellite data)","312015","(MSU brightness temperatures - channels 1-4)",,"202000","Change scale",,,"Operational"
4504.00,"12","Single level report sequences (satellite data)","312015","(MSU brightness temperatures - channels 1-4)",,"201000","Change data width",,,"Operational"
4505.00,"12","Single level report sequences (satellite data)","312016","(MSU satellite data)",,"312010","Orbital information, Part I",,,"Operational"
4506.00,"12","Single level report sequences (satellite data)","312016","(MSU satellite data)",,"312011","Orbital information, Part II",,,"Operational"
4507.00,"12","Single level report sequences (satellite data)","312016","(MSU satellite data)",,"312015","MSU brightness temperatures - channels 1-4",,,"Operational"
4508.00,"12","Single level report sequences (satellite data)","312017","(SSU brightness temperatures - channels 1-3)",,"109008","Replicate 9 descriptors 8 times",,,"Operational"
4509.00,"12","Single level report sequences (satellite data)","312017","(SSU brightness temperatures - channels 1-3)",,"301023","Latitude/longitude (coarse accuracy)",,,"Operational"
4510.00,"12","Single level report sequences (satellite data)","312017","(SSU brightness temperatures - channels 1-3)",,"005042","Channel number",,,"Operational"
4511.00,"12","Single level report sequences (satellite data)","312017","(SSU brightness temperatures - channels 1-3)",,"005052","Channel number increment",,,"Operational"
4512.00,"12","Single level report sequences (satellite data)","312017","(SSU brightness temperatures - channels 1-3)",,"202129","Change scale",,,"Operational"
4513.00,"12","Single level report sequences (satellite data)","312017","(SSU brightness temperatures - channels 1-3)",,"201132","Change data width",,,"Operational"
4514.00,"12","Single level report sequences (satellite data)","312017","(SSU brightness temperatures - channels 1-3)",,"101003","Replicate 1 descriptor 3 times",,,"Operational"
4515.00,"12","Single level report sequences (satellite data)","312017","(SSU brightness temperatures - channels 1-3)",,"012063","Brightness temperature",,,"Operational"
4516.00,"12","Single level report sequences (satellite data)","312017","(SSU brightness temperatures - channels 1-3)",,"202000","Change scale",,,"Operational"
4517.00,"12","Single level report sequences (satellite data)","312017","(SSU brightness temperatures - channels 1-3)",,"201000","Change data width",,,"Operational"
4518.00,"12","Single level report sequences (satellite data)","312018","(SSU satellite data)",,"312010","Orbital information, Part I",,,"Operational"
4519.00,"12","Single level report sequences (satellite data)","312018","(SSU satellite data)",,"312011","Orbital information, Part II",,,"Operational"
4520.00,"12","Single level report sequences (satellite data)","312018","(SSU satellite data)",,"312017","SSU brightness temperatures - channels 1-3",,,"Operational"
4521.00,"12","Single level report sequences (satellite data)","312019","(Wave scatterometer product with width change for wave number (spectral))",,"301047","ERS product header",,,"Operational"
4522.00,"12","Single level report sequences (satellite data)","312019","(Wave scatterometer product with width change for wave number (spectral))",,"301048","Radar parameters",,,"Operational"
4523.00,"12","Single level report sequences (satellite data)","312019","(Wave scatterometer product with width change for wave number (spectral))",,"015015","Maximum image spectral component before normalization",,,"Operational"
4524.00,"12","Single level report sequences (satellite data)","312019","(Wave scatterometer product with width change for wave number (spectral))",,"029002","Coordinate grid type",,,"Operational"
4525.00,"12","Single level report sequences (satellite data)","312019","(Wave scatterometer product with width change for wave number (spectral))",,"021076","Representation of intensities",,,"Operational"
4526.00,"12","Single level report sequences (satellite data)","312019","(Wave scatterometer product with width change for wave number (spectral))",,"106012","Replicate 6 descriptors 12 times",,,"Operational"
4527.00,"12","Single level report sequences (satellite data)","312019","(Wave scatterometer product with width change for wave number (spectral))",,"201129","Change data width","14 bits long",,"Operational"
4528.00,"12","Single level report sequences (satellite data)","312019","(Wave scatterometer product with width change for wave number (spectral))",,"006030","Wave number (spectral)",,,"Operational"
4529.00,"12","Single level report sequences (satellite data)","312019","(Wave scatterometer product with width change for wave number (spectral))",,"201000","Change data width","Cancel",,"Operational"
4530.00,"12","Single level report sequences (satellite data)","312019","(Wave scatterometer product with width change for wave number (spectral))",,"102012","Replicate 2 descriptors 12 times",,,"Operational"
4531.00,"12","Single level report sequences (satellite data)","312019","(Wave scatterometer product with width change for wave number (spectral))",,"005030","Direction (spectral)",,,"Operational"
4532.00,"12","Single level report sequences (satellite data)","312019","(Wave scatterometer product with width change for wave number (spectral))",,"021075","Image spectrum intensity",,,"Operational"
4533.00,"12","Single level report sequences (satellite data)","312019","(Wave scatterometer product with width change for wave number (spectral))",,"021066","Wave scatterometer product confidence data",,,"Operational"
4534.00,"12","Single level report sequences (satellite data)","312020","(Wave scatterometer product)",,"301047","ERS product header",,,"Operational"
4535.00,"12","Single level report sequences (satellite data)","312020","(Wave scatterometer product)",,"301048","Radar parameters",,,"Operational"
4536.00,"12","Single level report sequences (satellite data)","312020","(Wave scatterometer product)",,"015015","Maximum image spectral component before normalization",,,"Operational"
4537.00,"12","Single level report sequences (satellite data)","312020","(Wave scatterometer product)",,"029002","Coordinate grid type",,,"Operational"
4538.00,"12","Single level report sequences (satellite data)","312020","(Wave scatterometer product)",,"021076","Representation of intensities",,,"Operational"
4539.00,"12","Single level report sequences (satellite data)","312020","(Wave scatterometer product)",,"104012","Replicate 4 descriptors 12 times",,,"Operational"
4540.00,"12","Single level report sequences (satellite data)","312020","(Wave scatterometer product)",,"006030","Wave number (spectral)",,,"Operational"
4541.00,"12","Single level report sequences (satellite data)","312020","(Wave scatterometer product)",,"102012","Replicate 2 descriptors 12 times",,,"Operational"
4542.00,"12","Single level report sequences (satellite data)","312020","(Wave scatterometer product)",,"005030","Direction (spectral)",,,"Operational"
4543.00,"12","Single level report sequences (satellite data)","312020","(Wave scatterometer product)",,"021075","Image spectrum intensity",,,"Operational"
4544.00,"12","Single level report sequences (satellite data)","312020","(Wave scatterometer product)",,"021066","Wave scatterometer product confidence data",,,"Operational"
4545.00,"12","Single level report sequences (satellite data)","312021","(Wind scatterometer product)",,"301047","ERS product header",,,"Operational"
4546.00,"12","Single level report sequences (satellite data)","312021","(Wind scatterometer product)",,"101003","Replicate 1 descriptor 3 times",,,"Operational"
4547.00,"12","Single level report sequences (satellite data)","312021","(Wind scatterometer product)",,"301049","Radar beam data",,,"Operational"
4548.00,"12","Single level report sequences (satellite data)","312021","(Wind scatterometer product)",,"011012","Wind speed at 10 m",,,"Operational"
4549.00,"12","Single level report sequences (satellite data)","312021","(Wind scatterometer product)",,"011011","Wind direction at 10 m",,,"Operational"
4550.00,"12","Single level report sequences (satellite data)","312021","(Wind scatterometer product)",,"021067","Wind product confidence data",,,"Operational"
4551.00,"12","Single level report sequences (satellite data)","312022","(Radar altimeter product)",,"301047","ERS product header",,,"Operational"
4552.00,"12","Single level report sequences (satellite data)","312022","(Radar altimeter product)",,"008022","Total number (with respect to accumulation or average)","Number in average",,"Operational"
4553.00,"12","Single level report sequences (satellite data)","312022","(Radar altimeter product)",,"011012","Wind speed at 10 m",,,"Operational"
4554.00,"12","Single level report sequences (satellite data)","312022","(Radar altimeter product)",,"011050","Standard deviation of horizontal wind speed",,,"Operational"
4555.00,"12","Single level report sequences (satellite data)","312022","(Radar altimeter product)",,"022070","Significant wave height",,,"Operational"
4556.00,"12","Single level report sequences (satellite data)","312022","(Radar altimeter product)",,"022026","Standard deviation of significant wave height",,,"Operational"
4557.00,"12","Single level report sequences (satellite data)","312022","(Radar altimeter product)",,"312041","Altitude",,,"Operational"
4558.00,"12","Single level report sequences (satellite data)","312022","(Radar altimeter product)",,"010050","Standard deviation altitude",,,"Operational"
4559.00,"12","Single level report sequences (satellite data)","312022","(Radar altimeter product)",,"021068","Radar altimeter product confidence data",,,"Operational"
4560.00,"12","Single level report sequences (satellite data)","312022","(Radar altimeter product)",,"021071","Peakiness",,,"Operational"
4561.00,"12","Single level report sequences (satellite data)","312022","(Radar altimeter product)",,"021072","Satellite altimeter calibration status",,,"Operational"
4562.00,"12","Single level report sequences (satellite data)","312022","(Radar altimeter product)",,"021073","Satellite altimeter instrument mode",,,"Operational"
4563.00,"12","Single level report sequences (satellite data)","312022","(Radar altimeter product)",,"312042","Altitude corrections",,,"Operational"
4564.00,"12","Single level report sequences (satellite data)","312022","(Radar altimeter product)",,"021062","Backscatter",,,"Operational"
4565.00,"12","Single level report sequences (satellite data)","312022","(Radar altimeter product)",,"015011","Log10 of integrated electron density",,,"Operational"
4566.00,"12","Single level report sequences (satellite data)","312023","(ATSR sea-surface temperature product)",,"301047","ERS product header",,,"Operational"
4567.00,"12","Single level report sequences (satellite data)","312023","(ATSR sea-surface temperature product)",,"103003","Replicate 3 descriptors 3 times",,,"Operational"
4568.00,"12","Single level report sequences (satellite data)","312023","(ATSR sea-surface temperature product)",,"008022","Total number (with respect to accumulation or average)","Number in average",,"Operational"
4569.00,"12","Single level report sequences (satellite data)","312023","(ATSR sea-surface temperature product)",,"012061","Skin temperature",,,"Operational"
4570.00,"12","Single level report sequences (satellite data)","312023","(ATSR sea-surface temperature product)",,"022050","Standard deviation sea-surface temperature",,,"Operational"
4571.00,"12","Single level report sequences (satellite data)","312023","(ATSR sea-surface temperature product)",,"021069","SST product confidence data",,,"Operational"
4572.00,"12","Single level report sequences (satellite data)","312023","(ATSR sea-surface temperature product)",,"021085","ATSR sea-surface temperature across-track band number",,,"Operational"
4573.00,"12","Single level report sequences (satellite data)","312024","(Wave scatterometer product enhanced)",,"312020","Wave scatterometer product",,,"Operational"
4574.00,"12","Single level report sequences (satellite data)","312024","(Wave scatterometer product enhanced)",,"008060","Sample scanning mode significance","Range",,"Operational"
4575.00,"12","Single level report sequences (satellite data)","312024","(Wave scatterometer product enhanced)",,"008022","Total number (with respect to accumulation or average)","Number in sample",,"Operational"
4576.00,"12","Single level report sequences (satellite data)","312024","(Wave scatterometer product enhanced)",,"008060","Sample scanning mode significance","Horizontal",,"Operational"
4577.00,"12","Single level report sequences (satellite data)","312024","(Wave scatterometer product enhanced)",,"008022","Total number (with respect to accumulation or average)","Number in sample",,"Operational"
4578.00,"12","Single level report sequences (satellite data)","312024","(Wave scatterometer product enhanced)",,"025014","Azimuth clutter cut-off",,,"Operational"
4579.00,"12","Single level report sequences (satellite data)","312024","(Wave scatterometer product enhanced)",,"022101","Total energy (wavelength > 731m) at low wave numbers",,,"Operational"
4580.00,"12","Single level report sequences (satellite data)","312024","(Wave scatterometer product enhanced)",,"022097","Mean wavelength > 731 m of image spectrum at low wave numbers",,,"Operational"
4581.00,"12","Single level report sequences (satellite data)","312024","(Wave scatterometer product enhanced)",,"022098","Wavelength spread (wavelength > 731 m) at low wave numbers",,,"Operational"
4582.00,"12","Single level report sequences (satellite data)","312024","(Wave scatterometer product enhanced)",,"022099","Mean direction at low wave numbers (wavelength > 731 m)",,,"Operational"
4583.00,"12","Single level report sequences (satellite data)","312024","(Wave scatterometer product enhanced)",,"022100","Direction spread at low wave numbers (wavelength > 731 m)",,,"Operational"
4584.00,"12","Single level report sequences (satellite data)","312025","(Wave scatterometer enhanced product (with change of width for wave number (spectral))",,"312019","Wave scatterometer product with width change for wave number (spectral)",,,"Operational"
4585.00,"12","Single level report sequences (satellite data)","312025","(Wave scatterometer enhanced product (with change of width for wave number (spectral))",,"008060","Sample scanning mode significance","Range",,"Operational"
4586.00,"12","Single level report sequences (satellite data)","312025","(Wave scatterometer enhanced product (with change of width for wave number (spectral))",,"008022","Total number (with respect to accumulation or average)","Number in sample",,"Operational"
4587.00,"12","Single level report sequences (satellite data)","312025","(Wave scatterometer enhanced product (with change of width for wave number (spectral))",,"008060","Sample scanning mode significance","Horizontal",,"Operational"
4588.00,"12","Single level report sequences (satellite data)","312025","(Wave scatterometer enhanced product (with change of width for wave number (spectral))",,"008022","Total number (with respect to accumulation or average)","Number in sample",,"Operational"
4589.00,"12","Single level report sequences (satellite data)","312025","(Wave scatterometer enhanced product (with change of width for wave number (spectral))",,"025014","Azimuth clutter cut-off",,,"Operational"
4590.00,"12","Single level report sequences (satellite data)","312025","(Wave scatterometer enhanced product (with change of width for wave number (spectral))",,"022101","Total energy (wavelength > 731m) at low wave numbers",,,"Operational"
4591.00,"12","Single level report sequences (satellite data)","312025","(Wave scatterometer enhanced product (with change of width for wave number (spectral))",,"022097","Mean wavelength > 731 m of image spectrum at low wave numbers",,,"Operational"
4592.00,"12","Single level report sequences (satellite data)","312025","(Wave scatterometer enhanced product (with change of width for wave number (spectral))",,"022098","Wavelength spread (wavelength > 731 m) at low wave numbers",,,"Operational"
4593.00,"12","Single level report sequences (satellite data)","312025","(Wave scatterometer enhanced product (with change of width for wave number (spectral))",,"022099","Mean direction at low wave numbers (wavelength > 731 m)",,,"Operational"
4594.00,"12","Single level report sequences (satellite data)","312025","(Wave scatterometer enhanced product (with change of width for wave number (spectral))",,"022100","Direction spread at low wave numbers (wavelength > 731 m)",,,"Operational"
4595.00,"12","Single level report sequences (satellite data)","312026","(QUIKSCAT data)",,"301046","Satellite identifier, direction of motion, sensor, model function, software, resolution",,,"Operational"
4596.00,"12","Single level report sequences (satellite data)","312026","(QUIKSCAT data)",,"301011","Year, month, day",,,"Operational"
4597.00,"12","Single level report sequences (satellite data)","312026","(QUIKSCAT data)",,"301013","Hour, minute, second",,,"Operational"
4598.00,"12","Single level report sequences (satellite data)","312026","(QUIKSCAT data)",,"301023","Latitude/longitude (coarse accuracy)",,,"Operational"
4599.00,"12","Single level report sequences (satellite data)","312026","(QUIKSCAT data)",,"312031","SEAWINDS wind",,,"Operational"
4600.00,"12","Single level report sequences (satellite data)","312026","(QUIKSCAT data)",,"101004","Replicate 1 descriptor 4 times",,,"Operational"
4601.00,"12","Single level report sequences (satellite data)","312026","(QUIKSCAT data)",,"312030","Wind, formal uncertainty, likelihood",,,"Operational"
4602.00,"12","Single level report sequences (satellite data)","312026","(QUIKSCAT data)",,"021110","Number of inner-beam sigma-0 (forward of satellite)",,,"Operational"
4603.00,"12","Single level report sequences (satellite data)","312026","(QUIKSCAT data)",,"301023","Latitude/longitude (coarse accuracy)",,,"Operational"
4604.00,"12","Single level report sequences (satellite data)","312026","(QUIKSCAT data)",,"321027","Radar specification, normalized radar cross-section, Kp variance coefficient",,,"Operational"
4605.00,"12","Single level report sequences (satellite data)","312026","(QUIKSCAT data)",,"021111","Number of outer-beam sigma-0 (forward of satellite)",,,"Operational"
4606.00,"12","Single level report sequences (satellite data)","312026","(QUIKSCAT data)",,"301023","Latitude/longitude (coarse accuracy)",,,"Operational"
4607.00,"12","Single level report sequences (satellite data)","312026","(QUIKSCAT data)",,"321027","Radar specification, normalized radar cross-section, Kp variance coefficient",,,"Operational"
4608.00,"12","Single level report sequences (satellite data)","312026","(QUIKSCAT data)",,"021112","Number of inner-beam sigma-0 (aft of satellite)",,,"Operational"
4609.00,"12","Single level report sequences (satellite data)","312026","(QUIKSCAT data)",,"301023","Latitude/longitude (coarse accuracy)",,,"Operational"
4610.00,"12","Single level report sequences (satellite data)","312026","(QUIKSCAT data)",,"321027","Radar specification, normalized radar cross-section, Kp variance coefficient",,,"Operational"
4611.00,"12","Single level report sequences (satellite data)","312026","(QUIKSCAT data)",,"021113","Number of outer-beam sigma-0 (aft of satellite)",,,"Operational"
4612.00,"12","Single level report sequences (satellite data)","312026","(QUIKSCAT data)",,"301023","Latitude/longitude (coarse accuracy)",,,"Operational"
4613.00,"12","Single level report sequences (satellite data)","312026","(QUIKSCAT data)",,"321027","Radar specification, normalized radar cross-section, Kp variance coefficient",,,"Operational"
4614.00,"12","Single level report sequences (satellite data)","312027","(ATSR SST product (SADIST-2))",,"301047","ERS product header",,,"Operational"
4615.00,"12","Single level report sequences (satellite data)","312027","(ATSR SST product (SADIST-2))",,"105009","Replicate 5 descriptors 9 times",,,"Operational"
4616.00,"12","Single level report sequences (satellite data)","312027","(ATSR SST product (SADIST-2))",,"301023","Latitude/longitude (coarse accuracy)","10-arcmin cell",,"Operational"
4617.00,"12","Single level report sequences (satellite data)","312027","(ATSR SST product (SADIST-2))",,"007021","Elevation","Incidence angle nadir view | Set to zero",,"Operational"
4618.00,"12","Single level report sequences (satellite data)","312027","(ATSR SST product (SADIST-2))",,"012061","Skin temperature","SST (nadir-only view)",,"Operational"
4619.00,"12","Single level report sequences (satellite data)","312027","(ATSR SST product (SADIST-2))",,"007021","Elevation","Incidence angle dual view | Set to missing",,"Operational"
4620.00,"12","Single level report sequences (satellite data)","312027","(ATSR SST product (SADIST-2))",,"012061","Skin temperature","SST (dual view)",,"Operational"
4621.00,"12","Single level report sequences (satellite data)","312027","(ATSR SST product (SADIST-2))",,"021085","ATSR sea-surface temperature across-track band number","0-9",,"Operational"
4622.00,"12","Single level report sequences (satellite data)","312027","(ATSR SST product (SADIST-2))",,"021070","SST product confidence data (SADIST-2)","23-bit flag",,"Operational"
4623.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"301046","Satellite identifier, direction of motion, sensor, model function, software, resolution",,,"Operational"
4624.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"301011","Year, month, day",,,"Operational"
4625.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"301013","Hour, minute, second",,,"Operational"
4626.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"301023","Latitude/longitude (coarse accuracy)",,,"Operational"
4627.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"008025","Time difference qualifier",,,"Operational"
4628.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"201136","Change data width",,,"Operational"
4629.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"004006","Second",,,"Operational"
4630.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"201000","Change data width","Cancel",,"Operational"
4631.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"312031","SEAWINDS wind",,,"Operational"
4632.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"312032","SEAWINDS precipitation",,,"Operational"
4633.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"101004","Replicate 1 descriptor 4 times",,,"Operational"
4634.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"312030","Wind, formal uncertainty, likelihood",,,"Operational"
4635.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"101002","Replicate 1 descriptor 2 times",,,"Operational"
4636.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"312033","Antenna polarization, brightness temperature",,,"Operational"
4637.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"021110","Number of inner-beam sigma-0 (forward of satellite)",,,"Operational"
4638.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"301023","Latitude/longitude (coarse accuracy)",,,"Operational"
4639.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"321028","Radar specification, SEAWINDS normalized radar cross-section, Kp variance coefficient",,,"Operational"
4640.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"021111","Number of outer-beam sigma-0 (forward of satellite)",,,"Operational"
4641.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"301023","Latitude/longitude (coarse accuracy)",,,"Operational"
4642.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"321028","Radar specification, SEAWINDS normalized radar cross-section, Kp variance coefficient",,,"Operational"
4643.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"021112","Number of inner-beam sigma-0 (aft of satellite)",,,"Operational"
4644.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"301023","Latitude/longitude (coarse accuracy)",,,"Operational"
4645.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"321028","Radar specification, SEAWINDS normalized radar cross-section, Kp variance coefficient",,,"Operational"
4646.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"021113","Number of outer-beam sigma-0 (aft of satellite)",,,"Operational"
4647.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"301023","Latitude/longitude (coarse accuracy)",,,"Operational"
4648.00,"12","Single level report sequences (satellite data)","312028","(SEAWINDS QUIKSCAT data)",,"321028","Radar specification, SEAWINDS normalized radar cross-section, Kp variance coefficient",,,"Operational"
4649.00,"12","Single level report sequences (satellite data)","312030","(Wind, formal uncertainty, likelihood)",,"201130","Change data width",,,"Operational"
4650.00,"12","Single level report sequences (satellite data)","312030","(Wind, formal uncertainty, likelihood)",,"202129","Change scale",,,"Operational"
4651.00,"12","Single level report sequences (satellite data)","312030","(Wind, formal uncertainty, likelihood)",,"011012","Wind speed at 10 m",,,"Operational"
4652.00,"12","Single level report sequences (satellite data)","312030","(Wind, formal uncertainty, likelihood)",,"202000","Change scale","Cancel",,"Operational"
4653.00,"12","Single level report sequences (satellite data)","312030","(Wind, formal uncertainty, likelihood)",,"201000","Change data width","Cancel",,"Operational"
4654.00,"12","Single level report sequences (satellite data)","312030","(Wind, formal uncertainty, likelihood)",,"011052","Formal uncertainty in wind speed",,,"Operational"
4655.00,"12","Single level report sequences (satellite data)","312030","(Wind, formal uncertainty, likelihood)",,"201135","Change data width",,,"Operational"
4656.00,"12","Single level report sequences (satellite data)","312030","(Wind, formal uncertainty, likelihood)",,"202130","Change scale",,,"Operational"
4657.00,"12","Single level report sequences (satellite data)","312030","(Wind, formal uncertainty, likelihood)",,"011011","Wind direction at 10 m",,,"Operational"
4658.00,"12","Single level report sequences (satellite data)","312030","(Wind, formal uncertainty, likelihood)",,"202000","Change scale","Cancel",,"Operational"
4659.00,"12","Single level report sequences (satellite data)","312030","(Wind, formal uncertainty, likelihood)",,"201000","Change data width","Cancel",,"Operational"
4660.00,"12","Single level report sequences (satellite data)","312030","(Wind, formal uncertainty, likelihood)",,"011053","Formal uncertainty in wind direction",,,"Operational"
4661.00,"12","Single level report sequences (satellite data)","312030","(Wind, formal uncertainty, likelihood)",,"021104","Likelihood computed for solution",,,"Operational"
4662.00,"12","Single level report sequences (satellite data)","312031","(SEAWINDS wind)",,"005034","Along-track row number",,,"Operational"
4663.00,"12","Single level report sequences (satellite data)","312031","(SEAWINDS wind)",,"006034","Cross-track cell number",,,"Operational"
4664.00,"12","Single level report sequences (satellite data)","312031","(SEAWINDS wind)",,"021109","SEAWINDS wind vector cell quality",,,"Operational"
4665.00,"12","Single level report sequences (satellite data)","312031","(SEAWINDS wind)",,"011081","Model wind direction at 10 m",,,"Operational"
4666.00,"12","Single level report sequences (satellite data)","312031","(SEAWINDS wind)",,"011082","Model wind speed at 10 m",,,"Operational"
4667.00,"12","Single level report sequences (satellite data)","312031","(SEAWINDS wind)",,"021101","Number of vector ambiguities",,,"Operational"
4668.00,"12","Single level report sequences (satellite data)","312031","(SEAWINDS wind)",,"021102","Index of selected wind vector",,,"Operational"
4669.00,"12","Single level report sequences (satellite data)","312031","(SEAWINDS wind)",,"021103","Total number of sigma-0 measurements",,,"Operational"
4670.00,"12","Single level report sequences (satellite data)","312032","(SEAWINDS precipitation)",,"021120","Probability of rain",,,"Operational"
4671.00,"12","Single level report sequences (satellite data)","312032","(SEAWINDS precipitation)",,"021121","SEAWINDS NOF rain index",,,"Operational"
4672.00,"12","Single level report sequences (satellite data)","312032","(SEAWINDS precipitation)",,"013055","Intensity of precipitation",,,"Operational"
4673.00,"12","Single level report sequences (satellite data)","312032","(SEAWINDS precipitation)",,"021122","Attenuation correction on sigma-0 (from tB)",,,"Operational"
4674.00,"12","Single level report sequences (satellite data)","312033","(Antenna polarization, brightness temperature)",,"002104","Antenna polarization",,,"Operational"
4675.00,"12","Single level report sequences (satellite data)","312033","(Antenna polarization, brightness temperature)",,"008022","Total number (with respect to accumulation or average)",,,"Operational"
4676.00,"12","Single level report sequences (satellite data)","312033","(Antenna polarization, brightness temperature)",,"012063","Brightness temperature",,,"Operational"
4677.00,"12","Single level report sequences (satellite data)","312033","(Antenna polarization, brightness temperature)",,"012065","Standard deviation brightness temperature",,,"Operational"
4678.00,"12","Single level report sequences (satellite data)","312041","(Altitude)",,"201141","Change data width","28 bits long",,"Operational"
4679.00,"12","Single level report sequences (satellite data)","312041","(Altitude)",,"202130","Change scale","Scale: 2",,"Operational"
4680.00,"12","Single level report sequences (satellite data)","312041","(Altitude)",,"007001","Height of station",,,"Operational"
4681.00,"12","Single level report sequences (satellite data)","312041","(Altitude)",,"201000","Change data width","Cancel",,"Operational"
4682.00,"12","Single level report sequences (satellite data)","312041","(Altitude)",,"202000","Change scale","Cancel",,"Operational"
4683.00,"12","Single level report sequences (satellite data)","312042","(Altitude corrections)",,"021077","Altitude correction (ionosphere)",,,"Operational"
4684.00,"12","Single level report sequences (satellite data)","312042","(Altitude corrections)",,"021078","Altitude correction (dry troposphere)",,,"Operational"
4685.00,"12","Single level report sequences (satellite data)","312042","(Altitude corrections)",,"021079","Altitude correction (wet troposphere)",,,"Operational"
4686.00,"12","Single level report sequences (satellite data)","312042","(Altitude corrections)",,"021080","Altitude correction (calibration constant)",,,"Operational"
4687.00,"12","Single level report sequences (satellite data)","312042","(Altitude corrections)",,"021081","Open loop correction (height-time loop)",,,"Operational"
4688.00,"12","Single level report sequences (satellite data)","312042","(Altitude corrections)",,"021082","Open loop correction (auto gain control)",,,"Operational"
4689.00,"12","Single level report sequences (satellite data)","312045","(AATSR sea-surface temperatures)",,"001007","Satellite identifier",,,"Operational"
4690.00,"12","Single level report sequences (satellite data)","312045","(AATSR sea-surface temperatures)",,"002019","Satellite instruments",,,"Operational"
4691.00,"12","Single level report sequences (satellite data)","312045","(AATSR sea-surface temperatures)",,"001096","Station acquisition",,,"Operational"
4692.00,"12","Single level report sequences (satellite data)","312045","(AATSR sea-surface temperatures)",,"025061","Software identification and version number",,,"Operational"
4693.00,"12","Single level report sequences (satellite data)","312045","(AATSR sea-surface temperatures)",,"005040","Orbit number",,,"Operational"
4694.00,"12","Single level report sequences (satellite data)","312045","(AATSR sea-surface temperatures)",,"301011","Year, month, day",,,"Operational"
4695.00,"12","Single level report sequences (satellite data)","312045","(AATSR sea-surface temperatures)",,"301013","Hour, minute, second",,,"Operational"
4696.00,"12","Single level report sequences (satellite data)","312045","(AATSR sea-surface temperatures)",,"301021","Latitude/longitude (high accuracy)",,,"Operational"
4697.00,"12","Single level report sequences (satellite data)","312045","(AATSR sea-surface temperatures)",,"007002","Height or altitude",,,"Operational"
4698.00,"12","Single level report sequences (satellite data)","312045","(AATSR sea-surface temperatures)",,"012180","Averaged 12 micron BT for all clear pixels at nadir",,,"Operational"
4699.00,"12","Single level report sequences (satellite data)","312045","(AATSR sea-surface temperatures)",,"012181","Averaged 11 micron BT for all clear pixels at nadir",,,"Operational"
4700.00,"12","Single level report sequences (satellite data)","312045","(AATSR sea-surface temperatures)",,"012182","Averaged 3.7 micron BT for all clear pixels at nadir",,,"Operational"
4701.00,"12","Single level report sequences (satellite data)","312045","(AATSR sea-surface temperatures)",,"012183","Averaged 12 micron BT for all clear pixels, forward view",,,"Operational"
4702.00,"12","Single level report sequences (satellite data)","312045","(AATSR sea-surface temperatures)",,"012184","Averaged 11 micron BT for all clear pixels, forward view",,,"Operational"
4703.00,"12","Single level report sequences (satellite data)","312045","(AATSR sea-surface temperatures)",,"012185","Averaged 3.7 micron BT for all clear pixels, forward view",,,"Operational"
4704.00,"12","Single level report sequences (satellite data)","312045","(AATSR sea-surface temperatures)",,"002174","Mean across-track pixel number",,,"Operational"
4705.00,"12","Single level report sequences (satellite data)","312045","(AATSR sea-surface temperatures)",,"021086","Number of pixels in nadir only, average",,,"Operational"
4706.00,"12","Single level report sequences (satellite data)","312045","(AATSR sea-surface temperatures)",,"012186","Mean nadir sea-surface temperature",,,"Operational"
4707.00,"12","Single level report sequences (satellite data)","312045","(AATSR sea-surface temperatures)",,"021087","Number of pixels in dual view, average",,,"Operational"
4708.00,"12","Single level report sequences (satellite data)","312045","(AATSR sea-surface temperatures)",,"012187","Mean dual view sea-surface temperature",,,"Operational"
4709.00,"12","Single level report sequences (satellite data)","312045","(AATSR sea-surface temperatures)",,"033043","AST confidence",,,"Operational"
4710.00,"12","Single level report sequences (satellite data)","312050","(MERIS instrument reporting)",,"001007","Satellite identifier",,,"Operational"
4711.00,"12","Single level report sequences (satellite data)","312050","(MERIS instrument reporting)",,"002019","Satellite instruments",,,"Operational"
4712.00,"12","Single level report sequences (satellite data)","312050","(MERIS instrument reporting)",,"001096","Station acquisition",,,"Operational"
4713.00,"12","Single level report sequences (satellite data)","312050","(MERIS instrument reporting)",,"025061","Software identification and version number",,,"Operational"
4714.00,"12","Single level report sequences (satellite data)","312050","(MERIS instrument reporting)",,"005040","Orbit number",,,"Operational"
4715.00,"12","Single level report sequences (satellite data)","312050","(MERIS instrument reporting)",,"301011","Year, month, day",,,"Operational"
4716.00,"12","Single level report sequences (satellite data)","312050","(MERIS instrument reporting)",,"301013","Hour, minute, second",,,"Operational"
4717.00,"12","Single level report sequences (satellite data)","312050","(MERIS instrument reporting)",,"301021","Latitude/longitude (high accuracy)",,,"Operational"
4718.00,"12","Single level report sequences (satellite data)","312050","(MERIS instrument reporting)",,"007025","Solar zenith angle",,,"Operational"
4719.00,"12","Single level report sequences (satellite data)","312050","(MERIS instrument reporting)",,"005022","Solar azimuth",,,"Operational"
4720.00,"12","Single level report sequences (satellite data)","312050","(MERIS instrument reporting)",,"010080","Viewing zenith angle",,,"Operational"
4721.00,"12","Single level report sequences (satellite data)","312050","(MERIS instrument reporting)",,"027080","Viewing azimuth angle",,,"Operational"
4722.00,"12","Single level report sequences (satellite data)","312050","(MERIS instrument reporting)",,"008003","Vertical significance (satellite observations)",,,"Operational"
4723.00,"12","Single level report sequences (satellite data)","312050","(MERIS instrument reporting)",,"007004","Pressure",,,"Operational"
4724.00,"12","Single level report sequences (satellite data)","312050","(MERIS instrument reporting)",,"013093","Cloud optical thickness",,,"Operational"
4725.00,"12","Single level report sequences (satellite data)","312050","(MERIS instrument reporting)",,"008003","Vertical significance (satellite observations)",,,"Operational"
4726.00,"12","Single level report sequences (satellite data)","312050","(MERIS instrument reporting)",,"201131","Change data width",,,"Operational"
4727.00,"12","Single level report sequences (satellite data)","312050","(MERIS instrument reporting)",,"202129","Change scale",,,"Operational"
4728.00,"12","Single level report sequences (satellite data)","312050","(MERIS instrument reporting)",,"007004","Pressure",,,"Operational"
4729.00,"12","Single level report sequences (satellite data)","312050","(MERIS instrument reporting)",,"007004","Pressure",,,"Operational"
4730.00,"12","Single level report sequences (satellite data)","312050","(MERIS instrument reporting)",,"202000","Change scale","Cancel",,"Operational"
4731.00,"12","Single level report sequences (satellite data)","312050","(MERIS instrument reporting)",,"201000","Change data width","Cancel",,"Operational"
4732.00,"12","Single level report sequences (satellite data)","312050","(MERIS instrument reporting)",,"013095","Total column water vapour",,,"Operational"
4733.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"001007","Satellite identifier",,,"Operational"
4734.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"002019","Satellite instruments",,,"Operational"
4735.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"001096","Station acquisition",,,"Operational"
4736.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"025061","Software identification and version number",,,"Operational"
4737.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"005040","Orbit number",,,"Operational"
4738.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"008075","Ascending/descending orbit qualifier",,,"Operational"
4739.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"301011","Year, month, day",,,"Operational"
4740.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"301013","Hour, minute, second",,,"Operational"
4741.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"301021","Latitude/longitude (high accuracy)",,,"Operational"
4742.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"001012","Direction of motion of moving observing platform",,,"Operational"
4743.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"201131","Change data width",,,"Operational"
4744.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"001013","Speed of motion of moving observing platform",,,"Operational"
4745.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"201000","Change data width","Cancel",,"Operational"
4746.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"010032","Satellite distance to Earth's centre",,,"Operational"
4747.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"010033","Altitude (platform to ellipsoid)",,,"Operational"
4748.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"010034","Earth's radius",,,"Operational"
4749.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"007002","Height or altitude",,,"Operational"
4750.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"008012","Land/sea qualifier",,,"Operational"
4751.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"025110","Image processing summary",,,"Operational"
4752.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"025111","Number of input data gaps",,,"Operational"
4753.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"025102","Number of missing lines excluding data gaps",,,"Operational"
4754.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"002104","Antenna polarization",,,"Operational"
4755.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"025103","Number of directional bins",,,"Operational"
4756.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"025104","Number of wavelength bins",,,"Operational"
4757.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"025105","First directional bin",,,"Operational"
4758.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"025106","Directional bin step",,,"Operational"
4759.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"025107","First wavelength bin",,,"Operational"
4760.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"025108","Last wavelength bin",,,"Operational"
4761.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"002111","Radar incidence angle",,,"Operational"
4762.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"002121","Mean frequency",,,"Operational"
4763.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"002026","Cross-track resolution",,,"Operational"
4764.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"002027","Along-track resolution",,,"Operational"
4765.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"021130","Spectrum total energy",,,"Operational"
4766.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"021131","Spectrum max energy",,,"Operational"
4767.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"021132","Direction of spectrum max on higher resolution grid",,,"Operational"
4768.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"021133","Wavelength of spectrum max on higher resolution grid",,,"Operational"
4769.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"021064","Clutter noise estimate",,,"Operational"
4770.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"025014","Azimuth clutter cut-off",,,"Operational"
4771.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"021134","Range resolution of cress covariance spectrum",,,"Operational"
4772.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"107018","Replicate 7 descriptors 18 times",,,"Operational"
4773.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"005030","Direction (spectral)",,,"Operational"
4774.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"105024","Replicate 5 descriptors 24 times",,,"Operational"
4775.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"201130","Change data width",,,"Operational"
4776.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"006030","Wave number (spectral)",,,"Operational"
4777.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"201000","Change data width","Cancel",,"Operational"
4778.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"021135","Real part of cross spectra polar grid number of bins",,,"Operational"
4779.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"021136","Imaginary part of cross spectra polar grid number of bins",,,"Operational"
4780.00,"12","Single level report sequences (satellite data)","312051","(Ocean cross spectra - WVS)",,"033044","ASAR quality information",,,"Operational"
4781.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"001007","Satellite identifier",,,"Operational"
4782.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"002019","Satellite instruments",,,"Operational"
4783.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"001096","Station acquisition",,,"Operational"
4784.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"025061","Software identification and version number",,,"Operational"
4785.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"005040","Orbit number",,,"Operational"
4786.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"025120","RA2-L2-processing flag",,,"Operational"
4787.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"025121","RA2-L2-processing quality",,,"Operational"
4788.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"025124","MWR-L2-processing flag",,,"Operational"
4789.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"025125","MWR-L2-processing quality",,,"Operational"
4790.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"025122","Hardware configuration for RF",,,"Operational"
4791.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"025123","Hardware configuration for HPA",,,"Operational"
4792.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"301011","Year, month, day",,,"Operational"
4793.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"301013","Hour, minute, second",,,"Operational"
4794.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"301021","Latitude/longitude (high accuracy)",,,"Operational"
4795.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"007002","Height or altitude",,,"Operational"
4796.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"002119","RA-2 instrument operations",,,"Operational"
4797.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"033047","Measurement confidence data",,,"Operational"
4798.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"010081","Altitude of COG above reference ellipsoid",,,"Operational"
4799.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"010082","Instantaneous altitude rate",,,"Operational"
4800.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"010083","Squared off nadir angle of the satellite from platform data",,,"Operational"
4801.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"010084","Squared off nadir angle of the satellite from waveform data",,,"Operational"
4802.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"002116","Percentage of 320 MHz band processed",,,"Operational"
4803.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"002117","Percentage of 80 MHz band processed",,,"Operational"
4804.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"002118","Percentage of 20 MHz band processed",,,"Operational"
4805.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"002156","Percentage of valid Ku ocean retracker measurements",,,"Operational"
4806.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"002157","Percentage of valid S ocean retracker measurements",,,"Operational"
4807.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"014055","Solar activity index",,,"Operational"
4808.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"022150","Number of 18 Hz valid points for Ku band",,,"Operational"
4809.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"022151","Ku band ocean range",,,"Operational"
4810.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"022152","STD of 18 Hz Ku band ocean range",,,"Operational"
4811.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"022153","Number of 18 Hz valid points for S band",,,"Operational"
4812.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"022154","S band ocean range",,,"Operational"
4813.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"022155","STD of 18 Hz S band ocean range",,,"Operational"
4814.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"022156","Ku band significant wave height",,,"Operational"
4815.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"022157","STD of 18 Hz Ku band ocean range","Significant wave height",,"Operational"
4816.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"022158","S band significant wave height",,,"Operational"
4817.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"022159","STD of 18 Hz S band significant wave height",,,"Operational"
4818.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"021137","Ku band corrected ocean backscatter coefficient",,,"Operational"
4819.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"021138","STD Ku band corrected ocean backscatter coefficient",,,"Operational"
4820.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"021139","Ku band net instrumental correction for AGC",,,"Operational"
4821.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"021140","S band corrected ocean backscatter coefficient",,,"Operational"
4822.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"021141","STD S band corrected ocean backscatter coefficient",,,"Operational"
4823.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"021142","S band net instrumental correction for AGC",,,"Operational"
4824.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"010085","Mean sea-surface height",,,"Operational"
4825.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"010086","Geoid's height",,,"Operational"
4826.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"010087","Ocean depth/land elevation",,,"Operational"
4827.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"010088","Total geocentric ocean tide height (solution 1)",,,"Operational"
4828.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"010089","Total geocentric ocean tide height (solution 2)",,,"Operational"
4829.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"010090","Long period tide height",,,"Operational"
4830.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"010091","Tidal loading height",,,"Operational"
4831.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"010092","Solid Earth tide height",,,"Operational"
4832.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"010093","Geocentric pole tide height",,,"Operational"
4833.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"011002","Wind speed",,,"Operational"
4834.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"025126","Model dry tropospheric correction",,,"Operational"
4835.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"025127","Inverted barometer correction",,,"Operational"
4836.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"025128","Model wet tropospheric correction",,,"Operational"
4837.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"025129","MWR derived wet tropospheric correction",,,"Operational"
4838.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"025130","RA2 ionospheric correction on Ku band",,,"Operational"
4839.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"025131","Ionospheric correction from Doris on Ku band",,,"Operational"
4840.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"025132","Ionospheric correction from model on Ku band",,,"Operational"
4841.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"025133","Sea state bias correction on Ku band",,,"Operational"
4842.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"025134","RA2 ionospheric correction on S band",,,"Operational"
4843.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"025135","Ionospheric correction from Doris on S band",,,"Operational"
4844.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"025136","Ionospheric correction from model on S band",,,"Operational"
4845.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"025137","Sea state bias correction on S band",,,"Operational"
4846.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"013096","MWR water vapour content",,,"Operational"
4847.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"013097","MWR liquid water content",,,"Operational"
4848.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"011095","u-component of the model wind vector",,,"Operational"
4849.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"011096","v-component of the model wind vector",,,"Operational"
4850.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"012188","Interpolated 23.8 GHz brightness T from MWR",,,"Operational"
4851.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"012189","Interpolated 36.5 GHz brightness T from MWR",,,"Operational"
4852.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"002158","RA-2 instrument",,,"Operational"
4853.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"002159","MWR instrument",,,"Operational"
4854.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"033052","S band ocean retracking quality",,,"Operational"
4855.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"033053","Ku band ocean retracking quality",,,"Operational"
4856.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"021143","Ku band rain attenuation",,,"Operational"
4857.00,"12","Single level report sequences (satellite data)","312052","(RA2 - radar altimeter-2)",,"021144","Altimeter rain flag",,,"Operational"
4858.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"001007","Satellite identifier",,,"Operational"
4859.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"002019","Satellite instruments",,,"Operational"
4860.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"001096","Station acquisition",,,"Operational"
4861.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"025061","Software identification and version number",,,"Operational"
4862.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"005040","Orbit number",,,"Operational"
4863.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"008075","Ascending/descending orbit qualifier",,,"Operational"
4864.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"301011","Year, month, day",,,"Operational"
4865.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"301013","Hour, minute, second",,,"Operational"
4866.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"301021","Latitude/longitude (high accuracy)",,,"Operational"
4867.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"001012","Direction of motion of moving observing platform",,,"Operational"
4868.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"201131","Change data width",,,"Operational"
4869.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"001013","Speed of motion of moving observing platform",,,"Operational"
4870.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"201000","Change data width","Cancel",,"Operational"
4871.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"010032","Satellite distance to Earth's centre",,,"Operational"
4872.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"010033","Altitude (platform to ellipsoid)",,,"Operational"
4873.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"010034","Earth's radius",,,"Operational"
4874.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"007002","Height or altitude",,,"Operational"
4875.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"008012","Land/sea qualifier",,,"Operational"
4876.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"025110","Image processing summary",,,"Operational"
4877.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"025111","Number of input data gaps",,,"Operational"
4878.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"025102","Number of missing lines excluding data gaps",,,"Operational"
4879.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"002104","Antenna polarization",,,"Operational"
4880.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"025103","Number of directional bins",,,"Operational"
4881.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"025104","Number of wavelength bins",,,"Operational"
4882.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"025105","First directional bin",,,"Operational"
4883.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"025106","Directional bin step",,,"Operational"
4884.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"025107","First wavelength bin",,,"Operational"
4885.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"025108","Last wavelength bin",,,"Operational"
4886.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"011001","Wind direction",,,"Operational"
4887.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"011002","Wind speed",,,"Operational"
4888.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"022160","Normalized inverse wave age",,,"Operational"
4889.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"025138","Average signal-to-noise ratio",,,"Operational"
4890.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"201130","Change data width",,,"Operational"
4891.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"202129","Change scale",,,"Operational"
4892.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"022021","Height of waves",,,"Operational"
4893.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"202000","Change scale","Cancel",,"Operational"
4894.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"201000","Change data width","Cancel",,"Operational"
4895.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"033048","Confidence measure of SAR inversion",,,"Operational"
4896.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"033049","Confidence measure of wind retrieval",,,"Operational"
4897.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"002026","Cross-track resolution",,,"Operational"
4898.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"002027","Along-track resolution",,,"Operational"
4899.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"021130","Spectrum total energy",,,"Operational"
4900.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"021131","Spectrum max energy",,,"Operational"
4901.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"021132","Direction of spectrum max on higher resolution grid",,,"Operational"
4902.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"021133","Wavelength of spectrum max on higher resolution grid",,,"Operational"
4903.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"025014","Azimuth clutter cut-off",,,"Operational"
4904.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"106036","Replicate 6 descriptors 36 times",,,"Operational"
4905.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"005030","Direction (spectral)",,,"Operational"
4906.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"104024","Replicate 4 descriptors 24 times",,,"Operational"
4907.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"201130","Change data width",,,"Operational"
4908.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"006030","Wave number (spectral)",,,"Operational"
4909.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"201000","Change data width","Cancel",,"Operational"
4910.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"022161","Wave spectra",,,"Operational"
4911.00,"12","Single level report sequences (satellite data)","312053","(Ocean wave spectra)",,"033044","ASAR quality information",,,"Operational"
4912.00,"12","Single level report sequences (satellite data)","312055","(ASCAT level 1b cell information)",,"005033","Pixel size on horizontal-1",,,"Operational"
4913.00,"12","Single level report sequences (satellite data)","312055","(ASCAT level 1b cell information)",,"005040","Orbit number",,,"Operational"
4914.00,"12","Single level report sequences (satellite data)","312055","(ASCAT level 1b cell information)",,"006034","Cross-track cell number",,,"Operational"
4915.00,"12","Single level report sequences (satellite data)","312055","(ASCAT level 1b cell information)",,"010095","Height of atmosphere used",,,"Operational"
4916.00,"12","Single level report sequences (satellite data)","312055","(ASCAT level 1b cell information)",,"021157","Loss per unit length of atmosphere used",,,"Operational"
4917.00,"12","Single level report sequences (satellite data)","312056","(Scatterometer wind cell information)",,"025060","Software identification",,,"Operational"
4918.00,"12","Single level report sequences (satellite data)","312056","(Scatterometer wind cell information)",,"001032","Generating application",,,"Operational"
4919.00,"12","Single level report sequences (satellite data)","312056","(Scatterometer wind cell information)",,"011082","Model wind speed at 10 m",,,"Operational"
4920.00,"12","Single level report sequences (satellite data)","312056","(Scatterometer wind cell information)",,"011081","Model wind direction at 10 m",,,"Operational"
4921.00,"12","Single level report sequences (satellite data)","312056","(Scatterometer wind cell information)",,"020095","Ice probability",,,"Operational"
4922.00,"12","Single level report sequences (satellite data)","312056","(Scatterometer wind cell information)",,"020096","Ice age (""A"" parameter)",,,"Operational"
4923.00,"12","Single level report sequences (satellite data)","312056","(Scatterometer wind cell information)",,"021155","Wind vector cell quality",,,"Operational"
4924.00,"12","Single level report sequences (satellite data)","312056","(Scatterometer wind cell information)",,"201133","Change data width","Increase data width by 5 bits",,"Operational"
4925.00,"12","Single level report sequences (satellite data)","312056","(Scatterometer wind cell information)",,"021101","Number of vector ambiguities",,,"Operational"
4926.00,"12","Single level report sequences (satellite data)","312056","(Scatterometer wind cell information)",,"021102","Index of selected wind vector",,,"Operational"
4927.00,"12","Single level report sequences (satellite data)","312056","(Scatterometer wind cell information)",,"201000","Change data width","Cancel",,"Operational"
4928.00,"12","Single level report sequences (satellite data)","312057","(Ambiguous wind data)",,"201130","Change data width","Increase data width by 2 bits",,"Operational"
4929.00,"12","Single level report sequences (satellite data)","312057","(Ambiguous wind data)",,"202129","Change scale","Increase scaling by 10**1",,"Operational"
4930.00,"12","Single level report sequences (satellite data)","312057","(Ambiguous wind data)",,"011012","Wind speed at 10 m",,,"Operational"
4931.00,"12","Single level report sequences (satellite data)","312057","(Ambiguous wind data)",,"202000","Change scale","Cancel",,"Operational"
4932.00,"12","Single level report sequences (satellite data)","312057","(Ambiguous wind data)",,"201000","Change data width","Cancel",,"Operational"
4933.00,"12","Single level report sequences (satellite data)","312057","(Ambiguous wind data)",,"201131","Change data width","Increase data width by 3 bits",,"Operational"
4934.00,"12","Single level report sequences (satellite data)","312057","(Ambiguous wind data)",,"202129","Change scale","Increase scaling by 10**1",,"Operational"
4935.00,"12","Single level report sequences (satellite data)","312057","(Ambiguous wind data)",,"011011","Wind direction at 10 m",,,"Operational"
4936.00,"12","Single level report sequences (satellite data)","312057","(Ambiguous wind data)",,"202000","Change scale","Cancel",,"Operational"
4937.00,"12","Single level report sequences (satellite data)","312057","(Ambiguous wind data)",,"201000","Change data width","Cancel",,"Operational"
4938.00,"12","Single level report sequences (satellite data)","312057","(Ambiguous wind data)",,"021156","Backscatter distance",,,"Operational"
4939.00,"12","Single level report sequences (satellite data)","312057","(Ambiguous wind data)",,"021104","Likelihood computed for solution",,,"Operational"
4940.00,"12","Single level report sequences (satellite data)","312058","(ASCAT level 1b data)",,"301125","ASCAT header information",,,"Operational"
4941.00,"12","Single level report sequences (satellite data)","312058","(ASCAT level 1b data)",,"301011","Year, month, day",,,"Operational"
4942.00,"12","Single level report sequences (satellite data)","312058","(ASCAT level 1b data)",,"301013","Hour, minute, second",,,"Operational"
4943.00,"12","Single level report sequences (satellite data)","312058","(ASCAT level 1b data)",,"301021","Latitude/longitude (high accuracy)",,,"Operational"
4944.00,"12","Single level report sequences (satellite data)","312058","(ASCAT level 1b data)",,"312055","ASCAT level 1b cell information",,,"Operational"
4945.00,"12","Single level report sequences (satellite data)","312058","(ASCAT level 1b data)",,"021150","Beam co-location",,,"Operational"
4946.00,"12","Single level report sequences (satellite data)","312058","(ASCAT level 1b data)",,"101003","Replicate 1 descriptor 3 times",,,"Operational"
4947.00,"12","Single level report sequences (satellite data)","312058","(ASCAT level 1b data)",,"321030","ASCAT sigma-0 information",,,"Operational"
4948.00,"12","Single level report sequences (satellite data)","312059","(Scatterometer wind data)",,"312056","Scatterometer wind cell information",,,"Operational"
4949.00,"12","Single level report sequences (satellite data)","312059","(Scatterometer wind data)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
4950.00,"12","Single level report sequences (satellite data)","312059","(Scatterometer wind data)",,"031001","Delayed descriptor replication factor",,,"Operational"
4951.00,"12","Single level report sequences (satellite data)","312059","(Scatterometer wind data)",,"312057","Ambiguous wind data",,,"Operational"
4952.00,"12","Single level report sequences (satellite data)","312060","(Scatterometer soil moisture data)",,"025060","Software identification",,,"Operational"
4953.00,"12","Single level report sequences (satellite data)","312060","(Scatterometer soil moisture data)",,"025062","Database identification",,,"Operational"
4954.00,"12","Single level report sequences (satellite data)","312060","(Scatterometer soil moisture data)",,"040001","Surface soil moisture (ms)",,,"Operational"
4955.00,"12","Single level report sequences (satellite data)","312060","(Scatterometer soil moisture data)",,"040002","Estimated error in surface soil moisture",,,"Operational"
4956.00,"12","Single level report sequences (satellite data)","312060","(Scatterometer soil moisture data)",,"021062","Backscatter","Extrapolated backscatter at 40 deg incidence angle (sigma0_40)",,"Operational"
4957.00,"12","Single level report sequences (satellite data)","312060","(Scatterometer soil moisture data)",,"021151","Estimated error in sigma-0 at 40 degrees incidence angle",,,"Operational"
4958.00,"12","Single level report sequences (satellite data)","312060","(Scatterometer soil moisture data)",,"021152","Slope at 40 degrees incidence angle",,,"Operational"
4959.00,"12","Single level report sequences (satellite data)","312060","(Scatterometer soil moisture data)",,"021153","Estimated error in slope at 40 degrees incidence angle",,,"Operational"
4960.00,"12","Single level report sequences (satellite data)","312060","(Scatterometer soil moisture data)",,"021154","Soil moisture sensitivity",,,"Operational"
4961.00,"12","Single level report sequences (satellite data)","312060","(Scatterometer soil moisture data)",,"021062","Backscatter","Dry backscatter",,"Operational"
4962.00,"12","Single level report sequences (satellite data)","312060","(Scatterometer soil moisture data)",,"021088","Wet backscatter",,,"Operational"
4963.00,"12","Single level report sequences (satellite data)","312060","(Scatterometer soil moisture data)",,"040003","Mean surface soil moisture",,,"Operational"
4964.00,"12","Single level report sequences (satellite data)","312060","(Scatterometer soil moisture data)",,"040004","Rain fall detection",,,"Operational"
4965.00,"12","Single level report sequences (satellite data)","312060","(Scatterometer soil moisture data)",,"040005","Soil moisture correction flag",,,"Operational"
4966.00,"12","Single level report sequences (satellite data)","312060","(Scatterometer soil moisture data)",,"040006","Soil moisture processing flag",,,"Operational"
4967.00,"12","Single level report sequences (satellite data)","312060","(Scatterometer soil moisture data)",,"040007","Soil moisture quality",,,"Operational"
4968.00,"12","Single level report sequences (satellite data)","312060","(Scatterometer soil moisture data)",,"020065","Snow cover",,,"Operational"
4969.00,"12","Single level report sequences (satellite data)","312060","(Scatterometer soil moisture data)",,"040008","Frozen land surface fraction",,,"Operational"
4970.00,"12","Single level report sequences (satellite data)","312060","(Scatterometer soil moisture data)",,"040009","Inundation and wetland fraction",,,"Operational"
4971.00,"12","Single level report sequences (satellite data)","312060","(Scatterometer soil moisture data)",,"040010","Topographic complexity",,,"Operational"
4972.00,"12","Single level report sequences (satellite data)","312061","(ASCAT level 1b and level 2 data)",,"312058","ASCAT level 1b data",,,"Operational"
4973.00,"12","Single level report sequences (satellite data)","312061","(ASCAT level 1b and level 2 data)",,"312060","Scatterometer soil moisture data",,,"Operational"
4974.00,"12","Single level report sequences (satellite data)","312061","(ASCAT level 1b and level 2 data)",,"312059","Scatterometer wind data",,,"Operational"
4975.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"001007","Satellite identifier",,,"Operational"
4976.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"002019","Satellite instruments",,,"Operational"
4977.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"001144","Snapshot identifier",,,"Operational"
4978.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"001124","Grid point identifier",,,"Operational"
4979.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"030010","Number of grid points",,,"Operational"
4980.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"301011","Year, month, day",,,"Operational"
4981.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"301013","Hour, minute, second",,,"Operational"
4982.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"301021","Latitude/longitude (high accuracy)",,,"Operational"
4983.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"007012","Grid point altitude",,,"Operational"
4984.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"015012","Total electron count per square metre",,,"Operational"
4985.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"012165","Direct sun brightness temperature",,,"Operational"
4986.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"012166","Snapshot accuracy",,,"Operational"
4987.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"012167","Radiometric accuracy (pure polarization)",,,"Operational"
4988.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"012168","Radiometric accuracy (cross polarization)",,,"Operational"
4989.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"027010","Footprint axis 1",,,"Operational"
4990.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"028010","Footprint axis 2",,,"Operational"
4991.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"002099","Polarization",,,"Operational"
4992.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"013048","Water fraction",,,"Operational"
4993.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"025081","Incidence angle",,,"Operational"
4994.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"025082","Azimuth angle",,,"Operational"
4995.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"025083","Faraday rotational angle",,,"Operational"
4996.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"025084","Geometric rotational angle",,,"Operational"
4997.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"012080","Brightness temperature real part",,,"Operational"
4998.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"012081","Brightness temperature imaginary part",,,"Operational"
4999.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"012082","Pixel radiometric accuracy",,,"Operational"
5000.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"025174","SMOS information flag",,,"Operational"
5001.00,"12","Single level report sequences (satellite data)","312070","(SMOS data)",,"033028","Snapshot overall quality",,,"Operational"
5002.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"001007","Satellite identifier",,,"Operational"
5003.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"002019","Satellite instruments",,,"Operational"
5004.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"002139","SIRAL instrument configuration",,,"Operational"
5005.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"001096","Station acquisition","Acquisition station name",,"Operational"
5006.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"001040","Processing centre ID code",,,"Operational"
5007.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"025061","Software identification and version number",,,"Operational"
5008.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"005040","Orbit number",,,"Operational"
5009.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"005044","Satellite cycle number",,,"Operational"
5010.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"008075","Ascending/descending orbit qualifier",,,"Operational"
5011.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"008077","Radiometer sensed surface type",,,"Operational"
5012.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"004001","Year",,,"Operational"
5013.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"004002","Month",,,"Operational"
5014.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"004003","Day",,,"Operational"
5015.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"004004","Hour",,,"Operational"
5016.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"004005","Minute",,,"Operational"
5017.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"004006","Second",,,"Operational"
5018.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"005001","Latitude (high accuracy)",,,"Operational"
5019.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"006001","Longitude (high accuracy)",,,"Operational"
5020.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"010081","Altitude of COG above reference ellipsoid",,,"Operational"
5021.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"022156","Ku band significant wave height",,,"Operational"
5022.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"022142","Square of significant wave height",,,"Operational"
5023.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"101020","Replicate 1 descriptor 20 times",,,"Operational"
5024.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"022149","20 Hz significant wave height squared",,,"Operational"
5025.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"022143","STD of 20 Hz SWH squared",,,"Operational"
5026.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"022144","Number of 20 Hz valid points for SWH squared",,,"Operational"
5027.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"021137","Ku band corrected ocean backscatter coefficient",,,"Operational"
5028.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"101020","Replicate 1 descriptor 20 times",,,"Operational"
5029.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"021181","20 Hz ocean backscatter coefficient",,,"Operational"
5030.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"021138","STD Ku band corrected ocean backscatter coefficient",,,"Operational"
5031.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"021180","Number of 20 Hz valid points for ocean backscatter coefficient",,,"Operational"
5032.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"021177","Corrected OCOG backscatter coefficient",,,"Operational"
5033.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"021178","STD of 20 Hz OCOG backscatter coefficient",,,"Operational"
5034.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"021179","Number of 20 Hz valid points for OCOG backscatter coefficient",,,"Operational"
5035.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"010079","Off nadir angle of the satellite from platform data",,,"Operational"
5036.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"010085","Mean sea-surface height",,,"Operational"
5037.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"010086","Geoid's height",,,"Operational"
5038.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"010087","Ocean depth/land elevation",,,"Operational"
5039.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"010089","Total geocentric ocean tide height (solution 2)",,,"Operational"
5040.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"010090","Long period tide height",,,"Operational"
5041.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"010091","Tidal loading height",,,"Operational"
5042.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"010092","Solid Earth tide height",,,"Operational"
5043.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"010093","Geocentric pole tide height",,,"Operational"
5044.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"011097","Wind speed from altimeter",,,"Operational"
5045.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"021093","Ku band peakiness","Average of 20 Hz values",,"Operational"
5046.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"101020","Replicate 1 descriptor 20 times",,,"Operational"
5047.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"021182","20 Hz Ku band peakiness","20 values",,"Operational"
5048.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"033053","Ku band ocean retracking quality",,,"Operational"
5049.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"022151","Ku band ocean range",,,"Operational"
5050.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"022145","STD of 20 Hz ocean range",,,"Operational"
5051.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"022148","Number of 20 Hz valid points for ocean range",,,"Operational"
5052.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"022146","OCOG range",,,"Operational"
5053.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"022147","STD of 20 Hz OCOG range",,,"Operational"
5054.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"025126","Model dry tropospheric correction",,,"Operational"
5055.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"025128","Model wet tropospheric correction",,,"Operational"
5056.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"025127","Inverted barometer correction",,,"Operational"
5057.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"021176","High frequency variability correction",,,"Operational"
5058.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"025132","Ionospheric correction from model on Ku band",,,"Operational"
5059.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"025133","Sea state bias correction on Ku band",,,"Operational"
5060.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"025182","L1 processing flag",,,"Operational"
5061.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"025183","L1 processing quality",,,"Operational"
5062.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"025180","LRM mode per cent",,,"Operational"
5063.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"025184","L2 product status",,,"Operational"
5064.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"025181","L2 processing flag",,,"Operational"
5065.00,"12","Single level report sequences (satellite data)","312071","(CryoSat-2 SIRAL altimeter)",,"033080","Scan level quality flags","L2 processing quality",,"Operational"
5066.00,"13","Sequences common to image data","313009","(Radar reflectivity values)",,"021001","Horizontal reflectivity",,,"Operational"
5067.00,"13","Sequences common to image data","313009","(Radar reflectivity values)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
5068.00,"13","Sequences common to image data","313009","(Radar reflectivity values)",,"031001","Delayed descriptor replication factor",,,"Operational"
5069.00,"13","Sequences common to image data","313009","(Radar reflectivity values)",,"021001","Horizontal reflectivity",,,"Operational"
5070.00,"13","Sequences common to image data","313010","(Radar rainfall intensities)",,"021036","Radar rainfall intensity",,,"Operational"
5071.00,"13","Sequences common to image data","313010","(Radar rainfall intensities)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
5072.00,"13","Sequences common to image data","313010","(Radar rainfall intensities)",,"031001","Delayed descriptor replication factor",,,"Operational"
5073.00,"13","Sequences common to image data","313010","(Radar rainfall intensities)",,"021036","Radar rainfall intensity",,,"Operational"
5074.00,"13","Sequences common to image data","313031","(Non run-length encoded row for Pixel value (4 bits))",,"006002","Longitude (coarse accuracy)","First longitude location minus one increment",,"Operational"
5075.00,"13","Sequences common to image data","313031","(Non run-length encoded row for Pixel value (4 bits))",,"006012","Longitude increment (coarse accuracy)",,,"Operational"
5076.00,"13","Sequences common to image data","313031","(Non run-length encoded row for Pixel value (4 bits))",,"101000","Delayed replication of 1 descriptor",,,"Operational"
5077.00,"13","Sequences common to image data","313031","(Non run-length encoded row for Pixel value (4 bits))",,"031002","Extended delayed descriptor replication factor",,,"Operational"
5078.00,"13","Sequences common to image data","313031","(Non run-length encoded row for Pixel value (4 bits))",,"030001","Pixel value (4 bits)",,,"Operational"
5079.00,"13","Sequences common to image data","313032","(Non run-length encoded picture data for Pixel value (4 bits))",,"005002","Latitude (coarse accuracy)","First latitude location minus one increment",,"Operational"
5080.00,"13","Sequences common to image data","313032","(Non run-length encoded picture data for Pixel value (4 bits))",,"005012","Latitude increment (coarse accuracy)","Signed value so cannot cross pole",,"Operational"
5081.00,"13","Sequences common to image data","313032","(Non run-length encoded picture data for Pixel value (4 bits))",,"101000","Delayed replication of 1 descriptor",,,"Operational"
5082.00,"13","Sequences common to image data","313032","(Non run-length encoded picture data for Pixel value (4 bits))",,"031002","Extended delayed descriptor replication factor",,,"Operational"
5083.00,"13","Sequences common to image data","313032","(Non run-length encoded picture data for Pixel value (4 bits))",,"313031","Non run-length encoded row for Pixel value (4 bits)",,,"Operational"
5084.00,"13","Sequences common to image data","313041","(Run-length encoded row for Pixel value (4 bits))",,"006002","Longitude (coarse accuracy)","First longitude location minus one increment",,"Operational"
5085.00,"13","Sequences common to image data","313041","(Run-length encoded row for Pixel value (4 bits))",,"110000","Delayed replication of 10 descriptors",,,"Operational"
5086.00,"13","Sequences common to image data","313041","(Run-length encoded row for Pixel value (4 bits))",,"031001","Delayed descriptor replication factor",,,"Operational"
5087.00,"13","Sequences common to image data","313041","(Run-length encoded row for Pixel value (4 bits))",,"104000","Delayed replication of 4 descriptors",,,"Operational"
5088.00,"13","Sequences common to image data","313041","(Run-length encoded row for Pixel value (4 bits))",,"031001","Delayed descriptor replication factor",,,"Operational"
5089.00,"13","Sequences common to image data","313041","(Run-length encoded row for Pixel value (4 bits))",,"006012","Longitude increment (coarse accuracy)",,,"Operational"
5090.00,"13","Sequences common to image data","313041","(Run-length encoded row for Pixel value (4 bits))",,"101000","Delayed replication of 1 descriptor",,,"Operational"
5091.00,"13","Sequences common to image data","313041","(Run-length encoded row for Pixel value (4 bits))",,"031012","Extended delayed descriptor and data repetition factor",,,"Operational"
5092.00,"13","Sequences common to image data","313041","(Run-length encoded row for Pixel value (4 bits))",,"030001","Pixel value (4 bits)",,,"Operational"
5093.00,"13","Sequences common to image data","313041","(Run-length encoded row for Pixel value (4 bits))",,"006012","Longitude increment (coarse accuracy)",,,"Operational"
5094.00,"13","Sequences common to image data","313041","(Run-length encoded row for Pixel value (4 bits))",,"101000","Delayed replication of 1 descriptor",,,"Operational"
5095.00,"13","Sequences common to image data","313041","(Run-length encoded row for Pixel value (4 bits))",,"031001","Delayed descriptor replication factor",,,"Operational"
5096.00,"13","Sequences common to image data","313041","(Run-length encoded row for Pixel value (4 bits))",,"030001","Pixel value (4 bits)",,,"Operational"
5097.00,"13","Sequences common to image data","313042","(Run-length encoded picture data for Pixel value (4 bits))",,"005002","Latitude (coarse accuracy)","First latitude location minus one increment",,"Operational"
5098.00,"13","Sequences common to image data","313042","(Run-length encoded picture data for Pixel value (4 bits))",,"005012","Latitude increment (coarse accuracy)","Signed value so cannot cross pole",,"Operational"
5099.00,"13","Sequences common to image data","313042","(Run-length encoded picture data for Pixel value (4 bits))",,"101000","Delayed replication of 1 descriptor",,,"Operational"
5100.00,"13","Sequences common to image data","313042","(Run-length encoded picture data for Pixel value (4 bits))",,"031002","Extended delayed descriptor replication factor",,,"Operational"
5101.00,"13","Sequences common to image data","313042","(Run-length encoded picture data for Pixel value (4 bits))",,"313041","Run-length encoded row for pixel value (4 bits)",,,"Operational"
5102.00,"13","Sequences common to image data","313043","(Run-length encoded picture data for pixel value (4 bits), regular grid)",,"006002","Longitude (coarse accuracy)","First longitude location minus one increment",,"Operational"
5103.00,"13","Sequences common to image data","313043","(Run-length encoded picture data for pixel value (4 bits), regular grid)",,"005002","Latitude (coarse accuracy)","First latitude location minus one increment",,"Operational"
5104.00,"13","Sequences common to image data","313043","(Run-length encoded picture data for pixel value (4 bits), regular grid)",,"005012","Latitude increment (coarse accuracy)",,,"Operational"
5105.00,"13","Sequences common to image data","313043","(Run-length encoded picture data for pixel value (4 bits), regular grid)",,"112000","Delayed replication of 12 descriptors",,,"Operational"
5106.00,"13","Sequences common to image data","313043","(Run-length encoded picture data for pixel value (4 bits), regular grid)",,"031001","Delayed descriptor replication factor",,,"Operational"
5107.00,"13","Sequences common to image data","313043","(Run-length encoded picture data for pixel value (4 bits), regular grid)",,"110000","Delayed replication of 10 descriptors",,,"Operational"
5108.00,"13","Sequences common to image data","313043","(Run-length encoded picture data for pixel value (4 bits), regular grid)",,"031001","Delayed descriptor replication factor",,,"Operational"
5109.00,"13","Sequences common to image data","313043","(Run-length encoded picture data for pixel value (4 bits), regular grid)",,"104000","Delayed replication of 4 descriptors",,,"Operational"
5110.00,"13","Sequences common to image data","313043","(Run-length encoded picture data for pixel value (4 bits), regular grid)",,"031001","Delayed descriptor replication factor",,,"Operational"
5111.00,"13","Sequences common to image data","313043","(Run-length encoded picture data for pixel value (4 bits), regular grid)",,"006012","Longitude increment (coarse accuracy)",,,"Operational"
5112.00,"13","Sequences common to image data","313043","(Run-length encoded picture data for pixel value (4 bits), regular grid)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
5113.00,"13","Sequences common to image data","313043","(Run-length encoded picture data for pixel value (4 bits), regular grid)",,"031011","Delayed descriptor and data repetition factor",,,"Operational"
5114.00,"13","Sequences common to image data","313043","(Run-length encoded picture data for pixel value (4 bits), regular grid)",,"030001","Pixel value (4 bits)",,,"Operational"
5115.00,"13","Sequences common to image data","313043","(Run-length encoded picture data for pixel value (4 bits), regular grid)",,"006012","Longitude increment (coarse accuracy)",,,"Operational"
5116.00,"13","Sequences common to image data","313043","(Run-length encoded picture data for pixel value (4 bits), regular grid)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
5117.00,"13","Sequences common to image data","313043","(Run-length encoded picture data for pixel value (4 bits), regular grid)",,"031001","Delayed descriptor replication factor",,,"Operational"
5118.00,"13","Sequences common to image data","313043","(Run-length encoded picture data for pixel value (4 bits), regular grid)",,"030001","Pixel value (4 bits)",,,"Operational"
5119.00,"15","Oceanographic report sequences","315001","(Typically reported underwater sounding without optional fields)",,"001011","Ship or mobile land station identifier","Ship's call sign",,"Operational"
5120.00,"15","Oceanographic report sequences","315001","(Typically reported underwater sounding without optional fields)",,"301011","Year, month, day",,,"Operational"
5121.00,"15","Oceanographic report sequences","315001","(Typically reported underwater sounding without optional fields)",,"301012","Hour, minute",,,"Operational"
5122.00,"15","Oceanographic report sequences","315001","(Typically reported underwater sounding without optional fields)",,"301023","Latitude/longitude (coarse accuracy)",,,"Operational"
5123.00,"15","Oceanographic report sequences","315001","(Typically reported underwater sounding without optional fields)",,"306001","Depth, temperature",,,"Operational"
5124.00,"15","Oceanographic report sequences","315002","(Typically reported underwater sounding without optional fields)",,"001011","Ship or mobile land station identifier","Ship's call sign",,"Operational"
5125.00,"15","Oceanographic report sequences","315002","(Typically reported underwater sounding without optional fields)",,"301011","Year, month, day",,,"Operational"
5126.00,"15","Oceanographic report sequences","315002","(Typically reported underwater sounding without optional fields)",,"301012","Hour, minute",,,"Operational"
5127.00,"15","Oceanographic report sequences","315002","(Typically reported underwater sounding without optional fields)",,"301023","Latitude/longitude (coarse accuracy)",,,"Operational"
5128.00,"15","Oceanographic report sequences","315002","(Typically reported underwater sounding without optional fields)",,"306004","Depth, temperature, salinity",,,"Operational"
5129.00,"15","Oceanographic report sequences","315003","(Temperature and salinity profile observed by profile floats)",,"001087","WMO marine observing platform extended identifier",,,"Operational"
5130.00,"15","Oceanographic report sequences","315003","(Temperature and salinity profile observed by profile floats)",,"001085","Observing platform manufacturer's model",,,"Operational"
5131.00,"15","Oceanographic report sequences","315003","(Temperature and salinity profile observed by profile floats)",,"001086","Observing platform manufacturer's serial number",,,"Operational"
5132.00,"15","Oceanographic report sequences","315003","(Temperature and salinity profile observed by profile floats)",,"002036","Buoy type",,,"Operational"
5133.00,"15","Oceanographic report sequences","315003","(Temperature and salinity profile observed by profile floats)",,"002148","Data collection and/or location system",,,"Operational"
5134.00,"15","Oceanographic report sequences","315003","(Temperature and salinity profile observed by profile floats)",,"002149","Type of data buoy",,,"Operational"
5135.00,"15","Oceanographic report sequences","315003","(Temperature and salinity profile observed by profile floats)",,"022055","Float cycle number",,,"Operational"
5136.00,"15","Oceanographic report sequences","315003","(Temperature and salinity profile observed by profile floats)",,"022056","Direction of profile",,,"Operational"
5137.00,"15","Oceanographic report sequences","315003","(Temperature and salinity profile observed by profile floats)",,"022067","Instrument type for water temperature profile measurement",,,"Operational"
5138.00,"15","Oceanographic report sequences","315003","(Temperature and salinity profile observed by profile floats)",,"301011","Year, month, day",,,"Operational"
5139.00,"15","Oceanographic report sequences","315003","(Temperature and salinity profile observed by profile floats)",,"301012","Hour, minute",,,"Operational"
5140.00,"15","Oceanographic report sequences","315003","(Temperature and salinity profile observed by profile floats)",,"301021","Latitude/longitude (high accuracy)",,,"Operational"
5141.00,"15","Oceanographic report sequences","315003","(Temperature and salinity profile observed by profile floats)",,"008080","Qualifier for GTSPP quality flag",,,"Operational"
5142.00,"15","Oceanographic report sequences","315003","(Temperature and salinity profile observed by profile floats)",,"033050","Global GTSPP quality flag",,,"Operational"
5143.00,"15","Oceanographic report sequences","315003","(Temperature and salinity profile observed by profile floats)",,"109000","Delayed replication of 9 descriptors",,,"Operational"
5144.00,"15","Oceanographic report sequences","315003","(Temperature and salinity profile observed by profile floats)",,"031002","Extended delayed descriptor replication factor",,,"Operational"
5145.00,"15","Oceanographic report sequences","315003","(Temperature and salinity profile observed by profile floats)",,"007065","Water pressure",,,"Operational"
5146.00,"15","Oceanographic report sequences","315003","(Temperature and salinity profile observed by profile floats)",,"008080","Qualifier for GTSPP quality flag",,,"Operational"
5147.00,"15","Oceanographic report sequences","315003","(Temperature and salinity profile observed by profile floats)",,"033050","Global GTSPP quality flag",,,"Operational"
5148.00,"15","Oceanographic report sequences","315003","(Temperature and salinity profile observed by profile floats)",,"022045","Sea/water temperature",,,"Operational"
5149.00,"15","Oceanographic report sequences","315003","(Temperature and salinity profile observed by profile floats)",,"008080","Qualifier for GTSPP quality flag",,,"Operational"
5150.00,"15","Oceanographic report sequences","315003","(Temperature and salinity profile observed by profile floats)",,"033050","Global GTSPP quality flag",,,"Operational"
5151.00,"15","Oceanographic report sequences","315003","(Temperature and salinity profile observed by profile floats)",,"022064","Salinity",,,"Operational"
5152.00,"15","Oceanographic report sequences","315003","(Temperature and salinity profile observed by profile floats)",,"008080","Qualifier for GTSPP quality flag",,,"Operational"
5153.00,"15","Oceanographic report sequences","315003","(Temperature and salinity profile observed by profile floats)",,"033050","Global GTSPP quality flag",,,"Operational"
5155.00,"15","Oceanographic report sequences","315004","(XBT temperature profile data sequence)",,"001079","Unique identifier for the profile","Hexadecimal string",,"Operational"
5156.00,"15","Oceanographic report sequences","315004","(XBT temperature profile data sequence)",,"001011","Ship or mobile land station identifier","Ship's call sign",,"Operational"
5157.00,"15","Oceanographic report sequences","315004","(XBT temperature profile data sequence)",,"001103","IMO Number. Unique Lloyd's register","= 0 to 9999999",,"Operational"
5158.00,"15","Oceanographic report sequences","315004","(XBT temperature profile data sequence)",,"001087","WMO marine observing platform extended identifier",,"(see Note 1)","Operational"
5159.00,"15","Oceanographic report sequences","315004","(XBT temperature profile data sequence)",,"001019","Long station or site name","Ship name",,"Operational"
5160.00,"15","Oceanographic report sequences","315004","(XBT temperature profile data sequence)",,"001080","Ship line number according to SOOP",,,"Operational"
5161.00,"15","Oceanographic report sequences","315004","(XBT temperature profile data sequence)",,"005036","Ship transect number according to SOOP",,"(see Note 2)","Operational"
5162.00,"15","Oceanographic report sequences","315004","(XBT temperature profile data sequence)",,"001036","Agency in charge of operating the observing platform",,,"Operational"
5163.00,"15","Oceanographic report sequences","315004","(XBT temperature profile data sequence)",,"001013","Speed of motion of moving observing platform",,,"Operational"
5164.00,"15","Oceanographic report sequences","315004","(XBT temperature profile data sequence)",,"001012","Direction of motion of moving observing platform",,,"Operational"
5165.00,"15","Oceanographic report sequences","315004","(XBT temperature profile data sequence)",,"301011","Year, month, day",,,"Operational"
5166.00,"15","Oceanographic report sequences","315004","(XBT temperature profile data sequence)",,"301012","Hour, minute",,,"Operational"
5167.00,"15","Oceanographic report sequences","315004","(XBT temperature profile data sequence)",,"301021","Latitude/longitude (high accuracy)",,,"Operational"
5168.00,"15","Oceanographic report sequences","315004","(XBT temperature profile data sequence)",,"007032","Height of sensor above local ground (or deck of marine platform)",,,"Operational"
5169.00,"15","Oceanographic report sequences","315004","(XBT temperature profile data sequence)",,"007033","Height of sensor above water surface",,,"Operational"
5170.00,"15","Oceanographic report sequences","315004","(XBT temperature profile data sequence)",,"002002","Type of instrumentation for wind measurement",,,"Operational"
5171.00,"15","Oceanographic report sequences","315004","(XBT temperature profile data sequence)",,"011002","Wind speed",,,"Operational"
5172.00,"15","Oceanographic report sequences","315004","(XBT temperature profile data sequence)",,"011001","Wind direction",,,"Operational"
5173.00,"15","Oceanographic report sequences","315004","(XBT temperature profile data sequence)",,"007032","Height of sensor above local ground (or deck of marine platform)",,,"Operational"
5174.00,"15","Oceanographic report sequences","315004","(XBT temperature profile data sequence)",,"007033","Height of sensor above water surface",,,"Operational"
5175.00,"15","Oceanographic report sequences","315004","(XBT temperature profile data sequence)",,"012101","Temperature/air temperature",,,"Operational"
5176.00,"15","Oceanographic report sequences","315004","(XBT temperature profile data sequence)",,"012103","Dewpoint temperature",,,"Operational"
5177.00,"15","Oceanographic report sequences","315004","(XBT temperature profile data sequence)",,"007032","Height of sensor above local ground (or deck of marine platform)","Set to missing (cancel)",,"Operational"
5178.00,"15","Oceanographic report sequences","315004","(XBT temperature profile data sequence)",,"007033","Height of sensor above water surface","Set to missing (cancel)",,"Operational"
5179.00,"15","Oceanographic report sequences","315004","(XBT temperature profile data sequence)",,"302021","Waves",,,"Operational"
5180.00,"15","Oceanographic report sequences","315004","(XBT temperature profile data sequence)",,"002031","Duration and time of current measurement",,,"Operational"
5181.00,"15","Oceanographic report sequences","315004","(XBT temperature profile data sequence)",,"002030","Method of current measurement",,,"Operational"
5182.00,"15","Oceanographic report sequences","315004","(XBT temperature profile data sequence)",,"022005","Direction of sea-surface current",,,"Operational"
5183.00,"15","Oceanographic report sequences","315004","(XBT temperature profile data sequence)",,"022032","Speed of sea-surface current",,,"Operational"
5184.00,"15","Oceanographic report sequences","315004","(XBT temperature profile data sequence)",,"022063","Total water depth",,,"Operational"
5185.00,"15","Oceanographic report sequences","315004","(XBT temperature profile data sequence)",,"008080","Qualifier for GTSPP quality flag",,,"Operational"
5186.00,"15","Oceanographic report sequences","315004","(XBT temperature profile data sequence)",,"033050","Global GTSPP quality flag",,,"Operational"
5187.00,"15","Oceanographic report sequences","315004","(XBT temperature profile data sequence)",,"022178","XBT/XCTD launcher type",,,"Operational"
5188.00,"15","Oceanographic report sequences","315004","(XBT temperature profile data sequence)",,"022177","Height of XBT/XCTD launcher","Above sea level | 0 to 50 m in units of whole m",,"Operational"
5189.00,"15","Oceanographic report sequences","315004","(XBT temperature profile data sequence)",,"022067","Instrument type for water temperature profile measurement",,,"Operational"
5190.00,"15","Oceanographic report sequences","315004","(XBT temperature profile data sequence)",,"008041","Data significance",,,"Operational"
5191.00,"15","Oceanographic report sequences","315004","(XBT temperature profile data sequence)",,"026021","Year",,,"Operational"
5192.00,"15","Oceanographic report sequences","315004","(XBT temperature profile data sequence)",,"026022","Month",,,"Operational"
5193.00,"15","Oceanographic report sequences","315004","(XBT temperature profile data sequence)",,"026023","Day",,,"Operational"
5194.00,"15","Oceanographic report sequences","315004","(XBT temperature profile data sequence)",,"022068","Water temperature profile recorder types",,,"Operational"
5195.00,"15","Oceanographic report sequences","315004","(XBT temperature profile data sequence)",,"025061","Software identification and version number",,,"Operational"
5196.00,"15","Oceanographic report sequences","315004","(XBT temperature profile data sequence)",,"008041","Data significance","Set to missing (cancel)",,"Operational"
5197.00,"15","Oceanographic report sequences","315004","(XBT temperature profile data sequence)",,"008080","Qualifier for GTSPP quality flag","Set to missing (cancel)",,"Operational"
5198.00,"15","Oceanographic report sequences","315004","(XBT temperature profile data sequence)",,"002171","Instrument serial number for water temperature profile measurement",,,"Operational"
5199.00,"15","Oceanographic report sequences","315004","(XBT temperature profile data sequence)",,"302090","Sea/water temperature high precision",,,"Operational"
5200.00,"15","Oceanographic report sequences","315004","(XBT temperature profile data sequence)",,"002171","Instrument serial number for water temperature profile measurement",,,"Operational"
5201.00,"15","Oceanographic report sequences","315004","(XBT temperature profile data sequence)",,"002032","Indicator for digitization",,"(see Note 3)","Operational"
5202.00,"15","Oceanographic report sequences","315004","(XBT temperature profile data sequence)",,"315005","Water temperature profile (Temperature profile observed by XBT or buoy)",,,"Operational"
5203.00,"15","Oceanographic report sequences","315005","(Water temperature profile (Temperature profile observed by XBT or buoy)",,"106000","Delayed replication of 6 descriptors",,,"Operational"
5204.00,"15","Oceanographic report sequences","315005","(Water temperature profile (Temperature profile observed by XBT or buoy)",,"031002","Extended delayed descriptor replication factor",,,"Operational"
5205.00,"15","Oceanographic report sequences","315005","(Water temperature profile (Temperature profile observed by XBT or buoy)",,"007063","Depth below sea/water surface (cm)",,,"Operational"
5206.00,"15","Oceanographic report sequences","315005","(Water temperature profile (Temperature profile observed by XBT or buoy)",,"008080","Qualifier for GTSPP quality flag","= 13 Water depth at a level",,"Operational"
5207.00,"15","Oceanographic report sequences","315005","(Water temperature profile (Temperature profile observed by XBT or buoy)",,"033050","Global GTSPP quality flag",,,"Operational"
5208.00,"15","Oceanographic report sequences","315005","(Water temperature profile (Temperature profile observed by XBT or buoy)",,"022043","Sea/water temperature",,,"Operational"
5209.00,"15","Oceanographic report sequences","315005","(Water temperature profile (Temperature profile observed by XBT or buoy)",,"008080","Qualifier for GTSPP quality flag","= 11 Water temperature at a level",,"Operational"
5210.00,"15","Oceanographic report sequences","315005","(Water temperature profile (Temperature profile observed by XBT or buoy)",,"033050","Global GTSPP quality flag",,,"Operational"
5217.00,"16","Synoptic feature sequences","316001",,,"301011","Year, month, day",,,"Operational"
5218.00,"16","Synoptic feature sequences","316001",,,"004004","Hour",,,"Operational"
5219.00,"16","Synoptic feature sequences","316001",,,"301023","Latitude/longitude (coarse accuracy)",,,"Operational"
5220.00,"16","Synoptic feature sequences","316001",,,"001021","Synoptic feature identifier",,,"Operational"
5221.00,"16","Synoptic feature sequences","316001",,,"002041","Method for estimating reports related to synoptic features",,,"Operational"
5222.00,"16","Synoptic feature sequences","316001",,,"019001","Type of synoptic feature",,,"Operational"
5223.00,"16","Synoptic feature sequences","316001",,,"010051","Pressure reduced to mean sea level",,,"Operational"
5224.00,"16","Synoptic feature sequences","316001",,,"019002","Effective radius of feature",,,"Operational"
5225.00,"16","Synoptic feature sequences","316001",,,"019003","Wind speed threshold","15 m s-1 typically",,"Operational"
5226.00,"16","Synoptic feature sequences","316001",,,"019004","Effective radius with respect to wind speeds above threshold",,,"Operational"
5227.00,"16","Synoptic feature sequences","316002","(Header)",,"008021","Time significance","Data time (analysis)",,"Operational"
5228.00,"16","Synoptic feature sequences","316002","(Header)",,"004001","Year",,,"Operational"
5229.00,"16","Synoptic feature sequences","316002","(Header)",,"004002","Month",,,"Operational"
5230.00,"16","Synoptic feature sequences","316002","(Header)",,"004003","Day",,,"Operational"
5231.00,"16","Synoptic feature sequences","316002","(Header)",,"004004","Hour",,,"Operational"
5232.00,"16","Synoptic feature sequences","316002","(Header)",,"004005","Minute",,,"Operational"
5233.00,"16","Synoptic feature sequences","316002","(Header)",,"001033","Identification of originating/generating centre",,,"Operational"
5234.00,"16","Synoptic feature sequences","316002","(Header)",,"008021","Time significance","Validity time (forecast)",,"Operational"
5235.00,"16","Synoptic feature sequences","316002","(Header)",,"004001","Year",,,"Operational"
5236.00,"16","Synoptic feature sequences","316002","(Header)",,"004002","Month",,,"Operational"
5237.00,"16","Synoptic feature sequences","316002","(Header)",,"004003","Day",,,"Operational"
5238.00,"16","Synoptic feature sequences","316002","(Header)",,"004004","Hour",,,"Operational"
5239.00,"16","Synoptic feature sequences","316002","(Header)",,"004005","Minute",,,"Operational"
5240.00,"16","Synoptic feature sequences","316002","(Header)",,"007002","Height or altitude","Flight level (base of chart layer)",,"Operational"
5241.00,"16","Synoptic feature sequences","316002","(Header)",,"007002","Height or altitude","Flight level (top of chart layer)",,"Operational"
5242.00,"16","Synoptic feature sequences","316003","(Jet stream)",,"110000","Delayed replication of 10 descriptors",,,"Operational"
5243.00,"16","Synoptic feature sequences","316003","(Jet stream)",,"031001","Delayed descriptor replication factor",,,"Operational"
5244.00,"16","Synoptic feature sequences","316003","(Jet stream)",,"008011","Meteorological feature","Jet stream value",,"Operational"
5245.00,"16","Synoptic feature sequences","316003","(Jet stream)",,"008007","Dimensional significance","Value for line",,"Operational"
5246.00,"16","Synoptic feature sequences","316003","(Jet stream)",,"104000","Delayed replication of 4 descriptors",,,"Operational"
5247.00,"16","Synoptic feature sequences","316003","(Jet stream)",,"031001","Delayed descriptor replication factor",,,"Operational"
5248.00,"16","Synoptic feature sequences","316003","(Jet stream)",,"005002","Latitude (coarse accuracy)",,,"Operational"
5249.00,"16","Synoptic feature sequences","316003","(Jet stream)",,"006002","Longitude (coarse accuracy)",,,"Operational"
5250.00,"16","Synoptic feature sequences","316003","(Jet stream)",,"010002","Height","Flight level",,"Operational"
5251.00,"16","Synoptic feature sequences","316003","(Jet stream)",,"011002","Wind speed",,,"Operational"
5252.00,"16","Synoptic feature sequences","316003","(Jet stream)",,"008007","Dimensional significance","Cancel",,"Operational"
5253.00,"16","Synoptic feature sequences","316003","(Jet stream)",,"008011","Meteorological feature","Cancel | End of object",,"Operational"
5264.00,"16","Synoptic feature sequences","316004","(Turbulence)",,"111000","Delayed replication of 11 descriptors",,,"Operational"
5265.00,"16","Synoptic feature sequences","316004","(Turbulence)",,"031001","Delayed descriptor replication factor",,,"Operational"
5266.00,"16","Synoptic feature sequences","316004","(Turbulence)",,"008011","Meteorological feature","Value for turbulence",,"Operational"
5267.00,"16","Synoptic feature sequences","316004","(Turbulence)",,"008007","Dimensional significance","Value for area",,"Operational"
5268.00,"16","Synoptic feature sequences","316004","(Turbulence)",,"007002","Height or altitude","Flight level (base of layer)",,"Operational"
5269.00,"16","Synoptic feature sequences","316004","(Turbulence)",,"007002","Height or altitude","Flight level (top of layer)",,"Operational"
5270.00,"16","Synoptic feature sequences","316004","(Turbulence)",,"102000","Delayed replication of 2 descriptors",,,"Operational"
5271.00,"16","Synoptic feature sequences","316004","(Turbulence)",,"031001","Delayed descriptor replication factor",,,"Operational"
5272.00,"16","Synoptic feature sequences","316004","(Turbulence)",,"005002","Latitude (coarse accuracy)",,,"Operational"
5273.00,"16","Synoptic feature sequences","316004","(Turbulence)",,"006002","Longitude (coarse accuracy)",,,"Operational"
5274.00,"16","Synoptic feature sequences","316004","(Turbulence)",,"011031","Degree of turbulence",,"(see Note 1)","Operational"
5275.00,"16","Synoptic feature sequences","316004","(Turbulence)",,"008007","Dimensional significance","Cancel",,"Operational"
5276.00,"16","Synoptic feature sequences","316004","(Turbulence)",,"008011","Meteorological feature","Cancel | End of object",,"Operational"
5288.00,"16","Synoptic feature sequences","316005","(Storm)",,"108000","Delayed replication of 8 descriptors",,,"Operational"
5289.00,"16","Synoptic feature sequences","316005","(Storm)",,"031001","Delayed descriptor replication factor",,,"Operational"
5290.00,"16","Synoptic feature sequences","316005","(Storm)",,"008005","Meteorological attribute significance","Storm centre",,"Operational"
5291.00,"16","Synoptic feature sequences","316005","(Storm)",,"008007","Dimensional significance","Value for point",,"Operational"
5292.00,"16","Synoptic feature sequences","316005","(Storm)",,"005002","Latitude (coarse accuracy)",,,"Operational"
5293.00,"16","Synoptic feature sequences","316005","(Storm)",,"006002","Longitude (coarse accuracy)",,,"Operational"
5294.00,"16","Synoptic feature sequences","316005","(Storm)",,"001026","WMO storm name","Use ""UNKNOWN"" for a sandstorm",,"Operational"
5295.00,"16","Synoptic feature sequences","316005","(Storm)",,"019001","Type of synoptic feature","Value for type of storm",,"Operational"
5296.00,"16","Synoptic feature sequences","316005","(Storm)",,"008007","Dimensional significance","Cancel",,"Operational"
5297.00,"16","Synoptic feature sequences","316005","(Storm)",,"008005","Meteorological attribute significance","Cancel | End of object",,"Operational"
5307.00,"16","Synoptic feature sequences","316006","(Cloud)",,"112000","Delayed replication of 12 descriptors",,,"Operational"
5308.00,"16","Synoptic feature sequences","316006","(Cloud)",,"031001","Delayed descriptor replication factor",,,"Operational"
5309.00,"16","Synoptic feature sequences","316006","(Cloud)",,"008011","Meteorological feature","Value for cloud",,"Operational"
5310.00,"16","Synoptic feature sequences","316006","(Cloud)",,"008007","Dimensional significance","Value for area",,"Operational"
5311.00,"16","Synoptic feature sequences","316006","(Cloud)",,"007002","Height or altitude","Flight level (base of layer)",,"Operational"
5312.00,"16","Synoptic feature sequences","316006","(Cloud)",,"007002","Height or altitude","Flight level (top of layer)",,"Operational"
5313.00,"16","Synoptic feature sequences","316006","(Cloud)",,"102000","Delayed replication of 2 descriptors",,,"Operational"
5314.00,"16","Synoptic feature sequences","316006","(Cloud)",,"031001","Delayed descriptor replication factor",,,"Operational"
5315.00,"16","Synoptic feature sequences","316006","(Cloud)",,"005002","Latitude (coarse accuracy)",,,"Operational"
5316.00,"16","Synoptic feature sequences","316006","(Cloud)",,"006002","Longitude (coarse accuracy)",,,"Operational"
5317.00,"16","Synoptic feature sequences","316006","(Cloud)",,"020011","Cloud amount",,"(see Note 2)","Operational"
5318.00,"16","Synoptic feature sequences","316006","(Cloud)",,"020012","Cloud type",,,"Operational"
5319.00,"16","Synoptic feature sequences","316006","(Cloud)",,"008007","Dimensional significance","Cancel",,"Operational"
5320.00,"16","Synoptic feature sequences","316006","(Cloud)",,"008011","Meteorological feature","Cancel | End of object",,"Operational"
5333.00,"16","Synoptic feature sequences","316007","(Front)",,"110000","Delayed replication of 10 descriptors",,,"Operational"
5334.00,"16","Synoptic feature sequences","316007","(Front)",,"031001","Delayed descriptor replication factor",,,"Operational"
5335.00,"16","Synoptic feature sequences","316007","(Front)",,"008011","Meteorological feature","Value for type of front","(see Note 3)","Operational"
5336.00,"16","Synoptic feature sequences","316007","(Front)",,"008007","Dimensional significance","Value for line",,"Operational"
5337.00,"16","Synoptic feature sequences","316007","(Front)",,"104000","Delayed replication of 4 descriptors",,,"Operational"
5338.00,"16","Synoptic feature sequences","316007","(Front)",,"031001","Delayed descriptor replication factor",,,"Operational"
5339.00,"16","Synoptic feature sequences","316007","(Front)",,"005002","Latitude (coarse accuracy)",,,"Operational"
5340.00,"16","Synoptic feature sequences","316007","(Front)",,"006002","Longitude (coarse accuracy)",,,"Operational"
5341.00,"16","Synoptic feature sequences","316007","(Front)",,"019005","Direction of motion of feature",,,"Operational"
5342.00,"16","Synoptic feature sequences","316007","(Front)",,"019006","Speed of motion of feature",,,"Operational"
5343.00,"16","Synoptic feature sequences","316007","(Front)",,"008007","Dimensional significance","Cancel",,"Operational"
5344.00,"16","Synoptic feature sequences","316007","(Front)",,"008011","Meteorological feature","Cancel | End of object",,"Operational"
5355.00,"16","Synoptic feature sequences","316008","(Tropopause)",,"111000","Delayed replication of 11 descriptors",,,"Operational"
5356.00,"16","Synoptic feature sequences","316008","(Tropopause)",,"031001","Delayed descriptor replication factor",,,"Operational"
5357.00,"16","Synoptic feature sequences","316008","(Tropopause)",,"008001","Vertical sounding significance","Bit 3 set for tropopause",,"Operational"
5358.00,"16","Synoptic feature sequences","316008","(Tropopause)",,"008007","Dimensional significance","Value for point",,"Operational"
5359.00,"16","Synoptic feature sequences","316008","(Tropopause)",,"008023","First-order statistics","Type of tropopause value","(see Note 4)","Operational"
5360.00,"16","Synoptic feature sequences","316008","(Tropopause)",,"103000","Delayed replication of 3 descriptors",,,"Operational"
5361.00,"16","Synoptic feature sequences","316008","(Tropopause)",,"031001","Delayed descriptor replication factor",,,"Operational"
5362.00,"16","Synoptic feature sequences","316008","(Tropopause)",,"005002","Latitude (coarse accuracy)",,,"Operational"
5363.00,"16","Synoptic feature sequences","316008","(Tropopause)",,"006002","Longitude (coarse accuracy)",,,"Operational"
5364.00,"16","Synoptic feature sequences","316008","(Tropopause)",,"010002","Height",,,"Operational"
5365.00,"16","Synoptic feature sequences","316008","(Tropopause)",,"008023","First-order statistics","Cancel",,"Operational"
5366.00,"16","Synoptic feature sequences","316008","(Tropopause)",,"008007","Dimensional significance","Cancel",,"Operational"
5367.00,"16","Synoptic feature sequences","316008","(Tropopause)",,"008001","Vertical sounding significance","Cancel | End of object",,"Operational"
5379.00,"16","Synoptic feature sequences","316009","(Airframe icing area)",,"111000","Delayed replication of 11 descriptors",,,"Operational"
5380.00,"16","Synoptic feature sequences","316009","(Airframe icing area)",,"031001","Delayed descriptor replication factor",,,"Operational"
5381.00,"16","Synoptic feature sequences","316009","(Airframe icing area)",,"008011","Meteorological feature","Value for airframe icing",,"Operational"
5382.00,"16","Synoptic feature sequences","316009","(Airframe icing area)",,"008007","Dimensional significance","Value for area",,"Operational"
5383.00,"16","Synoptic feature sequences","316009","(Airframe icing area)",,"007002","Height or altitude","Flight level (base of layer)",,"Operational"
5384.00,"16","Synoptic feature sequences","316009","(Airframe icing area)",,"007002","Height or altitude","Flight level (top of layer)",,"Operational"
5385.00,"16","Synoptic feature sequences","316009","(Airframe icing area)",,"102000","Delayed replication of 2 descriptors",,,"Operational"
5386.00,"16","Synoptic feature sequences","316009","(Airframe icing area)",,"031001","Delayed descriptor replication factor",,,"Operational"
5387.00,"16","Synoptic feature sequences","316009","(Airframe icing area)",,"005002","Latitude (coarse accuracy)",,,"Operational"
5388.00,"16","Synoptic feature sequences","316009","(Airframe icing area)",,"006002","Longitude (coarse accuracy)",,,"Operational"
5389.00,"16","Synoptic feature sequences","316009","(Airframe icing area)",,"020041","Airframe icing","Type of airframe icing",,"Operational"
5390.00,"16","Synoptic feature sequences","316009","(Airframe icing area)",,"008007","Dimensional significance","Cancel",,"Operational"
5391.00,"16","Synoptic feature sequences","316009","(Airframe icing area)",,"008011","Meteorological feature","Cancel | End of object",,"Operational"
5403.00,"16","Synoptic feature sequences","316010","(Name of feature)",,"107000","Delayed replication of 7 descriptors",,,"Operational"
5404.00,"16","Synoptic feature sequences","316010","(Name of feature)",,"031001","Delayed descriptor replication factor",,,"Operational"
5405.00,"16","Synoptic feature sequences","316010","(Name of feature)",,"008011","Meteorological feature",,,"Operational"
5406.00,"16","Synoptic feature sequences","316010","(Name of feature)",,"008007","Dimensional significance","Value for point",,"Operational"
5407.00,"16","Synoptic feature sequences","316010","(Name of feature)",,"001022","Name of feature",,,"Operational"
5408.00,"16","Synoptic feature sequences","316010","(Name of feature)",,"005002","Latitude (coarse accuracy)",,,"Operational"
5409.00,"16","Synoptic feature sequences","316010","(Name of feature)",,"006002","Longitude (coarse accuracy)",,,"Operational"
5410.00,"16","Synoptic feature sequences","316010","(Name of feature)",,"008007","Dimensional significance","Cancel",,"Operational"
5411.00,"16","Synoptic feature sequences","316010","(Name of feature)",,"008011","Meteorological feature","Cancel | End of object",,"Operational"
5420.00,"16","Synoptic feature sequences","316011","(Volcano erupting)",,"117000","Delayed replication of 17 descriptors",,,"Operational"
5421.00,"16","Synoptic feature sequences","316011","(Volcano erupting)",,"031001","Delayed descriptor replication factor",,,"Operational"
5422.00,"16","Synoptic feature sequences","316011","(Volcano erupting)",,"008011","Meteorological feature","Value for special clouds",,"Operational"
5423.00,"16","Synoptic feature sequences","316011","(Volcano erupting)",,"001022","Name of feature","Volcano name",,"Operational"
5424.00,"16","Synoptic feature sequences","316011","(Volcano erupting)",,"008007","Dimensional significance","Value for point",,"Operational"
5425.00,"16","Synoptic feature sequences","316011","(Volcano erupting)",,"102000","Delayed replication of 2 descriptors",,,"Operational"
5426.00,"16","Synoptic feature sequences","316011","(Volcano erupting)",,"031001","Delayed descriptor replication factor",,,"Operational"
5427.00,"16","Synoptic feature sequences","316011","(Volcano erupting)",,"005002","Latitude (coarse accuracy)",,,"Operational"
5428.00,"16","Synoptic feature sequences","316011","(Volcano erupting)",,"006002","Longitude (coarse accuracy)",,,"Operational"
5429.00,"16","Synoptic feature sequences","316011","(Volcano erupting)",,"008021","Time significance","Eruption starting time",,"Operational"
5430.00,"16","Synoptic feature sequences","316011","(Volcano erupting)",,"004001","Year",,,"Operational"
5431.00,"16","Synoptic feature sequences","316011","(Volcano erupting)",,"004002","Month",,,"Operational"
5432.00,"16","Synoptic feature sequences","316011","(Volcano erupting)",,"004003","Day",,,"Operational"
5433.00,"16","Synoptic feature sequences","316011","(Volcano erupting)",,"004004","Hour",,,"Operational"
5434.00,"16","Synoptic feature sequences","316011","(Volcano erupting)",,"004005","Minute",,,"Operational"
5435.00,"16","Synoptic feature sequences","316011","(Volcano erupting)",,"020090","Special clouds","Clouds from volcanic eruptions",,"Operational"
5436.00,"16","Synoptic feature sequences","316011","(Volcano erupting)",,"008021","Time significance","Cancel",,"Operational"
5437.00,"16","Synoptic feature sequences","316011","(Volcano erupting)",,"008007","Dimensional significance","Cancel",,"Operational"
5438.00,"16","Synoptic feature sequences","316011","(Volcano erupting)",,"008011","Meteorological feature","Cancel | End of object",,"Operational"
5456.00,"16","Synoptic feature sequences","316020","(Tropical storm identification)",,"001033","Identification of originating/generating centre",,,"Operational"
5457.00,"16","Synoptic feature sequences","316020","(Tropical storm identification)",,"001025","Storm identifier",,,"Operational"
5458.00,"16","Synoptic feature sequences","316020","(Tropical storm identification)",,"001027","WMO long storm name",,,"Operational"
5459.00,"16","Synoptic feature sequences","316020","(Tropical storm identification)",,"301011","Year, month, day",,,"Operational"
5460.00,"16","Synoptic feature sequences","316020","(Tropical storm identification)",,"301012","Hour, minute",,,"Operational"
5461.00,"16","Synoptic feature sequences","316021","(Analysis data)",,"301023","Latitude/longitude (coarse accuracy)",,,"Operational"
5462.00,"16","Synoptic feature sequences","316021","(Analysis data)",,"002041","Method for estimating reports related to synoptic features",,,"Operational"
5463.00,"16","Synoptic feature sequences","316021","(Analysis data)",,"019001","Type of synoptic feature",,,"Operational"
5464.00,"16","Synoptic feature sequences","316021","(Analysis data)",,"019007","Effective radius of feature",,,"Operational"
5465.00,"16","Synoptic feature sequences","316021","(Analysis data)",,"019005","Direction of motion of feature",,,"Operational"
5466.00,"16","Synoptic feature sequences","316021","(Analysis data)",,"019006","Speed of motion of feature",,,"Operational"
5467.00,"16","Synoptic feature sequences","316021","(Analysis data)",,"019008","Vertical extent of circulation",,,"Operational"
5468.00,"16","Synoptic feature sequences","316021","(Analysis data)",,"008005","Meteorological attribute significance","= 1 Storm centre",,"Operational"
5469.00,"16","Synoptic feature sequences","316021","(Analysis data)",,"010004","Pressure","Storm centre by virtue of preceding significance qualifier",,"Operational"
5470.00,"16","Synoptic feature sequences","316021","(Analysis data)",,"008005","Meteorological attribute significance","= 2 Outer limit or edge of feature",,"Operational"
5471.00,"16","Synoptic feature sequences","316021","(Analysis data)",,"010004","Pressure","Outer limit",,"Operational"
5472.00,"16","Synoptic feature sequences","316021","(Analysis data)",,"019007","Effective radius of feature","Outer limit",,"Operational"
5473.00,"16","Synoptic feature sequences","316021","(Analysis data)",,"008005","Meteorological attribute significance","= 3 Location of maximum wind",,"Operational"
5474.00,"16","Synoptic feature sequences","316021","(Analysis data)",,"008021","Time significance","Time averaged",,"Operational"
5475.00,"16","Synoptic feature sequences","316021","(Analysis data)",,"004075","Short time period or displacement","Minutes",,"Operational"
5476.00,"16","Synoptic feature sequences","316021","(Analysis data)",,"011040","Maximum wind speed (mean wind)",,,"Operational"
5477.00,"16","Synoptic feature sequences","316021","(Analysis data)",,"019007","Effective radius of feature","Maximum wind",,"Operational"
5478.00,"16","Synoptic feature sequences","316021","(Analysis data)",,"105004","Replicate 5 descriptors 4 times",,,"Operational"
5479.00,"16","Synoptic feature sequences","316021","(Analysis data)",,"005021","Bearing or azimuth","Starting",,"Operational"
5480.00,"16","Synoptic feature sequences","316021","(Analysis data)",,"005021","Bearing or azimuth","Ending",,"Operational"
5481.00,"16","Synoptic feature sequences","316021","(Analysis data)",,"102002","Replicate 2 descriptors 2 times",,,"Operational"
5482.00,"16","Synoptic feature sequences","316021","(Analysis data)",,"019003","Wind speed threshold",,,"Operational"
5483.00,"16","Synoptic feature sequences","316021","(Analysis data)",,"019004","Effective radius with respect to wind speeds above threshold",,,"Operational"
5484.00,"16","Synoptic feature sequences","316022","(Forecast data)",,"001032","Generating application","NWP model name, etc. code table defined by originating/generating centre",,"Operational"
5485.00,"16","Synoptic feature sequences","316022","(Forecast data)",,"002041","Method for estimating reports related to synoptic features",,,"Operational"
5486.00,"16","Synoptic feature sequences","316022","(Forecast data)",,"019001","Type of synoptic feature",,,"Operational"
5487.00,"16","Synoptic feature sequences","316022","(Forecast data)",,"019010","Method for tracking the centre of synoptic feature",,,"Operational"
5488.00,"16","Synoptic feature sequences","316022","(Forecast data)",,"118000","Delayed replication of 18 descriptors",,,"Operational"
5489.00,"16","Synoptic feature sequences","316022","(Forecast data)",,"031001","Delayed descriptor replication factor",,,"Operational"
5490.00,"16","Synoptic feature sequences","316022","(Forecast data)",,"008021","Time significance","Forecast",,"Operational"
5491.00,"16","Synoptic feature sequences","316022","(Forecast data)",,"004014","Time increment","Hours",,"Operational"
5492.00,"16","Synoptic feature sequences","316022","(Forecast data)",,"008005","Meteorological attribute significance","Surface synoptic feature",,"Operational"
5493.00,"16","Synoptic feature sequences","316022","(Forecast data)",,"301023","Latitude/longitude (coarse accuracy)",,,"Operational"
5494.00,"16","Synoptic feature sequences","316022","(Forecast data)",,"019005","Direction of motion of feature",,,"Operational"
5495.00,"16","Synoptic feature sequences","316022","(Forecast data)",,"019006","Speed of motion of feature",,,"Operational"
5496.00,"16","Synoptic feature sequences","316022","(Forecast data)",,"010004","Pressure",,,"Operational"
5497.00,"16","Synoptic feature sequences","316022","(Forecast data)",,"011041","Maximum wind gust speed","For example, used in the United States",,"Operational"
5498.00,"16","Synoptic feature sequences","316022","(Forecast data)",,"008021","Time significance","Forecast time averaged",,"Operational"
5499.00,"16","Synoptic feature sequences","316022","(Forecast data)",,"004075","Short time period or displacement","Minutes",,"Operational"
5500.00,"16","Synoptic feature sequences","316022","(Forecast data)",,"011040","Maximum wind speed (mean wind)",,,"Operational"
5501.00,"16","Synoptic feature sequences","316022","(Forecast data)",,"019008","Vertical extent of circulation",,,"Operational"
5502.00,"16","Synoptic feature sequences","316022","(Forecast data)",,"105004","Replicate 5 descriptors 4 times",,,"Operational"
5503.00,"16","Synoptic feature sequences","316022","(Forecast data)",,"005021","Bearing or azimuth","Starting",,"Operational"
5504.00,"16","Synoptic feature sequences","316022","(Forecast data)",,"005021","Bearing or azimuth","Ending",,"Operational"
5505.00,"16","Synoptic feature sequences","316022","(Forecast data)",,"102002","Replicate 2 descriptors 2 times",,,"Operational"
5506.00,"16","Synoptic feature sequences","316022","(Forecast data)",,"019003","Wind speed threshold",,,"Operational"
5507.00,"16","Synoptic feature sequences","316022","(Forecast data)",,"019004","Effective radius with respect to wind speeds above threshold",,,"Operational"
5531.00,"16","Synoptic feature sequences","316026","(Tropical storm analysis information)",,"316020","Tropical storm identification",,,"Operational"
5532.00,"16","Synoptic feature sequences","316026","(Tropical storm analysis information)",,"316021","Analysis data",,,"Operational"
5533.00,"16","Synoptic feature sequences","316027","(Tropical storm forecast information)",,"316020","Tropical storm identification",,,"Operational"
5534.00,"16","Synoptic feature sequences","316027","(Tropical storm forecast information)",,"316022","Forecast data",,,"Operational"
5535.00,"16","Synoptic feature sequences","316030","(SIGMET header)",,"301014","Time period","For which SIGMET is valid",,"Operational"
5536.00,"16","Synoptic feature sequences","316030","(SIGMET header)",,"001037","SIGMET sequence identifier",,,"Operational"
5537.00,"16","Synoptic feature sequences","316030","(SIGMET header)",,"010064","SIGMET cruising level",,,"Operational"
5538.00,"16","Synoptic feature sequences","316030","(SIGMET header)",,"008019","Qualifier for following centre identifier","= 1 ATS unit serving FIR",,"Operational"
5539.00,"16","Synoptic feature sequences","316030","(SIGMET header)",,"001062","Short ICAO location indicator",,,"Operational"
5540.00,"16","Synoptic feature sequences","316030","(SIGMET header)",,"008019","Qualifier for following centre identifier","= 2 FIR, = 3 UIR, = 4 CTA",,"Operational"
5541.00,"16","Synoptic feature sequences","316030","(SIGMET header)",,"001065","ICAO region identifier",,,"Operational"
5542.00,"16","Synoptic feature sequences","316030","(SIGMET header)",,"008019","Qualifier for following centre identifier","= 6 MWO",,"Operational"
5543.00,"16","Synoptic feature sequences","316030","(SIGMET header)",,"001062","Short ICAO location indicator",,,"Operational"
5544.00,"16","Synoptic feature sequences","316030","(SIGMET header)",,"008019","Qualifier for following centre identifier","Set to missing (cancel)",,"Operational"
5545.00,"16","Synoptic feature sequences","316031","(SIGMET, Observed or forecast location and motion)",,"008021","Time significance","= 16 Analysis, = 4 Forecast",,"Operational"
5546.00,"16","Synoptic feature sequences","316031","(SIGMET, Observed or forecast location and motion)",,"301011","Year, month, day",,,"Operational"
5547.00,"16","Synoptic feature sequences","316031","(SIGMET, Observed or forecast location and motion)",,"301012","Hour, minute",,,"Operational"
5548.00,"16","Synoptic feature sequences","316031","(SIGMET, Observed or forecast location and motion)",,"301027","Description of a feature in 3-D or 2-D",,,"Operational"
5549.00,"16","Synoptic feature sequences","316031","(SIGMET, Observed or forecast location and motion)",,"019005","Direction of motion of feature",,,"Operational"
5550.00,"16","Synoptic feature sequences","316031","(SIGMET, Observed or forecast location and motion)",,"019006","Speed of motion of feature",,,"Operational"
5551.00,"16","Synoptic feature sequences","316031","(SIGMET, Observed or forecast location and motion)",,"020028","Expected change in intensity",,,"Operational"
5552.00,"16","Synoptic feature sequences","316031","(SIGMET, Observed or forecast location and motion)",,"008021","Time significance","Set to missing (cancel)",,"Operational"
5553.00,"16","Synoptic feature sequences","316032","(SIGMET, Forecast position)",,"008021","Time significance","= 4 Forecast",,"Operational"
5554.00,"16","Synoptic feature sequences","316032","(SIGMET, Forecast position)",,"301011","Year, month, day",,,"Operational"
5555.00,"16","Synoptic feature sequences","316032","(SIGMET, Forecast position)",,"301012","Hour, minute",,,"Operational"
5556.00,"16","Synoptic feature sequences","316032","(SIGMET, Forecast position)",,"301027","Description of a feature in 3-D or 2-D",,,"Operational"
5557.00,"16","Synoptic feature sequences","316032","(SIGMET, Forecast position)",,"008021","Time significance","Set to missing (cancel)",,"Operational"
5558.00,"16","Synoptic feature sequences","316033","(SIGMET, Outlook)",,"008021","Time significance","= 4 Forecast",,"Operational"
5559.00,"16","Synoptic feature sequences","316033","(SIGMET, Outlook)",,"301011","Year, month, day",,,"Operational"
5560.00,"16","Synoptic feature sequences","316033","(SIGMET, Outlook)",,"301012","Hour, minute",,,"Operational"
5561.00,"16","Synoptic feature sequences","316033","(SIGMET, Outlook)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
5562.00,"16","Synoptic feature sequences","316033","(SIGMET, Outlook)",,"031001","Delayed descriptor replication factor",,,"Operational"
5563.00,"16","Synoptic feature sequences","316033","(SIGMET, Outlook)",,"301027","Description of a feature in 3-D or 2-D",,,"Operational"
5564.00,"16","Synoptic feature sequences","316033","(SIGMET, Outlook)",,"008021","Time significance","Set to missing (cancel)",,"Operational"
5566.00,"16","Synoptic feature sequences","316034","(Volcanic Ash SIGMET)",,"008079","Product status","= 0 Normal issue, = 1 Correction",,"Operational"
5567.00,"16","Synoptic feature sequences","316034","(Volcanic Ash SIGMET)",,"316030","SIGMET header",,,"Operational"
5568.00,"16","Synoptic feature sequences","316034","(Volcanic Ash SIGMET)",,"008011","Meteorological feature","= 17 Volcano",,"Operational"
5569.00,"16","Synoptic feature sequences","316034","(Volcanic Ash SIGMET)",,"001022","Name of feature",,,"Operational"
5570.00,"16","Synoptic feature sequences","316034","(Volcanic Ash SIGMET)",,"008007","Dimensional significance","= 0 Point",,"Operational"
5571.00,"16","Synoptic feature sequences","316034","(Volcanic Ash SIGMET)",,"301023","Latitude/longitude (coarse accuracy)",,,"Operational"
5572.00,"16","Synoptic feature sequences","316034","(Volcanic Ash SIGMET)",,"008007","Dimensional significance","Set to missing (cancel)",,"Operational"
5573.00,"16","Synoptic feature sequences","316034","(Volcanic Ash SIGMET)",,"020090","Special clouds","= 5 Clouds from volcanic eruptions",,"Operational"
5574.00,"16","Synoptic feature sequences","316034","(Volcanic Ash SIGMET)",,"316031","SIGMET, Observed or forecast location and motion",,,"Operational"
5575.00,"16","Synoptic feature sequences","316034","(Volcanic Ash SIGMET)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
5576.00,"16","Synoptic feature sequences","316034","(Volcanic Ash SIGMET)",,"031000","Short delayed descriptor replication factor",,,"Operational"
5577.00,"16","Synoptic feature sequences","316034","(Volcanic Ash SIGMET)",,"316032","SIGMET, Forecast position",,,"Operational"
5578.00,"16","Synoptic feature sequences","316034","(Volcanic Ash SIGMET)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
5579.00,"16","Synoptic feature sequences","316034","(Volcanic Ash SIGMET)",,"031001","Delayed descriptor replication factor",,,"Operational"
5580.00,"16","Synoptic feature sequences","316034","(Volcanic Ash SIGMET)",,"316033","SIGMET, Outlook",,,"Operational"
5581.00,"16","Synoptic feature sequences","316034","(Volcanic Ash SIGMET)",,"008011","Meteorological feature","Set to missing (cancel)",,"Operational"
5582.00,"16","Synoptic feature sequences","316034","(Volcanic Ash SIGMET)",,"008079","Product status","Set to missing (cancel)",,"Operational"
5584.00,"16","Synoptic feature sequences","316035","(Thunderstorm SIGMET)",,"008079","Product status","= 0 Normal issue, = 1 Correction",,"Operational"
5585.00,"16","Synoptic feature sequences","316035","(Thunderstorm SIGMET)",,"316030","SIGMET header",,,"Operational"
5586.00,"16","Synoptic feature sequences","316035","(Thunderstorm SIGMET)",,"008011","Meteorological feature","= 21 Thunderstorm",,"Operational"
5587.00,"16","Synoptic feature sequences","316035","(Thunderstorm SIGMET)",,"020023","Other weather phenomena","Bit 2 = Squalls or all 18 bits = Missing",,"Operational"
5588.00,"16","Synoptic feature sequences","316035","(Thunderstorm SIGMET)",,"020021","Type of precipitation","Bit 14 = Hail or all 30 bits = Missing",,"Operational"
5589.00,"16","Synoptic feature sequences","316035","(Thunderstorm SIGMET)",,"020008","Cloud distribution for aviation","= 15 OBSC, = 16 EMBD, = 12 FRQ, = 31 Missing",,"Operational"
5590.00,"16","Synoptic feature sequences","316035","(Thunderstorm SIGMET)",,"316031","SIGMET, Observed or forecast location and motion",,,"Operational"
5591.00,"16","Synoptic feature sequences","316035","(Thunderstorm SIGMET)",,"008011","Meteorological feature","Set to missing (cancel)",,"Operational"
5592.00,"16","Synoptic feature sequences","316035","(Thunderstorm SIGMET)",,"008079","Product status","Set to missing (cancel)",,"Operational"
5593.00,"16","Synoptic feature sequences","316036","(Tropical cyclone SIGMET)",,"008079","Product status","= 0 Normal issue, = 1 Correction",,"Operational"
5594.00,"16","Synoptic feature sequences","316036","(Tropical cyclone SIGMET)",,"316030","SIGMET header",,,"Operational"
5595.00,"16","Synoptic feature sequences","316036","(Tropical cyclone SIGMET)",,"008011","Meteorological feature","= 22 Tropical cyclone",,"Operational"
5596.00,"16","Synoptic feature sequences","316036","(Tropical cyclone SIGMET)",,"001027","WMO long storm name",,,"Operational"
5597.00,"16","Synoptic feature sequences","316036","(Tropical cyclone SIGMET)",,"316031","SIGMET, Observed or forecast location and motion",,,"Operational"
5598.00,"16","Synoptic feature sequences","316036","(Tropical cyclone SIGMET)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
5599.00,"16","Synoptic feature sequences","316036","(Tropical cyclone SIGMET)",,"031000","Short delayed descriptor replication factor",,,"Operational"
5600.00,"16","Synoptic feature sequences","316036","(Tropical cyclone SIGMET)",,"316032","SIGMET, Forecast position",,,"Operational"
5601.00,"16","Synoptic feature sequences","316036","(Tropical cyclone SIGMET)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
5602.00,"16","Synoptic feature sequences","316036","(Tropical cyclone SIGMET)",,"031001","Delayed descriptor replication factor",,,"Operational"
5603.00,"16","Synoptic feature sequences","316036","(Tropical cyclone SIGMET)",,"316033","SIGMET, Outlook",,,"Operational"
5604.00,"16","Synoptic feature sequences","316036","(Tropical cyclone SIGMET)",,"008011","Meteorological feature","Set to missing (cancel)",,"Operational"
5605.00,"16","Synoptic feature sequences","316036","(Tropical cyclone SIGMET)",,"008079","Product status","Set to missing (cancel)",,"Operational"
5607.00,"16","Synoptic feature sequences","316037","(Turbulence SIGMET)",,"008079","Product status","= 0 Normal issue, = 1 Correction",,"Operational"
5608.00,"16","Synoptic feature sequences","316037","(Turbulence SIGMET)",,"316030","SIGMET header",,,"Operational"
5609.00,"16","Synoptic feature sequences","316037","(Turbulence SIGMET)",,"008011","Meteorological feature","= 13 Turbulence",,"Operational"
5610.00,"16","Synoptic feature sequences","316037","(Turbulence SIGMET)",,"011031","Degree of turbulence","= 10 Moderate, = 11 Severe",,"Operational"
5611.00,"16","Synoptic feature sequences","316037","(Turbulence SIGMET)",,"316031","SIGMET, Observed or forecast location and motion",,,"Operational"
5612.00,"16","Synoptic feature sequences","316037","(Turbulence SIGMET)",,"008011","Meteorological feature","Set to missing (cancel)",,"Operational"
5613.00,"16","Synoptic feature sequences","316037","(Turbulence SIGMET)",,"008079","Product status","Set to missing (cancel)",,"Operational"
5614.00,"16","Synoptic feature sequences","316038","(Icing SIGMET)",,"008079","Product status","= 0 Normal issue, = 1 Correction",,"Operational"
5615.00,"16","Synoptic feature sequences","316038","(Icing SIGMET)",,"316030","SIGMET header",,,"Operational"
5616.00,"16","Synoptic feature sequences","316038","(Icing SIGMET)",,"008011","Meteorological feature","= 15 Airframe icing",,"Operational"
5617.00,"16","Synoptic feature sequences","316038","(Icing SIGMET)",,"020041","Airframe icing","= 7 Severe",,"Operational"
5618.00,"16","Synoptic feature sequences","316038","(Icing SIGMET)",,"020021","Type of precipitation","Bit 3 = Liquid freezing or all 30 bits = Missing",,"Operational"
5619.00,"16","Synoptic feature sequences","316038","(Icing SIGMET)",,"316031","SIGMET, Observed or forecast location and motion",,,"Operational"
5620.00,"16","Synoptic feature sequences","316038","(Icing SIGMET)",,"008011","Meteorological feature","Set to missing (cancel)",,"Operational"
5621.00,"16","Synoptic feature sequences","316038","(Icing SIGMET)",,"008079","Product status","Set to missing (cancel)",,"Operational"
5622.00,"16","Synoptic feature sequences","316039","(Mountain wave, duststorm or sandstorm SIGMET)",,"008079","Product status","= 0 Normal issue, = 1 Correction",,"Operational"
5623.00,"16","Synoptic feature sequences","316039","(Mountain wave, duststorm or sandstorm SIGMET)",,"316030","SIGMET header",,,"Operational"
5624.00,"16","Synoptic feature sequences","316039","(Mountain wave, duststorm or sandstorm SIGMET)",,"008011","Meteorological feature","= 23 Mountain wave, = 24 Duststorm, = 25 Sandstorm",,"Operational"
5625.00,"16","Synoptic feature sequences","316039","(Mountain wave, duststorm or sandstorm SIGMET)",,"020024","Intensity of phenomena","= 3 Heavy, = 5 Severe",,"Operational"
5626.00,"16","Synoptic feature sequences","316039","(Mountain wave, duststorm or sandstorm SIGMET)",,"316031","SIGMET, Observed or forecast location and motion",,,"Operational"
5627.00,"16","Synoptic feature sequences","316039","(Mountain wave, duststorm or sandstorm SIGMET)",,"008011","Meteorological feature","Set to missing (cancel)",,"Operational"
5628.00,"16","Synoptic feature sequences","316039","(Mountain wave, duststorm or sandstorm SIGMET)",,"008079","Product status","Set to missing (cancel)",,"Operational"
5629.00,"16","Synoptic feature sequences","316040","(Cancellation of SIGMET)",,"316030","SIGMET header",,,"Operational"
5630.00,"16","Synoptic feature sequences","316040","(Cancellation of SIGMET)",,"008079","Product status","= 4 Cancellation",,"Operational"
5631.00,"16","Synoptic feature sequences","316040","(Cancellation of SIGMET)",,"301014","Time period","Of the SIGMET to be cancelled",,"Operational"
5632.00,"16","Synoptic feature sequences","316040","(Cancellation of SIGMET)",,"001037","SIGMET sequence identifier","Of the SIGMET to be cancelled",,"Operational"
5633.00,"16","Synoptic feature sequences","316040","(Cancellation of SIGMET)",,"010064","SIGMET cruising level","Of the SIGMET to be cancelled",,"Operational"
5634.00,"16","Synoptic feature sequences","316040","(Cancellation of SIGMET)",,"008079","Product status","Set to missing (cancel)",,"Operational"
5635.00,"16","Synoptic feature sequences","316050","(RADOB template - Part A: Information on tropical cyclone)",,"301001","WMO block and station numbers",,,"Operational"
5636.00,"16","Synoptic feature sequences","316050","(RADOB template - Part A: Information on tropical cyclone)",,"301011","Year, month, day",,,"Operational"
5637.00,"16","Synoptic feature sequences","316050","(RADOB template - Part A: Information on tropical cyclone)",,"301012","Hour, minute",,,"Operational"
5638.00,"16","Synoptic feature sequences","316050","(RADOB template - Part A: Information on tropical cyclone)",,"002160","Wave length of the radar",,,"Operational"
5639.00,"16","Synoptic feature sequences","316050","(RADOB template - Part A: Information on tropical cyclone)",,"008005","Meteorological attribute significance","= 1",,"Operational"
5640.00,"16","Synoptic feature sequences","316050","(RADOB template - Part A: Information on tropical cyclone)",,"005002","Latitude (coarse accuracy)",,,"Operational"
5641.00,"16","Synoptic feature sequences","316050","(RADOB template - Part A: Information on tropical cyclone)",,"006002","Longitude (coarse accuracy)",,,"Operational"
5642.00,"16","Synoptic feature sequences","316050","(RADOB template - Part A: Information on tropical cyclone)",,"008005","Meteorological attribute significance","Cancel",,"Operational"
5643.00,"16","Synoptic feature sequences","316050","(RADOB template - Part A: Information on tropical cyclone)",,"019100","Time interval to calculate the movement of the tropical cyclone",,,"Operational"
5644.00,"16","Synoptic feature sequences","316050","(RADOB template - Part A: Information on tropical cyclone)",,"019005","Direction of motion of feature",,,"Operational"
5645.00,"16","Synoptic feature sequences","316050","(RADOB template - Part A: Information on tropical cyclone)",,"019006","Speed of motion of feature",,,"Operational"
5646.00,"16","Synoptic feature sequences","316050","(RADOB template - Part A: Information on tropical cyclone)",,"019101","Accuracy of the position of the centre of the tropical cyclone",,,"Operational"
5647.00,"16","Synoptic feature sequences","316050","(RADOB template - Part A: Information on tropical cyclone)",,"019102","Shape and definition of the eye of the tropical cyclone",,,"Operational"
5648.00,"16","Synoptic feature sequences","316050","(RADOB template - Part A: Information on tropical cyclone)",,"019103","Diameter of major axis of the eye of the tropical cyclone",,,"Operational"
5649.00,"16","Synoptic feature sequences","316050","(RADOB template - Part A: Information on tropical cyclone)",,"019104","Change in character of the eye during the 30 minutes",,,"Operational"
5650.00,"16","Synoptic feature sequences","316050","(RADOB template - Part A: Information on tropical cyclone)",,"019105","Distance between the end of spiral band and the centre",,,"Operational"
5651.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"301005","Originating centre/sub-centre",,,"Operational"
5652.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"301011","Year, month, day",,,"Operational"
5653.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"301012","Hour, minute",,,"Operational"
5654.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"001007","Satellite identifier",,,"Operational"
5655.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"025150","Method of tropical cyclone intensity analysis using satellite data",,,"Operational"
5656.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"122000","Delayed replication of 22 descriptors",,,"Operational"
5657.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"031001","Delayed descriptor replication factor",,,"Operational"
5658.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"001027","WMO long storm name",,,"Operational"
5659.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"019150","Typhoon International Common Number (Typhoon Committee)",,,"Operational"
5660.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"019106","Identification number of tropical cyclone",,,"Operational"
5661.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"008005","Meteorological attribute significance","= 1",,"Operational"
5662.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"005002","Latitude (coarse accuracy)",,,"Operational"
5663.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"006002","Longitude (coarse accuracy)",,,"Operational"
5664.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"008005","Meteorological attribute significance","Cancel",,"Operational"
5665.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"019107","Time interval over which the movement of the tropical cyclone has been calculated",,,"Operational"
5666.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"019005","Direction of motion of feature",,,"Operational"
5667.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"019006","Speed of motion of feature",,,"Operational"
5668.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"019108","Accuracy of geographical position of the tropical cyclone",,,"Operational"
5669.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"019109","Mean diameter of the overcast cloud of the tropical cyclone",,,"Operational"
5670.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"019110","Apparent 24-hour change in intensity of the tropical cyclone",,,"Operational"
5671.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"019111","Current Intensity (CI) number of the tropical cyclone",,,"Operational"
5672.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"019112","Data Tropical (DT) number of the tropical cyclone",,,"Operational"
5673.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"019113","Cloud pattern type of the DT-number",,,"Operational"
5674.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"019114","Model Expected Tropical (MET) number of the tropical cyclone",,,"Operational"
5675.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"019115","Trend of the past 24-hour change (+: Developed, -: Weakened)",,,"Operational"
5676.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"019116","Pattern Tropical (PT) number of the tropical cyclone",,,"Operational"
5677.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"019117","Cloud picture type of the PT-number",,,"Operational"
5678.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"019118","Final Tropical (T) number of the tropical cyclone",,,"Operational"
5679.00,"16","Synoptic feature sequences","316052","(SAREP template - Part A: Information on tropical cyclone)",,"019119","Type of the final T-number",,,"Operational"
5708.00,"16","Synoptic feature sequences","316060","(Definition of squall line (by 3 points: Centre, North, South) and forecasted trajectory and evolution)",,"301011","Year, month, day",,,"Operational"
5709.00,"16","Synoptic feature sequences","316060","(Definition of squall line (by 3 points: Centre, North, South) and forecasted trajectory and evolution)",,"301012","Hour, minute",,,"Operational"
5710.00,"16","Synoptic feature sequences","316060","(Definition of squall line (by 3 points: Centre, North, South) and forecasted trajectory and evolution)","Position of squall line centre","005002","Latitude (coarse accuracy)",,,"Operational"
5711.00,"16","Synoptic feature sequences","316060","(Definition of squall line (by 3 points: Centre, North, South) and forecasted trajectory and evolution)","Position of squall line centre","006002","Longitude (coarse accuracy)",,,"Operational"
5712.00,"16","Synoptic feature sequences","316060","(Definition of squall line (by 3 points: Centre, North, South) and forecasted trajectory and evolution)","Position of squall line centre","019005","Direction of motion of feature",,,"Operational"
5713.00,"16","Synoptic feature sequences","316060","(Definition of squall line (by 3 points: Centre, North, South) and forecasted trajectory and evolution)","Position of squall line centre","019006","Speed of motion of feature",,,"Operational"
5714.00,"16","Synoptic feature sequences","316060","(Definition of squall line (by 3 points: Centre, North, South) and forecasted trajectory and evolution)","Amplitude of feature from most external points to centre point - North point","005002","Latitude (coarse accuracy)",,,"Operational"
5715.00,"16","Synoptic feature sequences","316060","(Definition of squall line (by 3 points: Centre, North, South) and forecasted trajectory and evolution)","Amplitude of feature from most external points to centre point - North point","006002","Longitude (coarse accuracy)",,,"Operational"
5716.00,"16","Synoptic feature sequences","316060","(Definition of squall line (by 3 points: Centre, North, South) and forecasted trajectory and evolution)","Amplitude of feature from most external points to centre point - South point","005002","Latitude (coarse accuracy)",,,"Operational"
5717.00,"16","Synoptic feature sequences","316060","(Definition of squall line (by 3 points: Centre, North, South) and forecasted trajectory and evolution)","Amplitude of feature from most external points to centre point - South point","006002","Longitude (coarse accuracy)",,,"Operational"
5718.00,"16","Synoptic feature sequences","316060","(Definition of squall line (by 3 points: Centre, North, South) and forecasted trajectory and evolution)","Amplitude of feature from most external points to centre point - Evolution","004074","Short time period or displacement","Period of validity",,"Operational"
5719.00,"16","Synoptic feature sequences","316060","(Definition of squall line (by 3 points: Centre, North, South) and forecasted trajectory and evolution)","Amplitude of feature from most external points to centre point - Evolution","020048","Evolution of feature",,,"Operational"
5720.00,"16","Synoptic feature sequences","316060","(Definition of squall line (by 3 points: Centre, North, South) and forecasted trajectory and evolution)","Amplitude of feature from most external points to centre point - Evolution","011041","Maximum wind gust speed","Maximum burst expected",,"Operational"
5721.00,"16","Synoptic feature sequences","316060","(Definition of squall line (by 3 points: Centre, North, South) and forecasted trajectory and evolution)","Amplitude of feature from most external points to centre point - Evolution","013055","Intensity of precipitation","Intensity of rain expected",,"Operational"
5722.00,"16","Synoptic feature sequences","316061","(Definition of squall line (by centre and several points: North points and South points) and forecasted trajectory and evolution)",,"301011","Year, month, day",,,"Operational"
5723.00,"16","Synoptic feature sequences","316061","(Definition of squall line (by centre and several points: North points and South points) and forecasted trajectory and evolution)",,"301012","Hour, minute",,,"Operational"
5724.00,"16","Synoptic feature sequences","316061","(Definition of squall line (by centre and several points: North points and South points) and forecasted trajectory and evolution)","Position of squall line centre","005002","Latitude (coarse accuracy)",,,"Operational"
5725.00,"16","Synoptic feature sequences","316061","(Definition of squall line (by centre and several points: North points and South points) and forecasted trajectory and evolution)","Position of squall line centre","006002","Longitude (coarse accuracy)",,,"Operational"
5726.00,"16","Synoptic feature sequences","316061","(Definition of squall line (by centre and several points: North points and South points) and forecasted trajectory and evolution)","Position of squall line centre","019005","Direction of motion of feature",,,"Operational"
5727.00,"16","Synoptic feature sequences","316061","(Definition of squall line (by centre and several points: North points and South points) and forecasted trajectory and evolution)","Position of squall line centre","019006","Speed of motion of feature",,,"Operational"
5728.00,"16","Synoptic feature sequences","316061","(Definition of squall line (by centre and several points: North points and South points) and forecasted trajectory and evolution)","Amplitude of feature from most external points to centre point - North points","102000","Delayed replication of 2 descriptors",,,"Operational"
5729.00,"16","Synoptic feature sequences","316061","(Definition of squall line (by centre and several points: North points and South points) and forecasted trajectory and evolution)","Amplitude of feature from most external points to centre point - North points","031001","Delayed descriptor replication factor",,,"Operational"
5730.00,"16","Synoptic feature sequences","316061","(Definition of squall line (by centre and several points: North points and South points) and forecasted trajectory and evolution)","Amplitude of feature from most external points to centre point - North points","005002","Latitude (coarse accuracy)",,,"Operational"
5731.00,"16","Synoptic feature sequences","316061","(Definition of squall line (by centre and several points: North points and South points) and forecasted trajectory and evolution)","Amplitude of feature from most external points to centre point - North points","006002","Longitude (coarse accuracy)",,,"Operational"
5732.00,"16","Synoptic feature sequences","316061","(Definition of squall line (by centre and several points: North points and South points) and forecasted trajectory and evolution)","Amplitude of feature from most external points to centre point - South points","102000","Delayed replication of 2 descriptors",,,"Operational"
5733.00,"16","Synoptic feature sequences","316061","(Definition of squall line (by centre and several points: North points and South points) and forecasted trajectory and evolution)","Amplitude of feature from most external points to centre point - South points","031001","Delayed descriptor replication factor",,,"Operational"
5734.00,"16","Synoptic feature sequences","316061","(Definition of squall line (by centre and several points: North points and South points) and forecasted trajectory and evolution)","Amplitude of feature from most external points to centre point - South points","005002","Latitude (coarse accuracy)",,,"Operational"
5735.00,"16","Synoptic feature sequences","316061","(Definition of squall line (by centre and several points: North points and South points) and forecasted trajectory and evolution)","Amplitude of feature from most external points to centre point - South points","006002","Longitude (coarse accuracy)",,,"Operational"
5736.00,"16","Synoptic feature sequences","316061","(Definition of squall line (by centre and several points: North points and South points) and forecasted trajectory and evolution)","Amplitude of feature from most external points to centre point - Evolution","004074","Short time period or displacement","Period of validity",,"Operational"
5737.00,"16","Synoptic feature sequences","316061","(Definition of squall line (by centre and several points: North points and South points) and forecasted trajectory and evolution)","Amplitude of feature from most external points to centre point - Evolution","020048","Evolution of feature",,,"Operational"
5738.00,"16","Synoptic feature sequences","316061","(Definition of squall line (by centre and several points: North points and South points) and forecasted trajectory and evolution)","Amplitude of feature from most external points to centre point - Evolution","011041","Maximum wind gust speed","Maximum burst expected",,"Operational"
5739.00,"16","Synoptic feature sequences","316061","(Definition of squall line (by centre and several points: North points and South points) and forecasted trajectory and evolution)","Amplitude of feature from most external points to centre point - Evolution","013055","Intensity of precipitation","Intensity of rain expected",,"Operational"
5756.00,"16","Synoptic feature sequences","316071","(Graphical AIRMET Sierra)",,"301014","Time period","For which AIRMET is valid",,"Operational"
5757.00,"16","Synoptic feature sequences","316071","(Graphical AIRMET Sierra)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
5758.00,"16","Synoptic feature sequences","316071","(Graphical AIRMET Sierra)",,"031002","Extended delayed descriptor replication factor",,,"Operational"
5759.00,"16","Synoptic feature sequences","316071","(Graphical AIRMET Sierra)",,"316075","GFA IFR ceiling and visibility",,,"Operational"
5760.00,"16","Synoptic feature sequences","316071","(Graphical AIRMET Sierra)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
5761.00,"16","Synoptic feature sequences","316071","(Graphical AIRMET Sierra)",,"031002","Extended delayed descriptor replication factor",,,"Operational"
5762.00,"16","Synoptic feature sequences","316071","(Graphical AIRMET Sierra)",,"316076","GFA mountain obscuration",,,"Operational"
5764.00,"16","Synoptic feature sequences","316072","(Graphical AIRMET Tango)",,"301014","Time period","For which AIRMET is valid",,"Operational"
5765.00,"16","Synoptic feature sequences","316072","(Graphical AIRMET Tango)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
5766.00,"16","Synoptic feature sequences","316072","(Graphical AIRMET Tango)",,"031002","Extended delayed descriptor replication factor",,,"Operational"
5767.00,"16","Synoptic feature sequences","316072","(Graphical AIRMET Tango)",,"316077","GFA turbulence",,,"Operational"
5768.00,"16","Synoptic feature sequences","316072","(Graphical AIRMET Tango)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
5769.00,"16","Synoptic feature sequences","316072","(Graphical AIRMET Tango)",,"031002","Extended delayed descriptor replication factor",,,"Operational"
5770.00,"16","Synoptic feature sequences","316072","(Graphical AIRMET Tango)",,"316078","GFA strong surface wind",,,"Operational"
5771.00,"16","Synoptic feature sequences","316072","(Graphical AIRMET Tango)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
5772.00,"16","Synoptic feature sequences","316072","(Graphical AIRMET Tango)",,"031002","Extended delayed descriptor replication factor",,,"Operational"
5773.00,"16","Synoptic feature sequences","316072","(Graphical AIRMET Tango)",,"316079","GFA low-level wind shear",,,"Operational"
5775.00,"16","Synoptic feature sequences","316073","(Graphical AIRMET Zulu)",,"301014","Time period","For which AIRMET is valid",,"Operational"
5776.00,"16","Synoptic feature sequences","316073","(Graphical AIRMET Zulu)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
5777.00,"16","Synoptic feature sequences","316073","(Graphical AIRMET Zulu)",,"031002","Extended delayed descriptor replication factor",,,"Operational"
5778.00,"16","Synoptic feature sequences","316073","(Graphical AIRMET Zulu)",,"316080","GFA icing",,,"Operational"
5779.00,"16","Synoptic feature sequences","316073","(Graphical AIRMET Zulu)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
5780.00,"16","Synoptic feature sequences","316073","(Graphical AIRMET Zulu)",,"031002","Extended delayed descriptor replication factor",,,"Operational"
5781.00,"16","Synoptic feature sequences","316073","(Graphical AIRMET Zulu)",,"316081","GFA freezing level",,,"Operational"
5783.00,"16","Synoptic feature sequences","316074","(GFA identifier and observed/forecast location)",,"001039","Graphical Area Forecast (GFA) sequence identifier",,,"Operational"
5784.00,"16","Synoptic feature sequences","316074","(GFA identifier and observed/forecast location)",,"008021","Time significance","= 4 Forecast, = 16 Analysis",,"Operational"
5785.00,"16","Synoptic feature sequences","316074","(GFA identifier and observed/forecast location)",,"301014","Time period","For which hazard is being observed/forecast",,"Operational"
5786.00,"16","Synoptic feature sequences","316074","(GFA identifier and observed/forecast location)",,"301027","Description of a feature in 3-D or 2-D",,,"Operational"
5787.00,"16","Synoptic feature sequences","316074","(GFA identifier and observed/forecast location)",,"008021","Time significance","Set to missing (cancel)",,"Operational"
5788.00,"16","Synoptic feature sequences","316075","(GFA IFR ceiling and visibility)",,"008079","Product status","= 0 Normal, = 1 COR, = 2 AMD, = 3 COR AMD, = 4 CNL",,"Operational"
5789.00,"16","Synoptic feature sequences","316075","(GFA IFR ceiling and visibility)",,"008041","Data significance","= 8 IFR ceiling and visibility",,"Operational"
5790.00,"16","Synoptic feature sequences","316075","(GFA IFR ceiling and visibility)",,"316074","GFA identifier and observed/forecast location",,,"Operational"
5791.00,"16","Synoptic feature sequences","316075","(GFA IFR ceiling and visibility)",,"020006","Flight rules","= 1 IFR",,"Operational"
5792.00,"16","Synoptic feature sequences","316075","(GFA IFR ceiling and visibility)",,"033042","Type of limit represented by following value","= 2 Exclusive upper limit, = 7 Missing",,"Operational"
5793.00,"16","Synoptic feature sequences","316075","(GFA IFR ceiling and visibility)",,"020013","Height of base of cloud",,,"Operational"
5794.00,"16","Synoptic feature sequences","316075","(GFA IFR ceiling and visibility)",,"033042","Type of limit represented by following value","= 2 Exclusive upper limit, = 7 Missing",,"Operational"
5795.00,"16","Synoptic feature sequences","316075","(GFA IFR ceiling and visibility)",,"020001","Horizontal visibility",,,"Operational"
5796.00,"16","Synoptic feature sequences","316075","(GFA IFR ceiling and visibility)",,"020025","Obscuration",,,"Operational"
5797.00,"16","Synoptic feature sequences","316075","(GFA IFR ceiling and visibility)",,"020026","Character of obscuration","= 6 Blowing, = 15 Missing",,"Operational"
5798.00,"16","Synoptic feature sequences","316075","(GFA IFR ceiling and visibility)",,"008041","Data significance","Set to missing (cancel)",,"Operational"
5799.00,"16","Synoptic feature sequences","316075","(GFA IFR ceiling and visibility)",,"008079","Product status","Set to missing (cancel)",,"Operational"
5800.00,"16","Synoptic feature sequences","316076","(GFA mountain obscuration)",,"008079","Product status","= 0 Normal, = 1 COR, = 2 AMD, = 3 COR AMD, = 4 CNL",,"Operational"
5801.00,"16","Synoptic feature sequences","316076","(GFA mountain obscuration)",,"008041","Data significance","= 9 Mountain obscuration",,"Operational"
5802.00,"16","Synoptic feature sequences","316076","(GFA mountain obscuration)",,"316074","GFA identifier and observed/forecast location",,,"Operational"
5803.00,"16","Synoptic feature sequences","316076","(GFA mountain obscuration)",,"020006","Flight rules","= 1 IFR",,"Operational"
5804.00,"16","Synoptic feature sequences","316076","(GFA mountain obscuration)",,"020025","Obscuration",,,"Operational"
5805.00,"16","Synoptic feature sequences","316076","(GFA mountain obscuration)",,"020026","Character of obscuration","= 6 Blowing, = 15 Missing",,"Operational"
5806.00,"16","Synoptic feature sequences","316076","(GFA mountain obscuration)",,"008041","Data significance","Set to missing (cancel)",,"Operational"
5807.00,"16","Synoptic feature sequences","316076","(GFA mountain obscuration)",,"008079","Product status","Set to missing (cancel)",,"Operational"
5808.00,"16","Synoptic feature sequences","316077","(GFA turbulence)",,"008079","Product status","= 0 Normal, = 1 COR, = 2 AMD, = 3 COR AMD, = 4 CNL",,"Operational"
5809.00,"16","Synoptic feature sequences","316077","(GFA turbulence)",,"008011","Meteorological feature","= 13 Turbulence",,"Operational"
5810.00,"16","Synoptic feature sequences","316077","(GFA turbulence)",,"316074","GFA identifier and observed/forecast location",,,"Operational"
5811.00,"16","Synoptic feature sequences","316077","(GFA turbulence)",,"011031","Degree of turbulence","= 6 Moderate",,"Operational"
5812.00,"16","Synoptic feature sequences","316077","(GFA turbulence)",,"008011","Meteorological feature","Set to missing (cancel)",,"Operational"
5813.00,"16","Synoptic feature sequences","316077","(GFA turbulence)",,"008079","Product status","Set to missing (cancel)",,"Operational"
5814.00,"16","Synoptic feature sequences","316078","(GFA strong surface wind)",,"008079","Product status","= 0 Normal, = 1 COR, = 2 AMD, = 3 COR AMD, = 4 CNL",,"Operational"
5815.00,"16","Synoptic feature sequences","316078","(GFA strong surface wind)",,"008041","Data significance","= 10 Strong surface wind",,"Operational"
5816.00,"16","Synoptic feature sequences","316078","(GFA strong surface wind)",,"316074","GFA identifier and observed/forecast location",,,"Operational"
5817.00,"16","Synoptic feature sequences","316078","(GFA strong surface wind)",,"033042","Type of limit represented by following value","= 0 Exclusive lower limit",,"Operational"
5818.00,"16","Synoptic feature sequences","316078","(GFA strong surface wind)",,"011012","Wind speed at 10 m",,,"Operational"
5819.00,"16","Synoptic feature sequences","316078","(GFA strong surface wind)",,"008041","Data significance","Set to missing (cancel)",,"Operational"
5820.00,"16","Synoptic feature sequences","316078","(GFA strong surface wind)",,"008079","Product status","Set to missing (cancel)",,"Operational"
5821.00,"16","Synoptic feature sequences","316079","(GFA low-level wind shear)",,"008079","Product status","= 0 Normal, = 1 COR, = 2 AMD, = 3 COR AMD, = 4 CNL",,"Operational"
5822.00,"16","Synoptic feature sequences","316079","(GFA low-level wind shear)",,"008011","Meteorological feature","= 16 Phenomenon",,"Operational"
5823.00,"16","Synoptic feature sequences","316079","(GFA low-level wind shear)",,"316074","GFA identifier and observed/forecast location",,,"Operational"
5824.00,"16","Synoptic feature sequences","316079","(GFA low-level wind shear)",,"020023","Other weather phenomena","Bit 12 = Wind shear",,"Operational"
5825.00,"16","Synoptic feature sequences","316079","(GFA low-level wind shear)",,"020024","Intensity of phenomena",,,"Operational"
5826.00,"16","Synoptic feature sequences","316079","(GFA low-level wind shear)",,"008011","Meteorological feature","Set to missing (cancel)",,"Operational"
5827.00,"16","Synoptic feature sequences","316079","(GFA low-level wind shear)",,"008079","Product status","Set to missing (cancel)",,"Operational"
5828.00,"16","Synoptic feature sequences","316080","(GFA icing)",,"008079","Product status","= 0 Normal, = 1 COR, = 2 AMD, = 3 COR AMD, = 4 CNL",,"Operational"
5829.00,"16","Synoptic feature sequences","316080","(GFA icing)",,"008011","Meteorological feature","= 15 Airframe icing",,"Operational"
5830.00,"16","Synoptic feature sequences","316080","(GFA icing)",,"316074","GFA identifier and observed/forecast location",,,"Operational"
5831.00,"16","Synoptic feature sequences","316080","(GFA icing)",,"020041","Airframe icing","= 4 Moderate icing",,"Operational"
5832.00,"16","Synoptic feature sequences","316080","(GFA icing)",,"008011","Meteorological feature","Set to missing (cancel)",,"Operational"
5833.00,"16","Synoptic feature sequences","316080","(GFA icing)",,"008079","Product status","Set to missing (cancel)",,"Operational"
5834.00,"16","Synoptic feature sequences","316081","(GFA freezing level)",,"008079","Product status","= 0 Normal, = 1 COR, = 2 AMD, = 3 COR AMD, = 4 CNL",,"Operational"
5835.00,"16","Synoptic feature sequences","316081","(GFA freezing level)",,"008041","Data significance","= 11 Freezing level, = 12 Multiple freezing level",,"Operational"
5836.00,"16","Synoptic feature sequences","316081","(GFA freezing level)",,"316074","GFA identifier and observed/forecast location",,,"Operational"
5837.00,"16","Synoptic feature sequences","316081","(GFA freezing level)",,"008041","Data significance","Set to missing (cancel)",,"Operational"
5838.00,"16","Synoptic feature sequences","316081","(GFA freezing level)",,"008079","Product status","Set to missing (cancel)",,"Operational"
5839.00,"18","Radiological report sequences","318001",,,"301025","Latitude/longitude (coarse accuracy), day/time",,,"Operational"
5840.00,"18","Radiological report sequences","318001",,,"024011","Dose",,,"Operational"
5841.00,"18","Radiological report sequences","318003",,,"301026","Latitude/longitude (high accuracy), time period (day, hour, minute)",,,"Operational"
5842.00,"18","Radiological report sequences","318003",,,"024005","Isotope mass",,,"Operational"
5843.00,"18","Radiological report sequences","318003",,,"024004","Element name",,,"Operational"
5844.00,"18","Radiological report sequences","318003",,,"024021","Air concentration (of named isotope type including gross beta)",,,"Operational"
5845.00,"18","Radiological report sequences","318004",,,"301025","Latitude/longitude (coarse accuracy), day/time",,,"Operational"
5846.00,"18","Radiological report sequences","318004",,,"004023","Time period or displacement",,,"Operational"
5847.00,"18","Radiological report sequences","318004",,,"013011","Total precipitation/total water equivalent",,,"Operational"
5848.00,"18","Radiological report sequences","318004",,,"024005","Isotope mass",,,"Operational"
5849.00,"18","Radiological report sequences","318004",,,"024004","Element name",,,"Operational"
5850.00,"18","Radiological report sequences","318004",,,"024022","Concentration in precipitation (of named isotope type)",,,"Operational"
5851.00,"21","Radar report sequences","321001","(Wind profiler - antenna characteristics)",,"002101","Type of antenna",,,"Operational"
5852.00,"21","Radar report sequences","321001","(Wind profiler - antenna characteristics)",,"002114","Antenna effective surface area",,,"Operational"
5853.00,"21","Radar report sequences","321001","(Wind profiler - antenna characteristics)",,"002105","Maximum antenna gain",,,"Operational"
5854.00,"21","Radar report sequences","321001","(Wind profiler - antenna characteristics)",,"002106","3-dB beamwidth",,,"Operational"
5855.00,"21","Radar report sequences","321001","(Wind profiler - antenna characteristics)",,"002107","Sidelobe suppression",,,"Operational"
5856.00,"21","Radar report sequences","321001","(Wind profiler - antenna characteristics)",,"002121","Mean frequency",,,"Operational"
5857.00,"21","Radar report sequences","321003","(Wind profiler - moment data)",,"021051","Signal power above 1 mW",,,"Operational"
5858.00,"21","Radar report sequences","321003","(Wind profiler - moment data)",,"021014","Doppler mean velocity (radial)",,,"Operational"
5859.00,"21","Radar report sequences","321003","(Wind profiler - moment data)",,"021017","Doppler velocity spectral width",,,"Operational"
5860.00,"21","Radar report sequences","321003","(Wind profiler - moment data)",,"021030","Signal to noise ratio",,,"Operational"
5861.00,"21","Radar report sequences","321004","(Wind profiler - moment data sounding)",,"301031","Identification and type of station, date/time, location (high accuracy), height of station",,,"Operational"
5862.00,"21","Radar report sequences","321004","(Wind profiler - moment data sounding)",,"002003","Type of measuring equipment used",,,"Operational"
5863.00,"21","Radar report sequences","321004","(Wind profiler - moment data sounding)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
5864.00,"21","Radar report sequences","321004","(Wind profiler - moment data sounding)",,"031001","Delayed descriptor replication factor",,,"Operational"
5865.00,"21","Radar report sequences","321004","(Wind profiler - moment data sounding)",,"321003","Wind profiler - moment data",,,"Operational"
5866.00,"21","Radar report sequences","321005","(Transmitter-receiver characteristics)",,"025004","Echo processing",,,"Operational"
5867.00,"21","Radar report sequences","321005","(Transmitter-receiver characteristics)",,"002121","Mean frequency",,,"Operational"
5868.00,"21","Radar report sequences","321005","(Transmitter-receiver characteristics)",,"002122","Frequency agility range",,,"Operational"
5869.00,"21","Radar report sequences","321005","(Transmitter-receiver characteristics)",,"002123","Peak power",,,"Operational"
5870.00,"21","Radar report sequences","321005","(Transmitter-receiver characteristics)",,"002124","Average power",,,"Operational"
5871.00,"21","Radar report sequences","321005","(Transmitter-receiver characteristics)",,"002125","Pulse repetition frequency",,,"Operational"
5872.00,"21","Radar report sequences","321005","(Transmitter-receiver characteristics)",,"002126","Pulse width",,,"Operational"
5873.00,"21","Radar report sequences","321005","(Transmitter-receiver characteristics)",,"002127","Receiver intermediate frequency",,,"Operational"
5874.00,"21","Radar report sequences","321005","(Transmitter-receiver characteristics)",,"002128","Intermediate frequency bandwidth",,,"Operational"
5875.00,"21","Radar report sequences","321005","(Transmitter-receiver characteristics)",,"002129","Minimum detectable signal",,,"Operational"
5876.00,"21","Radar report sequences","321005","(Transmitter-receiver characteristics)",,"002130","Dynamic range",,,"Operational"
5877.00,"21","Radar report sequences","321005","(Transmitter-receiver characteristics)",,"002131","Sensitivity time control (STC)",,,"Operational"
5878.00,"21","Radar report sequences","321006","(Integration characteristics)",,"025001","Range-gate length",,,"Operational"
5879.00,"21","Radar report sequences","321006","(Integration characteristics)",,"025002","Number of gates averaged",,,"Operational"
5880.00,"21","Radar report sequences","321006","(Integration characteristics)",,"025003","Number of integrated pulses",,,"Operational"
5881.00,"21","Radar report sequences","321006","(Integration characteristics)",,"025005","Echo integration",,,"Operational"
5882.00,"21","Radar report sequences","321007","(Corrections)",,"025009","Calibration method",,,"Operational"
5883.00,"21","Radar report sequences","321007","(Corrections)",,"025010","Clutter treatment",,,"Operational"
5884.00,"21","Radar report sequences","321007","(Corrections)",,"025011","Ground occultation correction (screening)",,,"Operational"
5885.00,"21","Radar report sequences","321007","(Corrections)",,"025012","Range attenuation correction",,,"Operational"
5886.00,"21","Radar report sequences","321007","(Corrections)",,"025013","Bright-band correction",,,"Operational"
5887.00,"21","Radar report sequences","321007","(Corrections)",,"025015","Radome attenuation correction",,,"Operational"
5888.00,"21","Radar report sequences","321007","(Corrections)",,"025016","Clear-air attenuation correction",,,"Operational"
5889.00,"21","Radar report sequences","321007","(Corrections)",,"025017","Precipitation attenuation correction",,,"Operational"
5890.00,"21","Radar report sequences","321008","(Z to R conversion)",,"025006","Z to R conversion",,,"Operational"
5891.00,"21","Radar report sequences","321008","(Z to R conversion)",,"025007","Z to R conversion factor",,,"Operational"
5892.00,"21","Radar report sequences","321008","(Z to R conversion)",,"025008","Z to R conversion exponent",,,"Operational"
5893.00,"21","Radar report sequences","321009","(A to Z law)",,"025018","A to Z law for attenuation factor",,,"Operational"
5894.00,"21","Radar report sequences","321009","(A to Z law)",,"025019","A to Z law for attenuation exponent",,,"Operational"
5895.00,"21","Radar report sequences","321010","(Antenna characteristics)",,"002101","Type of antenna",,,"Operational"
5896.00,"21","Radar report sequences","321010","(Antenna characteristics)",,"007002","Height or altitude","Altitude of the tower base",,"Operational"
5897.00,"21","Radar report sequences","321010","(Antenna characteristics)",,"002102","Antenna height above tower base",,,"Operational"
5898.00,"21","Radar report sequences","321010","(Antenna characteristics)",,"002103","Radome",,,"Operational"
5899.00,"21","Radar report sequences","321010","(Antenna characteristics)",,"002104","Antenna polarization",,,"Operational"
5900.00,"21","Radar report sequences","321010","(Antenna characteristics)",,"002105","Maximum antenna gain",,,"Operational"
5901.00,"21","Radar report sequences","321010","(Antenna characteristics)",,"002106","3-dB beamwidth",,,"Operational"
5902.00,"21","Radar report sequences","321010","(Antenna characteristics)",,"002107","Sidelobe suppression",,,"Operational"
5903.00,"21","Radar report sequences","321010","(Antenna characteristics)",,"002108","Crosspol discrimination (on axis)",,,"Operational"
5904.00,"21","Radar report sequences","321010","(Antenna characteristics)",,"002109","Antenna speed (azimuth)",,,"Operational"
5905.00,"21","Radar report sequences","321010","(Antenna characteristics)",,"002110","Antenna speed (elevation)",,,"Operational"
5906.00,"21","Radar report sequences","321010","(Antenna characteristics)",,"002132","Azimuth pointing accuracy",,,"Operational"
5907.00,"21","Radar report sequences","321010","(Antenna characteristics)",,"002133","Elevation pointing accuracy",,,"Operational"
5908.00,"21","Radar report sequences","321011","(General characteristics)",,"030031","Picture type",,,"Operational"
5909.00,"21","Radar report sequences","321011","(General characteristics)",,"030032","Combination with other data",,,"Operational"
5910.00,"21","Radar report sequences","321011","(General characteristics)",,"029002","Coordinate grid type",,,"Operational"
5911.00,"21","Radar report sequences","321012","(Antenna elevations)",,"101000","Delayed replication of 1 descriptor",,,"Operational"
5912.00,"21","Radar report sequences","321012","(Antenna elevations)",,"031001","Delayed descriptor replication factor",,,"Operational"
5913.00,"21","Radar report sequences","321012","(Antenna elevations)",,"002135","Antenna elevation",,,"Operational"
5914.00,"21","Radar report sequences","321021","(Basic information (system/site header) on wind profiler/RASS)",,"002003","Type of measuring equipment used",,,"Operational"
5915.00,"21","Radar report sequences","321021","(Basic information (system/site header) on wind profiler/RASS)",,"002101","Type of antenna",,,"Operational"
5916.00,"21","Radar report sequences","321021","(Basic information (system/site header) on wind profiler/RASS)",,"201130","Change data width","8 bits long",,"Operational"
5917.00,"21","Radar report sequences","321021","(Basic information (system/site header) on wind profiler/RASS)",,"002106","3-dB beamwidth",,,"Operational"
5918.00,"21","Radar report sequences","321021","(Basic information (system/site header) on wind profiler/RASS)",,"201000","Change data width","Cancel",,"Operational"
5919.00,"21","Radar report sequences","321021","(Basic information (system/site header) on wind profiler/RASS)",,"201132","Change data width","11 bits long",,"Operational"
5920.00,"21","Radar report sequences","321021","(Basic information (system/site header) on wind profiler/RASS)",,"202130","Change scale","Scale: -6",,"Operational"
5921.00,"21","Radar report sequences","321021","(Basic information (system/site header) on wind profiler/RASS)",,"002121","Mean frequency",,,"Operational"
5922.00,"21","Radar report sequences","321021","(Basic information (system/site header) on wind profiler/RASS)",,"202000","Change scale","Cancel",,"Operational"
5923.00,"21","Radar report sequences","321021","(Basic information (system/site header) on wind profiler/RASS)",,"201000","Change data width","Cancel",,"Operational"
5924.00,"21","Radar report sequences","321021","(Basic information (system/site header) on wind profiler/RASS)",,"201133","Change data width","11 bits long",,"Operational"
5925.00,"21","Radar report sequences","321021","(Basic information (system/site header) on wind profiler/RASS)",,"202129","Change scale","Scale: 0",,"Operational"
5926.00,"21","Radar report sequences","321021","(Basic information (system/site header) on wind profiler/RASS)",,"025001","Range-gate length",,,"Operational"
5927.00,"21","Radar report sequences","321021","(Basic information (system/site header) on wind profiler/RASS)",,"202000","Change scale","Cancel",,"Operational"
5928.00,"21","Radar report sequences","321021","(Basic information (system/site header) on wind profiler/RASS)",,"201000","Change data width","Cancel",,"Operational"
5929.00,"21","Radar report sequences","321022","(Wind profiler: processed-data winds)",,"007007","Height",,,"Operational"
5930.00,"21","Radar report sequences","321022","(Wind profiler: processed-data winds)",,"204001","Add associated field","1 bit long",,"Operational"
5931.00,"21","Radar report sequences","321022","(Wind profiler: processed-data winds)",,"031021","Associated field significance",,,"Operational"
5932.00,"21","Radar report sequences","321022","(Wind profiler: processed-data winds)",,"011001","Wind direction",,,"Operational"
5933.00,"21","Radar report sequences","321022","(Wind profiler: processed-data winds)",,"204000","Add associated field","Cancel",,"Operational"
5934.00,"21","Radar report sequences","321022","(Wind profiler: processed-data winds)",,"011002","Wind speed",,,"Operational"
5935.00,"21","Radar report sequences","321022","(Wind profiler: processed-data winds)",,"204001","Add associated field","1 bit long",,"Operational"
5936.00,"21","Radar report sequences","321022","(Wind profiler: processed-data winds)",,"031021","Associated field significance",,,"Operational"
5937.00,"21","Radar report sequences","321022","(Wind profiler: processed-data winds)",,"011006","w-component",,,"Operational"
5938.00,"21","Radar report sequences","321022","(Wind profiler: processed-data winds)",,"204000","Add associated field","Cancel",,"Operational"
5939.00,"21","Radar report sequences","321022","(Wind profiler: processed-data winds)",,"021030","Signal to noise ratio",,,"Operational"
5940.00,"21","Radar report sequences","321023","(Wind profiler: raw-data winds)",,"007007","Height",,,"Operational"
5941.00,"21","Radar report sequences","321023","(Wind profiler: raw-data winds)",,"021091","Radar signal Doppler spectrum 0th moment",,,"Operational"
5942.00,"21","Radar report sequences","321023","(Wind profiler: raw-data winds)",,"021030","Signal to noise ratio",,,"Operational"
5943.00,"21","Radar report sequences","321023","(Wind profiler: raw-data winds)",,"202129","Change scale","Scale: 2",,"Operational"
5944.00,"21","Radar report sequences","321023","(Wind profiler: raw-data winds)",,"021014","Doppler mean velocity (radial)",,,"Operational"
5945.00,"21","Radar report sequences","321023","(Wind profiler: raw-data winds)",,"201129","Change data width","9 bits long",,"Operational"
5946.00,"21","Radar report sequences","321023","(Wind profiler: raw-data winds)",,"021017","Doppler velocity spectral width",,,"Operational"
5947.00,"21","Radar report sequences","321023","(Wind profiler: raw-data winds)",,"202000","Change scale","Cancel",,"Operational"
5948.00,"21","Radar report sequences","321023","(Wind profiler: raw-data winds)",,"201000","Change data width","Cancel",,"Operational"
5949.00,"21","Radar report sequences","321024","(RASS-mode: processed-data RASS)",,"007007","Height",,,"Operational"
5950.00,"21","Radar report sequences","321024","(RASS-mode: processed-data RASS)",,"204001","Add associated field","1 bit long",,"Operational"
5951.00,"21","Radar report sequences","321024","(RASS-mode: processed-data RASS)",,"031021","Associated field significance",,,"Operational"
5952.00,"21","Radar report sequences","321024","(RASS-mode: processed-data RASS)",,"012007","Virtual temperature",,,"Operational"
5953.00,"21","Radar report sequences","321024","(RASS-mode: processed-data RASS)",,"011006","w-component",,,"Operational"
5954.00,"21","Radar report sequences","321024","(RASS-mode: processed-data RASS)",,"204000","Add associated field","Cancel",,"Operational"
5955.00,"21","Radar report sequences","321024","(RASS-mode: processed-data RASS)",,"021030","Signal to noise ratio",,,"Operational"
5956.00,"21","Radar report sequences","321025","(RASS-mode: raw-data RASS)",,"007007","Height",,,"Operational"
5957.00,"21","Radar report sequences","321025","(RASS-mode: raw-data RASS)",,"021091","Radar signal Doppler spectrum 0th moment",,,"Operational"
5958.00,"21","Radar report sequences","321025","(RASS-mode: raw-data RASS)",,"021030","Signal to noise ratio",,,"Operational"
5959.00,"21","Radar report sequences","321025","(RASS-mode: raw-data RASS)",,"202129","Change scale","Scale: 2",,"Operational"
5960.00,"21","Radar report sequences","321025","(RASS-mode: raw-data RASS)",,"021014","Doppler mean velocity (radial)",,,"Operational"
5961.00,"21","Radar report sequences","321025","(RASS-mode: raw-data RASS)",,"201129","Change data width","9 bits long",,"Operational"
5962.00,"21","Radar report sequences","321025","(RASS-mode: raw-data RASS)",,"021017","Doppler velocity spectral width",,,"Operational"
5963.00,"21","Radar report sequences","321025","(RASS-mode: raw-data RASS)",,"202000","Change scale","Cancel",,"Operational"
5964.00,"21","Radar report sequences","321025","(RASS-mode: raw-data RASS)",,"201000","Change data width","Cancel",,"Operational"
5965.00,"21","Radar report sequences","321025","(RASS-mode: raw-data RASS)",,"021092","RASS signal Doppler spectrum 0th moment, referring to RASS signal",,,"Operational"
5966.00,"21","Radar report sequences","321025","(RASS-mode: raw-data RASS)",,"021030","Signal to noise ratio","Referring to RASS signal",,"Operational"
5967.00,"21","Radar report sequences","321025","(RASS-mode: raw-data RASS)",,"025092","Acoustic propagation velocity",,,"Operational"
5968.00,"21","Radar report sequences","321025","(RASS-mode: raw-data RASS)",,"201129","Change data width","9 bits long",,"Operational"
5969.00,"21","Radar report sequences","321025","(RASS-mode: raw-data RASS)",,"202129","Change scale","Scale: 2",,"Operational"
5970.00,"21","Radar report sequences","321025","(RASS-mode: raw-data RASS)",,"021017","Doppler velocity spectral width","Referring to RASS signal",,"Operational"
5971.00,"21","Radar report sequences","321025","(RASS-mode: raw-data RASS)",,"202000","Change scale","Cancel",,"Operational"
5972.00,"21","Radar report sequences","321025","(RASS-mode: raw-data RASS)",,"201000","Change data width","Cancel",,"Operational"
5973.00,"21","Radar report sequences","321026","(RASS data - fluxes)",,"007007","Height",,,"Operational"
5974.00,"21","Radar report sequences","321026","(RASS data - fluxes)",,"204001","Add associated field","1 bit long",,"Operational"
5975.00,"21","Radar report sequences","321026","(RASS data - fluxes)",,"031021","Associated field significance",,,"Operational"
5976.00,"21","Radar report sequences","321026","(RASS data - fluxes)",,"012007","Virtual temperature",,,"Operational"
5977.00,"21","Radar report sequences","321026","(RASS data - fluxes)",,"025091","Structure constant of the refraction index (Cn2)",,,"Operational"
5978.00,"21","Radar report sequences","321026","(RASS data - fluxes)",,"011071","Turbulent vertical momentum flux",,,"Operational"
5979.00,"21","Radar report sequences","321026","(RASS data - fluxes)",,"011072","Turbulent vertical buoyancy flux",,,"Operational"
5980.00,"21","Radar report sequences","321026","(RASS data - fluxes)",,"011073","Turbulent kinetic energy",,,"Operational"
5981.00,"21","Radar report sequences","321026","(RASS data - fluxes)",,"011074","Dissipation energy",,,"Operational"
5982.00,"21","Radar report sequences","321026","(RASS data - fluxes)",,"204000","Add associated field","Cancel",,"Operational"
5983.00,"21","Radar report sequences","321027","(Radar specification, normalized radar cross-section, Kp variance coefficient)",,"021118","Attenuation correction on sigma-0",,,"Operational"
5984.00,"21","Radar report sequences","321027","(Radar specification, normalized radar cross-section, Kp variance coefficient)",,"202129","Change scale",,,"Operational"
5985.00,"21","Radar report sequences","321027","(Radar specification, normalized radar cross-section, Kp variance coefficient)",,"201132","Change data width",,,"Operational"
5986.00,"21","Radar report sequences","321027","(Radar specification, normalized radar cross-section, Kp variance coefficient)",,"002112","Radar look angle",,,"Operational"
5987.00,"21","Radar report sequences","321027","(Radar specification, normalized radar cross-section, Kp variance coefficient)",,"201000","Change data width","Cancel",,"Operational"
5988.00,"21","Radar report sequences","321027","(Radar specification, normalized radar cross-section, Kp variance coefficient)",,"201131","Change data width",,,"Operational"
5989.00,"21","Radar report sequences","321027","(Radar specification, normalized radar cross-section, Kp variance coefficient)",,"002111","Radar incidence angle",,,"Operational"
5990.00,"21","Radar report sequences","321027","(Radar specification, normalized radar cross-section, Kp variance coefficient)",,"201000","Change data width","Cancel",,"Operational"
5991.00,"21","Radar report sequences","321027","(Radar specification, normalized radar cross-section, Kp variance coefficient)",,"202000","Change scale","Cancel",,"Operational"
5992.00,"21","Radar report sequences","321027","(Radar specification, normalized radar cross-section, Kp variance coefficient)",,"002104","Antenna polarization",,,"Operational"
5993.00,"21","Radar report sequences","321027","(Radar specification, normalized radar cross-section, Kp variance coefficient)",,"021105","Normalized radar cross-section",,,"Operational"
5994.00,"21","Radar report sequences","321027","(Radar specification, normalized radar cross-section, Kp variance coefficient)",,"021106","Kp variance coefficient (alpha)",,,"Operational"
5995.00,"21","Radar report sequences","321027","(Radar specification, normalized radar cross-section, Kp variance coefficient)",,"021107","Kp variance coefficient (beta)",,,"Operational"
5996.00,"21","Radar report sequences","321027","(Radar specification, normalized radar cross-section, Kp variance coefficient)",,"021114","Kp variance coefficient (gamma)",,,"Operational"
5997.00,"21","Radar report sequences","321027","(Radar specification, normalized radar cross-section, Kp variance coefficient)",,"021115","SEAWINDS sigma-0 quality",,,"Operational"
5998.00,"21","Radar report sequences","321027","(Radar specification, normalized radar cross-section, Kp variance coefficient)",,"021116","SEAWINDS sigma-0 mode",,,"Operational"
5999.00,"21","Radar report sequences","321027","(Radar specification, normalized radar cross-section, Kp variance coefficient)",,"008018","SEAWINDS land/ice surface type",,,"Operational"
6000.00,"21","Radar report sequences","321027","(Radar specification, normalized radar cross-section, Kp variance coefficient)",,"021117","Sigma-0 variance quality control",,,"Operational"
6001.00,"21","Radar report sequences","321028","(Radar specification, SEAWINDS normalized radar cross-section, Kp variance coefficient)",,"021118","Attenuation correction on sigma-0",,,"Operational"
6002.00,"21","Radar report sequences","321028","(Radar specification, SEAWINDS normalized radar cross-section, Kp variance coefficient)",,"202129","Change scale",,,"Operational"
6003.00,"21","Radar report sequences","321028","(Radar specification, SEAWINDS normalized radar cross-section, Kp variance coefficient)",,"201132","Change data width",,,"Operational"
6004.00,"21","Radar report sequences","321028","(Radar specification, SEAWINDS normalized radar cross-section, Kp variance coefficient)",,"002112","Radar look angle",,,"Operational"
6005.00,"21","Radar report sequences","321028","(Radar specification, SEAWINDS normalized radar cross-section, Kp variance coefficient)",,"201000","Change data width","Cancel",,"Operational"
6006.00,"21","Radar report sequences","321028","(Radar specification, SEAWINDS normalized radar cross-section, Kp variance coefficient)",,"201131","Change data width",,,"Operational"
6007.00,"21","Radar report sequences","321028","(Radar specification, SEAWINDS normalized radar cross-section, Kp variance coefficient)",,"002111","Radar incidence angle",,,"Operational"
6008.00,"21","Radar report sequences","321028","(Radar specification, SEAWINDS normalized radar cross-section, Kp variance coefficient)",,"201000","Change data width","Cancel",,"Operational"
6009.00,"21","Radar report sequences","321028","(Radar specification, SEAWINDS normalized radar cross-section, Kp variance coefficient)",,"202000","Change scale","Cancel",,"Operational"
6010.00,"21","Radar report sequences","321028","(Radar specification, SEAWINDS normalized radar cross-section, Kp variance coefficient)",,"002104","Antenna polarization",,,"Operational"
6011.00,"21","Radar report sequences","321028","(Radar specification, SEAWINDS normalized radar cross-section, Kp variance coefficient)",,"021123","SEAWINDS normalized radar cross-section",,,"Operational"
6012.00,"21","Radar report sequences","321028","(Radar specification, SEAWINDS normalized radar cross-section, Kp variance coefficient)",,"021106","Kp variance coefficient (alpha)",,,"Operational"
6013.00,"21","Radar report sequences","321028","(Radar specification, SEAWINDS normalized radar cross-section, Kp variance coefficient)",,"021107","Kp variance coefficient (beta)",,,"Operational"
6014.00,"21","Radar report sequences","321028","(Radar specification, SEAWINDS normalized radar cross-section, Kp variance coefficient)",,"021114","Kp variance coefficient (gamma)",,,"Operational"
6015.00,"21","Radar report sequences","321028","(Radar specification, SEAWINDS normalized radar cross-section, Kp variance coefficient)",,"021115","SEAWINDS sigma-0 quality",,,"Operational"
6016.00,"21","Radar report sequences","321028","(Radar specification, SEAWINDS normalized radar cross-section, Kp variance coefficient)",,"021116","SEAWINDS sigma-0 mode",,,"Operational"
6017.00,"21","Radar report sequences","321028","(Radar specification, SEAWINDS normalized radar cross-section, Kp variance coefficient)",,"008018","SEAWINDS land/ice surface type",,,"Operational"
6018.00,"21","Radar report sequences","321028","(Radar specification, SEAWINDS normalized radar cross-section, Kp variance coefficient)",,"021117","Sigma-0 variance quality control",,,"Operational"
6019.00,"21","Radar report sequences","321030","(ASCAT sigma-0 information)",,"008085","Beam identifier",,,"Operational"
6020.00,"21","Radar report sequences","321030","(ASCAT sigma-0 information)",,"202129","Change scale","Increase scale by 101",,"Operational"
6021.00,"21","Radar report sequences","321030","(ASCAT sigma-0 information)",,"201131","Change data width","Increase width by 3 bits",,"Operational"
6022.00,"21","Radar report sequences","321030","(ASCAT sigma-0 information)",,"002111","Radar incidence angle",,,"Operational"
6023.00,"21","Radar report sequences","321030","(ASCAT sigma-0 information)",,"201000","Change data width","Cancel",,"Operational"
6024.00,"21","Radar report sequences","321030","(ASCAT sigma-0 information)",,"202000","Change scale","Cancel",,"Operational"
6025.00,"21","Radar report sequences","321030","(ASCAT sigma-0 information)",,"002134","Antenna beam azimuth",,,"Operational"
6026.00,"21","Radar report sequences","321030","(ASCAT sigma-0 information)",,"021062","Backscatter",,,"Operational"
6027.00,"21","Radar report sequences","321030","(ASCAT sigma-0 information)",,"021063","Radiometric resolution (noise value)",,,"Operational"
6028.00,"21","Radar report sequences","321030","(ASCAT sigma-0 information)",,"021158","ASCAT Kp estimate quality",,,"Operational"
6029.00,"21","Radar report sequences","321030","(ASCAT sigma-0 information)",,"021159","ASCAT sigma-0 usability",,,"Operational"
6030.00,"21","Radar report sequences","321030","(ASCAT sigma-0 information)",,"021160","ASCAT use of synthetic data",,,"Operational"
6031.00,"21","Radar report sequences","321030","(ASCAT sigma-0 information)",,"021161","ASCAT synthetic data quantity",,,"Operational"
6032.00,"21","Radar report sequences","321030","(ASCAT sigma-0 information)",,"021162","ASCAT satellite orbit and attitude quality",,,"Operational"
6033.00,"21","Radar report sequences","321030","(ASCAT sigma-0 information)",,"021163","ASCAT solar array reflection contamination",,,"Operational"
6034.00,"21","Radar report sequences","321030","(ASCAT sigma-0 information)",,"021164","ASCAT telemetry presence and quality",,,"Operational"
6035.00,"21","Radar report sequences","321030","(ASCAT sigma-0 information)",,"021165","ASCAT extrapolated reference function presence",,,"Operational"
6036.00,"21","Radar report sequences","321030","(ASCAT sigma-0 information)",,"021166","Land fraction",,,"Operational"
6037.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"001007","Satellite identifier",,,"Operational"
6038.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"002019","Satellite instruments",,,"Operational"
6039.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"004001","Year",,,"Operational"
6040.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"004002","Month",,,"Operational"
6041.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"004003","Day",,,"Operational"
6042.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"004004","Hour",,,"Operational"
6043.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"004005","Minute",,,"Operational"
6044.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"004006","Second",,,"Operational"
6045.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"005001","Latitude (high accuracy)",,,"Operational"
6046.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"006001","Longitude (high accuracy)",,,"Operational"
6047.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"027001","Latitude (high accuracy)",,,"Operational"
6048.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"028001","Longitude (high accuracy)",,,"Operational"
6049.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"027001","Latitude (high accuracy)",,,"Operational"
6050.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"028001","Longitude (high accuracy)",,,"Operational"
6051.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"027001","Latitude (high accuracy)",,,"Operational"
6052.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"028001","Longitude (high accuracy)",,,"Operational"
6053.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"027001","Latitude (high accuracy)",,,"Operational"
6054.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"028001","Longitude (high accuracy)",,,"Operational"
6055.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"010001","Height of land surface",,,"Operational"
6056.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"014019","Surface albedo",,,"Operational"
6057.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"007025","Solar zenith angle",,,"Operational"
6058.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"010080","Viewing zenith angle",,,"Operational"
6059.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"005023","Sun to satellite azimuth difference",,,"Operational"
6060.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"020010","Cloud cover (total)",,,"Operational"
6061.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"008003","Vertical significance (satellite observations)",,,"Operational"
6062.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"007004","Pressure",,,"Operational"
6063.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"014026","Albedo at the top of clouds",,,"Operational"
6064.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"020014","Height of top of cloud",,,"Operational"
6065.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"013093","Cloud optical thickness",,,"Operational"
6066.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"105000","Delayed replication of 5 descriptors",,,"Operational"
6067.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"031001","Delayed descriptor replication factor",,,"Operational"
6068.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"007004","Pressure",,,"Operational"
6069.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"007004","Pressure",,,"Operational"
6070.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"008043","Atmospheric chemical or physical constituent type",,,"Operational"
6071.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"008044","CAS registry number",,,"Operational"
6072.00,"22","Chemical and aerosol sequences","322028","(METOP GOME-2)",,"015021","Integrated mass density",,,"Operational"
6121.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"001007","Satellite identifier",,,"Operational"
6122.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"001031","Identification of originating/generating centre",,,"Operational"
6123.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"002019","Satellite instruments",,,"Operational"
6124.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"002020","Satellite classification",,,"Operational"
6125.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"004001","Year",,,"Operational"
6126.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"004002","Month",,,"Operational"
6127.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"004003","Day",,,"Operational"
6128.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"004004","Hour",,,"Operational"
6129.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"004005","Minute",,,"Operational"
6130.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"202131","Change scale","Add 3 to scale",,"Operational"
6131.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"201138","Change data width","Add 10 to width",,"Operational"
6132.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"004006","Second",,,"Operational"
6133.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"201000","Change data width","Cancel",,"Operational"
6134.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"202000","Change scale","Cancel",,"Operational"
6135.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"005001","Latitude (high accuracy)",,,"Operational"
6136.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"006001","Longitude (high accuracy)",,,"Operational"
6137.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"007024","Satellite zenith angle",,,"Operational"
6138.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"005021","Bearing or azimuth",,,"Operational"
6139.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"007025","Solar zenith angle",,,"Operational"
6140.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"005022","Solar azimuth",,,"Operational"
6141.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"005043","Field of view number",,,"Operational"
6142.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"005040","Orbit number",,,"Operational"
6143.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"201133","Change data width","Add 5 to width",,"Operational"
6144.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"005041","Scan line number",,,"Operational"
6145.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"201000","Change data width","Cancel",,"Operational"
6146.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"201132","Change data width","Add 4 to width",,"Operational"
6147.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"025070","Major frame count",,,"Operational"
6148.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"201000","Change data width","Cancel",,"Operational"
6149.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"202126","Change scale","Subtract 2 from scale",,"Operational"
6150.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"007001","Height of station",,,"Operational"
6151.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"202000","Change scale","Cancel",,"Operational"
6152.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"033060","GqisFlagQual - individual IASI-System quality flag",,,"Operational"
6153.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"033061","GqisQualIndex - indicator for instrument noise performance (contributions from spectral and radiometric calibration)",,,"Operational"
6154.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"033062","GqisQualIndexLoc - indicator for geometric quality index",,,"Operational"
6155.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"033063","GqisQualIndexRad - indicator for instrument noise performance (contributions from radiometric calibration)",,,"Operational"
6156.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"033064","GqisQualIndexSpect - indicator for instrument noise performance (contributions from spectral calibration)",,,"Operational"
6157.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"033065","GqisSysTecSondQual - output of system TEC (Technical Expertise Centre) quality function",,,"Operational"
6158.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"101010","Replicate 1 descriptor 10 times",,,"Operational"
6159.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"340002","IASI Level 1c band description",,,"Operational"
6160.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"101087","Replicate 1 descriptor 87 times",,,"Operational"
6161.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"340003","IASI Level 1c 100 channels",,,"Operational"
6162.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"002019","Satellite instruments",,,"Operational"
6163.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"025051","AVHRR channel combination",,,"Operational"
6164.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"101007","Replicate 1 descriptor 7 times",,,"Operational"
6165.00,"40","Additional satellite report sequences","340001","(IASI Level 1c data)",,"340004","IASI Level 1c AVHRR single scene",,,"Operational"
6166.00,"40","Additional satellite report sequences","340002","(IASI Level 1c band description)",,"025140","Start channel",,,"Operational"
6167.00,"40","Additional satellite report sequences","340002","(IASI Level 1c band description)",,"025141","End channel",,,"Operational"
6168.00,"40","Additional satellite report sequences","340002","(IASI Level 1c band description)",,"025142","Channel scale factor",,,"Operational"
6169.00,"40","Additional satellite report sequences","340003","(IASI Level 1c 100 channels)",,"104100","Replicate 4 descriptors 100 times",,,"Operational"
6170.00,"40","Additional satellite report sequences","340003","(IASI Level 1c 100 channels)",,"201136","Change data width","Add 8 to width",,"Operational"
6171.00,"40","Additional satellite report sequences","340003","(IASI Level 1c 100 channels)",,"005042","Channel number",,,"Operational"
6172.00,"40","Additional satellite report sequences","340003","(IASI Level 1c 100 channels)",,"201000","Change data width","Cancel",,"Operational"
6173.00,"40","Additional satellite report sequences","340003","(IASI Level 1c 100 channels)",,"014046","Scaled IASI radiance",,,"Operational"
6174.00,"40","Additional satellite report sequences","340004","(IASI Level 1c AVHRR single scene)",,"005060","Y angular position from centre of gravity",,,"Operational"
6175.00,"40","Additional satellite report sequences","340004","(IASI Level 1c AVHRR single scene)",,"005061","Z angular position from centre of gravity",,,"Operational"
6176.00,"40","Additional satellite report sequences","340004","(IASI Level 1c AVHRR single scene)",,"025085","Fraction of clear pixels in HIRS FOV",,,"Operational"
6177.00,"40","Additional satellite report sequences","340004","(IASI Level 1c AVHRR single scene)",,"105006","Replicate 5 descriptors 6 times",,,"Operational"
6178.00,"40","Additional satellite report sequences","340004","(IASI Level 1c AVHRR single scene)",,"005042","Channel number",,,"Operational"
6179.00,"40","Additional satellite report sequences","340004","(IASI Level 1c AVHRR single scene)",,"025142","Channel scale factor",,,"Operational"
6180.00,"40","Additional satellite report sequences","340004","(IASI Level 1c AVHRR single scene)",,"014047","Scaled mean AVHRR radiance",,,"Operational"
6181.00,"40","Additional satellite report sequences","340004","(IASI Level 1c AVHRR single scene)",,"025142","Channel scale factor",,,"Operational"
6182.00,"40","Additional satellite report sequences","340004","(IASI Level 1c AVHRR single scene)",,"014048","Scaled standard deviation AVHRR radiance",,,"Operational"
6183.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)",,"001007","Satellite identifier",,,"Operational"
6184.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)",,"002019","Satellite instruments",,,"Operational"
6185.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)",,"001096","Station acquisition",,,"Operational"
6186.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)",,"025061","Software identification and version number",,,"Operational"
6187.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)",,"005044","Satellite cycle number",,,"Operational"
6188.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)",,"005040","Orbit number",,,"Operational"
6189.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)",,"001030","Numerical model identifier",,,"Operational"
6190.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Datation","004001","Year",,,"Operational"
6191.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Datation","004002","Month",,,"Operational"
6192.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Datation","004003","Day",,,"Operational"
6193.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Datation","004004","Hour",,,"Operational"
6194.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Datation","004005","Minute",,,"Operational"
6195.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Datation","004007","Seconds within a minute (microsecond accuracy)",,,"Operational"
6196.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Location and surface type","005001","Latitude (high accuracy)",,,"Operational"
6197.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Location and surface type","006001","Longitude (high accuracy)",,,"Operational"
6198.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Location and surface type","008029","Surface type",,,"Operational"
6199.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Location and surface type","008074","Altimeter echo type",,,"Operational"
6200.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Location and surface type","008077","Radiometer sensed surface type",,,"Operational"
6201.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Flags","040011","Interpolation flag",,,"Operational"
6202.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Flags","025097","Three-dimensional error estimate of the navigator orbit",,,"Operational"
6203.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Flags","025095","Altimeter state flag",,,"Operational"
6204.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Flags","025098","Altimeter data quality flag",,,"Operational"
6205.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Flags","025099","Altimeter correction quality flag",,,"Operational"
6206.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Flags","021144","Altimeter rain flag",,,"Operational"
6207.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Flags","025096","Radiometer state flag",,,"Operational"
6208.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Flags","040012","Radiometer data quality flag",,,"Operational"
6209.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Flags","040013","Radiometer brightness temperature interpretation flag",,,"Operational"
6210.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Flags","021169","Ice presence indicator",,,"Operational"
6211.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: Ku band","022151","Ku band ocean range",,,"Operational"
6212.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: Ku band","022162","RMS of 20 Hz Ku band ocean range",,,"Operational"
6213.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: Ku band","022163","Number of 20 Hz valid points for Ku band",,,"Operational"
6214.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: Ku band","025160","Ku band net instrumental correction",,,"Operational"
6215.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: Ku band","025133","Sea state bias correction on Ku band",,,"Operational"
6216.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: Ku band","022156","Ku band significant wave height",,,"Operational"
6217.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: Ku band","022164","RMS 20 Hz Ku band significant wave height",,,"Operational"
6218.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: Ku band","022165","Number of 20 Hz valid points for Ku band significant wave height",,,"Operational"
6219.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: Ku band","022166","Ku band net instrumental correction for significant wave height",,,"Operational"
6220.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: Ku band","021137","Ku band corrected ocean backscatter coefficient",,,"Operational"
6221.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: Ku band","021138","STD Ku band corrected ocean backscatter coefficient",,,"Operational"
6222.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: Ku band","022167","Number of valid points for Ku band backscatter",,,"Operational"
6223.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: Ku band","021139","Ku band net instrumental correction for AGC",,,"Operational"
6224.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: Ku band","021118","Attenuation correction on sigma-0",,,"Operational"
6225.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: Ku band","021145","Ku band automatic gain control",,,"Operational"
6226.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: Ku band","021146","RMS Ku band automatic gain control",,,"Operational"
6227.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: Ku band","021147","Number of valid points for Ku band automatic gain control",,,"Operational"
6228.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: C band","022168","C band ocean range",,,"Operational"
6229.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: C band","022169","RMS of C band ocean range",,,"Operational"
6230.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: C band","022170","Number of 20 Hz valid points for C band",,,"Operational"
6231.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: C band","025161","C band net instrumental correction",,,"Operational"
6232.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: C band","025162","Sea state bias correction on C band",,,"Operational"
6233.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: C band","022171","C band significant wave height",,,"Operational"
6234.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: C band","022172","RMS 20 Hz C band significant wave height",,,"Operational"
6235.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: C band","022173","Number of 20 Hz valid points for C band significant wave height",,,"Operational"
6236.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: C band","022174","C band net instrumental correction for significant wave height",,,"Operational"
6237.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: C band","021170","C band corrected ocean backscatter coefficient",,,"Operational"
6238.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: C band","021171","RMS C band corrected ocean backscatter coefficient",,,"Operational"
6239.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: C band","022175","Number of valid points for C band backscatter",,,"Operational"
6240.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: C band","021172","C band net instrumental correction for AGC",,,"Operational"
6241.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: C band","021118","Attenuation correction on sigma-0",,,"Operational"
6242.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: C band","021173","C band automatic gain control",,,"Operational"
6243.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: C band","021174","RMS C band automatic gain control",,,"Operational"
6244.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Altimeter: C band","021175","Number of valid points for C band automatic gain control",,,"Operational"
6245.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Radiometer","002153","Satellite channel centre frequency",,,"Operational"
6246.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Radiometer","012063","Brightness temperature",,,"Operational"
6247.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Radiometer","002153","Satellite channel centre frequency",,,"Operational"
6248.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Radiometer","012063","Brightness temperature",,,"Operational"
6249.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Radiometer","002153","Satellite channel centre frequency",,,"Operational"
6250.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Radiometer","012063","Brightness temperature",,,"Operational"
6251.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Radiometer","013090","Radiometer water vapour content",,,"Operational"
6252.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Radiometer","013091","Radiometer liquid content",,,"Operational"
6253.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Wind","007002","Height or altitude",,,"Operational"
6254.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Wind","011097","Wind speed from altimeter",,,"Operational"
6255.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Wind","011098","Wind speed from radiometer",,,"Operational"
6256.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Wind","007002","Height or altitude",,,"Operational"
6257.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Wind","011095","u-component of the model wind vector",,,"Operational"
6258.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Wind","011096","v-component of the model wind vector",,,"Operational"
6259.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Dynamic topography","010096","Mean dynamic topography",,,"Operational"
6260.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Dynamic topography","010081","Altitude of COG above reference ellipsoid",,,"Operational"
6261.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Dynamic topography","010082","Instantaneous altitude rate",,,"Operational"
6262.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Dynamic topography","010083","Squared off nadir angle of the satellite from platform data",,,"Operational"
6263.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Dynamic topography","010101","Squared off nadir angle of the satellite from waveform data",,,"Operational"
6264.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Dynamic topography","025132","Ionospheric correction from model on Ku band",,,"Operational"
6265.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Dynamic topography","025163","Altimeter ionospheric correction on Ku band",,,"Operational"
6266.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Dynamic topography","025126","Model dry tropospheric correction",,,"Operational"
6267.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Dynamic topography","025128","Model wet tropospheric correction",,,"Operational"
6268.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Dynamic topography","025164","Radiometer wet tropospheric correction",,,"Operational"
6269.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Dynamic topography","010085","Mean sea-surface height",,,"Operational"
6270.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Dynamic topography","010097","Mean sea-surface height from altimeter only",,,"Operational"
6271.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Dynamic topography","010086","Geoid's height",,,"Operational"
6272.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Dynamic topography","010087","Ocean depth/land elevation",,,"Operational"
6273.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Dynamic topography","010092","Solid Earth tide height",,,"Operational"
6274.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Dynamic topography","010088","Total geocentric ocean tide height (solution 1)",,,"Operational"
6275.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Dynamic topography","010089","Total geocentric ocean tide height (solution 2)",,,"Operational"
6276.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Dynamic topography","010098","Loading tide height geocentric ocean tide solution 1",,,"Operational"
6277.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Dynamic topography","010099","Loading tide height geocentric ocean tide solution 2",,,"Operational"
6278.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Dynamic topography","010090","Long period tide height",,,"Operational"
6279.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Dynamic topography","010100","Non-equilibrium long period tide height",,,"Operational"
6280.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Dynamic topography","010093","Geocentric pole tide height",,,"Operational"
6281.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Dynamic topography","025127","Inverted barometer correction","Sea-surface height correction due to pressure loading",,"Operational"
6282.00,"40","Additional satellite report sequences","340005","(JASON2 OGDR data)","Dynamic topography","040014","High-frequency fluctuations of the sea-surface topography correction",,,"Operational"
6283.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"001007","Satellite identifier",,,"Operational"
6284.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"001031","Identification of originating/generating centre",,,"Operational"
6285.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"002019","Satellite instruments",,,"Operational"
6286.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"002020","Satellite classification",,,"Operational"
6287.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"004001","Year",,,"Operational"
6288.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"004002","Month",,,"Operational"
6289.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"004003","Day",,,"Operational"
6290.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"004004","Hour",,,"Operational"
6291.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"004005","Minute",,,"Operational"
6292.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"202131","Change scale","Add 3 to scale",,"Operational"
6293.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"201138","Change data width","Add 10 to width",,"Operational"
6294.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"004006","Second",,,"Operational"
6295.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"201000","Change data width","Cancel",,"Operational"
6296.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"202000","Change scale","Cancel",,"Operational"
6297.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"005001","Latitude (high accuracy)",,,"Operational"
6298.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"006001","Longitude (high accuracy)",,,"Operational"
6299.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"007024","Satellite zenith angle",,,"Operational"
6300.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"005021","Bearing or azimuth",,,"Operational"
6301.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"007025","Solar zenith angle",,,"Operational"
6302.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"005022","Solar azimuth",,,"Operational"
6303.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"005043","Field of view number",,,"Operational"
6304.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"005040","Orbit number",,,"Operational"
6305.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"201133","Change data width","Add 5 to width",,"Operational"
6306.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"005041","Scan line number",,,"Operational"
6307.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"201000","Change data width","Cancel",,"Operational"
6308.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"201132","Change data width","Add 4 to width",,"Operational"
6309.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"025070","Major frame count",,,"Operational"
6310.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"201000","Change data width","Cancel",,"Operational"
6311.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"202126","Change scale","Subtract 2 from scale",,"Operational"
6312.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"007001","Height of station",,,"Operational"
6313.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"202000","Change scale","Cancel",,"Operational"
6314.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"103003","Replicate 3 descriptors 3 times",,,"Operational"
6315.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"025140","Start channel",,,"Operational"
6316.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"025141","End channel",,,"Operational"
6317.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"033060","GqisFlagQual - individual IASI-System quality flag",,,"Operational"
6318.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"033061","GqisQualIndex - indicator for instrument noise performance (contributions from spectral and radiometric calibration)",,,"Operational"
6319.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"033062","GqisQualIndexLoc - indicator for geometric quality index",,,"Operational"
6320.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"033063","GqisQualIndexRad - indicator for instrument noise performance (contributions from radiometric calibration)",,,"Operational"
6321.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"033064","GqisQualIndexSpect - indicator for instrument noise performance (contributions from spectral calibration)",,,"Operational"
6322.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"033065","GqisSysTecSondQual - output of system TEC (Technical Expertise Centre) quality function",,,"Operational"
6323.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"040020","GqisFlagQualDetailed - quality flag for the system",,,"Operational"
6324.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"101010","Replicate 1 descriptor 10 times",,,"Operational"
6325.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"340002","IASI Level 1c band description",,,"Operational"
6326.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"101087","Replicate 1 descriptor 87 times",,,"Operational"
6327.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"340003","IASI Level 1c 100 channels",,,"Operational"
6328.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"002019","Satellite instruments",,,"Operational"
6329.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"025051","AVHRR channel combination",,,"Operational"
6330.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"101007","Replicate 1 descriptor 7 times",,,"Operational"
6331.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"340004","IASI Level 1c AVHRR single scene",,,"Operational"
6332.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"020081","Cloud amount in segment",,,"Operational"
6333.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"008029","Surface type",,,"Operational"
6334.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"020083","Amount of segment covered by scene",,,"Operational"
6335.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"008029","Surface type",,,"Operational"
6336.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"040018","GIacAvgImagIIS - average of imager measurements",,,"Operational"
6337.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"040019","GIacVarImagIIS - variance of imager measurements",,,"Operational"
6338.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"040021","Fraction of weighted AVHRR pixel in IASI FOV covered with snow/ice",,,"Operational"
6339.00,"40","Additional satellite report sequences","340007","(IASI Level 1c data (all channels))",,"040022","Number of missing, bad or failed AVHRR pixels",,,"Operational"
6340.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Satellite processing information","001007","Satellite identifier",,,"Operational"
6341.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Satellite processing information","001031","Identification of originating/generating centre",,,"Operational"
6342.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Satellite processing information","002019","Satellite instruments",,,"Operational"
6343.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Satellite processing information","002020","Satellite classification",,,"Operational"
6344.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Date and time","004001","Year",,,"Operational"
6345.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Date and time","004002","Month",,,"Operational"
6346.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Date and time","004003","Day",,,"Operational"
6347.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Date and time","004004","Hour",,,"Operational"
6348.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Date and time","004005","Minute",,,"Operational"
6349.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Date and time","202131","Change scale","Add 3 to scale",,"Operational"
6350.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Date and time","201138","Change data width","Add 10 to width",,"Operational"
6351.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Date and time","004006","Second",,,"Operational"
6352.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Date and time","201000","Change data width","Cancel",,"Operational"
6353.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Date and time","202000","Change scale","Cancel",,"Operational"
6354.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Location information","005001","Latitude (high accuracy)",,,"Operational"
6355.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Location information","006001","Longitude (high accuracy)",,,"Operational"
6356.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Location information","007024","Satellite zenith angle",,,"Operational"
6357.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Location information","005021","Bearing or azimuth",,,"Operational"
6358.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Location information","007025","Solar zenith angle",,,"Operational"
6359.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Location information","005022","Solar azimuth",,,"Operational"
6360.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Location information","005043","Field of view number",,,"Operational"
6361.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Location information","005040","Orbit number",,,"Operational"
6362.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Location information","201133","Change data width","Add 5 to width",,"Operational"
6363.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Location information","005041","Scan line number",,,"Operational"
6364.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Location information","201000","Change data width","Cancel",,"Operational"
6365.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Location information","201132","Change data width","Add 4 to width",,"Operational"
6366.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Location information","025070","Major frame count",,,"Operational"
6367.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Location information","201000","Change data width","Cancel",,"Operational"
6368.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Location information","202126","Change scale","Subtract 2 from scale",,"Operational"
6369.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Location information","007001","Height of station",,,"Operational"
6370.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Location information","202000","Change scale","Cancel",,"Operational"
6371.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Quality information","103003","Replicate 3 descriptors 3 times",,,"Operational"
6372.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Quality information","025140","Start channel",,,"Operational"
6373.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Quality information","025141","End channel",,,"Operational"
6374.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Quality information","033060","GqisFlagQual - individual IASI-System quality flag",,,"Operational"
6375.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Quality information","033061","GqisQualIndex - indicator for instrument noise performance (contributions from spectral and radiometric calibration)",,,"Operational"
6376.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Quality information","033062","GqisQualIndexLoc - indicator for geometric quality index",,,"Operational"
6377.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Quality information","033063","GqisQualIndexRad - indicator for instrument noise performance (contributions from radiometric calibration)",,,"Operational"
6378.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Quality information","033064","GqisQualIndexSpect - indicator for instrument noise performance (contributions from spectral calibration)",,,"Operational"
6379.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Quality information","033065","GqisSysTecSondQual - output of system TEC (Technical Expertise Centre) quality function",,,"Operational"
6380.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Quality information","040020","GqisFlagQualDetailed - quality flag for the system",,,"Operational"
6381.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","IASI subset of channels","101010","Replicate 1 descriptor 10 times",,,"Operational"
6382.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","IASI subset of channels","340002","IASI Level 1c band description",,,"Operational"
6383.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","IASI subset of channels","104000","Delayed replication of 4 descriptors",,,"Operational"
6384.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","IASI subset of channels","031002","Extended delayed descriptor replication factor",,,"Operational"
6385.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","IASI subset of channels","201136","Change data width","Add 8 to width",,"Operational"
6386.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","IASI subset of channels","005042","Channel number",,,"Operational"
6387.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","IASI subset of channels","201000","Change data width","Cancel",,"Operational"
6388.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","IASI subset of channels","014046","Scaled IASI radiance",,,"Operational"
6389.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Instrument band definition","108003","Replicate 8 descriptors 3 times",,,"Operational"
6390.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Instrument band definition","025140","Start channel",,,"Operational"
6391.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Instrument band definition","025141","End channel",,,"Operational"
6392.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Instrument band definition","040026","Score quantization factor",,,"Operational"
6393.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Instrument band definition","040016","Residual RMS in band",,,"Operational"
6394.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Instrument band definition","025062","Database identification",,,"Operational"
6395.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Principal component scores for band","101000","Delayed replication of 1 descriptor",,,"Operational"
6396.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Principal component scores for band","031002","Extended delayed descriptor replication factor",,,"Operational"
6397.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","Principal component scores for band","040017","Non-normalized principal component score",,,"Operational"
6398.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","AVHRR scene analysis","002019","Satellite instruments",,,"Operational"
6399.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","AVHRR scene analysis","025051","AVHRR channel combination",,,"Operational"
6400.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","AVHRR scene analysis","101007","Replicate 1 descriptor 7 times",,,"Operational"
6401.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","AVHRR scene analysis","340004","IASI Level 1c AVHRR single scene",,,"Operational"
6402.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","AVHRR scene analysis","020081","Cloud amount in segment",,,"Operational"
6403.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","AVHRR scene analysis","008029","Surface type",,,"Operational"
6404.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","AVHRR scene analysis","020083","Amount of segment covered by scene",,,"Operational"
6405.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","AVHRR scene analysis","008029","Surface type",,,"Operational"
6406.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","AVHRR scene analysis","040018","GIacAvgImagIIS - average of imager measurements",,,"Operational"
6407.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","AVHRR scene analysis","040019","GIacVarImagIIS - variance of imager measurements",,,"Operational"
6408.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","AVHRR scene analysis","040021","Fraction of weighted AVHRR pixel in IASI FOV covered with snow/ice",,,"Operational"
6409.00,"40","Additional satellite report sequences","340008","(IASI sequence combining PC scores, channel selection and enhanced data)","AVHRR scene analysis","040022","Number of missing, bad or failed AVHRR pixels",,,"Operational"
6410.00,"40","Additional satellite report sequences","340009","(Normalized differential vegetation index (NDVI))",,"001007","Satellite identifier",,,"Operational"
6411.00,"40","Additional satellite report sequences","340009","(Normalized differential vegetation index (NDVI))",,"001031","Identification of originating/generating centre",,,"Operational"
6412.00,"40","Additional satellite report sequences","340009","(Normalized differential vegetation index (NDVI))",,"002019","Satellite instruments",,,"Operational"
6413.00,"40","Additional satellite report sequences","340009","(Normalized differential vegetation index (NDVI))",,"002020","Satellite classification",,,"Operational"
6414.00,"40","Additional satellite report sequences","340009","(Normalized differential vegetation index (NDVI))",,"301011","Year, month, day",,,"Operational"
6415.00,"40","Additional satellite report sequences","340009","(Normalized differential vegetation index (NDVI))",,"301013","Hour, minute, second",,,"Operational"
6416.00,"40","Additional satellite report sequences","340009","(Normalized differential vegetation index (NDVI))",,"005040","Orbit number",,,"Operational"
6417.00,"40","Additional satellite report sequences","340009","(Normalized differential vegetation index (NDVI))",,"201136","Change data width","Add 8 to width",,"Operational"
6418.00,"40","Additional satellite report sequences","340009","(Normalized differential vegetation index (NDVI))",,"005041","Scan line number",,,"Operational"
6419.00,"40","Additional satellite report sequences","340009","(Normalized differential vegetation index (NDVI))",,"201000","Change data width","Cancel",,"Operational"
6420.00,"40","Additional satellite report sequences","340009","(Normalized differential vegetation index (NDVI))",,"025071","Frame count",,,"Operational"
6421.00,"40","Additional satellite report sequences","340009","(Normalized differential vegetation index (NDVI))",,"005001","Latitude (high accuracy)",,,"Operational"
6422.00,"40","Additional satellite report sequences","340009","(Normalized differential vegetation index (NDVI))",,"005001","Latitude (high accuracy)",,,"Operational"
6423.00,"40","Additional satellite report sequences","340009","(Normalized differential vegetation index (NDVI))",,"006001","Longitude (high accuracy)",,,"Operational"
6424.00,"40","Additional satellite report sequences","340009","(Normalized differential vegetation index (NDVI))",,"006001","Longitude (high accuracy)",,,"Operational"
6425.00,"40","Additional satellite report sequences","340009","(Normalized differential vegetation index (NDVI))",,"107064","Replicate 7 descriptors 64 times",,,"Operational"
6426.00,"40","Additional satellite report sequences","340009","(Normalized differential vegetation index (NDVI))",,"106032","Replicate 6 descriptors 32 times",,,"Operational"
6427.00,"40","Additional satellite report sequences","340009","(Normalized differential vegetation index (NDVI))",,"008012","Land/sea qualifier",,,"Operational"
6428.00,"40","Additional satellite report sequences","340009","(Normalized differential vegetation index (NDVI))",,"008013","Day/night qualifier",,,"Operational"
6429.00,"40","Additional satellite report sequences","340009","(Normalized differential vegetation index (NDVI))",,"008065","Sun-glint indicator",,,"Operational"
6430.00,"40","Additional satellite report sequences","340009","(Normalized differential vegetation index (NDVI))",,"008072","Pixel(s) type",,,"Operational"
6431.00,"40","Additional satellite report sequences","340009","(Normalized differential vegetation index (NDVI))",,"013039","Terrain type (ice/snow)",,,"Operational"
6432.00,"40","Additional satellite report sequences","340009","(Normalized differential vegetation index (NDVI))",,"040015","Normalized differential vegetation index (NDVI)",,,"Operational"
6433.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Satellite","001007","Satellite identifier",,,"Operational"
6434.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Satellite","002019","Satellite instruments",,,"Operational"
6435.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Satellite","001096","Station acquisition",,,"Operational"
6436.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Satellite","025061","Software identification and version number",,,"Operational"
6437.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Satellite","005044","Satellite cycle number",,,"Operational"
6438.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Satellite","005040","Orbit number",,,"Operational"
6439.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Satellite","001030","Numerical model identifier",,,"Operational"
6440.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Datation","004001","Year",,,"Operational"
6441.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Datation","004002","Month",,,"Operational"
6442.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Datation","004003","Day",,,"Operational"
6443.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Datation","004004","Hour",,,"Operational"
6444.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Datation","004005","Minute",,,"Operational"
6445.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Datation","004007","Seconds within a minute (microsecond accuracy)",,,"Operational"
6446.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Location and surface type","005001","Latitude (high accuracy)",,,"Operational"
6447.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Location and surface type","006001","Longitude (high accuracy)",,,"Operational"
6448.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Location and surface type","008029","Surface type",,,"Operational"
6449.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Location and surface type","008074","Altimeter echo type",,,"Operational"
6450.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Location and surface type","008077","Radiometer sensed surface type",,,"Operational"
6451.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Flags","040011","Interpolation flag",,,"Operational"
6452.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Flags","025097","Three-dimensional error estimate of the navigator orbit",,,"Operational"
6453.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Flags","025095","Altimeter state flag",,,"Operational"
6454.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Flags","025098","Altimeter data quality flag",,,"Operational"
6455.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Flags","025099","Altimeter correction quality flag",,,"Operational"
6456.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Flags","021144","Altimeter rain flag",,,"Operational"
6457.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Flags","025096","Radiometer state flag",,,"Operational"
6458.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Flags","040012","Radiometer data quality flag",,,"Operational"
6459.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Flags","040013","Radiometer brightness temperature interpretation flag",,,"Operational"
6460.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Flags","021169","Ice presence indicator",,,"Operational"
6461.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Flags","040023","Auxiliary altimeter state flags",,,"Operational"
6462.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Flags","040024","Meteorological map availability",,,"Operational"
6463.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Flags","040025","Interpolation flag for mean diurnal tide",,,"Operational"
6464.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: Ku band","022151","Ku band ocean range",,,"Operational"
6465.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: Ku band","022162","RMS of 20 Hz Ku band ocean range",,,"Operational"
6466.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: Ku band","022163","Number of 20 Hz valid points for Ku band",,,"Operational"
6467.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: Ku band","025160","Ku band net instrumental correction",,,"Operational"
6468.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: Ku band","025133","Sea state bias correction on Ku band",,,"Operational"
6469.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: Ku band","022156","Ku band significant wave height",,,"Operational"
6470.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: Ku band","022164","RMS 20 Hz Ku band significant wave height",,,"Operational"
6471.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: Ku band","022165","Number of 20 Hz valid points for Ku band significant wave height",,,"Operational"
6472.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: Ku band","022166","Ku band net instrumental correction for significant wave height",,,"Operational"
6473.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: Ku band","021137","Ku band corrected ocean backscatter coefficient",,,"Operational"
6474.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: Ku band","021138","STD Ku band corrected ocean backscatter coefficient",,,"Operational"
6475.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: Ku band","022167","Number of valid points for Ku band backscatter",,,"Operational"
6476.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: Ku band","021139","Ku band net instrumental correction for AGC",,,"Operational"
6477.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: Ku band","021118","Attenuation correction on sigma-0",,,"Operational"
6478.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: Ku band","021145","Ku band automatic gain control",,,"Operational"
6479.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: Ku band","021146","RMS Ku band automatic gain control",,,"Operational"
6480.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: Ku band","021147","Number of valid points for Ku band automatic gain control",,,"Operational"
6481.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: C band","022168","C band ocean range",,,"Operational"
6482.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: C band","022169","RMS of C band ocean range",,,"Operational"
6483.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: C band","022170","Number of 20 Hz valid points for C band",,,"Operational"
6484.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: C band","025161","C band net instrumental correction",,,"Operational"
6485.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: C band","025162","Sea state bias correction on C band",,,"Operational"
6486.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: C band","022171","C band significant wave height",,,"Operational"
6487.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: C band","022172","RMS 20 Hz C band significant wave height",,,"Operational"
6488.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: C band","022173","Number of 20 Hz valid points for C band significant wave height",,,"Operational"
6489.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: C band","022174","C band net instrumental correction for significant wave height",,,"Operational"
6490.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: C band","021170","C band corrected ocean backscatter coefficient",,,"Operational"
6491.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: C band","021171","RMS C band corrected ocean backscatter coefficient",,,"Operational"
6492.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: C band","022175","Number of valid points for C band backscatter",,,"Operational"
6493.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: C band","021172","C band net instrumental correction for AGC",,,"Operational"
6494.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: C band","021118","Attenuation correction on sigma-0",,,"Operational"
6495.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: C band","021173","C band automatic gain control",,,"Operational"
6496.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: C band","021174","RMS C band automatic gain control",,,"Operational"
6497.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Altimeter: C band","021175","Number of valid points for C band automatic gain control",,,"Operational"
6498.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Radiometer","002153","Satellite channel centre frequency",,,"Operational"
6499.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Radiometer","012063","Brightness temperature",,,"Operational"
6500.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Radiometer","002153","Satellite channel centre frequency",,,"Operational"
6501.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Radiometer","012063","Brightness temperature",,,"Operational"
6502.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Radiometer","002153","Satellite channel centre frequency",,,"Operational"
6503.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Radiometer","012063","Brightness temperature",,,"Operational"
6504.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Radiometer","013090","Radiometer water vapour content",,,"Operational"
6505.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Radiometer","013091","Radiometer liquid content",,,"Operational"
6506.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Wind","007002","Height or altitude",,,"Operational"
6507.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Wind","011097","Wind speed from altimeter",,,"Operational"
6508.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Wind","011098","Wind speed from radiometer",,,"Operational"
6509.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Wind","007002","Height or altitude",,,"Operational"
6510.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Wind","011095","u-component of the model wind vector",,,"Operational"
6511.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Wind","011096","v-component of the model wind vector",,,"Operational"
6512.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Dynamic topography","010096","Mean dynamic topography",,,"Operational"
6513.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Dynamic topography","010081","Altitude of COG above reference ellipsoid",,,"Operational"
6514.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Dynamic topography","010082","Instantaneous altitude rate",,,"Operational"
6515.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Dynamic topography","010083","Squared off nadir angle of the satellite from platform data",,,"Operational"
6516.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Dynamic topography","010101","Squared off nadir angle of the satellite from waveform data",,,"Operational"
6517.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Dynamic topography","025132","Ionospheric correction from model on Ku band",,,"Operational"
6518.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Dynamic topography","025163","Altimeter ionospheric correction on Ku band",,,"Operational"
6519.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Dynamic topography","025126","Model dry tropospheric correction",,,"Operational"
6520.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Dynamic topography","025128","Model wet tropospheric correction",,,"Operational"
6521.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Dynamic topography","025164","Radiometer wet tropospheric correction",,,"Operational"
6522.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Dynamic topography","010085","Mean sea-surface height",,,"Operational"
6523.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Dynamic topography","010097","Mean sea-surface height from altimeter only",,,"Operational"
6524.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Dynamic topography","010086","Geoid's height",,,"Operational"
6525.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Dynamic topography","010087","Ocean depth/land elevation",,,"Operational"
6526.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Dynamic topography","010092","Solid Earth tide height",,,"Operational"
6527.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Dynamic topography","010088","Total geocentric ocean tide height (solution 1)",,,"Operational"
6528.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Dynamic topography","010089","Total geocentric ocean tide height (solution 2)",,,"Operational"
6529.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Dynamic topography","010098","Loading tide height geocentric ocean tide solution 1",,,"Operational"
6530.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Dynamic topography","010099","Loading tide height geocentric ocean tide solution 2",,,"Operational"
6531.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Dynamic topography","010090","Long period tide height",,,"Operational"
6532.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Dynamic topography","010100","Non-equilibrium long period tide height",,,"Operational"
6533.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Dynamic topography","010093","Geocentric pole tide height",,,"Operational"
6534.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Dynamic topography","025127","Inverted barometer correction","Sea-surface height correction due to pressure loading",,"Operational"
6535.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Dynamic topography","040014","High-frequency fluctuations of the sea-surface topography correction",,,"Operational"
6536.00,"40","Additional satellite report sequences","340010","(JASON-2 OGDR data)","Dynamic topography","010102","Sea-surface height anomaly",,,"Operational"
