"No","Edition","FXY","OperatorName_E","OperationDefinition_E","Note_E","Status"
1,"1","C01YYY","Data width replacement","YYY characters (from 000 to 999) replace specified Table B data width",,"Operational"
2,"1","C02YYY","Scale factor replacement","YYY (from -99 to 999) replaces the specified Table B scale factor",,"Operational"
3,"1","C05YYY","Character insertion","YYY characters (from 001 to 999), including spaces, are inserted as a data field",,"Operational"
4,"1","C07YYY","Units replacement","Change unit to unit defined in Common Code table C-6 by code figure equal to YYY, for example:   YYY = 040 changes unit to Celsius   YYY = 741 changes unit to km h-1   YYY = 201 changes unit to knot   YYY = 740 changes unit to km",,"Operational"
5,"1","C60YYY","National letters insertion","YYY national letters including spaces are inserted as a data field.","(see Note)#CREX_16_0_0_TableC.doc#C_TableC_ed1","Operational"
6,"2","C01YYY","Data width replacement","YYY characters (from 000 to 999) replace specified Table B data width",,"Operational"
7,"2","C02YYY","Scale factor replacement","YYY (from -99 to 999) replaces the specified Table B scale factor",,"Operational"
8,"2","C05YYY","Character insertion","YYY characters (from 001 to 999), including spaces, are inserted as a data field",,"Operational"
9,"2","C07YYY","Units replacement","Change unit to unit defined in Common Code Table C-6 by code figure equal to YYY, for example:   YYY = 040 changes unit to Celsius   YYY = 741 changes unit to km h-1   YYY = 201 changes unit to knot   YYY = 740 changes unit to km",,"Operational"
10,"2","C41000","Define event","This operator denotes the beginning of the definition of an event.","(see Note 2).#CREX_16_0_0_TableC.doc#C_TableC_ed2","Operational"
11,"2","C41999","Cancel define event","This operator denotes the conclusion of the event definition that was begun via the previous C-41-000 operator.",,"Operational"
12,"2","C42000","Define conditioning event","This operator denotes the beginning of the definition of a conditioning event","(see Note 2)#CREX_16_0_0_TableC.doc#C_TableC_ed2","Operational"
13,"2","C42999","Cancel define conditioning event","This operator denotes the conclusion of the conditioning event definition that was begun via the previous C-42-000 operator.",,"Operational"
14,"2","C43000","Categorical forecast values follow","The values which follow are categorical forecast values.","(see Note 3)#CREX_16_0_0_TableC.doc#C_TableC_ed2","Operational"
15,"2","C43999","Cancel categorical forecast values follow","This operator denotes the conclusion of the definition of categorical forecast values that was begun via the previous C-43-000 operator.",,"Operational"
16,"2","C60YYY","National letters insertion","YYY national letters including spaces are inserted as a data field.","(see Note 4)#CREX_16_0_0_TableC.doc#C_TableC_ed2","Operational"
