"No","Title_E","OctetNo","Contents_E","Note_E","Status"
1.00,"Grid definition template 3.0 - latitude/longitude (or equidistant cylindrical, or Plate Carrée)","15","Shape of the Earth","(see Code table 3.2)#GRIB2_6_0_1_codeflag.doc#G2_CF32","Operational"
2.00,"Grid definition template 3.0 - latitude/longitude (or equidistant cylindrical, or Plate Carrée)","16","Scale factor of radius of spherical Earth",,"Operational"
3.00,"Grid definition template 3.0 - latitude/longitude (or equidistant cylindrical, or Plate Carrée)","17-20","Scaled value of radius of spherical Earth",,"Operational"
4.00,"Grid definition template 3.0 - latitude/longitude (or equidistant cylindrical, or Plate Carrée)","21","Scale factor of major axis of oblate spheroid Earth",,"Operational"
5.00,"Grid definition template 3.0 - latitude/longitude (or equidistant cylindrical, or Plate Carrée)","22-25","Scaled value of major axis of oblate spheroid Earth",,"Operational"
6.00,"Grid definition template 3.0 - latitude/longitude (or equidistant cylindrical, or Plate Carrée)","26","Scale factor of minor axis of oblate spheroid Earth",,"Operational"
7.00,"Grid definition template 3.0 - latitude/longitude (or equidistant cylindrical, or Plate Carrée)","27-30","Scaled value of minor axis of oblate spheroid Earth",,"Operational"
8.00,"Grid definition template 3.0 - latitude/longitude (or equidistant cylindrical, or Plate Carrée)","31-34","Ni - number of points along a parallel",,"Operational"
9.00,"Grid definition template 3.0 - latitude/longitude (or equidistant cylindrical, or Plate Carrée)","35-38","Nj - number of points along a meridian",,"Operational"
10.00,"Grid definition template 3.0 - latitude/longitude (or equidistant cylindrical, or Plate Carrée)","39-42","Basic angle of the initial production domain","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Gdt30n","Operational"
11.00,"Grid definition template 3.0 - latitude/longitude (or equidistant cylindrical, or Plate Carrée)","43-46","Subdivisions of basic angle used to define extreme longitudes and latitudes, and direction increments","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Gdt30n","Operational"
12.00,"Grid definition template 3.0 - latitude/longitude (or equidistant cylindrical, or Plate Carrée)","47-50","La1 - latitude of first grid point","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Gdt30n","Operational"
13.00,"Grid definition template 3.0 - latitude/longitude (or equidistant cylindrical, or Plate Carrée)","51-54","Lo1 - longitude of first grid point","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Gdt30n","Operational"
14.00,"Grid definition template 3.0 - latitude/longitude (or equidistant cylindrical, or Plate Carrée)","55","Resolution and component flags","(see Flag table 3.3)#GRIB2_6_0_1_codeflag.doc#G2_CF33","Operational"
15.00,"Grid definition template 3.0 - latitude/longitude (or equidistant cylindrical, or Plate Carrée)","56-59","La2 - latitude of last grid point","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Gdt30n","Operational"
16.00,"Grid definition template 3.0 - latitude/longitude (or equidistant cylindrical, or Plate Carrée)","60-63","Lo2 - longitude of last grid point","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Gdt30n","Operational"
17.00,"Grid definition template 3.0 - latitude/longitude (or equidistant cylindrical, or Plate Carrée)","64-67","Di - i direction increment","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Gdt30n","Operational"
18.00,"Grid definition template 3.0 - latitude/longitude (or equidistant cylindrical, or Plate Carrée)","68-71","Dj - j direction increment","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Gdt30n","Operational"
19.00,"Grid definition template 3.0 - latitude/longitude (or equidistant cylindrical, or Plate Carrée)","72","Scanning mode","(flags - see Flag table 3.4)#GRIB2_6_0_1_codeflag.doc#G2_CF34","Operational"
20.00,"Grid definition template 3.0 - latitude/longitude (or equidistant cylindrical, or Plate Carrée)","73-nn","List of number of points along each meridian or parallel.","(These octets are only present for quasi-regular grids as described in Notes 2 and 3)#GRIB2_6_0_1_temp.doc#G2_Gdt30n","Operational"
21.00,"Grid definition template 3.1 - rotated latitude/longitude (or equidistant cylindrical, or Plate Carrée)","15-72","Same as grid definition template 3.0","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Gdt31n","Operational"
22.00,"Grid definition template 3.1 - rotated latitude/longitude (or equidistant cylindrical, or Plate Carrée)","73-76","Latitude of the southern pole of projection",,"Operational"
23.00,"Grid definition template 3.1 - rotated latitude/longitude (or equidistant cylindrical, or Plate Carrée)","77-80","Longitude of the southern pole of projection",,"Operational"
24.00,"Grid definition template 3.1 - rotated latitude/longitude (or equidistant cylindrical, or Plate Carrée)","81-84","Angle of rotation of projection",,"Operational"
25.00,"Grid definition template 3.1 - rotated latitude/longitude (or equidistant cylindrical, or Plate Carrée)","85-nn","List of number of points along each meridian or parallel.","(These octets are only present for quasi-regular grids as described in Note 3)#GRIB2_6_0_1_temp.doc#G2_Gdt31n","Operational"
26.00,"Grid definition template 3.2 - stretched latitude/longitude (or equidistant cylindrical, or Plate Carrée)","15-72","Same as grid definition template 3.0","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Gdt32n","Operational"
27.00,"Grid definition template 3.2 - stretched latitude/longitude (or equidistant cylindrical, or Plate Carrée)","73-76","Latitude of the pole of stretching",,"Operational"
28.00,"Grid definition template 3.2 - stretched latitude/longitude (or equidistant cylindrical, or Plate Carrée)","77-80","Longitude of the pole of stretching",,"Operational"
29.00,"Grid definition template 3.2 - stretched latitude/longitude (or equidistant cylindrical, or Plate Carrée)","81-84","Stretching factor",,"Operational"
30.00,"Grid definition template 3.2 - stretched latitude/longitude (or equidistant cylindrical, or Plate Carrée)","85-nn","List of number of points along each meridian or parallel.","(These octets are only present for quasi-regular grids as described in Note 3)#GRIB2_6_0_1_temp.doc#G2_Gdt32n","Operational"
31.00,"Grid definition template 3.3 - stretched and rotated latitude/longitude (or equidistant cylindrical, or Plate Carrée)","15-72","Same as grid definition template 3.0","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Gdt33n","Operational"
32.00,"Grid definition template 3.3 - stretched and rotated latitude/longitude (or equidistant cylindrical, or Plate Carrée)","73-76","Latitude of the southern pole of projection",,"Operational"
33.00,"Grid definition template 3.3 - stretched and rotated latitude/longitude (or equidistant cylindrical, or Plate Carrée)","77-80","Longitude of the southern pole of projection",,"Operational"
34.00,"Grid definition template 3.3 - stretched and rotated latitude/longitude (or equidistant cylindrical, or Plate Carrée)","81-84","Angle of rotation of projection",,"Operational"
35.00,"Grid definition template 3.3 - stretched and rotated latitude/longitude (or equidistant cylindrical, or Plate Carrée)","85-88","Latitude of the pole of stretching",,"Operational"
36.00,"Grid definition template 3.3 - stretched and rotated latitude/longitude (or equidistant cylindrical, or Plate Carrée)","89-92","Longitude of the pole of stretching",,"Operational"
37.00,"Grid definition template 3.3 - stretched and rotated latitude/longitude (or equidistant cylindrical, or Plate Carrée)","93-96","Stretching factor",,"Operational"
38.00,"Grid definition template 3.3 - stretched and rotated latitude/longitude (or equidistant cylindrical, or Plate Carrée)","97-nn","List of number of points along each meridian or parallel.","(These octets are only present for quasi-regular grids as described in Note 4)#GRIB2_6_0_1_temp.doc#G2_Gdt33n","Operational"
39.00,"Grid definition template 3.10 - Mercator","15","Shape of the Earth","(see Code table 3.2)#GRIB2_6_0_1_codeflag.doc#G2_CF32","Operational"
40.00,"Grid definition template 3.10 - Mercator","16","Scale factor of radius of spherical Earth",,"Operational"
41.00,"Grid definition template 3.10 - Mercator","17-20","Scaled value of radius of spherical Earth",,"Operational"
42.00,"Grid definition template 3.10 - Mercator","21","Scale factor of major axis of oblate spheroid Earth",,"Operational"
43.00,"Grid definition template 3.10 - Mercator","22-25","Scaled value of major axis of oblate spheroid Earth",,"Operational"
44.00,"Grid definition template 3.10 - Mercator","26","Scale factor of minor axis of oblate spheroid Earth",,"Operational"
45.00,"Grid definition template 3.10 - Mercator","27-30","Scaled value of minor axis of oblate spheroid Earth",,"Operational"
46.00,"Grid definition template 3.10 - Mercator","31-34","Ni - number of points along a parallel",,"Operational"
47.00,"Grid definition template 3.10 - Mercator","35-38","Nj - number of points along a meridian",,"Operational"
48.00,"Grid definition template 3.10 - Mercator","39-42","La1 - latitude of first grid point",,"Operational"
49.00,"Grid definition template 3.10 - Mercator","43-46","Lo1 - longitude of first grid point",,"Operational"
50.00,"Grid definition template 3.10 - Mercator","47","Resolution and component flags","(see Flag table 3.3)#GRIB2_6_0_1_codeflag.doc#G2_CF33","Operational"
51.00,"Grid definition template 3.10 - Mercator","48-51","LaD - latitude(s) at which the Mercator projection intersects the Earth (Latitude(s) where Di and Dj are specified)",,"Operational"
52.00,"Grid definition template 3.10 - Mercator","52-55","La2 - latitude of last grid point",,"Operational"
53.00,"Grid definition template 3.10 - Mercator","56-59","Lo2 - longitude of last grid point",,"Operational"
54.00,"Grid definition template 3.10 - Mercator","60","Scanning mode","(flags - see Flag table 3.4)#GRIB2_6_0_1_codeflag.doc#G2_CF34","Operational"
55.00,"Grid definition template 3.10 - Mercator","61-64","Orientation of the grid, angle between i direction on the map and the Equator","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Gdt310n","Operational"
56.00,"Grid definition template 3.10 - Mercator","65-68","Di - longitudinal direction grid length","(see Note 2)#GRIB2_6_0_1_temp.doc#G2_Gdt310n","Operational"
57.00,"Grid definition template 3.10 - Mercator","69-72","Dj - latitudinal direction grid length","(see Note 2)#GRIB2_6_0_1_temp.doc#G2_Gdt310n","Operational"
58.00,"Grid definition template 3.10 - Mercator","73-nn","List of number of points along each meridian or parallel.","(These octets are only present for quasi-regular grids as described in Notes 2 and 3 of GDT 3.1)#GRIB2_6_0_1_temp.doc#G2_Gdt310n","Operational"
59.00,"Grid definition template 3.20 - polar stereographic projection","15","Shape of the Earth","(see Code table 3.2)#GRIB2_6_0_1_codeflag.doc#G2_CF32","Operational"
60.00,"Grid definition template 3.20 - polar stereographic projection","16","Scale factor of radius of spherical Earth",,"Operational"
61.00,"Grid definition template 3.20 - polar stereographic projection","17-20","Scaled value of radius of spherical Earth",,"Operational"
62.00,"Grid definition template 3.20 - polar stereographic projection","21","Scale factor of major axis of oblate spheroid Earth",,"Operational"
63.00,"Grid definition template 3.20 - polar stereographic projection","22-25","Scaled value of major axis of oblate spheroid Earth",,"Operational"
64.00,"Grid definition template 3.20 - polar stereographic projection","26","Scale factor of minor axis of oblate spheroid Earth",,"Operational"
65.00,"Grid definition template 3.20 - polar stereographic projection","27-30","Scaled value of minor axis of oblate spheroid Earth",,"Operational"
66.00,"Grid definition template 3.20 - polar stereographic projection","31-34","Nx - number of points along the x-axis",,"Operational"
67.00,"Grid definition template 3.20 - polar stereographic projection","35-38","Ny - number of points along the y-axis",,"Operational"
68.00,"Grid definition template 3.20 - polar stereographic projection","39-42","La1 - latitude of first grid point",,"Operational"
69.00,"Grid definition template 3.20 - polar stereographic projection","43-46","Lo1 - longitude of first grid point",,"Operational"
70.00,"Grid definition template 3.20 - polar stereographic projection","47","Resolution and component flags","(see Flag table 3.3 and Note 1)#GRIB2_6_0_1_temp.doc#G2_Gdt320n","Operational"
71.00,"Grid definition template 3.20 - polar stereographic projection","48-51","LaD - latitude where Dx and Dy are specified",,"Operational"
72.00,"Grid definition template 3.20 - polar stereographic projection","52-55","LoV - orientation of the grid","(see Note 2)#GRIB2_6_0_1_temp.doc#G2_Gdt320n","Operational"
73.00,"Grid definition template 3.20 - polar stereographic projection","56-59","Dx - x-direction grid length","(see Note 3)#GRIB2_6_0_1_temp.doc#G2_Gdt320n","Operational"
74.00,"Grid definition template 3.20 - polar stereographic projection","60-63","Dy - y-direction grid length","(see Note 3)#GRIB2_6_0_1_temp.doc#G2_Gdt320n","Operational"
75.00,"Grid definition template 3.20 - polar stereographic projection","64","Projection centre flag","(see Flag table 3.5)#GRIB2_6_0_1_codeflag.doc#G2_CF35","Operational"
76.00,"Grid definition template 3.20 - polar stereographic projection","65","Scanning mode","(see Flag table 3.4)#GRIB2_6_0_1_codeflag.doc#G2_CF34","Operational"
77.00,"Grid definition template 3.30 - Lambert conformal","15","Shape of the Earth","(see Code table 3.2)#GRIB2_6_0_1_codeflag.doc#G2_CF32","Operational"
78.00,"Grid definition template 3.30 - Lambert conformal","16","Scale factor of radius of spherical Earth",,"Operational"
79.00,"Grid definition template 3.30 - Lambert conformal","17-20","Scaled value of radius of spherical Earth",,"Operational"
80.00,"Grid definition template 3.30 - Lambert conformal","21","Scale factor of major axis of oblate spheroid Earth",,"Operational"
81.00,"Grid definition template 3.30 - Lambert conformal","22-25","Scaled value of major axis of oblate spheroid Earth",,"Operational"
82.00,"Grid definition template 3.30 - Lambert conformal","26","Scale factor of minor axis of oblate spheroid Earth",,"Operational"
83.00,"Grid definition template 3.30 - Lambert conformal","27-30","Scaled value of minor axis of oblate spheroid Earth",,"Operational"
84.00,"Grid definition template 3.30 - Lambert conformal","31-34","Nx - number of points along the x-axis",,"Operational"
85.00,"Grid definition template 3.30 - Lambert conformal","35-38","Ny - number of points along the y-axis",,"Operational"
86.00,"Grid definition template 3.30 - Lambert conformal","39-42","La1 - latitude of first grid point",,"Operational"
87.00,"Grid definition template 3.30 - Lambert conformal","43-46","Lo1 - longitude of first grid point",,"Operational"
88.00,"Grid definition template 3.30 - Lambert conformal","47","Resolution and component flags","(see Flag table 3.3)#GRIB2_6_0_1_codeflag.doc#G2_CF33","Operational"
89.00,"Grid definition template 3.30 - Lambert conformal","48-51","LaD - latitude where Dx and Dy are specified",,"Operational"
90.00,"Grid definition template 3.30 - Lambert conformal","52-55","LoV - longitude of meridian parallel to y-axis along which latitude increases as the y-coordinate increases",,"Operational"
91.00,"Grid definition template 3.30 - Lambert conformal","56-59","Dx - x-direction grid length","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Gdt330n","Operational"
92.00,"Grid definition template 3.30 - Lambert conformal","60-63","Dy - y-direction grid length","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Gdt330n","Operational"
93.00,"Grid definition template 3.30 - Lambert conformal","64","Projection centre flag","(see Flag table 3.5)#GRIB2_6_0_1_codeflag.doc#G2_CF35","Operational"
94.00,"Grid definition template 3.30 - Lambert conformal","65","Scanning mode","(see Flag table 3.4)#GRIB2_6_0_1_codeflag.doc#G2_CF34","Operational"
95.00,"Grid definition template 3.30 - Lambert conformal","66-69","Latin 1 - first latitude from the pole at which the secant cone cuts the sphere",,"Operational"
96.00,"Grid definition template 3.30 - Lambert conformal","70-73","Latin 2 - second latitude from the pole at which the secant cone cuts the sphere",,"Operational"
97.00,"Grid definition template 3.30 - Lambert conformal","74-77","Latitude of the southern pole of projection",,"Operational"
98.00,"Grid definition template 3.30 - Lambert conformal","78-81","Longitude of the southern pole of projection",,"Operational"
99.00,"Grid definition template 3.31 - Albers equal area","15","Shape of the Earth","(see Code table 3.2)#GRIB2_6_0_1_codeflag.doc#G2_CF32","Operational"
100.00,"Grid definition template 3.31 - Albers equal area","16","Scale factor of radius of spherical Earth",,"Operational"
101.00,"Grid definition template 3.31 - Albers equal area","17-20","Scaled value of radius of spherical Earth",,"Operational"
102.00,"Grid definition template 3.31 - Albers equal area","21","Scale factor of major axis of oblate spheroid Earth",,"Operational"
103.00,"Grid definition template 3.31 - Albers equal area","22-25","Scaled value of major axis of oblate spheroid Earth",,"Operational"
104.00,"Grid definition template 3.31 - Albers equal area","26","Scale factor of minor axis of oblate spheroid Earth",,"Operational"
105.00,"Grid definition template 3.31 - Albers equal area","27-30","Scaled value of minor axis of oblate spheroid Earth",,"Operational"
106.00,"Grid definition template 3.31 - Albers equal area","31-34","Nx - number of points along the x-axis",,"Operational"
107.00,"Grid definition template 3.31 - Albers equal area","35-38","Ny - number of points along the y-axis",,"Operational"
108.00,"Grid definition template 3.31 - Albers equal area","39-42","La1 - latitude of first grid point",,"Operational"
109.00,"Grid definition template 3.31 - Albers equal area","43-46","Lo1 - longitude of first grid point",,"Operational"
110.00,"Grid definition template 3.31 - Albers equal area","47","Resolution and component flags","(see Flag table 3.3)#GRIB2_6_0_1_codeflag.doc#G2_CF33","Operational"
111.00,"Grid definition template 3.31 - Albers equal area","48-51","LaD - latitude where Dx and Dy are specified",,"Operational"
112.00,"Grid definition template 3.31 - Albers equal area","52-55","LoV - longitude of meridian parallel to y-axis along which latitude increases as the y-coordinate increases",,"Operational"
113.00,"Grid definition template 3.31 - Albers equal area","56-59","Dx - x-direction grid length","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Gdt331n","Operational"
114.00,"Grid definition template 3.31 - Albers equal area","60-63","Dy - y-direction grid length","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Gdt331n","Operational"
115.00,"Grid definition template 3.31 - Albers equal area","64","Projection centre flag","(see Flag table 3.5)#GRIB2_6_0_1_codeflag.doc#G2_CF35","Operational"
116.00,"Grid definition template 3.31 - Albers equal area","65","Scanning mode","(see Flag table 3.4)#GRIB2_6_0_1_codeflag.doc#G2_CF34","Operational"
117.00,"Grid definition template 3.31 - Albers equal area","66-69","Latin 1 - first latitude from the pole at which the secant cone cuts the sphere",,"Operational"
118.00,"Grid definition template 3.31 - Albers equal area","70-73","Latin 2 - second latitude from the pole at which the secant cone cuts the sphere",,"Operational"
119.00,"Grid definition template 3.31 - Albers equal area","74-77","Latitude of the southern pole of projection",,"Operational"
120.00,"Grid definition template 3.31 - Albers equal area","78-81","Longitude of the southern pole of projection",,"Operational"
121.00,"Grid definition template 3.40 - Gaussian latitude/longitude","15","Shape of the Earth","(see Code table 3.2)#GRIB2_6_0_1_codeflag.doc#G2_CF32","Operational"
122.00,"Grid definition template 3.40 - Gaussian latitude/longitude","16","Scale factor of radius of spherical Earth",,"Operational"
123.00,"Grid definition template 3.40 - Gaussian latitude/longitude","17-20","Scaled value of radius of spherical Earth",,"Operational"
124.00,"Grid definition template 3.40 - Gaussian latitude/longitude","21","Scale factor of major axis of oblate spheroid Earth",,"Operational"
125.00,"Grid definition template 3.40 - Gaussian latitude/longitude","22-25","Scaled value of major axis of oblate spheroid Earth",,"Operational"
126.00,"Grid definition template 3.40 - Gaussian latitude/longitude","26","Scale factor of minor axis of oblate spheroid Earth",,"Operational"
127.00,"Grid definition template 3.40 - Gaussian latitude/longitude","27-30","Scaled value of minor axis of oblate spheroid Earth",,"Operational"
128.00,"Grid definition template 3.40 - Gaussian latitude/longitude","31-34","Ni - number of points along a parallel",,"Operational"
129.00,"Grid definition template 3.40 - Gaussian latitude/longitude","35-38","Nj - number of points along a meridian",,"Operational"
130.00,"Grid definition template 3.40 - Gaussian latitude/longitude","39-42","Basic angle of the initial production domain","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Gdt340n","Operational"
131.00,"Grid definition template 3.40 - Gaussian latitude/longitude","43-46","Subdivisions of basic angle used to define extreme longitudes and latitudes, and direction increments","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Gdt340n","Operational"
132.00,"Grid definition template 3.40 - Gaussian latitude/longitude","47-50","La1 - latitude of first grid point","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Gdt340n","Operational"
133.00,"Grid definition template 3.40 - Gaussian latitude/longitude","51-54","Lo1 - longitude of first grid point","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Gdt340n","Operational"
134.00,"Grid definition template 3.40 - Gaussian latitude/longitude","55","Resolution and component flags","(see Flag table 3.3)#GRIB2_6_0_1_codeflag.doc#G2_CF33","Operational"
135.00,"Grid definition template 3.40 - Gaussian latitude/longitude","56-59","La2 - latitude of last grid point","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Gdt340n","Operational"
136.00,"Grid definition template 3.40 - Gaussian latitude/longitude","60-63","Lo2 - longitude of last grid point","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Gdt340n","Operational"
137.00,"Grid definition template 3.40 - Gaussian latitude/longitude","64-67","Di - i direction increment","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Gdt340n","Operational"
138.00,"Grid definition template 3.40 - Gaussian latitude/longitude","68-71","N - number of parallels between a pole and the Equator","(see Note 2)#GRIB2_6_0_1_temp.doc#G2_Gdt340n","Operational"
139.00,"Grid definition template 3.40 - Gaussian latitude/longitude","72","Scanning mode","(flags - see Flag table 3.4)#GRIB2_6_0_1_codeflag.doc#G2_CF34","Operational"
140.00,"Grid definition template 3.40 - Gaussian latitude/longitude","73-nn","List of number of points along each meridian or parallel.","(These octets are only present for quasi-regular grids as described in Note 4)#GRIB2_6_0_1_temp.doc#G2_Gdt340n","Operational"
141.00,"Grid definition template 3.41 - rotated Gaussian latitude/longitude","15-72","Same as grid definition template 3.40","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Gdt341n","Operational"
142.00,"Grid definition template 3.41 - rotated Gaussian latitude/longitude","73-76","Latitude of the southern pole of projection",,"Operational"
143.00,"Grid definition template 3.41 - rotated Gaussian latitude/longitude","77-80","Longitude of the southern pole of projection",,"Operational"
144.00,"Grid definition template 3.41 - rotated Gaussian latitude/longitude","81-84","Angle of rotation of projection",,"Operational"
145.00,"Grid definition template 3.41 - rotated Gaussian latitude/longitude","85-nn","List of number of points along each meridian or parallel.","(These octets are only present for quasi-regular grids as described in Note 4)#GRIB2_6_0_1_temp.doc#G2_Gdt341n","Operational"
146.00,"Grid definition template 3.42 - stretched Gaussian latitude/longitude","15-72","Same as grid definition template 3.40","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Gdt342n","Operational"
147.00,"Grid definition template 3.42 - stretched Gaussian latitude/longitude","73-76","Latitude of the pole of stretching",,"Operational"
148.00,"Grid definition template 3.42 - stretched Gaussian latitude/longitude","77-80","Longitude of the pole of stretching",,"Operational"
149.00,"Grid definition template 3.42 - stretched Gaussian latitude/longitude","81-84","Stretching factor",,"Operational"
150.00,"Grid definition template 3.42 - stretched Gaussian latitude/longitude","85-nn","List of number of points along each meridian or parallel.","(These octets are only present for quasi-regular grids as described in Note 4)#GRIB2_6_0_1_temp.doc#G2_Gdt342n","Operational"
151.00,"Grid definition template 3.43 - stretched and rotated Gaussian latitude/longitude","15-72","Same as grid definition template 3.40","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Gdt343n","Operational"
152.00,"Grid definition template 3.43 - stretched and rotated Gaussian latitude/longitude","73-76","Latitude of the southern pole of projection",,"Operational"
153.00,"Grid definition template 3.43 - stretched and rotated Gaussian latitude/longitude","77-80","Longitude of the southern pole of projection",,"Operational"
154.00,"Grid definition template 3.43 - stretched and rotated Gaussian latitude/longitude","81-84","Angle of rotation of projection",,"Operational"
155.00,"Grid definition template 3.43 - stretched and rotated Gaussian latitude/longitude","85-88","Latitude of the pole of stretching",,"Operational"
156.00,"Grid definition template 3.43 - stretched and rotated Gaussian latitude/longitude","89-92","Longitude of the pole of stretching",,"Operational"
157.00,"Grid definition template 3.43 - stretched and rotated Gaussian latitude/longitude","93-96","Stretching factor",,"Operational"
158.00,"Grid definition template 3.43 - stretched and rotated Gaussian latitude/longitude","97-nn","List of number of points along each meridian or parallel.","(These octets are only present for quasi-regular grids as described in Note 5)#GRIB2_6_0_1_temp.doc#G2_Gdt343n","Operational"
159.00,"Grid definition template 3.50 - spherical harmonic coefficients","15-18","J - pentagonal resolution parameter",,"Operational"
160.00,"Grid definition template 3.50 - spherical harmonic coefficients","19-22","K - pentagonal resolution parameter",,"Operational"
161.00,"Grid definition template 3.50 - spherical harmonic coefficients","23-26","M - pentagonal resolution parameter",,"Operational"
162.00,"Grid definition template 3.50 - spherical harmonic coefficients","27","Representation type indicating the method used to define the norm","(see Code table 3.6)#GRIB2_6_0_1_codeflag.doc#G2_CF36","Operational"
163.00,"Grid definition template 3.50 - spherical harmonic coefficients","28","Representation mode indicating the order of the coefficients","(see Code table 3.7)#GRIB2_6_0_1_codeflag.doc#G2_CF37","Operational"
164.00,"Grid definition template 3.51 - rotated spherical harmonic coefficients","15-28","Same as grid definition template 3.50",,"Operational"
165.00,"Grid definition template 3.51 - rotated spherical harmonic coefficients","29-32","Latitude of the southern pole of projection",,"Operational"
166.00,"Grid definition template 3.51 - rotated spherical harmonic coefficients","33-36","Longitude of the southern pole of projection",,"Operational"
167.00,"Grid definition template 3.51 - rotated spherical harmonic coefficients","37-40","Angle of rotation of projection",,"Operational"
168.00,"Grid definition template 3.52 - stretched spherical harmonic coefficients","15-28","Same as grid definition template 3.50",,"Operational"
169.00,"Grid definition template 3.52 - stretched spherical harmonic coefficients","29-32","Latitude of the pole of stretching",,"Operational"
170.00,"Grid definition template 3.52 - stretched spherical harmonic coefficients","33-36","Longitude of the pole of stretching",,"Operational"
171.00,"Grid definition template 3.52 - stretched spherical harmonic coefficients","37-40","Stretching factor",,"Operational"
172.00,"Grid definition template 3.53 - stretched and rotated spherical harmonic coefficients","15-28","Same as grid definition template 3.50",,"Operational"
173.00,"Grid definition template 3.53 - stretched and rotated spherical harmonic coefficients","29-32","Latitude of the southern pole of projection",,"Operational"
174.00,"Grid definition template 3.53 - stretched and rotated spherical harmonic coefficients","33-36","Longitude of the southern pole of projection",,"Operational"
175.00,"Grid definition template 3.53 - stretched and rotated spherical harmonic coefficients","37-40","Angle of rotation of projection",,"Operational"
176.00,"Grid definition template 3.53 - stretched and rotated spherical harmonic coefficients","41-44","Latitude of pole of stretching",,"Operational"
177.00,"Grid definition template 3.53 - stretched and rotated spherical harmonic coefficients","45-48","Longitude of pole of stretching",,"Operational"
178.00,"Grid definition template 3.53 - stretched and rotated spherical harmonic coefficients","49-52","Stretching factor",,"Operational"
179.00,"Grid definition template 3.90 - space view perspective or orthographic","15","Shape of the Earth","(see Code table 3.2)#GRIB2_6_0_1_codeflag.doc#G2_CF32","Operational"
180.00,"Grid definition template 3.90 - space view perspective or orthographic","16","Scale factor of radius of spherical Earth",,"Operational"
181.00,"Grid definition template 3.90 - space view perspective or orthographic","17-20","Scaled value of radius of spherical Earth",,"Operational"
182.00,"Grid definition template 3.90 - space view perspective or orthographic","21","Scale factor of major axis of oblate spheroid Earth",,"Operational"
183.00,"Grid definition template 3.90 - space view perspective or orthographic","22-25","Scaled value of major axis of oblate spheroid Earth",,"Operational"
184.00,"Grid definition template 3.90 - space view perspective or orthographic","26","Scale factor of minor axis of oblate spheroid Earth",,"Operational"
185.00,"Grid definition template 3.90 - space view perspective or orthographic","27-30","Scaled value of minor axis of oblate spheroid Earth",,"Operational"
186.00,"Grid definition template 3.90 - space view perspective or orthographic","31-34","Nx - number of points along x-axis (columns)",,"Operational"
187.00,"Grid definition template 3.90 - space view perspective or orthographic","35-38","Ny - number of points along y-axis (rows or lines)",,"Operational"
188.00,"Grid definition template 3.90 - space view perspective or orthographic","39-42","Lap - latitude of sub-satellite point",,"Operational"
189.00,"Grid definition template 3.90 - space view perspective or orthographic","43-46","Lop - longitude of sub-satellite point",,"Operational"
190.00,"Grid definition template 3.90 - space view perspective or orthographic","47","Resolution and component flags","(see Flag table 3.3)#GRIB2_6_0_1_codeflag.doc#G2_CF33","Operational"
191.00,"Grid definition template 3.90 - space view perspective or orthographic","48-51","dx - apparent diameter of Earth in grid lengths, in x-direction",,"Operational"
192.00,"Grid definition template 3.90 - space view perspective or orthographic","52-55","dy - apparent diameter of Earth in grid lengths, in y-direction",,"Operational"
193.00,"Grid definition template 3.90 - space view perspective or orthographic","56-59","Xp - x-coordinate of sub-satellite point (in units of 10-3 grid length expressed as an integer)",,"Operational"
194.00,"Grid definition template 3.90 - space view perspective or orthographic","60-63","Yp - y-coordinate of sub-satellite point (in units of 10-3 grid length expressed as an integer)",,"Operational"
195.00,"Grid definition template 3.90 - space view perspective or orthographic","64","Scanning mode (flags - see Flag table 3.4)",,"Operational"
196.00,"Grid definition template 3.90 - space view perspective or orthographic","65-68","Orientation of the grid; i.e. the angle between the increasing y-axis and the meridian of the sub-satellite point in the direction of increasing latitude","(see Note 3)#GRIB2_6_0_1_temp.doc#G2_Gdt390n","Operational"
197.00,"Grid definition template 3.90 - space view perspective or orthographic","69-72","Nr - altitude of the camera from the Earth’s centre, measured in units of the Earth’s (equatorial) radius multiplied by a scale factor of 106","(see Notes 4 and 5)#GRIB2_6_0_1_temp.doc#G2_Gdt390n","Operational"
198.00,"Grid definition template 3.90 - space view perspective or orthographic","73-76","Xo - x-coordinate of origin of sector image",,"Operational"
199.00,"Grid definition template 3.90 - space view perspective or orthographic","77-80","Yo - y-coordinate of origin of sector image",,"Operational"
200.00,"Grid definition template 3.100 - triangular grid based on an icosahedron (see Attachment, Volume I.2, Part B, Att.GRIB)","15","n2 - exponent of 2 for the number of intervals on main triangle sides",,"Operational"
201.00,"Grid definition template 3.100 - triangular grid based on an icosahedron (see Attachment, Volume I.2, Part B, Att.GRIB)","16","n3 - exponent of 3 for the number of intervals on main triangle sides",,"Operational"
202.00,"Grid definition template 3.100 - triangular grid based on an icosahedron (see Attachment, Volume I.2, Part B, Att.GRIB)","17-18","ni - number of intervals on main triangle sides of the icosahedron",,"Operational"
203.00,"Grid definition template 3.100 - triangular grid based on an icosahedron (see Attachment, Volume I.2, Part B, Att.GRIB)","19","nd - number of diamonds",,"Operational"
204.00,"Grid definition template 3.100 - triangular grid based on an icosahedron (see Attachment, Volume I.2, Part B, Att.GRIB)","20-23","Latitude of the pole point of the icosahedron on the sphere",,"Operational"
205.00,"Grid definition template 3.100 - triangular grid based on an icosahedron (see Attachment, Volume I.2, Part B, Att.GRIB)","24-27","Longitude of the pole point of the icosahedron on the sphere",,"Operational"
206.00,"Grid definition template 3.100 - triangular grid based on an icosahedron (see Attachment, Volume I.2, Part B, Att.GRIB)","28-31","Longitude of the centre line of the first diamond of the icosahedron on the sphere",,"Operational"
207.00,"Grid definition template 3.100 - triangular grid based on an icosahedron (see Attachment, Volume I.2, Part B, Att.GRIB)","32","Grid point position","(see Code table 3.8)#GRIB2_6_0_1_codeflag.doc#G2_CF38","Operational"
208.00,"Grid definition template 3.100 - triangular grid based on an icosahedron (see Attachment, Volume I.2, Part B, Att.GRIB)","33","Numbering order of diamonds","(flags - see Flag table 3.9)#GRIB2_6_0_1_codeflag.doc#G2_CF39","Operational"
209.00,"Grid definition template 3.100 - triangular grid based on an icosahedron (see Attachment, Volume I.2, Part B, Att.GRIB)","34","Scanning mode for one diamond","(flags - see Flag table 3.10)#GRIB2_6_0_1_codeflag.doc#G2_CF310","Operational"
210.00,"Grid definition template 3.100 - triangular grid based on an icosahedron (see Attachment, Volume I.2, Part B, Att.GRIB)","35-38","nt - total number of grid points",,"Operational"
211.00,"Grid definition template 3.101 - general unstructured grid","15","Shape of the Earth","(see Code table 3.2)#GRIB2_6_0_1_codeflag.doc#G2_CF32","Validation"
212.00,"Grid definition template 3.101 - general unstructured grid","16-18","Number of grid used (defined by originating centre)",,"Validation"
213.00,"Grid definition template 3.101 - general unstructured grid","19","Number of grid in reference (to allow annotating for Arakawa C-grid on arbitrary grid)","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Gdt3101n","Validation"
214.00,"Grid definition template 3.110 - Equatorial azimuthal equidistant projection","15","Shape of the Earth","(see Code table 3.2)#GRIB2_6_0_1_codeflag.doc#G2_CF32","Operational"
215.00,"Grid definition template 3.110 - Equatorial azimuthal equidistant projection","16","Scale factor of radius of spherical Earth",,"Operational"
216.00,"Grid definition template 3.110 - Equatorial azimuthal equidistant projection","17-20","Scaled value of radius of spherical Earth",,"Operational"
217.00,"Grid definition template 3.110 - Equatorial azimuthal equidistant projection","21","Scale factor of major axis of oblate spheroid Earth",,"Operational"
218.00,"Grid definition template 3.110 - Equatorial azimuthal equidistant projection","22-25","Scaled value of major axis of oblate spheroid Earth",,"Operational"
219.00,"Grid definition template 3.110 - Equatorial azimuthal equidistant projection","26","Scale factor of minor axis of oblate spheroid Earth",,"Operational"
220.00,"Grid definition template 3.110 - Equatorial azimuthal equidistant projection","27-30","Scaled value of minor axis of oblate spheroid Earth",,"Operational"
221.00,"Grid definition template 3.110 - Equatorial azimuthal equidistant projection","31-34","Nx - number of points along x-axis",,"Operational"
222.00,"Grid definition template 3.110 - Equatorial azimuthal equidistant projection","35-38","Ny - number of points along y-axis",,"Operational"
223.00,"Grid definition template 3.110 - Equatorial azimuthal equidistant projection","39-42","La1 - latitude of tangency point (centre of grid)",,"Operational"
224.00,"Grid definition template 3.110 - Equatorial azimuthal equidistant projection","43-46","Lo1 - longitude of tangency point",,"Operational"
225.00,"Grid definition template 3.110 - Equatorial azimuthal equidistant projection","47","Resolution and component flags","(see Flag table 3.3)#GRIB2_6_0_1_codeflag.doc#G2_CF33","Operational"
226.00,"Grid definition template 3.110 - Equatorial azimuthal equidistant projection","48-51","Dx - x-direction grid length in units of 10-3 m as measured at the point of the axis",,"Operational"
227.00,"Grid definition template 3.110 - Equatorial azimuthal equidistant projection","52-55","Dy - y-direction grid length in units of 10-3 m as measured at the point of the axis",,"Operational"
228.00,"Grid definition template 3.110 - Equatorial azimuthal equidistant projection","56","Projection centre flag",,"Operational"
229.00,"Grid definition template 3.110 - Equatorial azimuthal equidistant projection","57","Scanning mode","(see Flag table 3.4)#GRIB2_6_0_1_codeflag.doc#G2_CF34","Operational"
230.00,"Grid definition template 3.120 - azimuth-range projection","15-18","Nb - number of data bins along radials","(see Note)#GRIB2_6_0_1_temp.doc#G2_Gdt3120n","Operational"
231.00,"Grid definition template 3.120 - azimuth-range projection","19-22","Nr - number of radials",,"Operational"
232.00,"Grid definition template 3.120 - azimuth-range projection","23-26","La1 - latitude of centre point",,"Operational"
233.00,"Grid definition template 3.120 - azimuth-range projection","27-30","Lo1 - longitude of centre point",,"Operational"
234.00,"Grid definition template 3.120 - azimuth-range projection","31-34","Dx - spacing of bins along radials",,"Operational"
235.00,"Grid definition template 3.120 - azimuth-range projection","35-38","Dstart - offset from origin to inner bound",,"Operational"
236.00,"Grid definition template 3.120 - azimuth-range projection","39","Scanning mode","(flags - see Flag table 3.4)#GRIB2_6_0_1_codeflag.doc#G2_CF34","Operational"
237.00,"Grid definition template 3.120 - azimuth-range projection",,"40-(39+4Nr)   For each of Nr radials:",,"Operational"
238.00,"Grid definition template 3.120 - azimuth-range projection","(40+4(X-1))-(41+4(X-1))","Azi - starting azimuth, degrees*10 (degrees as north)",,"Operational"
239.00,"Grid definition template 3.120 - azimuth-range projection","(42+4(X-1))-(43+4(X-1))","Adelta - azimuthal width, degrees*100 (+ clockwise, - counterclockwise), with X = 1 to Nr",,"Operational"
240.00,"Grid definition template 3.1000 - cross-section grid with points equally spaced on the horizontal","15","Shape of the Earth","(see Code table 3.2)#GRIB2_6_0_1_codeflag.doc#G2_CF32","Experimental"
241.00,"Grid definition template 3.1000 - cross-section grid with points equally spaced on the horizontal","16","Scale factor of radius of spherical Earth",,"Experimental"
242.00,"Grid definition template 3.1000 - cross-section grid with points equally spaced on the horizontal","17-20","Scaled value of radius of spherical Earth",,"Experimental"
243.00,"Grid definition template 3.1000 - cross-section grid with points equally spaced on the horizontal","21","Scale factor of major axis of oblate spheroid Earth",,"Experimental"
244.00,"Grid definition template 3.1000 - cross-section grid with points equally spaced on the horizontal","22-25","Scaled value of major axis of oblate spheroid Earth",,"Experimental"
245.00,"Grid definition template 3.1000 - cross-section grid with points equally spaced on the horizontal","26","Scale factor of minor axis of oblate spheroid Earth",,"Experimental"
246.00,"Grid definition template 3.1000 - cross-section grid with points equally spaced on the horizontal","27-30","Scaled value of minor axis of oblate spheroid Earth",,"Experimental"
247.00,"Grid definition template 3.1000 - cross-section grid with points equally spaced on the horizontal","31-34","Number of horizontal points",,"Experimental"
248.00,"Grid definition template 3.1000 - cross-section grid with points equally spaced on the horizontal","35-38","Basic angle of the initial production domain","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Gdt31000n","Experimental"
249.00,"Grid definition template 3.1000 - cross-section grid with points equally spaced on the horizontal","39-42","Subdivisions of basic angle used to define extreme longitudes and latitudes","(see Note)#GRIB2_6_0_1_temp.doc#G2_Gdt31000n","Experimental"
250.00,"Grid definition template 3.1000 - cross-section grid with points equally spaced on the horizontal","43-46","La1 - latitude of first grid point","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Gdt31000n","Experimental"
251.00,"Grid definition template 3.1000 - cross-section grid with points equally spaced on the horizontal","47-50","Lo1 - longitude of first grid point","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Gdt31000n","Experimental"
252.00,"Grid definition template 3.1000 - cross-section grid with points equally spaced on the horizontal","51","Scanning mode","(flags - see Flag table 3.4)#GRIB2_6_0_1_codeflag.doc#G2_CF34","Experimental"
253.00,"Grid definition template 3.1000 - cross-section grid with points equally spaced on the horizontal","52-55","La2 - latitude of last grid point","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Gdt31000n","Experimental"
254.00,"Grid definition template 3.1000 - cross-section grid with points equally spaced on the horizontal","56-59","Lo2 - longitude of last grid point","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Gdt31000n","Experimental"
255.00,"Grid definition template 3.1000 - cross-section grid with points equally spaced on the horizontal","60","Type of horizontal line","(see Code table 3.20)#GRIB2_6_0_1_codeflag.doc#G2_CF320","Experimental"
256.00,"Grid definition template 3.1000 - cross-section grid with points equally spaced on the horizontal","61-62","Number of vertical points",,"Experimental"
257.00,"Grid definition template 3.1000 - cross-section grid with points equally spaced on the horizontal","63","Physical meaning of vertical coordinate","(see Code table 3.15)#GRIB2_6_0_1_codeflag.doc#G2_CF315","Experimental"
258.00,"Grid definition template 3.1000 - cross-section grid with points equally spaced on the horizontal","64","Vertical dimension coordinate values definition","(see Code table 3.21)#GRIB2_6_0_1_codeflag.doc#G2_CF321","Experimental"
259.00,"Grid definition template 3.1000 - cross-section grid with points equally spaced on the horizontal","65-66","NC - number of coefficients or values used to specify vertical coordinates",,"Experimental"
260.00,"Grid definition template 3.1000 - cross-section grid with points equally spaced on the horizontal","67-(66+NC*4)","Coefficients to define vertical dimension coordinate values in functional form, or the explicit coordinate values (IEEE 32-bit floating-point values)",,"Experimental"
261.00,"Grid definition template 3.1100 - Hovmöller diagram grid with points equally spaced on the horizontal","15","Shape of the Earth","(see Code table 3.2)#GRIB2_6_0_1_codeflag.doc#G2_CF32","Experimental"
262.00,"Grid definition template 3.1100 - Hovmöller diagram grid with points equally spaced on the horizontal","16","Scale factor of radius of spherical Earth",,"Experimental"
263.00,"Grid definition template 3.1100 - Hovmöller diagram grid with points equally spaced on the horizontal","17-20","Scaled value of radius of spherical Earth",,"Experimental"
264.00,"Grid definition template 3.1100 - Hovmöller diagram grid with points equally spaced on the horizontal","21","Scale factor of major axis of oblate spheroid Earth",,"Experimental"
265.00,"Grid definition template 3.1100 - Hovmöller diagram grid with points equally spaced on the horizontal","22-25","Scaled value of major axis of oblate spheroid Earth",,"Experimental"
266.00,"Grid definition template 3.1100 - Hovmöller diagram grid with points equally spaced on the horizontal","26","Scale factor of minor axis of oblate spheroid Earth",,"Experimental"
267.00,"Grid definition template 3.1100 - Hovmöller diagram grid with points equally spaced on the horizontal","27-30","Scaled value of minor axis of oblate spheroid Earth",,"Experimental"
268.00,"Grid definition template 3.1100 - Hovmöller diagram grid with points equally spaced on the horizontal","31-34","Number of horizontal points",,"Experimental"
269.00,"Grid definition template 3.1100 - Hovmöller diagram grid with points equally spaced on the horizontal","35-38","Basic angle of the initial production domain","(see Note)#GRIB2_6_0_1_temp.doc#G2_Gdt31100n","Experimental"
270.00,"Grid definition template 3.1100 - Hovmöller diagram grid with points equally spaced on the horizontal","39-42","Subdivisions of basic angle used to define extreme longitudes and latitudes","(see Note)#GRIB2_6_0_1_temp.doc#G2_Gdt31100n","Experimental"
271.00,"Grid definition template 3.1100 - Hovmöller diagram grid with points equally spaced on the horizontal","43-46","La1 - latitude of first grid point","(see Note)#GRIB2_6_0_1_temp.doc#G2_Gdt31100n","Experimental"
272.00,"Grid definition template 3.1100 - Hovmöller diagram grid with points equally spaced on the horizontal","47-50","Lo1 - longitude of first grid point","(see Note)#GRIB2_6_0_1_temp.doc#G2_Gdt31100n","Experimental"
273.00,"Grid definition template 3.1100 - Hovmöller diagram grid with points equally spaced on the horizontal","51","Scanning mode","(flags - see Flag table 3.4)#GRIB2_6_0_1_codeflag.doc#G2_CF34","Experimental"
274.00,"Grid definition template 3.1100 - Hovmöller diagram grid with points equally spaced on the horizontal","52-55","La2 - latitude of last grid point","(see Note)#GRIB2_6_0_1_temp.doc#G2_Gdt31100n","Experimental"
275.00,"Grid definition template 3.1100 - Hovmöller diagram grid with points equally spaced on the horizontal","56-59","Lo2 - longitude of last grid point","(see Note)#GRIB2_6_0_1_temp.doc#G2_Gdt31100n","Experimental"
276.00,"Grid definition template 3.1100 - Hovmöller diagram grid with points equally spaced on the horizontal","60","Type of horizontal line","(see Code table 3.20)#GRIB2_6_0_1_codeflag.doc#G2_CF320","Experimental"
277.00,"Grid definition template 3.1100 - Hovmöller diagram grid with points equally spaced on the horizontal","61-64","NT - number of time steps",,"Experimental"
278.00,"Grid definition template 3.1100 - Hovmöller diagram grid with points equally spaced on the horizontal","65","Unit of offset from reference time","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Experimental"
279.00,"Grid definition template 3.1100 - Hovmöller diagram grid with points equally spaced on the horizontal","66-69","Offset from reference of first time (negative value when first bit set)",,"Experimental"
280.00,"Grid definition template 3.1100 - Hovmöller diagram grid with points equally spaced on the horizontal","70","Type of time increment","(see Code table 4.11)#GRIB2_6_0_1_codeflag.doc#G2_CF411","Experimental"
281.00,"Grid definition template 3.1100 - Hovmöller diagram grid with points equally spaced on the horizontal","71","Unit of time increment","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Experimental"
282.00,"Grid definition template 3.1100 - Hovmöller diagram grid with points equally spaced on the horizontal","72-75","Time increment (negative value when first bit set)",,"Experimental"
283.00,"Grid definition template 3.1100 - Hovmöller diagram grid with points equally spaced on the horizontal",,"76-82   Last date/time",,"Experimental"
284.00,"Grid definition template 3.1100 - Hovmöller diagram grid with points equally spaced on the horizontal","76-77","Year",,"Experimental"
285.00,"Grid definition template 3.1100 - Hovmöller diagram grid with points equally spaced on the horizontal","78","Month",,"Experimental"
286.00,"Grid definition template 3.1100 - Hovmöller diagram grid with points equally spaced on the horizontal","79","Day",,"Experimental"
287.00,"Grid definition template 3.1100 - Hovmöller diagram grid with points equally spaced on the horizontal","80","Hour",,"Experimental"
288.00,"Grid definition template 3.1100 - Hovmöller diagram grid with points equally spaced on the horizontal","81","Minute",,"Experimental"
289.00,"Grid definition template 3.1100 - Hovmöller diagram grid with points equally spaced on the horizontal","82","Second",,"Experimental"
290.00,"Grid definition template 3.1200 - time section grid","15-18","NT - number of time steps",,"Experimental"
291.00,"Grid definition template 3.1200 - time section grid","19","Unit of offset from reference time","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Experimental"
292.00,"Grid definition template 3.1200 - time section grid","20-23","Offset from reference of first time (negative value when first bit set)",,"Experimental"
293.00,"Grid definition template 3.1200 - time section grid","24","Type of time increment","(see Code table 4.11)#GRIB2_6_0_1_codeflag.doc#G2_CF411","Experimental"
294.00,"Grid definition template 3.1200 - time section grid","25","Unit of time increment","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Experimental"
295.00,"Grid definition template 3.1200 - time section grid","26-29","Time increment (negative value when first bit set)",,"Experimental"
296.00,"Grid definition template 3.1200 - time section grid",,"30-36   Last date/time",,"Experimental"
297.00,"Grid definition template 3.1200 - time section grid","30-31","Year",,"Experimental"
298.00,"Grid definition template 3.1200 - time section grid","32","Month",,"Experimental"
299.00,"Grid definition template 3.1200 - time section grid","33","Day",,"Experimental"
300.00,"Grid definition template 3.1200 - time section grid","34","Hour",,"Experimental"
301.00,"Grid definition template 3.1200 - time section grid","35","Minute",,"Experimental"
302.00,"Grid definition template 3.1200 - time section grid","36","Second",,"Experimental"
303.00,"Grid definition template 3.1200 - time section grid","37-38","Number of vertical points",,"Experimental"
304.00,"Grid definition template 3.1200 - time section grid","39","Physical meaning of vertical coordinate","(see Code table 3.15)#GRIB2_6_0_1_codeflag.doc#G2_CF315","Experimental"
305.00,"Grid definition template 3.1200 - time section grid","40","Vertical dimension coordinate values definition","(see Code table 3.21)#GRIB2_6_0_1_codeflag.doc#G2_CF321","Experimental"
306.00,"Grid definition template 3.1200 - time section grid","41-42","NC - number of coefficients or values used to specify vertical coordinates",,"Experimental"
307.00,"Grid definition template 3.1200 - time section grid","43-(42+NC*4)","Coefficients to define vertical dimension coordinate values in functional form, or the explicit coordinate values (IEEE 32-bit floating-point values)",,"Experimental"
308.00,"Product definition template 4.0 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time","10","Parameter category","(see Code table 4.1)#GRIB2_6_0_1_codeflag.doc#G2_CF41","Operational"
309.00,"Product definition template 4.0 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time","11","Parameter number","(see Code table 4.2)#GRIB2_6_0_1_codeflag.doc#G2_CF42","Operational"
310.00,"Product definition template 4.0 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time","12","Type of generating process","(see Code table 4.3)#GRIB2_6_0_1_codeflag.doc#G2_CF43","Operational"
311.00,"Product definition template 4.0 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time","13","Background generating process identifier (defined by originating centre)",,"Operational"
312.00,"Product definition template 4.0 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time","14","Analysis or forecast generating process identifier (defined by originating centre)",,"Operational"
313.00,"Product definition template 4.0 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time","15-16","Hours of observational data cutoff after reference time","(see Note)#GRIB2_6_0_1_temp.doc#G2_Pdt40n","Operational"
314.00,"Product definition template 4.0 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time","17","Minutes of observational data cutoff after reference time",,"Operational"
315.00,"Product definition template 4.0 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time","18","Indicator of unit of time range","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Operational"
316.00,"Product definition template 4.0 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time","19-22","Forecast time in units defined by octet 18",,"Operational"
317.00,"Product definition template 4.0 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time","23","Type of first fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Operational"
318.00,"Product definition template 4.0 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time","24","Scale factor of first fixed surface",,"Operational"
319.00,"Product definition template 4.0 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time","25-28","Scaled value of first fixed surface",,"Operational"
320.00,"Product definition template 4.0 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time","29","Type of second fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Operational"
321.00,"Product definition template 4.0 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time","30","Scale factor of second fixed surface",,"Operational"
322.00,"Product definition template 4.0 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time","31-34","Scaled value of second fixed surface",,"Operational"
323.00,"Product definition template 4.1 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time","10","Parameter category","(see Code table 4.1)#GRIB2_6_0_1_codeflag.doc#G2_CF41","Operational"
324.00,"Product definition template 4.1 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time","11","Parameter number","(see Code table 4.2)#GRIB2_6_0_1_codeflag.doc#G2_CF42","Operational"
325.00,"Product definition template 4.1 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time","12","Type of generating process","(see Code table 4.3)#GRIB2_6_0_1_codeflag.doc#G2_CF43","Operational"
326.00,"Product definition template 4.1 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time","13","Background generating process identifier (defined by originating centre)",,"Operational"
327.00,"Product definition template 4.1 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time","14","Forecast generating process identifier (defined by originating centre)",,"Operational"
328.00,"Product definition template 4.1 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time","15-16","Hours after reference time of data cutoff","(see Note)#GRIB2_6_0_1_temp.doc#G2_Pdt41n","Operational"
329.00,"Product definition template 4.1 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time","17","Minutes after reference time of data cutoff",,"Operational"
330.00,"Product definition template 4.1 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time","18","Indicator of unit of time range","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Operational"
331.00,"Product definition template 4.1 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time","19-22","Forecast time in units defined by octet 18",,"Operational"
332.00,"Product definition template 4.1 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time","23","Type of first fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Operational"
333.00,"Product definition template 4.1 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time","24","Scale factor of first fixed surface",,"Operational"
334.00,"Product definition template 4.1 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time","25-28","Scaled value of first fixed surface",,"Operational"
335.00,"Product definition template 4.1 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time","29","Type of second fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Operational"
336.00,"Product definition template 4.1 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time","30","Scale factor of second fixed surface",,"Operational"
337.00,"Product definition template 4.1 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time","31-34","Scaled value of second fixed surface",,"Operational"
338.00,"Product definition template 4.1 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time","35","Type of ensemble forecast","(see Code table 4.6)#GRIB2_6_0_1_codeflag.doc#G2_CF46","Operational"
339.00,"Product definition template 4.1 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time","36","Perturbation number",,"Operational"
340.00,"Product definition template 4.1 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time","37","Number of forecasts in ensemble",,"Operational"
341.00,"Product definition template 4.2 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer at a point in time","10","Parameter category","(see Code table 4.1)#GRIB2_6_0_1_codeflag.doc#G2_CF41","Operational"
342.00,"Product definition template 4.2 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer at a point in time","11","Parameter number","(see Code table 4.2)#GRIB2_6_0_1_codeflag.doc#G2_CF42","Operational"
343.00,"Product definition template 4.2 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer at a point in time","12","Type of generating process","(see Code table 4.3)#GRIB2_6_0_1_codeflag.doc#G2_CF43","Operational"
344.00,"Product definition template 4.2 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer at a point in time","13","Background generating process identifier (defined by originating centre)",,"Operational"
345.00,"Product definition template 4.2 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer at a point in time","14","Forecast generating process identifier (defined by originating centre)",,"Operational"
346.00,"Product definition template 4.2 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer at a point in time","15-16","Hours after reference time of data cutoff","(see Note)#GRIB2_6_0_1_temp.doc#G2_Pdt42n","Operational"
347.00,"Product definition template 4.2 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer at a point in time","17","Minutes after reference time of data cutoff",,"Operational"
348.00,"Product definition template 4.2 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer at a point in time","18","Indicator of unit of time range","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Operational"
349.00,"Product definition template 4.2 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer at a point in time","19-22","Forecast time in units defined by octet 18",,"Operational"
350.00,"Product definition template 4.2 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer at a point in time","23","Type of first fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Operational"
351.00,"Product definition template 4.2 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer at a point in time","24","Scale factor of first fixed surface",,"Operational"
352.00,"Product definition template 4.2 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer at a point in time","25-28","Scaled value of first fixed surface",,"Operational"
353.00,"Product definition template 4.2 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer at a point in time","29","Type of second fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Operational"
354.00,"Product definition template 4.2 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer at a point in time","30","Scale factor of second fixed surface",,"Operational"
355.00,"Product definition template 4.2 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer at a point in time","31-34","Scaled value of second fixed surface",,"Operational"
356.00,"Product definition template 4.2 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer at a point in time","35","Derived forecast","(see Code table 4.7)#GRIB2_6_0_1_codeflag.doc#G2_CF47","Operational"
357.00,"Product definition template 4.2 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer at a point in time","36","Number of forecasts in ensemble",,"Operational"
358.00,"Product definition template 4.3 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer at a point in time","10","Parameter category","(see Code table 4.1)#GRIB2_6_0_1_codeflag.doc#G2_CF41","Operational"
359.00,"Product definition template 4.3 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer at a point in time","11","Parameter number","(see Code table 4.2)#GRIB2_6_0_1_codeflag.doc#G2_CF42","Operational"
360.00,"Product definition template 4.3 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer at a point in time","12","Type of generating process","(see Code table 4.3)#GRIB2_6_0_1_codeflag.doc#G2_CF43","Operational"
361.00,"Product definition template 4.3 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer at a point in time","13","Background generating process identifier (defined by originating centre)",,"Operational"
362.00,"Product definition template 4.3 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer at a point in time","14","Forecast generating process identifier (defined by originating centre)",,"Operational"
363.00,"Product definition template 4.3 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer at a point in time","15-16","Hours after reference time of data cutoff","(see Note)#GRIB2_6_0_1_temp.doc#G2_Pdt43n","Operational"
364.00,"Product definition template 4.3 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer at a point in time","17","Minutes after reference time of data cutoff",,"Operational"
365.00,"Product definition template 4.3 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer at a point in time","18","Indicator of unit of time range","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Operational"
366.00,"Product definition template 4.3 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer at a point in time","19-22","Forecast time in units defined by octet 18",,"Operational"
367.00,"Product definition template 4.3 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer at a point in time","23","Type of first fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Operational"
368.00,"Product definition template 4.3 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer at a point in time","24","Scale factor of first fixed surface",,"Operational"
369.00,"Product definition template 4.3 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer at a point in time","25-28","Scaled value of first fixed surface",,"Operational"
370.00,"Product definition template 4.3 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer at a point in time","29","Type of second fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Operational"
371.00,"Product definition template 4.3 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer at a point in time","30","Scale factor of second fixed surface",,"Operational"
372.00,"Product definition template 4.3 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer at a point in time","31-34","Scaled value of second fixed surface",,"Operational"
373.00,"Product definition template 4.3 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer at a point in time","35","Derived forecast","(see Code table 4.7)#GRIB2_6_0_1_codeflag.doc#G2_CF47","Operational"
374.00,"Product definition template 4.3 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer at a point in time","36","Number of forecasts in the ensemble (N)",,"Operational"
375.00,"Product definition template 4.3 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer at a point in time","37","Cluster identifier",,"Operational"
376.00,"Product definition template 4.3 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer at a point in time","38","Number of cluster to which the high resolution control belongs",,"Operational"
377.00,"Product definition template 4.3 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer at a point in time","39","Number of cluster to which the low resolution control belongs",,"Operational"
378.00,"Product definition template 4.3 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer at a point in time","40","Total number of clusters",,"Operational"
379.00,"Product definition template 4.3 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer at a point in time","41","Clustering method","(see Code table 4.8)#GRIB2_6_0_1_codeflag.doc#G2_CF48","Operational"
380.00,"Product definition template 4.3 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer at a point in time","42-45","Northern latitude of cluster domain",,"Operational"
381.00,"Product definition template 4.3 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer at a point in time","46-49","Southern latitude of cluster domain",,"Operational"
382.00,"Product definition template 4.3 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer at a point in time","50-53","Eastern longitude of cluster domain",,"Operational"
383.00,"Product definition template 4.3 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer at a point in time","54-57","Western longitude of cluster domain",,"Operational"
384.00,"Product definition template 4.3 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer at a point in time","58","Nc - number of forecasts in the cluster",,"Operational"
385.00,"Product definition template 4.3 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer at a point in time","59","Scale factor of standard deviation in the cluster",,"Operational"
386.00,"Product definition template 4.3 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer at a point in time","60-63","Scaled value of standard deviation in the cluster",,"Operational"
387.00,"Product definition template 4.3 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer at a point in time","64","Scale factor of distance of the cluster from ensemble mean",,"Operational"
388.00,"Product definition template 4.3 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer at a point in time","65-68","Scaled value of distance of the cluster from ensemble mean",,"Operational"
389.00,"Product definition template 4.3 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer at a point in time","69-(68+Nc)","List of Nc ensemble forecast numbers (Nc is given in octet 58)",,"Operational"
390.00,"Product definition template 4.4 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer at a point in time","10","Parameter category","(see Code table 4.1)#GRIB2_6_0_1_codeflag.doc#G2_CF41","Operational"
391.00,"Product definition template 4.4 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer at a point in time","11","Parameter number","(see Code table 4.2)#GRIB2_6_0_1_codeflag.doc#G2_CF42","Operational"
392.00,"Product definition template 4.4 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer at a point in time","12","Type of generating process","(see Code table 4.3)#GRIB2_6_0_1_codeflag.doc#G2_CF43","Operational"
393.00,"Product definition template 4.4 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer at a point in time","13","Background generating process identifier (defined by originating centre)",,"Operational"
394.00,"Product definition template 4.4 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer at a point in time","14","Forecast generating process identifier (defined by originating centre)",,"Operational"
395.00,"Product definition template 4.4 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer at a point in time","15-16","Hours after reference time of data cutoff","(see Note)#GRIB2_6_0_1_temp.doc#G2_Pdt44n","Operational"
396.00,"Product definition template 4.4 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer at a point in time","17","Minutes after reference time of data cutoff",,"Operational"
397.00,"Product definition template 4.4 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer at a point in time","18","Indicator of unit of time range","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Operational"
398.00,"Product definition template 4.4 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer at a point in time","19-22","Forecast time in units defined by octet 18",,"Operational"
399.00,"Product definition template 4.4 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer at a point in time","23","Type of first fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Operational"
400.00,"Product definition template 4.4 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer at a point in time","24","Scale factor of first fixed surface",,"Operational"
401.00,"Product definition template 4.4 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer at a point in time","25-28","Scaled value of first fixed surface",,"Operational"
402.00,"Product definition template 4.4 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer at a point in time","29","Type of second fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Operational"
403.00,"Product definition template 4.4 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer at a point in time","30","Scale factor of second fixed surface",,"Operational"
404.00,"Product definition template 4.4 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer at a point in time","31-34","Scaled value of second fixed surface",,"Operational"
405.00,"Product definition template 4.4 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer at a point in time","35","Derived forecast","(see Code table 4.7)#GRIB2_6_0_1_codeflag.doc#G2_CF47","Operational"
406.00,"Product definition template 4.4 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer at a point in time","36","Number of forecasts in the ensemble (N)",,"Operational"
407.00,"Product definition template 4.4 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer at a point in time","37","Cluster identifier",,"Operational"
408.00,"Product definition template 4.4 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer at a point in time","38","Number of cluster to which the high resolution control belongs",,"Operational"
409.00,"Product definition template 4.4 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer at a point in time","39","Number of cluster to which the low resolution control belongs",,"Operational"
410.00,"Product definition template 4.4 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer at a point in time","40","Total number of clusters",,"Operational"
411.00,"Product definition template 4.4 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer at a point in time","41","Clustering method","(see Code table 4.8)#GRIB2_6_0_1_codeflag.doc#G2_CF48","Operational"
412.00,"Product definition template 4.4 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer at a point in time","42-45","Latitude of central point in cluster domain",,"Operational"
413.00,"Product definition template 4.4 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer at a point in time","46-49","Longitude of central point in cluster domain",,"Operational"
414.00,"Product definition template 4.4 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer at a point in time","50-53","Radius of cluster domain",,"Operational"
415.00,"Product definition template 4.4 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer at a point in time","54","Nc - number of forecasts in the cluster",,"Operational"
416.00,"Product definition template 4.4 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer at a point in time","55","Scale factor of standard deviation in the cluster",,"Operational"
417.00,"Product definition template 4.4 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer at a point in time","56-59","Scaled value of standard deviation in the cluster",,"Operational"
418.00,"Product definition template 4.4 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer at a point in time","60","Scale factor of distance of the cluster from ensemble mean",,"Operational"
419.00,"Product definition template 4.4 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer at a point in time","61-64","Scaled value of distance of the cluster from ensemble mean",,"Operational"
420.00,"Product definition template 4.4 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer at a point in time","65-(64+Nc)","List of Nc ensemble forecast numbers (Nc is given in octet 54)",,"Operational"
421.00,"Product definition template 4.5 - probability forecasts at a horizontal level or in a horizontal layer at a point in time","10","Parameter category","(see Code table 4.1)#GRIB2_6_0_1_codeflag.doc#G2_CF41","Operational"
422.00,"Product definition template 4.5 - probability forecasts at a horizontal level or in a horizontal layer at a point in time","11","Parameter number","(see Code table 4.2)#GRIB2_6_0_1_codeflag.doc#G2_CF42","Operational"
423.00,"Product definition template 4.5 - probability forecasts at a horizontal level or in a horizontal layer at a point in time","12","Type of generating process","(see Code table 4.3)#GRIB2_6_0_1_codeflag.doc#G2_CF43","Operational"
424.00,"Product definition template 4.5 - probability forecasts at a horizontal level or in a horizontal layer at a point in time","13","Background generating process identifier (defined by originating centre)",,"Operational"
425.00,"Product definition template 4.5 - probability forecasts at a horizontal level or in a horizontal layer at a point in time","14","Forecast generating process identifier (defined by originating centre)",,"Operational"
426.00,"Product definition template 4.5 - probability forecasts at a horizontal level or in a horizontal layer at a point in time","15-16","Hours after reference time of data cutoff","(see Note)#GRIB2_6_0_1_temp.doc#G2_Pdt45n","Operational"
427.00,"Product definition template 4.5 - probability forecasts at a horizontal level or in a horizontal layer at a point in time","17","Minutes after reference time of data cutoff",,"Operational"
428.00,"Product definition template 4.5 - probability forecasts at a horizontal level or in a horizontal layer at a point in time","18","Indicator of unit of time range","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Operational"
429.00,"Product definition template 4.5 - probability forecasts at a horizontal level or in a horizontal layer at a point in time","19-22","Forecast time in units defined by octet 18",,"Operational"
430.00,"Product definition template 4.5 - probability forecasts at a horizontal level or in a horizontal layer at a point in time","23","Type of first fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Operational"
431.00,"Product definition template 4.5 - probability forecasts at a horizontal level or in a horizontal layer at a point in time","24","Scale factor of first fixed surface",,"Operational"
432.00,"Product definition template 4.5 - probability forecasts at a horizontal level or in a horizontal layer at a point in time","25-28","Scaled value of first fixed surface",,"Operational"
433.00,"Product definition template 4.5 - probability forecasts at a horizontal level or in a horizontal layer at a point in time","29","Type of second fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Operational"
434.00,"Product definition template 4.5 - probability forecasts at a horizontal level or in a horizontal layer at a point in time","30","Scale factor of second fixed surface",,"Operational"
435.00,"Product definition template 4.5 - probability forecasts at a horizontal level or in a horizontal layer at a point in time","31-34","Scaled value of second fixed surface",,"Operational"
436.00,"Product definition template 4.5 - probability forecasts at a horizontal level or in a horizontal layer at a point in time","35","Forecast probability number",,"Operational"
437.00,"Product definition template 4.5 - probability forecasts at a horizontal level or in a horizontal layer at a point in time","36","Total number of forecast probabilities",,"Operational"
438.00,"Product definition template 4.5 - probability forecasts at a horizontal level or in a horizontal layer at a point in time","37","Probability type","(see Code table 4.9)#GRIB2_6_0_1_codeflag.doc#G2_CF49","Operational"
439.00,"Product definition template 4.5 - probability forecasts at a horizontal level or in a horizontal layer at a point in time","38","Scale factor of lower limit",,"Operational"
440.00,"Product definition template 4.5 - probability forecasts at a horizontal level or in a horizontal layer at a point in time","39-42","Scaled value of lower limit",,"Operational"
441.00,"Product definition template 4.5 - probability forecasts at a horizontal level or in a horizontal layer at a point in time","43","Scale factor of upper limit",,"Operational"
442.00,"Product definition template 4.5 - probability forecasts at a horizontal level or in a horizontal layer at a point in time","44-47","Scaled value of upper limit",,"Operational"
443.00,"Product definition template 4.6 - percentile forecasts at a horizontal level or in a horizontal layer at a point in time","10","Parameter category","(see Code table 4.1)#GRIB2_6_0_1_codeflag.doc#G2_CF41","Operational"
444.00,"Product definition template 4.6 - percentile forecasts at a horizontal level or in a horizontal layer at a point in time","11","Parameter number","(see Code table 4.2)#GRIB2_6_0_1_codeflag.doc#G2_CF42","Operational"
445.00,"Product definition template 4.6 - percentile forecasts at a horizontal level or in a horizontal layer at a point in time","12","Type of generating process","(see Code table 4.3)#GRIB2_6_0_1_codeflag.doc#G2_CF43","Operational"
446.00,"Product definition template 4.6 - percentile forecasts at a horizontal level or in a horizontal layer at a point in time","13","Background generating process identifier (defined by originating centre)",,"Operational"
447.00,"Product definition template 4.6 - percentile forecasts at a horizontal level or in a horizontal layer at a point in time","14","Forecast generating process identifier (defined by originating centre)",,"Operational"
448.00,"Product definition template 4.6 - percentile forecasts at a horizontal level or in a horizontal layer at a point in time","15-16","Hours after reference time of data cutoff","(see Note)#GRIB2_6_0_1_temp.doc#G2_Pdt46n","Operational"
449.00,"Product definition template 4.6 - percentile forecasts at a horizontal level or in a horizontal layer at a point in time","17","Minutes after reference time of data cutoff",,"Operational"
450.00,"Product definition template 4.6 - percentile forecasts at a horizontal level or in a horizontal layer at a point in time","18","Indicator of unit of time range","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Operational"
451.00,"Product definition template 4.6 - percentile forecasts at a horizontal level or in a horizontal layer at a point in time","19-22","Forecast time in units defined by octet 18",,"Operational"
452.00,"Product definition template 4.6 - percentile forecasts at a horizontal level or in a horizontal layer at a point in time","23","Type of first fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Operational"
453.00,"Product definition template 4.6 - percentile forecasts at a horizontal level or in a horizontal layer at a point in time","24","Scale factor of first fixed surface",,"Operational"
454.00,"Product definition template 4.6 - percentile forecasts at a horizontal level or in a horizontal layer at a point in time","25-28","Scaled value of first fixed surface",,"Operational"
455.00,"Product definition template 4.6 - percentile forecasts at a horizontal level or in a horizontal layer at a point in time","29","Type of second fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Operational"
456.00,"Product definition template 4.6 - percentile forecasts at a horizontal level or in a horizontal layer at a point in time","30","Scale factor of second fixed surface",,"Operational"
457.00,"Product definition template 4.6 - percentile forecasts at a horizontal level or in a horizontal layer at a point in time","31-34","Scaled value of second fixed surface",,"Operational"
458.00,"Product definition template 4.6 - percentile forecasts at a horizontal level or in a horizontal layer at a point in time","35","Percentile value (from 100% to 0%)",,"Operational"
459.00,"Product definition template 4.7 - analysis or forecast error at a horizontal level or in a horizontal layer at a point in time","10","Parameter category","(see Code table 4.1)#GRIB2_6_0_1_codeflag.doc#G2_CF41","Operational"
460.00,"Product definition template 4.7 - analysis or forecast error at a horizontal level or in a horizontal layer at a point in time","11","Parameter number","(see Code table 4.2)#GRIB2_6_0_1_codeflag.doc#G2_CF42","Operational"
461.00,"Product definition template 4.7 - analysis or forecast error at a horizontal level or in a horizontal layer at a point in time","12","Type of generating process","(see Code table 4.3)#GRIB2_6_0_1_codeflag.doc#G2_CF43","Operational"
462.00,"Product definition template 4.7 - analysis or forecast error at a horizontal level or in a horizontal layer at a point in time","13","Background generating process identifier (defined by originating centre)",,"Operational"
463.00,"Product definition template 4.7 - analysis or forecast error at a horizontal level or in a horizontal layer at a point in time","14","Analysis or forecast generating process identifier (defined by originating centre)",,"Operational"
464.00,"Product definition template 4.7 - analysis or forecast error at a horizontal level or in a horizontal layer at a point in time","15-16","Hours after reference time of data cutoff","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Pdt47n","Operational"
465.00,"Product definition template 4.7 - analysis or forecast error at a horizontal level or in a horizontal layer at a point in time","17","Minutes after reference time of data cutoff",,"Operational"
466.00,"Product definition template 4.7 - analysis or forecast error at a horizontal level or in a horizontal layer at a point in time","18","Indicator of unit of time range","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Operational"
467.00,"Product definition template 4.7 - analysis or forecast error at a horizontal level or in a horizontal layer at a point in time","19-22","Forecast time in units defined by octet 18",,"Operational"
468.00,"Product definition template 4.7 - analysis or forecast error at a horizontal level or in a horizontal layer at a point in time","23","Type of first fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Operational"
469.00,"Product definition template 4.7 - analysis or forecast error at a horizontal level or in a horizontal layer at a point in time","24","Scale factor of first fixed surface",,"Operational"
470.00,"Product definition template 4.7 - analysis or forecast error at a horizontal level or in a horizontal layer at a point in time","25-28","Scaled value of first fixed surface",,"Operational"
471.00,"Product definition template 4.7 - analysis or forecast error at a horizontal level or in a horizontal layer at a point in time","29","Type of second fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Operational"
472.00,"Product definition template 4.7 - analysis or forecast error at a horizontal level or in a horizontal layer at a point in time","30","Scale factor of second fixed surface",,"Operational"
473.00,"Product definition template 4.7 - analysis or forecast error at a horizontal level or in a horizontal layer at a point in time","31-34","Scaled value of second fixed surface",,"Operational"
474.00,"Product definition template 4.8 - average, accumulation and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","10","Parameter category","(see Code table 4.1)#GRIB2_6_0_1_codeflag.doc#G2_CF41","Operational"
475.00,"Product definition template 4.8 - average, accumulation and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","11","Parameter number","(see Code table 4.2)#GRIB2_6_0_1_codeflag.doc#G2_CF42","Operational"
476.00,"Product definition template 4.8 - average, accumulation and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","12","Type of generating process","(see Code table 4.3)#GRIB2_6_0_1_codeflag.doc#G2_CF43","Operational"
477.00,"Product definition template 4.8 - average, accumulation and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","13","Background generating process identifier (defined by originating centre)",,"Operational"
478.00,"Product definition template 4.8 - average, accumulation and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","14","Analysis or forecast generating process identifier (defined by originating centre)",,"Operational"
479.00,"Product definition template 4.8 - average, accumulation and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","15-16","Hours after reference time of data cutoff","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Pdt48n","Operational"
480.00,"Product definition template 4.8 - average, accumulation and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","17","Minutes after reference time of data cutoff",,"Operational"
481.00,"Product definition template 4.8 - average, accumulation and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","18","Indicator of unit of time range","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Operational"
482.00,"Product definition template 4.8 - average, accumulation and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","19-22","Forecast time in units defined by octet 18","(see Note 2)#GRIB2_6_0_1_temp.doc#G2_Pdt48n","Operational"
483.00,"Product definition template 4.8 - average, accumulation and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","23","Type of first fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Operational"
484.00,"Product definition template 4.8 - average, accumulation and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","24","Scale factor of first fixed surface",,"Operational"
485.00,"Product definition template 4.8 - average, accumulation and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","25-28","Scaled value of first fixed surface",,"Operational"
486.00,"Product definition template 4.8 - average, accumulation and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","29","Type of second fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Operational"
487.00,"Product definition template 4.8 - average, accumulation and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","30","Scale factor of second fixed surface",,"Operational"
488.00,"Product definition template 4.8 - average, accumulation and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","31-34","Scaled value of second fixed surface",,"Operational"
489.00,"Product definition template 4.8 - average, accumulation and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","35-36","Year - time of end of overall time interval",,"Operational"
490.00,"Product definition template 4.8 - average, accumulation and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","37","Month - time of end of overall time interval",,"Operational"
491.00,"Product definition template 4.8 - average, accumulation and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","38","Day - time of end of overall time interval",,"Operational"
492.00,"Product definition template 4.8 - average, accumulation and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","39","Hour - time of end of overall time interval",,"Operational"
493.00,"Product definition template 4.8 - average, accumulation and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","40","Minute - time of end of overall time interval",,"Operational"
494.00,"Product definition template 4.8 - average, accumulation and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","41","Second - time of end of overall time interval",,"Operational"
495.00,"Product definition template 4.8 - average, accumulation and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","42","n - number of time range specifications describing the time intervals used to calculate the statistically-processed field",,"Operational"
496.00,"Product definition template 4.8 - average, accumulation and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","43-46","Total number of data values missing in statistical process",,"Operational"
497.00,"Product definition template 4.8 - average, accumulation and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval",,"47-58   Specification of the outermost (or only) time range over which statistical processing is done",,"Operational"
498.00,"Product definition template 4.8 - average, accumulation and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","47","Statistical process used to calculate the processed field from the field at each time increment during the time range","(see Code table 4.10)#GRIB2_6_0_1_codeflag.doc#G2_CF410","Operational"
499.00,"Product definition template 4.8 - average, accumulation and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","48","Type of time increment between successive fields used in the statistical processing","(see Code table 4.11)#GRIB2_6_0_1_codeflag.doc#G2_CF411","Operational"
500.00,"Product definition template 4.8 - average, accumulation and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","49","Indicator of unit of time for time range over which statistical processing is done","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Operational"
501.00,"Product definition template 4.8 - average, accumulation and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","50-53","Length of the time range over which statistical processing is done, in units defined by the previous octet",,"Operational"
502.00,"Product definition template 4.8 - average, accumulation and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","54","Indicator of unit of time for the increment between the successive fields used","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Operational"
503.00,"Product definition template 4.8 - average, accumulation and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","55-58","Time increment between successive fields, in units defined by the previous octet","(see Notes 3 and 4)#GRIB2_6_0_1_temp.doc#G2_Pdt48n","Operational"
504.00,"Product definition template 4.8 - average, accumulation and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval",,"59-nn   These octets are included only if n>1, where nn = 46 + 12*n",,"Operational"
505.00,"Product definition template 4.8 - average, accumulation and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","59-70","As octets 47 to 58, next innermost step of processing",,"Operational"
506.00,"Product definition template 4.8 - average, accumulation and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","71-nn","Additional time range specifications, included in accordance with the value of n. Contents as octets 47 to 58, repeated as necessary",,"Operational"
507.00,"Product definition template 4.9 - probability forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","10","Parameter category","(see Code table 4.1)#GRIB2_6_0_1_codeflag.doc#G2_CF41","Operational"
508.00,"Product definition template 4.9 - probability forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","11","Parameter number","(see Code table 4.2)#GRIB2_6_0_1_codeflag.doc#G2_CF42","Operational"
509.00,"Product definition template 4.9 - probability forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","12","Type of generating process","(see Code table 4.3)#GRIB2_6_0_1_codeflag.doc#G2_CF43","Operational"
510.00,"Product definition template 4.9 - probability forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","13","Background generating process identifier (defined by originating centre)",,"Operational"
511.00,"Product definition template 4.9 - probability forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","14","Forecast generating process identifier (defined by originating centre)",,"Operational"
512.00,"Product definition template 4.9 - probability forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","15-16","Hours after reference time of data cutoff","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Pdt49n","Operational"
513.00,"Product definition template 4.9 - probability forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","17","Minutes after reference time of data cutoff",,"Operational"
514.00,"Product definition template 4.9 - probability forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","18","Indicator of unit of time range","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Operational"
515.00,"Product definition template 4.9 - probability forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","19-22","Forecast time in units defined by octet 18","(see Note 2)#GRIB2_6_0_1_temp.doc#G2_Pdt49n","Operational"
516.00,"Product definition template 4.9 - probability forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","23","Type of first fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Operational"
517.00,"Product definition template 4.9 - probability forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","24","Scale factor of first fixed surface",,"Operational"
518.00,"Product definition template 4.9 - probability forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","25-28","Scaled value of first fixed surface",,"Operational"
519.00,"Product definition template 4.9 - probability forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","29","Type of second fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Operational"
520.00,"Product definition template 4.9 - probability forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","30","Scale factor of second fixed surface",,"Operational"
521.00,"Product definition template 4.9 - probability forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","31-34","Scaled value of second fixed surface",,"Operational"
522.00,"Product definition template 4.9 - probability forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","35","Forecast probability number",,"Operational"
523.00,"Product definition template 4.9 - probability forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","36","Total number of forecast probabilities",,"Operational"
524.00,"Product definition template 4.9 - probability forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","37","Probability type","(see Code table 4.9)#GRIB2_6_0_1_codeflag.doc#G2_CF49","Operational"
525.00,"Product definition template 4.9 - probability forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","38","Scale factor of lower limit",,"Operational"
526.00,"Product definition template 4.9 - probability forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","39-42","Scaled value of lower limit",,"Operational"
527.00,"Product definition template 4.9 - probability forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","43","Scale factor of upper limit",,"Operational"
528.00,"Product definition template 4.9 - probability forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","44-47","Scaled value of upper limit",,"Operational"
529.00,"Product definition template 4.9 - probability forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","48-49","Year of end of overall time interval",,"Operational"
530.00,"Product definition template 4.9 - probability forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","50","Month of end of overall time interval",,"Operational"
531.00,"Product definition template 4.9 - probability forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","51","Day of end of overall time interval",,"Operational"
532.00,"Product definition template 4.9 - probability forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","52","Hour of end of overall time interval",,"Operational"
533.00,"Product definition template 4.9 - probability forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","53","Minute of end of overall time interval",,"Operational"
534.00,"Product definition template 4.9 - probability forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","54","Second of end of overall time interval",,"Operational"
535.00,"Product definition template 4.9 - probability forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","55","n - number of time range specifications describing the time intervals used to calculate the statistically-processed field",,"Operational"
536.00,"Product definition template 4.9 - probability forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","56-59","Total number of data values missing in the statistical process",,"Operational"
537.00,"Product definition template 4.9 - probability forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval",,"60-71   Specification of the outermost (or only) time range over which statistical processing is done",,"Operational"
538.00,"Product definition template 4.9 - probability forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","60","Statistical process used to calculate the processed field from the field at each time increment during the time range","(see Code table 4.10)#GRIB2_6_0_1_codeflag.doc#G2_CF410","Operational"
539.00,"Product definition template 4.9 - probability forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","61","Type of time increment between successive fields used in the statistical processing","(see Code table 4.11)#GRIB2_6_0_1_codeflag.doc#G2_CF411","Operational"
540.00,"Product definition template 4.9 - probability forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","62","Indicator of unit of time for time range over which statistical processing is done","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Operational"
541.00,"Product definition template 4.9 - probability forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","63-66","Length of the time range over which statistical processing is done, in units defined by the previous octet",,"Operational"
542.00,"Product definition template 4.9 - probability forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","67","Indicator of unit of time for the increment between the successive fields used","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Operational"
543.00,"Product definition template 4.9 - probability forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","68-71","Time increment between successive fields, in units defined by the previous octet","(see Note 3)#GRIB2_6_0_1_temp.doc#G2_Pdt49n","Operational"
544.00,"Product definition template 4.9 - probability forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval",,"72-nn   These octets are included only if n>1, where nn = 59 + 12*n",,"Operational"
545.00,"Product definition template 4.9 - probability forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","72-83","As octets 60 to 71, next innermost step of processing",,"Operational"
546.00,"Product definition template 4.9 - probability forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","84-nn","Additional time range specifications, included in accordance with the value of n. Contents as octets 60 to 71, repeated as necessary.",,"Operational"
547.00,"Product definition template 4.10 - percentile forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","10","Parameter category","(see Code table 4.1)#GRIB2_6_0_1_codeflag.doc#G2_CF41","Validation"
548.00,"Product definition template 4.10 - percentile forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","11","Parameter number","(see Code table 4.2)#GRIB2_6_0_1_codeflag.doc#G2_CF42","Validation"
549.00,"Product definition template 4.10 - percentile forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","12","Type of generating process","(see Code table 4.3)#GRIB2_6_0_1_codeflag.doc#G2_CF43","Validation"
550.00,"Product definition template 4.10 - percentile forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","13","Background generating process identifier (defined by originating centre)",,"Validation"
551.00,"Product definition template 4.10 - percentile forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","14","Forecast generating process identifier (defined by originating centre)",,"Validation"
552.00,"Product definition template 4.10 - percentile forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","15-16","Hours after reference time of data cutoff","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Pdt410n","Validation"
553.00,"Product definition template 4.10 - percentile forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","17","Minutes after reference time for data cutoff",,"Validation"
554.00,"Product definition template 4.10 - percentile forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","18","Indicator of unit of time range","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Validation"
555.00,"Product definition template 4.10 - percentile forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","19-22","Forecast time in units defined by previous octet","(see Note 2)#GRIB2_6_0_1_temp.doc#G2_Pdt410n","Validation"
556.00,"Product definition template 4.10 - percentile forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","23","Type of first fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Validation"
557.00,"Product definition template 4.10 - percentile forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","24","Scale factor of first fixed surface",,"Validation"
558.00,"Product definition template 4.10 - percentile forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","25-28","Scaled value of first fixed surface",,"Validation"
559.00,"Product definition template 4.10 - percentile forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","29","Type of second fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Validation"
560.00,"Product definition template 4.10 - percentile forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","30","Scale factor of second fixed surface",,"Validation"
561.00,"Product definition template 4.10 - percentile forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","31-34","Scaled value of second fixed surface",,"Validation"
562.00,"Product definition template 4.10 - percentile forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","35","Percentile value (from 100% to 0%)",,"Validation"
563.00,"Product definition template 4.10 - percentile forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","36-37","Year of end of overall time interval",,"Validation"
564.00,"Product definition template 4.10 - percentile forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","38","Month of end of overall time interval",,"Validation"
565.00,"Product definition template 4.10 - percentile forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","39","Day of end of overall time interval",,"Validation"
566.00,"Product definition template 4.10 - percentile forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","40","Hour of end of overall time interval",,"Validation"
567.00,"Product definition template 4.10 - percentile forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","41","Minute of end of overall time interval",,"Validation"
568.00,"Product definition template 4.10 - percentile forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","42","Second of end of overall time interval",,"Validation"
569.00,"Product definition template 4.10 - percentile forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","43","n - number of time range specifications describing the time intervals used to calculate the statistically-processed field",,"Validation"
570.00,"Product definition template 4.10 - percentile forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","44-47","Total number of data values missing in the statistical process",,"Validation"
571.00,"Product definition template 4.10 - percentile forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval",,"48-59   Specification of the outermost (or only) time range over which statistical processing is done",,"Validation"
572.00,"Product definition template 4.10 - percentile forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","48","Statistical process used to calculate the processed field from the field at each time increment during the time range","(see Code table 4.10)#GRIB2_6_0_1_codeflag.doc#G2_CF410","Validation"
573.00,"Product definition template 4.10 - percentile forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","49","Type of time increment between successive fields used in the statistical processing","(see Code table 4.11)#GRIB2_6_0_1_codeflag.doc#G2_CF411","Validation"
574.00,"Product definition template 4.10 - percentile forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","50","Indicator of unit of time for time range over which statistical processing is done","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Validation"
575.00,"Product definition template 4.10 - percentile forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","51-54","Length of the time range over which statistical processing is done, in units defined by the previous octet",,"Validation"
576.00,"Product definition template 4.10 - percentile forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","55","Indicator of unit of time for the increment between the successive fields used","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Validation"
577.00,"Product definition template 4.10 - percentile forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","56-59","Time increment between successive fields, in units defined by the previous octet","(see Note 3)#GRIB2_6_0_1_temp.doc#G2_Pdt410n","Validation"
578.00,"Product definition template 4.10 - percentile forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval",,"60-nn   These octets are included only if n>1, where nn = 47 + 12 x n",,"Validation"
579.00,"Product definition template 4.10 - percentile forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","60-71","As octets 48-59, next innermost step of processing",,"Validation"
580.00,"Product definition template 4.10 - percentile forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","72-nn","Additional time range specifications, included in accordance with the value of n. Contents as octets 48 to 59, repeated as necessary.",,"Validation"
581.00,"Product definition template 4.11 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","10","Parameter category","(see Code table 4.1)#GRIB2_6_0_1_codeflag.doc#G2_CF41","Operational"
582.00,"Product definition template 4.11 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","11","Parameter number","(see Code table 4.2)#GRIB2_6_0_1_codeflag.doc#G2_CF42","Operational"
583.00,"Product definition template 4.11 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","12","Type of generating process","(see Code table 4.3)#GRIB2_6_0_1_codeflag.doc#G2_CF43","Operational"
584.00,"Product definition template 4.11 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","13","Background generating process identifier (defined by originating centre)",,"Operational"
585.00,"Product definition template 4.11 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","14","Forecast generating process identifier (defined by originating centre)",,"Operational"
586.00,"Product definition template 4.11 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","15-16","Hours after reference time of data cutoff","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Pdt411n","Operational"
587.00,"Product definition template 4.11 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","17","Minutes after reference time of data cutoff",,"Operational"
588.00,"Product definition template 4.11 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","18","Indicator of unit of time range","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Operational"
589.00,"Product definition template 4.11 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","19-22","Forecast time in units defined by octet 18","(see Note 2)#GRIB2_6_0_1_temp.doc#G2_Pdt411n","Operational"
590.00,"Product definition template 4.11 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","23","Type of first fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Operational"
591.00,"Product definition template 4.11 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","24","Scale factor of first fixed surface",,"Operational"
592.00,"Product definition template 4.11 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","25-28","Scaled value of first fixed surface",,"Operational"
593.00,"Product definition template 4.11 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","29","Type of second fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Operational"
594.00,"Product definition template 4.11 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","30","Scale factor of second fixed surface",,"Operational"
595.00,"Product definition template 4.11 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","31-34","Scaled value of second fixed surface",,"Operational"
596.00,"Product definition template 4.11 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","35","Type of ensemble forecast","(see Code table 4.6)#GRIB2_6_0_1_codeflag.doc#G2_CF46","Operational"
597.00,"Product definition template 4.11 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","36","Perturbation number",,"Operational"
598.00,"Product definition template 4.11 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","37","Number of forecasts in ensemble",,"Operational"
599.00,"Product definition template 4.11 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","38-39","Year of end of overall time interval",,"Operational"
600.00,"Product definition template 4.11 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","40","Month of end of overall time interval",,"Operational"
601.00,"Product definition template 4.11 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","41","Day of end of overall time interval",,"Operational"
602.00,"Product definition template 4.11 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","42","Hour of end of overall time interval",,"Operational"
603.00,"Product definition template 4.11 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","43","Minute of end of overall time interval",,"Operational"
604.00,"Product definition template 4.11 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","44","Second of end of overall time interval",,"Operational"
605.00,"Product definition template 4.11 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","45","n - number of time range specifications describing the time intervals used to calculate the statistically-processed field",,"Operational"
606.00,"Product definition template 4.11 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","46-49","Total number of data values missing in statistical process",,"Operational"
607.00,"Product definition template 4.11 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval",,"50-61   Specification of the outermost (or only) time range over which statistical processing is done",,"Operational"
608.00,"Product definition template 4.11 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","50","Statistical process used to calculate the processed field from the field at each time increment during the time range","(see Code table 4.10)#GRIB2_6_0_1_codeflag.doc#G2_CF410","Operational"
609.00,"Product definition template 4.11 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","51","Type of time increment between successive fields used in the statistical processing","(see Code table 4.11)#GRIB2_6_0_1_codeflag.doc#G2_CF411","Operational"
610.00,"Product definition template 4.11 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","52","Indicator of unit of time for time range over which statistical processing is done","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Operational"
611.00,"Product definition template 4.11 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","53-56","Length of the time range over which statistical processing is done, in units defined by the previous octet",,"Operational"
612.00,"Product definition template 4.11 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","57","Indicator of unit of time for the increment between the successive fields used","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Operational"
613.00,"Product definition template 4.11 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","58-61","Time increment between successive fields, in units defined by the previous octet","(see Note 3)#GRIB2_6_0_1_temp.doc#G2_Pdt411n","Operational"
614.00,"Product definition template 4.11 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval",,"62-nn   These octets are included only if n>1, where nn = 49 + 12*n",,"Operational"
615.00,"Product definition template 4.11 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","62-73","As octets 50 to 61, next innermost step of processing",,"Operational"
616.00,"Product definition template 4.11 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","74-nn","Additional time range specifications, included in accordance with the value of n. Contents as octets 50 to 61, repeated as necessary",,"Operational"
617.00,"Product definition template 4.12 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","10","Parameter category","(see Code table 4.1)#GRIB2_6_0_1_codeflag.doc#G2_CF41","Operational"
618.00,"Product definition template 4.12 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","11","Parameter number","(see Code table 4.2)#GRIB2_6_0_1_codeflag.doc#G2_CF42","Operational"
619.00,"Product definition template 4.12 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","12","Type of generating process","(see Code table 4.3)#GRIB2_6_0_1_codeflag.doc#G2_CF43","Operational"
620.00,"Product definition template 4.12 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","13","Background generating process identifier (defined by originating centre)",,"Operational"
621.00,"Product definition template 4.12 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","14","Forecast generating process identifier (defined by originating centre)",,"Operational"
622.00,"Product definition template 4.12 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","15-16","Hours after reference time of data cutoff","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Pdt412n","Operational"
623.00,"Product definition template 4.12 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","17","Minutes after reference time of data cutoff",,"Operational"
624.00,"Product definition template 4.12 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","18","Indicator of unit of time range","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Operational"
625.00,"Product definition template 4.12 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","19-22","Forecast time in units defined by octet 18","(see Note 2)#GRIB2_6_0_1_temp.doc#G2_Pdt412n","Operational"
626.00,"Product definition template 4.12 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","23","Type of first fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Operational"
627.00,"Product definition template 4.12 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","24","Scale factor of first fixed surface",,"Operational"
628.00,"Product definition template 4.12 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","25-28","Scaled value of first fixed surface",,"Operational"
629.00,"Product definition template 4.12 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","29","Type of second fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Operational"
630.00,"Product definition template 4.12 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","30","Scale factor of second fixed surface",,"Operational"
631.00,"Product definition template 4.12 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","31-34","Scaled value of second fixed surface",,"Operational"
632.00,"Product definition template 4.12 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","35","Derived forecast","(see Code table 4.7)#GRIB2_6_0_1_codeflag.doc#G2_CF47","Operational"
633.00,"Product definition template 4.12 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","36","Number of forecasts in the ensemble (N)",,"Operational"
634.00,"Product definition template 4.12 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","37-38","Year of end of overall time interval",,"Operational"
635.00,"Product definition template 4.12 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","39","Month of end of overall time interval",,"Operational"
636.00,"Product definition template 4.12 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","40","Day of end of overall time interval",,"Operational"
637.00,"Product definition template 4.12 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","41","Hour of end of overall time interval",,"Operational"
638.00,"Product definition template 4.12 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","42","Minute of end of overall time interval",,"Operational"
639.00,"Product definition template 4.12 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","43","Second of end of overall time interval",,"Operational"
640.00,"Product definition template 4.12 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","44","n - number of time range specifications describing the time intervals used to calculate the statistically-processed field",,"Operational"
641.00,"Product definition template 4.12 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","45-48","Total number of data values missing in statistical process",,"Operational"
642.00,"Product definition template 4.12 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval",,"49-60   Specification of the outermost (or only) time range over which statistical processing is done",,"Operational"
643.00,"Product definition template 4.12 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","49","Statistical process used to calculate the processed field from the field at each time increment during the time range","(see Code table 4.10)#GRIB2_6_0_1_codeflag.doc#G2_CF410","Operational"
644.00,"Product definition template 4.12 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","50","Type of time increment between successive fields used in the statistical processing","(see Code table 4.11)#GRIB2_6_0_1_codeflag.doc#G2_CF411","Operational"
645.00,"Product definition template 4.12 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","51","Indicator of unit of time for time range over which statistical processing is done","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Operational"
646.00,"Product definition template 4.12 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","52-55","Length of the time range over which statistical processing is done, in units defined by the previous octet",,"Operational"
647.00,"Product definition template 4.12 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","56","Indicator of unit of time for the increment between the successive fields used","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Operational"
648.00,"Product definition template 4.12 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","57-60","Time increment between successive fields, in units defined by the previous octet","(see Notes 3 and 4)#GRIB2_6_0_1_temp.doc#G2_Pdt412n","Operational"
649.00,"Product definition template 4.12 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval",,"61-nn   These octets are included only if n>1, where nn = 48 + 12*n",,"Operational"
650.00,"Product definition template 4.12 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","61-72","As octets 49 to 60, next innermost step of processing",,"Operational"
651.00,"Product definition template 4.12 - derived forecasts based on all ensemble members at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","73-nn","Additional time range specifications, included in accordance with the value of n. Contents as octets 49 to 60, repeated as necessary",,"Operational"
652.00,"Product definition template 4.13 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","10","Parameter category","(see Code table 4.1)#GRIB2_6_0_1_codeflag.doc#G2_CF41","Operational"
653.00,"Product definition template 4.13 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","11","Parameter number","(see Code table 4.2)#GRIB2_6_0_1_codeflag.doc#G2_CF42","Operational"
654.00,"Product definition template 4.13 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","12","Type of generating process","(see Code table 4.3)#GRIB2_6_0_1_codeflag.doc#G2_CF43","Operational"
655.00,"Product definition template 4.13 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","13","Background generating process identifier (defined by originating centre)",,"Operational"
656.00,"Product definition template 4.13 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","14","Forecast generating process identifier (defined by originating centre)",,"Operational"
657.00,"Product definition template 4.13 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","15-16","Hours after reference time of data cutoff","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Pdt413n","Operational"
658.00,"Product definition template 4.13 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","17","Minutes after reference time of data cutoff",,"Operational"
659.00,"Product definition template 4.13 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","18","Indicator of unit of time range","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Operational"
660.00,"Product definition template 4.13 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","19-22","Forecast time in units defined by octet 18","(see Note 2)#GRIB2_6_0_1_temp.doc#G2_Pdt413n","Operational"
661.00,"Product definition template 4.13 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","23","Type of first fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Operational"
662.00,"Product definition template 4.13 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","24","Scale factor of first fixed surface",,"Operational"
663.00,"Product definition template 4.13 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","25-28","Scaled value of first fixed surface",,"Operational"
664.00,"Product definition template 4.13 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","29","Type of second fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Operational"
665.00,"Product definition template 4.13 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","30","Scale factor of second fixed surface",,"Operational"
666.00,"Product definition template 4.13 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","31-34","Scaled value of second fixed surface",,"Operational"
667.00,"Product definition template 4.13 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","35","Derived forecast","(see Code table 4.7)#GRIB2_6_0_1_codeflag.doc#G2_CF47","Operational"
668.00,"Product definition template 4.13 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","36","Number of forecasts in the ensemble (N)",,"Operational"
669.00,"Product definition template 4.13 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","37","Cluster identifier",,"Operational"
670.00,"Product definition template 4.13 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","38","Number of cluster to which the high resolution control belongs",,"Operational"
671.00,"Product definition template 4.13 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","39","Number of cluster to which the low resolution control belongs",,"Operational"
672.00,"Product definition template 4.13 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","40","Total number of clusters",,"Operational"
673.00,"Product definition template 4.13 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","41","Clustering method","(see Code table 4.8)#GRIB2_6_0_1_codeflag.doc#G2_CF48","Operational"
674.00,"Product definition template 4.13 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","42-45","Northern latitude of cluster domain",,"Operational"
675.00,"Product definition template 4.13 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","46-49","Southern latitude of cluster domain",,"Operational"
676.00,"Product definition template 4.13 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","50-53","Eastern longitude of cluster domain",,"Operational"
677.00,"Product definition template 4.13 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","54-57","Western longitude of cluster domain",,"Operational"
678.00,"Product definition template 4.13 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","58","NC - number of forecasts in the cluster",,"Operational"
679.00,"Product definition template 4.13 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","59","Scale factor of standard deviation in the cluster",,"Operational"
680.00,"Product definition template 4.13 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","60-63","Scaled value of standard deviation in the cluster",,"Operational"
681.00,"Product definition template 4.13 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","64","Scale factor of distance of the cluster from ensemble mean",,"Operational"
682.00,"Product definition template 4.13 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","65-68","Scaled value of distance of the cluster from ensemble mean",,"Operational"
683.00,"Product definition template 4.13 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","69-70","Year of end of overall time interval",,"Operational"
684.00,"Product definition template 4.13 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","71","Month of end of overall time interval",,"Operational"
685.00,"Product definition template 4.13 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","72","Day of end of overall time interval",,"Operational"
686.00,"Product definition template 4.13 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","73","Hour of end of overall time interval",,"Operational"
687.00,"Product definition template 4.13 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","74","Minute of end of overall time interval",,"Operational"
688.00,"Product definition template 4.13 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","75","Second of end of overall time interval",,"Operational"
689.00,"Product definition template 4.13 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","76","n - number of time range specifications describing the time intervals used to calculate the statistically-processed field",,"Operational"
690.00,"Product definition template 4.13 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","77-80","Total number of data values missing in statistical process",,"Operational"
691.00,"Product definition template 4.13 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval",,"81-92   Specification of the outermost (or only) time range over which statistical processing is done",,"Operational"
692.00,"Product definition template 4.13 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","81","Statistical process used to calculate the processed field from the field at each time increment during the time range","(see Code table 4.10)#GRIB2_6_0_1_codeflag.doc#G2_CF410","Operational"
693.00,"Product definition template 4.13 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","82","Type of time increment between successive fields used in the statistical processing","(see Code table 4.11)#GRIB2_6_0_1_codeflag.doc#G2_CF411","Operational"
694.00,"Product definition template 4.13 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","83","Indicator of unit of time for time range over which statistical processing is done","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Operational"
695.00,"Product definition template 4.13 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","84-87","Length of the time range over which statistical processing is done, in units defined by the previous octet",,"Operational"
696.00,"Product definition template 4.13 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","88","Indicator of unit of time for the increment between the successive fields used","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Operational"
697.00,"Product definition template 4.13 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","89-92","Time increment between successive fields, in units defined by the previous octet","(see Notes 3 and 4)#GRIB2_6_0_1_temp.doc#G2_Pdt413n","Operational"
698.00,"Product definition template 4.13 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval",,"93-nn   These octets are included only if n>1, where nn = 80 + 12*n",,"Operational"
699.00,"Product definition template 4.13 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","93-104","As octets 81 to 92, next innermost step of processing",,"Operational"
700.00,"Product definition template 4.13 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","105-nn","Additional time range specifications, included in accordance with the value of n. Contents as octets 81 to 92, repeated as necessary",,"Operational"
701.00,"Product definition template 4.13 - derived forecasts based on a cluster of ensemble members over a rectangular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","(nn+1)-(nn+ NC)","List of NC ensemble forecast numbers (NC is given in octet 58)",,"Operational"
702.00,"Product definition template 4.14 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","10","Parameter category","(see Code table 4.1)#GRIB2_6_0_1_codeflag.doc#G2_CF41","Operational"
703.00,"Product definition template 4.14 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","11","Parameter number","(see Code table 4.2)#GRIB2_6_0_1_codeflag.doc#G2_CF42","Operational"
704.00,"Product definition template 4.14 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","12","Type of generating process","(see Code table 4.3)#GRIB2_6_0_1_codeflag.doc#G2_CF43","Operational"
705.00,"Product definition template 4.14 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","13","Background generating process identifier (defined by originating centre)",,"Operational"
706.00,"Product definition template 4.14 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","14","Forecast generating process identifier (defined by originating centre)",,"Operational"
707.00,"Product definition template 4.14 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","15-16","Hours after reference time of data cutoff","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Pdt414n","Operational"
708.00,"Product definition template 4.14 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","17","Minutes after reference time of data cutoff",,"Operational"
709.00,"Product definition template 4.14 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","18","Indicator of unit of time range","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Operational"
710.00,"Product definition template 4.14 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","19-22","Forecast time in units defined by octet 18","(see Note 2)#GRIB2_6_0_1_temp.doc#G2_Pdt414n","Operational"
711.00,"Product definition template 4.14 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","23","Type of first fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Operational"
712.00,"Product definition template 4.14 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","24","Scale factor of first fixed surface",,"Operational"
713.00,"Product definition template 4.14 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","25-28","Scaled value of first fixed surface",,"Operational"
714.00,"Product definition template 4.14 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","29","Type of second fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Operational"
715.00,"Product definition template 4.14 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","30","Scale factor of second fixed surface",,"Operational"
716.00,"Product definition template 4.14 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","31-34","Scaled value of second fixed surface",,"Operational"
717.00,"Product definition template 4.14 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","35","Derived forecast","(see Code table 4.7)#GRIB2_6_0_1_codeflag.doc#G2_CF47","Operational"
718.00,"Product definition template 4.14 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","36","Number of forecasts in the ensemble (N)",,"Operational"
719.00,"Product definition template 4.14 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","37","Cluster identifier",,"Operational"
720.00,"Product definition template 4.14 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","38","Number of cluster to which the high resolution control belongs",,"Operational"
721.00,"Product definition template 4.14 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","39","Number of cluster to which the low resolution control belongs",,"Operational"
722.00,"Product definition template 4.14 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","40","Total number of clusters",,"Operational"
723.00,"Product definition template 4.14 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","41","Clustering method","(see Code table 4.8)#GRIB2_6_0_1_codeflag.doc#G2_CF48","Operational"
724.00,"Product definition template 4.14 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","42-45","Latitude of central point in cluster domain",,"Operational"
725.00,"Product definition template 4.14 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","46-49","Longitude of central point in cluster domain",,"Operational"
726.00,"Product definition template 4.14 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","50-53","Radius of cluster domain",,"Operational"
727.00,"Product definition template 4.14 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","54","NC - number of forecasts in the cluster",,"Operational"
728.00,"Product definition template 4.14 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","55","Scale factor of standard deviation in the cluster",,"Operational"
729.00,"Product definition template 4.14 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","56-59","Scaled value of standard deviation in the cluster",,"Operational"
730.00,"Product definition template 4.14 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","60","Scale factor of distance of the cluster from ensemble mean",,"Operational"
731.00,"Product definition template 4.14 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","61-64","Scaled value of distance of the cluster from ensemble mean",,"Operational"
732.00,"Product definition template 4.14 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","65-66","Year of end of overall time interval",,"Operational"
733.00,"Product definition template 4.14 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","67","Month of end of overall time interval",,"Operational"
734.00,"Product definition template 4.14 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","68","Day of end of overall time interval",,"Operational"
735.00,"Product definition template 4.14 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","69","Hour of end of overall time interval",,"Operational"
736.00,"Product definition template 4.14 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","70","Minute of end of overall time interval",,"Operational"
737.00,"Product definition template 4.14 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","71","Second of end of overall time interval",,"Operational"
738.00,"Product definition template 4.14 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","72","n - number of time range specifications describing the time intervals used to calculate the statistically-processed field",,"Operational"
739.00,"Product definition template 4.14 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","73-76","Total number of data values missing in statistical process",,"Operational"
740.00,"Product definition template 4.14 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval",,"77-88   Specification of the outermost (or only) time range over which statistical processing is done",,"Operational"
741.00,"Product definition template 4.14 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","77","Statistical process used to calculate the processed field from the field at each time increment during the time range","(see Code table 4.10)#GRIB2_6_0_1_codeflag.doc#G2_CF410","Operational"
742.00,"Product definition template 4.14 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","78","Type of time increment between successive fields used in the statistical processing","(see Code table 4.11)#GRIB2_6_0_1_codeflag.doc#G2_CF411","Operational"
743.00,"Product definition template 4.14 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","79","Indicator of unit of time for time range over which statistical processing is done","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Operational"
744.00,"Product definition template 4.14 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","80-83","Length of the time range over which statistical processing is done, in units defined by the previous octet",,"Operational"
745.00,"Product definition template 4.14 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","84","Indicator of unit of time for the increment between the successive fields used","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Operational"
746.00,"Product definition template 4.14 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","85-88","Time increment between successive fields, in units defined by the previous octet","(see Notes 3 and 4)#GRIB2_6_0_1_temp.doc#G2_Pdt414n","Operational"
747.00,"Product definition template 4.14 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval",,"89-nn   These octets are included only if n>1, where nn = 76 + 12*n",,"Operational"
748.00,"Product definition template 4.14 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","89-110","As octets 77 to 88, next innermost step of processing",,"Operational"
749.00,"Product definition template 4.14 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","111-nn","Additional time range specifications, included in accordance with the value of n. Contents as octets 77 to 88, repeated as necessary",,"Operational"
750.00,"Product definition template 4.14 - derived forecasts based on a cluster of ensemble members over a circular area at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","(nn+1)-(nn+NC)","List of NC ensemble forecast numbers (NC is given in octet 54)",,"Operational"
751.00,"Product definition template 4.15 - average, accumulation, extreme values, or other statistically-processed values over a spatial area at a horizontal level or in a horizontal layer at a point in time","10","Parameter category","(see Code table 4.1)#GRIB2_6_0_1_codeflag.doc#G2_CF41","Operational"
752.00,"Product definition template 4.15 - average, accumulation, extreme values, or other statistically-processed values over a spatial area at a horizontal level or in a horizontal layer at a point in time","11","Parameter number","(see Code table 4.2)#GRIB2_6_0_1_codeflag.doc#G2_CF42","Operational"
753.00,"Product definition template 4.15 - average, accumulation, extreme values, or other statistically-processed values over a spatial area at a horizontal level or in a horizontal layer at a point in time","12","Type of generating process","(see Code table 4.3)#GRIB2_6_0_1_codeflag.doc#G2_CF43","Operational"
754.00,"Product definition template 4.15 - average, accumulation, extreme values, or other statistically-processed values over a spatial area at a horizontal level or in a horizontal layer at a point in time","13","Background generating process identifier (defined by originating centre)",,"Operational"
755.00,"Product definition template 4.15 - average, accumulation, extreme values, or other statistically-processed values over a spatial area at a horizontal level or in a horizontal layer at a point in time","14","Analysis or forecast generating processes identifier (defined by originating centre)",,"Operational"
756.00,"Product definition template 4.15 - average, accumulation, extreme values, or other statistically-processed values over a spatial area at a horizontal level or in a horizontal layer at a point in time","15-16","Hours of observational data cutoff after reference time","(see Note)#GRIB2_6_0_1_temp.doc#G2_Pdt415n","Operational"
757.00,"Product definition template 4.15 - average, accumulation, extreme values, or other statistically-processed values over a spatial area at a horizontal level or in a horizontal layer at a point in time","17","Minutes of observational data cutoff after reference time",,"Operational"
758.00,"Product definition template 4.15 - average, accumulation, extreme values, or other statistically-processed values over a spatial area at a horizontal level or in a horizontal layer at a point in time","18","Indicator of unit of time range","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Operational"
759.00,"Product definition template 4.15 - average, accumulation, extreme values, or other statistically-processed values over a spatial area at a horizontal level or in a horizontal layer at a point in time","19-22","Forecast time in units defined by octet 18",,"Operational"
760.00,"Product definition template 4.15 - average, accumulation, extreme values, or other statistically-processed values over a spatial area at a horizontal level or in a horizontal layer at a point in time","23","Type of first fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Operational"
761.00,"Product definition template 4.15 - average, accumulation, extreme values, or other statistically-processed values over a spatial area at a horizontal level or in a horizontal layer at a point in time","24","Scale factor of first fixed surface",,"Operational"
762.00,"Product definition template 4.15 - average, accumulation, extreme values, or other statistically-processed values over a spatial area at a horizontal level or in a horizontal layer at a point in time","25-28","Scaled value of first fixed surface",,"Operational"
763.00,"Product definition template 4.15 - average, accumulation, extreme values, or other statistically-processed values over a spatial area at a horizontal level or in a horizontal layer at a point in time","29","Type of second fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Operational"
764.00,"Product definition template 4.15 - average, accumulation, extreme values, or other statistically-processed values over a spatial area at a horizontal level or in a horizontal layer at a point in time","30","Scale factor of second fixed surface",,"Operational"
765.00,"Product definition template 4.15 - average, accumulation, extreme values, or other statistically-processed values over a spatial area at a horizontal level or in a horizontal layer at a point in time","31-34","Scaled value of second fixed surface",,"Operational"
766.00,"Product definition template 4.15 - average, accumulation, extreme values, or other statistically-processed values over a spatial area at a horizontal level or in a horizontal layer at a point in time","35","Statistical process used within the spatial area defined by octet 36","(see Code table 4.10)#GRIB2_6_0_1_codeflag.doc#G2_CF410","Operational"
767.00,"Product definition template 4.15 - average, accumulation, extreme values, or other statistically-processed values over a spatial area at a horizontal level or in a horizontal layer at a point in time","36","Type of spatial processing used to arrive at given data value from source data","(see Code table 4.15)#GRIB2_6_0_1_codeflag.doc#G2_CF415","Operational"
768.00,"Product definition template 4.15 - average, accumulation, extreme values, or other statistically-processed values over a spatial area at a horizontal level or in a horizontal layer at a point in time","37","Number of data points used in spatial processing defined in octet 36",,"Operational"
769.00,"Product definition template 4.20 - radar product","10","Parameter category","(see Code table 4.1)#GRIB2_6_0_1_codeflag.doc#G2_CF41","Operational"
770.00,"Product definition template 4.20 - radar product","11","Parameter number","(see Code table 4.2)#GRIB2_6_0_1_codeflag.doc#G2_CF42","Operational"
771.00,"Product definition template 4.20 - radar product","12","Type of generating process","(see Code table 4.3)#GRIB2_6_0_1_codeflag.doc#G2_CF43","Operational"
772.00,"Product definition template 4.20 - radar product","13","Number of radar sites used",,"Operational"
773.00,"Product definition template 4.20 - radar product","14","Indicator of unit of time range",,"Operational"
774.00,"Product definition template 4.20 - radar product","15-18","Site latitude (in 10**-6 degree)",,"Operational"
775.00,"Product definition template 4.20 - radar product","19-22","Site longitude (in 10**-6 degree)",,"Operational"
776.00,"Product definition template 4.20 - radar product","23-24","Site elevation (metres)",,"Operational"
777.00,"Product definition template 4.20 - radar product","25-28","Site ID (alphanumeric)",,"Operational"
778.00,"Product definition template 4.20 - radar product","29-30","Site ID (numeric)",,"Operational"
779.00,"Product definition template 4.20 - radar product","31","Operating mode","(see Code table 4.12)#GRIB2_6_0_1_codeflag.doc#G2_CF412","Operational"
780.00,"Product definition template 4.20 - radar product","32","Reflectivity calibration constant (tenths of dB)",,"Operational"
781.00,"Product definition template 4.20 - radar product","33","Quality control indicator","(see Code table 4.13)#GRIB2_6_0_1_codeflag.doc#G2_CF413","Operational"
782.00,"Product definition template 4.20 - radar product","34","Clutter filter indicator","(see Code table 4.14)#GRIB2_6_0_1_codeflag.doc#G2_CF414","Operational"
783.00,"Product definition template 4.20 - radar product","35","Constant antenna elevation angle (tenths of degree true)",,"Operational"
784.00,"Product definition template 4.20 - radar product","36-37","Accumulation interval (minutes)",,"Operational"
785.00,"Product definition template 4.20 - radar product","38","Reference reflectivity for echo top (dB)",,"Operational"
786.00,"Product definition template 4.20 - radar product","39-41","Range bin spacing (metres)",,"Operational"
787.00,"Product definition template 4.20 - radar product","42-43","Radial angular spacing (tenths of degree true)",,"Operational"
788.00,"Product definition template 4.30 - satellite product","10","Parameter category","(see Code table 4.1)#GRIB2_6_0_1_codeflag.doc#G2_CF41","Deprecated"
789.00,"Product definition template 4.30 - satellite product","11","Parameter number","(see Code table 4.2)#GRIB2_6_0_1_codeflag.doc#G2_CF42","Deprecated"
790.00,"Product definition template 4.30 - satellite product","12","Type of generating process","(see Code table 4.3)#GRIB2_6_0_1_codeflag.doc#G2_CF43","Deprecated"
791.00,"Product definition template 4.30 - satellite product","13","Observation generating process identifier (defined by originating centre)",,"Deprecated"
792.00,"Product definition template 4.30 - satellite product","14","Number of contributing spectral bands (NB)",,"Deprecated"
793.00,"Product definition template 4.30 - satellite product",,"Repeat the following 10 octets for each contributing band (nb = 1, NB)",,"Deprecated"
794.00,"Product definition template 4.30 - satellite product","(15+10(nb-1))-(16+10(nb-1))","Satellite series of band nb (code table defined by originating/generating centre)",,"Deprecated"
795.00,"Product definition template 4.30 - satellite product","(17+10(nb-1))-(18+10(nb-1))","Satellite numbers of band nb (code table defined by originating/generating centre)",,"Deprecated"
796.00,"Product definition template 4.30 - satellite product","(19+10(nb-1))","Instrument types of band nb (code table defined by originating/generating centre)",,"Deprecated"
797.00,"Product definition template 4.30 - satellite product","(20+10(nb-1))","Scale factor of central wave number of band nb",,"Deprecated"
798.00,"Product definition template 4.30 - satellite product","(21+10(nb-1))-(24+10(nb-1))","Scaled value of central wave number of band nb (units: m-1)",,"Deprecated"
799.00,"Product definition template 4.31 - satellite product","10","Parameter category","(see Code table 4.1)#GRIB2_6_0_1_codeflag.doc#G2_CF41","Operational"
800.00,"Product definition template 4.31 - satellite product","11","Parameter number","(see Code table 4.2)#GRIB2_6_0_1_codeflag.doc#G2_CF42","Operational"
801.00,"Product definition template 4.31 - satellite product","12","Type of generating process","(see Code table 4.3)#GRIB2_6_0_1_codeflag.doc#G2_CF43","Operational"
802.00,"Product definition template 4.31 - satellite product","13","Observation generating process identifier (defined by originating centres)",,"Operational"
803.00,"Product definition template 4.31 - satellite product","14","Number of contributing spectral bands (NB)",,"Operational"
804.00,"Product definition template 4.31 - satellite product",,"Repeat the following 11 octets for each contributing band (nb = 1, NB)",,"Operational"
805.00,"Product definition template 4.31 - satellite product","(15+11(nb-1))-(16+11(nb-1))","Satellite series of band nb (code table defined by originating/generating centre)",,"Operational"
806.00,"Product definition template 4.31 - satellite product","(17+11(nb-1))-(18+11(nb-1))","Satellite numbers of band nb (code table defined by originating/generating centre)",,"Operational"
807.00,"Product definition template 4.31 - satellite product","(19+11(nb-1))-(20+11(nb-1))","Instrument types of band nb (code table defined by originating/generating centre)",,"Operational"
808.00,"Product definition template 4.31 - satellite product","(21+11(nb-1))","Scale factor of central wave number of band nb",,"Operational"
809.00,"Product definition template 4.31 - satellite product","(22+11(nb-1))-(25+11(nb-1))","Scaled value of central wave number of band nb (units: m-1)",,"Operational"
810.00,"Product definition template 4.32 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for simulated (synthetic) satellite data","10","Parameter category","(see Code table 4.1)#GRIB2_6_0_1_codeflag.doc#G2_CF41","Validation"
811.00,"Product definition template 4.32 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for simulated (synthetic) satellite data","11","Parameter number","(see Code table 4.2)#GRIB2_6_0_1_codeflag.doc#G2_CF42","Validation"
812.00,"Product definition template 4.32 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for simulated (synthetic) satellite data","12","Type of generating process","(see Code table 4.3)#GRIB2_6_0_1_codeflag.doc#G2_CF43","Validation"
813.00,"Product definition template 4.32 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for simulated (synthetic) satellite data","13","Background generating process identifier (defined by originating centres)",,"Validation"
814.00,"Product definition template 4.32 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for simulated (synthetic) satellite data","14","Analysis or forecast generating process identified",,"Validation"
815.00,"Product definition template 4.32 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for simulated (synthetic) satellite data","15-16","Hours of observational data cutoff after reference time","(see Note)#GRIB2_6_0_1_temp.doc#G2_Pdt432n","Validation"
816.00,"Product definition template 4.32 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for simulated (synthetic) satellite data","17","Minutes of observational data cutoff after reference time","(see Note)#GRIB2_6_0_1_temp.doc#G2_Pdt432n","Validation"
817.00,"Product definition template 4.32 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for simulated (synthetic) satellite data","18","Indicator of unit of time range","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Validation"
818.00,"Product definition template 4.32 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for simulated (synthetic) satellite data","19-22","Forecast time in units defined by octet 18",,"Validation"
819.00,"Product definition template 4.32 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for simulated (synthetic) satellite data","23","Number of contributing spectral bands (NB)",,"Validation"
820.00,"Product definition template 4.32 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for simulated (synthetic) satellite data",,"Repeat the following 11 octets for each contributing band (nb = 1, NB)",,"Validation"
821.00,"Product definition template 4.32 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for simulated (synthetic) satellite data","(24+11(nb-1))-(25+11(nb-1))","Satellite series of band nb (Code table defined by originating/generating centre)",,"Validation"
822.00,"Product definition template 4.32 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for simulated (synthetic) satellite data","(26+11(nb-1))-(27+11(nb-1))","Satellite number of band nb (Code table defined by originating/generating centre)",,"Validation"
823.00,"Product definition template 4.32 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for simulated (synthetic) satellite data","(28+11(nb-1))-(29+11(nb-1))","Instrument types of band nb (Code table defined by originating/generating centre)",,"Validation"
824.00,"Product definition template 4.32 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for simulated (synthetic) satellite data","(30 +11(nb-1))","Scale factor of central wave number of band nb",,"Validation"
825.00,"Product definition template 4.32 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for simulated (synthetic) satellite data","(31+11(nb-1))-(34+11(nb-1))","Scaled value of central wave number of band nb (units: m-1)",,"Validation"
826.00,"Product definition template 4.40 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for atmospheric chemical constituents","10","Parameter category","(see Code table 4.1)#GRIB2_6_0_1_codeflag.doc#G2_CF41","Operational"
827.00,"Product definition template 4.40 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for atmospheric chemical constituents","11","Parameter number","(see Code table 4.2)#GRIB2_6_0_1_codeflag.doc#G2_CF42","Operational"
828.00,"Product definition template 4.40 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for atmospheric chemical constituents","12-13","Atmospheric chemical constituent type","(see Code table 4.230)#GRIB2_6_0_1_codeflag.doc#G2_CF4230","Operational"
829.00,"Product definition template 4.40 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for atmospheric chemical constituents","14","Type of generating process","(see Code table 4.3)#GRIB2_6_0_1_codeflag.doc#G2_CF43","Operational"
830.00,"Product definition template 4.40 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for atmospheric chemical constituents","15","Background generating process identifier (defined by originating centre)",,"Operational"
831.00,"Product definition template 4.40 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for atmospheric chemical constituents","16","Analysis or forecast generating process identifier (defined by originating centre)",,"Operational"
832.00,"Product definition template 4.40 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for atmospheric chemical constituents","17-18","Hours of observational data cutoff after reference time","(see Note)#GRIB2_6_0_1_temp.doc#G2_Pdt440n","Operational"
833.00,"Product definition template 4.40 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for atmospheric chemical constituents","19","Minutes of observational data cutoff after reference time",,"Operational"
834.00,"Product definition template 4.40 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for atmospheric chemical constituents","20","Indicator of unit of time range","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Operational"
835.00,"Product definition template 4.40 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for atmospheric chemical constituents","21-24","Forecast time in units defined by octet 20",,"Operational"
836.00,"Product definition template 4.40 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for atmospheric chemical constituents","25","Type of first fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Operational"
837.00,"Product definition template 4.40 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for atmospheric chemical constituents","26","Scale factor of first fixed surface",,"Operational"
838.00,"Product definition template 4.40 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for atmospheric chemical constituents","27-30","Scaled value of first fixed surface",,"Operational"
839.00,"Product definition template 4.40 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for atmospheric chemical constituents","31","Type of second fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Operational"
840.00,"Product definition template 4.40 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for atmospheric chemical constituents","32","Scale factor of second fixed surface",,"Operational"
841.00,"Product definition template 4.40 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for atmospheric chemical constituents","33-36","Scaled value of second fixed surface",,"Operational"
842.00,"Product definition template 4.41 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time for atmospheric chemical constituents","10","Parameter category","(see Code table 4.1)#GRIB2_6_0_1_codeflag.doc#G2_CF41","Operational"
843.00,"Product definition template 4.41 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time for atmospheric chemical constituents","11","Parameter number","(see Code table 4.2)#GRIB2_6_0_1_codeflag.doc#G2_CF42","Operational"
844.00,"Product definition template 4.41 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time for atmospheric chemical constituents","12-13","Atmospheric chemical constituent type","(see Code table 4.230)#GRIB2_6_0_1_codeflag.doc#G2_CF4230","Operational"
845.00,"Product definition template 4.41 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time for atmospheric chemical constituents","14","Type of generating process","(see Code table 4.3)#GRIB2_6_0_1_codeflag.doc#G2_CF43","Operational"
846.00,"Product definition template 4.41 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time for atmospheric chemical constituents","15","Background generating process identifier (defined by originating centre)",,"Operational"
847.00,"Product definition template 4.41 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time for atmospheric chemical constituents","16","Forecast generating process identifier (defined by originating centre)",,"Operational"
848.00,"Product definition template 4.41 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time for atmospheric chemical constituents","17-18","Hours after reference time of data cutoff","(see Note)#GRIB2_6_0_1_temp.doc#G2_Pdt441n","Operational"
849.00,"Product definition template 4.41 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time for atmospheric chemical constituents","19","Minutes after reference time of data cutoff",,"Operational"
850.00,"Product definition template 4.41 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time for atmospheric chemical constituents","20","Indicator of unit of time range","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Operational"
851.00,"Product definition template 4.41 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time for atmospheric chemical constituents","21-24","Forecast time in units defined by octet 20",,"Operational"
852.00,"Product definition template 4.41 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time for atmospheric chemical constituents","25","Type of first fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Operational"
853.00,"Product definition template 4.41 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time for atmospheric chemical constituents","26","Scale factor of first fixed surface",,"Operational"
854.00,"Product definition template 4.41 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time for atmospheric chemical constituents","27-30","Scaled value of first fixed surface",,"Operational"
855.00,"Product definition template 4.41 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time for atmospheric chemical constituents","31","Type of second fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Operational"
856.00,"Product definition template 4.41 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time for atmospheric chemical constituents","32","Scale factor of second fixed surface",,"Operational"
857.00,"Product definition template 4.41 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time for atmospheric chemical constituents","33-36","Scaled value of second fixed surface",,"Operational"
858.00,"Product definition template 4.41 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time for atmospheric chemical constituents","37","Type of ensemble forecast","(see Code table 4.6)#GRIB2_6_0_1_codeflag.doc#G2_CF46","Operational"
859.00,"Product definition template 4.41 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time for atmospheric chemical constituents","38","Perturbation number",,"Operational"
860.00,"Product definition template 4.41 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time for atmospheric chemical constituents","39","Number of forecasts in ensemble",,"Operational"
861.00,"Product definition template 4.42 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","10","Parameter category","(see Code table 4.1)#GRIB2_6_0_1_codeflag.doc#G2_CF41","Operational"
862.00,"Product definition template 4.42 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","11","Parameter number","(see Code table 4.2)#GRIB2_6_0_1_codeflag.doc#G2_CF42","Operational"
863.00,"Product definition template 4.42 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","12-13","Atmospheric chemical constituent type","(see Code table 4.230)#GRIB2_6_0_1_codeflag.doc#G2_CF4230","Operational"
864.00,"Product definition template 4.42 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","14","Type of generating process","(see Code table 4.3)#GRIB2_6_0_1_codeflag.doc#G2_CF43","Operational"
865.00,"Product definition template 4.42 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","15","Background generating process identifier (defined by originating centre)",,"Operational"
866.00,"Product definition template 4.42 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","16","Analysis or forecast generating process identifier (defined by originating centre)",,"Operational"
867.00,"Product definition template 4.42 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","17-18","Hours after reference time of data cutoff","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Pdt442n","Operational"
868.00,"Product definition template 4.42 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","19","Minutes after reference time of data cutoff",,"Operational"
869.00,"Product definition template 4.42 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","20","Indicator of unit of time range","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Operational"
870.00,"Product definition template 4.42 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","21-24","Forecast time in units defined by octet 20","(see Note 2)#GRIB2_6_0_1_temp.doc#G2_Pdt442n","Operational"
871.00,"Product definition template 4.42 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","25","Type of first fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Operational"
872.00,"Product definition template 4.42 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","26","Scale factor of first fixed surface",,"Operational"
873.00,"Product definition template 4.42 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","27-30","Scaled value of first fixed surface",,"Operational"
874.00,"Product definition template 4.42 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","31","Type of second fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Operational"
875.00,"Product definition template 4.42 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","32","Scale factor of second fixed surface",,"Operational"
876.00,"Product definition template 4.42 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","33-36","Scaled value of second fixed surface",,"Operational"
877.00,"Product definition template 4.42 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","37-38","Year",,"Operational"
878.00,"Product definition template 4.42 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","39","Month",,"Operational"
879.00,"Product definition template 4.42 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","40","Day",,"Operational"
880.00,"Product definition template 4.42 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","41","Hour",,"Operational"
881.00,"Product definition template 4.42 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","42","Minute",,"Operational"
882.00,"Product definition template 4.42 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","43","Second",,"Operational"
883.00,"Product definition template 4.42 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","44","n - number of time range specifications describing the time intervals used to calculate the statistically-processed field",,"Operational"
884.00,"Product definition template 4.42 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","45-48","Total number of data values missing in statistical process",,"Operational"
885.00,"Product definition template 4.42 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents",,"49-60   Specification of the outermost (or only) time range over which statistical processing is done",,"Operational"
886.00,"Product definition template 4.42 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","49","Statistical process used to calculate the processed field from the field at each time increment during the time range","(see Code table 4.10)#GRIB2_6_0_1_codeflag.doc#G2_CF410","Operational"
887.00,"Product definition template 4.42 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","50","Type of time increment between successive fields used in the statistical processing","(see Code table 4.11)#GRIB2_6_0_1_codeflag.doc#G2_CF411","Operational"
888.00,"Product definition template 4.42 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","51","Indicator of unit of time for time range over which statistical processing is done","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Operational"
889.00,"Product definition template 4.42 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","52-55","Length of the time range over which statistical processing is done, in units defined by the previous octet",,"Operational"
890.00,"Product definition template 4.42 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","56","Indicator of unit of time for the increment between the successive fields used","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Operational"
891.00,"Product definition template 4.42 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","57-60","Time increment between successive fields, in units defined by the previous octet","(see Notes 3 and 4)#GRIB2_6_0_1_temp.doc#G2_Pdt442n","Operational"
892.00,"Product definition template 4.42 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents",,"61-nn   These octets are included only if n>1, where nn = 48 + 12*n",,"Operational"
893.00,"Product definition template 4.42 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","61-72","As octets 49 to 60, next innermost step of processing",,"Operational"
894.00,"Product definition template 4.42 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","73-nn","Additional time range specifications, included in accordance with the value of n. Contents as octets 49 to 60, repeated as necessary.",,"Operational"
895.00,"Product definition template 4.43 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","10","Parameter category","(see Code table 4.1)#GRIB2_6_0_1_codeflag.doc#G2_CF41","Operational"
896.00,"Product definition template 4.43 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","11","Parameter number","(see Code table 4.2)#GRIB2_6_0_1_codeflag.doc#G2_CF42","Operational"
897.00,"Product definition template 4.43 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","12-13","Atmospheric chemical constituent type","(see Code table 4.230)#GRIB2_6_0_1_codeflag.doc#G2_CF4230","Operational"
898.00,"Product definition template 4.43 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","14","Type of generating process","(see Code table 4.3)#GRIB2_6_0_1_codeflag.doc#G2_CF43","Operational"
899.00,"Product definition template 4.43 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","15","Background generating process identifier (defined by originating centre)",,"Operational"
900.00,"Product definition template 4.43 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","16","Forecast generating process identifier (defined by originating centre)",,"Operational"
901.00,"Product definition template 4.43 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","17-18","Hours after reference time of data cutoff","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Pdt443n","Operational"
902.00,"Product definition template 4.43 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","19","Minutes after reference time of data cutoff",,"Operational"
903.00,"Product definition template 4.43 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","20","Indicator of unit of time range","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Operational"
904.00,"Product definition template 4.43 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","21-24","Forecast time in units defined by octet 20","(see Note 2)#GRIB2_6_0_1_temp.doc#G2_Pdt443n","Operational"
905.00,"Product definition template 4.43 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","25","Type of first fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Operational"
906.00,"Product definition template 4.43 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","26","Scale factor of first fixed surface",,"Operational"
907.00,"Product definition template 4.43 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","27-30","Scaled value of first fixed surface",,"Operational"
908.00,"Product definition template 4.43 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","31","Type of second fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Operational"
909.00,"Product definition template 4.43 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","32","Scale factor of second fixed surface",,"Operational"
910.00,"Product definition template 4.43 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","33-36","Scaled value of second fixed surface",,"Operational"
911.00,"Product definition template 4.43 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","37","Type of ensemble forecast","(see Code table 4.6)#GRIB2_6_0_1_codeflag.doc#G2_CF46","Operational"
912.00,"Product definition template 4.43 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","38","Perturbation number",,"Operational"
913.00,"Product definition template 4.43 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","39","Number of forecasts in ensemble",,"Operational"
914.00,"Product definition template 4.43 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","40-41","Year of end of overall time interval",,"Operational"
915.00,"Product definition template 4.43 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","42","Month of end of overall time interval",,"Operational"
916.00,"Product definition template 4.43 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","43","Day of end of overall time interval",,"Operational"
917.00,"Product definition template 4.43 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","44","Hour of end of overall time interval",,"Operational"
918.00,"Product definition template 4.43 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","45","Minute of end of overall time interval",,"Operational"
919.00,"Product definition template 4.43 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","46","Second of end of overall time interval",,"Operational"
920.00,"Product definition template 4.43 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","47","n - number of time range specifications describing the time intervals used to calculate the statistically-processed field",,"Operational"
921.00,"Product definition template 4.43 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","48-51","Total number of data values missing in statistical process",,"Operational"
922.00,"Product definition template 4.43 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents",,"52-63   Specification of the outermost (or only) time range over which statistical processing is done",,"Operational"
923.00,"Product definition template 4.43 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","52","Statistical process used to calculate the processed field from the field at each time increment during the time range","(see Code table 4.10)#GRIB2_6_0_1_codeflag.doc#G2_CF410","Operational"
924.00,"Product definition template 4.43 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","53","Type of time increment between successive fields used in the statistical processing","(see Code table 4.11)#GRIB2_6_0_1_codeflag.doc#G2_CF411","Operational"
925.00,"Product definition template 4.43 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","54","Indicator of unit of time for time range over which statistical processing is done","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Operational"
926.00,"Product definition template 4.43 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","55-58","Length of the time range over which statistical processing is done, in units defined by the previous octet",,"Operational"
927.00,"Product definition template 4.43 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","59","Indicator of unit of time for the increment between the successive fields used","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Operational"
928.00,"Product definition template 4.43 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","60-63","Time increment between successive fields, in units defined by the previous octet","(see Notes 3 and 4)#GRIB2_6_0_1_temp.doc#G2_Pdt443n","Operational"
929.00,"Product definition template 4.43 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents",,"64-nn   These octets are included only if n>1, where nn = 51 + 12*n",,"Operational"
930.00,"Product definition template 4.43 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","64-75","As octets 52 to 63, next innermost step of processing",,"Operational"
931.00,"Product definition template 4.43 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for atmospheric chemical constituents","76-nn","Additional time range specifications, included in accordance with the value of n. Contents as octets 52 to 63, repeated as necessary.",,"Operational"
932.00,"Product definition template 4.44 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for aerosol","10","Parameter category","(see Code table 4.1).#GRIB2_6_0_1_codeflag.doc#G2_CF41","Validation"
933.00,"Product definition template 4.44 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for aerosol","11","Parameter number","(see Code table 4.2).#GRIB2_6_0_1_codeflag.doc#G2_CF42","Validation"
934.00,"Product definition template 4.44 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for aerosol","12-13","Aerosol type","(see Code table 4.233)#GRIB2_6_0_1_codeflag.doc#G2_CF4233","Validation"
935.00,"Product definition template 4.44 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for aerosol","14","Type of interval for first and second size","(see Code table 4.91)#GRIB2_6_0_1_codeflag.doc#G2_CF491","Validation"
936.00,"Product definition template 4.44 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for aerosol","15","Scale factor of first size",,"Validation"
937.00,"Product definition template 4.44 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for aerosol","16-19","Scaled value of first size in meters",,"Validation"
938.00,"Product definition template 4.44 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for aerosol","20","Scale factor of second size",,"Validation"
939.00,"Product definition template 4.44 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for aerosol","21-24","Scaled value of second size in meters",,"Validation"
940.00,"Product definition template 4.44 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for aerosol","25","Type of generating process","(see Code table 4.3)#GRIB2_6_0_1_codeflag.doc#G2_CF43","Validation"
941.00,"Product definition template 4.44 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for aerosol","26","Background generating process identifier (defined by originating centre)",,"Validation"
942.00,"Product definition template 4.44 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for aerosol","27","Analysis or forecast generating processes identifier (defined by originating centre)",,"Validation"
943.00,"Product definition template 4.44 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for aerosol","28-29","Hours of observational data cutoff after reference time","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Pdt444n","Validation"
944.00,"Product definition template 4.44 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for aerosol","30","Minutes of observational data cutoff after reference time",,"Validation"
945.00,"Product definition template 4.44 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for aerosol","31","Indicator of unit of time range","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Validation"
946.00,"Product definition template 4.44 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for aerosol","32-33","Forecast time in units defined by octet 18",,"Validation"
947.00,"Product definition template 4.44 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for aerosol","34","Type of first fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Validation"
948.00,"Product definition template 4.44 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for aerosol","35","Scale factor of first fixed surface",,"Validation"
949.00,"Product definition template 4.44 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for aerosol","36-39","Scaled value of first fixed surface",,"Validation"
950.00,"Product definition template 4.44 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for aerosol","40","Type of second fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Validation"
951.00,"Product definition template 4.44 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for aerosol","41","Scale factor of second fixed surface",,"Validation"
952.00,"Product definition template 4.44 - analysis or forecast at a horizontal level or in a horizontal layer at a point in time for aerosol","42-45","Scaled value of second fixed surface",,"Validation"
953.00,"Product definition template 4.45 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time for aerosol","10","Parameter category","(see Code table 4.1)#GRIB2_6_0_1_codeflag.doc#G2_CF41","Validation"
954.00,"Product definition template 4.45 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time for aerosol","11","Parameter number","(see Code table 4.2)#GRIB2_6_0_1_codeflag.doc#G2_CF42","Validation"
955.00,"Product definition template 4.45 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time for aerosol","12-13","Aerosol type","(see Code table 4.233)#GRIB2_6_0_1_codeflag.doc#G2_CF4233","Validation"
956.00,"Product definition template 4.45 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time for aerosol","14","Type of interval for first and second size","(see Code table 4.91)#GRIB2_6_0_1_codeflag.doc#G2_CF491","Validation"
957.00,"Product definition template 4.45 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time for aerosol","15","Scale factor of first size",,"Validation"
958.00,"Product definition template 4.45 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time for aerosol","16-19","Scaled value of first size in meters",,"Validation"
959.00,"Product definition template 4.45 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time for aerosol","20","Scale factor of second size",,"Validation"
960.00,"Product definition template 4.45 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time for aerosol","21-24","Scaled value of second size in meters",,"Validation"
961.00,"Product definition template 4.45 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time for aerosol","25","Type of generating process","(see Code table 4.3)#GRIB2_6_0_1_codeflag.doc#G2_CF43","Validation"
962.00,"Product definition template 4.45 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time for aerosol","26","Background generating process identifier (defined by originating centre)",,"Validation"
963.00,"Product definition template 4.45 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time for aerosol","27","Forecast generating process identifier (defined by originating centre)",,"Validation"
964.00,"Product definition template 4.45 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time for aerosol","28-29","Hours after reference time of data cutoff","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Pdt445n","Validation"
965.00,"Product definition template 4.45 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time for aerosol","30","Minutes after reference time of data cutoff",,"Validation"
966.00,"Product definition template 4.45 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time for aerosol","31","Indicator of unit of time range","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Validation"
967.00,"Product definition template 4.45 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time for aerosol","32-35","Forecast time in units defined by octet 18",,"Validation"
968.00,"Product definition template 4.45 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time for aerosol","36","Type of first fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Validation"
969.00,"Product definition template 4.45 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time for aerosol","37","Scale factor of first fixed surface",,"Validation"
970.00,"Product definition template 4.45 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time for aerosol","38-41","Scaled value of first fixed surface",,"Validation"
971.00,"Product definition template 4.45 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time for aerosol","42","Type of second fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Validation"
972.00,"Product definition template 4.45 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time for aerosol","43","Scale factor of second fixed surface",,"Validation"
973.00,"Product definition template 4.45 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time for aerosol","44-47","Scaled value of second fixed surface",,"Validation"
974.00,"Product definition template 4.45 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time for aerosol","48","Type of ensemble forecast","(see Code table 4.6)#GRIB2_6_0_1_codeflag.doc#G2_CF46","Validation"
975.00,"Product definition template 4.45 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time for aerosol","49","Perturbation number",,"Validation"
976.00,"Product definition template 4.45 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer at a point in time for aerosol","50","Number of forecasts in ensemble",,"Validation"
977.00,"Product definition template 4.46 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","10","Parameter category","(see Code table 4.1)#GRIB2_6_0_1_codeflag.doc#G2_CF41","Validation"
978.00,"Product definition template 4.46 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","11","Parameter number","(see Code table 4.2)#GRIB2_6_0_1_codeflag.doc#G2_CF42","Validation"
979.00,"Product definition template 4.46 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","12-13","Aerosol type","(see Code table 4.233)#GRIB2_6_0_1_codeflag.doc#G2_CF4233","Validation"
980.00,"Product definition template 4.46 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","14","Type of interval for first and second size","(see Code table 4.91)#GRIB2_6_0_1_codeflag.doc#G2_CF491","Validation"
981.00,"Product definition template 4.46 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","15","Scale factor of first size",,"Validation"
982.00,"Product definition template 4.46 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","16-19","Scaled value of first size in meters",,"Validation"
983.00,"Product definition template 4.46 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","20","Scale factor of second size",,"Validation"
984.00,"Product definition template 4.46 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","21-24","Scaled value of second size in meters",,"Validation"
985.00,"Product definition template 4.46 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","25","Type of generating process","(see Code table 4.3)#GRIB2_6_0_1_codeflag.doc#G2_CF43","Validation"
986.00,"Product definition template 4.46 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","26","Background generating process identifier (defined by originating centre)",,"Validation"
987.00,"Product definition template 4.46 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","27","Analysis or forecast generating process identifier (defined by originating centre)",,"Validation"
988.00,"Product definition template 4.46 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","28-29","Hours after reference time of data cutoff","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Pdt446n","Validation"
989.00,"Product definition template 4.46 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","30","Minutes after reference time of data cutoff",,"Validation"
990.00,"Product definition template 4.46 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","31","Indicator of unit of time range","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Validation"
991.00,"Product definition template 4.46 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","32-35","Forecast time in units defined by octet 18","(see Note 2)#GRIB2_6_0_1_temp.doc#G2_Pdt446","Validation"
992.00,"Product definition template 4.46 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","36","Type of first fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Validation"
993.00,"Product definition template 4.46 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","37","Scale factor of first fixed surface",,"Validation"
994.00,"Product definition template 4.46 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","38-41","Scaled value of first fixed surface",,"Validation"
995.00,"Product definition template 4.46 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","42","Type of second fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Validation"
996.00,"Product definition template 4.46 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","43","Scale factor of second fixed surface",,"Validation"
997.00,"Product definition template 4.46 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","44-47","Scaled value of second fixed surface",,"Validation"
998.00,"Product definition template 4.46 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","48-49","Year - time of end of overall time interval",,"Validation"
999.00,"Product definition template 4.46 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","50","Month - time of end of overall time interval",,"Validation"
1000.00,"Product definition template 4.46 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","51","Day - time of end of overall time interval",,"Validation"
1001.00,"Product definition template 4.46 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","52","Hour - time of end of overall time interval",,"Validation"
1002.00,"Product definition template 4.46 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","53","Minute - time of end of overall time interval",,"Validation"
1003.00,"Product definition template 4.46 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","54","Second - time of end of overall time interval",,"Validation"
1004.00,"Product definition template 4.46 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","55","n - number of time range specifications describing the time intervals used to calculate the statistically-processed field",,"Validation"
1005.00,"Product definition template 4.46 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","56-59","Total number of data values missing in statistical process.",,"Validation"
1006.00,"Product definition template 4.46 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol",,"60-71   Specification of the outermost (or only) time range over which statistical processing is done",,"Validation"
1007.00,"Product definition template 4.46 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","60","Statistical process used to calculate the processed field from the field at each time increment during the time range","(see Code table 4.10)#GRIB2_6_0_1_codeflag.doc#G2_CF410","Validation"
1008.00,"Product definition template 4.46 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","61","Type of time increment between successive fields used in the statistical processing","(see Code table 4.11)#GRIB2_6_0_1_codeflag.doc#G2_CF411","Validation"
1009.00,"Product definition template 4.46 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","62","Indicator of unit of time for time range over which statistical processing is done","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Validation"
1010.00,"Product definition template 4.46 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","63-66","Length of the time range over which statistical processing is done, in units defined by the previous octet",,"Validation"
1011.00,"Product definition template 4.46 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","67","Indicator of unit of time for the increment between the successive fields used","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Validation"
1012.00,"Product definition template 4.46 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","68-71","Time increment between successive fields, in units defined by the previous octet","(see Notes 3 and 4)#GRIB2_6_0_1_temp.doc#G2_Pdt446n","Validation"
1013.00,"Product definition template 4.46 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol",,"72-nn   These octets are included only if n>1, where nn = 59 + 12*n",,"Validation"
1014.00,"Product definition template 4.46 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","72-83","As octets 60 to 71, next innermost step of processing",,"Validation"
1015.00,"Product definition template 4.46 - average, accumulation, and/or extreme values or other statistically-processed values at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","84-nn","Additional time range specifications, included in accordance with the value of n.  Contents as octets 60 to 71, repeated as necessary.",,"Validation"
1016.00,"Product definition template 4.47 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","10","Parameter category","(see Code table 4.1)#GRIB2_6_0_1_codeflag.doc#G2_CF41","Validation"
1017.00,"Product definition template 4.47 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","11","Parameter number","(see Code table 4.2)#GRIB2_6_0_1_codeflag.doc#G2_CF42","Validation"
1018.00,"Product definition template 4.47 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","12","Type of generating process","(see Code table 4.3)#GRIB2_6_0_1_codeflag.doc#G2_CF43","Validation"
1019.00,"Product definition template 4.47 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","13-14","Aerosol type","(see Code table 4.233)#GRIB2_6_0_1_codeflag.doc#G2_CF4233","Validation"
1020.00,"Product definition template 4.47 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","15","Type of interval for first and second size","(see Code table 4.91)#GRIB2_6_0_1_codeflag.doc#G2_CF491","Validation"
1021.00,"Product definition template 4.47 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","16","Scale factor of first size",,"Validation"
1022.00,"Product definition template 4.47 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","17-20","Scaled value of first size in meters",,"Validation"
1023.00,"Product definition template 4.47 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","21","Scale factor of second size",,"Validation"
1024.00,"Product definition template 4.47 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","22-25","Scaled value of second size in meters",,"Validation"
1025.00,"Product definition template 4.47 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","26","Background generating process identifier (defined by originating centre)",,"Validation"
1026.00,"Product definition template 4.47 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","27","Forecast generating process identifier (defined by originating centre)",,"Validation"
1027.00,"Product definition template 4.47 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","28-29","Hours after reference time of data cutoff","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Pdt447n","Validation"
1028.00,"Product definition template 4.47 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","30","Minutes after reference time of data cutoff",,"Validation"
1029.00,"Product definition template 4.47 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","31","Indicator of unit of time range","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Validation"
1030.00,"Product definition template 4.47 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","32-35","Forecast time in units defined by octet 18","(see Note 2)#GRIB2_6_0_1_temp.doc#G2_Pdt447n","Validation"
1031.00,"Product definition template 4.47 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","36","Type of first fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Validation"
1032.00,"Product definition template 4.47 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","37","Scale factor of first fixed surface",,"Validation"
1033.00,"Product definition template 4.47 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","38-41","Scaled value of first fixed surface",,"Validation"
1034.00,"Product definition template 4.47 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","42","Type of second fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Validation"
1035.00,"Product definition template 4.47 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","43","Scale factor of second fixed surface",,"Validation"
1036.00,"Product definition template 4.47 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","44-47","Scaled value of second fixed surface",,"Validation"
1037.00,"Product definition template 4.47 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","48","Type of ensemble forecast","(see Code table 4.6)#GRIB2_6_0_1_codeflag.doc#G2_CF46","Validation"
1038.00,"Product definition template 4.47 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","49","Perturbation number",,"Validation"
1039.00,"Product definition template 4.47 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","50","Number of forecasts in ensemble",,"Validation"
1040.00,"Product definition template 4.47 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","51-52","Year of end of overall time interval",,"Validation"
1041.00,"Product definition template 4.47 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","53","Month of end of overall time interval",,"Validation"
1042.00,"Product definition template 4.47 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","54","Day of end of overall time interval",,"Validation"
1043.00,"Product definition template 4.47 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","55","Hour of end of overall time interval",,"Validation"
1044.00,"Product definition template 4.47 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","56","Minute of end of overall time interval",,"Validation"
1045.00,"Product definition template 4.47 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","57","Second of end of overall time interval",,"Validation"
1046.00,"Product definition template 4.47 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","58","n - number of time range specifications describing the time intervals used to calculate the statistically-processed field",,"Validation"
1047.00,"Product definition template 4.47 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","59-62","Total number of data values missing in statistical process",,"Validation"
1048.00,"Product definition template 4.47 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol",,"63-74   Specification of the outermost (or only) time range over which statistical processing is done",,"Validation"
1049.00,"Product definition template 4.47 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","63","Statistical process used to calculate the processed field from the field at each time increment during the time range","(see Code table 4.10)#GRIB2_6_0_1_codeflag.doc#G2_CF410","Validation"
1050.00,"Product definition template 4.47 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","64","Type of time increment between successive fields used in the statistical processing","(see Code table 4.11)#GRIB2_6_0_1_codeflag.doc#G2_CF411","Validation"
1051.00,"Product definition template 4.47 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","65","Indicator of unit of time for time range over which statistical processing is done","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Validation"
1052.00,"Product definition template 4.47 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","66-69","Length of the time range over which statistical processing is done, in units defined by the previous octet",,"Validation"
1053.00,"Product definition template 4.47 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","70","Indicator of unit of time for the increment between the successive fields used","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Validation"
1054.00,"Product definition template 4.47 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","71-74","Time increment between successive fields, in units defined by the previous octet","(see Note 3)#GRIB2_6_0_1_temp.doc#G2_Pdt447n","Validation"
1055.00,"Product definition template 4.47 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol",,"75-nn   These octets are included only if n>1, where nn = 62 + 12*n",,"Validation"
1056.00,"Product definition template 4.47 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","75-86","As octets 63 to 74, next innermost step of processing",,"Validation"
1057.00,"Product definition template 4.47 - individual ensemble forecast, control and perturbed, at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval for aerosol","87-nn","Additional time range specifications, included in accordance with the value of n. Contents as octets 62 to 73, repeated as necessary",,"Validation"
1058.00,"Product definition template 4.50 - analysis or forecast of a multi component parameter or matrix element at a point in time","10","Parameter category","(see Code table 4.1)#GRIB2_6_0_1_codeflag.doc#G2_CF41","Validation"
1059.00,"Product definition template 4.50 - analysis or forecast of a multi component parameter or matrix element at a point in time","11","Parameter number","(see Code table 4.2)#GRIB2_6_0_1_codeflag.doc#G2_CF42","Validation"
1060.00,"Product definition template 4.50 - analysis or forecast of a multi component parameter or matrix element at a point in time","12","Type of generating process","(see Code table 4.3)#GRIB2_6_0_1_codeflag.doc#G2_CF43","Validation"
1061.00,"Product definition template 4.50 - analysis or forecast of a multi component parameter or matrix element at a point in time","13","Background generating process identifier (defined by originating centre)",,"Validation"
1062.00,"Product definition template 4.50 - analysis or forecast of a multi component parameter or matrix element at a point in time","14","Analysis or forecast generating processes identifier (defined by originating centre)",,"Validation"
1063.00,"Product definition template 4.50 - analysis or forecast of a multi component parameter or matrix element at a point in time","15-16","Hours of observational data cutoff after reference time","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Pdt450n","Validation"
1064.00,"Product definition template 4.50 - analysis or forecast of a multi component parameter or matrix element at a point in time","17","Minutes of observational data cutoff after reference time",,"Validation"
1065.00,"Product definition template 4.50 - analysis or forecast of a multi component parameter or matrix element at a point in time","18","Indicator of unit of time range","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Validation"
1066.00,"Product definition template 4.50 - analysis or forecast of a multi component parameter or matrix element at a point in time","19-22","Forecast time in units defined by octet 18",,"Validation"
1067.00,"Product definition template 4.50 - analysis or forecast of a multi component parameter or matrix element at a point in time","23","Type of first fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Validation"
1068.00,"Product definition template 4.50 - analysis or forecast of a multi component parameter or matrix element at a point in time","24","Scale factor of first fixed surface",,"Validation"
1069.00,"Product definition template 4.50 - analysis or forecast of a multi component parameter or matrix element at a point in time","25-28","Scaled value of first fixed surface",,"Validation"
1070.00,"Product definition template 4.50 - analysis or forecast of a multi component parameter or matrix element at a point in time","29","Type of second fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Validation"
1071.00,"Product definition template 4.50 - analysis or forecast of a multi component parameter or matrix element at a point in time","30","Scale factor of second fixed surface",,"Validation"
1072.00,"Product definition template 4.50 - analysis or forecast of a multi component parameter or matrix element at a point in time","31-34","Scaled value of second fixed surface",,"Validation"
1073.00,"Product definition template 4.50 - analysis or forecast of a multi component parameter or matrix element at a point in time","35","First dimension physical significance","(Code table 5.3)  (see Note 2)G2_Pdt45n#http://(Code table 5.3)  (see Note 2)#GRIB2_6_0_1_temp.doc#G2_Pdt45n#","Validation"
1074.00,"Product definition template 4.50 - analysis or forecast of a multi component parameter or matrix element at a point in time","36","Second dimension physical significance","(Code table 5.3)  (see Note 2)G2_Pdt45n#http://(Code table 5.3)  (see Note 2)#GRIB2_6_0_1_temp.doc#G2_Pdt45n#","Validation"
1075.00,"Product definition template 4.50 - analysis or forecast of a multi component parameter or matrix element at a point in time","37-40","First dimension coordinate value (IEEE 32-bit floating-point value)",,"Validation"
1076.00,"Product definition template 4.50 - analysis or forecast of a multi component parameter or matrix element at a point in time","41-44","Second dimension coordinate value (IEEE 32-bit floating-point value)",,"Validation"
1077.00,"Product definition template 4.50 - analysis or forecast of a multi component parameter or matrix element at a point in time","45-48","First dimension (rows) of the complete matrix","(see Note 3)#GRIB2_6_0_1_temp.doc#G2_Pdt450n","Validation"
1078.00,"Product definition template 4.50 - analysis or forecast of a multi component parameter or matrix element at a point in time","49-52","Second dimension (columns) of the complete matrix","(see Note 3)#GRIB2_6_0_1_temp.doc#G2_Pdt450n","Validation"
1079.00,"Product definition template 4.51 - categorical forecasts at a horizontal level or in a horizontal layer at a point in time","10","Parameter category","(see Code table 4.1)#GRIB2_6_0_1_codeflag.doc#G2_CF41","Validation"
1080.00,"Product definition template 4.51 - categorical forecasts at a horizontal level or in a horizontal layer at a point in time","11","Parameter number","(see Code table 4.2)#GRIB2_6_0_1_codeflag.doc#G2_CF42","Validation"
1081.00,"Product definition template 4.51 - categorical forecasts at a horizontal level or in a horizontal layer at a point in time","12","Type of generating process","(see Code table 4.3)#GRIB2_6_0_1_codeflag.doc#G2_CF43","Validation"
1082.00,"Product definition template 4.51 - categorical forecasts at a horizontal level or in a horizontal layer at a point in time","13","Background generating process identifier (defined by originating centre)",,"Validation"
1083.00,"Product definition template 4.51 - categorical forecasts at a horizontal level or in a horizontal layer at a point in time","14","Forecast generating process identifier (defined by originating centre)",,"Validation"
1084.00,"Product definition template 4.51 - categorical forecasts at a horizontal level or in a horizontal layer at a point in time","15-16","Hours after reference time of data cutoff","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Pdt451n","Validation"
1085.00,"Product definition template 4.51 - categorical forecasts at a horizontal level or in a horizontal layer at a point in time","17","Minutes after reference time of data cutoff",,"Validation"
1086.00,"Product definition template 4.51 - categorical forecasts at a horizontal level or in a horizontal layer at a point in time","18","Indicator of unit of time range","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Validation"
1087.00,"Product definition template 4.51 - categorical forecasts at a horizontal level or in a horizontal layer at a point in time","19-22","Forecast time in units defined by octet 18",,"Validation"
1088.00,"Product definition template 4.51 - categorical forecasts at a horizontal level or in a horizontal layer at a point in time","23","Type of first fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Validation"
1089.00,"Product definition template 4.51 - categorical forecasts at a horizontal level or in a horizontal layer at a point in time","24","Scale factor of first fixed surface",,"Validation"
1090.00,"Product definition template 4.51 - categorical forecasts at a horizontal level or in a horizontal layer at a point in time","25-28","Scaled value of first fixed surface",,"Validation"
1091.00,"Product definition template 4.51 - categorical forecasts at a horizontal level or in a horizontal layer at a point in time","29","Type of second fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Validation"
1092.00,"Product definition template 4.51 - categorical forecasts at a horizontal level or in a horizontal layer at a point in time","30","Scale factor of second fixed surface",,"Validation"
1093.00,"Product definition template 4.51 - categorical forecasts at a horizontal level or in a horizontal layer at a point in time","31-34","Scaled value of second fixed surface",,"Validation"
1094.00,"Product definition template 4.51 - categorical forecasts at a horizontal level or in a horizontal layer at a point in time","35","NC - number of categories",,"Validation"
1095.00,"Product definition template 4.51 - categorical forecasts at a horizontal level or in a horizontal layer at a point in time",,"Repeat the following 12 octets for each category (i = 1,NC)",,"Validation"
1096.00,"Product definition template 4.51 - categorical forecasts at a horizontal level or in a horizontal layer at a point in time","(36+12(i-1))","Code figure",,"Validation"
1097.00,"Product definition template 4.51 - categorical forecasts at a horizontal level or in a horizontal layer at a point in time","(37+12(i-1))","Type of interval for first and second limit","(see Code table 4.91)#GRIB2_6_0_1_codeflag.doc#G2_CF491","Validation"
1098.00,"Product definition template 4.51 - categorical forecasts at a horizontal level or in a horizontal layer at a point in time","(38+12(i-1))","Scale factor of first limit",,"Validation"
1099.00,"Product definition template 4.51 - categorical forecasts at a horizontal level or in a horizontal layer at a point in time","(39+12(i-1))-(42+12(i-1))","Scaled value of first limit",,"Validation"
1100.00,"Product definition template 4.51 - categorical forecasts at a horizontal level or in a horizontal layer at a point in time","(43+12(i-1))","Scale factor of second limit",,"Validation"
1101.00,"Product definition template 4.51 - categorical forecasts at a horizontal level or in a horizontal layer at a point in time","(44+12(i-1))-(47+12(i-1))","Scaled value of second limit",,"Validation"
1102.00,"Product definition template 4.91 - categorical forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval"," 10","Parameter category","(see Code table 4.1)#GRIB2_6_0_1_codeflag.doc#G2_CF41","Validation"
1103.00,"Product definition template 4.91 - categorical forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval"," 11","Parameter number","(see Code table 4.2)#GRIB2_6_0_1_codeflag.doc#G2_CF42","Validation"
1104.00,"Product definition template 4.91 - categorical forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval"," 12","Type of generating process","(see Code table 4.3)#GRIB2_6_0_1_codeflag.doc#G2_CF43","Validation"
1105.00,"Product definition template 4.91 - categorical forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval"," 13","Background generating process identifier (defined by originating centre)",,"Validation"
1106.00,"Product definition template 4.91 - categorical forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval"," 14","Forecast generating process identifier (defined by originating centre)",,"Validation"
1107.00,"Product definition template 4.91 - categorical forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval"," 15-16","Hours after reference time of data cutoff","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Pdt491n","Validation"
1108.00,"Product definition template 4.91 - categorical forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval"," 17","Minutes after reference time of data cutoff",,"Validation"
1109.00,"Product definition template 4.91 - categorical forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval"," 18","Indicator of unit of time range","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Validation"
1110.00,"Product definition template 4.91 - categorical forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval"," 19-22","Forecast time in units defined by octet 18","(see Note 2)#GRIB2_6_0_1_temp.doc#G2_Pdt491n","Validation"
1111.00,"Product definition template 4.91 - categorical forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval"," 23","Type of first fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Validation"
1112.00,"Product definition template 4.91 - categorical forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval"," 24","Scale factor of first fixed surface",,"Validation"
1113.00,"Product definition template 4.91 - categorical forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval"," 25-28","Scaled value of first fixed surface",,"Validation"
1114.00,"Product definition template 4.91 - categorical forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval"," 29","Type of second fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Validation"
1115.00,"Product definition template 4.91 - categorical forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval"," 30","Scale factor of second fixed surface",,"Validation"
1116.00,"Product definition template 4.91 - categorical forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval"," 31-34","Scaled value of second fixed surface",,"Validation"
1117.00,"Product definition template 4.91 - categorical forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval"," 35","NC - number of categories",,"Validation"
1118.00,"Product definition template 4.91 - categorical forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval",,"Repeat the following 12 octets for each category (i = 1,NC)",,"Validation"
1119.00,"Product definition template 4.91 - categorical forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","(36+12(i-1))","Code figure",,"Validation"
1120.00,"Product definition template 4.91 - categorical forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","(37+12(i-1))","Type of interval for first and second limit","(see Code table 4.91)#GRIB2_6_0_1_codeflag.doc#G2_CF491","Validation"
1121.00,"Product definition template 4.91 - categorical forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","(38+12(i-1))","Scale factor of first limit",,"Validation"
1122.00,"Product definition template 4.91 - categorical forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","(39+12(i-1))-(42+12(i-1))","Scaled value of first limit",,"Validation"
1123.00,"Product definition template 4.91 - categorical forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","(43+12(i-1))","Scale factor of second limit",,"Validation"
1124.00,"Product definition template 4.91 - categorical forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","(44+12(i-1))-(47+12(i-1))","Scaled value of second limit",,"Validation"
1125.00,"Product definition template 4.91 - categorical forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","(48+12(NC-1))-(49+12(NC-1))","Year of end of overall time interval",,"Validation"
1126.00,"Product definition template 4.91 - categorical forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","(50+12(NC-1))","Month of end of overall time interval",,"Validation"
1127.00,"Product definition template 4.91 - categorical forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","(51+12(NC-1))","Day of end of overall time interval",,"Validation"
1128.00,"Product definition template 4.91 - categorical forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","(52+12(NC-1))","Hour of end of overall time interval",,"Validation"
1129.00,"Product definition template 4.91 - categorical forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","(53+12(NC-1))","Minute of end of overall time interval",,"Validation"
1130.00,"Product definition template 4.91 - categorical forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","(54+12(NC-1))","Second of end of overall time interval",,"Validation"
1131.00,"Product definition template 4.91 - categorical forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","(55+12(NC-1))","n - number of time range specifications describing the time intervals used to calculate the statistically-processed field",,"Validation"
1132.00,"Product definition template 4.91 - categorical forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","(56+12(NC-1))-(59+12(NC-1))","Total number of data values missing in statistical process",,"Validation"
1133.00,"Product definition template 4.91 - categorical forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval",,"60-71   Specification of the outermost (or only) time range over which statistical processing is done",,"Validation"
1134.00,"Product definition template 4.91 - categorical forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","(60+12(NC-1))","Statistical process used to calculate the processed field from the field at each time increment during the time range","(see Code table 4.10)#GRIB2_6_0_1_codeflag.doc#G2_CF410","Validation"
1135.00,"Product definition template 4.91 - categorical forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","(61+12(NC-1))","Type of time increment between successive fields used in the statistical processing","(see Code table 4.11)#GRIB2_6_0_1_codeflag.doc#G2_CF411","Validation"
1136.00,"Product definition template 4.91 - categorical forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","(62+12(NC-1))","Indicator of unit of time for time range over which statistical processing is done","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Validation"
1137.00,"Product definition template 4.91 - categorical forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","(63+12(NC-1))-(66+12(NC-1))","Length of the time range over which statistical processing is done, in units defined by the previous octet",,"Validation"
1138.00,"Product definition template 4.91 - categorical forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","(67+12(NC-1))","Indicator of unit of time for the increment between the successive fields used","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Validation"
1139.00,"Product definition template 4.91 - categorical forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","(68+12(NC-1))-(71+12(NC-1))","Time increment between successive fields, in units defined by the previous octet","(see Note 3)#GRIB2_6_0_1_temp.doc#G2_Pdt491n","Validation"
1140.00,"Product definition template 4.91 - categorical forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval",,"72-nn   These octets are included only if n>1, where nn = 72+12(n-1)+12(NC-1)",,"Validation"
1141.00,"Product definition template 4.91 - categorical forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","(72+12(NC-1))-(83+12(NC-1))","As octets (60+12(NC-1)) to (71+12(NC-1)), next innermost step of processing",,"Validation"
1142.00,"Product definition template 4.91 - categorical forecasts at a horizontal level or in a horizontal layer in a continuous or non-continuous time interval","(84+12(NC-1))-nn","Additional time range specifications, included in accordance with the value of n.  Contents as octets (60+12(NC -1)) to (71+12(NC -1)), repeated as necessary",,"Validation"
1143.00,"Product definition template 4.254 - CCITT IA5 character string","10","Parameter category","(see Code table 4.1)#GRIB2_6_0_1_codeflag.doc#G2_CF41","Operational"
1144.00,"Product definition template 4.254 - CCITT IA5 character string","11","Parameter number","(see Code table 4.2)#GRIB2_6_0_1_codeflag.doc#G2_CF42","Operational"
1145.00,"Product definition template 4.254 - CCITT IA5 character string","12-15","Number of characters",,"Operational"
1146.00,"Product definition template 4.1000 - cross-section of analysis and forecast at a point in time","10","Parameter category","(see Code table 4.1)#GRIB2_6_0_1_codeflag.doc#G2_CF41","Experimental"
1147.00,"Product definition template 4.1000 - cross-section of analysis and forecast at a point in time","11","Parameter number","(see Code table 4.2)#GRIB2_6_0_1_codeflag.doc#G2_CF42","Experimental"
1148.00,"Product definition template 4.1000 - cross-section of analysis and forecast at a point in time","12","Type of generating process","(see Code table 4.3)#GRIB2_6_0_1_codeflag.doc#G2_CF43","Experimental"
1149.00,"Product definition template 4.1000 - cross-section of analysis and forecast at a point in time","13","Background generating process identifier (defined by originating centre)",,"Experimental"
1150.00,"Product definition template 4.1000 - cross-section of analysis and forecast at a point in time","14","Analysis or forecast generating process identifier (defined by originating centre)",,"Experimental"
1151.00,"Product definition template 4.1000 - cross-section of analysis and forecast at a point in time","15-16","Hours of observational data cutoff after reference time","(see Note)#GRIB2_6_0_1_temp.doc#G2_Pdt41000n","Experimental"
1152.00,"Product definition template 4.1000 - cross-section of analysis and forecast at a point in time","17","Minutes of observational data cutoff after reference time",,"Experimental"
1153.00,"Product definition template 4.1000 - cross-section of analysis and forecast at a point in time","18","Indicator of unit of time range","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Experimental"
1154.00,"Product definition template 4.1000 - cross-section of analysis and forecast at a point in time","19-22","Forecast time in units defined by octet 18",,"Experimental"
1155.00,"Product definition template 4.1001 - cross-section of averaged or otherwise statistically-processed analysis or forecast over a range of time","10","Parameter category","(see Code table 4.1)#GRIB2_6_0_1_codeflag.doc#G2_CF41","Experimental"
1156.00,"Product definition template 4.1001 - cross-section of averaged or otherwise statistically-processed analysis or forecast over a range of time","11","Parameter number","(see Code table 4.2)#GRIB2_6_0_1_codeflag.doc#G2_CF42","Experimental"
1157.00,"Product definition template 4.1001 - cross-section of averaged or otherwise statistically-processed analysis or forecast over a range of time","12","Type of generating process","(see Code table 4.3)#GRIB2_6_0_1_codeflag.doc#G2_CF43","Experimental"
1158.00,"Product definition template 4.1001 - cross-section of averaged or otherwise statistically-processed analysis or forecast over a range of time","13","Background generating process identifier (defined by originating centre)",,"Experimental"
1159.00,"Product definition template 4.1001 - cross-section of averaged or otherwise statistically-processed analysis or forecast over a range of time","14","Analysis or forecast generating process identifier (defined by originating centre)",,"Experimental"
1160.00,"Product definition template 4.1001 - cross-section of averaged or otherwise statistically-processed analysis or forecast over a range of time","15-16","Hours of observational data cutoff after reference time","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Pdt41001n","Experimental"
1161.00,"Product definition template 4.1001 - cross-section of averaged or otherwise statistically-processed analysis or forecast over a range of time","17","Minutes of observational data cutoff after reference time",,"Experimental"
1162.00,"Product definition template 4.1001 - cross-section of averaged or otherwise statistically-processed analysis or forecast over a range of time","18","Indicator of unit of time range","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Experimental"
1163.00,"Product definition template 4.1001 - cross-section of averaged or otherwise statistically-processed analysis or forecast over a range of time","19-22","Forecast time in units defined by octet 18",,"Experimental"
1164.00,"Product definition template 4.1001 - cross-section of averaged or otherwise statistically-processed analysis or forecast over a range of time","23-26","Total number of data values missing in the statistical process",,"Experimental"
1165.00,"Product definition template 4.1001 - cross-section of averaged or otherwise statistically-processed analysis or forecast over a range of time","27","Statistical process used to calculate the processed field from the field at each time increment during the time range","(see Code table 4.10)#GRIB2_6_0_1_codeflag.doc#G2_CF410","Experimental"
1166.00,"Product definition template 4.1001 - cross-section of averaged or otherwise statistically-processed analysis or forecast over a range of time","28","Type of time increment between successive fields used in the statistical processing","(see Code table 4.11)#GRIB2_6_0_1_codeflag.doc#G2_CF411","Experimental"
1167.00,"Product definition template 4.1001 - cross-section of averaged or otherwise statistically-processed analysis or forecast over a range of time","29","Indicator of unit of time for time range over which statistical processing is done","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Experimental"
1168.00,"Product definition template 4.1001 - cross-section of averaged or otherwise statistically-processed analysis or forecast over a range of time","30-33","Length of the time range over which statistical processing is done, in units defined by the previous octet",,"Experimental"
1169.00,"Product definition template 4.1001 - cross-section of averaged or otherwise statistically-processed analysis or forecast over a range of time","34","Indicator of unit of time for the increment between the successive fields used","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Experimental"
1170.00,"Product definition template 4.1001 - cross-section of averaged or otherwise statistically-processed analysis or forecast over a range of time","35-38","Time increment between successive fields, in units defined by the previous octet","(see Note 2)#GRIB2_6_0_1_temp.doc#G2_Pdt41001n","Experimental"
1171.00,"Product definition template 4.1002 - cross-section of analysis and forecast, averaged or otherwise statistically-processed over latitude or longitude","10","Parameter category","(see Code table 4.1)#GRIB2_6_0_1_codeflag.doc#G2_CF41","Experimental"
1172.00,"Product definition template 4.1002 - cross-section of analysis and forecast, averaged or otherwise statistically-processed over latitude or longitude","11","Parameter number","(see Code table 4.2)#GRIB2_6_0_1_codeflag.doc#G2_CF42","Experimental"
1173.00,"Product definition template 4.1002 - cross-section of analysis and forecast, averaged or otherwise statistically-processed over latitude or longitude","12","Type of generating process","(see Code table 4.3)#GRIB2_6_0_1_codeflag.doc#G2_CF43","Experimental"
1174.00,"Product definition template 4.1002 - cross-section of analysis and forecast, averaged or otherwise statistically-processed over latitude or longitude","13","Background generating process identifier (defined by originating centre)",,"Experimental"
1175.00,"Product definition template 4.1002 - cross-section of analysis and forecast, averaged or otherwise statistically-processed over latitude or longitude","14","Analysis or forecast generating process identifier (defined by originating centre)",,"Experimental"
1176.00,"Product definition template 4.1002 - cross-section of analysis and forecast, averaged or otherwise statistically-processed over latitude or longitude","15-16","Hours of observational data cutoff after reference time","(see Note)#GRIB2_6_0_1_temp.doc#G2_Pdt41002n","Experimental"
1177.00,"Product definition template 4.1002 - cross-section of analysis and forecast, averaged or otherwise statistically-processed over latitude or longitude","17","Minutes of observational data cutoff after reference time",,"Experimental"
1178.00,"Product definition template 4.1002 - cross-section of analysis and forecast, averaged or otherwise statistically-processed over latitude or longitude","18","Indicator of unit of time range","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Experimental"
1179.00,"Product definition template 4.1002 - cross-section of analysis and forecast, averaged or otherwise statistically-processed over latitude or longitude","19-22","Forecast time in units defined by octet 18",,"Experimental"
1180.00,"Product definition template 4.1002 - cross-section of analysis and forecast, averaged or otherwise statistically-processed over latitude or longitude","23","Horizontal dimension processed","(see Code table 4.220)#GRIB2_6_0_1_codeflag.doc#G2_CF4220","Experimental"
1181.00,"Product definition template 4.1002 - cross-section of analysis and forecast, averaged or otherwise statistically-processed over latitude or longitude","24","Treatment of missing data (e.g. below ground)","(see Code table 4.221)#GRIB2_6_0_1_codeflag.doc#G2_CF4221","Experimental"
1182.00,"Product definition template 4.1002 - cross-section of analysis and forecast, averaged or otherwise statistically-processed over latitude or longitude","25","Type of statistical processing","(see Code table 4.10)#GRIB2_6_0_1_codeflag.doc#G2_CF410","Experimental"
1183.00,"Product definition template 4.1002 - cross-section of analysis and forecast, averaged or otherwise statistically-processed over latitude or longitude","26-29","Start of range",,"Experimental"
1184.00,"Product definition template 4.1002 - cross-section of analysis and forecast, averaged or otherwise statistically-processed over latitude or longitude","30-33","End of range",,"Experimental"
1185.00,"Product definition template 4.1002 - cross-section of analysis and forecast, averaged or otherwise statistically-processed over latitude or longitude","34-35","Number of values",,"Experimental"
1186.00,"Product definition template 4.1100 - Hovmöller-type grid with no averaging or other statistical processing","10","Parameter category","(see Code table 4.1)#GRIB2_6_0_1_codeflag.doc#G2_CF41","Experimental"
1187.00,"Product definition template 4.1100 - Hovmöller-type grid with no averaging or other statistical processing","11","Parameter number","(see Code table 4.2)#GRIB2_6_0_1_codeflag.doc#G2_CF42","Experimental"
1188.00,"Product definition template 4.1100 - Hovmöller-type grid with no averaging or other statistical processing","12","Type of generating process","(see Code table 4.3)#GRIB2_6_0_1_codeflag.doc#G2_CF43","Experimental"
1189.00,"Product definition template 4.1100 - Hovmöller-type grid with no averaging or other statistical processing","13","Background generating process identifier (defined by originating centre)",,"Experimental"
1190.00,"Product definition template 4.1100 - Hovmöller-type grid with no averaging or other statistical processing","14","Analysis or forecast generating process identifier (defined by originating centre)",,"Experimental"
1191.00,"Product definition template 4.1100 - Hovmöller-type grid with no averaging or other statistical processing","15-16","Hours of observational data cutoff after reference time","(see Note)#GRIB2_6_0_1_temp.doc#G2_Pdt41100n","Experimental"
1192.00,"Product definition template 4.1100 - Hovmöller-type grid with no averaging or other statistical processing","17","Minutes of observational data cutoff after reference time",,"Experimental"
1193.00,"Product definition template 4.1100 - Hovmöller-type grid with no averaging or other statistical processing","18","Indicator of unit of time range","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Experimental"
1194.00,"Product definition template 4.1100 - Hovmöller-type grid with no averaging or other statistical processing","19-22","Forecast time in units defined by octet 18",,"Experimental"
1195.00,"Product definition template 4.1100 - Hovmöller-type grid with no averaging or other statistical processing","23","Type of first fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Experimental"
1196.00,"Product definition template 4.1100 - Hovmöller-type grid with no averaging or other statistical processing","24","Scale factor of first fixed surface",,"Experimental"
1197.00,"Product definition template 4.1100 - Hovmöller-type grid with no averaging or other statistical processing","25-28","Scaled value of first fixed surface",,"Experimental"
1198.00,"Product definition template 4.1100 - Hovmöller-type grid with no averaging or other statistical processing","29","Type of second fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Experimental"
1199.00,"Product definition template 4.1100 - Hovmöller-type grid with no averaging or other statistical processing","30","Scale factor of second fixed surface",,"Experimental"
1200.00,"Product definition template 4.1100 - Hovmöller-type grid with no averaging or other statistical processing","31-34","Scaled value of second fixed surface",,"Experimental"
1201.00,"Product definition template 4.1101 - Hovmöller-type grid with averaging or other statistical processing","10","Parameter category","(see Code table 4.1)#GRIB2_6_0_1_codeflag.doc#G2_CF41","Experimental"
1202.00,"Product definition template 4.1101 - Hovmöller-type grid with averaging or other statistical processing","11","Parameter number","(see Code table 4.2)#GRIB2_6_0_1_codeflag.doc#G2_CF42","Experimental"
1203.00,"Product definition template 4.1101 - Hovmöller-type grid with averaging or other statistical processing","12","Type of generating process","(see Code table 4.3)#GRIB2_6_0_1_codeflag.doc#G2_CF43","Experimental"
1204.00,"Product definition template 4.1101 - Hovmöller-type grid with averaging or other statistical processing","13","Background generating process identifier (defined by originating centre)",,"Experimental"
1205.00,"Product definition template 4.1101 - Hovmöller-type grid with averaging or other statistical processing","14","Analysis or forecast generating process identifier (defined by originating centre)",,"Experimental"
1206.00,"Product definition template 4.1101 - Hovmöller-type grid with averaging or other statistical processing","15-16","Hours of observational data cutoff after reference time","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Pdt41101n","Experimental"
1207.00,"Product definition template 4.1101 - Hovmöller-type grid with averaging or other statistical processing","17","Minutes of observational data cutoff after reference time",,"Experimental"
1208.00,"Product definition template 4.1101 - Hovmöller-type grid with averaging or other statistical processing","18","Indicator of unit of time range","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Experimental"
1209.00,"Product definition template 4.1101 - Hovmöller-type grid with averaging or other statistical processing","19-22","Forecast time in units defined by octet 18","(see Note 2)#GRIB2_6_0_1_temp.doc#G2_Pdt41101n","Experimental"
1210.00,"Product definition template 4.1101 - Hovmöller-type grid with averaging or other statistical processing","23","Type of first fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Experimental"
1211.00,"Product definition template 4.1101 - Hovmöller-type grid with averaging or other statistical processing","24","Scale factor of first fixed surface",,"Experimental"
1212.00,"Product definition template 4.1101 - Hovmöller-type grid with averaging or other statistical processing","25-28","Scaled value of first fixed surface",,"Experimental"
1213.00,"Product definition template 4.1101 - Hovmöller-type grid with averaging or other statistical processing","29","Type of second fixed surface","(see Code table 4.5)#GRIB2_6_0_1_codeflag.doc#G2_CF45","Experimental"
1214.00,"Product definition template 4.1101 - Hovmöller-type grid with averaging or other statistical processing","30","Scale factor of second fixed surface",,"Experimental"
1215.00,"Product definition template 4.1101 - Hovmöller-type grid with averaging or other statistical processing","31-34","Scaled value of second fixed surface",,"Experimental"
1216.00,"Product definition template 4.1101 - Hovmöller-type grid with averaging or other statistical processing","35-38","Total number of data values missing in the statistical process",,"Experimental"
1217.00,"Product definition template 4.1101 - Hovmöller-type grid with averaging or other statistical processing","39","Statistical process used to calculate the processed field from the field at each time increment during the time range","(see Code table 4.10)#GRIB2_6_0_1_codeflag.doc#G2_CF410","Experimental"
1218.00,"Product definition template 4.1101 - Hovmöller-type grid with averaging or other statistical processing","40","Type of time increment between successive fields used in the statistical processing","(see Code table 4.11)#GRIB2_6_0_1_codeflag.doc#G2_CF411","Experimental"
1219.00,"Product definition template 4.1101 - Hovmöller-type grid with averaging or other statistical processing","41","Indicator of unit of time for time range over which statistical processing is done","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Experimental"
1220.00,"Product definition template 4.1101 - Hovmöller-type grid with averaging or other statistical processing","42-45","Length of the time range over which statistical processing is done, in units defined by the previous octet",,"Experimental"
1221.00,"Product definition template 4.1101 - Hovmöller-type grid with averaging or other statistical processing","46","Indicator of unit of time for increment between the successive fields used","(see Code table 4.4)#GRIB2_6_0_1_codeflag.doc#G2_CF44","Experimental"
1222.00,"Product definition template 4.1101 - Hovmöller-type grid with averaging or other statistical processing","47-50","Time increment between successive fields, in units defined by the previous octet","(see Note 3)#GRIB2_6_0_1_temp.doc#G2_Pdt41101n","Experimental"
1223.00,"Data representation template 5.0 - Grid point data - simple packing","12-15","Reference value (R) (IEEE 32-bit floating-point value)",,"Operational"
1224.00,"Data representation template 5.0 - Grid point data - simple packing","16-17","Binary scale factor (E)",,"Operational"
1225.00,"Data representation template 5.0 - Grid point data - simple packing","18-19","Decimal scale factor (D)",,"Operational"
1226.00,"Data representation template 5.0 - Grid point data - simple packing","20","Number of bits used for each packed value for simple packing, or for each group reference value for complex packing or spatial differencing",,"Operational"
1227.00,"Data representation template 5.0 - Grid point data - simple packing","21","Type of original field values","(see Code table 5.1)#GRIB2_6_0_1_codeflag.doc#G2_CF51","Operational"
1228.00,"Data representation template 5.1 - Matrix values at grid point - simple packing","12-21","Same as data representation template 5.0",,"Operational"
1229.00,"Data representation template 5.1 - Matrix values at grid point - simple packing","22","0, no matrix bit maps present; 1-matrix bit maps present",,"Operational"
1230.00,"Data representation template 5.1 - Matrix values at grid point - simple packing","23-26","Number of data values encoded in Section 7",,"Operational"
1231.00,"Data representation template 5.1 - Matrix values at grid point - simple packing","27-28","NR - first dimension (rows) of each matrix",,"Operational"
1232.00,"Data representation template 5.1 - Matrix values at grid point - simple packing","29-30","NC - second dimension (columns) of each matrix",,"Operational"
1233.00,"Data representation template 5.1 - Matrix values at grid point - simple packing","31","First dimension coordinate value definition","(Code table 5.2)#GRIB2_6_0_1_codeflag.doc#G2_CF52","Operational"
1234.00,"Data representation template 5.1 - Matrix values at grid point - simple packing","32","NC1 - number of coefficients or values used to specify first dimension coordinate function",,"Operational"
1235.00,"Data representation template 5.1 - Matrix values at grid point - simple packing","33","Second dimension coordinate value definition","(Code table 5.2)#GRIB2_6_0_1_codeflag.doc#G2_CF52","Operational"
1236.00,"Data representation template 5.1 - Matrix values at grid point - simple packing","34","NC2 - number of coefficients or values used to specify second dimension coordinate function",,"Operational"
1237.00,"Data representation template 5.1 - Matrix values at grid point - simple packing","35","First dimension physical significance","(Code table 5.3)#GRIB2_6_0_1_codeflag.doc#G2_CF53","Operational"
1238.00,"Data representation template 5.1 - Matrix values at grid point - simple packing","36","Second dimension physical significance","(Code table 5.3)#GRIB2_6_0_1_codeflag.doc#G2_CF53","Operational"
1239.00,"Data representation template 5.1 - Matrix values at grid point - simple packing","37-(36+NC1*4)","Coefficients to define first dimension coordinate values in functional form, or the explicit coordinate values (IEEE 32-bit floating-point value)",,"Operational"
1240.00,"Data representation template 5.1 - Matrix values at grid point - simple packing","(37+NC1*4)-(36+4(NC1+NC2))","Coefficients to define second dimension coordinate values in functional form, or the explicit coordinate values (IEEE 32-bit floating-point value)",,"Operational"
1241.00,"Data representation template 5.2 - Grid point data - complex packing","12-21","Same as data representation template 5.0",,"Operational"
1242.00,"Data representation template 5.2 - Grid point data - complex packing","22","Group splitting method used","(see Code table 5.4)#GRIB2_6_0_1_codeflag.doc#G2_CF54","Operational"
1243.00,"Data representation template 5.2 - Grid point data - complex packing","23","Missing value management used","(see Code table 5.5)#GRIB2_6_0_1_codeflag.doc#G2_CF55","Operational"
1244.00,"Data representation template 5.2 - Grid point data - complex packing","24-27","Primary missing value substitute",,"Operational"
1245.00,"Data representation template 5.2 - Grid point data - complex packing","28-31","Secondary missing value substitute",,"Operational"
1246.00,"Data representation template 5.2 - Grid point data - complex packing","32-35","NG - number of groups of data values into which field is split",,"Operational"
1247.00,"Data representation template 5.2 - Grid point data - complex packing","36","Reference for group widths","(see Note 12)#GRIB2_6_0_1_temp.doc#G2_Drt52n","Operational"
1248.00,"Data representation template 5.2 - Grid point data - complex packing","37","Number of bits used for the group widths (after the reference value in octet 36 has been removed)",,"Operational"
1249.00,"Data representation template 5.2 - Grid point data - complex packing","38-41","Reference for group lengths","(see Note 13)#GRIB2_6_0_1_temp.doc#G2_Drt52n","Operational"
1250.00,"Data representation template 5.2 - Grid point data - complex packing","42","Length increment for the group lengths","(see Note 14)#GRIB2_6_0_1_temp.doc#G2_Drt52n","Operational"
1251.00,"Data representation template 5.2 - Grid point data - complex packing","43-46","True length of last group",,"Operational"
1252.00,"Data representation template 5.2 - Grid point data - complex packing","47","Number of bits used for the scaled group lengths (after subtraction of the reference value given in octets 38-41 and division by the length increment given in octet 42)",,"Operational"
1253.00,"Data representation template 5.3 - Grid point data - complex packing and spatial differencing","12-47","Same as data representation template 5.2",,"Operational"
1254.00,"Data representation template 5.3 - Grid point data - complex packing and spatial differencing","48","Order of spatial differencing","(see Code table 5.6)#GRIB2_6_0_1_codeflag.doc#G2_CF56","Operational"
1255.00,"Data representation template 5.3 - Grid point data - complex packing and spatial differencing","49","Number of octets required in the data section to specify extra descriptors needed for spatial differencing (octets 6-ww in data template 7.3)",,"Operational"
1256.00,"Data representation template 5.4 - Grid point data - IEEE floating point data","12","Precision","(see Code table 5.7)#GRIB2_6_0_1_codeflag.doc#G2_CF57","Operational"
1257.00,"Data representation template 5.40 - Grid point data - JPEG 2000 code stream format","12-15","Reference value (R) (IEEE 32-bit floating-point value)",,"Operational"
1258.00,"Data representation template 5.40 - Grid point data - JPEG 2000 code stream format","16-17","Binary scale factor (E)",,"Operational"
1259.00,"Data representation template 5.40 - Grid point data - JPEG 2000 code stream format","18-19","Decimal scale factor (D)",,"Operational"
1260.00,"Data representation template 5.40 - Grid point data - JPEG 2000 code stream format","20","Number of bits required to hold the resulting scaled and referenced data values (i.e. depth of the grayscale image)","(see Note 2)#GRIB2_6_0_1_temp.doc#G2_Drt540n","Operational"
1261.00,"Data representation template 5.40 - Grid point data - JPEG 2000 code stream format","21","Type of original field values (see Code table 5.1)",,"Operational"
1262.00,"Data representation template 5.40 - Grid point data - JPEG 2000 code stream format","22","Type of compression used. (see Code table 5.40)",,"Operational"
1263.00,"Data representation template 5.40 - Grid point data - JPEG 2000 code stream format","23","Target compression ratio, M:1 (with respect to the bit-depth specified in octet 20), when octet 22 indicates lossy compression. Otherwise, set to missing","(see Note 3)#GRIB2_6_0_1_temp.doc#G2_Drt540n","Operational"
1264.00,"Data representation template 5.41 - Grid point data - Portable Network Graphics (PNG) format","12-15","Reference value (R) (IEEE 32-bit floating-point value)",,"Operational"
1265.00,"Data representation template 5.41 - Grid point data - Portable Network Graphics (PNG) format","16-17","Binary scale factor (E)",,"Operational"
1266.00,"Data representation template 5.41 - Grid point data - Portable Network Graphics (PNG) format","18-19","Decimal scale factor (D)",,"Operational"
1267.00,"Data representation template 5.41 - Grid point data - Portable Network Graphics (PNG) format","20","Number of bits required to hold the resulting scaled and referenced data values (i.e. depth of the image)","(see Note 2)#GRIB2_6_0_1_temp.doc#G2_Drt541n","Operational"
1268.00,"Data representation template 5.41 - Grid point data - Portable Network Graphics (PNG) format","21","Type of original field values","(see Code table 5.1)#GRIB2_6_0_1_codeflag.doc#G2_CF51","Operational"
1269.00,"Data representation template 5.42 - Grid point and spectral data - CCSDS szip","12-15","Reference value (R) (IEEE 32-bit floating-point value)",,"Validation"
1270.00,"Data representation template 5.42 - Grid point and spectral data - CCSDS szip","16-17","Binary scale factor (E)",,"Validation"
1271.00,"Data representation template 5.42 - Grid point and spectral data - CCSDS szip","18-19","Decimal scale factor (D)",,"Validation"
1272.00,"Data representation template 5.42 - Grid point and spectral data - CCSDS szip","20","Number of bits required to hold the resulting scaled and referenced data values.",,"Validation"
1273.00,"Data representation template 5.42 - Grid point and spectral data - CCSDS szip","21","Type of original field values","(see Code table 5.1)#GRIB2_6_0_1_codeflag.doc#G2_CF51","Validation"
1274.00,"Data representation template 5.42 - Grid point and spectral data - CCSDS szip","22","szip options mask",,"Validation"
1275.00,"Data representation template 5.42 - Grid point and spectral data - CCSDS szip","23","szip bits per pixel",,"Validation"
1276.00,"Data representation template 5.42 - Grid point and spectral data - CCSDS szip","24-25","szip pixels per block",,"Validation"
1277.00,"Data representation template 5.42 - Grid point and spectral data - CCSDS szip","26-27","szip pixels per scan line",,"Validation"
1278.00,"Data representation template 5.50 - Spectral data - simple packing","12-15","Reference value (R) (IEEE 32-bit floating-point value)",,"Operational"
1279.00,"Data representation template 5.50 - Spectral data - simple packing","16-17","Binary scale factor (E)",,"Operational"
1280.00,"Data representation template 5.50 - Spectral data - simple packing","18-19","Decimal scale factor (D)",,"Operational"
1281.00,"Data representation template 5.50 - Spectral data - simple packing","20","Number of bits used for each packed value (field width)",,"Operational"
1282.00,"Data representation template 5.50 - Spectral data - simple packing","21-24","Real part of (0.0) coefficient (IEEE 32-bit floating-point value)",,"Operational"
1283.00,"Data representation template 5.51 - Spherical harmonics data - complex packing","12-20","Same as data representation template 5.50",,"Operational"
1284.00,"Data representation template 5.51 - Spherical harmonics data - complex packing","21-24","P - Laplacian scaling factor (expressed in 10**-6 units)",,"Operational"
1285.00,"Data representation template 5.51 - Spherical harmonics data - complex packing","25-26","JS - pentagonal resolution parameter of the unpacked subset","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Drt551n","Operational"
1286.00,"Data representation template 5.51 - Spherical harmonics data - complex packing","27-28","KS - pentagonal resolution parameter of the unpacked subset","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Drt551n","Operational"
1287.00,"Data representation template 5.51 - Spherical harmonics data - complex packing","29-30","MS - pentagonal resolution parameter of the unpacked subset","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Drt551n","Operational"
1288.00,"Data representation template 5.51 - Spherical harmonics data - complex packing","31-34","TS - total number of values in the unpacked subset","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Drt551n","Operational"
1289.00,"Data representation template 5.51 - Spherical harmonics data - complex packing","35","Precision of the unpacked subset","(see Code table 5.7)#GRIB2_6_0_1_codeflag.doc#G2_CF57","Operational"
1290.00,"Data representation template 5.61 - Grid point data - simple packing with logarithm pre-processing","12-15","Reference value (R) (IEEE 32-bit floating-point value)",,"Experimental"
1291.00,"Data representation template 5.61 - Grid point data - simple packing with logarithm pre-processing","16-17","Binary scale factor (E)",,"Experimental"
1292.00,"Data representation template 5.61 - Grid point data - simple packing with logarithm pre-processing","18-19","Decimal scale factor (D)",,"Experimental"
1293.00,"Data representation template 5.61 - Grid point data - simple packing with logarithm pre-processing","20","Number of bits used for each packed value",,"Experimental"
1294.00,"Data representation template 5.61 - Grid point data - simple packing with logarithm pre-processing","21-24","Pre-processing parameter (B) (IEEE 32-bit floating-point value)",,"Experimental"
1295.00,"Data representation template 5.200 - Grid point data - run length packing with level values","12","Number of bits used for each packed value in the run length packing with level values",,"Operational"
1296.00,"Data representation template 5.200 - Grid point data - run length packing with level values","13-14","MV - maximum value within the levels that are used in the packing",,"Operational"
1297.00,"Data representation template 5.200 - Grid point data - run length packing with level values","15-16","MVL - maximum value of level (predefined)",,"Operational"
1298.00,"Data representation template 5.200 - Grid point data - run length packing with level values","17","Decimal scale factor of representative value of each level",,"Operational"
1299.00,"Data representation template 5.200 - Grid point data - run length packing with level values","18-(19+2(lv-1))","List of MVL scaled representative values of each level from lv=1 to MVL",,"Operational"
1300.00,"Data template 7.0 - Grid point data - simple packing","6-nn","Binary data values - binary string, with each (scaled) data value",,"Operational"
1301.00,"Data template 7.1 - Matrix values at grid point - simple packing","6-nn","Binary data values - binary string, with each (scaled) data value",,"Validation"
1302.00,"Data template 7.2 - Grid point data - complex packing","6-xx","NG group reference values (X1 in the decoding formula), each of which is encoded using the number of bits specified in octet 20 of data representation template 5.0. Bits set to zero shall be appended as necessary to ensure this sequence of numbers ends on",,"Operational"
1303.00,"Data template 7.2 - Grid point data - complex packing","[xx+1]-yy","NG group widths, each of which is encoded using the number of bits specified in octet 37 of data representation template 5.2. Bits set to zero shall be appended as necessary to ensure this sequence of numbers ends on an octet boundary",,"Operational"
1304.00,"Data template 7.2 - Grid point data - complex packing","[yy+1]-zz","NG scaled group lengths, each of which is encoded using the number of bits specified in octet 47 of data representation template 5.2. Bits set to zero shall be appended as necessary to ensure this sequence of numbers ends on an octet boundary","(see Note 14 of data representation template 5.2)#GRIB2_6_0_1_temp.doc#G2_Drt52n","Operational"
1305.00,"Data template 7.2 - Grid point data - complex packing","[zz+1]-nn","Packed values (X2 in the decoding formula), where each value is a deviation from its respective group reference value",,"Operational"
1306.00,"Data template 7.3 - Grid point data - complex packing and spatial differencing","6-ww","First value(s) of original (undifferenced) scaled data values, followed by the overall minimum of the differences. The number of values stored is 1 greater than the order of differentiation, and the field width is described at octet 49 of data representation template 5.3","(see Note 1)#GRIB2_6_0_1_temp.doc#G2_Dt73n","Operational"
1307.00,"Data template 7.3 - Grid point data - complex packing and spatial differencing","[ww+1]-xx","NG group reference values (X1 in the decoding formula), each of which is encoded using the number of bits specified in octet 20 of data representation template 5.0. Bits set to zero shall be appended where necessary to ensure this sequence of numbers ends on an octet boundary",,"Operational"
1308.00,"Data template 7.3 - Grid point data - complex packing and spatial differencing","[xx+1]-nn","Same as for data representation template 7.2",,"Operational"
1309.00,"Data template 7.4 - Grid point data - IEEE floating point data","6-nn","Binary data values",,"Operational"
1310.00,"Data template 7.40 - Grid point data - JPEG 2000 code stream format","6-nn","JPEG 2000 code stream as described in Part 1 of the JPEG 2000 standard. (ISO/IEC 15444-1:2000)",,"Operational"
1311.00,"Data template 7.41 - Grid point data - Portable Network Graphics (PNG) format","6-nn","PNG encoded image",,"Operational"
1312.00,"Data template 7.50 - Spectral data - simple packing","6-nn","Binary data values - binary string, with each (scaled) data value",,"Operational"
1313.00,"Data template 7.51 - Spherical harmonics - complex packing","6-(5+IxTS)","Data values from the unpacked subset (IEEE floating-point values on I octets)",,"Operational"
1314.00,"Data template 7.51 - Spherical harmonics - complex packing","(6+IxTS)-nn","Binary data values - binary string, with each (scaled) data value out of the unpacked subset",,"Operational"
